arXiv:0705.0517v1 [cond-mat.supr-con] 3 May 2007

Superconductivity in epitaxial thin films of Na_xCoO_2·yD_2O

Y. Krockenberger,^{1, 2} I. Fritsch,^1 G. Christiani,^1 H.-U. Habermeier,^1 Li Yu,^1 C. Bernhard,^1 B. Keimer,^1 and L. Alff^2 1Max-Planck-Institute for Solid State Research, Heisenbergstr. 1, 70569 Stuttgart, Germany 2Darmstadt University of Technology, Petersenstr. 23, 64287 Darmstadt, Germany (Dated: 24th November 2005)

The observation of superconductivity in the layered transition metal oxide NaxCoO2 · yH2O (K. Takada, H. Sakurai, E. Takayama-Muromachi, F. Izumi, R. A. Dilanian, and T. Sasaki, Nature (London) 422, 53 (2003)) has caused a tremendous upsurge of scientific interest due to its similarities and its differences to the copper based high-temperature superconductors. Two years after the discovery, we report the fabrication of single-phase superconducting epitaxial thin films of Na0.3CoO2 · 1.3D2 O grown by pulsed laser deposition technique. This opens additional roads for experimental research exploring the superconducting state and the phase diagram of this unconventional material.

PACS numbers: 74.90.+n 81.05.Zx 81.15.Fg

Superconductivity in Na_xCoO_2 · yH_2O is a property of the cobalt oxide planes. Like in the case of the cuprates, the phase diagram of sodium cobaltate encompasses several competing electronic phases [2, 3, 4], and there are many indications that the superconducting state is unconventional [5, 6]. While in high-temperature superconductors the two-dimensional character of the corresponding copper oxide planes is stabilized by the intrinsically strongly anisotropic crystal structure, in Na_xCoO_2 a complicated water intercalation process is needed to amplify this anisotropy and induce superconductivity. The main difficulties in fabricating high-quality bulk material of Na_xCoO_2 ·yH_2O are the following: First, sodium can be inhomogeneously distributed in the entire bulk sample, resulting in an ill-defined doping level. Second, impurity Co oxides such as CoO and Co_3O_4 are likely to grow due to the high volatility of sodium. Third, it is difficult to avoid the formation of Na_2CO_3 in conventional bulk sample fabrication. As a result, high-quality single crystals or bulk samples of Na_xCoO_2 · yH_2O are rare, and it is even more difficult to obtain clean surfaces for optical spectroscopy and tunnelling experiments in this material. While high-quality thin films of hightemperature superconductors has allowed a large variety of phase-sensitive experiments to explore the symmetry of the superconducting order parameter, corresponding studies have thus far not proven possible for waterintercalated sodium cobaltate, due to the lack of superconducting thin films. Thin-film deposition techniques offer major advantages in the synthesis of high-quality samples, such as a well-defined vacuum and oxidizing environment. Recently, epitaxial growth of high-quality, ”dry” Na_xCoO_2 films by pulsed laser deposition on Sr- TiO3 substrates has been reported [7, 8]. In these thin films, phase purity was established within the detection limits of x-ray diffraction in four-circle geometry, and flat surfaces are obtained. As a further milestone, we now report the fabrication of superconducting thin films of Na_xCoO_2 · yH_2O.

The control and the determination of the sodium contents are essential to the growth of Na_xCoO_2. For bulk materials, methods such as inductively coupled plasma - atomic emission spectroscopy (ICP-AES) and energy dispersive x-ray (EDX) analysis are available, but the results are often difficult to interpret due to the presence of the above mentioned impurity phases. These methods cannot be applied to thin films, because the material quantity is too low. However, it is well known that for doped oxide materials the lattice parameters depend strongly on the doping level. A well-known example are the high-temperature superconductors, see for instance Ref. [9]. For Na_xCoO_2, the in-plane lattice constant a shows almost no dependence on doping, but doping does have a significant effect on the c-axis parameter (see Fig. 1). With increasing Na contents, positive charge accumulates between the CoO_2 layers, and as a result, the c-axis shrinks. The linear decrease of the c-axis lattice

Figure 1: Lattice parameters from literature for independently refined diffraction and ICP-AES measurements for different x in NaxCoO2. Between x = 0.85 and 0.95 there is a symmetry change of the crystal structure from point group 194 to 165. In the doping range from x = 0.25 to x = 0.85 the c-axis parameter varies linearly with doping. The a-axis parameter varies only about 20 pm throughout the whole doping range.

Figure 2: White light interferometric scan image of the surface of a Na0.3CoO2 · 1.3D2 O thin film on SrTiO3 (001). Within the blue regions the surface roughness is below 10 nm. The rare spikes arise from sodium carbonate.

parameter with increased doping is a useful and accurate, albeit indirect, tool to determine the sodium contents of Na_xCoO_2.

In order to obtain superconducting Na_xCoO_2 · yH_2O thin films, it is necessary to intercalate water into samples with doping levels of about x = 0.3. This goal can be achieved by first stabilizing Na_xCoO_2 thin films with x ≃ 0.6 on SrTiO_3 (001) substrates [7]. For obtaining a film at the desired composition x = 0.3, it is vital to provide a strong oxidizing agent to deintercalate Na^+ ions. In principle, this can in be accomplished by the standard Br_2-CH_3CN-solution method, which is also used for bulk synthesis [1]. However, we have found that NO_2-BF_4 is superior to the conventional method, as Br is avoided and the deintercalation time scale is considerably accelerated. The decisive step is the intercalation of water into the thin films. In contrast to bulk materials, single-phase thin films cannot be simply immersed into water, because the thin films tend to peel off the substrate. Only a much milder method allows the successful fabrication of superconducting thin films. Oxygen flow with 100% humidity supplied by a D_2O bath at a well-defined temperature (19^∘C) is provided to the sample over several days (196 h). In contrast to alternative preparation routes, this method also yields a clean and smooth surface (see Fig. 2), which is a necessary prerequisite for meaningful surface-sensitive measurements. Xray diffraction clearly confirms the synthesis of correctly water-intercalated sodium cobaltate Na_xCoO_2·yD_2O epitaxial thin film with the desired doping level x = 0.3 and water content y = 1.3 (see Fig. 3).

The water-intercalated Na_xCoO_2 · yD_2O thin films indeed show superconductivity for x = 0.3 and y = 1.3 with T_{C,zero} about 4.2 K (see Fig. 4). The relatively sharp superconducting transition with a width of 1.5 K in the resistivity vs. temperature curve confirms the high quality of the thin films. Above the critical temperature, the thin films show metallic behavior up to room temperature

Figure 3: X-ray diffraction pattern for epitaxial Na0.3CoO2 · 1.3D2 O on SrTiO3 (001). Impurity phases are below the detection limit.

with almost linear slope, similar to the high-temperature superconductors.

As a first flavor of the experimental possibilities which are opened through the achievement of these high quality Na_xCoO_2 thin films we present in Fig. 5 the far-infrared dielectric response function, ε = ε_1 + iε_2, at T = 10 K of a series of water-free samples that cover a wide range of doping from 0.31 < x < 0.84. Displayed are the real parts of the optical conductivity, σ_1 = ω/4πε_2 and of the dielectric function, ε_1, as measured directly by spectral ellipsometry using the ANKA synchrotron light source at Forschungszentrum Karlsruhe [10] (the contributions of the SrTiO_3 or the LaAlO_3 substrates are subtracted). The inset displays the evolution of the corre-

sponding squared plasma frequency, ω^2_p = 4πn m^∗ , with n

Figure 4: Resistivity vs temperature for an epitaxial Na0.3CoO2 · 1.3D2 O thin film on SrTiO3 (001). In the inset superconducting quantum interference device (SQUID) magnetization measurement shows unambiguously the flux expulsion effect at the critical temperature of about 4.2 K.

Figure 5: Real parts of optical conductivity and dielectric function as a function of doping x in NaxCoO2 films on SrTiO3 (S) or LaAlO3 (L) substrates. The free carrier plasma frequency, ω^2_p (see inset) clearly tracks the phase diagram of sodium cobaltate [4] consisting of two metallic regions that are separated by an insulating region at half filling of x = 1/2.

the carrier density and m^∗ their effective mass, that has been deduced with a Drude-Lorentz fitting function. The free carrier response evidently exhibits a very strong and characteristic variation as a function of Na content. It has fairly sharp maxima near x = 1/3 and 2/3 that are separated by a deep minimum near x = 1/2. It has indeed previously been noted that the range of x = 1/2 separates two metallic regions with high conductivity for x < 0.5 and x > 0.5 [2, 3]. Notably, a correspondingly rapid variation in the FIR electronic response was not observed in previous optical measurements on single crystals [11, 12]. This suggests that the films can offer significant advantages concerning the homogeneity (in particular concerning the Na content) and the surface quality that is critical for optical measurements. The high structural quality and homogeneity of these films is also evident from very narrow phonon modes in the FIR spectra whose analysis is omitted here.

The achievement of superconducting thin films of Na_xCoO_2 · yD_2O paves the way for additional experiments with this unconventional superconductor. Thin film based Josephson and tunnelling experiments, which are expected to yield important clues to the unconventional nature of superconductivity in this material, can now readily be performed. Further, superconducting quantum interference device (SQUID) experiments now come within reach. Such experiments could confirm that, following the discovery of p-wave superconductivity in Sr_2RuO_4 [13], the compound Na_xCoO_2 · yH_2O is another metallic solid-state analog to liquid^3He with an even higher transition temperature. In a very recent paper, it was even suggested that Na_xCoO_2 · yH_2O is an f-wave superconductor [14] which would make this material the most exotic one discovered so far. Following the successful example of high-temperature superconductors, high-quality superconducting thin film samples of waterintercalated sodium cobaltate thus promise to enhance our knowledge about this complex material.

[1] K. Takada, H. Sakurai, E. Takayama-Muromachi, F. Izumi, R. A. Dilanian, and T. Sasaki, Nature (London) 422, 53 (2003).

[2] C. J. Milne, T. Klimczuk, M. L. Foo, and R. J. Cava, Nature (London) 424, 527 (2003).

[3] C. J. Milne, D. N. Argyriou, A. Chemseddine, N. Aliouane, J. Veira, S. Landsgesell, and D. Alber, Phys. Rev. Lett. 93, 247007 (2004).

[4] N. P. Ong and R. J. Cava, Science 305, 52 (2004). [5] T. Fujimoto, Guo-qing Zheng, Y. Kitaoka, R. L. Meng, J. Cmaidalka, and C. W. Chu, Phys. Rev. Lett. 92, 047004 (2004).

[6] Y. Bang, M. J. Graf, and A. V. Balatsky, Phys. Rev. B 68, 212504 (2003).

[7] Y. Krockenberger, I. Fritsch, G. Cristiani, A. Matveev, L. Alff, H.-U. Habermeier, and B. Keimer. Appl. Phys. Lett. 86, 191913 (2005).

[8] H. Ohta, S.-W. Kim, S. Ohta, K. Koumoto, M. Hirano, and H. Hosono, Crystal Growth & Design 5, 25 (2005).

[9] M. Naito and M. Hepp, Jpn. J. Appl. Phys. 39, L485 (2000).

[10] C. Bernhard, J. Humlícek, and B. Keimer, Thin Solid Films 455, 143 (2004).

[11] S. Lupi, M. Ortolani, L. Baldassarre, P. Calvani, D. Prabhakaran, and A. T. Boothroyd, Phys. Rev. B 72, 024550 (2005).

[12] J. Hwang, J. Yang, T. Timusk, and F. C. Chou, Phys. Rev. B 72, 024549 (2005).

[13] K. D. Nelson, Z. Q. Mao, Y. Maeno, and Y. Liu, Science 306, 1151 (2004).

[14] I. I. Mazin and M. D. Johannes, Nature Physics (London) 1, 91 (2005).