arXiv:0707.3368v1 [astro-ph] 23 Jul 2007

Astronomy & Astrophysics manuscript no. aapaper © ESO 2023 April 27, 2023

30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (Research Note)

S. R. Lowe^1, M. P. Gawroński^2, P. N. Wilkinson^1 , A. J. Kus^2, I. W. A. Browne^1, E. Pazderski^2, R. Feiler^2, and D. Kettle^1

1 University of Manchester, Jodrell Bank Observatory, Macclesfield, Cheshire, SK11 9DL, UK

e-mail: Stuart.Lowe@manchester.ac.uk 2 Toruń Centre for Astronomy, Nicolaus Copernicus University, 87-148 Toruń/Piwnice, Poland

Received June 7, 2007; accepted ???

ABSTRACT

Aims. To measure the 30-GHz flux densities of the 293 sources in the Caltech-Jodrell Bank flat-spectrum (CJF) sample. The measurements are part of an ongoing programme to measure the spectral energy distributions of flat spectrum radio sources and to correlate them with the milliarcsecond structures from VLBI and other measured astrophysical properties.

Methods. The 30-GHz data were obtained with a twin-beam differencing radiometer system mounted on the Toruń 32-m telescope. The system has an angular resolution of 1.2^′.

Results. Together with radio spectral data obtained from the literature, the 30-GHz data have enabled us to identify 42 of the CJF sources as Giga-hertz Peaked Spectrum (GPS) sources. Seventeen percent of the sources have rising spectra (α > 0) between 5 and 30 GHz.

Key words. Astronomical data bases: miscellaneous – Radio continuum: galaxies

1. Introduction

The emission from most flat-spectrum radio sources, from radio frequencies through gamma-rays, is thought to arise in relativistic jets and be beamed synchrotron self-Compton emission. Often described as blazar emission it is characterized by two peaks in the spectral energy distribution (SED), one synchrotron and one inverse Compton. From object to object the peak frequency can occur anywhere between 10^{10} Hz to 10^{15} Hz. There are claims that where the peaks occur depends systematically on radio luminosity (Fossati et al. 1998; Ghisellini et al. 2002). The correlation is in the sense that the synchrotron peak frequency increases as the luminosity decreases. This is potentially an important result but has been questioned by several authors (e.g. Antón & Browne 2005). A major problem is, however, the lack of good quality SEDs on well-defined samples of objects and for this reason we have embarked on a programme to try to rectify this deficiency. Flux density measurements at centimeter wavelengths and shorter are the most important in order to define the position of the synchrotron peak. Here we report measurements with a new receiver, OCRA-p on the Torun 32m Telescope at a wavelength of 1cm.

The CJF sample is currently the best studied sample of flatspectrum radio sources. The CJF sample (Taylor et al. 1996) consists of 293 sources selected from three previous VLBI surveys: the PR survey (Pearson & Readhead 1988), the first Caltech-Jodrell (CJ) survey (CJ1: Polatidis et al. 1995) and the second Caltech-Jodrell survey (CJ2: Taylor et al. 1994). The selection criteria were:

Send offprint requests to: S. R. Lowe

1. S_{4.85 GHz} ≥ 350 mJy

2. α^{4.85 GHz}

1.4 GHz ≥ −0.5 1 3. δ(1950) ≥ 35^∘

4. |b| ≥ 10^∘

In addition to the structural information obtained in the CJ VLBI surveys, extensive follow-up observations have been made with the VLBA (Britzen et al. in prep) to study the statistics of superluminal motions; redshift information is available for > 90% of the sample. Furthermore, all 293 sources have been observed in soft X-rays, either as part of the ROSAT All-Sky Survey or in ROSAT pointed observations (Britzen et al. 2002). The CJF sample is therefore a natural starting point for a programme aimed at understanding the relationships between the broadband SEDs and the spatial structure, kinematics and X-ray properties of compact radio sources. Several different types of objects are found in samples selected, like CJF, from radio surveys made at relatively low (few GHz) frequencies. While the sample is dominated by highly-relativistic “core-jet” sources it also contains the precursors of large-scale double sources (the Compact Symmetric Objects, CSOs: e.g. Wilkinson et al. 1994; Readhead et al. 1996a,b) and perhaps a few ULIRGS (typically more distant and luminous versions of the starburst galaxy, Arp 220). VLBI observations immediately distinguish between these different types: the core-jet sources are highly asymmetric, in contrast to the CSOs, while ULIRGS are highly resolved.

The complementary radio spectral information is available from hundreds of MHz to typically ∼ 10 GHz but information

1 S ∝ ν^α

2 S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN)

Table 1. Nominal system specifications for OCRA-p on the Toruń 32-m telescope.

Frequency Range 27 − 33 GHz System Temperature, T_{sys} 40 K Individual beam FWHM 1.2^′ Beam spacing 3.1^′ Aperture Efficiency 45%

at higher frequencies is sparse. As part of the commissioning programme for the new One Centimetre Radio Array prototype (OCRA-p) we have measured the flux densities of all the CJF sources at 30 GHz using the Toruń 32-m Telescope. In addition to their intrinsic astrophysical interest the CJF sources are relatively strong and hence provide a first test of the OCRA-p system. Other early results with the OCRA-p system are presented elsewhere (Lancaster et al. 2007).

In sections 2 and 3 we briefly describe the OCRA-p system and the observing techniques we used to take the 30-GHz data. In section 4 we present the results in the form of a Table of 30- GHz flux densities. In section 5 we discuss the contribution of the new data to the classification of the CJF sample into source types, in particular CSO/GPS sources, and count the number of sources whose spectra are rising at 30 GHz.

2. OCRA-p on the Toruń 32-m telescope

The OCRA-p receiver was constructed by the University of Manchester. The basic design of the radiometer was taken from the prototype demonstrator radiometer for the Planck Low Frequency Instrument (LFI, Mandolesi et al. 2000) and is similar to the K-band receivers onboard the WMAP satellite (Jarosik et al. 2003).

Rather than switching between a source and a fixed temperature load, as in Planck, OCRA-p switches between two closely spaced horns observing the sky continuously. When mounted on the Toruń 32-m, the two beams are separated by 3.1^′, a figure set by the optics of the telescope, and therefore both receive very similar atmospheric contributions from the near-field. A phase switch in one of the radiometer arms alternates the input signals between the two output channels and, by taking the difference between the channels and between switch states, it is possible to reduce the effects of both the atmospheric and gain fluctuations in the back-end amplifiers. The differencing scheme produces positive and negative beams (see Figure 1) and this is characterised by an s-shaped response. The nominal specifications for OCRA-p are given in Table 1. The construction and commissioning of the instrument is described in detail in Lowe (2005).

The switching scheme works well despite the low altitude (200 m) of the Toru’n site. OCRA-p has been able to make good observations even during summer nights.

3. Observations

At the time these observations were taken (April - August 2005), the pointing accuracy of the 32-m radio telescope was dependent on elevation and azimuth in a complex manner. The pointing accuracy was best at relatively high elevations (50^∘ − 70^∘) and so it was desirable to confine most of our observations to this range. A pointing observation was incorporated within the overall observing strategy for each source. For each source measurement, an elevation scan of the source was first recorded.

Fig. 1. A figure to illustrate the scan strategy. An initial pointing correction is found by fitting a Gaussian function to an elevation scan (left) through the source. This correction is applied to the telescope position and then an azimuthal scan is performed. The initial pointing error can be seen in the difference in amplitudes of the beams in the two scans. The elevation scan did not pass through the centre of the source, so the amplitude is lower than the azimuth scan (right) with the elevation correction.

Custom software then fitted a Gaussian function to these data, in real time, and the central point was used to generate a pointing correction for the elevation coordinate. With the calculated elevation correction an azimuthal scan was then performed. The length of the scan was chosen to be several beam spacings in extent to allow for azimuthal pointing errors and to determine a good baseline. Figure 1 shows an indicative illustration of the scan strategy. To the left is the preliminary elevation scan and to the right, the azimuthal scan. The s-shaped response, generated as the source passes through each beam in turn, can clearly be seen in the azimuthal scan.

For each azimuthal scan a baseline and two independent Gaussian functions were fitted for each beam. At this stage, every observation that was significantly affected by atmospheric fluctuations, or that showed large asymmetries in the amplitudes of the beams, was rejected.

The amplitudes of the fitted Gaussian functions are directly related to the strength of the source. To convert the measured signal to a flux density it is necessary to calibrate against a source of known strength. Our primary flux calibrator was chosen to be the planetary nebula NGC 7027 which has an optical diameter of ∼ 15^{′′}and is circumpolar at the latitude of Toru’n. There is a recent absolute temperature calibration of NGC 7027 performed by Mason et al. (1999) who report a flux density of 5.45±0.20 Jy at 32 GHz. Assuming a spectral index of −0.1 ± 0.1 and estimating the beam dilution factor, using a simple geometric model of the emission created from 6-cm radio maps from Bryce et al. (1997), gives an expected flux density of 5.46 ± 0.20 Jy at 30 GHz. All the final flux density values have been scaled to this figure.

Although NGC 7027 is circumpolar, it is not always at a suitable elevation and can be too far from the CJF target sources for reliable calibration. A network of secondary flux density calibrators was therefore generated. The secondary calibrators were: 0010+405, 0016+731, 0109+351, 0309+411, 0633+734, 0642+449, 0821+394, 0833+585, 0955+476, 1044+719, 1144+402, 1418+546, 1638+398, 1758+388, 2007+777, 2021+614. Several of these sources show long-term variability in their emission, however the level of intrinsic

S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN) 3

intra-day variations did not contribute significantly to our final error budget.

Every three to six target observations, a secondary calibrator source was observed. The secondary calibrator measurements were calibrated using the measurements of NGC 7027. The final flux densities take into account atmospheric absorption (estimated uncertainty ∼ 2% in the correction) and a gainelevation correction (∼ 2.5%). Uncertainties in these corrections as well as pointing errors (< 1% for this observing method), uncertainties in the extrapolated flux density of NGC7027 (3.6%) and in the secondary calibration (∼ 6%) have been incorporated into the final error budget. The typical uncertainty for a single flux density measurement is in the range 8 − 10%. Since six or more measurements were usually made for each source and the errors are independent, the final uncertainties are typically around 5%.

The flux density measurements are made over a 6 GHz bandwidth (27 − 33 GHz). We note that sources with spectral curvature that is different to the primary calibrator will have systematic errors in their flux densities. However, as NGC 7027 and the majority of our sample are flat-spectrum, we neglect this effect given the other uncertainties.

4. Results

The final 30-GHz flux densities are given in Table 2. Column (1) gives the IAU B1950 source name for consistency with previous CJF observations by other authors. The J2000 coordinates are given in Columns (2) and (3) and are taken from Taylor et al. (1996). The flux densities at 5 GHz, Column (4), are also taken from Taylor et al. (1996) and are reproduced for comparison with those measured by OCRA-p at 30 GHz in Column (5). Column (6) lists the associated uncertainties in the 30 GHz flux densities. The spectral index between 1.4 GHz and 5 GHz, α^5_{1.4}, from Taylor et al. (1996) is given in Column (7) and the spectral index between 5 GHz and 30 GHz, α^{30}_5 , is given in Column (8). The formal uncertainty on α^{30}_5 , given the typical uncertainties in both the 5 and 30 GHz measurements, is < 0.1. We note however, that the uncertainties for a few objects may be larger due to variability and the fact that the observations at 5 and 30 GHz are not co-eval. The morphology, from inspection of VLBI maps, is given in Column (9).

To classify the spectral behaviour of the CJF sources, the latest spectral information was obtained from NED. For the spectral plots including the 30 GHz values, refer to http://www.manchester.ac.uk/jodrellbank/research/ocra/cjf/

5. Discussion

Figure 2 shows the distribution of spectral indices as given in Table 2. The distribution can be compared with Figure 1b in Taylor et al. (1996) which shows the spectral index distribution between 1.4 GHz and 4.85 GHz, α^{4.85}_{1.4} . The major difference is the shift to lower spectral indices mainly due to the spectral index cut-off of the CJF sample (−0.5 at 5 GHz). A significant fraction (∼ 31%) of sources are seen to have spectral indices, α^{30}_5 steeper than −0.5. This is the expected behaviour of GPS sources peaking at or above ∼ 5 GHz. Looking at the spectra as a whole we classify 42 (∼ 14%) sources as having GPS spectra (0018+729; 0102+480; 0108+388; 0145+386; 0248+430; 0615+820; 0627+532; 0636+680; 0646+600; 0700+470; 0710+439; 0711+356; 0740+768; 0859+681; 0900+520; 0950+748; 1031+567; 1107+607; 1144+352; 1205+544;

Fig. 2. Distribution of spectral indices calculated between 5 GHz and 30 GHz. Using data from Table 2.

1206+415; 1223+395; 1226+373; 1312+533; 1333+459; 1337+637; 1342+663; 1355+441; 1356+478; 1413+373; 1442+637; 1526+670; 1534+501; 1543+480; 1550+582; 1622+665; 1755+578; 1758+388; 1826+796; 1946+708; 2352+495; 2356+385). We note that O’Dea (1998) found that ∼ 10% of sources, selected at 5 GHz, were GPS. Our results on a 5 GHz sample, selected against sources with steep spectra, are therefore in rough accord with O’Dea (1998) statistics.

There are a total of 49 sources (∼ 17%) which have α^{30}_5 > 0 and can therefore be considered to have rising spectra. Only one source, 0109+351, has α^{30}_5 > 0.5 compared to the 41 which have α^5_{1.4} > 0.5 (Taylor et al. 1996). We do not, however, claim that this is clear evidence for a decrease in the number of steeply rising sources with increasing frequency but is, we suspect, simply a result of selection bias. If for example we had selected sources at 30 GHz we assert that we would have found many more sources with spectra steeply rising between 5 and 30 GHz. The same effect is seen in the results reported by Bolton et al. (2004) on the α^{43}_{15} spectral index distribution, for sources selected at 15 GHz from the 9C survey; these indicate that around 1% of these sources have spectra rising faster than 0.5 between 15 GHz and 43 GHz.

The number of sources with steeply rising spectra in high frequency surveys is of great interest because sources act as a confusing foreground to CMB studies and to SZ decrement measurements. Waldram et al. (2003) have made surveys of areas of sky at 15 GHz coincident with small area CMB fields studied with the Very Small Array (VSA, Scott et al. 2003). OCRAp measurements of these sources will be reported elsewhere. However, with the higher sensitivity over the whole sky which will be achieved by Planck, wide-field 30 GHz surveys are urgently required. We plan to install a 30 GHz 16-beam array (OCRA-F) on the Toruń telescope in 2008 and one of its main tasks will be to do such a blind survey.

Further work on spectral energy distributions is in progress and is planned for the future. Observations of 145 (130 have signal-to-noise greater than 3) of the CJF sources have been made at 850 μm with SCUBA and will be reported in Anton et al. (2007). With an improved telescope control system it will be possible to improve greatly the speed and accuracy of flux density measurements made with OCRA-p. This will facilitate a much larger programme of blazar flux density measurements and variability monitoring to be undertaken in support of the GLAST satellite which will be launched later this year.

4 S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN)

Acknowledgements. We gratefully acknowledge the financial support of the Royal Society Paul Instrument Fund which allowed us to construct the 30 GHz receiver. We are also grateful to the Polish Ministry of Science and Higher Education (grant KBN 5 P03D 024 21) which provided support for operating the receiver on the Toruń 32-m telescope. This research has made use of the NASA/IPAC Extragalactic Database (NED) which is operated by the Jet Propulsion Laboratory, California Institute of Technology, under contract with the National Aeronautics and Space Administration. S.R Lowe was supported by a PPARC studentship.

References

Antón, S. & Browne, I. W. A. 2005, MNRAS, 356, 225 Bolton, R. C., Cotter, G., Pooley, G. G., et al. 2004, MNRAS, 354, 485 Britzen, S., Brinkmann, W., Vermeulen, R. C., et al. 2002, in Proceedings of the 6th EVN Symposium, ed. E. Ros, R. W. Porcas, A. P. Lobanov, & J. A. Zensus, 99 Bryce, M., Pedlar, A., Muxlow, T., Thomasson, P., & Mellema, G. 1997, MNRAS, 284, 815 Fossati, G., Maraschi, L., Celotti, A., Comastri, A., & Ghisellini, G. 1998, MNRAS, 299, 433 Ghisellini, G., Celotti, A., & Costamante, L. 2002, A&A, 386, 833 Jarosik, N., Bennett, C. L., Halpern, M., et al. 2003, ApJS, 145, 413 Kuehr, H., Pauliny-Toth, I. I. K., Witzel, A., & Schmidt, J. 1981, AJ, 86, 854 Lancaster, K., Birkinshaw, M., Gawroński, M. P., et al. 2007, MNRAS, 378, 673 Lowe, S. R. 2005, PhD thesis, University of Manchester Mandolesi, N., Bersanelli, M., Burigana, C., & Villa, F. 2000, Astrophysical Letters Communications, 37, 151 Mason, B. S., Leitch, E. M., Myers, S. T., Cartwright, J. K., & Readhead, A. C. S.

1999, AJ, 118, 2908 O’Dea, C. P. 1998, PASP, 110, 493 Pearson, T. & Readhead, A. 1988, ApJ, 328, 114 Polatidis, A., Wilkinson, P., Xu, W., et al. 1995, ApJS, 98, 1 Readhead, A. C. S., Taylor, G. B., Pearson, T. J., & Wilkinson, P. N. 1996a, ApJ, 460, 634 Readhead, A. C. S., Taylor, G. B., Xu, W., et al. 1996b, ApJ, 460, 612 Rossetti, A., Mantovani, F., Dallacasa, D., Fanti, C., & Fanti, R. 2005, A&A, 434, 449 Scott, P. F., Carreira, P., Cleary, K., et al. 2003, MNRAS, 341, 1076 Taylor, G. B., Vermeulen, R. C., Pearson, T. J., et al. 1994, ApJS, 95, 345 Taylor, G. B., Vermeulen, R. C., Readhead, A. C. S., et al. 1996, ApJS, 107, 37 Waldram, E. M., Pooley, G. G., Grainge, K. J. B., et al. 2003, MNRAS, 342, 915 Wilkinson, P., Polatidis, A., Readhead, A., Xu, W., & Pearson, T. 1994, ApJ, 432, L87

S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN) 5

Table 2. 30-GHz flux density measurements with OCRA-p and the Toru’n 32-m telescope.; col. (1) gives the IAU B1950 source name; cols. (2) and (3) give the J2000 positions; col. (4) gives the flux densities at 5 GHz; col. (5) gives the 30-GHz OCRA-p flux densities; col. (6) gives the associated uncertainty; cols. (7) and (8) give the calculated spectral indices between 1.4 and 5 GHz (α^5_{1.4} taken from Taylor et al. 1996), and between 5 and 30 GHz (α^{30}_5 ); col. (9) indicates the VLBI morphology where c=compact, cj=core-jet, d=double, cso=compact symmetric object, mso=medium symmetric object, t=triple, g=gravitational lens.

Name R.A. (J2000) Declination (J2000) S_{5.0} (Jy) S_{30} (Jy) ΔS_{30} (Jy) α^5_{1.4} α^{30}_5 Morph. (1) (2) (3) (4) (5) (6) (7) (8) (9) 0003+380 00 05 57.2 38 20 15 0.549 0.654 0.037 -0.07 0.10 cj 0010+405 00 13 31.1 40 51 37 1.040 0.775 0.032 -0.43 -0.16 cj 0014+813 00 17 08.5 81 35 08 0.551^a 0.629 0.030 -0.17^a 0.07 cj 0016+731 00 19 45.8 73 27 30 1.712 1.612 0.067 0.54 -0.03 cj 0018+729 00 21 27.4 73 12 41 0.397 0.071 0.004 -0.42 -0.96 cj 0022+390 00 25 26.2 39 19 35 0.663 0.282 0.020 -0.11 -0.48 cj 0035+367 00 37 46.1 36 59 10 0.482 0.184 0.010 -0.47 -0.54 cj 0035+413 00 38 24.8 41 37 06 1.114 0.395 0.020 0.73 -0.58 cj 0102+480 01 05 49.9 48 19 03 1.088 0.428 0.024 0.15 -0.52 cj/c 0108+388 01 11 37.3 39 06 28 1.321 0.200 0.010 0.92 -1.05 cso 0109+351 01 12 12.9 35 22 19 0.362 1.014 0.043 0.00 0.57 cj 0110+495 01 13 27.0 49 48 24 0.710 0.570 0.032 0.30 -0.12 cj 0133+476 01 36 58.6 47 51 29 1.816 3.271 0.171 0.21 0.33 cj 0145+386 01 48 24.4 38 54 05 0.370 0.229 0.017 0.18 -0.27 cj? 0151+474 01 54 56.3 47 43 26 0.505 0.500 0.026 0.28 -0.01 cj 0153+744 01 57 35.0 74 42 43 1.549 0.148 0.007 -0.23 -1.31 cj 0205+722 02 09 51.8 72 29 26 0.560 0.715 0.037 -0.32 0.14 cj 0212+735 02 17 30.8 73 49 32 2.278 2.726 0.136 -0.11 0.10 cj 0218+357 02 21 05.5 35 56 13 1.498 0.846 0.043 0.02 -0.32 g 0219+428 02 22 39.6 43 02 07 0.806 0.801 0.043 0.00 -0.00 cj 0227+403 02 30 45.7 40 32 53 0.436 0.421 0.022 -0.00 -0.02 cj 0248+430 02 51 34.5 43 15 15 1.414 0.503 0.025 0.41 -0.58 cj/t 0249+383 02 53 08.9 38 35 24 0.450 0.286 0.015 -0.43 -0.25 cj 0251+393 02 54 42.6 39 31 34 0.408 0.321 0.019 0.25 -0.13 cj 0256+424 02 59 37.7 42 35 49 0.366 0.132 0.009 -0.41 -0.57 cj 0307+380 03 10 49.9 38 14 53 0.760 0.686 0.034 1.52 -0.06 c 0309+411 03 13 02.0 41 20 01 0.516 1.019 0.042 0.08 0.38 cj 0316+413 03 19 48.2 41 30 42 42.370 10.803 0.507 0.54 -0.76 cj 0340+362 03 43 29.0 36 22 12 0.376 0.232 0.012 0.23 -0.27 cj? 0344+405 03 47 60.0 40 43 58 0.478 0.099 0.006 -0.47 -0.88 d 0346+800 03 54 46.1 80 09 28 0.396^a 0.272 0.015 -0.25^a -0.21 cj 0402+379 04 05 49.3 38 03 32 0.937 0.285 0.016 -0.38 -0.66 cj 0424+670 04 29 06.0 67 10 16 0.362 0.080 0.004 -0.47 -0.84 c? 0444+634 04 49 23.3 63 32 09 0.606 0.699 0.034 0.39 0.08 cj 0454+844 05 08 42.4 84 32 04 1.398^a 0.266 0.015 0.40^a -0.93 cj 0537+531 05 41 16.2 53 12 24 0.665 0.230 0.011 0.01 -0.59 cj 0546+726 05 52 53.0 72 40 45 0.401 0.074 0.005 -0.16 -0.94 cj? 0554+580 05 59 13.4 58 04 03 0.906 0.496 0.024 0.70 -0.34 cj 0600+442 06 04 35.6 44 13 58 0.705 0.212 0.014 -0.42 -0.67 cj 0602+673 06 07 52.7 67 20 55 0.657 0.897 0.049 0.62 0.17 cj 0604+728 06 10 48.9 72 48 53 0.654 0.273 0.015 -0.35 -0.49 cj 0609+607 06 14 23.9 60 46 21 1.059 0.375 0.021 -0.00 -0.58 cj 0615+820 06 26 03.0 82 02 25 0.999^a 0.343 0.021 -0.03^a -0.60 c 0620+389 06 24 19.0 38 56 48 0.811 0.450 0.028 -0.32 -0.33 cj 0621+446 06 25 18.3 44 40 01 0.369 0.211 0.013 0.63 -0.31 c 0627+532 06 31 34.7 53 11 27 0.485 0.104 0.006 -0.40 -0.86 cj 0633+596 06 38 02.9 59 33 22 0.482 0.691 0.037 0.58 0.20 cj 0633+734 06 39 22.0 73 24 58 0.748 0.787 0.032 -0.30 0.03 cj 0636+680 06 42 04.3 67 58 35 0.499 0.113 0.006 1.06 -0.83 c 0641+393 06 44 53.7 39 14 47 0.453 0.322 0.016 0.17 -0.19 cj 0642+449 06 46 32.0 44 51 16 1.191 2.420 0.100 0.55 0.40 cj? 0646+600 06 50 31.3 60 01 44 0.920 0.470 0.024 0.58 -0.37 d 0650+371 06 53 58.3 37 05 40 0.977 0.619 0.036 0.40 -0.25 cj 0650+453 06 54 23.7 45 14 23 0.420 0.516 0.027 -0.27 0.11 cj 0651+410 06 55 10.0 41 00 10 0.425 0.284 0.015 0.27 -0.22 cj? 0700+470 07 04 09.6 47 00 56 0.443 0.120 0.007 -0.49 -0.73 cj

6 S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN)

Table 2. continued.

Name R.A. (J2000) Declination (J2000) S_{5.0} (Jy) S_{30} (Jy) ΔS_{30} (Jy) α^5_{1.4} α^{30}_5 Morph. (1) (2) (3) (4) (5) (6) (7) (8) (9) 0702+612 07 07 00.6 61 10 11 0.370 0.433 0.024 0.10 0.09 cj 0707+476 07 10 46.1 47 32 11 0.906 0.739 0.038 -0.06 -0.11 cj 0710+439 07 13 38.2 43 49 17 1.629 0.423 0.024 -0.09 -0.75 cso 0711+356 07 14 24.8 35 34 39 0.901 0.171 0.011 -0.36 -0.93 d 0714+457 07 17 51.9 45 38 03 0.480 0.995 0.052 0.13 0.41 cj 0716+714 07 21 53.4 71 20 36 0.788 0.546 0.029 -0.02 -0.20 cj 0718+793 07 26 11.7 79 11 31 0.631^a 0.382 0.022 0.03^a -0.28 cj 0724+571 07 28 49.6 57 01 24 0.393 0.389 0.021 -0.03 -0.01 cj 0727+409 07 30 51.3 40 49 50 0.468 0.093 0.005 0.10 -0.90 cj 0730+504 07 33 52.5 50 22 09 0.890 0.428 0.026 0.66 -0.41 cj 0731+479 07 35 02.3 47 50 08 0.533 0.256 0.015 0.17 -0.41 cj 0733+597 07 37 30.1 59 41 03 0.357 0.165 0.009 -0.34 -0.43 cj 0738+491 07 42 02.8 49 00 15 0.352 0.319 0.019 1.05 -0.05 cj? 0740+768 07 47 14.6 76 39 17 0.592^a 0.336 0.020 0.87^a -0.32 d? 0743+744 07 49 22.5 74 20 41 0.479 0.306 0.016 0.24 -0.25 cj 0746+483 07 50 20.4 48 14 53 0.860 0.422 0.030 0.21 -0.40 cj 0749+426 07 53 03.3 42 31 30 0.461 0.058 0.004 -0.33 -1.16 cj/d? 0749+540 07 53 01.4 53 52 59 0.877 0.913 0.051 0.08 0.02 cj 0800+618 08 05 18.2 61 44 23 0.981 0.539 0.029 0.25 -0.33 cj 0803+452 08 06 33.5 45 04 32 0.414 0.350 0.018 0.05 -0.09 cj 0804+499 08 08 39.7 49 50 36 1.222 1.599 0.113 0.25 0.15 cj 0805+410 08 08 56.7 40 52 44 0.743 0.694 0.036 0.57 -0.04 cj 0806+573 08 11 00.6 57 14 12 0.405 0.418 0.023 -0.04 0.02 cj 0812+367 08 15 25.9 36 35 15 0.980 0.414 0.022 -0.03 -0.48 cj 0814+425 08 18 16.0 42 22 45 1.891 0.595 0.036 0.20 -0.65 cj 0820+560 08 24 47.2 55 52 42 1.199 0.595 0.031 -0.05 -0.39 cj 0821+394 08 24 55.5 39 16 41 1.012 1.179 0.055 -0.24 0.09 cj 0821+621 08 25 38.6 61 57 28 0.615 0.294 0.017 -0.05 -0.41 d 0824+355 08 27 38.6 35 25 05 0.746 0.294 0.016 -0.12 -0.52 cj 0831+557 08 34 54.9 55 34 21 5.780 0.633 0.034 -0.23 -1.23 cj 0833+416 08 36 36.9 41 25 54 0.385 0.306 0.016 -0.08 -0.13 cj 0833+585 08 37 22.4 58 25 01 0.669 0.832 0.036 0.09 0.12 cj 0836+710 08 41 24.4 70 53 42 2.423 1.309 0.064 -0.44 -0.34 cj 0843+575 08 47 28.1 57 23 38 0.384 0.043 0.004 0.24 -1.22 cj 0847+379 08 50 24.7 37 47 09 0.382 0.287 0.016 -0.37 -0.16 cj 0850+581 08 54 42.0 57 57 29 1.187 0.299 0.017 -0.14 -0.77 cj 0859+470 09 03 04.0 46 51 04 1.285 0.823 0.044 -0.45 -0.25 cj 0859+681 09 03 53.2 67 57 22 0.751 0.272 0.016 0.19 -0.57 cj 0900+520 09 03 58.6 51 51 00 0.395 0.182 0.010 0.16 -0.43 cj? 0902+490 09 05 27.5 48 50 49 0.547 0.096 0.005 -0.12 -0.97 cj? 0917+449 09 20 58.5 44 41 53 1.033 1.704 0.101 0.22 0.28 cj 0917+624 09 21 36.2 62 15 52 1.322 0.813 0.040 0.06 -0.27 d 0923+392 09 27 03.0 39 02 20 7.480 5.726 0.388 0.80 -0.15 cj 0925+504 09 29 15.4 50 13 35 0.558 0.469 0.027 0.58 -0.10 cj 0927+352 09 30 55.3 35 03 37 0.383 0.294 0.018 -0.08 -0.15 cj 0929+533 09 32 41.2 53 06 33 0.384 0.141 0.008 -0.26 -0.56 cj 0930+493 09 34 15.8 49 08 21 0.574 0.161 0.009 -0.19 -0.71 cj 0942+468 09 45 42.1 46 36 50 0.354 0.192 0.010 0.19 -0.34 cj 0945+408 09 48 55.3 40 39 44 1.592 1.018 0.076 0.05 -0.25 cj 0945+664 09 49 12.2 66 14 59 1.407 0.270 0.016 -0.36 -0.92 mso^b 0949+354 09 52 32.0 35 12 52 0.403 0.216 0.013 0.12 -0.35 cj 0950+748 09 54 47.4 74 35 57 0.738 0.106 0.007 -0.37 -1.08 cj 0954+556 09 57 38.2 55 22 57 2.270 1.016 0.076 -0.22 -0.45 mso^b 0954+658 09 58 47.2 65 33 54 1.417 1.002 0.075 0.61 -0.19 cj 0955+476 09 58 19.7 47 25 07 0.834 1.389 0.059 0.15 0.28 cj 1003+830 10 10 15.8 82 50 14 0.716^a 0.422 0.034 -0.14^a -0.30 cj 1010+350 10 13 49.6 34 45 50 0.597 0.420 0.025 0.28 -0.20 cj 1014+615 10 17 25.9 61 16 27 0.631 0.302 0.016 0.44 -0.41 cj 1015+359 10 18 11.0 35 42 39 0.587 1.007 0.058 -0.34 0.30 cj 1020+400 10 23 11.6 39 48 15 0.785 0.571 0.029 -0.31 -0.18 cj

S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN) 7

Table 2. continued.

Name R.A. (J2000) Declination (J2000) S_{5.0} (Jy) S_{30} (Jy) ΔS_{30} (Jy) α^5_{1.4} α^{30}_5 Morph. (1) (2) (3) (4) (5) (6) (7) (8) (9) 1030+398 10 33 22.1 39 35 51 0.645 0.128 0.007 0.42 -0.90 cj 1030+415 10 33 03.7 41 16 06 0.485 0.617 0.036 -0.37 0.13 cj 1030+611 10 33 51.4 60 51 07 0.579 0.490 0.026 -0.22 -0.09 cj 1031+567 10 35 07.0 56 28 46 1.200 0.184 0.010 -0.30 -1.05 cso 1038+528 10 41 46.8 52 33 28 0.709 0.393 0.020 -0.00 -0.33 cj 1039+811 10 44 23.1 80 54 39 1.144^a 0.864 0.064 0.40^a -0.16 cj 1041+536 10 44 10.7 53 22 20 0.481 0.370 0.019 -0.10 -0.15 cj 1044+719 10 48 27.6 71 43 35 2.410 2.480 0.109 1.06 0.02 c 1053+704 10 56 53.6 70 11 45 0.675 1.073 0.060 0.08 0.26 cj 1053+815 10 58 11.5 81 14 32 0.770^a 0.643 0.047 -0.36^a -0.10 cj 1058+629 11 01 53.4 62 41 50 0.700 0.105 0.006 0.12 -1.06 cj 1058+726 11 01 48.8 72 25 37 0.953 0.493 0.030 -0.33 -0.37 cj 1101+384 11 04 27.3 38 12 31 0.722 0.393 0.020 -0.11 -0.34 cj 1105+437 11 08 23.5 43 30 53 0.375 0.382 0.023 0.27 0.01 cj 1106+380 11 09 28.9 37 44 30 0.867 0.240 0.013 -0.38 -0.72 cj 1107+607 11 10 13.1 60 28 42 0.404 0.053 0.004 0.12 -1.13 cj 1124+455 11 26 57.7 45 16 06 0.355 0.060 0.004 -0.26 -0.99 cj 1124+571 11 27 40.1 56 50 14 0.597 0.237 0.014 -0.20 -0.52 cj 1125+596 11 28 13.3 59 25 14 0.393 0.605 0.034 0.06 0.24 c 1128+385 11 30 53.3 38 15 18 0.746 1.094 0.055 -0.18 0.21 cj 1143+590 11 46 26.9 58 48 34 0.674 0.422 0.025 0.70 -0.26 cj 1144+352 11 47 22.1 35 01 07 0.663 0.182 0.010 -0.04 -0.72 cj 1144+402 11 46 58.3 39 58 34 0.739 1.129 0.047 -0.17 0.24 cj 1144+542 11 46 44.2 53 56 43 0.484 0.391 0.024 0.14 -0.12 cj 1146+596 11 48 50.4 59 24 56 0.627 0.362 0.022 0.32 -0.31 cj/cso 1150+812 11 53 12.5 80 58 29 1.181^a 1.522 0.091 -0.09^a 0.14 cj 1151+408 11 53 54.7 40 36 52 0.380 0.246 0.013 -0.48 -0.24 cj? 1155+486 11 58 26.8 48 25 16 0.445 0.214 0.013 -0.07 -0.41 cj 1205+544 12 08 27.5 54 13 19 0.397 0.091 0.006 -0.12 -0.82 d? 1206+415 12 09 22.8 41 19 41 0.515 0.197 0.010 0.37 -0.54 c 1213+350 12 15 55.6 34 48 15 1.152 0.540 0.030 -0.32 -0.42 cj 1216+487 12 19 06.4 48 29 56 0.680 0.670 0.040 -0.18 -0.01 cj 1218+444 12 21 27.0 44 11 29 0.478 0.206 0.013 -0.18 -0.47 cj 1221+809 12 23 40.5 80 40 04 0.518^a 0.392 0.028 0.43^a -0.16 cj 1223+395 12 25 50.6 39 14 22 0.438 0.154 0.009 -0.16 -0.58 cj 1226+373 12 28 47.4 37 06 12 0.953 0.168 0.009 1.26 -0.97 cj 1239+376 12 42 09.8 37 20 05 0.446 0.203 0.012 -0.16 -0.44 cj 1240+381 12 42 51.4 37 51 00 0.768 0.375 0.022 0.59 -0.40 cj 1246+586 12 48 18.8 58 20 28 0.414 0.123 0.008 0.43 -0.68 cj 1250+532 12 53 11.9 53 01 11 0.396 0.380 0.023 -0.24 -0.02 cj 1254+571 12 56 14.2 56 52 25 0.419 0.129 0.009 0.29 -0.66 cj? 1258+507 13 00 41.2 50 29 36 0.391 0.280 0.015 -0.23 -0.19 cj 1300+580 13 02 52.5 57 48 37 0.758 0.759 0.047 0.72 0.00 cj 1305+804 13 06 05.7 80 08 20 0.375^a 0.108 0.012 -0.47^a -0.69 cj 1306+360 13 08 23.7 35 46 37 0.437 0.510 0.029 0.54 0.09 cj 1307+562 13 09 09.8 55 57 38 0.416 0.279 0.018 0.27 -0.22 cj 1308+471 13 10 53.6 46 53 52 0.393 0.281 0.017 1.08 -0.19 cj? 1309+555 13 11 03.2 55 13 54 0.677 0.278 0.017 0.91 -0.50 cj 1312+533 13 14 43.8 53 06 27 0.433 0.066 0.004 0.49 -1.05 cj 1321+410 13 24 12.1 40 48 11 0.413 0.057 0.004 0.11 -1.11 d 1322+835 13 21 45.6 83 16 13 0.506^a 0.194 0.015 0.23^a -0.54 cj 1323+800 13 23 51.6 79 42 51 0.458^a 0.307 0.019 0.22^a -0.22 cj 1325+436 13 27 21.0 43 26 27 0.533 0.194 0.011 -0.22 -0.56 cj 1333+459 13 35 22.0 45 42 38 0.598 0.230 0.013 0.51 -0.53 cj? 1333+589 13 35 25.9 58 44 00 0.820 0.200 0.011 -0.07 -0.79 d 1335+552 13 37 49.6 55 01 02 0.811 0.378 0.023 0.10 -0.43 cj 1337+637 13 39 23.8 63 28 58 0.431 0.080 0.005 -0.12 -0.94 cj 1342+663 13 44 08.7 66 06 11 0.510 0.300 0.017 -0.43 -0.30 cj 1347+539 13 49 34.7 53 41 17 0.635 0.438 0.024 -0.46 -0.21 cj 1355+441 13 57 40.7 43 53 59 0.464 0.101 0.007 -0.33 -0.85 cj

8 S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN)

Table 2. continued.

Name R.A. (J2000) Declination (J2000) S_{5.0} (Jy) S_{30} (Jy) ΔS_{30} (Jy) α^5_{1.4} α^{30}_5 Morph. (1) (2) (3) (4) (5) (6) (7) (8) (9) 1356+478 13 58 40.7 47 37 58 0.428 0.070 0.006 -0.26 -1.01 d/cso? 1357+769 13 57 55.4 76 43 21 0.844^a 0.698 0.043 0.62^a -0.11 cj 1413+373 14 15 28.5 37 06 21 0.383 0.060 0.004 0.04 -1.03 cj 1415+463 14 17 08.2 46 07 05 0.904 0.489 0.026 -0.09 -0.34 cj 1417+385 14 19 46.6 38 21 48 0.871 0.543 0.032 0.16 -0.26 cj 1418+546 14 19 46.6 54 23 14 1.707 0.781 0.033 0.07 -0.44 cj 1421+482 14 23 06.2 48 02 10 0.536 0.249 0.014 0.31 -0.43 cj 1424+366 14 26 37.1 36 25 09 0.429 0.278 0.015 0.62 -0.24 cj 1427+543 14 29 21.9 54 06 11 0.718 0.178 0.009 -0.18 -0.78 cj 1432+422 14 34 05.7 42 03 16 0.353 0.109 0.007 0.19 -0.66 cj 1435+638 14 36 45.8 63 36 37 0.795 0.541 0.032 -0.44 -0.21 cj 1438+385 14 40 22.3 38 20 13 0.944 0.321 0.018 -0.06 -0.60 cj 1442+637 14 43 58.6 63 32 26 0.456 0.088 0.006 -0.32 -0.92 cj 1448+762 14 48 28.8 76 01 11 0.683^a 0.501 0.028 0.33^a -0.17 cj 1456+375 14 58 44.8 37 20 21 0.591 0.151 0.008 0.45 -0.76 cj 1459+480 15 00 48.7 47 51 15 0.489 0.282 0.016 0.16 -0.31 cj 1504+377 15 06 09.5 37 30 51 1.003 0.555 0.034 -0.13 -0.33 cj 1505+428 15 06 53.0 42 39 23 0.404 0.547 0.030 -0.06 0.17 cj 1526+670 15 26 42.9 66 50 54 0.417 0.078 0.005 -0.02 -0.94 cj 1531+722 15 31 33.6 72 06 41 0.452 0.161 0.009 -0.30 -0.58 cj 1534+501 15 35 52.0 49 57 39 0.359 0.169 0.010 0.35 -0.42 c 1543+480 15 45 08.5 47 51 54 0.441 0.078 0.006 -0.32 -0.97 d/cso 1543+517 15 45 02.8 51 35 00 0.544 0.093 0.005 0.09 -0.99 cj 1545+497 15 47 21.1 49 37 05 0.549 0.163 0.010 -0.42 -0.68 c 1547+507 15 49 17.5 50 38 05 0.724 0.738 0.039 0.06 0.01 cj 1550+582 15 51 58.2 58 06 44 0.367 0.254 0.014 0.38 -0.21 cj 1619+491 16 20 31.2 49 01 53 0.469 0.214 0.012 0.00 -0.44 cj 1622+665 16 23 04.5 66 24 01 0.520 0.122 0.007 0.74 -0.81 cj? 1623+578 16 24 24.8 57 41 16 0.590 0.424 0.025 0.13 -0.18 cj 1624+416 16 25 57.7 41 34 40 1.362 0.521 0.030 -0.17 -0.54 cj 1629+495 16 31 16.5 49 27 39 0.394 0.458 0.026 0.16 0.08 cj 1633+382 16 35 15.5 38 08 04 3.189 2.976 0.173 0.41 -0.04 cj 1636+473 16 37 45.1 47 17 33 1.330 1.031 0.053 0.27 -0.14 cj 1637+574 16 38 13.5 57 20 23 1.807 1.317 0.071 0.30 -0.18 c 1638+398 16 40 29.6 39 46 46 1.285 0.612 0.025 0.53 -0.41 cj? 1638+540 16 39 39.8 53 57 47 0.369 0.172 0.011 0.14 -0.43 cj 1641+399 16 42 58.8 39 48 36 8.363 4.929 0.287 0.05 -0.30 cj 1642+690 16 42 07.8 68 56 39 1.516 2.746 0.128 0.00 0.33 d/cj? 1645+410 16 46 56.9 40 59 17 0.388 0.185 0.009 0.16 -0.41 cj 1645+635 16 45 58.6 63 30 10 0.444 0.410 0.023 0.31 -0.04 cj 1652+398 16 53 52.2 39 45 36 1.371 1.219 0.071 -0.04 -0.07 cj 1656+477 16 58 02.8 47 37 49 1.420 0.582 0.031 0.47 -0.50 cj 1656+482 16 57 46.9 48 08 33 0.847 0.697 0.045 -0.12 -0.11 cj 1656+571 16 57 20.7 57 05 53 0.844 0.487 0.027 0.04 -0.31 cj 1700+685 17 00 09.3 68 30 06 0.435 0.338 0.017 0.29 -0.14 cj 1716+686 17 16 13.9 68 36 38 0.988 0.536 0.025 0.69 -0.34 cj 1719+357 17 21 09.5 35 42 16 0.874 0.210 0.011 0.03 -0.80 cj 1722+401 17 24 05.4 40 04 36 0.532 0.619 0.037 -0.03 0.08 cj 1726+455 17 27 27.7 45 30 39 1.066 0.715 0.043 0.72 -0.22 cj 1732+389 17 34 20.6 38 57 51 0.561 1.105 0.075 -0.26 0.38 cj 1734+508 17 35 49.0 50 49 11 0.798 0.420 0.028 0.06 -0.36 d 1738+476 17 39 57.1 47 37 58 0.789 0.621 0.038 -0.04 -0.13 cj 1738+499 17 39 27.4 49 55 03 0.478 0.427 0.026 -0.13 -0.06 cj 1739+522 17 40 37.0 52 11 43 1.133 0.826 0.045 -0.44 -0.18 cj 1744+557 17 44 56.6 55 42 17 0.599 0.301 0.017 -0.17 -0.38 cj 1745+624 17 46 14.0 62 26 54 0.580 0.205 0.011 -0.22 -0.58 cj 1746+470 17 47 26.6 46 58 50 0.634 0.194 0.010 0.31 -0.66 cj? 1747+433 17 49 00.4 43 21 51 0.367 0.423 0.026 0.06 0.08 cj 1749+701 17 48 32.8 70 05 50 0.728 0.430 0.023 -0.46 -0.29 cj 1751+441 17 53 22.6 44 09 45 0.998 0.551 0.029 0.19 -0.33 cj

S. R. Lowe et al.: 30 GHz flux density measurements of the Caltech-Jodrell flat-spectrum sources with OCRA-p (RN) 9

Table 2. continued.

Name R.A. (J2000) Declination (J2000) S_{5.0} (Jy) S_{30} (Jy) ΔS_{30} (Jy) α^5_{1.4} α^{30}_5 Morph. (1) (2) (3) (4) (5) (6) (7) (8) (9) 1755+578 17 56 03.6 57 48 47 0.455 0.062 0.004 -0.37 -1.11 cj/cso? 1758+388 18 00 24.8 38 48 30 0.722 0.876 0.037 0.27 0.11 cj 1800+440 18 01 32.3 44 04 21 1.148 0.736 0.042 0.21 -0.25 cj 1803+784 18 00 45.7 78 28 04 2.633^a 1.211 0.063 0.27^a -0.43 cj 1807+698 18 06 50.7 69 49 28 2.189 1.493 0.080 -0.03 -0.21 cj 1809+568 18 10 03.3 56 49 22 0.576 0.269 0.013 0.01 -0.42 cj 1812+412 18 14 22.7 41 13 05 0.534 0.266 0.018 -0.15 -0.39 cj 1818+356 18 20 42.1 35 40 39 0.573 0.195 0.012 -0.43 -0.60 cj 1823+568 18 24 07.1 56 51 01 1.135 1.642 0.100 -0.21 0.21 cj 1826+796 18 23 14.1 79 38 49 0.577^a 0.169 0.008 0.41^a -0.69 cso 1828+399 18 29 56.5 39 57 34 0.353 0.266 0.014 0.80 -0.16 cj? 1834+612 18 35 19.7 61 19 40 0.590 0.202 0.011 0.22 -0.60 cj 1839+389 18 40 57.2 39 00 45 0.476 0.171 0.010 0.26 -0.57 cj? 1842+681 18 42 33.6 68 09 25 0.936 0.986 0.055 0.34 0.03 cj 1843+356 18 45 35.1 35 41 16 0.794 0.111 0.007 -0.21 -1.10 cj 1849+670 18 49 16.1 67 05 41 0.992 0.575 0.029 0.08 -0.30 cj 1850+402 18 52 30.4 40 19 06 0.535 0.382 0.025 -0.02 -0.19 cj 1851+488 18 52 28.5 48 55 47 0.351 0.196 0.011 0.15 -0.33 c 1856+737 18 54 57.3 73 51 19 0.546 0.530 0.027 -0.02 -0.02 cj 1908+484 19 09 46.6 48 34 31 0.423 0.151 0.008 -0.24 -0.57 c 1910+375 19 12 25.1 37 40 36 0.402 0.282 0.016 -0.18 -0.20 cj 1924+507 19 26 06.3 50 52 57 0.354 0.213 0.011 -0.48 -0.28 cj 1926+611 19 27 30.4 61 17 32 0.618 0.837 0.044 -0.06 0.17 cj 1928+738 19 27 48.5 73 58 01 3.561 2.961 0.159 -0.07 -0.10 cj 1936+714 19 36 03.6 71 31 31 0.391 0.235 0.012 -0.36 -0.28 cj? 1943+546 19 44 31.5 54 48 07 0.938 0.225 0.011 -0.44 -0.80 d 1946+708 19 45 53.5 70 55 48 0.645 0.217 0.011 -0.28 -0.61 cso 1950+573 19 51 07.0 57 27 17 0.476 0.226 0.011 -0.14 -0.42 cj 1954+513 19 55 42.7 51 31 48 1.610 0.891 0.047 -0.01 -0.33 cj 2005+642 20 06 17.7 64 24 45 0.739 0.234 0.012 1.14 -0.64 cj 2007+659 20 07 28.8 66 07 22 0.756 0.463 0.024 -0.24 -0.27 cj 2007+777 20 05 31.0 77 52 43 1.279^a 1.117 0.046 0.73^a -0.08 cj 2010+723 20 09 52.3 72 29 19 0.910 0.916 0.045 -0.18 0.00 cj 2017+745 20 17 13.1 74 40 48 0.500 0.309 0.016 0.05 -0.27 cj 2021+614 20 22 06.7 61 36 58 2.743 1.433 0.060 0.20 -0.36 d? 2023+760 20 22 35.6 76 11 26 0.426^a 0.479 0.025 -0.13^a 0.07 cj 2054+611 20 55 38.8 61 22 00 0.414 0.262 0.014 -0.02 -0.26 cj 2116+818 21 14 01.2 82 04 48 0.376^a 0.224 0.012 -0.22^a -0.29 cj 2136+824 21 33 34.1 82 39 06 0.509^a 0.161 0.009 -0.48^a -0.64 cj 2138+389 21 40 16.9 39 11 44 0.502 0.226 0.012 -0.22 -0.45 cj 2200+420 22 02 43.3 42 16 39 3.593 5.570 0.301 -0.21 0.24 cj 2214+350 22 16 20.0 35 18 14 0.477 0.319 0.018 -0.06 -0.22 cj? 2229+695 22 30 36.5 69 46 28 1.365 0.591 0.031 0.80 -0.47 cj 2235+731 22 36 38.6 73 22 52 0.424 0.165 0.009 0.27 -0.53 cj 2238+410 22 41 07.2 41 20 11 0.677 0.226 0.012 0.12 -0.61 cj 2253+417 22 55 36.7 42 02 52 1.120 0.577 0.031 -0.18 -0.37 cj 2255+416 22 57 22.1 41 54 16 1.111 0.216 0.012 -0.41 -0.91 cj 2259+371 23 01 27.7 37 26 49 0.406 0.513 0.026 -0.30 0.13 cj 2309+454 23 11 47.4 45 43 56 0.597 0.401 0.020 0.53 -0.22 cj 2310+385 23 12 58.8 38 47 42 0.484 0.166 0.009 -0.28 -0.60 d 2319+444 23 22 20.4 44 45 42 0.366 0.282 0.015 0.14 -0.15 cj 2346+385 23 49 20.8 38 49 17 0.640 0.535 0.029 0.54 -0.10 cj 2351+456 23 54 21.7 45 53 04 1.145 1.223 0.062 -0.37 0.04 cj 2352+495 23 55 09.5 49 50 08 1.552 0.328 0.020 -0.32 -0.87 cso 2353+816 23 56 22.8 81 52 52 0.476^a 0.526 0.025 0.13^a 0.06 cj 2356+385 23 59 33.2 38 50 42 0.449 0.188 0.010 -0.28 -0.49 cj? 2356+390 23 58 59.9 39 22 28 0.371 0.414 0.020 -0.11 0.06 cj

a These spectral indicies are calculated between 2.727 GHz and 5 GHz using data from Kuehr et al. (1981).^b These identifications were made by Rossetti et al. (2005).