arXiv:0909.2440v2 [cond-mat.other] 21 Oct 2009

Combining high pressure and coherent diffraction: a first feasibility test

D. Le Bolloc’h,^1 J.P. Itié,^2 A. Polian,^3 and S. Ravy^2 1Laboratoire de Physique des Solides (CNRS-UMR 8502), Bât. 510, Université Paris-sud, 91405 Orsay cedex, France 2Synchrotron SOLEIL - L’Orme des Merisiers Saint-Aubin - BP 48 91192 GIF-sur-YVETTE, France 3IMPMC, Campus Boucicaut 140, rue de Lourmel, 75015 Paris, France

We present a first experiment combining high pression and coherent X-ray diffraction. By using a dedicated diamond anvil cell, we show that the degree of coherence of the X-ray beam is preserved when the X-ray beam passes through the diamond cell. This observation opens the possibility of studying the dynamics of slow fluctuations under high pressure.

PACS numbers:

INTRODUCTION

Coherent diffraction techniques provide a new insight into a wide variety of phenomenon. In particular, disordered samples which are coherently illuminated give rise to speckle pattern and speckle fluctuations analysis gives access to the dynamic of fluctuations of matter.

In situ experiments using various external constraints as temperature, external current or magnetic field can be easily combined with coherent x-rays as far as the sample environment does not destroy the coherence properties of the beam. Up to now this has not been demonstrated for diamond anvil cell. In classical anvil cell, the x-ray beam goes through the diamonds or the gasket which may induce an irreparable loss of coherence.

We show in this paper that high pression and coherent diffraction can both be combined, going through the diamond anvils. We exclude the other geometry, through a Be gasket for example, because such materials with non perfect surfaces strongly affect the degree of coherence of the beam. This is not the case of the diamond anvils which are nearly perfect single crystals with a well polished surface. In that case, we show that the degree of coherence of the beam is almost not perturbated when the beam passes through the diamond cell. This setup opens the possibility to study time fluctuations under high pressure.

PROPAGATION PROPERTIES OF THE TRANSVERSE COHERENCE LENGTH

Thanks to third generation synchrotron radiation sources, it is possible to obtain X-ray beams with an excellent degree of coherence. This experimental fact may be surprising since synchrotron sources are only weakly coherent. In fact, this is possible thanks to the propagation properties of the transverse coherence length. The propagation properties of a partially coherent beam can be obtained from the mutual coherence function

γ(⃗r_1, ⃗r_2, z_0) = ⟨A(⃗r_1)A^∗(⃗r_2)⟩ , which characterizes the spatial coherence properties of the amplitude A(⃗r) of the field at a pair of points (⃗r_1, ⃗r_2), located in the plane perpendicular to the direction of propagation. If the beam profile at z_0 is assumed to be Gaussian, in the Schell approximation[1], an analytical expression of the transverse coherence length ξ(z) can be obtained:

ξ^2(z) = ξ^2_0 + ( zλ 2π )_2 ( ξ^2_0 + 2σ^2 σ^4 ) . This last equation gives the transverse coherence length ξ(z) of the beam at any distance z from the source as a function of the beam size σ and of the coherence properties of the source ξ_0. For example, in the case of a totally incoherent source ξ_0 = 0, the transverse coherence length ξ(z) will not be zero: ξ(z) ∝ zλ σ . (1)

As an example, if the source is totally incoherent and located at 40m from the sample position, we should obtain transverse coherence lengths up to ξ_v (z) ≈ 200μm (with λ = 1.5Å and σ_{rms} = 10μm). Unfortunatly, optical aberrations, mainly due to focussing mirrors, reduce considerably this value. In practice, secondary slits are located 10m upstream from the sample positon with 100- 250 μm apertures in order to clean the wavefront. We then obtained ξ_v (z) around 10μm at the sample position. We just need to reduce the beam size close to Φ = 10μm to obtain a degree of coherence β = ξ_v/σ which tends towards 1.

DIFFRACTION PATTERN OF A SQUARED SLIT FROM A PRATIALLY COHERENT X-RAY BEAM

The mutual coherence function can be used to reproduce the diffraction pattern of a squared slit as a function of the coherence properties of the x-ray beam. In the case of a totally coherent beam, we obtain the well-known

FIG. 1: a) Design of the diamond anvil cell. b) Theoretical cross-like diffraction profile of a rectangular slit for two values of the degree of coherence ξv (a=10μm). c) Contrast of fringes of the cross-like diffraction of a rectangular slit (Φ = 5μm), with and without the anvil cell along the optical path. The two white arrows indicate two slight deformations of the profile of fringe induced by the anvil cell.

cross-like intensity profile:

I(x) = I_0 sin^2 (^{πa}_{zλ} x) (^{πa}_{zλ} x)^2

, (2)

where a is the slit aperture. As ξ decreases, the contrast of fringes is getting more and more reduced as displayed in figure 1a). Provided that the slit blades are carefully polished[2], the measurement of the contrast of fringes gives a good estimation of the degree of coherence. In the following, we have measured how a coherent beam propagates through the anvil diamond cell from the contrast of fringes of a rectangular slits diffraction pattern.

Combining pressure and coherent diffraction

To combine high pressure and coherent diffraction will provide an unique way to measure fluctuations under high pressure. From an experimental point of view, the combination of both techniques is not obvious. A good compromise has to be found between the degree of coherence (which decreases with increasing photons energy), the absorption of the anvils, the opening of the cell and the maximum pressure expected. The geometry of the diamond anvil cell is displayed in figure 1b). We use 1.2 mm thick diamonds and 10 keV x-rays. Compared to 8 keV x-rays usually used in coherent diffraction experiments, the degree of coherence is reduced by 20% (see Eq.1) but the transmission is increased by a factor 3. The cell is designed to have an opening of 2×40^∘ with such diamonds. Diffraction patterns of rectangular slit has been recorded with and without the presence of the anvil cell at the sample position (see figure 1c). The secondary slits

FIG. 2: a)For larger pressure (P=8GPa), the cross-like intensity profile is more disturbed (Φ = 6.5μm). b) Diffraction patterns of the (200), (100) and (110) Bragg reflections in SrT iO3 at various pressure up to 8GPa. The speckle patterns were obtained with F5=100μm × 100μm and Φ = 10μm × 10μm. The profile of fringes of the (200) Bragg peak at P=0.2GPa is also displayed. At P=6 Gpa, the (200) bragg reflection is cut by the anvil cell aperture (see arrow) at 2θ = 38^o.

were closed at 100μm and the slit located at the sample position at ϕ = 5μm. The 2D images have been recorded with a CCD camera (13μm pixels size) located at 2m from the sample position. The degree of coherence without diamond cell has been estimated from the contrast of fringes around β = 70%. The main result of this paper is to establish that when using such anvil cell, with a residual pressure of 0.2GPa, similar contrast of fringes is observed. The coherence properties of the beam are not altered by our anvil cell. This opens the possibility to do coherent diffraction experiment under high pressure. In fact, the contrast of fringes is slightly stronger with the anvil cell (see figure 1c). This is probably due to the fact that the anvil cell absorbs X-rays scattered by air or kapton foils upstream. Note also that the diffraction pattern is locally perturbed at two positions along the cross-like profile (see arrows in figure 1c).

A similar experiment has been performed at higher pressure, up to 8GPa. Unfortunatly, the figure 2a has not been exactly obtained in the same configuration. The secondary slits were opened at 200μm and the last slits at Φ = 6.5μm. The contrast of fringes is thus smaller. Nevertheless, it seems that for larger pressure, the contrast decreases. We can not exclude that the degree of coherence decreases for higher pressure due to larger de-

Combining high pressure and coherent diffraction 3

formations of the diamond cell.

As an example of coherent diffraction at wide angles, we choose the SrT iO_3 system which has been recently study by this method close to its displacive transition[3]. We have measured different fundamental Bragg peaks, in the scattering plane (the (100) and (200) reflections) and out-of-plane (the (110) reflection), at several pressures (see figure 2b). Reflections up to the (200) are reachable thanks to the large angular aperture of our diamond cell. We obtained speckles with a good contrast up to 8GPa. The micrometer-size SrT iO_3 sample was not a perfect monocrystal. Speckles are probably due to interferences between misoriented domains. In addition, the crystal broke up into several pieces under higher pressure.

[1] M. Born and E. Wolf, Principles of optics, Pergamon Press, Oxford; L. Mandel and E. Wolf, Optical coherence and quantum optics, Cambridge University Press (1995).

[2] D. Le Bolloc’h, et al., J. Synchrotron Rad. 9, 258 (2002). [3] S. Ravy,D. Le Bolloc’h, R. Currat,A. Fluerasu,C. Mocuta and B. Dkhil, Phys. Rev. Lett. 98 105501 (2007).