arXiv:0912.0621v1 [astro-ph.CO] 3 Dec 2009

Mon. Not. R. Astron. Soc. 000, 000–000 (0000) Printed 6 May 2019 (MN L^ATEX style file v2.2)

High-frequency radio polarization measurements of WMAP point sources

N. Jackson^1, I.W.A. Browne^1, R.A. Battye^1, D. Gabuzda^2, and A.C. Taylor^3

1Jodrell Bank Centre for Astrophysics, University of Manchester, Turing Building, Oxford Road, Manchester M13 9PL 2Physics Department, University College Cork, Ireland 3Oxford Astrophysics, University of Oxford, Denys Wilkinson Building, Keble Road, Oxford, OX1 3RH, UK

6 May 2019

ABSTRACT

We present polarization measurements at 8.4, 22, and 43 GHz made with the VLA of a complete sample of extragalactic sources stronger than 1 Jy in the 5-year WMAP catalogue and with declinations north of −34^∘. The observations were motivated by the need to know the polarization properties of radio sources at frequencies of tens of GHz in order to subtract polarized foregrounds for future sensitive Cosmic Microwave Background (CMB) experiments. The total intensity and polarization measurements are generally consistent with comparable VLA calibration measurements for less-variable sources, and within a similar range to WMAP fluxes for unresolved sources. A further paper will present correlations between measured parameters and derive implications for CMB measurements.

Key words: radio:polarization

1 INTRODUCTION

Radio source samples, selected at high frequency and with flux densities of the order of 1 Jy, mostly contain compact flat spectrum objects associated with the nuclei of active galaxies which have relativistic outflows pointing close to the direction of the observer (e.g. Blandford & Rees 1978; Scheuer & Readhead 1979; Orr & Browne 1982). This emission consists of a number of synchrotron components, each with a steep optically thin synchrotron spectrum at high frequencies and a self-absorbed spectrum at lower frequencies; the combination of many such components with different cutoff frequencies produces the observed “flat” radio spectrum. These components are frequently linearly polarized, and in principle useful information on jet physics can be obtained from the distribution of polarization in frequency and space. Although high frequency-selected samples are dominated by flat spectrum objects the samples do contain a minority of intrinsically more powerful sources in which the extended, steep-spectrum synchrotron emission dominates rather than the emission from a beamed core. Such sources also display linearly polarized emission, often at a higher level than the flat spectrum sources.

In recent years there has been particular interest in high-frequency properties of radio sources because discrete radio sources act as a confusing foreground for measurements of the Cosmic Microwave Background (e.g. Tegmark & Efstathiou 1996). Such sources contribute most to the power spectrum on small angular scales (high ℓ), and efforts have been made to subtract their effects in several different ways. For total intensity, high frequency observations of sources selected from lower frequency surveys have been used. For example, the Very Small Array CMB interferometer, working at 31 GHz, used 15-GHz source-finding observations with the Ryle Telescope followed by monitoring of discrete sources with dedicated long baselines (Dickinson et al. 2004) and/or single dish observations made with

© 0000 RAS

2 N. Jackson et al.

the Torun 32 m (Gawronski et al. 2009), while for the Cosmic Background Imager experiment high frequency observations were made with the OVRO 42 m and GBT of sources selected at 1.4 GHz (Mason et al. 2003; Mason et al. 2009). Alternatively, population models based on extrapolations from lower frequency catalogues can be used statistically to ameliorate the effects of the extragalactic source foreground.

Although large-scale blind surveys at high frequencies are difficult to do, because of the small field of view at high frequencies, there are a number of both blind and pointed surveys in existence. The southern hemisphere has been completely surveyed by the AT20G survey (Ricci et al. 2004), which has been conducted with the Australia Telescope Compact Array (ATCA) at 18 GHz down to a limiting flux density of 50 mJy. A detailed study of brighter sources in this survey has been presented by Massardi et al. (2008). The whole sky has been covered to a brighter limiting flux density of about 1Jy by WMAP at a number of frequencies ≥20 GHz (Wright et al. 2009), and smaller areas of the northern sky have been covered to greater depth by surveys such as the 15-GHz 9C survey (Waldram et al. 2003). These surveys generally find that sources that are bright at high frequencies have complex spectra. About 30% are significantly inverted (Ricci et al. 2004), and the mean spectral index around 20–40 GHz tends to be around zero, generally steepening at higher frequencies (Ricci et al. 2006; Massardi et al. 2008; Vol’Vach et al. 2008). There is some evidence that the spectra of most sources turn over by 95 GHz (Sadler et al. 2008) but in general extrapolation to both higher frequencies and to lower flux density levels is needed in order to realistically simulate the CMB discrete foregrounds (e.g. Waldram et al. 2007). Importantly, there is convincing evidence that the mix of flat and steep spectrum sources changes with flux density. This is a prediction of beaming models (e.g. Orr & Browne 1982; Wall & Jackson 1997). There is also direct observational evidence provided by Gawronski et al. (2009) that the proportion of steep-spectrum sources with extended radio emission increases from ≤20% in a WMAP 22-GHz sample to ≥50% in Ryle-selected 15-GHz sample which has a flux density limit about two orders of magnitude weaker than that of the WMAP sample. Thus care must be taken when extrapolating to both higher frequencies and lower flux densities. The sensitivity of instruments such as Planck require this to be done as accurately as possible, and hence it is important to base the models on as firm an observational footing as possible.

The situation with polarized foregrounds is less developed but it is becoming urgent to solve because inflation models make different predictions for the strength of B-modes in the CMB polarization distribution. A heroic effort is going into experiments to detect B-modes. These include Planck and ground-based projects like QUIET (Samtleben 2008) and the balloon-borne experiment SPIDER (Montroy et al. 2006). All CMB observations are technically challenging because they rely on extreme stability of the equipment and on meticulous subtraction of foregrounds to get at the true distribution of the CMB fluctuations. The detection of the B-mode signal will be particularly difficult (though just how difficult depends on its strength which varies over a wide range depending on the inflation model). For scalar-to-tensor ratio r=0.01, the peak signal (at around 1^∘ scales) is ∼30nK. B-mode experiments operate at high frequencies (e.g. QUIET: 44 and 90GHz; Spider: 90, 145 and 220 GHz; PLANCK 30,70, 100, 143, 217 and 353 GHz). Hence observations at the highest frequencies possible are desirable. Estimates of synchrotron source total intensity contamination have been made by extrapolating from observations made at 1.4 and 5 GHz (e.g. Tucci et al. 2004). The current best-guess models are presented by Toffolatti et al. (1998, 2005). However, additional assumptions need to be made if the polarized foreground is to be characterized; one needs to know about the high frequency polarization properties of sources. Ideally one would like direct observations of polarized source counts but this is impractical. An alternative is to use high frequency total intensity source counts and a knowledge of how the percentage polarizations of sources change with both frequency and flux density to predict polarized source counts.

The work reported in this paper is the first phase in a programme aimed at improving knowledge about the polarization properties of radio sources at high radio frequencies. We begin with bright sources from the WMAP sample of Wright et al. (2009) which have S_{22GHz} >1 Jy. In this work, all but four of the sample of 203 WMAP sources with flux density of ≥1 Jy at 22 GHz and with declination δ > −34 have been imaged with the VLA in total intensity and polarization. The second phase of our programme will be to measure the polarization properties

Polarization of WMAP point sources 3

of a high frequency-selected sample of much weaker sources designed to look for any dependence of polarization properties on flux density. Given that Gawronski et al. (2009) find that the population mix changes with flux density there is every reason to expect that average polarization properties also change.

2 OBSERVATIONS AND DATA REDUCTION

Observations were conducted using the VLA in D-configuration between 01.40 and 19.30 UT on 2008 August 1. During this period 16 antennas were equipped with EVLA receivers while the remaining 11 had original VLA receivers. Each source was normally observed at three frequencies: two 50-MHz bands centred on 8.4351 and 8.4851 GHz (X-band), two 50-MHz bands centred on 22.4351 and 22.4851 GHz (K-band), and two 50-MHz bands centred on 43.3149 and 43.3649 MHz (Q-band). Pointing calibration was carried out approximately every 15-20 minutes. The available time allowed observations to be made of all the sources at 22 GHz and 43 GHz, and approximately two-thirds of the sources at 8 GHz. Four sources (WMAP 0823+224, WMAP 0824+392, WMAP 1014+231 and WMAP 1840+797) were missed during the observations, leaving a total of 199 sources out of 203 with attempted measurements. The source 3C48 was observed in order to provide an additional flux and polarization calibrator; the primary flux and polarization calibrator, 3C286 (WMAP 1331+305) was already part of the sample. Additionally, three much weaker sources from the 9C survey were also observed as a pilot for a future observing programme aimed at much weaker sources.

The nominal time on each source was 37 seconds at 8 GHz, 30 seconds at 22 GHz and 80 seconds at 43 GHz, giving a theoretical rms of 0.2, 0.5 and 0.7 mJy/beam, respectively, for natural weighting. However, the rms noise in most images is typically greater than this, being between 1 mJy/beam and 2 mJy/beam in the majority of images. This is partly due to the use of uniform weighting during the imaging process, which increases the noise level typically by factors between 1.2 and 1.5. However, in particular, 8-GHz observations were affected by a combination of missing antennas and slightly longer than predicted slew and setup times on many sources. A sampling time of 3 seconds per integration was used, the minimum allowed by the observing system.

All data analysis and processing was carried out in the aips package, distributed by the US National Radio Astronomy Observatory. Data were examined and flagged manually. The 22-GHz data were relatively clean, but extensive flagging of bad telescopes was performed source by source on both 8-GHz and 43-GHz data, resulting in the removal of up to half of the data on any given source. The major problems were loss of correlation on some telescopes during setup at the beginning of a scan, together with intermittent bad data on many individual telescopes.

Overall amplitude calibration was performed using observations of the source 3C286 at each frequency and normalising to the flux scale of Baars et al. (1977). Amplitude and phase solutions were made using the sources stronger than a limiting flux density; the process was iterated, adjusting this limiting flux, until the amplitude and phase solutions appeared to vary in a coherent manner. Amplitude solutions were smoothed using an averaging time of 1 hour for 43 GHz and 0.1 hours for the other frequencies. In the case of the 8-GHz observations, a further calibration was made, again using a standard model for 3C286, for baseline-dependent offsets. This was necessary because of the mixture of receivers in the array, approximately equally distributed between old (VLA) and new (EVLA) receivers.

Polarization calibration was then carried out. Telescope polarization offsets were calibrated by use of the source 3C84, which was assumed to have zero polarization. This assumption is correct for the level of accuracy required here: Taylor et al. (2006) report levels of <0.1% polarization in the core of the source at frequencies less than 22 GHz, with approximately 0.2% at 22GHz, and a somewhat higher level (0.8-7.5%) in the weak mas-scale jet component. The overall level of polarization in 3C84 is likely to be about 0.1%. 3C84 was not observed at 8 GHz. In this case the source 0125−001, a bright point source for which no significant polarization was detected in either 22-GHz or 43-GHz observations, was used instead. The polarization position angle was calibrated by use of the 3C286 data, applying corrections to the R−L phase difference to rotate the 3C286 polarization position angle to

Figure 1. Estimates of the Stokes parameters Q and U for the mapped sources, in mJy, for the two methods described in the text (fitting to the images and to the (u, v) data). In each case, Q, in mJy, is the abscissa and U, in mJy, is the ordinate, and lines on the plot join the (Q, U) coordinates of the first measurement to those of the second. Note that for most sources the methods agree well and the lines are relatively short. In cases of disagreement we provide a note in Table 2 explaining the choice of polarized flux densities used in the data tables.

33^∘. The baseline-to-baseline scatter in this quantity was 0.6, 3.3 and 8.5 degrees for 8 GHz, 22 GHz and 43 GHz respectively.

Imaging was performed using the AIPS task IMAGR with uniform weighting, on a default 128×128 grid and cellsizes of 1.^{′′}8, 0.^{′′}7 and 0.^{′′}35 for 8 GHz, 22 GHz and 43 GHz respectively. For strong sources (roughly speaking, those containing sufficient flux density to have been used as phase calibrators), one iteration of phase-only self-calibration and one iteration of amplitude self-calibration was applied. Final total intensity images were produced using 1000 clean iterations (Högbom 1974); images in Stokes Q and U were produced using a limited number (40) of iterations to avoid reduction in the signal due to clean bias (e.g. Condon et al. 1998).

Estimation of the Stokes I, Q and U flux densities was performed in two ways. The first method consisted of fitting to the calibrated (u, v) data, constraining the fit by fixing the position to the peak of the I map, constraining the intrinsic size of the peak component to be < 1^{′′}, but allowing the Q and U flux density to vary. Constraints are necessary to avoid instability in the fits due to noise in the polarization data. The alternative method consisted of finding, and fitting to, the highest absolute value in the Q and U images, within a square of side 10 pixels. Neither method is ideal. Fitting to the (u, v) data has the advantage of independence from effects due to deconvolution, notably the effects of clean bias. On the other hand, stabilising the fit requires fixing the peak of the Stokes Q and U to the peak of the I data, and this may not be appropriate for sources with extended polarized structure. Fig. 1 shows a comparison of the two methods, and demonstrates that for the majority of sources the two methods agree well. Approximately 10% of sources show significant disagreement, mostly those with low polarized flux densities. In Table 2, where the data are presented, detailed comments are given in cases where the two methods disagree. Errors given in Table 2 are a quadrature combination of the random error, as output by aips, and the systematic calibration error, assumed to be 5% for 43 GHz and 22 GHz and 2% at 8.4 GHz.

Because the total polarization is a quadratic sum of Q and U, it is positive-biased; values of polarized flux density of three times the rms noise cannot therefore be regarded as significant detections. Many studies of this

© 0000 RAS, MNRAS 000, 000–000

Polarization of WMAP point sources 5

Frequency 1.4 8.4 22 43 (GHz) 1.4-8.4 8.4-22 22-43

Polarization (%) 2.2±0.2 3.1±0.2 2.7±0.2 3.1±0.2 (1.6) (2.6) (2.2) (2.6) Intensity spectral index 0.01±0.04 −0.20±0.05 −0.49±0.04 (0.04) (−0.15) (−0.37) Polarization spectral index 0.35±0.07 0.01±0.10 −0.09±0.06 (0.28) (−0.15) (−0.14)

Table 1. Average intensity and polarization quantities for the sample, counting polarization limits as zero. 1.4-GHz observations are from NVSS, 8.4-GHz observations from CLASS and this work, and the remainder from this work. Median values are given in brackets. Spectral indices are defined as S_ν = ν^α.

effect have been made. For example, Simmons & Stewart (1985) give a relation of estimated signal-to-noise, p_o, and observed signal-to-noise p, in polarization for four different indicators. These all converge towards equality for p > 4 as p_o = (p^2 − 1)^{1/2}, and diverge strongly for p < 2, reaching values of 1 < p < 1.5 for p_o = 0. The issue in these observations is complicated by the different values of rms noise in different images. Inspection of the images suggests that polarized flux densities of 10mJy are likely to be significant at all frequencies in both methods.

Fig. 2 shows the complete total intensity and Stokes maps, together with the spectrum in total intensity and polarization, for the first source in order of right ascension, WMAP 0006−063. The other images can be found in the online material associated with this article.

3 COMPARISON WITH OTHER OBSERVATIONS

3.1 Consistency of polarization with the VLA calibrator programme

A few polarization calibrators are observed regularly by the VLA (Taylor & Myers 2000)^1. We compare the total intensity and polarization measurements of these sources with our measurements for 22 GHz and 43 GHz in Fig. 3. Sources included in this comparison are those which were observed by the VLA in the D-configuration of 2008, interpolated if necessary to the date of our observation. Those sources which appear non-variable to 15% are plotted as separate symbols; it appears that our measurements compare well with the VLA calibration programme.

3.2 Comparison with WMAP fluxes

Ricci et al. (2006) comment that their AT20G flux densities from ATCA data on southern sources are systematically different from those of WMAP, in that the WMAP 30 GHz observations of flat spectrum sources seem to be low by a factor of about 1.2. Differences in this sense cannot be the result of resolution effects, since the larger beam of WMAP should result in a higher detected flux density in any resolved sources. We can investigate this with the northern-hemisphere 22-GHz data presented here, and the results are shown in Fig. 4.

It is clear that there is a population of resolved sources, for which the WMAP flux densities at 22 and 43 GHz are higher than those of this work. A population of sources unresolved with either set of observations cluster around the line of equal flux density, although there will be some scatter induced by variability of sources between the two epochs of observation. At the 20% level, there is no evidence for the flux scales being significantly different at 22 GHz. There is marginal evidence at 43 GHz for slightly lower flux densities in these observations than in the WMAP observations, which may be an indication that even some relatively compact sources are beginning to be resolved at this frequency. It may also be a consequence of variability bias, in which some sources which are on average just below the 1-Jy limit, happened to be in a relatively high state when observed with WMAP. More

1 Online data from the VLA polarization calibration programme is available on http://www.vla.nrao.edu/astro/calib/polar/.

6 N. Jackson et al.

Figure 2. Full data for the first WMAP source, 0006−063. The spectrum (top) is given in units of log (flux density/mJy) against log (frequency/GHz); error bars are shown but are smaller than the plot symbols in many cases. Filled circles are total intensity points, and open circles are polarized flux density points measured by fitting to the (u, v) data. Stars are polarized flux density points measured by maxima from the Q, U maps. The maps of the source (bottom) include, in columns from left to right, a plot of the correlated amplitude as a function of baseline length, maps in Stokes I, Q and U, and a plot of the polarized flux vectors superimposed upon contours of Stokes I. Rows, from top to bottom, correspond to maps at 8, 22 and 43 GHz.

generally, the WMAP flux densities are significantly affected by CMB fluctuations, since a ∼ 50μK fluctuation in a 30^′ beam corresponds to a flux density of about 100 mJy between 20–30 GHz.

3.3 Comparison with CLASS

We now compare the 8-GHz data from this project with the polarization measurements made in CLASS (Jackson et al. 2008), typically between 1990 and 1992, which are shown in Fig. 5 for sources with significant (6σ) polarization detections in both works. As expected, the total flux densities cluster around equal values for these point sources,

Figure 3. Comparison of intensity and polarized flux density measurements between this work and the VLA polarization calibrator monitoring programme (Taylor & Myers 2000). Sources are plotted if they were observed in the D-configuration of 2008 by the monitoring programme, interpolated to the date of our observation if necessary. Encircled points represent sources which were stable during the period 3C286, 3C48, 1310+323, 1924−292, 2136+006). Dashed lines represent variation of 20% from the line of equal flux density between these observations and VLA calibration monitoring observations.

but the polarized flux densities are lower for CLASS. Again, this is likely to be a resolution effect, since the CLASS observations were taken in A-configuration of the VLA, which has a maximum baseline a factor of 35 greater than that of the D-configuration used for these observations. We pick up more polarized flux in these D-configuration observations. The implication is that there is polarized emission present on arcsecond scales and therefore resolved out by CLASS. The relative degrees of resolution of the total intensity and polarized flux indicates that the structure being resolved out is more highly polarized than that which is not.

3.4 Position angle differences and multiple components

In Fig. 6 we plot the histograms of differences in position angle between 8-GHz and 22-GHz polarization, and between 22-GHz and 43-GHz polarization, for objects with significant detections of polarization, have contemporaneous polarization measurements at all three frequencies, and have no obviously heavily resolved structure. It is obvious that the two lower frequencies are less well correlated in polarization position angle. Correlation is, unsurprisingly, slightly worse if the CLASS 8-GHz observations are used in addition to the contemporaneous 8-GHz observations. There is no obvious difference in position angle correlation between brighter and fainter sources.

The obvious interpretation of these data are that significant Faraday rotation is present at the lower frequencies; since this effect is proportional to λ^2, the angle of rotation would be expected to be about 6-7 times larger between the lower two frequencies. Galactic Faraday rotation is unlikely to be responsible for this effect, since the <100 rad m^{−2} typical of the Galactic foreground is an order of magnitude smaller than the rotations needed significantly to affect 8-GHz measurement, and indeed in our data there is no correlation of this rotation with galactic latitude. Zavala &

© 0000 RAS, MNRAS 000, 000–000

Figure 4. Comparison of the 22-GHz and 43-GHz flux densities in this work with those of Wright et al. (2009; quoted to two significant figures in that paper). Lines are drawn at 20% either side of the line of equal flux.

Figure 5. Comparison between flux densities in this work and CLASS of total flux density (filled circles) and polarized flux density (open circles) for cases where both surveys detect significant polarized flux. Note the generally lower polarized flux density in CLASS.

Taylor (2004), in a study of parsec-scale polarization of quasar radio cores, find core RMs from 500 to a few thousand rad m^{−2}, and suggest that these are due to a foreground Faraday screen close to the radio jet. Such parsec-scale components are likely to dominate the 22- and 43-GHz flux densities. On the larger scales probed by the lowerfrequency observations, it is possible that in many sources there are multiple polarized components with different position angles. The fact that more polarization is detected here in D-configuration than in the A-configuration

© 0000 RAS, MNRAS 000, 000–000

Figure 6. Differences in position angle between observed polarization at different frequencies. Solid line: difference between 22 GHz and 43 GHz. Dashed line: difference between 8 and 22 GHz for contemporaneous observations. Dash-dotted line: difference between 8 and 22 GHz for objects where only archival CLASS 8-GHz data is available. Only observations with significant detections of polarized flux (defined as 6σ in CLASS and as objects with visible polarized flux in the Q and U maps in these observations) are plotted. Known heavily resolved sources are excluded.

CLASS observations suggests that a more extended jet component, with a lower RM than the core, may be present. Future high-sensitivity observations with e-MERLIN and the EVLA should reveal any such low surface-brightness components.

4 CONCLUSIONS

We have presented observations at 22 and 43 GHz of 199 of the 203 radio sources in the WMAP5 list of Wright et al. (2009) which have flux density >1Jy at 22 GHz, and observations at 8.4 GHz of 133 of these objects. The total flux densities are broadly consistent with those listed by WMAP. For the few objects with previous VLA observations of polarized flux densities, there is also good agreement. There is evidence for extra polarized flux density on arcsecond scales at 8.4 GHz compared to earlier observations at higher resolution. Polarization position angles are very similar at 22 and 43 GHz, but are much less well correlated with position angles measured at 8.4 GHz. This is likely to be due to multiple polarized components which make up the generally complex radio spectra of flat-spectrum radio sources. In a further paper we discuss correlations between the measured intensity and polarization parameters in more detail, and calculate the implications for future CMB polarization measurements of the distribution of polarized flux densities in these discrete sources.

ONLINE MATERIAL

The complete maps can be accessed at http://www.jb.man.ac.uk/∼njj/pol maps/. This figure includes, for each source, in columns from left to right, a plot of the correlated amplitude as a function of baseline length for each source, maps in Stokes I, Q and U, and a plot of the polarized flux vectors superimposed upon contours of Stokes I. For each object, rows are given corresponding to maps at 8, 22 and 43 GHz respectively.

Plots of spectra can be accessed at http://www.jb.man.ac.uk/∼njj/pol spec/ and are given in units of log(flux density/mJy) against log(frequency/GHz). Filled circles are total intensity points, and open circles are polarized flux points measured by fitting to the (u, v) data. Stars are polarized flux points measured by maxima from the Q, U maps.

© 0000 RAS, MNRAS 000, 000–000

10 N. Jackson et al.

ACKNOWLEDGEMENTS

The Very Large Array, National Radio Astronomy Observatory, is a facility of the National Science Foundation operated under cooperative agreement by Associated Universities, Inc.

REFERENCES

Baars J.W.M., Genzel R., Pauliny-Toth I.I.K., Witzel A. 1977, A&A, 61, 99. Blandford R.D., Rees M.J. 1978, Phys S, 17, 265 Condon J.J., Cotton W.D., Greisen E.W., Yin Q.F., Perley R.A., Taylor G.B., Broderick J.J. 1998, AJ, 115, 1693. Dickinson C., Battye R.A., Carreira P., Cleary K., Davies R.D., Davis R.J., Genova-Santos R., Grainge K., Gutiérrez C.M., Hafez Y.A., 2004, MNRAS, 353, 732. Gawronski M.P., et al., 2009, in preparation Gizani N.A.B., Leahy J.P. 2003, MNRAS, 342, 399. Hogbom J.A. , A&AS, 15, 417. Laing R.A. 1981, MNRAS, 195, 261. Leahy J.P., Perley R.A. 1991, AJ, 102, 537.

Leahy J.P., Black A.R.S., Dennett-Thorpe J., Hardcastle M.J., Komissarov S., Perley R.A., Riley J.M., Scheuer P.A.G. 1997, MNRAS, 291, 20.

Mason B.S., Pearson T.J., Readhead A.C.S., Shepherd M.C., Sievers J., Udomprasert P.S., Cartwright J.K., Farmer A.J., Padin S., Myers S.T., 2003, ApJ, 591, 540.

Mason B.S., Weintraub L.C., Sievers J.L., Bond J.R., Myers S.T., Perason T.J., Readhead A.C.S., Shepherd M.C., 2009, astro-ph/0901.4330 Massardi M., Ekers R.D., Murphy T., Ricci R., Sadler E.M., Burke S., deZotti G., Edwards P.G., Hancock P.J., Jackson C.A., 2008, MNRAS, 384, 775.

Montroy, T.E., et al. 2006, Ground-based and Airborne Telescopes. Edited by Stepp, L.M., Proc. SPIE, 6267, 62670R Orr M.J.L., Browne I.W.A. 1982, MNRAS, 200, 1067. Perley R.A., Bridle A.H., Willis A.G. 1984, ApJS, 54, 291.

Reid A., Shone D.L., Akujor C.E., Browne I.W.A., Murphy D.W., Pedelty J., Rudnick L., Walsh D. , A&AS, 110, 213.

Ricci R., Prandoni I., Gruppioni C., Sault R.J., DeZotti G. 2004, A&A, 415, 549. Ricci R., Prandoni I., Gruppioni C., Sault R.J., deZotti G. 2006, A&A, 445, 465.

Sadler E.M., Ricci R., Ekers R.D.., Ekers J.A., Hancock P.J., Jackson C.A., Kesteven M.J., Murphy T., Phillips C., Reinfrank R.F., 2006, MNRAS, 371, 898.

Sadler E.M., Ricci R., Ekers R.D.., Sault RobertJ., Jackson C.A., deZotti G. 2008, MNRAS, 385, 1656. Samtleben D., 2008, To be published in the Proceedings of the 43rd ”Rencontres de Moriond” on Cosmology 2008, arXiv0806.4334 Saikia D.J., Kulkarni V.K., Porcas R.W. 1986, MNRAS, 219, 719.

Saikia D.J., Subrahmanya C.R., Patnaik A.R., Unger S.W., Cornwell T.J., Graham D.A., Prabhu T.P. 1986, MNRAS, 219, 545.

Scheuer P.A.G., Readhead A.C.S. 1979, Natur, 277, 182. Simmons J.F.L., Stewart B.G. 1985, A&A, 142, 100.

Taylor G.B., Gugliucci N.E., Fabian A.C., Sanders J.S., Gentile G., Allen S.W., 2006, MNRAS 368, 1500 Taylor G.B., Myers S.T., 2000, VLA Scientific Memo 26. Available from NRAO or from http://www.vlba.nrao.edu/memos/sci/ Tegmark M., Efstathiou G. 1996, MNRAS, 281, 1297.

Polarization of WMAP point sources 11

Toffolatti L., Argueso Gomez F., de Zotti G., Mazzei P, Franceschini A., Danese L., Burigana C., 1998, MNRAS 297, 116 Toffolatti L., Negrello M., González-Nuevo J., de Zotti G., Silva L., Granato G.L., Argueso F., 2005, A&A 438, 475 Tucci M., Martínez-González E., Toffolatti L., González-Nuevo J., de Zotti G., 2004, MNRAS 349, 1267 Vol’Vach A.E., Vol’Vach L.N., Kardashev N.S., Larionov M.G. 2008, ARep 52, 429.

Waldram E.M., Pooley G.G., Grainge K.J.B., Jones M.E., Saunders R.D.E., Scott P.F., Taylor A.C. 2003, MNRAS 342, 915.

Waldram E.M., Bolton R.C., Pooley G.G., Riley J.M. 2007, MNRAS 379, 1442. Wall J.V., Jackson C.A., 1997, MNRAS 290, L17 Wright E.L., Chen X., Odegard N., Bennett C.L., Hill R.S., Hinshaw G., Jarosik N., Komatsu E., Nolta M.R., Page L., 2009, ApJS 180, 283.

Zavala R.T., Taylor G.B. 2004, ApJ 612, 749

12 N. Jackson et al.

X-band K-band Q-band I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘)

0006−063 2100±40 20.5±0.4 155.9±0.5 1820±90 65.4±2.5 22.8±1.1 1540±80 52.5±2.5 10.9±0.9 0010+110 469.0±0.1 0.2±0.1 87±7 710±40 6.3±2.4† 115±10 1550±80 13.4±1.3 29±3 0019+203 1275.1±0.4 55.8±0.2 106.9±0.1 650±30 7.1±1.9† 149±12 475±24 <10 - 0019+260 389±8 8.1±0.2 9.4±0.7 347±17 <10 - 270±14 <10 - 1 0029+059 740±15 19.8±0.3 116.0±0.5 630±30 17.5±2.0 130±4 423±21 15.9±1.3 146.9±2.6 0043+521 179±11 <10 - 46.7±2.9 <10 - 2 0047−252 268±16 <10 - 73±8 <10 - 3 0050−068 940±19 23.0±0.5 144.8±0.4 1370±70 36±3 145±5 1320±70 39.1±2.1 127.9±1.2 0051−094 1480±70 62.6±2.8 156.6±1.3 1470±70 77±3 147.2±0.9 4 0108+015 1620±30 66.0±1.0 112.9±0.5 1980±100 38.2±2.4 103.3±1.3 1670±80 29.1±2.0 115.3±2.2 0108+133 900±27 78.4±1.8 95.8±0.3 39.5±2.3 <10 - 28.9±1.9 <10 - 5 0116−116 912±18 19.0±0.4 105.6±0.5 910±50 <10 - 960±50 13.1±1.3 171.1±2.2 0121+118 3810±80 59.0±1.2 90.3±0.1 3130±160 178±7 15.8±0.9 1990±100 143±7 8.0±0.6 0125−001 1089±22 <10 - 1030±50 <10 - 780±40 4.7±2.1† 111±14 6 0132−168 830±17 18.0±0.4 104.5±0.6 1250±60 13±6† 11±6 1660±80 39.4±2.1 164.1±1.4 7 0137−244 949±19 19.1±0.4 113.3±0.6 910±50 <10 - 690±30 16.8±2.0 12±3 0137+478 3140±60 26.6±0.6 116.3±0.5 2660±130 59.1±3.0 71.5±1.3 1750±90 19.1±1.4 58.5±2.3 0149+058 1137±23 25.4±0.4 112.7±0.5 730±40 <10 - 421±21 <10 - 0152+221 1038.5±0.1 20.9±0.1 56.8±0.1 890±40 42.4±2.4 3.5±0.8 730±40 46.5±2.5 177.1±0.9 8 0204+152 1485±30 30.1±0.6 142.1±0.3 820±40 6.3±1.0† 58±5 547±27 18.8±1.3† 168.9±1.9 0205+322 626.8±2.3 5.2±0.1 48.4±0.4 3060±150 102±6 99.1±0.7 2150±110 87±4 92.4±0.6 0218+016 1209.5±0.7 17.7±0.3 149.7±0.4 1720±90 20.1±1.6 5.7±1.9 1690±80 31.8±1.5 19.0±1.3 0220+359 1720±30 134.2±2.4 35.8±0.2 1400±70 194±8 31.0±0.8 950±50 145±5 25.4±1.0 0223+430 231±6 9.5±0.5 170.3±1.1 152±8 <10 - 94±6 <10 - 9 0231+133 1732.2±1.4 11.5±0.2 157.0±0.6 1390±70 9.4±1.3† 157±4 1030±50 11.1±1.8† 117±4 0237+288 3640±70 144.8±2.1 67.6±0.4 3050±150 49.3±2.6 78.0±1.2 2380±120 47.9±1.9 112.4±1.2 0238+166 3190±60 30.8±0.7 91.7±0.3 3340±170 85±4 34.0±0.8 3160±160 57.7±2.3 23.2±1.1 0241−083 1060±50 <10 - 960±50 11.3±1.2 140.0±2.7 10 0259−002 1067±21 25.5±0.4 116.5±0.5 860±40 14.0±2.4 55±3 508±25 <10 - 0308+040 833±21 29.3±0.8 105.0±0.6 542±27 6.4±1.1† 63±5 372±19 6.1±1.1† 116±5 11 0309+104 1243.1±1.1 25.9±0.3 124.5±0.3 810±40 33.9±2.1 74.5±1.6 760±40 34.1±1.6 63.9±1.4 0319+415 14530±730 12±3 99±7 10620±530 51±5 57.3±1.8 12 0329−239 1137±23 35.3±0.6 157.0±0.5 1250±60 13.2±1.5 104±4 1040±50 11.2±1.9 110±5 0336−129 453±23 11.4±1.7 171±7 399±20 13.5±1.3 163.6±2.7 0339−017 2040±100 67±4 91.6±0.4 1780±90 48.0±2.5 96.5±1.1 0340−213 1054±21 26.9±0.6 132.3±0.4 900±50 14±3 39±4 720±40 14.6±1.4 30.3±2.9 0348−277 760±40 46±4 41.8±1.5 760±40 41.8±2.6 43±5 0358+104 75±4 18.2±0.5 103.4±0.8 6.7±1.1 <10 - 6.4±1.1 <10 - 13 0405−130 2230±40 31.1±0.6 157.9±0.5 1300±70 68±4 169.4±1.0 850±40 22.4±2.3 166.4±2.3 14 0411+769 2060±40 48.9±0.8 120.4±0.4 1060±50 71±4 176.7±0.9 570±29 44.2±1.9 156.6±1.2 0416−208 1103±23 40.7±0.8 121.8±0.4 650±30 11.8±2.1† 52±5 544±27 <10 - 0423−013 3920±80 157.9±3.0 97.6±0.2 4340±220 145±8 89.6±0.3 3710±190 130±6 85.6±0.6 0423+023 266±5 5.6±0.3 126.0±2.4 201±10 7.3±0.9 124±4 113±6 7.2±1.3 116±5 15 0424+005 518±10 21.7±0.5 88.0±0.4 481±24 20.0±1.8 60.4±2.2 411±21 20.4±1.6 43.0±1.9 0433+053 3660±70 90.1±1.7 144.0±0.3 2650±130 126±6 170.2±0.7 1950±100 86±3 154.7±1.0 0453−281 1960±40 43±8 123.8±2.4 1700±90 21±5 63±5 1440±70 14.1±2.5 11±6 0456−233 2080±40 44.7±1.1 120.3±0.6 1950±100 11.7±2.3† 117±5 1530±80 18.4±2.7† 106±4 16 0501−019 995±20 8.3±0.3 109.7±0.9 960±50 6.3±1.1 33±6 890±40 33.6±1.8 34.1±1.0 0513−219 1041±21 7.5±0.6 122.1±1.7 800±40 43.7±2.8 136±4 620±30 38.7±2.6 134.1±1.2 0519−056 8.1±0.3 <10 - 3.8±1.4 <10 - 2.6±0.9 <10 - 17 0527−126 470±50 <10 - 104±13 <10 - 18 0542+498 4680±90 119.9±2.1 168.9±0.3 1820±90 67.8±2.8 73.9±1.0 820±40 41.4±2.1 79.1±1.0 0555+397 7200±18 51.8±0.1 64.4±0.1 3110±160 21.6±1.7 158.4±2.3 2040±100 32.9±1.7 151.9±1.4 19 0607+673 611.5±0.4 21.5±0.3 121.8±0.3 600±30 <10 - 435±23 49±18† 20±11 0608−223 1376±28 28.8±0.7 89.2±0.4 1470±70 68±4 50.0±2.2 1150±60 74±4 45.3±0.8 0609−156 2990±150 54±5 52.8±1.4 2190±110 40±6 68±4 0629−199 682±14 8.8±0.3 53.4±0.9 610±30 7.9±1.7† 27±6 407±20 9.2±1.9† 173±13 0636−205 283±8 42.0±1.0 116.6±0.7 34.9±2.9 <10 - 9.2±2.1 <10 - 20 0646+448 3800±80 84.7±1.7 44.8±0.1 3160±160 21.8±1.3 122.9±1.5 2120±110 31.9±2.0 140.6±1.8 0721+713 2070±40 67.1±1.4 180.0±0.1 4050±200 91±12 28±6 4680±230 127±6 52.0±0.5 0738+177 891±18 15.6±0.4 147.4±0.8 640±30 21.0±1.9 160.7±2.3 407±20 14.9±1.9 155±4 0739+016 1809.3±0.9 58.9±0.3 45.1±0.1 1520±80 45.1±2.3 22.0±1.5 1480±70 29.6±1.8 9.4±1.2

Polarization of WMAP point sources 13

X-band K-band Q-band I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘)

0741+311 1610±30 79.2±1.5 36.9±0.2 760±40 19.1±3.0 74±7 458±23 17.8±1.3 68.9±2.0 0745+102 970±50 10.3±1.5† 14±3 312±16 <10 - 21 0746−007 1910±40 65.7±1.3 93.7±0.2 1060±50 27.9±1.5 147.1±1.3 567±28 18.4±1.5 139±7 0750+125 4810±110 129.7±1.9 69.4±0.4 4230±210 148±7 33.2±0.8 2800±140 113±4 27.1±1.0 0753+539 967±19 103.2±1.8 34.2±0.3 1020±50 91±4 37.0±0.7 910±50 76±3 30.7±1.0 0757+099 1118±22 47.5±1.0 46.7±0.2 1010±50 50.3±2.4 23.0±1.3 750±40 38.6±1.7 17.8±1.2 0808−078 710±40 15.3±2.0 43±10 700±30 23.5±1.6 43.6±1.1 0813+482 1960±60 24.9±0.5 11.9±0.5 440±40 12.0±1.1 134.4±2.2 172±16 6.1±0.8 119±4 22 0825+031 1218±24 84.3±1.5 54.6±0.3 1460±70 78±4 35.6±0.9 1340±70 45.9±2.6 39.8±0.7 0831+241 - - - - - - 1360±70 35.8±2.4† 13.2±2.0 23 0836−202 2730±50 70.3±1.0 111.3±0.4 1790±90 44±3† 23.4±2.0 1020±50 9.1±1.3† 161±4 24 0838+583 518±8 19.1±0.1 179.8±0.1 1160±60 29.3±2.0 167.1±1.7 810±40 18.5±1.1 158.6±1.7 0840+132 710±40 13.0±1.3 13.3±2.7 670±30 18.1±1.7 166.8±2.1 0841+708 1610±30 63.3±1.2 96.3±0.2 1650±80 55.7±2.5 111.9±1.3 2020±100 52.0±2.1 118.0±1.1 0854+201 3910±290 98.9±0.2 79.9±0.0 3020±150 96±5 178.1±0.5 2620±130 116±6 178.3±0.3 0902−142 1383±28 66.7±1.6 84.7±0.2 581±30 10.2±1.7† 57±4 356±18 10.5±1.7† 102±4 0907−203 338±17 17.0±2.6† 14±6 96±17 <10 - 25 0909+013 1295±26 63.9±1.0 112.3±0.4 1400±70 36.2±2.1 139.5±1.6 1260±60 23.8±1.5 153.3±1.7 0909+428 970±50 25.1±1.9 126.2±1.6 740±40 32.9±2.0 146.3±1.8 0914+028 1194±24 44.7±0.8 104.6±0.4 840±40 25.8±1.8 119.7±2.5 581±29 20.2±1.5 119.7±2.4 0918−120 2460±120 121.3±2.3 101.8±0.4 500±40 52±3 125.8±1.7 39±7 <10 - 26 0920+446 1373±27 31.6±0.5 162.6±0.4 2180±110 25.4±2.2 126.3±2.0 1960±100 30.1±1.9 93.3±2.5 0921−263 2090±40 7.5±0.3 172.5±1.1 1190±60 30±3 78.8±2.9 660±30 14.3±1.9 165±4 27 0927+390 8456±13 195.7±0.4 130.2±0.0 9000±450 315±14 148.6±1.0 5670±290 212±9 148.4±1.1 28 0948+406 1910±40 90.6±1.7 35.2±0.3 1590±80 48.4±2.5 18.3±1.5 1110±60 29.0±1.5 22.9±1.5 0955+695 1000±30 19.1±0.5 40.2±0.4 270±20 <10 - 61±6 <10 - 29 0958+473 1498±30 38.6±0.6 19.5±0.5 970±50 10.1±1.1 150.0±3.0 585±29 7.0±1.1 156±5 1014−231 - - - - - - - - - 30 1037−295 - - - - - - 31 1038+051 491.8±0.3 4.0±0.2 143.4±1.4 1180±60 99±7 50±7 700±40 72±4 176.4±0.6 1041+061 1530±30 71.6±1.3 80.1±0.3 1150±60 20.4±1.8 36.3±2.8 600±30 12.6±1.9 34.1±2.7 1047−191 1166±23 31.4±0.6 75.8±0.4 - - - - - - 32 1047+717 1215±24 32.5±0.7 37.3±0.3 1370±70 32.9±2.1 159.9±1.8 1140±60 31.1±1.9 146.5±1.4 1058+015 3853.1±0.4 46.9±0.1 122.4±0.1 4370±220 347±16 125.2±0.7 3340±170 335±14 123.4±0.7 1118−125 - - - - - - 33 1127−189 2250±50 69.4±1.4 84.2±0.3 1630±80 <10 - 830±40 <10 - 34 1130−148 2970±60 109.5±2.4 131.6±0.1 1460±70 56±9 167.8±2.8 561±28 29±4 158±4 35 1130+382 882.5±0.8 2.5±0.2 44.7±2.7 1090±50 23.2±1.6 127.3±1.7 660±30 17.6±1.2 118.6±2.1 1153+495 1064±23 28.3±0.7 90.6±0.2 990±50 10.1±1.2 14±3 650±30 12.6±1.9 26±5 1155+810 1464±29 35.1±0.6 74.0±0.4 930±50 22.2±2.4 86.0±2.3 564±28 17.3±2.8 74±5 36 1159+292 1232.8±0.1 7.7±0.1 167.3±0.2 2580±130 41±7 153±6 2260±110 64.9±2.7 160.8±1.1 1209−240 576±12 16.6±0.6 170.2±0.7 445±23 <10 - 373±19 <10 - 1215−174 1630±80 61±5 74.1±2.1 1240±60 66±3 60.8±1.2 1219+058 340±7 2.2±0.6 76±7 381±19 <10 - 222±11 <10 - 37 1229+020 31730±810 1560±30 134.2±0.1 24510±1230 1130±60 137.1±0.4 15280±760 920±40 126.3±0.6 38 1230+123 3190±320 70±15 2±4 1490±70 46±5 158.9±3.0 39 1239+074 876±18 47.4±1.0 138.4±0.6 690±30 55±4 127.8±1.1 423±21 29.7±2.5 114.8±2.3 1246−257 871±18 24.0±0.4 22.1±0.5 830±40 19±26 54±14 760±40 32.7±2.5 43.5±1.6 1256−057 13950±280 648±9 70.4±0.4 16800±850 760±40 49.3±0.6 - - - 40 1258−223 700±40 15±13† 27±19 578±29 11.5±2.8† 61±6 41 1258−319 980±50 104±16 70±5 573±29 60±4 56.2±1.4 1310+323 2277.1±0.4 15.3±0.1 23.4±0.1 2110±110 59.2±2.9 31.6±1.1 2330±120 103±5 41.2±0.7 1316−336 1820±40 80.2±1.5 168.1±0.4 - - - 1730±90 65±8 118±5 42 1330+250 960±50 25.8±1.9 0.8±1.8 556±28 14.1±1.3 5.4±1.8 1331+305 5210±100 717±12 33.0±0.3 2520±130 306±13 32.7±0.8 1480±70 194±8 32.6±0.8 43 1332+020 556±11 16.8±0.4 177.7±0.4 800±40 5.5±1.3† 162±6 890±40 13.6±1.5† 61±3 1336−339 90±3 <10 - 22±6 <10 - 8±3 <10 - 44 1337−129 5850±290 164±8 42.5±0.5 5470±270 178±7 29.0±1.0 1347+123 1130±60 14.4±1.7 113±3 760±40 18.7±1.4 17.3±1.8 1354−106 884±18 48.5±0.8 152.7±0.4 750±40 17.3±2.0 36±4 650±30 8.0±1.6 15±5 1356+193 1820±40 54.6±1.2 46.9±0.2 2070±100 32.8±1.9 69.0±1.6 1680±80 38.5±2.1 79.3±1.0 1408−078 811±16 42.9±0.8 166.2±0.4 770±40 13.5±1.5† 66±3 640±30 18.5±1.4† 24.9±2.1 45

14 N. Jackson et al.

X-band K-band Q-band I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘)

1419+383 283±6 7.2±0.3 46.7±1.0 249±13 <10 - 209±17 <10 - 1427−330 31.7±1.9 1.0±0.2 173±7 - - - 4.4±1.9 <10 - 46 1446−163 574±11 14.5±0.3 153.8±0.5 323±16 12.6±1.5 88±3 196±10 7.6±1.9 62±9 1458+716 1090±50 31.9±2.6 49.3±1.4 690±40 17.0±1.5 40.5±2.1 1504+105 1540±30 53.7±0.8 155.9±0.4 1750±90 32.3±1.9 105.0±1.8 1700±90 56.7±2.4 72.9±1.1 1506−167 870±40 <10 - 650±30 <10 - 1510−057 1730±40 18.8±0.3 109.9±0.5 1190±60 50.5±2.8 86.7±0.7 840±40 40.7±2.0 78.0±1.1 1512−090 2880±60 15.7±0.4 117.4±0.7 3060±150 93±5 112.1±1.5 2560±130 80±3 114.6±1.1 1513−100 1121±22 44.9±2.3 157.5±1.5 1220±60 36.2±2.6 154.2±1.9 1080±50 18.8±1.4 154.6±2.1 1516+002 954.6±1.0 3.9±0.2 106.4±1.6 910±50 18±3 58±7 870±40 17.9±1.5 50.6±1.9 1517−243 2150±110 87±5 46.0±0.8 1940±100 68±3 33.7±1.0 1540+147 1610±30 169.5±2.5 154.8±0.4 1270±60 125±6 142.5±0.6 1000±50 99±5 140.5±0.5 1549+026 975.2±0.8 5.6±0.1 50.6±0.5 2420±120 67±7 61±5 2170±110 73±4 51.2±0.6 1550+054 3300±70 240±4 144.9±0.3 2710±140 180±9 141.3±0.5 2170±110 139±7 139.8±0.4 1608+104 1497±30 21.7±0.5 161.7±0.6 1260±60 12.7±1.3† 74.9±2.6 980±50 12.5±1.0† 65.7±2.4 47 1613+342 3060±130 86.8±0.4 4.8±0.0 2610±130 38.7±2.4 25.2±1.8 1680±80 22.5±1.6 36.3±2.6 1633+824 781±16 13.6±0.3 110.3±0.6 820±40 <10 - - - - 48 1635+381 2770±60 96.9±1.9 52.5±0.2 2770±140 23.3±1.8 53.0±1.5 2670±130 56.5±2.4 64.6±1.2 1638+573 1356±7 27.5±0.1 125.7±0.1 2210±110 12.8±1.5 98±5 1880±90 22.2±2.4 88.5±1.4 1642+398 5653.8±1.9 238.5±0.5 24.8±0.1 4540±230 79±4 38.9±0.8 4200±210 77±4 48.9±0.5 49 1642+689 4660±230 54±4 148.0±2.1 4670±230 270±11 103.2±0.8 1651+049 1630±90 195±5 26.7±0.7 231±18 <10 - 18.3±2.6 <10 - 50 1654+396 1311±26 36.5±0.6 14.3±0.4 1020±50 33.4±2.2 138.0±1.1 860±40 22.9±1.6 140.9±1.9 1657+479 743±15 8.8±0.2 71.5±0.7 670±30 15.1±0.7 148.5±1.3 630±30 12.9±0.8 135±8 1658+077 917.9±0.4 16.5±0.1 153.0±0.1 1800±90 92±10 113.6±2.8 1590±80 82±3 114.1±1.1 1734+389 955±19 6.1±0.3 3.2±1.1 1230±60 67.7±2.8 107.1±1.1 1220±60 98±4 101.5±0.8 1740+522 1357.8±0.6 15.9±0.1 21.1±0.2 910±50 15.6±1.4 151.8±2.5 730±40 20.9±1.3 160.3±1.8 1753+288 518.8±1.0 27.1±0.1 162.1±0.1 1740±90 62±5 156.6±2.4 1380±70 38.6±1.7 157.4±1.3 1800+784 3000±60 118.2±1.7 111.7±0.4 2940±150 115±5 99.9±0.8 2380±120 98±5 97.2±0.6 1801+440 1329±27 62.4±1.2 49.9±0.2 1350±70 44±9 44.2±0.5 1300±70 27.7±1.9 48.5±2.6 1806+698 1720±40 59.3±1.0 151.4±0.4 1620±80 7.5±1.3 147±4 1460±70 8.4±1.1 30±4 51 1824+568 1385±28 50.4±1.0 33.2±0.3 1450±70 111±4 19.4±1.1 1230±60 116±5 15.4±0.9 1829+487 3370±80 71.2±1.2 63.2±0.4 2510±130 50.2±2.6 101.1±1.1 1750±90 57±3 91.8±0.5 52 1842+681 1640±30 88.8±1.6 9.9±0.3 1650±80 100±4 15.9±1.0 1440±70 74±4 8.3±0.7 1849+670 1487±30 34.0±0.7 143.9±0.4 2120±110 10.5±1.3† 117±4 2100±100 32.4±1.5† 155.4±1.3 53 1850+283 1493±30 31.2±0.6 23.4±0.5 840±40 <10 - 432±22 <10 - 1902+318 1590±30 50.5±1.0 44.2±0.2 990±50 14.6±1.2 27.9±2.4 660±30 14.0±1.2 43.2±2.0 1923−210 1520±80 31±4 134.1±1.4 1450±70 16±5 9±10 1924−292 11920±240 224±4 147.0±0.3 13670±680 1010±50 84.9±0.4 12870±640 1150±50 81.4±0.6 1927+613 1035±21 65.9±1.2 126.6±0.2 810±40 38.6±2.0 112.4±1.5 583±29 27.2±1.8 96.5±1.6 1927+739 3220±60 44.3±0.7 117.8±0.4 2820±140 43.3±2.2 67.4±1.4 2230±110 50.9±2.6 54.5±1.3 1939−154 789±16 12.8±0.2 157.0±0.5 720±40 6.8±1.4† 62±6 509±25 7.4±1.1† 30±3 2000−178 2040±40 72.9±1.2 148.8±0.4 2010±100 15.9±2.1† 62±4 1790±90 26.8±1.7† 18.3±1.8 54 2011−157 2080±40 46.0±1.1 149.7±0.9 1810±90 37±10 125±3 1360±70 22.1±2.9 95±8 2022+616 3028.5±1.2 0.0±0.1 180±70 1810±90 6.9±1.3 59±5 1000±50 6.5±1.1 51±5 2101+037 831±17 41.0±0.8 130.7±0.2 720±40 33.6±1.8 115.5±1.5 620±30 13.5±1.3 102.3±2.6 2123+056 1910±40 56.6±1.2 5.2±0.2 1460±70 82±3 28.1±1.0 1120±60 69.2±2.6 21.0±1.1 2131−121 1980±100 41.5±2.9 149.4±1.6 1600±80 35.9±2.1 174.3±1.2 2134−019 2040±100 162±8 91.0±0.2 1620±80 130±5 72.4±1.0 2136+006 7549±12 44.7±0.4 161.7±0.2 5220±260 134±5 18.0±1.0 3180±160 61±3 0.8±0.4 2139+144 2515.8±0.7 14.2±0.1 32.1±0.2 2110±110 38±9 19±5 1310±70 40.8±2.2 172.8±1.0 2143+176 561±11 9.7±0.5 142.4±0.8 690±30 24.3±2.0 11.4±1.7 620±30 17.4±1.9 13.7±2.1 2148+069 6220±120 122.2±2.3 126.2±0.3 5250±260 95±4 66.3±1.2 4690±230 54.5±2.9 41.9±1.4 2151−304 1750±40 39.4±0.6 67.5±0.4 1740±90 35±4 30.7±2.6 1300±70 33.0±2.4 17.0±1.9 2158−150 1970±40 71.2±1.8 71.6±0.7 1360±70 62±3 44.7±0.6 1120±60 61.6±2.4 23.3±1.1 2202+422 2690±130 184±7 17.8±1.0 2410±120 180±8 12.5±0.8 2203+173 1346±27 44.7±0.9 7.3±0.2 1340±70 67.4±2.6 20.3±1.1 1090±50 70.5±3.0 14.1±0.9 2203+317 2700±50 46.4±0.9 37.8±0.2 2140±110 19.1±1.6 87.5±1.4 1320±70 44.0±1.9 110.4±1.2 2206−186 3150±60 41.6±0.9 55.0±0.7 1720±90 60±4 40.5±0.9 1080±50 33.1±2.4 32.2±1.5 2211+238 1220±24 66.9±1.3 6.5±0.2 950±50 47.3±2.0 27.1±1.2 640±30 36.1±1.7 24.0±1.3 2218−035 1640±80 15±3 75±9 1180±60 6.9±1.4 49±5 2225−049 7510±150 161.3±2.8 163.2±0.4 8630±430 264±10 19.6±1.0 7620±380 204±8 17.6±1.0

Polarization of WMAP point sources 15

X-band K-band Q-band I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘) I(mJy) P(mJy) Angle(^∘)

2229−085 3390±70 107.5±2.1 139.1±0.1 3040±150 55±3 178.1±0.8 3210±160 62±3 7.3±0.8 2232+117 3029.9±2.4 39.1±0.5 89.0±0.2 4860±240 88±4 67.9±1.3 4300±220 85±7 92.8±0.6 2236+284 2160.5±0.2 33.7±0.1 51.8±0.1 1330±70 25.7±2.0 163.9±2.0 1140±60 52.0±2.9 175.2±1.0 2246−121 2420±50 27.3±0.7 119.9±0.5 2350±120 30.3±2.0 2.8±2.3 1980±100 61.5±2.5 163.7±1.0 2254+161 9660±190 470±9 176.4±0.1 15520±780 269±19 140.9±0.6 20620±1030 250±30 101±3 55 2255+420 727±15 15.7±0.4 105.8±0.9 438±22 <10 - 183±9 <10 - 2258−279 2860±140 18±6 160±8 3060±160 77±4 166.4±1.4 56 2330+109 1018.4±0.1 16.4±0.1 38.6±0.1 770±40 23.4±1.8 45.5±1.0 590±30 4.9±1.3 28±7 2331−159 690±30 50±3 72.6±1.8 524±26 32.3±1.7 69.4±1.6 2334+075 1137±23 41.2±0.8 146.2±0.3 1490±70 42.8±2.7 141.4±0.8 1320±70 54.9±2.5 149.2±1.1 2346+094 1281±26 45.2±0.9 130.5±0.2 980±50 30.4±2.1 150.3±1.7 640±30 21.7±1.3 154.0±1.7 2348−165 1590±30 10.6±0.3 76.7±0.8 1990±100 28.1±2.3 16.4±2.5 2230±110 51.3±2.2 158.8±1.2 2354+458 1253±25 17.0±0.5 176.9±0.3 770±40 10.1±1.5 101±4 392±20 <10 - 2358−102 1202±24 31.0±0.6 122.8±0.3 980±50 15.7±3.0 32±5 820±40 21.7±2.2 17±4

16 N. Jackson et al.

Caption to Table 2.

Flux densities of observed sources at X-, K- and Q-bands. Fluxes in italics are from CLASS, in the case of multiple observations using that with the lowest error in polarized flux density. A dagger indicates that the measurement has been taken from the Q and U maps, rather than the fits to the u-v data (see text for details). A “zero” error means smaller than 1 mJy. Notes to the table: 1. Nearest plausible ID is 4C+25.01 (00 19 39.21 +26 02 45.4) which is 0.5 Jy at 1.4 GHz (NVSS); multiple sources may contribute to the WMAP flux density. The NVSS position was observed, leading to the detection of a resolved, polarized source at X-band. 2. Source is identified with 3C20 which is a 50^{′′} steep-spectrum double (Laing 1981). Nearly all structure is resolved out by these observations. 3. Identification is the star-forming galaxy NGC253. Structure is nearly resolved out by these observations. 4. No X-band polarization available from CLASS. 5. Identification is 3C33 which is a 5^′ steep spectrum double (e.g. Leahy & Perley 1991). Only the central regions are seen in these observations. 6. Used as the zero-polarization calibrator at X-band. 7. Offset polarized component? Fit to the K-band images gives 13.4 mJy polarized flux density at 11^∘. No significant difference between methods at Q-band. 8. CLASS X-band polarization measured on two occasions: 21 mJy in PA 57 (total flux density 1039 mJy), 29mJy in PA 25 (total flux density 1061 mJy). 9. Identification is the pair of sources 3C 66A, 3C 66B. Observation pointed at 3C 66A and structure heavily resolved; most of the high-frequency contribution to the flux is probably from 3C 66B, however. 10. No X-band polarization available. K-band polarization from fitting to u − v data probably underestimated; images give 10.2 mJy in PA 25^∘. 11. Source is identified with 3C78 (e.g. Saikia et al. 1986); heavily resolved by these observations. 12. Identified with 3C84; used as zero-polarization calibrator for K-band and Q-band observations. Polarization level difficult to measure because of residual errors; best guess from analysis of images is 13 mJy polarized flux density in PA 129^∘ 13. Identified with 3C98 which is a 216 arcsec steep spectrum double (e.g. Leahy et al. 1997); heavily resolved by these observations. 14. Probably resolved; peak in the Q-band image has a polarized flux density of 11mJy at PA 0^∘. 15. Extreme discrepancy between flux observed in all VLA bands and the WMAP flux. No obvious identification from NVSS; the observed position (04 24 2.58 +02 26 42) is the closest NVSS source (about 10^′) from the WMAP position; WMAP flux may be a combination of this and two other ∼1-Jy sources at only slightly larger distance. 16. Fits to K-band image suggest 12mJy polarized flux density in PA 117^∘, but sparse data make estimation difficult. 17. Blended source (see note in Wright et al. 2008). 18. ID is a planetary nebula (IC0418). 19. Several X-band measurements from CLASS with highly variable polarized flux density and PA. 20. Identification is a very large (15^′ ) double-lobed radio source, PKS0634−20. One of the lobes was observed, and is heavily resolved. 21. Possible offset polarized component in K-band; analysis of image suggests 10mJy in PA 14^∘. 22. ID is probably the strong source 4.5^′ SSE, 3C196. This is a small double (e.g. Reid et al 1995) both of whose components are detected. 23. Very little data obtained at X-band and K-band, no reliable results at these frequencies. 24. Phase errors limit reliability; analysis of images suggests K-band polarization 44mJy at PA 23^∘. No significant polarization detected at Q-band. 25. Extremely steep spectral index between K-band and Q-band. 26. ID is Hydra A, a large radio source (e.g. Taylor et al. 1990). Core of the source was observed, consisting of extended feature 45^{′′} across. Polarization level depends strongly on aperture used. 27. Analysis of images suggests higher K-band polarization (50 mJy) at same PA. 28. Identification is 4C39.25. X-band polarization (CLASS) highly variable. 29. Identification is M82 (starburst galaxy). 30. Error in pointing of array. 31. Clear ID, but data of poor quality, phase solutions not good. Polarization measurements unreliable at K and Q-band. 32. Poor quality data at K-band and Q-band, phase solutions not good. Polarization measurements unreliable at both frequencies. 33. Most plausible ID is 4^′ W, little data at K-band and phase solutions not good. 34. Good ID, poor quality data at K-band and Q-band, phase solutions not good and polarization measurements unreliable. 35. Good ID, poor quality data at Q-band, phase solutions not good and polarization measurements unreliable. 36. Analysis of Q-band image suggest slightly lower polarized flux density, 12mJy at PA 80^∘. 37. ID is 3C270; pointing position is that of the core (Birkinshaw & Davies 1985). 38. ID is 3C273; polarization at X-band (CLASS) is high and variable. 39. ID is M87; the polarized jet pointing WNW is visible. Very little data at K-band; this polarization measurement is unreliable. 40. Sparse data at K and Q-band; image at Q-band suggests that this polarization measurement is unreliable. 41. Fits to Q-band images suggest polarized flux density of 12mJy in PA 61^∘. 42. Little data at K-band; unreliable polarization measurement at this frequency. 43. ID is 3C286; primary flux and polarization position angle calibrator; also used for non-closing offset calibration at X-band. 44. IC4296. This is 2.5 arcmin double with compact core. No significant polarization detected. 45. Possible offset polarized component in K-band; analysis of image suggests 14mJy at PA 66^∘. 46. No obvious catalogued source. Nearest radio source is MRC 1424−328 (NVSS position 14 27 35.7, −33 02 22, 253 mJy at 1.4 GHz) approximately 1.3 arcminutes E. This position yields 180 mJy of correlated flux at 8.4 GHz and no detections at higher frequencies. WMAP flux density of 1 Jy at 22 GHz may be the sum of a number of nearby sources. 47. Analysis of K-band image suggests slightly higher polarization: 13mJy at PA 75^∘; detection is significant. 48. ID is NGC6251; position of core observed (e.g. Perley, Bridle & Willis 1984). 49. ID is 3C345. Phase errors in K-band observation; analysis of image suggests slightly higher polarized flux density of 75mJy in PA 164^∘. 50. ID is Hercules A; core observed (e.g. Gizani & Leahy 2003), highly resolved. The core lies in between two polarized components, and its polarized flux density is much less than that inferred from the u − v data by the automatic fitting. 51. Fits to Q-band images suggest polarized flux density 14mJy in PA 60^∘. 52. ID is 3C380. 53. K-band images reveal significant detection of polarized flux density, ∼10mJy in PA 117^∘. 54. Possibly offset polarized component at K-band of 16mJy in PA 62^∘. 55. ID is 3C454.3. 56. K-band polarization measurement unreliable; noisy map with significant phase errors.