arXiv:0912.1365v1 [physics.optics] 7 Dec 2009

Spectroscopy of 1.55 μm PbS Quantum Dots on Si Photonic Crystal Cavities with a Fiber Taper Waveguide

M. T. Rakher,^{1, ∗} R. Bose,^{2, †} C. W. Wong,^2 and K. Srinivasan^1 1Center for Nanoscale Science and Technology, National Institute of Standards and Technology, Gaithersburg, MD 20899, USA 2Optical Nanostructures Laboratory, Center for Integrated Science and Engineering, Solid-State Science and Engineering and Mechanical Engineering, Columbia University, New York, NY 10027, USA (Dated: September 6, 2018)

We use an optical fiber taper waveguide to probe PbS quantum dots (QDs) dried on Si photonic crystal cavities near 1.55 μm. We demonstrate that a low density (≲ 100 μm^{−2}) of QDs does not significantly degrade cavity quality factors as high as ≈3×10^4. We also show that the tapered fiber can be used to excite the QDs and collect the subsequent cavity-filtered photoluminescence, and present measurements of reversible photodarkening and QD saturation. This method represents an important step towards spectroscopy of single colloidal QDs in the telecommunications band.

PACS numbers: 78.67.Hc, 42.70.Qs, 42.60.Da

The combination of low optical absorption and mature device processing has resulted in the development of low loss silicon photonic devices such as high quality factor (Q) photonic crystal cavities (PCCs) operating in the technologically relevant 1.55 μm wavelength range^{1,2,3}. Silicon’s indirect bandgap represents a challenge in making light-emitting devices and as a result there has been considerable interest in developing hybrid systems integrating a light-emitting material^{4,5}. Lead salt colloidal quantum dots^{6,7} (QDs) represent one such approach. In addition, their atomic-like properties suggest the potential for Si-based quantum information processing in the single QD limit. In this work, we use colloidal PbS QDs as the active material to interact with Si PCCs with resonances near 1.55 μm. Due to the long radiative lifetime (≈ 700 ns^{8,9}) and small radiative efficiency of these dried QDs (≈ 1 %^{8,10}), as well as challenges associated with measuring low light levels with InGaAs detectors^{11}, it is of the utmost importance to collect as many emitted photons as possible. Previous studies of PbS/PbSe QDs coupled to Si microcavities^{12,13,14,15} have relied on free-space microphotoluminescence methods to pump and collect the emission from moderately high-Q cavities (Q ≈ 10^3), and have generally operated at relatively high QD densities, or else have sacrificed spectral resolution to achieve the count rates needed to operate at a lower QD density^{16}. In this work, we use an optical fiber taper waveguide^{2,17,18} to couple to the modes of high-Q PCCs (Q ≈ 10^4), thereby allowing for an efficient out-coupling mechanism for PbS QD emission. We measure photoluminescence from a low density (≲ 100 μm^{−2}) of spun QDs and show that the Q does not degrade due to QD absorption up to Q ≈ 3 × 10^4. We also measure photodarkening and saturation of the QD emission into the cavity mode. This approach may enable the future interrogation of cavity quantum electrodynamics (cQED) in the PbS/Si system, in much the same way as has been demonstrated for epitaxial III-V QDs^{19}.

The PbS QDs^{20} are chemically synthesized^{21} and suspended in chloroform. As shown in the inset of Fig. 2(a), the emission is centered near 1460 nm with a width of 100 nm due to a combination of size inhomogeneities and a large homogeneous linewidth at room temperature. The solution is further diluted with chloroform in a 1:200 mixture. Ap-

FIG. 1: (a)-(c) SEM images of the H1, L3, and MH cavities, respectively. The lattice constants in (c) are {a_1,a_2,a_3}={410 nm,415 nm,420 nm}. (d)-(f) Transmission spectrum of the H1, L3, and MH cavities before QD spin with fits (dashed). (d) and (f) were taken with the taper in contact with the cavity, while (e) was taken with the taper above the cavity. (g)-(i) Same as (d)-(f), but after QD spin. Inset to (g): SEM image of QDs in a 256 nm × 173 nm area.

proximately 20 μL is spin-coated directly onto the substrate containing PCCs, yielding an areal density of ≲ 100 μm^{−2} (inset Fig. 1(g)) as measured by a scanning electron microscope (SEM). The PCCs measured (Fig. 1(a)-(c)) are the welldeveloped H1^{22}, L3^1, and multi-heterostructure (MH) cavities^3, and have been fabricated in a 250 nm thick Si device layer using standard silicon-on-insulator fabrication methods. The devices are probed using an optical fiber taper waveguide, which can be used to measure the spectral response of the devices in transmission as well to collect photoluminescence (PL).

Transmission measurements follow the approach of Ref. 2, where light from a swept wavelength external cavity diode laser (1520 nm to 1630 nm) is sent through a variable optical attenuator and polarization controller before it is directed through the tapered optical fiber to an InGaAs photodiode.

The taper and sample separation is controlled via x,y, and z stepper stages with 50 nm resolution, and the system is imaged under a 50X microscope objective. The measurement setup rests in a N_2-rich environment at room temperature to prevent irreversible photoxidation of the QDs^{23} and taper degradation.

This technique enables resonant spectroscopy of the cavity with and without the active material. In this way, we measured the cavity Q, before and after addition of the PbS QDs. Figure 1(d)-(f) shows a cavity resonance of the H1, L3, and MH in transmission without QDs. The estimated Q (with waveguide coupling loss removed^{17,24}) values are 4900, 19 800, and 30 100 respectively. Figure 1(g)-(i) shows the cavity’s response in transmission with QDs with corresponding Q = 4500, 23 200, and 29 500. For these low QD densities, the variation in the extracted Qs due to differences in taper position is greater than the loss induced by QD absorption, at least up to Q ≈ 3 × 10^4. The ability to maintain high-Q in the presence of the QDs is promising for a number of potential applications, such as single QD cQED and low-threshold microcavity lasers.

For PL measurements, a 980 nm diode laser is coupled through a variable optical attenuator into the fiber taper, which is brought into contact with the devices. The transmitted signal is then directed through a long pass 1064 nm filter and into a grating spectrometer coupled with a liquid N_2 cooled InGaAs array. Spectra are recorded with a 180 s integration time under a typical excitation power of 100 μW. PL spectra from each cavity are shown in Fig. 2, including another mode in the MH cavity that did not appear in transmission (Fig. 2(c)). The Q factors observed in PL are consistent with those seen in transmission measurements, though our spectral resolution is limited to ≈0.09 nm. We note that the cavity modes operate on the long wavelength tail-end of the QD distribution, as seen in the reference PL spectrum shown in the inset of Fig. 2(a) for an ensemble of QDs not in a cavity. This suggests the number of QDs interacting with the cavity modes may be significantly reduced with respect to the number that physically reside in the cavity, though a measurement of the QD homogeneous linewidth is needed to confirm this.

Using the transmission measurements in Fig. 1, we can estimate the efficiency η_o with which a cavity photon out-couples into the fiber taper. A QD’s out-coupling efficiency would then be the product of η_o with the fraction of QD radiation into the cavity mode. η_o is estimated^{17,24} from the on-resonance transmission level T_{res} as η_o = (1− √ T_{res})/2 when the system is in the under-coupled regime and η_0 represents collection in transmission. For the H1 cavity in Fig. 1(g), T_{res} = 0.381 so that η_o = 19.1 %. A similar efficiency (T_{res} = 0.562, η_o = 12.5 %) has been measured when the taper is in contact with the L3 cavity (inset of Fig. 2(b)), while coupling to the MH cavity as shown in Fig. 1(i) yields a somewhat smaller value (T_{res} = 0.670, η_o = 9.07 %); fluctuations in the detected signal result in uncertainties in η_o of ≤ 0.1 %. These results generally compare favorably to calculated free-space collection efficiencies of ≈ 10 % using high numerical aperture objectives^{25}, with the added advantage of direct collection into a single mode optical fiber.

FIG. 2: Fiber-collected PL spectra for (a) H1, (b) L3, and (c)-(d) MH. Inset to (a): Room-temperature PL of an ensemble of QDs without cavity. Inset to (b): L3 transmission with taper in contact with cavity.

Our experimental configuration also enabled measurement of photodarkening behavior previously observed in PbS QDs^{23}. In this case, PL from the MH cavity is directed through long pass filters at 1064 nm and 1400 nm and detected at an InGaAs single photon counting module (SPCM)^{11} with 2.5 ns gate width, 20 % detection efficency, and 5 μs dead time. As shown in Fig. 3(a), the PL is monitored continuously with a 0.6 s integration time while the 980 nm excitation source is turned on (P_{drop} = 154.0 μW ± 9.5 μW) and off. The PL clearly decays with time and requires an off time of at least 150 s to completely recover. This kind of photodarkening has been attributed to an average of single particle blinking where the overall ensemble PL decreases with time due to increasing numbers of emitters transitioning to a longlived dark state^{26,27,28}. Fig. 3(b) shows a normalized photodarkening trace taken under the same excitation conditions as (a). The data has been fit with a stretched exponential^{28}, I(t) = I_{eq} +(1−I_{eq})exp[−(t/T_o)^α], yielding fit parameters with 95 % confidence intervals I_{eq} = 0.435 ± 0.006, T_o = 8.84 ± 0.54, and α = 0.57 ± 0.38. While the fit parameters T_o and α are consistent with literature^{28}, the actual physical parameters associated with QD blinking can only be determined with further single QD measurements beyond the scope of this work. However, I_{eq} is directly related to the ratio of average time spent in the dark state to the bright state, which for our QDs computes to a value of 1.30 ± 0.03. Short-timescale photodarkening and the difficulties associated with detection at 1.55 μm make low density QD measurements that much more challenging.

The final experiment we performed was a saturation spectroscopy measurement of the two modes of the MH cavity. In this measurement, a PL spectrum was recorded (60 s integration) as the dropped excitation power was increased over more than four decades. To avoid photodarkening effects, the excitation was blocked for 30 s after each measurement and the spectrum was taken only after the excitation had been on for 30 s. Two lorentzians were fit to each spectrum and the integrated count rate under each peak is plotted as a function of dropped power in Fig. 3(c),(d). Each of these curves was fit to

FIG. 3: (a) Continuous measurement of PL on an SPCM while the excitation is intermittently turned off and on. (b) Close-up of one of the photodarkening curves taken in (a) along with fit (dashed). (c), (d) PL saturation measurements of the modes at 1522.7 nm and 1532.1 nm in the MH cavity with fits (dashed).

a two-level saturation with an adjustable power dependence, I(P) = A[P/(P + P_{sat} )]^b. Interestingly, the saturation curves display a clear sub-linear dependence on the dropped power below saturation. The mode at 1522.7 nm (1532.1 nm) fits to a value of b = 0.518 ± 0.046 (b = 0.795 ± 0.082). This sublinear dependence could be symptomatic of the trapped states associated with blinking^{29}. The saturation curves are truncated due to heating in the tapered fiber and in the Si at excitation powers near 2 mW as evidenced by few nm redshifts of the cavity modes. Nonetheless, the saturation power can still be extracted from the data, albeit with a large uncertainty. We fit to P_{sat} = 153.2 μW ±65.3 μW (P_{sat} = 42.6 μW ±17.2 μW) for the mode at 1522.7 nm (1532.1 nm). For a single PbS QD with absorption cross-section^{30} σ = 4.59 × 10^{−16} cm^2 and room-temperature excited state lifetime of ≈ 100 ns^9, the expected saturation excitation power for our tapered fiber setup is ≈ 22 μW. Because the cross-section is so low, a nondiminished pump approximation is valid and the single particle saturation power should be accurate for small QD densities. Given the uncertainties in the fits as well as in the values for the cross-section and lifetime, the extracted saturation powers seem quite reasonable.

In conclusion, we have performed spectroscopy of 1.55 μm PbS QDs dried on Si photonic crystal cavities using a fiber taper waveguide. Future experiments will build towards single QD spectroscopy by lowering the QD density and improving the radiative efficiency by working in cryogenic conditions^9 and/or using brighter and more stable colloidal QDs^{31}. A combination of these strategies will lead to the development of novel and useful active nanophotonic devices in the telecommunications band.

The authors acknowledge fabrication support from D. L. Kwong and M. Yu at the Institute of Microelectronics in Singapore, partial funding support from NSF ECCS 0747787 and the New York State Foundation for Science, Technology, and Innovation, and useful discussion with Marcelo Davanço at NIST.

∗ Electronic address: mrakher@nist.gov † Current Address: Institute for Research in Electronics and Applied Physics, University of Maryland, College Park, MD 20742, USA 1. Y. Akahane, T. Asano, B.-S. Song, and S. Noda, Nature 425, 944 (2003).

2. K. Srinivasan, P. E. Barclay, M. Borselli, and O. Painter, Phys.

Rev. B 70, 081306R (2004).

3. B.-S. Song, S. Noda, T. Asano, and Y. Akahane, Nature Materials 4, 207 (2005).

4. A. Polman, J. Appl. Phys. 82, 1 (1997).

5. H. Park, A. Fang, S. Kodama, and J. Bowers, Opt. Express 13, 9460 (2005).

6. F. Wise, Acc. Chem. Res. 33, 773 (2000). 7. D. V. Talapin and C. B. Murray, Science 310, 86 (2005). 8. E. H. Sargent, Advanced Materials (Weinheim, Ger.) 17, 515 (2004).

9. M. T. Rakher, C. W. Wong, and K. Srinivasan, in preparation (2009).

10. J. S. Steckel, S. Coe-Sullivan, V. Bulović, and M. G. Bawendi, Advanced Materials (Weinheim, Ger.) 15, 1862 (2003).

11. G. Ribordy, N. Gisin, O. Guinnard, D. Stucki, M. Wegmuller, and H. Zbinden, Journal of Modern Optics 51, 1381 (2004).

12. I. Fushman, D. Englund, and J. Vuckovic, Appl. Phys. Lett. 87 (2005).

13. R. Bose, X. Yang, R. Chatterjee, J. Gao, and C. W. Wong, Applied Physics Letters 90, 111117 (2007).

14. Z. Wu, Z. Mi, P. Bhattacharya, T. Zhu, and J. Xu, Applied Physics Letters 90, 171105 (2007).

15. A. G. Pattantyus-Abraham, H. Qiao, J. Shan, K. A. Abel, T.-S.

Wang, F. C. J. M. van Veggel, and J. F. Young, Nano Letters 9, 2849 (2009).

16. R. Bose, J. F. McMillan, J. Gao, and C. W. Wong, Applied Physics Letters 95, 131112 (2009).

17. S. M. Spillane, T. J. Kippenberg, O. J. Painter, and K. J. Vahala, Phys. Rev. Lett. 91, 043902 (2003).

18. I.-K. Hwang, S.-K. Kim, J.-K. Yang, S.-H. Kim, S. H. Lee, and Y.-H. Lee, Appl. Phys. Lett. 87, 131107 (2005).

19. K. Srinivasan and O. Painter, Nature (London) 450, 862 (2007). 20. Purchased from Evident Technologies and identified in this paper to foster understanding, without implying recommendation or endorsement by NIST.

21. M. A. Hines and G. D. Scholes, Adv. Mater. (Weinheim, Ger.)

15, 1844 (2003).

22. O. Painter, R. K. Lee, A. Yariv, A. Scherer, J. D. O’Brien, P. D.

Dapkus, and I. Kim, Science 284, 1819 (1999).

23. J. J. Peterson and T. D. Krauss, Phys. Chem. Chem. Phys. 8, 3851 (2006).

24. P. Barclay, K. Srinivasan, and O. Painter, Opt. Express 13, 801 (2005).

25. N.-V.-Q. Tran, S. Combrié, and A. D. Rossi, Phys. Rev. B 79, 041101 (2009).

26. I. Chung and M. G. Bawendi, Phys. Rev. B 70, 165304 (2004). 27. M. Pelton, D. G. Grier, and P. Guyot-Sionnest, Applied Physics

Letters 85, 819 (2004).

28. J. Tang and R. A. Marcus, The Journal of Chemical Physics 123, 204511 (2005).

29. V. Babentsov, J. Riegler, J. Schneider, M. Fiederle, and T. Nann, J. Phys. Chem. B 109, 15349 (2005).

30. L. Cademartiri, E. Montanari, G. Calestani, A. Migliori,

A. Guagliardi, and G. A. Ozin, Journal of the American Chemical Society 128, 10337 (2006).

31. J. M. Pietryga, D. J. Werder, D. J. Williams, J. L. Casson, R. D.

Schaller, V. I. Klimov, and J. A. Hollingsworth, J. Am. Chem. Soc. 130, 4879 (2008).