arXiv:1006.1335v1 [astro-ph.IM] 7 Jun 2010

Data acquisition electronics and reconstruction software 1 for directional detection of Dark Matter with MIMAC 2 O. Bourrion^{a,∗}, G. Bosson^a, C. Grignon^a, J. L. Bouly^a, J. P. Richer^a, O. 3 Guillaudin^a, F. Mayet^a, D. Santos^a 4 aLaboratoire de Physique Subatomique et de Cosmologie, 5 Université Joseph Fourier Grenoble 1, 6 CNRS/IN2P3, Institut Polytechnique de Grenoble, 7 53, rue des Martyrs, Grenoble, France 8

Abstract 9 Directional detection of galactic Dark Matter requires 3D reconstruction of low 10 energy nuclear recoils tracks. A dedicated acquisition electronics with auto trig- 11 gering feature and a real time track reconstruction software have been developed 12 within the framework of the MIMAC project of detector. This auto-triggered 13 acquisition electronic uses embedded processing to reduce data transfer to its 14 useful part only, i.e. decoded coordinates of hit tracks and corresponding energy 15 measurements. An acquisition software with on-line monitoring and 3D track 16 reconstruction is also presented. 17

1. Introduction 18 Directional detection is a promising search strategy of galactic Dark Matter. 19 The idea is to take advantage on the rotation of the Solar system around the 20 galactic center to show a direction dependance of WIMP signals, which should 21 then be clearly discriminated from background ones [1, 2, 3, 4, 5]. Recently, a 22 statistical map-based analysis has been developed [6], showing for the first time 23 the possibility to extract from data samples of forthcoming directional detec- 24 tors, both the main direction of the incoming events, thus proving the galactic 25 origin of the signal, and the number of WIMP events contained in the map. 26 Several directional detectors are being developed and/or operated : MIMAC [7], 27 DRIFT [8], NEWAGE [9], DM-TPC [10]. A detailed overview of the status of 28 experimental efforts devoted to directional dark matter detection may be found 29 in [11]. A common issue amongst these detectors is the fact that directional 30 detection requires track reconstruction of recoiling nuclei down to low energies 31 (a few keV). This can be achieved with low pressure gaseous detectors [12] and 32 several gases have been suggested : CF_4,^3 He + C_4H_{10} or CS_2. Ideally, recoiling 33 tracks should be 3D reconstructed [4] with sense recognition [13, 14]. 34 The MIMAC (MIcro tpc MAtrix of Chambers) collaboration [7] is planning 35 to build a multi-target detector, composed of a matrix of gaseous micro-TPC 36

∗Corresponding author Email address: olivier.bourrion@lpsc.in2p3.fr (O. Bourrion) Preprint submitted to Elsevier December 24, 2018

detectors. A pixelized bulk Micromegas [15] is used in order to perform a 3D re- 37 construction of few mm tracks. It is segmented in 350 μm pixels associated to a 38 dedicated ASIC previously described [16]. Indeed, the coordinates in the anode 39 plane (x and y coordinates) are reconstructed by collecting primary electrons 40 produced in the drift region with an electric field (≤1 kV/cm) and amplified in 41 the avalanche region (20 → 80 kV/cm). The track of the recoil is thus projected 42 on the anode, providing 2D information. As stated above, 3D track reconstruc- 43 tion is needed for directional detection of dark matter. This is achieved by 44 sampling the anode signal every 25 ns. Knowing the electron drift velocity, in- 45 formation on the third coordinate is retrieved. 46 47 To demonstrate the relevance of the concept, a specific acquisition electronic 48 has been developed in order to equip a prototype detector featuring an anode 49 of 3.36 × 3.36 cm^2 where 2 × 96 strips are monitored with these ASICs. This 50 auto-triggered acquisition electronic uses embedded processing to reduce data 51 transfer to its useful part only, i.e. decoded coordinates of hit tracks and corre- 52 sponding energy measurements. To be fully exploited, an acquisition software 53 with on-line monitoring and track reconstruction has been written. 54 55 This paper is organised as follows : section 2 presents the hardware de- 56 sign, emphasizing on the front end digital interface (FPGA) implemented on 57 the acquisition board. Then the acquisition software and the 3D reconstruc- 58 tion strategy are presented in section 3. Eventually, experimental results are 59 presented in section 4. 60 2. Hardware design and architecture 61 2.1. Overview of the MIMAC acquisition board 62 As shown on figure 1, the acquisition board is composed of 12 front end 63 ASICs, 6 for each coordinate (X and Y). The data processing was split in 3 64 FPGA, one for each side and one for merging the data. The LVDS serial links 65 are directly connected to the XY FPGA, which de-serializes the ASIC com- 66 parators data. Then the XY FPGA processes each ASIC position data for 67 suppressing the zeros, decoding the coordinates and assembling them with the 68 data coming from the neighbouring ASICs. At the end of the processing, the 69 data in the first level FPGA are time sorted and placed in a data buffer (called 70 position buffer). 71 The two analogue outputs of each ASIC go through peak detectors in order to 72 find the maximum amplitude of the shaper signals. Each high gain peak de- 73 tector is equipped with a comparator whose threshold is tuned by a DAC. The 74 ADC readout is automatically performed by the XY FPGA for each group of 75 16 strips when some track has been detected and if the amplitude of the signal 76 went above the threshold. As for the position data, the energy data are time 77 sorted and placed in a data buffer. 78 At this stage, for both channels (position and energy), 2 data sources are avail- 79 able: one for the X coordinate and an other for the Y coordinate. The merger 80

Figure 1: Block diagram of the MIMAC acquisition board

FPGA is in charge of concatenating them in a time sorted way and make them 81 available for data readout. An Ethernet ready micro-controller configured as a 82 TCP socket server is used as a communication link with the acquisition com- 83 puter. It is at the same time used as the slow control interface for: 84 • remote configuration of the FPGA (this allows easy upgrades of the firmwares) 85 • tuning the energy measurement thresholds 86 • tuning the strips discriminators thresholds 87 In the following, we describe the various components of the acquisition board. 88 2.2. Front end ASICs 89 As a preliminary building block for the MIMAC (MIcro tpc MAtrix of Cham- 90 bers) framework a front ASIC was developed [16]. These chips were designed to 91 monitor 16 strips of pixels with low noise charge pre-amplifiers and to provide 92 in real time their time over threshold. 93 The comparator outputs are coupled to a data serializer with a compression 94 ratio of 8 in order to reduce consumption and connectivity. Indeed, for the 95 first phase of the MIMAC project, following this prototype phase, the goal 96 is to equip an 20 cm × 20 cm anode featuring 1024 strips). De-serializing 97 these data provides a picture of the strips of pixels at a 40 MHz rate. Then, 98 providing the electron drift velocity in the gas mixture the third coordinate of 99 the track is reconstructed by using consecutive samples of the strips of pixels. 100

The thresholds are individually tuned by 5 bit current DACs. 101 For providing a mean to measure the total energy released in the ionisation 102 channel by the incident particle, the sixteen pre-amplifier outputs are summed 103 and provided in two gains via two shapers. More details may be found in [16]. 104 2.3. Energy measurement with peak detectors 105 Each ASIC shaper output is connected to a peak detector (fig. 2) which is 106 designed to memorise the maximum amplitude when enabled. Both high and 107 low gain analogical values are digitized by ADCs when the shaper high gain 108 output goes back below the threshold programmed by a DAC (comparator part 109 not shown on fig. 2). The first stage amplifies and inverts the negative input

Figure 2: Block diagram of the peak detector used for the energy measurement. 110 signal to deliver a positive signal to the second stage. As long as this signal 111 increases, the feedback diode stays in conduction mode and the capacitor volt- 112 age follows the signal. Once the maximum amplitude is reached, i.e. when the 113 shaper signal starts to decrease, the feedback diode switches in blocking mode 114 and thus, the peak amplitude is kept in the capacitor. At this stage, the peak 115 detector amplifier toggles to non linear mode. An anti-saturation loop is imple- 116 mented in order to maintain the peak detector amplifier differential input to a 117 minimum value. Indeed one of the bipolar amplifier drawbacks is the fact that 118 they exhibit a dramatic input leakage current increase when input differential 119 voltage increases, which would compromise the analogue memorisation func- 120 tion. The reset signal is used to disable the peak search and also to discharge 121 the capacitor at the end of the conversion. Bipolar operational amplifiers were 122 chosen for implementation as it was required to work with low voltage supplies 123 and thus having rail to rail input amplifiers was mandatory. 124

2.4. Front end digital interface: XY FPGA 125 The XY FPGA^1 is composed of two parts. The first one, identical for each 126 ASIC, deserializes the data and performs the local triggering, ADC readout and 127 local data buffering. The second one is in charge of data time sorting and coor- 128 dinate decoding. 129 The deserializer is designed to allow operation with low performance FPGA by 130 using two shifters working on opposite edges at half of the incoming data fre- 131 quency (figure 3). The sampling phase is adjusted by setting the DCM (Digital 132 Clock Manager provided in Xilinx FPGAs) to the appropriate value by slow 133 control. 134 The ASIC management is detailed on figure 4. The deserializer first provides

Figure 3: Block diagram of the low cost deserializer 135 data for the local triggering (an OR of the 16 channels), when a trigger is found, 136 a copy of the free running time counter is inserted in the raw position memory, 137 meanwhile the strip data are delayed by one clock cycle to allow this. After the 138 time count is written in the memory, the strip data are pushed in the memory 139 while the stop condition is not fulfilled. Experimental results show that primary 140 electron distribution can be non continuous and therefore strips can be untrig- 141 gered for a short amount of time. The stop condition is therefore no trigger on 142 the monitored channel for more than n clock cycles. This value can be adjusted 143 by slow control. 144 The memory depth is a key issue. It has to be dimensioned in order to cope 145 with long tracks like alpha particle, because readout is performed at a much 146 slower speed than the memory writing. For instance, in^3He at 350 mbar the 147 drift speed is 16 μm/ns, so an alpha particle arriving orthogonally to the anode 148

1so called because the processing is identical on the X and Y side

Figure 4: Block diagram of the ASIC management logic

will use

15 cm 16 μm/ns

× 40 MHz ≃ 375 memory cells. Then, each position word in 149 memory can potentially be decoded as 16 valid positions. The memory blocks 150 used in the FPGA are several times larger than this value. 151 The trigger is also used by the energy measurement channel. When detected, 152 the ADC readout system saves the trigger date and waits until a peak is de- 153 tected within a predefined time limit (shaping time). If none is detected, a null 154 value is inserted in the energy memory in order to keep raw position memory 155 and raw energy memory aligned and facilitate later reconstruction. The raw 156 energy memory is smaller, because for a full particle track only one amplitude 157 will be coded in two gains. Distributed RAM is sufficient for this task. 158 Once all data are stored in local buffers, the next step is to assemble them with 159 the data originating from other ASICs. This operation is done by Finite State 160 Machine (FSM), like the one used for sorting the position data (figure 5). The 161 only difference with the one used for sorting the energy data is the position 162 decoding (scan word state), each bit at one in position word is decoded as a 163 strip number. Starting from the idle state, the FSM waits for the first ASIC 164 (or group) to present data. When it is the case, the current date is saved and 165 the position decoding is performed. Then the FSM looks if an other group 166 presents position data marked with the same date, if yes the data are decoded 167 and appended to the output buffer in the same time slot, if not the time slot is 168 closed and the search for a new time slot continues. At this stage, 2 possibilities 169 remain: 170 • no more data are available and the FSM returns to IDLE 171

• data are still available and the earliest data has to be found 172 For that, a scan of the dates is made (seek next group) in order to find the 173 first ASIC in time. This scanning is complexified by the fact that the time 174 counter has a short span (13 bit which corresponds to ∼1.31 ms), therefore it is 175 performed in 2 stages. First the search is performed from the current date up 176 to the maximum counter value, and if not successful, the current date is set to 177 zero and the searching is performed again until the group is found (check roll 178 over state). 179 Position data and energy data are stored in separate buffers (see template in 180 table 1). Both tables are organised in order to optimize bit usage and therefore 181 data are encoded on 16 bit. For a specific time-stamp, all useful position or 182 energy data are grouped under a unique TAG. The time slice is closed by the 183 End of TAG label. 184 bit 15 14 13 12 11 10 9 8 7 6 5 4 3 2 1 0 TAG 0 date position DATA n 1 0 ASIC # strip # energy DATA n 1 0 ASIC # ADC value End of TAG 1 1 unused

Table 1: Organisation of the 16 bit words containing position or energy information.

2.5. FPGA merger 185 This FPGA is in charge of merging the data from the X and Y side. For 186 this task, it is working similarly to the sorting FSM of the XY FPGA, the only 187 difference being the fact that only 2 data producers are managed instead of 188 6. Once the data are processed, they are stored in large buffers. They can be 189 accessed directly for readout by the Ethernet micro-controller. Also, being the 190 direct interface with the micro-controller, it is used as the slow control interface 191 for: 192 • Enabling or disabling an ASIC 193 • Activating the calibration mode. In this mode a constant pattern is sent 194 by the ASICs and for reducing the data amount, only one out of 65536 195 triggers is accepted. 196 • Configuring the energy channel thresholds 197 2.6. Ethernet interface 198 This interface is based on a 32 bit micro controller, using a flash memory 199 and 16 MB of SDRAM. Its purpose is to provide an easy computer interface 200 and to test the possibility for multi chamber acquisition. 201

At power up, a TCP socket server service is started and the acquisition computer 202 (the client) can open a socket and communicate with the hardware via a custom 203 protocol. It is used for slow control and acquisition, they are implemented in 2 204 threads. When in run mode, the acquisition thread is resumed and start polling 205 the empty flags of the position and energy buffers, once a non empty flag is 206 found, the corresponding fifo level is read. Then the appropriate number of 207 readout is made and the data are transmitted through the socket with a header 208 specifying the data type and count. 209 In order to allow flexibility and easy prototyping, the micro-controller firmware 210 is the only one resident on the electronic board and the 3 FPGA are remotely 211 reconfigured at each start up via the TCP socket. 212 3. Acquisition software 213 The acquisition software was developed in C++ and coded to allow operation 214 on Linux and Windows platforms. In order to keep a good separation between 215 functionalities, it is built with three different parts as described below. 216 3.1. Software driver 217 The low level driver is in charge of providing low level functions for con- 218 trolling the hardware and managing the acquisition. It features a platform 219 independent non blocking socket client manager, routine for reading FPGA 220 configuration file and remotely configuring them, methods for interpreting po- 221 sition and energy threshold files and set DAC values. 222 For a proper tuning of the serializers sampling phase, a scanning algorithm is 223 also provided. Basically, it puts the hardware in calibration mode (in order 224 to significantly decrease the trigger rate), validate one ASIC at a time and try 225 every possible value of de-phasing (256 values) and record the results of the 226 reception of a known test pattern. The test pattern is supposed to be received 227 correctly many thousand times in order to consider that the sampling phase 228 is correct for the selected ASIC. When the stability range common to the 12 229 ASICs has been determined, the mean value is computed and transferred to the 230 XY FPGA. 231 The data acquisition has to be performed with a blocking call method (returns 232 only when the required number of bytes are read or when a time out occurs). 233 This function reads data frame received from the socket and separates them be- 234 tween energy and position. They are then pushed in 2 STL (Standard Template 235 Library) queues. The readout is performed this way, because the electronic pro- 236 cessing time from particle interaction to data available in computer varies with 237 energy and position data path. 238 3.2. Acquisition thread and event building 239 The acquisition is performed in a thread loop, with the software driver and 240 Qt framework [17]. The algorithm of the event building is depicted on figure 241 6. When the thread is awaken, it starts looping on the data readout method 242

provided by the software driver. As soon as both position and energy queues 243 are not empty any more the event building processing part starts. 244 In order to properly assemble an event, the position queue is processed first in 245 order to find out when it starts and when it stops. All triggered strips with 246 dates separated by less then the allowed number of empty clock ticks are kept 247 as member of the same event. But as soon as the date of the currently processed 248 triggered strips jumps from more than the allowed number of clock ticks, it is 249 considered to be a member of the next event and the current event position 250 retrieval is finished. At this stage the event start date and duration are known 251 and the corresponding energy data may be found in the energy queue. In other 252 word, the continuous triggering of the anode defines an event. 253 254 3.3. Individual strip threshold calibration 255 In order to operate correctly a MIMAC prototype equipped with the ASIC 256 described, each strip threshold has to be properly tuned. This task would be 257 cumbersome if not automated, especially when the aim is to monitor 1024 strips 258 per chamber. Therefore an automated calibration method was developed and 259 tested with the prototype. 260 The procedure is to shut down all high voltage applied to the chamber in order 261 to have no real events and to try to find the best DAC setting that will put the 262 thresholds just above noise. This is done by running short acquisitions (∼ 15 s) 263 with each settings until the good one is found. 264 First the calibration algorithm will start with all thresholds set at their maxi- 265 mum values and try to decrease them as long as each individual strip doesn’t 266 trigger (all strip thresholds are tuned at the same time). When a strip has 267 reached its lowest threshold, it is marked as such. But since there is some 268 crosstalk on the board, a second phase is necessary. It has been observed that, 269 when other thresholds lower, some noise is generated on the acquisition board 270 and picked again by the strips whose threshold were marked as tuned. So in the 271 second step, the threshold is increased, one digit at a time, until the triggering 272 is stopped. The chamber is declared calibrated when all strip thresholds are 273 marked as having reached their minimum value and no more trigger is counted 274 in the acquisition. 275 3.4. Graphical interface and event display 276 As stated above, the readout is performed in 2D with strips of pixels, which 277 means that an event is considered as valid if, for a given time slot, at least one 278 strip of pixels in each dimension (X and Y) is fired. When such a coincidence 279 happens, the position of the fired pixels can be evaluated as the intersection of 280 the fired X strips and Y strips. Each time slot gives access to a 2D slice of the 281 track, and each slice following each other will lead to a 3D track. 282 Once an event is built by the 3D reconstruction algorithm, it has to be 283 displayed with a visualization software both in online and offline modes. This 284 real-time visualisation software allows to monitor several parameters of the de- 285 tector during a run, such as the energy deposit, the position of the interaction 286

and the length of the track. Real-time access to these information offers the 287 possibility to adjust the detector parameters, such as the gas pressure, anode 288 and micro-mesh voltages or the electronic thresholds in order to reach optimized 289 working conditions during an acquisition run. Furthermore, the event display 290 software enables the testing and debugging of the reconstruction software and 291 the analysis strategy in an offline mode. 292 To meet these specifications, a visualization tool mainly based on the Qt [17] 293 and ROOT [18] framework was developed. Qt offers a well documented user 294 interface framework implemented in C++. A third interface layer nammed “Qt 295 layer” [19] was used to build the application software. 296 The user interface of the online software is segmented in several tabs: 297 • one dedicated only to acquisition process: automated calibration, start/stop 298 runs 299 • another tab displays the energy spectrum (both in low and high gain) in 300 real time 301 • Event display, used also in offline mode, provides projection of the 3D 302 track 303 As shown on figure 7, the main canvas of the event display panel is segmented 304 in 4 panels: 305 • the top left panel represents a 2D view of the event, as seen by the anode 306 (XY projection) 307 • the top right panel shows the evolution of the number of fired strips versus 308 time, for the X side (solid line curve) and the Y side (dashed line curve) 309 • the bottom pads represent projections of the track on the XZ plane (left 310 panel) and YZ plane (right panel) 311 Event by event display of the projected 3D track (XY, XZ and YZ his- 312 tograms) is provided by the visualisation software. Whether in online or offline 313 mode, the list of event to display can be adjusted through several criterion like: 314 number of images (equivalent to length along Z axis), energy deposit or even a 315 combination of those. 316 4. Experimental results of the MIMAC Data AcQuisition 317 As required by the specifications, the MIMAC DAQ is able to reconstruct 318 3D tracks of nuclear recoils and electrons between a few keV and hundreds of 319 keV. 320 First experimental results were obtained with a 5.9 keV X-ray source (^{55}Fe) 321 producing 5.9 keV electrons in a 350 mbar^4He + 5% C_4H_{10} mixture used as 322 detection medium. These electron tracks (figure 9) have a specific length over 323 energy ratio and will be typical background events in the final MIMAC dectector 324 designed to detect dark matter in an underground laboratory. 325

Ultimately, the goal of MIMAC is to reconstruct recoil tracks of nuclei in 326 3D. In order to test the MIMAC prototype associated to the dedicated ac- 327 quisition electronics with nuclei recoils, the detector was placed in front of a 328 mono-energetic neutron beam at the Amande facility [20]. Depending on the 329 target gas used, recoils of hydrogen ions, helium ions or event fluorine ions were 330 reconstructed [21]. 331 For instance, on figure 8, a 100 keV proton recoil obtained in a 350 mbar 332 4He + 5% C_4H_{10} mixture is displayed in three dimensions. Left panel presents 333 the raw 3D track, ie images of the anode in each z slice. Right panel presents 334 the barycentre of each z slice. This shows the possibility to achieve 3D track 335 reconstruction of recoiling nuclei in low pressure gaseous TPC. Figure 9 presents 336 the same views of 5.9 keV electrons, highlighting the possibility to reach low 337 energies with this technique. This last event is of crucial interest as it features a 338 typical background event for Dark Matter search. A comprehensive study of an- 339 gular resolutions obtained with this 3D reconstruction method will be presented 340 in a forthcoming paper [22]. This dedicated acquisition electronics associated 341 with 3D reconstruction software offers a major breakthrough towards 3D recon- 342 struction of low energy tracks, thus opening great opportunities for directional 343 Dark Matter search [21]. 344 5. Conclusion 345 A dedicated acquisition electronics with auto triggering feature and a real 346 time track reconstruction software have been developed within the framework 347 of the MIMAC project of detector. It has been shown by experimental results, 348 that the MIMAC ASIC [16], the prototype acquisition board (fig. 10) and soft- 349 ware coupled together offer great possibilities for 3D track reconstruction and 350 ultimately for directional dark matter detection. 351 352 Acknowledgement 353 C.G. and the MIMAC collaboration acknowledge the ANR-07-BLAN-0255- 354 03 funding. 355

Figure 5: Description of the finite state machine (FSM) used for position data sorting

Figure 6: Event building algorithm embedded in the acquisition thread

Figure 7: Snapshot of the event display tab of the MIMAC real-time visualization software. Top left panel represents a 2D view of the event, as seen by the anode (XY projection). Top right panel shows the evolution of the number of fired strips versus time, for the X side (solid line curve) and the Y side (dashed line curve). Bottom pads represent projections of the track on the XZ plane (left panel) and YZ plane (right panel)

Figure 8: 100 keV H recoil in a 350 mbar^4He + 5% C_4H_{10} mixture: left panel represents the raw 3D track while the right panel shows barycentres of each time slice

Figure 9: 5.9 keV electron recoil in a 350 mbar^4He + 5% C_4H_{10} mixture (barycentre on the right panel)

Figure 10: Picture of the 260 mm × 246 mm MIMAC acquisition board. Ethernet interface board and connectors are missing on this view. X side of the dectector is connected on the top connector and Y side on the bottom one. The 2 × 6 ASIC are fed by the connectors. In the middle the 3 FPGA perform the processing.

References 356 [1] D. N. Spergel, Phys. Rev. D 37 (1988) 1353 357 [2] B. Morgan, A. M. Green and N. J. C. Spooner, Phys. Rev. D 71 (2005) 358 103507 359 [3] B. Morgan and A. M. Green, Phys. Rev. D 72 (2005) 123501 360 [4] A. M. Green and B. Morgan, Astropart. Phys. 27 (2007) 142 361 [5] A. M. Green and B. Morgan, Phys. Rev. D 77 (2008) 027303 362 [6] J. Billard et al., arXiv:0911.4086 363 [7] D. Santos et al., J. Phys. Conf. Ser. 65 (2007) 012012 364 [8] G. J. Alner et al., Nucl. Instr. Meth. A 555 (2005) 173. 365 [9] K. Miuchi et al., Phys. Lett. B 654 (2007) 58 366 [10] G. Sciolla et al., J. Phys. Conf. Ser. 179 (2009) 012009 367 [11] S. Ahlen et al., Int. J. Mod. Phys. A 25 (2010) 1 368 [12] G. Sciolla and C. J. Martoff, New J. Phys. 11, 105018 (2009) 369 [13] D. Dujmic et al., Nucl. Instrum. Meth. A 584 (2008) 327 370 [14] S. Burgos et al., arXiv:0809.1831 371 [15] Y. Giomataris et al., Nucl. Instr. and Meth. A560 (2006) 405 372 [16] J. P. Richer et al., arXiv:0912.0186, to appear in Nucl. Instr. Meth. A, 373 doi:10.1016/j.nima.2010.04.041 374 [17] Qt framework, http://qt.nokia.com/ 375 [18] ROOT, an object-oriented data analysis framework. 376

http://root.cern.ch/

377 [19] V. Fine, Nucl. Instr. and Meth. A502 (2003) 681-683, 378

http://root.bnl.gov/

379 [20] A. Allaoua et al., Radiat. Meas. 44 (2009) 755-758 380 [21] D. Santos et al., in preparation 381 [22] C. Grignon et al., in preparation 382