arXiv:1201.0002v1 [astro-ph.IM] 25 Dec 2011

New air fluorescence detectors employed in the Telescope Array experiment

H. Tokuno^{a,∗}, Y. Tameda^b, M. Takeda^b, K. Kadota^c, D. Ikeda^b, M. Chikawa^d, T. Fujii^e, M. Fukushima^{b,f}, K. Honda^g, N. Inoue^h, F. Kakimoto^a, S. Kawana^h, E. Kido^b, J. N. Matthews^i, T. Nonaka^b, S. Ogio^e, T. Okuda^e, S. Ozawa^j, H. Sagawa^b, N. Sakurai^e, T. Shibata^b, A. Taketa^k, S. B. Thomas^i, T. Tomida^g, Y. Tsunesada^a, S. Udo^l, T. Abu-zayyad^i, R. Aida^g, M. Allen^i, R. Anderson^i, R. Azuma^a, E. Barcikowski^i, J.W. Belz^i, D.R. Bergman^i, S.A. Blake^i, R. Cady^i, B.G. Cheon^m, J. Chiba^n, E.J. Cho^m, W.R. Cho^o, H. Fujii^p, T. Fukuda^a, D. Gorbunov^q, W. Hanlon^i, K. Hayashi^a, Y. Hayashi^e, N. Hayashida^l, K. Hibino^l, K. Hiyama^b, T. Iguchi^a, K. Ikuta^g, T. Ishii^g, R. Ishimori^a, D. Ivanov^{i,r}, S. Iwamoto^g, C.C.H. Jui^i, O. Kalashev^q, T. Kanbe^g, K. Kasahara^j, H. Kawai^s, S. Kawakami^e, H.B. Kim^m, H.K. Kim^o, J.H. Kim^m, J.H. Kim^t, K. Kitamoto^d, K. Kobayashi^n, Y. Kobayashi^a, Y. Kondo^b, K. Kuramoto^e, V. Kuzmin^q, Y.J. Kwon^o, S.I. Lim^v, S. Machida^a, K. Martens^f, J. Martineau^i, T. Matsuda^p, T. Matsuura^a, T. Matsuyama^e, I. Myers^i, M. Minamino^e, K. Miyata^n, H. Miyauchi^e, Y. Murano^a, T. Nakamura^u, S.W. Nam^v, M. Ohnishi^b, H. Ohoka^b, K. Oki^b, D. Oku^g, A. Oshima^e, I.H. Park^v, M.S. Pshirkov^w, D. Rodriguez^i, S.Y. Roh^t, G. Rubtsov^q, D. Ryu^t, A.L. Sampson^i, L.M. Scott^r, P.D. Shah^i, F. Shibata^g, H. Shimodaira^b, B.K. Shin^m, J.I. Shin^o, T. Shirahama^h, J.D. Smith^i, P. Sokolsky^i, T.J. Sonley^i, R.W. Springer^i, B.T. Stokes^i, S.R. Stratton^{i,r}, T. Stroman^i, S. Suzuki^p, Y. Takahashi^b, M. Takita^b, H. Tanaka^e, K. Tanaka^x, M. Tanaka^p, G.B. Thomson^i, P. Tinyakov^{q,w}, I. Tkachev^q, S. Troitsky^q, K. Tsutsumi^a, Y. Tsuyuguchi^g, Y. Uchihori^y, H. Ukai^g, G. Vasiloff^i, Y. Wada^h, T. Wong^i, M. Wood^i, Y. Yamakawa^b, H. Yamaoka^p, K. Yamazaki^e, J. Yang^v, S. Yoshida^s, H. Yoshii^z, R. Zollinger^i, Z. Zundel^i

aTokyo Institute of Technology, Meguro, Tokyo, Japan bInstitute for Cosmic Ray Research, University of Tokyo, Kashiwa, Chiba, Japan cTokyo City University, Setagaya-ku, Tokyo, Japan

∗Corresponding author. Tel.: +81-357342462, Fax: +81-357342756. E-mail address: htokuno@cr.phys.titech.ac.jp (H. Tokuno).

Preprint submitted to Nuclear Instruments and Methods in Physics Research Section AFebruary 1, 2020 dKinki University, Higashi Osaka, Osaka, Japan eOsaka City University, Osaka, Osaka, Japan fUniversity of Tokyo, Institute for the Physics and Mathematics of the Universe, Kashiwa, Chiba, Japan gUniversity of Yamanashi, Interdisciplinary Graduate School of Medicine and Engineering, Kofu, Yamanashi, Japan hSaitama University, Saitama, Saitama, Japan iUniversity of Utah, High Energy Astrophysics Institute, Salt Lake City, Utah, USA jWaseda University, Advanced Research Institute for Science and Engineering, Shinjuku-ku, Tokyo, Japan kEarthquake Research Institute, University of Tokyo, Bunkyo-ku, Tokyo, Japan lKanagawa University, Yokohama, Kanagawa, Japan mHanyang University, Seongdong-gu, Seoul, Korea nTokyo University of Science, Noda, Chiba, Japan oYonsei University, Seodaemun-gu, Seoul, Korea pInstitute of Particle and Nuclear Studies, KEK, Tsukuba, Ibaraki, Japan qInstitute for Nuclear Research of the Russian Academy of Sciences, Moscow, Russia rRutgers University, Piscataway, USA sChiba University, Chiba, Chiba, Japan tChungnam National University, Yuseong-gu, Daejeon, Korea uKochi University, Kochi, Kochi, Japan vEwha Womans University, Seodaaemun-gu, Seoul, Korea wUniversity Libre de Bruxelles, Brussels, Belgium xHiroshima City University, Hiroshima, Hiroshima, Japan yNational Institute of Radiological Science, Chiba, Chiba, Japan zEhime University, Matsuyama, Ehime, Japan

Abstract

Since 2007, the Telescope Array (TA) experiment, based in Utah, USA, has

been observing ultra high energy cosmic rays to understand their origins.

The experiment involves a surface detector (SD) array and three fluores-

cence detector (FD) stations. FD stations, installed surrounding the SD

array, measure the air fluorescence light emitted from extensive air showers

(EASs) for precise determination of their energies and species. The detec-

tors employed at one of the three FD stations were relocated from the High

Resolution Fly’s Eye experiment. At the other two stations, newly designed detectors were constructed for the TA experiment. An FD consists of a primary mirror and a camera equipped with photomultiplier tubes. To obtain the EAS parameters with high accuracies, understanding the FD optical characteristics is important. In this paper, we report the characteristics and installation of new FDs and the performances of the FD components. The results of the monitored mirror reflectance during the observation time are also described in this report.

Keywords: Ultra high energy cosmic rays, Extensive air showers, Air fluorescence light detectors

1. Introduction 1 The Telescope Array project is a collaboration with 120 scientists from 2 four nations (Japan, USA, Korea, and Russia), with the observatory located 3 in Utah, USA [1, 2]. The detectors involved in the Telescope Array experi- 4 ment consist of surface detectors (SDs) arranged in an array and fluorescence 5 detector (FD) telescopes. Fig. 1 shows the detector map (squares: SD po- 6 sitions, triangles: FD station positions). The SD array consists of 507 SDs, 7 arranged over an area of approximately 700 km^2 with 1.2 km spacing be- 8 tween the SDs [4]. The SDs measure the arrival timing and particle densities 9 of extensive air showers (EASs) using two-layered plastic scintillators of 3 m^2. 10 Three FD stations are placed around the SD array. The FDs measure the 11 air fluorescence light emitted from EASs; the FD data are analyzed and the 12 longitudinal development of EASs is reconstructed to estimate primary en- 13 ergies, arrival directions, and particle species with the aim of studying the 14

nature of ultra high energy cosmic rays. 15 The FD station near the northwest corner of the SD array houses fourteen 16 FDs that were relocated from the High Resolution Fly’s Eye (HiRes) experi- 17 ment (e.g. [3]). For these FDs and for the data obtained using these FDs, we 18 can use the same calibration and analysis methods used in the HiRes experi- 19 ment [5]. The specifications, configurations, and calibrations of the relocated 20 FDs can be obtained from previous reports on HiRes (e.g. [3]). On the other 21 hand, the southeast (BRM) and southwest (LR) FD sites have twelve FDs 22 each; these FDs were newly designed for the TA experiment. A picture of 23 the FD station is shown in Fig. 2. 24 An FD consists of a primary mirror and a photomultiplier tube (PMT) 25 camera. We employed a spherical mirror to obtain a wide field of view (FOV) 26 with a sufficient focusing power. In addition, the size of the collecting area 27 of the mirror was determined from the maximum distance for detectable 28 EASs at the highest energies. The mirror aperture and curvature radius 29 were determined to be 3300 mm (area of 6.8 m^2) and 6067 mm, respectively. 30 This setting realizes the detection of EASs with a sufficiently high accuracy 31 from a distance of 30 km and with the primary energy of 10^{20} eV. 32 A primary mirror is segmented into eighteen small hexagonal mirrors; 33 the distance between the parallel sides of the hexagonal mirror was 660 mm. 34 A PMT camera consisting of 16×16 PMTs and having an effective area of 35 860 mm × 992 mm is set at a distance of 3000 mm from the mirror. The FOV 36 of each PMT is approximately 1^∘, and that of the camera is 15^∘ in elevation 37 and 18^∘ in azimuth. Fig. 3 shows a schematic view of the FD telescope 38 frame equipped with a pair of telescopes, one each in the upper and lower 39

parts of the frame. The heights of the upper and lower mirror centers and 40 the upper and lower camera centers from the floor are 5.5, 1.5, 6.0, and 41 2.8 m, respectively. The FOV centers of the upper and lower telescopes are 42 at elevations of 10.5^∘, and 25.5^∘, respectively. As shown in Fig. 3, no segment 43 mirror is installed at the center of the primary mirror. At this position, a 44 jig was mounted for alignment of the optical system of the telescope when it 45 was constructed. Similarly, during normal operations, a UV light flasher is 46 mounted here as a standard light source for the calibrations and adjustments 47 of PMT gains [6]. The projected view of the FD station onto the station 48 floor is shown in Fig. 4. The station has six telescope frames; accordingly, 49 the FOV of a station is from 3^∘ to 33^∘ in elevation and 108^∘ in azimuth. 50 To evaluate the accuracies of the measured shower parameters such as 51 arrival direction, primary energy, and longitudinal development, studies of 52 resolutions and systematic uncertainties of FD telescope optics are impor- 53 tant. Thus, we ensured that we accurately manufactured, constructed, and 54 installed the FD telescopes with utmost care and after confirmation of their 55 optical characteristics. 56 In this paper, we describe the elements that constitute an FD telescope 57 and the installation process of the telescopes. Moreover, the reflectance of 58 segment mirrors, which are continuously monitored after the installations, 59 is also presented. The contents of this paper are as follows. In Sec. 2 and 60 Sec. 3, we report the designs and productions of the PMT cameras and those 61 of the segment mirrors, respectively. Sec. 4 explains the installation of the 62 cameras and mirrors. Mirror reflectance and its variations are described in 63 Sec. 5. 64

2. Camera production 65 In this section, we describe the configuration of the newly designed PMT 66 cameras and the results of user acceptance tests. 67 2.1. Photomultiplier tube 68 Each camera has 256 PMTs. 7000 PMTs including spares have been 69 produced. The PMT used in the TA experiment, Hamamatsu R9508 based 70 on R6234-01, is specially manufactured for the experiment. The photoelectric 71 surface on the top of a tube is hexagonal in shape with a distance of 60 mm 72 between the parallel side; its effective area is equivalent to that of circle of 73 57 mm diameter [6]. On the bottom of the tube, a printed circuit board of a 74 bleeder and a preamplifier is installed. In order to reduce the contamination 75 of the night sky background photons into fluorescence signals, we use a 4 mm 76 thick optical filter (SCHOTT AG, BG3). The filter is mounted on the surface 77 of each PMT using a self-fusing tape (Hitachi Chemical Co., Ltd., HIGHBON 78 TAPE No.2) and a polyimide film tape (3M, 5434). The transmittance of 79 BG3 is higher than 80% in the wavelength range of 305−395 nm, which is 80 within the range of all the major air fluorescence lines [6]. 81 The PMTs were inspected by the supplier before shipping and were se- 82 lected based on their cathode and anode sensitivities, dark current, and other 83 basic parameters. In addition, the quantum efficiency (including collection 84 efficiency), and cathode uniformity were measured for sampled PMTs, once 85 for 1000 PMTs. We also imposed sufficiently high gains and low noise levels 86 on PMTs at the experimental sites. The minimum required gain was 6×10^4 87 with the maximum applied high voltage of −1200 V. 88

After installation of camera, we adjusted PMT gains to absolutely cali- 89 brated PMTs [7] and measured the uniformity of the PMT response at its 90 photoelectric surface on the sites [6]. During FD observations, each PMT 91 gain was monitored every one hour using UV flashers. We exchanged two of 92 the 6144 PMTs because the gains of these two PMTs had decreased in the 93 first half year. Since then, no PMT has been exchanged. 94 2.2. Camera 95 A PMT camera has been placed at the primary focus of each FD telescope. 96 Fig. 5 shows the schematic view of the PMT camera. The camera has a UV 97 transparent acrylic window (KURARAY, PARAGLAS-UV00) attached in 98 front of PMTs for protection from dust. The transmittance of the window 99 is more than 90% in the wavelength range of 300−400 nm [6]. PMTs were 100 fixed on a 16 mm thick plate of extra super duralumin and were arranged on 101 a triangular grid with a clearance gap of approximately 1 mm among them. 102 The gap geometries were measured based on the uniformity of the camera 103 surface response [6]. 104 Signals from the PMTs and the DC power to the PMTs are transferred 105 through shielded LAN cables of category 5 (length: 50−100 cm) between the 106 PMTs and the patch panels inside a camera. The patch panels connected 107 to the LAN cables are shown in Fig. 6. We use a shielded 40 core twisted 108 pair cable (Bando Densen Co., Ltd., BIOS-A-2820P) each for sixteen PMTs 109 to transfer the PMT signals from the patch panels in a camera to a data 110 acquisition (DAQ) system in the electronics room with temperature control, 111 situated 20 m from the camera location. The cable length for the upper and 112 lower cameras is 25.5 m and 22.3 m, respectively. Detailed descriptions of 113

the electronics and DAQ system are presented elsewhere [8, 9]. 114 High voltages (HVs) are applied to PMTs via coaxial cables (Bando 115 Densen Co., Ltd., 1.5D-2V) using an order-made power supply (Takasago 116 Co., Ltd.). The power supply has 256 outputs, and HV value on each out- 117 put can be controlled and monitored separately through Ethernet, with the 118 accuracy of ±0.2%. This uncertainty corresponds to approximately ±2% 119 of the PMT gains under our setting. The typical applied HV to PMTs is 120 −880 V, and the rated maximum voltage is −1200 V. As a safety measure 121 to protect human beings, PMTs, and the power supply, the power supply is 122 automatically shut down when unusually high values are detected. 123 A DC power supply (KENWOOD, PW18-3AD) is connected to two patch 124 panels to distribute DC voltage of ±5 V to the 256 preamplifiers, each con- 125 nected to one PMT. In this manner, we prepared one DC power supply for 126 each camera. 127 3. Segment mirrors and their production 128 In this section, we describe the specifications of the segment mirrors em- 129 ployed in the new FD telescopes of the TA experiment, their pre-shipment 130 and acceptance inspections, and the inspection results. 131 3.1. Segment mirrors 132 The 3.3 m aperture spherical mirror of the FD telescope is segmented into 133 eighteen small mirrors, as shown in Fig. 3. The mirror is made of borosilicate 134 glass (SCHOTT AG, TEMPAX), and each segment is hexagonal in shape 135 with a thickness of 10.5 mm and a distance of 660 mm between the parallel 136 sides. On the surface of the mirror was deposited a 200 nm thick reflection 137

coating of aluminum through vacuum deposition, and on this coating was 138 deposited a 50 nm thick protective coating of Al_2O_3 through anodization 139 process. The wavelength that induces maximum reflectance depends on the 140 thickness of the anodized coating. This thickness was optimized to obtain 141 the maximum reflectance at wavelength of 350 nm. 142 The optical parameters and fabrication accuracies of segment mirrors de- 143 pend on the experimental requirement. In order to optimize the optical 144 parameters, we studied the reconstruction accuracies of EASs using ray- 145 tracing, EAS simulation, and reconstruction programs. From our studies, 146 we determined the specifications of the optical parameters and the fabrica- 147 tion accuracies; the curvature radius of the segment mirror was 6067 mm 148 ±100 mm, the spot size at the focal point was smaller than 40 mm (it is 149 comparable size of the PMT surface), and the reflectance in the wavelength 150 range of 300 nm−400 nm was more than 85%. 151 3.2. Segment mirror production 152 Segment mirrors were manufactured (Sanko Seikohjyo Co., Ltd.) from 153 January to November, 2004, for the BRM station and from March to De- 154 cember, 2006, for the LR station. In all, 500 segment mirrors, including 155 spares, were produced. The procedure for mirror production is as follows. 156 First, the segment mirror was shaped by heating a planar glass on a ceramic 157 model plate in a temperature-controlled electric oven. After this spherical 158 mirror fabrication, the mirrors were selected through curvature radius mea- 159 surement. Next, the mirror surface was coated with 200 nm thick aluminum 160 through the vacuum deposition. To protect the surface, 50 nm thick Al_2O_3 161 crystal layer was coated on it; these Al_2O_3 crystals were produced from a 162

solution containing ammonium hydroxide, tartaric acid, and ethylene glycol. 163 After the surface fabrication, the mirrors were selected based on reflectance 164 measurement. Finally, a 150 mm diameter support disk made of the same 165 material as the mirror and a stainless steel flange were bonded to the back 166 of the mirror using glue (3M, Dymax 840). The flange was used to support 167 the segment mirror from the telescope frame. 168 3.3. Acceptance test for curvature radius and spot size 169 For the acceptance inspections, we measured the curvature radius and 170 spot size at the curvature center. From our ray-tracing studies, we estimated 171 an acceptable spot diameter of 20 mm, in which 90% of the reflected photons 172 fall, at the center of the curvature. Because of this phenomenon, parallel 173 incident light makes a spot of 40 mm diameter on the camera, in which 68% of 174 reflected photons fall, in the case of a normal FD observation. We developed 175 a test system to measure the curvature radius of mirrors as the distance 176 corresponding to the minimum spot size. Fig. 7 shows the schematic view 177 of the system, and Fig. 8 shows the photograph of the same. This system 178 consisted of a linear precision motion stage (range: ±250 mm, accuracy: 179 0.04 mm, Chuo Precision Industrial Co.,Ltd., MM STAGE ALS-250-C2P 180 with controller QT-CD1); a diffused light source, i.e., a green laser (Kochi 181 Toyonaka Giken Co.,Ltd., GLM-D2) with a diffuser plate; an image scanner 182 (range: 16 bit, resolution: 2400−4800 dpi, Canon, CanoScan LiDE80); and a 183 laser distance meter (accuracy: ±1 mm, Murakami Giken, DIST pro^4a). The 184 diffused light source was set 100 mm away from the optical axis of the mirror, 185 and the center of the scanner’s sensitive area was fixed at the axisymmetrical 186 point to the optical axis. Both the light source and the scanner were mounted 187

on the motion stage and were collectively moved between 6067 ±100 mm from 188 the center of the mirror in 5 mm steps. Next, we determined the curvature 189 radius by searching for the point where the spot size was minimized. From our 190 ray-tracing calculations, we confirmed that the spot size of the light reflected 191 on the scanner was minimized at the same distance as the curvature radius 192 in spite of the off-axis alignments of the light source and the scanner. 193 A typical observed spot image is shown in Fig. 9. In this analysis, the 194 image size was defined as the diameter of the circle in which 90% of the 195 detected photons fall; this circle was centered at the weighted center of the 196 image. Circles in Fig. 10 show an example relation between the spot size 197 and the distance from a mirror. From the data points (circles) in Fig. 10, we 198 obtain the curvature radius to be 6082 mm. Typically, as shown in Fig. 9, 199 the image shape was non ideal circle, because the surface of the mirrors 200 was slightly elliptical. Accordingly, we required an additional criterion for 201 elliptical mirrors. We also measured spot sizes of elliptical mirrors as follows. 202 First, we fitted a shot image at the beginning of a distance of 5967 mm 203 with a line (called X axis), and another line (called Y axis) was obtained 204 perpendicular to the X axis. These axes were fixed during the subsequent 205 calculations. The shot image was projected on these axes, and the projected 206 spot sizes on these axes were calculated at each distance step that the stage 207 away from the mirror. Finally, we obtained the curvature radii on these axes 208 from the minimum of these plots. We also required the curvature radii on 209 the two axes to be within 6067±100 mm. The projected spot sizes on the X 210 and Y axes for the sampled mirror are shown as square and triangle points, 211 respectively, in Fig. 10. From this figure, the curvature radii on the X and Y 212

axes are 6072 mm and 6087 mm, respectively, and these radii also satisfy the 213 above requirement. Fig. 11 shows the distribution of the curvature radius of 214 the accepted mirrors, and Fig. 12 shows the distribution of the normal spot 215 size in diameter at the curvature radius. The curvature radius of the accepted 216 mirrors is 6057 mm (1σ: −20/+30 mm), and their spot size is 12 mm (1σ: 217 −2/+3 mm) in diameter. Henceforth, 1 σ indicates 68% confidence level. 218 From the acceptance test, we found that 5% mirrors were unacceptable. 219 To complement the required number of mirrors, other acceptable mirrors 220 were produced additionally. 221 3.4. Acceptance test for reflectance 222 We employed two different acceptance tests for the segment mirror re- 223 flectance. One is an accurate measurement in the laboratory for a wide 224 wavelength range for sampled mirrors, which was performed by the manufac- 225 turer. The other is a simple measurement with a portable spectrophotometer 226 for a narrow wavelength range for all the segment mirrors. 227 As it is difficult to measure the reflectance of the curved and large segment 228 mirrors accurately, the manufacturer produced small flat pieces of mirrors 229 simultaneously with sampled segment mirrors and precisely measured the 230 reflectance of the flat pieces as part of the delivery inspection process. The 231 reflectance of the small flat mirrors was measured using a spectrometer (Jasco 232 Inc., Ubest V-550), whose range, resolution, and accuracy are 190−900 nm, 233 2 nm, and 1%, respectively. Fig. 13 shows the typical reflectance of sampled 234 small flat mirrors. This reflectance is more than 90% in the wavelength range 235 of 300−400 nm, containing all the major air fluorescence lines. 236 We use a portable spectrophotometer (Konica Minolta, Inc., CM-2500d) 237

for acceptance inspections of all the manufactured segment mirrors and for 238 routine monitoring of reflectance. The range and its resolution are 360−740 nm 239 and 10 nm, respectively. The nominal uncertainties of measurement are less 240 than 1%. To confirm the accuracy and stability of the spectrophotometer, 241 we measured the reflectance of a reference mirror eighteen times in the pe- 242 riod from June 2008 to November 2010. The reference mirror (Ocean Optics 243 Inc., STAN-SSH-NIST) is quartz-coated; its reflectance was measured by the 244 National Institute of Standards and Technology (NIST), USA. Fig. 14 shows 245 a comparison between our measurements and those done by NIST. From 246 this figure, the systematic differences are within ±1% and the deviations are 247 within ±1% in the concerned wavelength range. Fig. 15 shows the varia- 248 tion in the reflectance of the reference mirror at the wavelength of 360 nm, 249 measured using a portable spectrophotometer. The stability was 0.6% (1σ) 250 during the period from June 2008 to November 2010. 251 The typical reflectance of a primary mirror composed of eighteen segments 252 is shown in Fig. 16. This figure shows that the reflectance in the wavelength 253 range of 360−400 nm is higher than 90%. The distribution of the reflectance 254 at 360 nm for all the segment mirrors is shown in Fig. 17. This distribution 255 shows that the differences in the reflectance depend on 108 sampling points 256 of each primary mirror and that the variance is less than 1%, which is within 257 measurement accuracies. Fig. 18 shows the reflectance of the primary mirrors 258 in BRM and LR stations, which is the average of eighteen segment mirrors, 259 with 1σ error bars. All the telescopes fulfilled the requirement that the 260 averaged reflectance was greater than 90% in the wavelength range of 360 nm. 261

4. Telescope installation 262 Mirrors and cameras were shipped from Japan to our observatory in Utah, 263 USA, and these items were installed at BRM from February 2005 to July 2006 264 and at LR in March 2007. In this section, we describe the installations of 265 the FD telescopes and their alignment. 266 4.1. Installation of telescope frame 267 As shown in Fig. 4, six telescope frames were installed in each station 268 (BRM and LR) with each frame having two telescopes. Hence, in all, twelve 269 telescopes were installed in each station. 270 A station building has three rolling doors to protect the telescopes from 271 sunlight, rain, wind, and other natural conditions. The telescopes are directly 272 exposed to air during FD observation, because no other protection windows 273 were installed. 274 When the wind speed was higher than 15 m/s, doors were closed to pre- 275 vent themselves from being stuck. We required less than 0.1^∘ FOV deflections 276 of the telescope with wind speeds lower than 15 m/s. Wind-induced deflec- 277 tions of the telescopes were studied by the manufacturer (Mitsui Engineering 278 & Shipbuilding Co., Ltd.) using simulation programs and by applying wind- 279 tunnel tests on a structure model of a station including telescopes. From 280 their studies, winds from the side of the telescope building induce the max- 281 imum deflections in the telescope frame. Because winds pass through the 282 building from one door to another, their effective speed is not reduced by 283 the building. However, the current design of the frame fulfills our require- 284 ment with regard to frame deflections, even in the worst condition. Based 285

on the studies of the manufactures, the design of telescope frame structure 286 was fixed. 287 To install the telescope frames precisely, we conducted a survey and drew 288 datum lines and points for telescope geometry. Using a gyro-compass, the 289 absolute azimuthal direction was measured with reference to a mountain’s 290 peak. Uncertainties of the gyro-compass measurement was 1^′, which was 291 confirmed from the star observation using the gyro-compass. Three datum 292 lines, shown as solid lines in Fig. 4, were drawn on the floor with relative 293 accuracies of 1^′ between these lines. Azimuthal lines of each telescope frame, 294 shown as dashed lines in Fig. 4, were drawn from the datum lines with 295 accuracies of 0.1^∘ using a measuring tape. From the azimuthal lines, reference 296 points for the telescope frames were marked with accuracies of 1 mm. 297 We installed the telescope frames, which can be separated into frames for 298 cameras and mirrors, as shown in Fig. 3, in accordance with the following 299 procedures. The telescope frames were placed and fixed on the reference 300 points, and before installing real cameras, a prototype standard camera was 301 attached to the camera frames. This prototype standard camera had the 302 same weight and size of a real camera and was equipped with reference lines 303 on the surface for adjusting positions. A steel cylinder with a diameter of 304 500 mm is mounted at the center of each primary mirror, as shown in Fig. 3. 305 The central cylinder was used to adjust the alignment of segment mirrors 306 and the camera of the telescope. 307 Telescope directions were adjusted by the following procedures. First, we 308 installed a laser range meter on the central cylinder. Next, we adjusted the 309 elevation angle to the specified value, monitored using a digital tilt meter, 310

(Digital Protractor, Pro 360), with an accuracy of ±0.2^∘. We adjusted the 311 azimuthal angle of the cylinder for the central axis laser to point the string of 312 a plumb 3000 mm away from the cylinder set exactly above the reference line 313 on the floor. Then, the position of the camera frame was precisely adjusted 314 with reference to the central axis laser. The upper limit for the installed error 315 on the distance between the camera and the cylinder is ±30 mm. However, 316 this misalignment was resolved when we installed mounts of segment mirrors 317 whose heights were adjusted to remove the distance error. On the other 318 hand, to reduce the construction cost, we required relatively low accuracies 319 of the direction of the camera, which are within 1^∘. This affects the negligible 320 uncertainties of the effective area of the camera, the order of which is cos(1^∘). 321 After the adjustment of the camera position, the prototype standard camera 322 was unmounted from the camera frame. 323 Finally, the positions of the segment mirror mount were adjusted. Fig. 19 324 shows the schematic view of a jig called “BANANA1” for adjusting the posi- 325 tions of the segment mirror mount. BANANA1 was mounted on the central 326 cylinder of mirrors and can be rotated around the central axis of the cylin- 327 der. The equipment had two arms, one of which had three protruding legs 328 of different lengths; the other arm had a counter weight. By rotating BA- 329 NANA1, we adjusted the length of every segment mirror mount for one of 330 the three legs on BANANA1 to be aligned with the reference point on the 331 mount surface. At the same time, the direction of each segment mirror was 332 roughly adjusted using BANANA1. 333

4.2. Installation of cameras and mirrors 334 The cameras and mirrors were set on the telescope frame by the follow- 335 ing procedures. We set the segment mirrors on their mounts and precisely 336 aligned each direction by screwing in and out two adjusting bolts on a mount. 337 To adjust the direction of segment mirrors, we use an equipment called “BA- 338 NANA3”, shown in Fig. 20. The equipment was mounted on the camera 339 frame, and a white board was perpendicularly set on the optical axis of the 340 primary mirror. The distance between segment mirrors and the board was 341 6067 mm, which is the same distance as the curvature radius of the mirrors. 342 Green LEDs were connected to the white board, 5, 10, and 15 cm away from 343 the center of curvature, as shown in Fig. 21. When the direction of the seg- 344 ment mirror was adjusted, the LED lights were reflected to the symmetrical 345 point about the center of curvature. The direction was adjusted with an 346 accuracy of less than 0.1^∘, which was estimated from the accuracy of cen- 347 ter position determination of reflected light of 5 mm (1/4 diameter of the 348 reflected lights) and from the distance between mirror and the white board, 349 6067 mm. For parallel lights, this setting accuracy provided us the spots 350 of 40 mm diameter, in which 68% of reflected photons fall, at the camera 351 surface. After these adjustments, the segment mirror mounts were locked 352 up. 353 PMT cameras were mounted on the camera frames with an accuracy of 354 10 mm on the camera plane. This accuracy corresponds to ∼0.2^∘ uncer- 355 tainty of the telescope’s pointing direction. PMT cameras were connected 356 by signal, HV, and DC cables. Finally, the wiring was confirmed through 357 test operations. 358

In all, the directions of the telescope are adjusted with a few 0.1^∘ accura- 359 cies. These directions were confirmed with a star light analysis, which uses a 360 similar method as in reference [10]. Our FDs record air fluorescence signals 361 with background photons (BGPs), as we employ a DC coupling for the PMT 362 signal readout. Thus, we obtain the variations in BGP with a normal trigger 363 rate of 2−3 Hz. When a star traverses the FOV of a PMT, the number of 364 BGPs increases and decreases in a few minutes. The time variations of BGPs 365 are simulated from star positions and telescope directions. Using these esti- 366 mated time variations of BGPs, we studied the telescope directions and spot 367 sizes of the primary mirror. The correction values of the FOV direction of 368 FD obtained from this study are used in our simulation and the EAS recon- 369 struction programs. Our results of the star light analysis will be reported in 370 a future paper. 371

5. Mirror reflectance monitoring 372 The reflectance of the segment mirrors is monitored every months. Mir- 373 ror reflectance decreases with time, because our FDs are exposed to the air 374 directly and because dust is attached to the mirrors during observations. In 375 addition, the reflectance of lower mirrors decreases more rapidly than that of 376 upper mirrors. Fig. 22 shows the time variations of the averaged mirror re- 377 flectance at 360 nm of a typical lower telescope LR04. The largest decrement 378 of 4 % occurred between June 2007 and March 2008. When we analyze the 379 FD data from that period, we take this 4 % as the systematic uncertainty of 380 the mirror reflectance. 381 Every summer, the mirrors are washed using purified water and deter- 382

gent for sensitive equipments (Alconox, Inc., LIQUI-NOX). Purified water 383 is obtained from tap water filtered through charcoal and deionization filters. 384 After washing, the mirrors are rinsed using purified water and dried naturally. 385 Fig. 22 shows that the reflectance of the mirror after washing is recovered 386 to the same level as in the first installation. Fig. 23 shows the differences 387 in mirror reflectance before and after washing at each wavelength; these dif- 388 ferences have no clear wavelength dependencies. Based on this result, we 389 mainly monitor the reflectance at 360 nm. 390

6. Summary 391 In Japan, we have produced PMT cameras and mirrors for use in the air 392 fluorescence detector of the Telescope Array experiment. The cameras and 393 mirrors that passed our acceptance inspections were shipped to our experi- 394 mental site in Utah, USA. The telescope frames, mirrors, and cameras were 395 installed at the FD stations. The directions of the telescope are adjusted 396 with an accuracy of a few 0.1^∘, and the directions are confirmed with a star 397 light analysis. These parameters are used in our detector simulation and 398 the EAS reconstruction programs. Monitoring of the performances of the 399 cameras and mirrors begin according to the following schedules: the gains of 400 PMT camera, hour by hour during FD operation; mirror reflectance, every 401 few months. Our mirrors are washed every summer, and their reflectance 402 after washing is recovered to the same level as in the first installation. 403

Acknowledgments 404 The Telescope Array experiment is supported by the Japan Society for 405 the Promotion of Science through Grants-in-Aid for Scientific Research on 406 Specially Promoted Research (21000002) “Extreme Phenomena in the Uni- 407 verse Explored by Highest Energy Cosmic Rays”, and the Inter-University 408 Research Program of the Institute for Cosmic Ray Research; by the U.S. 409 National Science Foundation awards PHY-0307098, PHY-0601915, PHY- 410 0703893, PHY-0758342, and PHY-0848320 (Utah) and PHY-0649681 (Rut- 411 gers); by the National Research Foundation of Korea (2006-0050031, 2007- 412 0056005, 2007-0093860, 2010-0011378, 2010-0028071, R32-10130); by the 413 Russian Academy of Sciences, RFBR grants 10-02-01406a and 11-02-01528a 414 (INR), IISN project No. 4.4509.10 and Belgian Science Policy under IUAP 415 VI/11 (ULB). The foundations of Dr. Ezekiel R. and Edna Wattis Dumke, 416 Willard L. Eccles and the George S. and Dolores Dore Eccles all helped 417 with generous donations. The State of Utah supported the project through 418 its Economic Development Board, and the University of Utah through the 419 Office of the Vice President for Research. The experimental site became 420 available through the cooperation of the Utah School and Institutional Trust 421 Lands Administration (SITLA), U.S. Bureau of Land Management and the 422 U.S. Air Force. We also wish to thank the people and the officials of Millard 423 County, Utah, for their steadfast and warm support. We gratefully acknowl- 424 edge the contributions from the technical staffs of our home institutions and 425 the University of Utah Center for High Performance Computing (CHPC). We 426 thank HAMAMATSU Photonics K.K., Sanko Seikohjyo Co., Ltd., Quality 427 Steel Fabricating And Welding, Inc, T&D Maintenance, Nitto Kogyo Cor- 428

poration, and Mitsui Engineering & Shipbuilding Co., Ltd. for their kind 429 support. 430

References 431 [1] H. Kawai et al., Nucl. Phys. B Proc. Suppl, 175-176, (2008) 221 432 [2] H. Kawai et al., J. Phys. Soc. Jpn. Suppl. A, 78 (2009) 108 433 [3] T. Abu-Zayyad et al., NIM A, 450 (2000) 253 434 [4] T. Nonaka et al., Proc. of 30th ICRC, 5 (2007) 1005, and now preparing 435 a detailed paper 436 [5] J. N. Matthews et al., Proc. of 30th ICRC, 5 (2007) 1157 437 [6] H. Tokuno et al., NIM A, 601 (2009) 364 438 [7] H. Tokuno et al., Proc. of 30th ICRC, 5 (2007) 1013, and now preparing 439 a detailed paper 440 [8] Y. Tameda et al., NIM A, 609 (2009) 227 441 [9] A. Taketa et al., Proc. of 29th ICRC, 8 (2005) 209, and now preparing 442 a detailed paper 443 [10] P. A. Sadowski et al., Astropart. Phys, 18 (2002) 237 444

Figure 1: Detector positions in the telescope array experiment. Squares: surface detectors (SDs), triangles: fluorescence detector (FD) telescope stations. SD array area: 700 km, SD spacing: 1.2 km, and distance between FD stations: ∼35 km.

Figure 2: Picture of the fluorescence detector station.

Figure 3: Schematic view of the air fluorescence detectors. For visibility of mirror mounts, seven segment mirrors are removed from the upper telescope.

Figure 4: Schematic projected view of the FD station onto the floor (solid lines: datum lines, dashed lines: azimuthal lines of each telescope frame). The telescopes are numbered according to their FOVs, as shown in this figure; the lower (upper) telescopes have even (odd) numbers.

Figure 5: Schematic side view of a PMT camera. Inside the camera, there are 256 PMTs, connected with signal and HV cables, and a temperature sensor.

Figure 6: Rear view of the PMT camera.

Figure 7: Setup for the measurement of curvature radius of segment mirror.

Figure 8: Photograph of the equipment for measuring the curvature radius of segment mirror. This equipment includes a scanner, a distance meter, and a laser source with a diffuser plate, placed to the right on the linear stage.

Figure 9: Scanned image of reflected light at the distance equal to the curvature radius of the mirror. Colors show intensities of light in the electrical article.

Figure 10: Typical relation between spot size and distance from a segment mirror (circles: spot sizes; squares and triangles: projected spot sizes on X and Y axes, respectively).

Figure 11: Distribution of the curvature radius of segment mirrors (left: BRM, right: LR).

Figure 12: Distribution of the spot size of segment mirrors (left: BRM, right: LR).

Figure 13: Typical reflectance of small flat mirror, measured by the manufacturer (systematic error and measurement error are less than 1%).

Figure 14: The comparison of mirror reflectance between the NIST measurement and our measurement (plots: our measurement value divided by the NIST one, error bars: 1σ).

Figure 15: Variation in the reflectance of a reference mirror at 360 nm from June 2008 to November 2010 (plots: median value, error bars: 1σ, horizontal line: mean value of the plots).

Figure 16: Wavelength dependence of the reflectance of all segment mirrors in March 2007 (plots: median value of 24 primary mirrors, error bars: 1σ).

Figure 17: Distribution of mirror reflectance of 24 primary mirrors at 360 nm in March 2007.

Figure 18: mirror reflectance at 360 nm (horizontal axis: telescope ID, B: BRM, L: LR, plots: median value of 18 segment mirrors, error bars: 1σ, horizontal line: mean value of the plots).

Figure 19: Schematic view of the equipment used for adjusting segment mirror mount. The equipment was mounted on the central cylinder of the mirror.

Figure 20: Schematic view of the equipment for adjusting segment mirror direction. The equipment is mounted on a camera support frame. A white board with LEDs is placed at a distance same as the mirror curvature radius of 6067 mm using this equipment.

Figure 21: Schematic view of LED positions on the white board of BANANA3.

Figure 22: Variation in the mirror reflectance at 360 nm of a typical lower telescope LR04 (plots: median value, error bars: 1σ). The mirror was washed after these measurements in July 2008, August 2009, and May 2010.

Figure 23: Differences in mirror reflectance before and after mirror washing at each wavelength (ratio: before/after, plots: median value of 24 telescopes, error bars: 1σ, circles: 2008, squares: 2009, triangles: 2010). These error bars show the non-uniformity of reflectance just before mirror washing. For visibility, the circles and triangles are slightly moved on the horizontal axis.