arXiv:1201.4964v3 [astro-ph.IM] 25 May 2012

The surface detector array of the Telescope Array 1 experiment 2 T. Abu-Zayyad^a, R. Aida^b, M. Allen^a, R. Anderson^a, R. Azuma^c, 3 E. Barcikowski^a, J. W. Belz^a, D. R. Bergman^a, S. A. Blake^a, R. Cady^a, 4 B. G. Cheon^d, J. Chiba^e, M. Chikawa^f, E. J. Cho^d, W. R. Cho^g, H. Fujii^h, 5 T. Fujii^i, T. Fukuda^c, M. Fukushima^{j,t}, D. Gorbunov^k, W. Hanlon^a, 6 K. Hayashi^c, Y. Hayashi^i, N. Hayashida^l, K. Hibino^l, K. Hiyama^j, 7 K. Honda^b, T. Iguchi^c, D. Ikeda^j, K. Ikuta^b, N. Inoue^m, T. Ishii^b, 8 R. Ishimori^c, D. Ivanov^{a,n}, S. Iwamoto^b, C. C. H. Jui^a, K. Kadota^o, 9 F. Kakimoto^c, O. Kalashev^k, T. Kanbe^b, K. Kasahara^p, H. Kawai^q, 10 S. Kawakami^i, S. Kawana^m, E. Kido^j, H. B. Kim^d, H. K. Kim^g, J. H. Kim^d, 11 J. H. Kim^r, K. Kitamoto^f, K. Kobayashi^e, Y. Kobayashi^c, Y. Kondo^j, 12 K. Kuramoto^i, V. Kuzmin^k, Y. J. Kwon^g, S. I. Lim^s, S. Machida^c, 13 K. Martens^t, J. Martineau^a, T. Matsuda^h, T. Matsuura^c, T. Matsuyama^i, 14 J. N. Matthews^a, I. Myers^a, M. Minamino^i, K. Miyata^e, H. Miyauchi^i, 15 Y. Murano^c, T. Nakamura^u, S. W. Nam^s, T. Nonaka^{j,∗}, S. Ogio^i, 16 M. Ohnishi^j, H. Ohoka^j, K. Oki^j, D. Oku^b, T. Okuda^i, A. Oshima^i, 17 S. Ozawa^p, I. H. Park^s, M. S. Pshirkov^v, D. Rodriguez^a, S. Y. Roh^r, 18 G. Rubtsov^k, D. Ryu^r, H. Sagawa^j, N. Sakurai^i, A. L. Sampson^a, 19 L. M. Scott^n, P. D. Shah^a, F. Shibata^b, T. Shibata^j, H. Shimodaira^j, 20 B. K. Shin^d, J. I. Shin^g, T. Shirahama^m, J. D. Smith^a, P. Sokolsky^a, 21 T. J. Sonley^a, R. W. Springer^a, B. T. Stokes^a, S. R. Stratton^{a,n}, 22 T. A. Stroman^a, S. Suzuki^h, Y. Takahashi^j, M. Takeda^j, A. Taketa^w, 23 M. Takita^j, Y. Tameda^j, H. Tanaka^i, K. Tanaka^x, M. Tanaka^h, 24 S. B. Thomas^a, G. B. Thomson^a, P. Tinyakov^{k,v}, I. Tkachev^k, H. Tokuno^c, 25 T. Tomida^b, S. Troitsky^k, Y. Tsunesada^c, K. Tsutsumi^c, Y. Tsuyuguchi^b, 26 Y. Uchihori^y, S. Udo^l, H. Ukai^b, G. Vasiloff^a, Y. Wada^m, T. Wong^a, 27 M. Wood^a, Y. Yamakawa^j, H. Yamaoka^h, K. Yamazaki^i, J. Yang^s, 28 S. Yoshida^q, H. Yoshii^z, R. Zollinger^a, Z. Zundel^a 29 aUniversity of Utah, High Energy Astrophysics Institute, Salt Lake City, Utah, USA 30 bUniversity of Yamanashi, Interdisciplinary Graduate School of Medicine and 31 Engineering, Kofu, Yamanashi, Japan 32

∗Corresponding author Email address: nonaka@icrr.u-tokyo.ac.jp (T. Nonaka)

Preprint submitted to Elsevier May 28, 2012 cTokyo Institute of Technology, Meguro, Tokyo, Japan 33 dHanyang University, Seongdong-gu, Seoul, Korea 34 eTokyo University of Science, Noda, Chiba, Japan 35 fKinki University, Higashi Osaka, Osaka, Japan 36 gYonsei University, Seodaemun-gu, Seoul, Korea 37 hInstitute of Particle and Nuclear Studies, KEK, Tsukuba, Ibaraki, Japan 38 iOsaka City University, Osaka, Osaka, Japan 39 jInstitute for Cosmic Ray Research, University of Tokyo, Kashiwa, Chiba, Japan 40 kInstitute for Nuclear Research of the Russian Academy of Sciences, Moscow, Russia 41 lKanagawa University, Yokohama, Kanagawa, Japan 42 mSaitama University, Saitama, Saitama, Japan 43 nRutgers University, Piscataway, USA 44 oTokyo City University, Setagaya-ku, Tokyo, Japan 45 pWaseda University, Advanced Research Institute for Science and Engineering, 46 Shinjuku-ku, Tokyo, Japan 47 qChiba University, Chiba, Chiba, Japan 48 rChungnam National University, Yuseong-gu, Daejeon, Korea 49 sEwha Womans University, Seodaaemun-gu, Seoul, Korea 50 tUniversity of Tokyo, Institute for the Physics and Mathematics of the Universe, 51 Kashiwa, Chiba, Japan 52 uKochi University, Kochi, Kochi, Japan 53 vUniversity Libre de Bruxelles, Brussels, Belgium 54 wEarthquake Research Institute, University of Tokyo, Bunkyo-ku, Tokyo, Japan 55 xHiroshima City University, Hiroshima, Hiroshima, Japan 56 yNational Institute of Radiological Science, Chiba, Chiba, Japan 57 zEhime University, Matsuyama, Ehime, Japan 58

Abstract 59 The Telescope Array (TA) experiment, located in the western desert of Utah, USA, is designed for observation of extensive air showers from extremely high energy cosmic rays. The experiment has a surface detector array surrounded by three fluorescence detectors to enable simultaneous detection of shower particles at ground level and fluorescence photons along the shower track. The TA surface detectors and fluorescence detectors started full hybrid observation in March, 2008. In this article we describe the design and technical features of the TA surface detector.

Keywords: Ultra-high energy cosmic rays; Telescope Array experiment; 60 Extensive air shower array 61

1. Introduction 62 The main aim of the Telescope Array (TA) experiment [1] is to explore 63 the origin of ultra high energy cosmic rays (UHECR) using their energy 64 spectrum, composition and anisotropy. There are two major methods of ob- 65 servation for detecting cosmic rays in the energy region above 10^{17.5} eV. One 66 method which was used at the High Resolution Fly’s Eye (HiRes) experiment 67 is to detect air fluorescence light along air shower track using fluorescence 68 detectors. The other method, adopted by the AGASA experiment, is to de- 69 tect air shower particles at ground level using surface detectors deployed over 70 a wide area (∼100 km^2). 71 The AGASA experiment reported that there were 11 events above 10^{20} 72 eV in the energy spectrum [2, 3]. However, the existence of the GZK cutoff 73 [4, 5] was reported by the HiRes experiment [6]. The Pierre Auger experiment 74 confirmed the suppression on the cosmic ray flux at energy above 4×10^{19} eV 75 [7] using an energy scale obtained by fluorescence light telescopes (FD). The 76 contradiction between results from fluorescence detectors and those from sur- 77 face detector arrays (SD) remains to be investigated by having independent 78 energy scales using both techniques. Hybrid observations with SD and FD 79 enable us to compare both energy scales. Information about core location 80 and impact timing from SD observation improves accuracy of reconstruction 81 of FD observations. Observations with surface detectors have a nearly 100% 82

duty cycle, which is an advantage especially for studies of anisotropy. Cor- 83 relations between arrival directions of cosmic rays and astronomical objects 84 in this energy region should give a key to exploring the origin of UHECR [8] 85 and their propagation in the galactic magnetic field. 86 In this article we describe the design and technical features of the TA 87 surface detector. 88

2. Telescope Array experiment 89 The TA site is located in the desert about 1400 m above sea level cen- 90 tered at 39.3^∘N and 112.9^∘W in Millard County, Utah, USA, about 200 km 91 southwest of Salt Lake City. A control center to support construction and 92 operation of the TA instruments is in the city of Delta located near the north- 93 east side of the array. The experiment is aimed at observing cascade showers 94 induced by cosmic rays above 10^{19} eV. The altitude of the experimental site 95 is optimal for observing particle showers at nearly maximum development of 96 the cascade. For hybrid observation the site also needed to be located in a 97 semi-desert area with less light pollution from the town. The dry climate 98 allows us to have a high duty cycle for FD-SD hybrid exposure; about 10% 99 of real time. 100 Below we describe the major advantages of the TA experiment: 101 1) The TA experiment utilizes plastic scintillators similar to AGASA ex- 102 periment. For energies of about 10^{20} eV, more than 90% of the primary 103 energy is absorbed as the electromagnetic component (e^+,e^− and γ) in the 104 air. Plastic scintillators are sensitive to all charged particles, and the en- 105 ergy measurement is less affected by the difference of the details of unknown 106

Figure 1: Layout of the Telescope Array in Utah, USA. Squares denote 507 SDs. There are three subarrays controlled by three communication towers denoted by triangles. The three star symbols denote the FD stations.

hadron interactions and the primary composition. 2) The HiRes-I telescope 107 system was partially moved to the Middle Drum (MD) hill in TA site and 108 installed as one of the three FD stations after the HiRes experiment was shut 109 down in 2006 [9]. Using an energy spectrum obtained with MD station data, 110 it is possible to cross-check the new TA FD data and analysis method. The 111 surface detector observes lateral distribution of the shower particle. Energy 112 deposition at a certain distance from shower core is used as an estimator of 113 the energy by comparing with air shower Monte Carlo simulation. It is pos- 114 sible to compare the estimated energy with that obtained from longitudinal 115 shower development observed by FD data analysis. 116 3) In addition to the conventional calibration and monitor system, we plan to 117 perform absolute end-to-end calibration of a fluorescence telescope by using 118 pseudo air shower events that are induced by electron beams with known to- 119 tal energy from a compact electron linear accelerator at the TA site [10, 11]. 120 As described above, the TA experiment is well-balanced to determine the 121 energy of air shower events. 122 4) The anisotropy of arrival directions of ultra-high energy cosmic rays is 123 being studied in the northern hemisphere where the effect of the galactic 124 magnetic field is smaller than that in the southern hemisphere. A typical 125 angular resolution of TA SD array is better than 1.5^∘ for the shower above 126 10 EeV [12]. 127

3. Surface detector array 128 The SD array consists of 507 detector units, which were deployed in a 129 square grid with 1.2 km spacing to cover a total area of approximately 700 130

km^2. Fig. 1 shows a layout of the TA experiment. Each surface detector 131 has a plastic scintillation counter of 3 m^2 in size, and transmits SD data 132 via a wireless LAN modem. As shown in Fig. 1, the SD array is divided 133 into three subarrays each controlled by its trigger-decision electronics at the 134 communication tower. The Long Ridge (LR), Black Rock (BR), and Smelter 135 Knolls (SK) subarrays have 189, 170 and 148 SDs respectively. (The numbers 136 of SDs in LR , BR and SK from March 2008 to November 2009 were 207, 190 137 and 110 respectively.) All detectors are powered by solar panels and batteries 138 [13]. For events with energies beyond 10^{19} eV and with zenith angles below 139 45 degrees, the trigger efficiency reaches ∼100% and the aperture is 1100 140 km^2·sr. The observed energy region for the TA experiment has sufficient 141 overlap with those for the previous experiments of UHECR. 142 3.1. Surface detector 143 The TA detector will operate for more than 10 years and must be de- 144 signed to survive the expected conditions at the site. The detector must be 145 robust and durable for long-term exposure to the desert environment where 146 the detector temperature ranges from −20^∘C to +50^∘C with large diurnal 147 variations. And the system requires detailed monitoring and periodic cali- 148 brations to track variations of detector response along time. 149 Fig. 2 shows one of the deployed SDs that communicate with the commu- 150 nication tower placed at Smelter Knolls (SK), a nearby hill. A communication 151 antenna (ADAF2414; ADTEC Co.) with adjustable height is mounted on 152 a 3-m long iron pole. A square solar panel 1 m on one side is mounted on 153 the platform to supply power to the electronics. Front-end electronics and a 154 battery are contained in a box made with 1.2 mm thick stainless steel. The 155

Figure 2: A deployed SD in the field. The electronics box and scintillator box are on the iron frame. An electronics unit is installed under the solar panel, and the scintillator box is mounted on the platform under the roof.

Figure 3: Inside of a scintillator box with scintillator plates, WLS fibers and PMTs. A total of 104 WLS fibers are laid on each layer to collect and transmit scintillation light to a PMT [14].

box is mounted under the solar panel. The box that contains the scintillators 156 and photomultiplier tubes (PMTs) is mounted under the 1.2-mm thick iron 157 roof to protect the detector from large temperature variations. 158 Fig. 3 shows a schematic of the inside of a scintillator box. Each surface 159 detector consists of two layers of plastic scintillator. Each layer of scintillator 160 has an area of 3 m^2 and a thickness of 1.2 cm. A Stainless-steel plate has 161 1 mm in thickness and is inserted between the layers. As shown in Fig. 3, 162 each scintillator layer consists of 2 segments, and each segment consists of 4 163 slabs. The size of one segment is 1.5 m × 1.0 m. The size of each slab is 164 1.5 m × 0.25 m and thickness is 1.2 cm. On top side of the scintillator slab, 165 there are grooves in parallel along the length of the slab. The span of grooves 166 is 2.0 cm and the depth is 1.5 mm. Scintillation light is collected through 167 104 wavelength-shifting (WLS) fibers (Y-11; Kuraray Co. Ltd.) that are 168

laid along each groove. Total length of a WLS fiber is 5 m. The fibers are 169 put in the grooves on the surfaces of the scintillator slabs without oil and 170 grease, and are fixed at both edges of the slabs with tape (polyester tape 171 #850 silver; 3M). The segment is wrapped with two layer of Tyvek (1073B; 172 Dupont Co.) sheet. Both ends of the fibers from a layer are bundled together 173 and connected to a PMT (9124SA; Electron Tubes Ltd.). 174 Each PMT is calibrated to obtain the relation of high voltage and gain. 175 Linearity between input light amount and output charge is also obtained 176 in the calibration [15]. Two LEDs (NSPB320BS; Nichia Corp.) are also 177 installed on the side of each layer to calibrate linearity of output for input 178 light. Scintillator plates and PMTs are contained in a 1.5 mm thick box made 179 of stainless steel (top cover is 1.5 mm thick, with a 1.2 mm thick bottom) 180 (TAITO Co. Ltd.). 181 3.2. Detector Electronics 182 Fig. 4 shows the detector electronics for a scintillator counter installed in 183 a stainless-steel box under the solar panel. The output signals from PMTs 184 are digitized by a 12bit FADC (AD9235RU- 65; Analog Devices Co.) with 185 a 50 MHz sampling rate on the CPU board (SH4; Renesas Electronics Co.). 186 Signals greater than approximately 0.3 minimum ionizing particles (MIP) are 187 stored in a memory buffer on CPU board as Level-0 trigger data. The stored 188 waveform is 2.56 μsec long (128 FADC bins). Signals greater than 3.0 MIP 189 are stored as a Level-1 trigger event, which are sent to the trigger-decision 190 electronics at the communication tower for the subarray via a wireless LAN 191 modem (ADLINK540F; ADTEC. Co) using a custom-made communication 192 protocol [16]. The local trigger rates are ∼750 Hz for the Level-0 trigger 193

Figure 4: Detector electronics of the TA surface detector. The wireless LAN board is mounted under the main CPU board.

and ∼30 Hz for the Level-1 trigger. In FPGA, the FADC pedestals are 194 monitored every second to keep threshold values for the trigger. The pedestal 195 value is defined as the average of FADC values within 160 nsec (8 FADC 196 bins). The threshold value for Level-0 trigger is fixed to 15 counts above the 197 average of pedestal. Triggered waveforms mostly from atmospheric particles 198 are counted into histograms based on integrated count and maximum count 199 of the waveform. For the monitoring of detector gain, the signal part of the 200 waveform is integrated for 240 nsec (-80 nsec from trigger timing and up to 201 +160 nsec after) and the values are accumulated into histograms for each 202 layer of scintillator. The integrated FADC value and the maximum value 203 of the signal waveform within 2.56 μsec are also accumulated in histograms. 204 These are used for detector linearity monitoring. The synchronization of 205

electronics of the surface detectors is done by PPS signals received by GPS 206 units (Motorola M12+ oncore module). A time stamp with a precision of 20 207 nsec is created by the 50 MHz sub-clock on the main board. The total counts 208 of the sub-clock between PPS signals are also sent to the trigger-decision 209 electronics along with a Level-1 event list to correct the time stamp of the 210 waveform in later analysis. The power bases (PS1806/12F-02; Electrontube 211 Co. Ltd.) for PMTs are powered and controlled through DAC on the detector 212 electronics. Each SD unit described above is powered by one solar panel 213 (KC125TJ; KYOCERA Corp.) and one deep cycle battery (DCS100; C&D 214 technologies, Inc.). The solar panel has 125 W of charging power. The 215 battery has 100 Ah of capacity. The charging of the battery is controlled 216 by home made charge control board that works with main CPU board. The 217 solar panel system provides sufficient power required from the electronics (∼5 218 W). 219 3.3. Assembly and deployment 220 Detector assembly is divided into two parts. First, two layers of plastic 221 scintillator are installed in the stainless-steel box and WLS fibers are laid 222 on each layer. To increase the light intensity, each layer of scintillator is 223 wrapped with two layers of Dupont Tyvek sheeting. Both ends of a bundle 224 of WLS fibers from a layer are glued together with epoxy inserted into an 225 acrylic sheath. The sheath is sized to fit the PMT surface. The ends of the 226 WLS fibers are smoothed with a grinder and polished after making a bundle 227 in the sheath. To ensure good optical contact, optical grease (Optseal; Shin- 228 Etsu Chemical Co. Ltd.) is also applied on the surface of the PMT. The 229 production rate of scintillator boxes was three boxes per day. In total 512 230

SD boxes were assembled in Japan and those boxes were shipped to Utah, 231 USA. Second, the final assembly of other components such as solar panels, 232 batteries, and electronics along with mounting these on to iron frames (T&D 233 Co. Ltd.) was performed at the control center in Delta. Each SD unit was 234 deployed to its location by using helicopter after transporting the units by 235 trucks with a flatbed trailer to staging areas accessible from existing roads 236 inside the TA site. From October 2006 to the end of February 2007, 485 237 surface detectors were deployed. A total of 503 SDs were deployed by the 238 end of December 2007. Additional 4 SDs were deployed in December 2008. 239 3.4. Long-distance network for remote operation 240 Fig. 5 shows one of the communication towers, which is located at Smelter 241 Knolls (SK) near the north edge of the SD array. The other two towers also 242 have the same size and are located on hills (Black Rock and Long Ridge) 243 near the western and eastern edges of the SD array, respectively. The com- 244 munication towers have the role of collecting trigger information from the 245 SDs and providing communications for the FD stations and CLF (Central 246 Laser Facility) [17] site for general purposes. 247 Fig. 6 shows the long-distance links for all the facilities and air fluores- 248 cence detectors in the entire TA site. The open triangles in Fig. 6 represent 249 the locations of the communication towers. The data collected from the SDs 250 are temporarily stored at the communication tower and regularly transferred 251 to Delta City through this network every 12 hours. There are two types of 252 antenna units (Canopy P2P100; Motorola Co. Ltd.) which are operated in 253 different frequency ranges. The tower-to-tower and tower-to-FD links are 254 operated at 5.7 GHz and the tower-to-SD links are operated at 2.4 GHz 255

Figure 5: The Smelter Knolls communication tower, one of three in the array. There are three stands each with four solar panels. Those stands contain batteries, data acquisition PC and network instruments for long distance link.

Figure 6: The long-distance links for all the facilities and three FD stations in the entire TA site. The open triangles represent the communication towers where the triggerdecision electronics for subarrays are installed. The lines that connect the towers and facilities represent the links between antennas. The red lines are used for trigger decision. The dotted line represents the border of the entire surface detector array.

Figure 7: Long-term stability of the network from August 2008. Red histograms in the top two panels show daily packet loss rate in the line between the SK to BR towers and in the line between the SK to LR towers, respectively. The bottom panel shows the same in the line between the BR and LR FD stations. The monitor data for daily packet loss rate were not recorded in the green regions.

range. The line between the SK and BR towers and the line between the SK 256 and LR towers are used for SD data acquisition. No access to FD stations 257 and CLF for general purposes interferes with the SD data acquisition lines. 258 The long distance networks are currently operated at 3 Mbps throughput, 259 which is sufficient for SD data acquisitions, data transfer and operation of 260 FD stations. 261 Fig. 7 shows the daily average values of packet loss rate in the lines 262 monitored in the current system. The network is stable enough, except for 263 some periods of major maintenances. More details of long distance network 264

Figure 8: Trigger pattern taken at the TA surface array. If any three adjacent SDs have Level-1 trigger, timing differences are within 8 μsec of which the Level-2 trigger will be generated.

in the TA experiment are described in papers [18, 19]. 265

4. Data communication and air shower trigger 266 There is a trigger-decision module at each tower. The electronics is the 267 same as shown in Fig. 4, running a different firmware program. The data 268 communication between the trigger-decision electronics at communication 269 tower and SDs is done by 2.4 GHz wireless LAN using a custom-made com- 270 munication protocol. The baud rate of the data acquisition is ∼1 Mbps. 271 Every second, the trigger-decision electronics at the communication tower 272 requests each surface detector to send a Level-1 trigger event list and the 273 total counts of the sub-clock between PPS signals. From the event lists, an 274 air shower trigger is generated when three adjacent SDs are coincident within 275 8 μsec. Fig. 8 shows the current trigger pattern of three adjacent SDs that 276

are hit. We call this trigger the Level-2 trigger. With this trigger, collec- 277 tion of waveforms stored in each SD electronics starts. The trigger-decision 278 electronics collects waveforms coincident within ±32 μsec from the trigger 279 timing. When the Level-2 trigger is generated within one subarray, the trig- 280 ger time information is transmitted to the central trigger decision process. 281 The process is running at the data acquisition PC (TS7800; Technologic sys- 282 tems, Co. Ltd.) in the SK tower. From the SK tower, the Level-2 trigger 283 signal is distributed to other two towers. The broadcasting of this trigger en- 284 ables to collect waveforms associated with a shower which impacts multiple 285 subarrays. Fig. 9 shows an event triggered at BR subarray. Fig. 10 shows 286 a sample of waveforms. 287 To collect air shower event at the boundary of subarrays, the Level-1 trigger 288 event lists from the SDs at the boundary of subarrays are also sent to the 289 central trigger process in SK tower. The central trigger process combines 290 Level-1 trigger information collected from SDs at the boundary of subarrays. 291 The central trigger process verifies whether the same trigger condition was 292 satisfied only by the boundary detectors. 293 As shown in Fig. 8, in the case of pattern 1 or 6 , the hit pattern that sat- 294 isfies the Level-2 trigger condition can be spread over 2 subarrays, but the 295 condition is not satisfied with edge detectors only. To trigger such a case, 296 central trigger process searches for the coincidence of two adjacent hits in 297 the boundary detectors from Level-1 trigger list. If such a coincidence exists, 298 the central trigger process sends time and position information of the coinci- 299 dence to all towers. Trigger-decision electronics at towers verify the Level-2 300 trigger condition using the received information from the central trigger pro- 301

Figure 9: An example of triggered event at BR array. Red open circles represent SDs in BR subarray. The triggered SDs are shown with color code, which corresponds to the arrival time. The radius of a circle is proportional to the logarithm of the integrated signal amount in the unit of MIP.

Figure 10: Waveforms obtained from the event shown in Fig. 9

cess. Shower events of relatively small size that fall near the boundary of 302 subarrays is collected by this trigger scheme. 303 With the above trigger conditions, trigger efficiency reaches 97% for pri- 304 mary particle with energy of 10^{19.0} eV. Here the efficiency includes the effect 305 of dead counters [16, 20, 23]. Fig. 11 shows trigger efficiency as a function of 306 energy of primary particle obtained using CORSIKA [24] air shower Monte 307 Carlo simulation and GEANT4 [25] detector Monte Carlo simulation [26]. 308 To improve the efficiency of detecting FD-SD hybrid events at lower ener- 309 gies (< 10^{18.7} eV), an external trigger called Hybrid Trigger was installed to 310 collect waveforms associated with air showers detected by FD. From nearest 311 FD, the SD data acquisition system at a tower receives trigger timing and 312 time window for requesting waveforms stored at each SD in the subarray. 313 The efficiency of the waveform collection is greater than 97% for the primary 314

Figure 11: Trigger efficiency as a function of energy for primary proton calculated using CORSIKA air shower Monte Carlo simulation and GEANT4 detector Monte Carlo simulation.

particle with energy of 10^{17.5} eV triggered by FD [27]. The extended hybrid 315 trigger observations started in October 2010. 316

5. Detector Calibration and Monitoring 317 For stable observation, the status and environment of the batteries need 318 to be monitored continuously. For calibration in later analysis, it is very 319 important to monitor the detector response. For this purpose, a monitoring 320 process runs on each SD in a 10 min cycle. The monitored items are summa- 321 rized in Table 1 [28]. The size of monitoring data for 10 min is 9600 bytes. 322 The data is divided into 600 subsets. All the subsets are sent along with the 323 Level-1 trigger tables within 10 min. 324

Table 1: Items and resolutions of TA Surface Detector monitor. Item Data Resolution 1MIP histogram 12bin sum of FADC 1 FADC count 10min Pedestal histogram 8bin sum of FADC 1 FADC count 10min Pulse height histogram Maximum FADC 32 FADC count 10min Total charge histogram 128bin sum of FADC Δ log_2(FADC sum)=0.2 Power cycle data Battery (voltage, current) 1min Environmental data Temperature, humidity 1min Trigger rate Level-0, Level-1 trigger rate 1min GPS status Number of satellites, status 10min

5.1. The 1-MIP monitor 325 The charge output by atmospheric charged particles is used to estimate 326 the total energy deposited by shower particles. The integrated FADC value 327

Figure 12: Example of FADC count distribution from Level-0 trigger events obtained as 1-MIP monitor data. The hatched histogram is a pedestal distribution collected as monitor data. The pedestal distribution is scaled to have the same entry as the Level-0 trigger data. The same distribution is collected from every PMT at 10 min intervals.

recorded by the Level-0 trigger is collected as monitoring data from each 328 surface detector. Here the time window for the integration is 240 nsec (12 329 bins). The time window ranges between -4 bins from trigger timing and +8 330 bins after trigger timing. That is sufficient to evaluate MIP peak count of 331 FADC. Fig. 12 shows an example of the charge output distribution. The 332 last bin of the histogram is the overflow bin. The temperature coefficient 333 of gain of the surface detectors is typically -0.8%/^∘C for a diurnal variation 334 of temperature that reaches up to 25^∘C [21]. Fig. 13 shows examples of 335 the monitored time variations of temperature, relative humidity inside the 336 scintillator box, and 1-MIP peak value. Change of detector response caused 337 mainly by the variation of the outside temperature is monitored by this 338 distribution continuously to the nearest ten minutes. 339

Figure 13: Examples of time variations of temperature (top) and relative humidity (middle) inside the scintillator box, and the 1-MIP peak value (bottom).

5.2. Linearity monitor 340 A check on the linearity of charge output was performed by using two 341 LEDs attached at each layer of scintillator. This was done for all the detectors 342 before deployment. Two LEDs were flashed with 400 nsec wide square pulses 343 alternately or simultaneously. The amount of light from each LED is changed 344 by changing the pulse height of the square pulse. From the ratio of the 345 measured output to the expected output, the linearity curves were measured. 346 Here we describe the light amount as x and the peak of the pulse from a 347 PMT in FADC count as F (x) while driving one LED. The PMT output 348 while driving LED 1 and 2 simultaneously is represented as F (x_1 + x_2). The 349 linearity was checked by comparing F (x_1 + x_2) and F (x_1) + F (x_2) while 350 changing x_1 and x_2. Fig. 14 shows a typical example of observed relation 351

Figure 14: An example of observed relation between F (x_1 + x_2) and F (x_1) + F (x_2).

between F (x_1 + x_2) and F (x_1) + F (x_2). 352 To check the linearity and its variation in the long term of operation, 353 pulse-height (FADC peak) histograms are also taken as monitoring data. 354 The pulse height of the signal that satisfies the level-0 trigger condition is 355 counted into a histogram. The high voltage values of the PMTs of all the 356 detectors are adjusted to obtain almost the same FADC counts for 1 MIP 357 peaks. So the histograms differ between detectors because of the difference of 358 the linearity of the PMTs. We monitor the histogram to detect time variation 359 of the linearity. By comparing the tail of the histogram and the one from 360 the tubes with good linearity, it is possible to estimate non-linearity. Fig. 15 361 shows an example of comparison between pulse-height linearity obtained from 362 LED calibration and the one estimated using the pulse-height monitor. It 363 shows fairly good agreement and it was confirmed that the histogram can be 364 used for monitoring the stability of linearity. When the pulse height of signal 365 is larger than the expected height of saturation, the signal is not used for 366 analyzing lateral distribution of shower particle. But the timing information 367 is used for calculating arrival direction. 368 5.3. Power monitor, GPS and environmental parameters 369 Since each SD is locally powered by a solar panel and a battery, it is very 370 important to monitor the status of the output voltage and current from the 371 battery. The 1PPS signals are generated by GPS modules using the signals 372 from the satellites that are visible through the GPS antennas. To understand 373 the status of the GPS module, the number of satellites visible through the 374 GPS module and conductivity of the antenna are read out every 600 sec. 375 Each surface detector is equipped with five temperature sensors and two 376

Figure 15: Analyzed linearity of pulse height from monitor data [16]. In the top left panel, the green open circles denote the relative deviation from the estimated linear response by LED calibration, and the red open circles denote the relative deviation by pulse-height monitor for the upper layer of one SD (SD #0114). The top right panel shows the same for the lower layer. In the bottom left panel, the red open circles denote the scaled pulse height distribution observed for the upper layer, and the green line denotes the average from good tubes. The bottom right panel shows the same for the lower layer.

humidity sensors to record the environment of the detector and electronics 377 box. 378 Fig. 16 gives an example of the time variations in the number of de- 379 tected GPS satellites, the battery voltage and charging current, the Level-0 380 and Level-1 trigger rates for one detector, and the barometric pressure and 381 atmospheric temperature measured at the CLF [17] site. 382

6. Summary 383 The SD array of the TA experiment consists of 507 plastic scintillation 384 detectors of 3 m^2 in size. The array has the largest total area in the northern 385 hemisphere. The detector enables us to compare estimated energy of primary 386 particle using longitudinal shower development observed at FD and lateral 387 distribution of shower particles detected with the SD array. The observation 388 with the SD array is continuous to have ∼100% of duty cycle. This feature 389 enables us to explore the anisotropy of arrival directions of highest energy 390 cosmic rays with larger exposure than observation with FD. 391 The deployment of the surface detectors started in October 2006. Totally 392 507 surface detectors were deployed by November 2008. The deployed detec- 393 tors have been calibrated and tuned. The air shower array began operation 394 in March 2008. For more than three years, air shower events from UHECR 395 have been collected along with detailed monitoring data. The monitoring 396 data enables us to calibrate the variation of detector responses with enough 397 accuracy. We showed the running status after three years of SD operation. 398 An upgrade of the DAQ system was performed and additional deployment 399 was made in November 2008. Including maintenance periods, the array has 400

Figure 16: An example of time variations in the number of GPS satellites (top panel), battery voltage and charging current (second panel) , local Level-0 and Level-1 trigger rates (third panel) for one surface detector, and the barometric pressure and atmospheric temperature measured at the CLF site using a weather transmitter (WXT510; VAISALA Inc.)(bottom panel).

Figure 17: Running status of the SD array. Daily duty ratio of running. Evolution of the number of triggered event is also shown using right vertical axis.

been operating with a 95% of duty cycle on average. The variations of de- 401 tector response and status are recorded in 10 min resolution and are well 402 understood. The number of triggers collected as of March 2011 has reached 403 5 × 10^5. 404

Acknowledgments 405 The Telescope Array experiment is supported by the Japan Society for 406 the Promotion of Science through Grants-in-Aid for Scientific Research on 407 Specially Promoted Research (21000002) “Extreme Phenomena in the Uni- 408 verse Explored by Highest Energy Cosmic Rays”, and the Inter-University 409 Research Program of the Institute for Cosmic Ray Research; by the U.S. 410 National Science Foundation awards PHY-0307098, PHY-0601915, PHY- 411 0703893, PHY-0758342, and PHY-0848320 (Utah) and PHY-0649681 (Rut- 412

gers); by the National Research Foundation of Korea (2006-0050031, 2007- 413 0056005, 2007-0093860, 2010-0011378, 2010-0028071, R32-10130, 2011-0002617); 414 by the Russian Academy of Sciences, RFBR grants 10-02-01406a and 11- 415 02-01528a (INR), IISN project No. 4.4509.10 and Belgian Science Policy 416 under IUAP VI/11 (ULB). The foundations of Dr. Ezekiel R. and Edna 417 Wattis Dumke, Willard L. Eccles and the George S. and Dolores Dore Ec- 418 cles all helped with generous donations. The State of Utah supported the 419 project through its Economic Development Board, and the University of 420 Utah through the Office of the Vice President for Research. The experi- 421 mental site became available through the cooperation of the Utah School 422 and Institutional Trust Lands Administration (SITLA), U.S. Bureau of Land 423 Management and the U.S. Air Force. We also wish to thank the people and 424 the officials of Millard County, Utah, for their steadfast and warm support. 425 We gratefully acknowledge the contributions from the technical staffs of our 426 home institutions and the University of Utah Center for High Performance 427 Computing (CHPC). 428

References 429 [1] H. Kawai, et al., Nucl. Phys. Proc, suppl, vol 175-176 (2008) 221-226. 430 [2] M. Takeda, et al., Phys. Rev. Lett. 81 (1998) 1163. 431 [3] M. Takeda, et al., Astroparticle Physics 19 4 (2003) 447. 432 [4] K. Greisen, Phys. Rev. Lett. 16 (1966) 748. 433 [5] T. Zatsepin and V.A.Kuzmin, JETP Lett 4 (1966) 178. 434

[6] T. Abu-Zayyad, et al., Phys. Rev. Lett. 92 (2004) 151101. 435 [7] J. Abraham, et al., Phys. Rev. Lett. 101 (2008) 061101. 436 [8] N. Hayashida, et al., Astroparticle Physics 10 (1999) 303-311. 437 [9] J.N. Matthews, et al., Proceedings of the 30th International Cosmic Ray 438 Conference in Merida Vol.4 (2007) 417-420 . 439 [10] T. Shibata, et al., Proceedings of the 30th International Cosmic Ray 440 Conference in Merida Vol.5 (2007) 1069-1072 . 441 [11] T. Shibata, et al., Nucl. Instrum. Methods Phys. Res., Sect, A 597, 61 442 (2008). 443 [12] I. Tkachev, et al., Proceedings of the 31th International Cosmic Ray 444 Conference in Beijing ID 1311 (2011). 445 [13] T. Tomida, Master thesis University of Yamanashi (2008). 446 [14] S. Kawakami, et al., Proceedings of the 29th International Cosmic Ray 447 Conference in Pune 8 (2005) 161. 448 [15] S. Yoshida, et al., Proceedings of the 29th International Cosmic Ray 449 Conference in Pune 8 (2005) 2411. 450 [16] A. Taketa, et al., Proceedings of the 31th International Cosmic Ray 451 Conference in Łódź ID 924 (2009). 452 [17] S. Udo, et al., Proceedings of the 30th International Cosmic Ray Con- 453 ference in Merida Vol.5 (2007) 1021. 454

[18] T. Nonaka et al., Proceedings of the 31th International Cosmic Ray 455 Conference C in Łódź ID 977 (2009). 456 [19] S. Iwamoto, Master thesis University of Yamanashi (2009). 457 [20] N.Sakurai, et al., Proceedings of the 30th International Cosmic Ray 458 Conference in Merida, Vol.5 (2007) 1159. 459 [21] T. Nonaka, et al., Proceedings of the 30th International Cosmic Ray 460 Conference in Merida,Vol 5 (2007) 1005. 461 [22] A. Taketa, et al., in preperation. 462 [23] Y. Yamakawa, Master thesis University of Tokyo (2009). 463 [24] D. Heck, et al., Forschungszentrum Karlsruhe Report FZKA 6019 464 (1998). 465 [25] S. Agostinelli, et al., Nuclear Instruments and Methods in Physics Re- 466 search A 506 (2003) 250-303. 467 [26] B. Stokes, et al., Proceedings of the 31th International Cosmic Ray 468 Conference in Łódź ID 1328 (2009). 469 [27] R. Ishimori, et al., Proceedings of International Symposium on the Re- 470 cent Progress of Ultra-high Energy Cosmic Ray Observation, Nagoya 471 (2010). 472 [28] T. Nonaka, et al., Proceedings of the 31th International Cosmic Ray 473 Conference C in Łódź ID 974 (2009). 474