arXiv:1205.2831v1 [cond-mat.soft] 13 May 2012

Photoinduced reordering in thin azo-dye films and light-induced reorientation dynamics of nematic liquid-crystal easy axis

Alexei D. Kiselev,^{1, 2, ∗} V.G. Chigrinov,^{2, †} S.V. Pasechnik,^{3, 2} and A.V. Dubtsov^3 1Institute of Physics of National Academy of Sciences of Ukraine, prospekt Nauki 46, 03028 Kiev, Ukraine 2Hong Kong University of Science and Technology, Clear Water Bay, Kowloon, Hong Kong 3Moscow State University of Instrument Engineering and Computer Science, Stromynka 20, 107846 Moscow, Russia (Dated: December 2, 2020) We theoretically study the kinetics of photoinduced reordering triggered by linearly polarized (LP) reorienting light in thin azo-dye films that were initially illuminated with LP ultraviolet (UV) pumping beam. The process of reordering is treated as a rotational diffusion of molecules in the light intensity-dependent mean-field potential. The two dimensional (2D) diffusion model which is based on the free energy rotational Fokker-Planck equation and describes the regime of in-plane reorientation is generalized to analyze the dynamics of the azo-dye order parameter tensor at varying polarization azimuth of the reorienting light. It is found that, in the photosteady state, the intensity of LP reorienting light determines the scalar order parameter (the largest eigenvalue of the order parameter tensor), whereas the steady state orientation of the corresponding eigenvector (the in-plane principal axis) depends solely on the polarization azimuth. We show that, under certain conditions, reorientation takes place only if the reorienting light intensity exceeds its critical value. Such threshold behavior is predicted to occur in the bistability region provided that the initial principal axis lies in the polarization plane of reorienting light. The model is used to interpret the experimental data on the light-induced azimuthal gliding of liquid-crystal easy axis on photoaligned azo-dye substrates.

PACS numbers: 61.30.Hn, 42.70.Gi Keywords: nematic liquid crystal; easy axis gliding; photo-alignment

I. INTRODUCTION

Linearly polarized (LP) ultraviolet (UV) or visible light is known to have a profound effect on the physical properties of some photosensitive materials such as compounds containing azobenzene and its derivatives [1]. In particular, such materials may become dichroic and birefringent under the action of LPUV light. Over the past few decades this phenomenon — the so-called effect of photoinduced optical anisotropy (POA) — which has a long history dating back almost a century to the original paper by Weigert [2] has been attracted much attention for both technological and fundamental reasons. POA is of primary importance

∗ Email address: kiselev@iop.kiev.ua † Email address: eechigr@ust.hk

in the development of tools dealing with the light-controlled anisotropy and the materials that exhibit POA are very promising for use in many photonic applications [3–6].

POA also lies at the heart of the photoalignment (PA) technique which is employed in the manufacturing process of liquid crystal displays for fabricating high quality aligning substrates [7, 8]. This method avoids the drawbacks of the traditional mechanical surface treatment and uses LPUV light to induce anisotropy of the angular distribution of molecules in a photosensitive film [8, 9].

When the irradiated layer is brought in contact with a liquid crystal (LC), the surface ordering originated from the photoinduced anisotropy manifests itself in the anisotropic part of the surface tension known as the anchoring energy and determines the anchoring characteristics such as the anchoring strengths and the easy axis, n_e, that defines the direction of preferential orientation of LC molecules at the surface. In this way, the light can be used as a means to control the anchoring properties of photosensitive materials.

This is the light-induced anisotropy of the orientational distribution of molecules that reveals itself in POA and can be described as the photoinduced orientational ordering in photosensitive materials. Such ordering, though not being understood very well, can generally occur by a variety of photochemically induced processes. These typically may involve such transformations as photoisomerization, crosslinking, photodimerization and photodecomposition (a recent review can be found in Refs. [8, 10]).

The mechanism of photoinduced ordering underlying POA and related photoaligning properties therefore cannot be universal. Rather they crucially depend on the material in question and on a number of additional factors such as irradiation conditions, surface interactions etc. These factors combined with the action of light may result in different regimes of the photoinduced ordering kinetics leading to the formation of various photoinduced orientational structures.

The photoalignment has been studied in a number of polymer systems including dye doped polymer layers [11, 12], cinnamate polymer derivatives [13–16] and side chain polymers containing chemically linked azochromophores (azopolymers) [17–20]. POA observed in similar polymers [3, 4, 17–19, 21, 22] was found to be long term stable so that the photoinduced anisotropy does not disappear after switching off the irradiation.

Most of the above mentioned polymer systems represent azocompounds that exhibit POA driven by the trans-cis photoisomerization. In theoretical models [22–28], they are treated as ensembles of the stable trans isomers characterized by elongated rod-like molecular conformation and the bent banana-like shaped cis isomers.

The mechanism of photoisomerization implies that the key processes behind the photoinduced orientational ordering of azo-dye molecules are photochemically induced trans-cis isomerization and subsequent thermal and/or photochemical cis-trans back isomerization of azobenzene chromophores. Owing to pronounced absorption dichroism of photoactive groups, the photoisomerization rate strongly depends on orientation of the azo-dye molecules relative to the polarization vector of the pumping light, E_{UV} .

When the cis isomers are short-living, the cis state becomes temporary populated during photoisomerization but reacts immediately back to the stable trans isomeric form. The trans-cis-trans isomerization cycles are accompanied by rotations of the azo-dye molecules that tend to minimize the absorption and become oriented along directions normal to the polarization vector of the exciting light E_{UV} (the molecules with the optical transition dipole moment oriented perpendicular to E_{UV} are almost inactive). Non-photoactive groups may then undergo reorientation due to cooperative motion [18, 25, 27–29].

From the above it might be concluded that the photoinduced orientational structures will be uniaxially anisotropic with the optical axis directed along the polarization vector, E_{UV} . Experimentally, this is, however, not the case. For example, constraints imposed by a medium may suppress out-of-plane reorientation of the azobenzene chromophores giving rise to the structures with strongly preferred in-plane alignment [22]. Another symmetry breaking effect induced by polymeric environment is that the photoinduced orientational structures can be biaxial [21, 22, 27, 30–32] (a recent review of medium effects on photochemical processes can be found in [33]).

It was recently found that, similar to the polymer systems, the long-term stable POA in the films containing photochemically stable azo-dye structures (azobenzene sulfuric dyes) is characterized by the biaxial photoinduced structures with favored in-plane alignment [34, 35]. Unlike azopolymers, photochromism in these films is extremely weak so that it is very difficult to unambiguously detect the presence of a noticeable fraction of cis isomers.

Over the last decade the photoaligning properties of such azo-dye (SD1) films has been the subject of intense studies [8, 36–38]. It was found that, owing to high degree of the photoinduced ordering, these films used as aligning substrates are characterized by the anchoring energy strengths comparable to the rubbed polyimide films. For these materials, the voltage holding ratio and thermal stability of the alignment turned out to be high. The azo-dye films are thus promising materials for applications in liquid crystal devices.

The anchoring characteristics of the azo-dye films such as the polar and azimuthal anchoring energies are strongly influenced by the photoinduced ordering. In particular, the easy axis is dictated by the polarization of the pumping LPUV light, whereas the azimuthal and polar anchoring strengths may depend on a number of the governing parameters such as the wavelength and the irradiation dose [38].

In a LC cell with the initially irradiated layer, the easy axis may rotate under the action of secondary irradiation with reorienting LP light which polarization differs from the one used to prepare the aligning layer. This effect — the so-called light-induced reorientation of the easy axis — is governed by the photoinduced reordering of azo-dye molecules triggered by the reorienting light and may be of considerable interest for applications such as LC rewritable devices [39]. Note that slow reorientation of the easy axis (the light-induced easy axis gliding) on the photosensitive layers prepared using the PA technique was originally observed on poly-(vinyl)-alcohol (PVA) coatings with embedded azo-dye molecules [40]. For the azo-dye films, similar results were reported in Ref. [41].

In this paper the kinetics of photoinduced reordering underlying the light-induced easy axis reorientation on the azo-dye films will be our primary concern. In particular, we apply a generalized version of the theoretical analysis presented in Ref. [35] to examine how the initial ordering of azo-dye molecules and the characteristics of reorienting light affect the regime of kinetics and the photosteady states.

There are two phenomenological models formulated in Ref. [35] by using different theoretical approaches: (a) the two-state model is based on the above discussed mechanism of photoisomerization with short living excited cis state which is characterized by weak photochromism and negligibly small fraction of cis molecules that rapidly decays after switching off irradiation; and (b) the diffusion model describes the light-induced reorientation of azodye molecules as rotational Brownian motion governed by the light intensity-dependent mean-field potential. It turned out that predictions of the models are quite similar and they both were successfully used to interpret the experimental data. This equivalence points to the fact that, in the limiting case of short-living cis states, the photoisomerization cycles with orientation dependent isomerization rates may generally be viewed as a random walk on the sphere described by the Fokker-Planck equation for rotational diffusion. For our purposes, the latter will be conveniently employed to perform the theoretical analysis and to model the kinetics of reordering.

The layout of the paper is as follows. In Sec. II we briefly recapitulate the theory [35] introducing the diffusion models where the process of photoinduced reordering is treated as a rotational diffusion in the effective mean-field potential. Then, in Sec. II B, we discuss the regime of purely in-plane reorientation and analyze the general properties of the corresponding two dimensional (2D) diffusion model. In Sec. III these results are used to study bifurcations of the photosteady states and the kinetics of photoinduced reordering depending on the initial ordering, the light intensity, I_{UV} and the polarization azimuth, α_p, that characterizes orientation of the polarization vector of reorienting LPUV light, E_{UV} . In Sec. IV we apply the model to interpret the experimental data on the light-induced azimuthal gliding of the easy axis on the photoaligned SD1 substrate measured as part of the investigation into effects of the polarization azimuth in the dynamics of the electrically assisted light-induced gliding [42]. Finally, in Sec. V we draw the results together and make some concluding remarks.

Figure 1: (Color online) Frame of reference: the z axis is normal to the substrate and the polarization vector of the activating light makes the angle α_p with the y axis.

II. MODEL

In this section our starting point is the approach of Ref. [35] in which the light-induced reorientation of azo-dye molecules is described as rotational Brownian motion governed by the effective mean-field potential.

Following Ref. [35], we assume that azo-dye molecules are cylindrically symmetric, so that orientation of a molecule can be specified by the unit vector, û = (sin θ cos ϕ, sin θ sin ϕ, cos θ), directed along the long molecular axis. Quadrupolar orientational ordering of such molecules is characterized using the traceless symmetric second-rank tensor [43]

Q(û) = (3 û ⊗ û − I_3)/2, (1)

where I_n is the n × n identity matrix. The dyadic (1) can be averaged over orientation of molecules with the normalized angular distribution function f(û, t) to yield the order parameter tensor S ⟨Q⟩ = ∫ Q(û)f(û, t) dû = S, (2)

where dû ≡ sin θdθdϕ.

A. Rotational mean-field Fokker-Planck equation

The key assumption taken in the diffusion models formulated in Ref. [35] is that the angular distribution function, f(û, t), of rodlike azo-dye molecules must satisfy the rotational free energy Fokker-Planck (FP) equation

∂_tf = −L_iD^{(rot)}_{ij} { f L_j δF [f] δf } ≡ −L · D_{rot} { f · L δF [f] δf } , (3)

where D^{(rot)}_{ij} is the rotational diffusion tensor and L is the angular momentum operator that can be expressed in terms of of the azimuthal and zenithal (polar) angles, ϕ and θ, as follows

i L = [r × ∇] = ê_ϕ ∂_θ − [sin θ]^{−1}ê_θ ∂_ϕ, (4)

where ê_θ = (cos θ cos ϕ, cos θ sin ϕ, − sin θ) and ê_ϕ = (− sin ϕ, cos ϕ, 0).

When the effective free energy functional is a sum of the effective internal energy, U[f], and the Boltzmann entropy, ⟨ln f⟩, F [f] = U[f] + ⟨ln f⟩, the free energy FP (3) can be recast into the form of the mean-field FP equation

∂_tf = −L · D_{rot} {L f + f · L V } , V = δU δf . (5)

describing the rotational diffusion governed by the effective mean-field potential, V .

1. Effective mean-field potential

In the lowest order approximation based on the truncated expansion for the internal energy functional U[f] retaining one-particle (linear) and two-particle (quadratic) terms, the effective potential, V , is given by

V (û) = δU δf(û) = U_1(û) + ∫ U_2(û, û^′)f(û^′) dû^′, (6) where U_1(û) is the external field potential and the last term proportional to the symmetrized two-particle kernel, U_2(û, û^′), represents the contribution coming from the intermolecular interactions.

The one-particle part of the effective potential (6) can be written as a sum of the lightinduced contribution

U_I (û) = u_I E^∗_{UV} · Q(û) · E_{UV} , (7)

where an asterisk indicates complex conjugation, that comes from the interaction of azomolecules with the reorienting UV light and the surface-induced potential

U_s(û) = u_s ẑ · Q(û) · ẑ = u_s Q_{zz}(û) (8)

that takes into account conditions at the bounding surfaces of the azo-dye layer. So, for the two-particle interaction taken in the Maier-Saupe form

U_2(û_1, û_2) = u_2 Tr[Q(û_1) · Q(û_2)] = u_2 Q_{ij} (û_1)Q_{ij}(û_2), (9)

we obtain the following expression for the effective potential of azo-dye molecules:

V (û) = u_I I_{UV} ê_p · Q(û) · ê_p + u_s Q_{zz}(û) + u_2S_{ij} Q_{ij}(û), (10)

where I_{UV} is the intensity of the reorienting UV light which is assumed to be linearly polarized along the unit polarization vector ê_p

ê_p = R_{rot}(α_p) ŷ, R_{rot}(α_p) = ( cos α_p − sin α_p sin α_p cos α_p ) (11)

that makes the angle α_p with the y axis directed along the polarization vector of the initial irradiation: E_{ini} ‖ ŷ (see Fig. 1).

Note that, in the limiting case of non-interacting molecules with U_2 = 0, the rotational mean-field FP equation (5) reduces to the well-known linear rotational diffusion equation that has been widely used to study a large variety of problems based on the rotational diffusion model for the rotational motion of molecules in the presence of external fields. These include dielectric and Kerr effect relaxation of polar liquids [44–51], rotational diffusion of a probe molecule dissolved in a liquid crystal phase [52–57] and the molecular reorientation in liquid crystal phases [58–61].

2. Steady states

The equilibrium angular distribution can generally be obtained as a stationary solution to the FP equation (5). It can be readily checked that the Boltzmann distribution

f_{st}(û) = Z^{−1}_{st} exp[−V (û)], Z_{st} = ∫ exp[−V (û)]dû (12)

determined by the effective potential gives the stationary solution. Note that the energy scale is determined by the temperature factor k_B T incorporated into the rotation diffusion tensor, so that the internal energy, U[f], and the potential, V , are both dimensionless.

When the FP equation is linear, the stationary distribution (12) describing the equilibrium state is unique. By contrast, this is no longer the case when the effective potential (10) depends on the elements of the averaged orientational order parameter tensor (2): V (û) = V (û|S). In this case, the components of the order parameter tensor in the stationary state, S_{ij} = S^{(st)}_{ij} , can be found from the self-consistency equation S_{ij} = ∫ Q_{ij}(û) f_{st}(û|S) dû. (13)

which generally possesses several solutions representing multiple local extrema (stationary points) of the free energy

F [f_{st}] ≡ F_{st}(S) = − u_2 2 S_{ij}S_{ij} − ln Z_{st}(S). (14)

Following the line of reasoning presented in Ref. [62] and using the effective free energy as the Lyapunov functional, it is not difficult to prove the H theorem for nonlinear FP equations of the form (3). It follows that, in the long time limit, all transient solutions converge to stationary ones. So, each stable stationary distribution is characterized by the basin of attraction giving orientational states (angular distributions) that evolve in time approaching the stationary distribution.

B. Two-dimensional model of purely in-plane reorientation

In the previous section our model has been formulated as the free energy FP equation (5) describing rotational diffusion of azo-dye molecules governed by the effective mean field potential (10). In this section, we concentrate on the limiting case of purely in-plane reorientation and deal with the simplified two-dimensional model ∂_τ f =∂_ϕ [ ∂_ϕf + f∂_ϕV ] = ∂^2_ϕf + 1 2 [ ∂^2_ϕ(fV )

+ f∂^2_ϕV − V ∂^2_ϕf ] , τ = D^{(rot)}_z t. (15)

can be derived by assuming that the out-of-plane component of the unit vector û describing orientation of the azo-dye molecules is suppressed and, as is shown in Fig. 1, û = (sin ϕ, cos ϕ, 0). It implies that, similar to the model of a single axis rotator with two equivalent sites [44, 45], the molecules are constrained to be parallel to the substrate plane (the x-y plane).

1. Potential

When the out-of-plane reorientation is completely suppressed and û = (sin ϕ, cos ϕ, 0), the order parameter dyadic (1) simplifies as follows

Q(ϕ) = ( Q_2(ϕ) 0 0 −1/2 ) (16) where Q_2 is the two-dimensional in-plane part of the tensor. The in-plane order parameter tensor is given by the 2 × 2 block-matrix

4Q_2(ϕ) = I_2 − 3 cos(2ϕ) σ_3 + 3 sin(2ϕ) σ_1 (17)

expressed in terms of the Pauli matrices: σ_3 = ( 1 0 0 −1 ) and σ_1 = ( 0 1 1 0 ) . We can now substitute the expression for the order parameter tensor (16) into the effective potential (10) and use the algebraic identity

R_{rot}(−α)Q_2(ϕ)R_{rot}(α) = Q_2(ϕ + α) (18)

to derive the angular dependent part of the potential in the following form: V = ( v^∗ exp[2iϕ] + v exp[−2iϕ] ) /2, (19a) v = v_1 exp[−2iα_p] + v_2⟨exp[2iϕ]⟩, (19b) v_1 ≡ 3u_I I_{UV} /4, v_2 = 9u_2/8, (19c) where ⟨. . .⟩ = ∫_{2π} 0 . . . fdϕ; v_1 and v_2 are the photoexcitation and intermolecular interaction parameters, respectively.

2. Fourier harmonics and order parameters

Our next step is to obtain the system of equations for the averaged complex harmonics, h_n(τ) = ⟨exp[inϕ]⟩(τ), that are proportional to the Fourier coefficients of the distribution function, f(ϕ, τ) f(ϕ, τ) = (2π)^{−1} ∞∑ n=−∞ h_n(τ) exp[−inϕ]. (20)

To this end, we integrate the FP equation (15) multiplied by exp[inϕ] over the azimuthal angle. The resulting system reads

∂_τ h_n(τ) = −n^2h_n + n { v^∗(α_p, h_2)h_{n+2}(τ) − v(α_p, h_2)h_{n−2}(τ) } , (21)

where v(α_p, h_2) ≡ v = v_1 exp[−2iα_p] + v_2h_2.

When f(ϕ + π) = f(ϕ), the odd numbered harmonics vanish, h_{2k+1} = 0. For the even numbered harmonics, ρ_k ≡ h_{2k}, the system (21) can be conveniently recast into the form

∂_τ ρ_k = −4k^2ρ_k + 2k (v^∗ρ_{k+1} − vρ_{k−1}), k = 1, 2, . . . (22) ρ_k = p_k + iq_k = ⟨cos(2kϕ)⟩ + i⟨sin(2kϕ)⟩ ≡ h_{2k}, ρ_0 = 1, (23)

where ρ_1 = p_1 + iq_1 = ⟨exp[2iϕ]⟩ is the complex order parameter harmonics.

For the in-plane order parameter tensor (17) averaged over the azimuthal angle

⟨Q_2⟩ = S_2 = 1 4 ( 1 − 3p_1 q_1

q_1 1 + 3p_1 ) = R_{rot}(α_e) ( s_+ 0 0 s_− ) R_{rot}(−α_e), (24)

s_± = (1 ± 3|ρ_1|)/4, 2α_e = arg(−ρ_1^∗), (25) the order parameter harmonics, ρ_1, defines the principal values (eigenvalues), s_+ and s_−, and the eigenvector, (cos α_e, sin α_e), for the largest eigenvalue s_+ giving the in-plane principal axis: n̂_e = (cos α_e, sin α_e, 0). So, the tensor (24) can be rewritten in the form of the in-plane order parameter dyadic:

S_2 = s_−I_2 + (s_+ − s_−)n̂_e ⊗ n̂_e. (26)

Temporal evolution of the in-plane order parameter tensor is determined by the order parameter harmonics, ρ_1(t), that can be computed as a function of time by solving the initial value problem for the system (22) with the initial values of the harmonics ρ_k(0) = ρ^{(ini)}_k representing the initial angular distribution f(ϕ, 0) = f_{ini}(ϕ).

3. Symmetry

It is not difficult to check that the system (21) is invariant under the symmetry transformation

h_n → h̃_n = exp[inα]h_n, v → ṽ = exp[2iα]v = v(α_p − α, h̃_2). (27)

An important consequence of these relations concerns the special case where the reorienting light is switched off and v_1 = 0. It can be readily seen that, at v = v_2ρ_1, a set of the harmonics, {ρ_k}_k, and that of the transformed harmonics {exp[2ikα]ρ_k}_k both satisfy the system of equations (22). In particular, at I_{UV} = 0, the stationary angular distribution, f_{st}(ϕ), and the shifted (rotated) one, f_{st}(ϕ − α), both represent steady states.

By using the symmetry relations (27) dynamical equations (22) can be conveniently changed into the system with the zero polarization azimuth, α_p = 0. More precisely, from Eq. (27), it follows that the transformed harmonics

ρ̃_k = exp[2ikα_p]ρ_k (28)

satisfy the system (22) with the coupling coefficient v(α_p, ρ) and the initial distribution f_{ini}(ϕ) replaced by ṽ = v(0, ρ̃_1) and f̃_{ini} = f_{ini}(ϕ − α_p), respectively. Geometrically, such transformation can be described as a transition to the frame of reference where the y axis is directed along the polarization vector of reorienting light.

So, in the subsequent section, we shall restrict our considerations to the special case of the system with the coupling coefficient

ṽ = v_1 + v_2ρ̃_1 (29)

taken at α_p = 0. In this case, the polarization azimuth, α_p, enters the initial data, ρ̃^{(ini)}_k = exp[2ikα_p]ρ^{(ini)}_k , and the formula

α_e = α_p + 1 2 arg(−ρ̃^∗_1) (30)

gives the azimuthal angle of the principal axis (25) expressed in terms of the order parameter harmonics ρ̃_1.

Figure 2: (Color online) (a) Steady state order parameter harmonics p_{st} as a function of the photoexcitation parameter v_1 at v_2 = −2.5; (b) bifurcation curves in the v_2-v_1 plane are typical of the cusp catastrophe with the cusp singularity located at (−2, 0).

III. KINETICS OF PHOTOINDUCED IN-PLANE REORDERING

A. Bifurcations of equilibria

The expression for the stationary distributions

f_{st} = Z^{−1}_{st} exp[−V ] = Z^{−1}_{st} exp[−|ṽ| cos(2ϕ − α̃)], Z_{st} = ∫_{2π} 0 exp[−V ]dϕ (31) comes from the general formula (12) and represents the photosteady states in the two dimensional case with the potential given in Eq. (19) where the coupling coefficient is changed from v to ṽ = |ṽ| exp[iα̃].

Equation (31) can now be combined with the relation

exp[−v cos 2ϕ] = I_0(v) + 2 ∞∑ k=1 (−1)^kI_k(v) cos 2kϕ, (32)

where I_k is the modified Bessel function of integer order [63], to derive the stationary state statistical integral Z_{st} = 2πI_0(|ṽ|) (33) and the stationary state free energy (14)

F_{st}(ṽ) = v^{−1}_2 [ − |ṽ|^2 2 + v_1|ṽ| cos α̃ ] − ln I_0(|ṽ|), (34)

Figure 3: (Color online) Bifurcation diagram as the cusp surface in the three dimensional (v_1, v_2, p_1) space.

where the additive constant is chosen so as to have the free energy vanishing at ṽ = 0.

The stationary points of the energy (34), ṽ = ṽ_{st} = v_1 + v_2ρ̃^{(st)}_1 , define the steady state distributions (31) characterized by the stationary values of the order parameter harmonics, ρ̃^{(st)}_1 = p̃^{(st)}_1 +iq̃^{(st)}_1 , which can also be found as solutions of the self-consistency equation (13). Close inspection of the formula (34) shows that, for stationary points, the steady state coupling (potential strength) coefficient is real, ṽ_{st} = v_1 + v_2p̃^{(st)}_1 ≡ v_1 + v_2p_{st}, with q̃^{(st)}_1 = 0 and sin α̃_{st} = 0. So, we may closely follow the line of reasoning presented in Ref. [35] to perform the bifurcation analysis.

According to Ref. [35], the steady state harmonics are given

ρ̃^{(st)}_k = p̃^{(st)}_k = (−1)^kI_k(ṽ_{st})/I_0(ṽ_{st}), (35) where ṽ_{st} satisfies the self-consistency condition

p_{st} = (ṽ_{st} − v_1)/v_2 = −I_1(ṽ_{st})/I_0(ṽ_{st}). (36)

As is evident from the curve depicted in Fig. 2(a), the number of solutions of the selfconsistency equation (36) varies between one and three depending on the values of the parameters v_1 and v_2. Figure 2(a) shows the order parameter harmonics, p̃^{(st)}_1 ≡ p_{st}, plotted in the v_1-p_1 plane by using the parametrization

p_{st} = { p_1 = p_1(ξ) = −I_1(ξ)/I_0(ξ), v_1 = v_1(ξ) = ξ − v_2 p_1(ξ)

(37)

and demonstrates that, for the intermolecular interaction parameter v_2 = −2.5 and sufficiently small photoexcitation parameters, the steady state free energy (34) has two local minima separated by the energy barrier and thus possesses three stationary points. More specifically, the steady states are determined by the free energy of the double-well potential form only if the inequalities

v_2 < v^{(c)}_2 = −2, v^{(−)}_c < v_1 < v^{(+)}_c (38)

are satisfied.

The critical values of the parameter v_1 depend on the reduced strength of intermolecular interaction v_2 and can be parametrized as follows

v_c = v_1 = v_1(ξ) = ξ − v_2p_1(ξ),

v_2 = v_2(ξ) = −[ ( I_1(ξ)/I_0(ξ) )_′ ξ]^{−1} = 1 1 + p_1(ξ)/ξ − p^2_1(ξ) . (39)

Geometrically, in the v_2-v_1 plane, equation (39) defines the bifurcation curves shown in Fig. 2(b). These curves form a bifurcation set which is the projection of the cusp surface

S_B = v_1 = ξ − ζp_1(ξ), v_2 = ζ, p_1 = −I_1(ξ)/I_0(ξ)

(40)

representing the bifurcation diagram in the three dimensional (v_1, v_2, p_1) space (see Fig. 3). Note that the cusp bifurcation occurs as a canonical model of a codimension 2 singularity [64] and the surface shown in Fig. 3 is typical of the cusp catastrophe [65, 66].

B. Steady-state order parameter tensor

From the discussion at the end of Sec. II B 3 and the relation (35), at α_p ≠ 0, the stationary angular distributions are defined by the steady state harmonics

ρ^{(st)}_k = exp[−2ikα_p](−1)^kI_k(ṽ_{st})/I_0(ṽ_{st}), (41)

which are expressed in terms of the steady state coupling coefficient, ṽ_{st} = v_1 + v_2p_{st}, that meets the self-consistency condition (36). For each steady state characterized by the corresponding solution of Eq. (36), ṽ_{st}, the principal values of the in-plane order parameter tensor (24), s^{(st)}_± , can be computed from Eq. (25) by setting ρ_1 = p_{st} = (ṽ_{st} − v_1)/v_2, whereas the azimuthal angle, α^{(st)}e , characterizing steady state orientation of the principal axis is given by the formula (30) with ρ̃_1 = p_{st}:

s^{(st)}_± = (1 ± 3|p_{st}|)/4, (42a)

α^{(st)}_e = α_p + 1 2 arg(−p_{st}) = { α_p and n̂^{(st)}e ⊥ E_{UV} , p_{st} < 0 α_p + π/2 and n̂^{(st)}e ‖ E_{UV} , p_{st} > 0

. (42b)

(a) Order parameter harmonics (b) Angular distribution function

Figure 4: (a) Order parameter harmonics, ρ_1, computed as a function of dimensionless time parameter τ by numerically solving the initial value problem for the system (22) with the initial angular distribution (43) at α_{ini} = 65 deg and p_{ini} = −0.41. The photoexcitation and interaction parameters are: v_1 = 3 and v_2 = −1. The stationary state is unique and is characterized by the steady state harmonics p_{st} = p^{(−)}_{st} ≈ −0.86. (b) Angular dependence of the orientational distribution function (46), f(ϕ, τ), at different values of the time parameter, τ. The distribution is π-periodic and solid circles indicate the angles, ϕ_{max} = π/2 − α_e, where peaks are located.

An important conclusion to draw from this result is that, upon reaching the stationary state, the principal axis reorients along the direction perpendicular (parallel) to the polarization vector of the reorienting light, ê_p = (− sin α_p, cos α_p, 0), with α_e → α^{(st)}e = α_p (α_e → α^{(st)}e = π/2 + α_p) when the steady state order parameter harmonics is negative (positive), p_{st} = p^{(−)}_{st} < 0 (p_{st} = p^{(+)}_{st} > 0). Thus, in the photosaturated regime, the orientation of azo-dye molecules turned out to be defined solely by the polarization azimuth of the reorienting UV light.

As it has been discussed in Sec. II B 3, when the activating light is switched off and I_{UV} = 0 (v_1 = 0), the steady states are continuously degenerate with the azimuthal angle of the principal axis playing the role of the degeneracy parameter. The reason for such degeneracy is that the intermolecular interaction is taken in the rotationally invariant Maier- Saupe form (9). The effect of the reorienting linearly polarized light is to lift the degeneracy by breaking the rotational symmetry of the intermolecular interaction.

Figure 5: Angular dependence of the orientational distribution function, f, within the span of the period computed for various values of the time parameter, τ = D_{rot}t, at α_{ini} = 65 deg and p_{ini} = −0.58. The photoexcitation and interaction parameters are v_1 = 1.3 and v_2 = −5, respectively.

C. Computational procedure and bistability effects

According to the results of Ref. [38], when the photoaligned azo-dye film is used as an aligning substrate in a NLC cell, orientation of the easy axis at the azo-dye substrate is dictated by the principal axis of the order parameter tensor (24). In particular, under certain conditions, the difference between the angle α_e and the easy axis azimuthal angle can be negligible. In this case, the kinetics of the easy axis can be modeled by solving the system (22) and computing the angle α_e (see Eq. (30)) as a function of time.

In our modeling, we numerically solve the initial value problem for the harmonics ρ̃_k with the initial angular distribution

f̃_{ini} ∝ exp[−v_{ini} cos 2(ϕ − ϕ_{ini})]. (43)

The distribution (43) is characterized by the initial value of the order parameter harmonics ρ^{(ini)}_1 = p_{ini} = −I_1(v_{ini})/I_0(v_{ini}) that gives the coupling coefficient v_{ini}. At the initial instant

Figure 6: Order parameter harmonics, p_1, computed as a function of time parameter, τ = D_{rot}t, by numerically solving the initial value problem for the system (22) with the initial angular distribution (43) at α_{ini} = 90 deg and α_{ini} = 0.0 deg for −p_{ini} = p_u ± 0.05. The photoexcitation and interaction parameters are: v_1 = 1.3 and v_2 = −5. The stationary states are characterized by the steady state harmonics: p^{(−)}_{st} ≈ −0.91, p^{(+)}_{st} ≈ 0.77 and p_u ≈ 0.48.

of time, the harmonics are thus given by

ρ̃_k(0) = exp[2ikα_{ini}](−1)^kI_k(v_{ini})/I_0(v_{ini}). (44)

In particular, for the order parameter harmonics, we have

p̃_1(0) = p_{ini} cos(2α_{ini}), q̃_1(0) = p_{ini} sin(2α_{ini}). (45)

The initial data defined in Eqs. (43) and (44) represent the angular distribution of azo-dye molecules formed in the film after the preparatory stage of initial irradiation with linearly polarized UV light, E_{ini}. Note that, when the polarization vector E_{ini} is parallel to the y axis, the angle α_{ini} is equal to the polarization azimuth of the reorienting light α_p.

The system (22) with the coupling coefficient v = ṽ = v_1 + v_2ρ̃_1 describes how the harmonics evolve in time approaching, in the long time limit, the steady state values given in Eq. (35). These values are determined by the steady state order parameter harmonics that can be found by solving the self-consistency equation (36)

At sufficiently large positive photoexcitation parameter, v_1 > |v_c|, the equilibrium (photosteady) state is unique and is characterized by the steady state order parameter harmonics p^{(−)}_{st} . This case is illustrated in figure 4a that shows how the order parameter harmonics, ρ̃_1 = p_1 + iq_1, relaxes to the equilibrium state, p_1(t) → p^{(−)}_{st} < 0 and q_1(t) → 0 at t → ∞. The equilibrium value of the principle (easy) axis angle (30) then equals the polarization azimuth α_p and α_e(t) → α_p. The latter implies that, in the regime of photosaturation, the azo-dye molecules align perpendicular to the polarization vector of the reorienting, n̂_e → (cos α_p, sin α_p, 0) ⊥ E_{UV} . Such behavior is in complete agreement with our experimental data described in Sec. IV and has been previously observed in a number of experimental studies (see, e.g., the monograph [8] and references therein).

Figure 4a additionally illustrates that the magnitude of the order parameter harmonics, |ρ_1|, related to the scalar order parameter, s_+, given in Eq. (42a) can be a nonmonotonic function of time. For the angular distribution function f(ϕ, τ) = (2π)^{−1} ∞∑ k=−∞ ρ̃_k(τ) exp[−2ik(ϕ + α_p)] (46)

this implies that the distribution may experience broadening at the early stage of relaxation whereas it is getting narrower during the subsequent relaxation to the highly ordered photosteady state. The effect of early stage disordering can be seen in Fig. 4b that shows how the orientational distribution function (46) of azo-dye molecules evolves in time. Note, however, that such transient disordering is typically either less pronounced or completely suppressed. The latter case is demonstrated in Fig. 5.

Temporal evolution of the angular distribution shown in Fig. 5 is computed in the bistability region where the intermolecular interaction parameter, v_2, is below its critical value, v^{(c)}_2 = −2, and the photoexcitation parameter, v_1 > 0, is sufficiently small, v_1 < |v_c| (see Eq. (38)). This is the region where, in addition to the equilibrium state with the negative order parameter harmonics ρ̃_1 = p^{(−)}_{st} , the metastable state with the harmonics of opposite sign ρ̃_1 = p^{(+)}_{st} is formed.

Figure 7: Order parameter harmonics, p_1, computed as a function of time parameter, τ = D_{rot}t, by numerically solving the initial value problem for the system (22) with the initial angular distribution (43) at α_{ini} = 90 deg and −p_{ini} = 0.65 for v_1 = |v_c| ± 0.05. The interaction parameter and the critical value of the photoexcitation parameter are: v_2 = −5 and |v_c| ≈ 1.51, respectively.

Hence the stationary state free energy (34) takes the form of double-well potential with two local minima located at p^{(−)}_{st} and p^{(+)}_{st} . There is also a local maximum peaked at the point p_u in the interval ranged from p^{(−)}_{st} to p^{(+)}_{st} . Referring to Fig. 2(a), at v_1 > 0, this point with p_u > 0 lies on the upper half part of the branch representing unstable stationary states. In the case of real valued harmonics with q_k = 0, it is the boundary point of the basins of attraction of the two steady states. In particular, this means that the order parameter harmonics p_1 converges to either p^{(−)}_{st} or p^{(+)}_{st} depending on whether its initial value p_1(0) is below or above the boundary value p_u.

At α_{ini} = 0 and α_{ini} = π/2, the initial data (44) are represented by two sets of real valued harmonics. From Eq. (44) it is evident that the only difference between the sets is the sign of the odd numbered harmonics . In particular, we have p_1(0) = p_{ini} and p_1(0) = −p_{ini} at α_{ini} = α_p = 0 and α_{ini} = π/2, respectively.

At α_{ini} = 0 and p_{ini} < 0, the harmonics characterizing the equilibrium state, p^{(−)}_{st} , is the attracting point for the order parameter harmonics and the azimuthal angle of the principal (easy) axis, remains intact, α^{(st)}e = 0. The latter comes as no surprise because the polarization vectors of the initial irradiation and of the reorienting light are parallel, E_{UV} ‖ E_{ini}

Interestingly, orientation of the easy axis may stay unchanged even if the vectors, E_{UV} and E_{ini}, are perpendicular and α_{ini} = α_p = π/2. This occurs when the initial ordering is high, so that −p_{ini} is greater than p_u, −p_{ini} > p_u. As demonstrated in Fig. 6, in this case, the attracting point is the metastable harmonics p^{(+)}_{st} rather than the equilibrium one p^{(−)}_{st} and α^{(st)}e = 0.

Figure 8: Order parameter harmonics, ρ_1, computed as a function of time parameter, τ = D_{rot}t, at α_{ini} = 89.8 deg and p_{ini} = −p^{(+)}_{st} . Other parameters are listed in the caption of Fig. 6.

It can also be seen from the curves of Fig. 6 that, in the opposite case of low ordered initial states with −p_{ini} < p_u, the order parameter harmonics p_1 relaxes back to the equilibrium value p^{(−)}_{st} . So, at −p_{ini} < p_u, the azimuthal angle, α^{(st)}e = α_p = π/2, defines the steady state easy axis which is normal to the direction of its initial orientation.

In Fig. 7, we show that, when the initial ordering is sufficiently high, the process of reorientation crucially depends on whether the photoexcitation parameter, v_1, which is proportional to the intensity of the reorienting light, I_{UV} , exceeds its critical value, |v_c|. This critical value determines the intensity threshold, I_c = 4|v_c/(3u_I )|, and the easy axis reorientation is suppressed at α_p = π/2 in the low intensity region below the threshold where I_{UV} < I_c. Similar threshold behavior has been previously observed in a number of experimental studies on light-induced easy axis reorientation in nematic liquid crystal cells with photosensitive polymer substrates [8, 14, 67, 68]. For azo-dye films, the experimental data of Refs. [42, 69] also suggest the presence of a threshold when the polarization vector E_{UV} is directed along the initial easy axis (see the subsequent section for more details). Our result that under certain conditions highly ordered initial distributions may relax to the metastable stationary state offers a possible explanation for this.

Referring to Fig. 8, it is seen that small deviations of the angle α_{ini} from π/2 have a destructive effect on metastability of the attracting point even if −p_{ini} = p^{(+)}_{st} . It turned out that the basin of attraction of the metastable state is unstable with respect to fluctuations of the polarization azimuth α_p. In the vicinity of the critical angle α_{ini} = π/2, the presence of the metastable state manifests itself as appreciably retarded relaxation to the equilibrium state (see Fig. 8). Similarly, the shape of the azimuthal angle (30) vs time curve shown in Fig. 9 points to a time delay in the process of principal (easy) axis reorientation.

Figure 9: Principal axis azimuthal angle, α_e, computed as a function of time parameter, τ = D_{rot}t, at α_{ini} = α_p = 89.8 deg and p_{ini} = −p^{(+)}_{st} . Other parameters are listed in the caption of Fig. 6.

IV. THEORY VERSUS EXPERIMENT

In the previous section we have examined the experimentally important predictions of the model. These predictions can, in principle, be tested and, in this section, we discuss some of our recent experimental results on the reorientational dynamics of the electrically assisted light-induced azimuthal gliding of the easy axis at varying polarization azimuth of LPUV reorienting light [42].

Such gliding is found to take place on photoaligned azo-dye layers when irradiation of nematic LC (NLC) cells with LPUV light is combined with the application of ac in-plane electric field [69, 70]. Since the effects of electric field is well beyond the scope of the theoretical approach under consideration, the regime of purely light-induced reorientation will be our primary concern and we deal with the data measured in the electric field-free regions

In our experiments, LC cells (d = 17.4 ± 0.2 μm) of sandwich like type were assembled between two amorphous glass plates. The upper glass plate was covered with a rubbed polyimide film giving the strong planar anchoring conditions. A film of the azobenzene sulfric dye SD1 (Dainippon Ink and Chemicals) [8] was deposited onto the bottom substrate on which transparent indium tin oxide (ITO) electrodes were placed. The electrodes and the interelectrode stripes (the gap was about g = 50 μm and the in-plane ac voltage was U = 100 V with f = 3 kHz) were arranged to be parallel to the direction of rubbing (the x axis).

The azo-dye SD1 layer was initially illuminated by LPUV light at the wavelength λ = 365 nm. The preliminary irradiation produced the zones of different energy dose exposure D_p = 0.27, 0.55 J/cm^2 characterized by relatively weak azimuthal anchoring strength. The light propagating along the normal to the substrates (the z axis) was selected by an interference filter. Initial orientation of the polarization vector of the actinic light, E_{ini}, was chosen so as to align azo-dye molecules at a small angle of 4 degrees to the x axis, φ_0 ≈ 4 deg.

The LC cell was filled with the nematic LC mixture E7 (Merck) in isotropic phase and then slowly cooled down to room temperature. Thus we prepared the LC cell with a weakly twisted planar orientational structure where the director at the bottom surface n_0 is clockwise rotated through the initial twist angle φ_0 ≈ 4 deg which is the angle between n_0 and the director at the upper substrate (the x axis).

In addition to the electric field, E = 2 V/μm, the cell was irradiated with the reorienting LPUV light beam (I_{UV} = 0.26 mW/cm^2 and λ = 365 nm) normally impinging onto the bottom substrate. For this secondary LPUV irradiation, orientation of the polarization plane is determined by the polarization azimuth, α_p.

Our experimental method has already been described in Refs. [69, 70]. In this method, NLC orientational structures were observed via a polarizing microscope connected with a digital camera and a fiber optics spectrometer. The rotating polarizer technique was used to measure the azimuthal angle φ_e characterizing orientation of the easy axis. In order to register microscopic images and to measure the value of φ_e, the electric field and the reorienting light were switched off for about 1 min. This time interval is short enough to ensure that orientation of the easy axis remains essentially intact in the course of measurements. The measurements were carried out at a temperature of 26^∘C.

The case where the reorienting light is linearly polarized along the initial surface director n_0 and α_p = π/2, was studied in Refs. [69, 70]. It turned out that, by contrast to the electrically assisted light-induced gliding, the purely photoinduced reorientation is almost

Figure 10: Easy axis angle versus the irradiation time at different values of the polarization azimuthal angle of the reorienting UV light α_p. The experimental data were measured by using the linearly polarized activating light with λ = 365 nm and I = 2.6 W/m^2. Solid lines represent the theoretical curves computed by numerically solving the initial value problem for the system (22) with the initial angular distribution (43). The parameters used in calculations are as follows: the photoexcitation (interaction) parameter is v_1 = 1.3 (v_2 = −5); p_{ini} = p^{(−)}_{st} (α_p = 25 deg and α_p = 43 deg) and p_{ini} = −0.25 at α_p = 65 deg. Other parameters are listed in the caption of Fig. 6.

entirely inhibited at α_p = π/2. As it can be seen from Fig. 10, the latter is no longer the case for the reorienting light with α_p ≠ π/2.

Thus the result is that, as opposed to the cases with non-vanishing electric field and α_p ≠ π/2, the purely photoinduced reorientation of the easy axis has been completely suppressed when the polarization plane is parallel to the initial easy axis. From the above discussion, our model predicts similar behavior that occurs in the bistability region where the reorientation is characterized by the threshold for the intensity of reorienting light.

Figure 10 shows the easy axis angle measured as a function of the irradiation time at various values of the polarization azimuth. The measurements were performed in the region outside the interelectrode gaps where the ac electric field is negligibly small. In the zerofield curves, the easy axis angle increases with the irradiation time starting from the angle of initial twist, φ_0, and approaches the photosteady state characterized by the photosaturated value of the angle close to α_p.

The experimental data can be fitted by the theoretical curves computed from the formula (30), where the order parameter harmonics, ρ̃_1, is found by numerically solving the initial value problem for the system (22) with the initial angular distribution (43). In Fig. 10 we make a comparison between the experimental data and the theoretical curves computed in the bistability region by setting the photoexcitation and interaction parameters, v_1 and v_2, equal to 1.3 and −5, respectively. In this region, the equilibrium state is characterized by the steady state harmonics p_{st} = p^{(−)}_{st} ≈ −0.91, whereas the stationary harmonics p^{(+)}_{st} ≈ 0.77 corresponds to the metastable state. For α_p = 25 deg and α_p = 43 deg, the curves were computed at p_{ini} = p^{(−)}_{st} . It follows that |ρ_1(0)| = |ρ_{st}| and the angle α_{ini} is assumed to be the only parameter describing difference between the initial and the equilibrium angular distributions. The rotational diffusion coefficient D_{rot} can be estimated at about 1.6 × 10^{−4} s^{−1} Using this value to fit the data measured at α_p = 65 deg, we find that the theoretical and experimental results are in agreement when the initial ordering parameter p_{ini} ≈ −0.25 differs from the equilibrium value.

Figure 11: Easy axis angle versus the irradiation time in the electric field-free region at different values of the polarization azimuthal angle of the reorienting UV light. The experimental data were measured by using the linearly polarized activating light with λ = 365 nm and I = 2.6 W/m^2. Solid lines represent the theoretical curves computed from the formula (48) at t_e = γ_e/W_e = 23 min (for φ_m = 25 deg and φ_m = 43 deg), and t_e ≈ 14.4 min. for φ_m = 65 deg.

We conclude this section with the remark concerning the phenomenological model formulated in Refs. [41, 70] to describe the effect of the electrically assisted photoinduced gliding of the easy axis. According to this model, in the absence of ac electric field, temporal evolution of the easy axis azimuthal angle φ_e can be described by the balance torque equation [42] γ_e ∂φ_e ∂t = − W_e 2 sin 2(φ_e − φ_m), (47)

where γ_e is the specific viscosity of gliding; W_e is the effective anchoring parameter which defines the strength of coupling between the easy axis n_e and the initial state of surface orientation; φ_m is the polarization dependent phase shift. The solution of the dynamic equation (47)

tan(φ_e(t) − φ_m) = tan(φ_e(0) − φ_m) exp[−t/t_e], (48)

where t_e = γ_e/W_e the characteristic time of easy axis reorientation, can now be used to fit the experimental data. The results are presented in Fig. 11.

From the curves depicted in Fig. 11 it can be inferred that the phase shift φ_m is close to the polarization azimuth of the reorienting light. The value of the characteristic time, t_e ≈ 14.4 min, estimated for φ_m = 65 deg differs from the one t_e ≈ 23 min obtained for other two angles, φ_m = 25 deg and φ_m = 43 deg. From the other hand, in Fig. 10, the case with α_p ≈ 65 deg is distinctive in initial ordering of the film. This result points to the fact that the coupling strength of the easy axis W_e depends on the photoinduced order parameter of the initially irradiated azo-dye layer. Such dependence was one of the key assumptions taken in Ref. [69] when applying the phenomenological model [41, 70] to interpret the experimental data for photoaligned azo-dye layers prepared at different initial irradiation doses.

V. DISCUSSION AND CONCLUSIONS

In this paper we have studied the kinetics of orientational reordering that takes place in the azo-dye films under the action of LPUV reorienting light. In our theoretical approach, the process of reordering is described in terms of a rotational Brownian motion and we have employed the 2D diffusion model formulated in Ref. [35] to explore the peculiarities of the photoinduced reordering in the regime of purely in-plane reorientation.

Orientational ordering of azo-dye molecules is characterized by the in-plane (2D) order parameter tensor (24). This tensor is expressed in terms of the order parameter harmonics, ρ_1, that enters the formula (25) giving both the value of the scalar order parameter, s_+, and the azimuthal angle, α_e, of the principal (easy) axis, n̂_e.

It is found that dynamics of the order parameter harmonics essentially depends on the initial ordering and the polarization azimuth of the LP reorienting light. In the long time limit, the order parameter harmonics approaches its steady state value reaching the regime of photosaturation. We have proved that, in the steady state, the easy axis azimuthal angle is dictated solely by the polarization azimuth, α_p, (see Eq. (42)), whereas the photostationary value of the scalar order parameter is determined by the photoexcitation and intermolecular interaction parameters, v_1 ∝ I_{UV} and v_2, defined in Eq. (19c).

In the v_1-v_2 plane, inequalities (38) define the bistability region (see Fig. 2(b)) with two locally stable stationary states: equilibrium and metastable ones. An experimentally important bistability effect is that the easy axis reorientation is inhibited when the intensity of the reorienting light linearly polarization along the initial easy axis is below its critical (threshold) value. Such threshold behavior was observed in our experiments where the easy axis angle was measured as a function of the irradiation time at varying polarization azimuth of LPUV reorienting light.

An alternative phenomenological model that also predicts the presence of the reorientation threshold was suggested in Ref. [71]. In that model, the threshold effect comes about from the interplay between two competing easy axes. By contrast, in our model, the bistability appears as an intrinsic property of the reordering process in azo-dye films that manifests itself as the threshold of reorientation.

There is another interesting bistability effect that occurs when the light is switched off (I_{UV} = 0) and v_2 < v^{(c)}_2 = −2. In this case, owing to the rotational symmetry of the twoparticle interaction (9), the easy axis angle, α_e, becomes undetermined and plays the role of the degeneracy parameter. The LPUV light field lifts the degeneracy and the dynamics of the angle turned out to be predominately governed by the photoexcitation parameter, v_1.

For the scalar order parameter which is related to the magnitude of the order parameter harmonics, |ρ_1|, the rate of relaxation is typically at least twice faster than that for the easy axis angle. As is illustrated in Fig. 4a, depending on the initial conditions, temporal evolution of this order parameter can be non-monotonic. These effects can also be seen from

Figs. 4b and 5 that show how the orientational angular distribution of azo-dye molecules evolves in time.

By numerically solving the dynamical system for the angular distribution harmonics (22) we have fitted the experimental data on the light-induced azimuthal gliding of the easy axis at the photoaligned azo-dye SD1 layer. In our analysis, the photoinduced reordering of azo-dye molecules was assumed to be the key factor dominating the easy axis reorientation.

Despite the fact that good agreement between the computed curves and the data (see Fig. 10) counts in favor of our simplified approach, a deeper insight into complicated molecular mechanisms behind the gliding under consideration requires additional experimental studies and a more systematic theoretical treatment of the processes involved. Such treatment has to deal with the interplay of photoinduced ordering in azo-dye films, the anchoring energy effects [38] and the adsorption-desorption processes [72–75] underlying the gliding phenomenon.

This work was partially supported by grants: Development of the Higher Schools Scientific Potential 2.1.1/5873; Grant NK-410P; HKUST CERG RPC07/08.EG01 and CERG 612208, 612409.

[1] Yue Zhao and Tomiki Ikeda, eds., Smart light-responsive materials: Azobenzene-containing polymers and liquid crystals (Wiley, New Jersey, USA, 2009) p. 514.

[2] F. Weigert, “A new effect of the rays in light-sensitive layers,” Verh. Dtsch. Phys. Ges. 21, 479–491 (1919).

[3] M. Eich, J. H. Wendorff, B. Reck, and H. Ringsdorf, “Reversible digital and holographic optical storage in polymeric liquid crystals,” Makromol. Chem., Rap. Commun. 8, 59–63 (1987).

[4] A. Natansohn, S. Xie, and P. Rochon, “Azo polymers for reversible optical storage. 2.

Poly[4^′-[[2-(acryloyloxy)ethyl]ethylamino]-2-chloro-4-nitroazobenzene],” Macromolecules 25, 5531–5532 (1992).

[5] P. N. Prasad, J. E. Mark, and T. J. Fai, eds., Polymers and other advanced materials (Plemun Press, NY, 1995).

[6] L. M. Blinov, M. V. Kozlovsky, and G. Cipparrone, “Photochromism and holographic grating recording on a chiral side-chain liquid crystalline copolymer containing azobenzene chromophores,” Chem. Phys. 245, 473–485 (1999).

[7] D.-K. Yang and S.-T. Wu, Fundamentals of Liquid Crystal Devices, Series in Display Technology (Wiley, Chichester, 2006) p. 378.

[8] V. G. Chigrinov, V. M. Kozenkov, and H.-S. Kwok, Photoalignment of Liquid Crystalline Materials: Physics and Applications, Series in Display Technology (Wiley, Chichester, 2008) p. 219.

[9] M. O’Neill and S. M. Kelly, “Photoinduced surface photoalignment for liquid crystal displays,” J. Phys. D: Appl. Phys. 33, R67–R84 (2000).

[10] V. G. Chigrinov, V. M. Kozenkov, and H. S. Kwok, “New developments in photo-aligning and photo-patterning technologies: physics and applications,” in Optical applications in photoaligning, edited by L. Vicari (Inst. of Physics, Bristol, UK, 2003) pp. 201–244.

[11] W. M. Gibbons, P. J. Shannon, S.-T. Sun, and B. J. Swetlin, “Surface-mediated alignment of nematic liquid crystals with polarized laser light,” Nature 351, 49–50 (1991).

[12] S. Furumi, M. Nakagawa, S. Morino, and K. Ichimura, “Photogeneration of high pretilt angles of nematic liquid crystals by azobenzene-containing polymer films,” Appl. Phys. Lett. 74, 2438–2440 (1999).

[13] M. Schadt, K. Schmitt, V. Kozinkov, and V. Chigrinov, “Surface-induced parallel alignment of liquid crystals by linearly polymerized photopolymers,” Jpn. J. Appl. Phys. 31, 2155–2164 (1992).

[14] A. G. Dyadyusha, T. Ya. Marusii, Yu. A. Reznikov, A. I. Khizhnyak, and V. Yu. Reshetnyak, “Orientational effect due to a change in the anisotropy of the interaction between a liquid crystal and a bounding surface,” JETP Lett. 56, 17 (1992).

[15] H. G. Galabova, D. W. Allender, and J. Chen, “Orientation and surface anchoring of nematic liquid crystals on linearly polymerized photopolymers,” Phys. Rev. E 55, 1627–1631 (1996).

[16] S. Perny, P. Le Barny, J. Delaire, T. Buffeteau, C. Sourisseau, I. Dozov, S. Forget, and P. Martinot-Lagarde, “Photoinduced orientation in poly(vinylcinnamate) and poly(7- methacryloyloxycoumarin) thin films and the consequences on liquid crystal alignment,” Liq. Cryst. 27, 329–340 (2000).

[17] A. Petry, S. Kummer, H. Anneser, F. Feiner, and Ch. Bräuchle, “Photoinduced reorientation of cholesteric liquid crystalline polysiloxinanes and applications in optical information storage and second harmonic,” Ber. Bunsenges. Phys. Chem. 97, 1281–1286 (1993).

[18] N. C. R. Holme, P. S. Ramanujam, and S. Hvilsted, “Photoinduced anisotropy measurements in liquid-crystalline azobenzene side-chain polyesters,” Applied Optics 35, 4622–4627 (1996).

[19] L. Blinov, M. Kozlovsky, M. Ozaki, K. Skarp, and K. Yoshino, “Photoinduced dichroism and optical anisotropy in a liquid-crystalline azobenzene side chain polymer caused by anisotropic angular distribution of trans and cis isomers,” J. Appl. Phys. 84, 3860–3866 (1998).

[20] Y. Wu, J.-I. Mamiya, O. Tsutsumi, A. Kanazawa, T. Shiono, and T. Ikeda, “Photoinduced alignment of polymer liquid crystals containing azobenzene moieties in the side group VII. On He-Ne laser beam irradiation,” Liq. Cryst. 27, 749–753 (2000).

[21] U. Wiesner, N. Reynolds, Ch. Boeffel, and H. W. Spiess, “An infrared spectroscopic study of photo-induced reorientation in dye containing liquid-crystalline polymers,” Liq. Cryst. 11, 251–267 (1992).

[22] O. Yaroshchuk, A. D. Kiselev, Yu. Zakrevskyy, J. Stumpe, and J. Lindau, “Spatial reorientation of azobenzene side groups of a liquid crystalline polymer induced by linearly polarized light,” Eur. Phys. J. E 6, 57–67 (2001).

[23] T. G. Pedersen and P. M. Johansen, “Mean-field theory of photoinduced molecular reorientation in azobenzene liquid crystalline side-chain polymers,” Phys. Rev. Lett. 79, 2470–2473 (1997).

[24] T. G. Pedersen, P. M. Johansen, N. C. R. Holme, P. S. Ramanujam, and S. Hvilsted, “Theoretical model of photoinduced anisotropy in liquid crystalline azobenzene side-chain polyesters,” J. Opt. Soc. Am. B 15, 1120–1129 (1998).

[25] G. A. Puchkovs’ka, V. Yu. Reshetnyak, A. G. Tereshchenko, O. V. Yaroshchuk, and J. Lindau, “Kinetic characteristics of light induced anisotropy and mechanisms of the molecular alignment in azo dye containing polymer films,” Mol. Cryst. Liq. Cryst. 321, 31–43 (1998).

[26] Sz. Sajti, Á. Kerekes, M. Barabás, E. Lörincz, S. Hvilsted, and P. S. Ramanujam, “Simulation of erasure of photoinduced anisotropy by circularly polarized light,” Opt. Commun. 194, 435– 442 (2001).

[27] A. D. Kiselev, “Kinetics of photoinduced anisotropy in azopolymers: models and mechanisms,” J. Phys.: Condens. Matter 14, 13417–13428 (2002).

[28] Z. Sekkat, D. Yasumatsu, and S. Kawata, “Pure photoorientation of azo dye in polyurethanes and quantification of orientation of spectrally overlapping isomers,” Journal of Physical Chemistry B 106, 12407–12417 (2002).

[29] A. Natansohn, P. Rochon, X. Meng, C. Barett, T. Buffeteau, S. Bonenfant, and M. Pezolet, Macromolecules 31, 1155 (1998).

[30] T. Buffeteau and M. Pézolet, “Photoinduced orientation in azopolymers studied by infrared spectroscopy: cooperative and biaxial orientation in semicrystalline polymers,” Macromolecules 31, 2631–2635 (1998).

[31] A. Kiselev, O. Yaroshchuk, Yu. Zakrevskyy, and A. Tereshchenko, “On biaxiality of photoinduced structures in azopolymer films,” Condens. Matter Phys. 4, 67–75 (2001).

[32] O. V. Yaroshchuk, A. D. Kiselev, Yu. Zakrevskyy, T. Bidna, J. Kelly, L.-C. Chien, and J. Lindau, “Photoinduced three-dimensional order in side chain liquid crystalline azopolymers,” Phys. Rev. E 68, 011803–(1–15) (2003).

[33] L. S. Kaanumalle, A. Natarayan, and V. Ramamurthy, “Medium effects on photochemical processes: Organized and confined media,” in Synthetic Organic Chemistry, Molecular and supramolecular photochemistry, Vol. 12, edited by G. G. Axel and J. Mattay (Marcel Dekker, NY, 2005) Chap. 18, pp. 553–618.

[34] A. D. Kiselev, V. G. Chigrinov, H.-S. Kwok, An. Murauski, and Al. Muravsky, “Biaxiality effects in kinetics of photoinduced orientational structures in azo-dye films,” in Proceedings of the VIII-th International Display Workshop’08 (SID, Nigata, Japan, 2008) pp. 573–574.

[35] A. D. Kiselev, V. G. Chigrinov, and H.-S. Kwok, “Kinetics of photoinduced ordering in azo-dye films: Two-state and diffusion models,” Phys. Rev. E 80, 011706 (2009).

[36] V. Chigrinov, E. Prudnikova, V. Kozenkov, H. Kwok, H. Akiyama, T. Kawara, H. Takada, and H. Takatsu, “Syntesis and properties of azo dye aligning layers for liquid crystal cells,” Liq. Cryst. 29, 1321–1327 (2002).

[37] V. Chigrinov, A. Muravski, and H. S. Kwok, “Anchoring properties of photoaligned azo-dye materials,” Phys. Rev. E 68, 061702 (2003).

[38] A. D. Kiselev, V. G. Chigrinov, and D. D. Huang, “Photo-induced ordering and anchoring properties of azo-dye films,” Phys. Rev. E 72, 061703 (2005).

[39] A. Muravsky, A. Murauski, V. Chigrinov, and H.-S. Kwok, “Light printing of grayscale pixel images on optical rewritable electronic paper,” Jpn. J. Appl. Phys. 47, 6347–6353 (2008).

[40] V. P. Vorflusev, H-S Kitzerow, and V. Chigrinov, “Azimuthal surface gliding of a nematic liquid crystal,” Appl. Phys. Lett. 70, 3359 (1997).

[41] S. V. Pasechnik, V. G. Chigrinov, D. V. Shmeliova, V. A. Tsvetkov, V. N. Kremenetsky, L. Zhijian, and A. V. Dubtsov, “Slow relaxation processes in nematic liquid crystals at weak surface anchoring,” Liq. Cryst. 33, 175–185 (2006).

[42] A. V. Dubtsov, D. V. Shmeliova, S. V. Pasechnik, Alexei D. Kiselev, and V. G. Chigrinov, “Effects of polarization azimuth in dynamics of electrically assisted light-induced gliding of nematic liquid-crystal easy axis,” Appl. Phys. Lett. 100, 141608 (2012).

[43] P. G. de Gennes and J. Prost, The Physics of Liquid Crystals (Clarendon Press, Oxford, 1993) p. 596.

[44] J. I. Lauritzen and R. Zwanzig, “Dielectric relaxation of a single axis rotator with two equivalent sites,” Advances in Molecular Relaxation Processes 5, 339–361 (1973).

[45] W. T. Coffey, Yu. P. Kalmykov, E. S. Massawe, and J. T. Waldron, “Exact solution for the correlation times of dielectric relaxation of a single axis rotor with two equivalent sites,” J. Chem. Phys. 99, 4011–4023 (1993).

[46] J.-L. Dejárdin, G. Debiais, and A. Ouadjou, “On the dielectric behavior of dielectric relaxation in alternating fields. II. Analytic expressions of nonlinear susceptibilities,” J. Chem. Phys. 98, 8149–8153 (1993).

[47] J.-L. Dejárdin and Yu. P. Kalmykov, “Nonlinear dielectric relaxation of polar molecules in a strong ac electric field: Steady state response,” Phys. Rev. E 61, 1211–1217 (2000).

[48] Y. P. Kalmykov and K. P. Quinn, “The rotational Brownian motion in a linear molecule and its application to the theory of Kerr effect relaxation,” J. Chem. Phys. 95, 9142–9147 (1991).

[49] B. U. Felderhof, “Nonlinear response of a dipolar system with rotational diffusion to a rotating field,” Phys. Rev. E 66, 051503 (2002).

[50] Y. P. Kalmykov, “Rotational Brownian motion and nonlinear dielectric relaxation asymmetric top molecules in strong electric fields,” Phys. Rev. E 65, 021101 (2001).

[51] Y. P. Kalmykov and S. V. Titov, “Anisotropic rotational diffusion and transient nonlinear responses of rigid macromolecules in a strong external electric field,” J. Chem. Phys. 126, 174903 (2007).

[52] P. L. Nordio and P. Busolin, “Electron spin resonance line shapes in partially oriented systems,” J. Chem. Phys. 55, 5485–5490 (1971).

[53] R. Tarroni and C. Zannoni, “On the rotational diffusion of asymmetric molecules in liquid crystals,” J. Chem. Phys. 95, 4550–4564 (1991).

[54] G. R. Luckhurst and A. Sanson, “Angular dependent line widths for a spin probe dissolved in a liquid crystal,” Mol. Phys. 24, 1297–1311 (1972).

[55] D. Berggren, R. Tarroni, and C. Zannoni, “Rotational diffusion of uniaxial probes in biaxial liquid crystal phases,” J. Chem. Phys. 99, 6180–6200 (1993).

[56] A. Ferrarini, P. L. Nordio, and G. J. Moro, “Diffusion models for molecular motion in uniaxial mesophases,” in The molecular physics of liquid cristals, edited by G. R. Luckhurst and C. A. Veracini (Kluwer Academic, Dordrecht, 1994) pp. 41–69.

[57] A. Brognara, P. Pasini, and C. Zannoni, “Roto-translational diffusion of biaxial probes in uniaxial liquid crystal phases,” J. Chem. Phys. 112, 4836–4848 (2000).

[58] P. L. Nordio and U. Serge, “Rotational dynamics,” in The molecular physics of liquid cristals, edited by G. R. Luckhurst and G. W. Gray (Academic Press, London, 1979) Chap. 18.

[59] G. Moro and P. L. Nordio, “Orientation dependent friction in liquid crystals,” Mol. Cryst.

Liq. Cryst. 104, 361–376 (1984).

[60] I. Dozov, N. Kirov, and B. Petroff, “Molecular biaxiality and reorientational correlation functions in nematic phases: theory,” Phys. Rev. A 36, 2870–2878 (1987).

[61] M. P. Fontana, B. Rosi, N. Kirov, and I. Dozov, “Molecular orientational motion in liquid crystals: a study by Raman and infrared band-shape analysis,” Phys. Rev. A 33, 4132–4142 (1986).

[62] T. D. Frank, Nonlinear Fokker–Planck Equations, edited by H. Haken, Springer Series in Synergetics (Springer, Berlin, Heidelberg, 2005) p. 404.

[63] M. Abramowitz and I. A. Stegun, eds., Handbook of Mathematical Functions (Dover, New York, 1972).

[64] Yu. A. Kuznetsov, Elements of Applied Bifurcation Theory, 2nd ed., Applied Mathematical Sciences, Vol. 112 (Springer, NY, 1998) p. 592.

[65] J. K. Hale and H. Kocak, Dynamics and Bifurcations, Texts in Applied Mathematics, Vol. 3 (Springer, NY, 1991) p. 567.

[66] F. C. Hoppensteadt, Analysis and Simulation of Chaotic Systems, 2nd ed., Applied Mathematical Sciences, Vol. 94 (Springer, NY, 2000) p. 315.

[67] D. Voloshchenko, A. Khizhnyak, Yu. Reznikov, and V. Reshetnyak, “Control of an easy axis on nematic-polymer interface by light action to nematic bulk,” Jpn. J. Appl. Phys. 34, 566–571 (1995).

[68] D. Andrienko, A. Dyadyusha, Yu. Kurioz, V. Reshetnyak, and Yu. Reznikov, “Light-induced anchoring transitions and bistable nematic alignment on polysiloxane-based alignment surface,” Mol. Cryst. Liq. Cryst. 321, 299–307 (1998).

[69] A. V. Dubtsov, S. V. Pasechnik, Alexei D. Kiselev, D. V. Shmeliova, and V. G. Chigrinov, “Electrically assisted light-induced azimuthal gliding of the nematic liquid-crystal easy axis on photoaligned substrates,” Phys. Rev. E 82, 011702 (2010).

[70] S. V. Pasechnik, A. V. Dubtsov, D. V. Shmeliova, V. A. Tsvetkov, and V. G. Chigrinov, “Effect of combined action of electric field and light on gliding of the easy axis in nematic liquid crystals,” Liq. Cryst. 35, 569–579 (2008).

[71] A. L. Alexe-Ionescu, C. Uncheselu, L. Luchetti, and G. Barbero, “Phenomenological model for the optically induced easy direction,” Phys. Rev. E 75, 021701 (2007).

[72] P. Vetter, Y. Ochmura, and T. Uchida, “Study of memory alignment of nematic liquid crystals on polyvinyl alcohol coatings,” Jpn. J. Appl. Phys. 32, L1239–L1241 (1993).

[73] E. Ouskova, Yu. Reznikov, S. V. Shiyanovskii, L. Su, J. L. West, O. V. Kuksenok, O. Francescangeli, and F. Simoni, “Photo-orientation of liquid crystals due to light-induced desorption and adsorption of dye molecules on an aligning surface,” Phys. Rev. E 64, 051709 (2001).

[74] G. Barbero and L. R. Evangelista, Adsorption phenomena and anchoring energy in nematic liquid crystals, The Liquid Crystals Book Series (Taylor & Francis Group, LLC, Boca Raton, 2006) p. 352.

[75] D. Fedorenko, K. Slyusarenko, E. Ouskova, V. Reshetnyak, K. Ha, R. Karapinar, and Yu.

Reznikov, “Light-induced gliding of the easy orientation axis of a dye-doped nematic liquid crystal,” Phys. Rev. E 77, 061705 (2008).