arXiv:1210.3465v1 [astro-ph.CO] 12 Oct 2012

AKARI Infrared Camera Survey of the Large Magellanic Cloud. I. Point Source Catalog

Daisuke Kato^{1,2,3}, Yoshifusa Ita^4, Takashi Onaka^1, Toshihiko Tanabé^5, Takashi Shimonishi^{1,10}, Itsuki Sakon^1, Hidehiro Kaneda^6, Akiko Kawamura^7, Takehiko Wada^2, Fumihiko Usui^2, Bon-Chul Koo^8, Mikako Matsuura^9, and Hidenori Takahashi^5

kato@ir.isas.jaxa.jp; onaka@astron.s.u-tokyo.ac.jp

1Department of Astronomy, Graduate School of Science, The University of Tokyo, 7-3-1, Hongo, Bunkyo-ku, Tokyo, 113-0033, Japan

– 2 –

Received ; accepted

2Institute of Space and Astronautical Science, Japan Aerospace Exploration Agency, 3- 1-1, Yoshino-dai, Chuo-ku, Sagamihara, Kanagawa, 252-5210, Japan 3Center for Low Carbon Society Strategy, Japan Science and Technology Agency, 7, Goban-cho, Chiyoda-ku, Tokyo, 102-0076, Japan

4Astronomical Institute, Tohoku University, 6-3, Aramaki, Aoba-ku, Sendai, Miyagi, 980- 8578, Japan

5Institute of Astronomy, School of Science, The University of Tokyo, 2-21-1 Osawa, Mitaka, Tokyo 181-0015, Japan

6Department of Astrophysics, Nagoya University, Chikusa-ku, Nagoya, 464-8602, Japan 7National Astronomical Observatory of Japan, 2-21-1 Osawa, Mitaka, Tokyo, 181-8588, Japan

8Department of Physics and Astronomy, Seoul National University, Seoul 151-742, Korea 9Department of Physics and Astronomy, University College London, Gower Street, London WC1E 6BT, UK

10Present address: Department of Earth and Planetary Sciences, Graduate School of Science, Kobe University, Nada Kobe 657-8501, Japan

– 3 –

ABSTRACT

We present a near- to mid-infrared point source catalog of 5 photometric bands at 3.2, 7, 11, 15 and 24 μm for a 10 deg^2 area of the Large Magellanic Cloud (LMC) obtained with the Infrared Camera (IRC) onboard the AKARI satellite. To cover the survey area the observations were carried out at 3 separate seasons from 2006 May to June, 2006 October to December, and 2007 March to July.

The 10-σ limiting magnitudes of the present survey are 17.9, 13.8, 12.4, 9.9, and 8.6 mag at 3.2, 7, 11, 15 and 24 μm, respectively. The photometric accuracy is estimated to be about 0.1 mag at 3.2 μm and 0.06–0.07 mag in the other bands. The position accuracy is 0.^{′′}3 at 3.2, 7 and 11 μm and 1.^{′′}0 at 15 and 24 μm. The sensitivities at 3.2, 7, and 24 μm are roughly comparable to those of the Spitzer SAGE LMC point source catalog, while the AKARI catalog provides the data at 11 and 15 μm, covering the mid-infrared spectral range contiguously. Two types of catalog are provided: a Catalog and an Archive. The Archive contains all the detected sources, while the Catalog only includes the sources that have a counterpart in the Spitzer SAGE point source catalog. The Archive contains about 650,000, 140,000, 97,000, 43,000, and 52,000 sources at 3.2, 7, 11, 15, and 24 μm, respectively. Based on the catalog, we discuss the luminosity functions at each band, the color-color diagram, and the color-magnitude diagram using the 3.2, 7, and 11 μm band data. Stars without circumstellar envelopes, dusty C-rich and O-rich stars, young stellar objects, and background galaxies are located at distinct regions in the diagrams, suggesting that the present catalog is useful for the classification of objects towards the LMC.

Subject headings: Galaxies: Magellanic Clouds — Infrared: stars — Infrared: galaxies

– 4 –

— Surveys — Catalogues

– 5 –

1. Introduction

The Large Magellanic Cloud (LMC) is one of the nearest galaxies. The proximity of the LMC (∼50 kpc; e.g., Alves 2004) allows us to study individual stars in detail. The mean metallicity of the LMC is also known to be small (∼1/4) compared to the solar abundance (e.g., Luck et al. 1998), providing us with an ideal place to study formation and evolution of stars in low metallicity environments.

Individual stars in the LMC have been observed by large area surveys at optical and near-infrared (NIR) wavelengths. Zaritsky et al. (2004) detected about 2.4 × 10^7 point sources in a UBV I survey over a 64 deg^2 area of the LMC, whereas Kato et al. (2007) observed about 1.5 × 10^7 point sources with a JHK_s survey of a 40 deg^2 region. At mid-infrared (MIR) wavelengths, the Midcourse Space Experiment (MSX) carried out a survey over a 100 deg^2 area of the LMC (Egan et al. 2001, 2003) and detected a few thousand sources despite of the short integration time and low spatial resolution. Two recent infrared satellites, Spitzer Space Telescope (Werner et al. 2004) and AKARI (Murakami et al. 2007), provided a capability of deep mid-infrared observations with better spatial resolution. The Spitzer SAGE project (Meixner et al. 2006) carried out a uniform and unbiased imaging survey of a 49 deg^2 area of the LMC at 4 photometric bands from 3 to 8 μm of IRAC (Fazio et al. 2004) and 3 bands at 24, 70, and 160 μm of MIPS (Rieke et al. 2004), to which the SAGE-Spec performed follow-up spectroscopic observations in the MIR and far-infrared (FIR) (Kemper et al. 2010; van Loon et al. 2010; Woods et al. 2011). Recently Herschel Space Observatory also made a survey observation over a 8^∘ × 8.5^∘ area of the LMC with spatial resolution higher than Spitzer in the FIR (Meixner et al. 2010).

The AKARI Large Magellanic Cloud Survey consists of a NIR to MIR imaging and near-infrared spectroscopic survey toward the LMC. The survey aims at a thorough study of the lifecycle of matters and the star-formation history of the LMC on a galactic scale

– 6 –

owing to its wide spatial coverage and high sensitivities over the wide spectral range (Ita et al. 2008). The sensitivities are comparable to those of the Spitzer SAGE survey and the AKARI survey covers the MIR spectral range contiguously, which fills the gap between the Spitzer/IRAC and MIPS bands. In addition to the dedicated survey observations, the entire LMC was observed as part of the all-sky survey at 6 bands from the MIR to the FIR (Ishihara et al. 2010; Kawada et al. 2007). The MIR point source catalog at 9 and 18 μm and the FIR point source catalog at 65, 90, 140 and 160 μm have been produced from the all-sky survey observations and released to the public (Ishihara et al. 2010; Yamamura et al. 2010). These AKARI observations provide 11 band data of the LMC from the NIR to the FIR, which give us a unique and useful database for the study of the LMC.

A brief description of the AKARI LMC survey and early results have been given in Ita et al. (2008) based on a preliminary version of the catalog. The catalog has been revised by improving the data reduction procedure, which increases the reliability and accuracy of the photometric results. In this paper, we describe the point source catalog from the imaging survey of the LMC from the NIR to the MIR using the latest version of the data reduction process, which will be released to the public. We outline the AKARI LMC survey observations in §2, the data reduction procedures in §3, and the structure of the catalog in §4. The general characteristics of the catalog are presented in §5, and the properties of the sources in the catalog are discussed in §6. A summary is given in §7.

2. Observations

The AKARI telescope has an effective aperture of 685 mm (Kaneda et al. 2007) and the whole telescope system including the focal-plane instruments was cooled by liquid Helium and onboard mechanical coolers. The AKARI spacecraft was brought into a sun-synchronous polar orbit at an altitude of 700 km along the twilight zone, similar to that

– 7 –

of the IRAS satellite. The LMC is located near the south ecliptic pole, where the polar orbit has high visibility. Taking this advantage, we observed the main part of the LMC contiguously.

The AKARI LMC survey was carried out with the Infrared Camera (IRC: Onaka et al. 2007) in the pointing observation mode (Murakami et al. 2007). It has 3 independent channels: NIR (1.8−5.5 μm), MIR-S (4.6−13.4 μm), and MIR-L (12.6−26.5 μm). Each channel has a wide field of view (FoV) of about 10^′ × 10^′ and is equipped with 3 imaging filters and 2 dispersion elements, which can be switched during a pointing observation. Of these, we use 5 imaging filters at 3.2 (N3), 7 (S7), 11 (S11), 15 (L15), and 24 μm (L24), and the prism for slitless spectroscopy in 2–5 μm (NP) of a spectral resolution of λ/Δλ ∼ 20 (Ohyama et al. 2007), where the symbol in parentheses indicates the filter designation. The imaging bands cover the spectral range from 5 to 26 μm contiguously and the S11 and L15 bands fill the gap in the wavelength coverage between the IRAC and MIPS onboard Spitzer. The present photometric catalog is produced from the imaging data. Part of the data taken in the slit-less spectroscopic mode are reported in Shimonishi et al. (2008). The data reduction and the extracted spectra with the slit-less spectroscopic mode will be given separately (Shimonishi et al. 2012).

We use the AKARI IRC AOT02 observation template with a special option (using the prism instead of the N4 filter) prepared for the LMC survey. The template is designed to take images with 2 filters in each channel at 3 dithered sky positions in a pointing observation. At each position, both short- and long-exposure data are taken. The net integration time for a long-exposure image is typically 133, 147, and 147 s for the NIR, MIR-S, and MIR-L channels, respectively, and that for a short-exposure image is 14.0, 1.75, and 1.75 s, respectively (Table 3). The long-to-short exposure time ratio of a pointing observation is 9.5, 28, and 28 for the NIR, MIR-S, and MIR-L channels, respectively, which

– 8 –

increases the dynamic range of the observations (see §3.5.2).

The NIR and MIR-S channels share the same FoV by means of the beam splitter, and thus N3, NP, S7, and S11 images are taken at the same region simultaneously. L15 and L24 images of the same region are taken at a different pointing observation since their FoV is located 20^′ away from that of the NIR/MIR-S in the direction perpendicular to the AKARI orbit (Onaka et al. 2007). The FoV of the AKARI telescope moves along the ecliptic meridian in the twilight zone, which changes its direction with the Earth’s yearly round. Therefore, the telescope can observe a given celestial position twice a year. The position of the MIR-L channel relative to the NIR and MIR-S channels is flipped in projection on the sky at a season separated by half a year because the satellite moves in the opposite direction. Taking account of the change in the projection direction, we optimize the target positions to maximize the area observed by all the three IRC channels with the overlapping region of 1.^′5 for each image.

Observations were carried out in 3 separate seasons, from 2006 May 6 to June 8, from 2006 October 2 to December 31, and from 2007 March 24 to July 2. Over 600 pointing observations were devoted to this project, yielding imaging and spectroscopic maps of about a 10 deg^2 area of the main part of the LMC. Figure 1 shows the area where the AKARI survey was carried out together with the areas of other surveys.

3. Data reduction and compilation of the point source catalog

3.1. Imaging data reduction

Standard procedures for the reduction of imaging data obtained with infrared arrays, dark subtraction, flat-fielding, and image co-addition, are performed in the IRC data reduction toolkit version 20110304 (Lorente et al. 2008). Since the basic data reduction

– 9 –

is carried out in the standard tool kit with the default options, we briefly summarize the procedures below.

1. Firstly the detector non-linearity is corrected for in each exposure image. Deviations from the ideal linear response are estimated to be smaller than 5% at 12000, 20000, and 20000 ADU for NIR, MIR-S, and MIR-L, respectively, which roughly correspond to the saturation levels of 0.26, 1.9, 1.8, 2.5, and 22 Jy for the short-exposure data at N3, S7, S11, L15, and L24, respectively (see also Table 3).

2. The dark image is subtracted from each image. We use the dark data taken at the beginning of the pointing observation sequence (“pre-dark”) for the MIR-S and MIR-L long-exposure images by averaging 3 long-exposure data (“self-dark”). For all the short-exposure and NIR long-exposure images, we use the “super-dark” images, which are created by averaging more than 70 “pre-dark” images in the LMC observations and are provided as the default dark data in the IRC toolkit. To correct for the possible time variation between the “super-dark” and the dark image at the time of observation, the signal level of the “super-dark” image is scaled to that of the observed image at the slit mask region before the dark subtraction, assuming that the dark image pattern does not change with time.

3. Signals due to high-energy ionizing particle hits (hereafter cosmic-rays) are removed with the task COSMICRAYS in IRAF. Remaining faint comic-ray events are removed by median-average in step 6.

4. Each image is divided by the flat-field image to correct for the the pixel-to-pixel variation in the sensitivity over the arrays. We employ the “super flat-field” images created from images near the North Ecliptic Pole, where the smooth zodiacal emission dominates. We use the MIR-L flat data, in which the effect of the artifacts by internal reflections is corrected (Arimatsu et al. 2011).

– 10 –

5. The aspect ratio of each image is adjusted to 1 to 1 by resampling the image. After the adjustment, the deviation from an ideal grid square is 0.2–0.3 pixel in the NIR and MIR-S images. In the MIR-L images, the deviation becomes ∼1 pixel at the edge of the detector. The final pixel scale of the rescaled images is 1.^{′′}446, 2.^{′′}340 and 2.^{′′}384 for the NIR, MIR-S, and MIR-L images, respectively.

6. Images taken at dithered positions are spatially aligned and co-added by taking their median to eliminate any array anomalies, such as bad, dead, or hot pixels, and remaining cosmic-ray events. Images are taken at least at 3 different positions in a pointing observation in the observation template AOT02.

3.2. Source Detection and Photometry

We perform source detection with the IRAF^1/DAOFIND and photometry with the IRAF/DAOPHOT package (Stetson 1987) on co-added images. We develop a procedure for the photometry with the point spread function (PSF) fitting, which is similar to that used by the Spitzer GLIMPSE^2 team (Benjamin et al. 2003). The procedure of the source detection and photometry involves the following steps:

1. DAOFIND is used to extract point-like sources whose fluxes are more than 2 σ above the background. The extracted sources include those slightly extended compared to the PSF.

1 IRAF is distributed by the National Optical Astronomy Observatories, which are operated by the Association of Universities for Research in Astronomy, Inc., under cooperative agreement with the National Science Foundation.

2 http://www.astro.wisc.edu/glimpse/, and see the document “Description of Point Source Photometry Steps Used by GLIMPSE”, by B. L. Babler.

– 11 –

2. The aperture photometry is performed on the extracted sources with an aperture radius of 10.0 pixels for N3 images, and of 3.0 pixels for other band images using the PHOT task in IRAF. The radius of 10.0 pix at N3 is the same as the one used for the absolute flux calibration (Tanabé et al. 2008). Therefore, we do not apply aperture corrections for the photometry at N3. For the MIR band images, we adopt a smaller aperture than that used in the calibration (7.5 pix) because of the large background emission in the LMC at the MIR and thus the aperture correction is needed (see step 6). The inner radius of the sky annulus is set as the same as the aperture radius and the width of the sky annulus is set as 5.0 pixels.

3. Bright but unsaturated sources without any other sources within 7 pixels are selected from the results of step 2 to construct the PSF. At least 8 of such “good” sources are selected in the N3, S7, and S11 images, and 5 in the L15 and L24 images.

4. The “good” sources selected in step 3 are used to construct a model PSF for each N3 image since the PSF in the N3 images notably varies from pointing to pointing possibly due to jitters in the satellite pointing. We use the PSF task in DAOPHOT to choose the best fitting function by trying several different types of fitting functions in each image.

For the S7, S11, L15, and L24 images, we use the common PSFs constructed in advance for each band, instead of constructing them from each image since the effect of the jitter in the satellite pointing is negligible compared to the size of the PSFs. The common PSFs are constructed from about 10 “good” sources, which are selected from the images taken with the LMC survey and the observations of 47 Tuc (Ita et al. 2007); sources free from diffuse emission are carefully chosen by eyes. To construct the common PSFs, the “moffat25”, “lorentz”, “moffat15”, and “gauss” models are applied at S7, S11, L15, and L24, respectively.

– 12 –

5. The PSF-fitting photometry is performed for the extracted sources in step 2 using ALLSTAR in DAOPHOT in an iterative manner. After the first ALLSTAR procedure is applied for the extracted sources, the sources for which photometry has been carried out are removed from the output image of ALLSTAR. Then the ALLSTAR is applied again for the remaining sources. We repeat the ALLSTAR procedure 3 times to have photometry for all the extracted sources. This is a procedure similar to the one adopted by the GLIMPSE team.

6. The aperture correction is applied to the PSF-fitting results. The aperture correction factors and the PSFs of each band are assumed to be the same among the images. The correction factor is estimated from the median of the differences between the results of the aperture photometry with an aperture of 7.5 and 3.0 pixels applied to all the sources used to construct the “common” PSFs since the absolute calibration was carried out with the aperture photometry with the 7.5 pixel radius for the MIR-S and MIR-L images (Tanabé et al. 2008).

We compare the results of the aperture photometry with those of the PSF-fitting photometry. For the aperture photometry, only steps 1, 2 and 6 above are performed.

3.3. Photometric Calibration

The resultant instrumental signals are converted into physical units using the IRC flux conversion factors (Lorente et al. 2008). Then the calibrated flux densities are converted into magnitudes of the IRC-Vega system using the zero-magnitude flux densities tabulated in Table 3. The differences between the instrumental and the calibrated magnitudes are constants. The zero-magnitude flux densities are estimated for the short- and long-exposure images in each band using the relative spectral response in Onaka et al. (2007). The

– 13 –

IRC flux is calibrated against the spectral energy distribution (SED) of f_λ ∝ λ^{−1} or f_ν ∝ ν^{−1}. The color correction factors for objects with different SEDs are tabulated in Lorente et al. (2008). The photometric uncertainty includesthe read-out noises, and the errors in the aperture correction factors and the ADU-to-Jy conversion factors. The values of the read-out noises and the errors of the ADU-to-Jy conversion factors are taken from Tanabé et al. (2008).

3.4. Astrometric Calibration

The attitude control system of the AKARI satellite has an absolute position accuracy no better than 5^{′′} (the requirement was 30^{′′}) and thus the astrometric calibration using other catalogs is necessary to improve the position information of the images. We calculate the coordinate transformation matrix that relates the image pixel coordinates to the sky coordinates by matching the detected point sources in the N3 images with the Two Micron All Sky Survey Point Source Catalog (2MASS-PSC; Skrutskie et al. 2006), and those in the MIR-S and MIR-L images with the Spitzer SAGE LMC point source catalog version 3.1^3(SAGE-PSC; Meixner et al. 2006). Sources detected in the MIR-S images are matched with the IRAC [8.0] sources, and those detected in the MIR-L images are with the MIPS [24] sources, respectively, where the numbers bracketed by [ ] designate the band of the SAGE catalog; for instance, [3.6] indicates the IRAC 3.6 μm band. The procedure is summarized in the following.

1. The equatorial coordinates (α_i, δ_i) of the 2MASS/SAGE sources in each field are converted to (X_i, Y_i) in the World Coordinate System (WCS).

2. Bright sources in each long-exposure image are extracted.

3 http://ssc.spitzer.caltech.edu/spitzermission/observingprograms/legacy/sage/

– 14 –

3. A triangle matching between the 2MASS/SAGE sources in the WCS (X_i, Y_i) and the sources in the pixel coordinates (x_j , y_j) in AKARI images is performed with the task XYXYMATCH in IRAF.

4. The transformation matrix is calculated using the pixel coordinates (x_i, y_i) and the equatorial coordinates (α_i, δ_i) of the matched catalog sources with CCMAP in IRAF. The second, third, and fourth orders of polynomials are examined, and then the one with the smallest residuals is adopted.

We use at least 5 sources that match with the catalogued sources for the calculation. For one S11, 5 L15, and 74 L24 images, automatic matching with the SAGE catalog is unsuccessful due to the small number of the sources in the images. In such cases, we match the detected point sources with the SAGE-PSC by eye. We use only 4 sources for the manual matching and thus the positional accuracy in these images could be worse than those in others. Point source matching does not always work for short-exposure images due to the paucity of detected point sources. For 32 S7 and 150 S11 short-exposure images, we could not obtain a sufficient number of sources and the same matrix calculated for the corresponding long-exposure image is applied. The catalog used as the position reference (2MASS-PSC or SAGE-PSC) and the method (e.g., by eye) used for the matching are indicated by the flags for each source (see §4).

As described above, the astrometric reference of the present catalog is the 2MASS-PSC and SAGE-PSC. The equatorial coordinates of the 2MASS-PSC are based on the International Celestial Reference System (ICRS), and so is the SAGE-PSC via the 2MASS-PSC. Hence, the equatorial coordinates of the present catalog indirectly refer to the ICRS.

– 15 –

3.5. Final Product Generation

3.5.1. Duplicate Source

Each image has overlapping regions of 1.^′5 × 10.^′0 in its contiguous images. Duplicate sources in the overlapping regions are merged together with the criterion of the spatial proximity of |Δr| ≤ 3.^{′′}0. The flux density of the one with a better signal-to-noise ratio (S/N) is adopted and the other(s) is discarded. The number of the duplicate sources for each source in each band is denoted by the corresponding code (see §4). Note that in most cases the overlapping regions were observed in close pointing opportunities, but in some cases, they were observed in a different season. For a variable source, therefore, the present catalog gives the flux density at a brighter phase.

3.5.2. Merging Short- and Long-exposure Data

The above analysis produces 4 sets of the result of photometry for a source; 2 photometry methods (aperture or PSF-fitting) and 2 exposure time data (short or long). Taking account of the errors estimated from the 2 photometry methods, we adopt the results of the PSF-fitting photometry for the long-exposure data for all the 5 band images. For the short-exposure data, we adopt the results of the PSF-fitting photometry for the N3 images and those of the aperture photometry for the S7 and S11 images because reliable PSFs cannot be created for the S7 and S11. The consistency between the longand short-exposure data is confirmed by the aperture correction procedure in step 6 in § 3.2 (see also Tanabé et al. 2008). The MIR-L short-exposure data are not adopted in the production of the catalog because of their poor S/N.

To increase the dynamic range, we merge the photometry results of the short- and long-exposure data with a positional tolerance of 3.^{′′}0 at the N3, S7 and S11 bands. If a

– 16 –

source is detected both in the short- and long-exposure images, we adopt the one with a better S/N and discard the other. The adopted photometry method and the exposure time for a given source are indicated by the corresponding codes (see §4).

3.5.3. Band Merging

The photometry results are merged to collect 5 photometric band data for a given source by the following procedures: (1) merge the N3 list with the S7 list with a positional tolerance of 3.^{′′}0 to produced the N3-S7 list, (2) merge the N3-S7 list with the S11 list with a tolerance of 3.^{′′}0 to obtain the N3-S7-S11 list, (3) merge the N3-S7-S11 list with the L15 list with a tolerance of 5.^{′′}0 to make the N3-S7-S11-L15 list, and (4) merge the N3-S7-S11-L15 list with the L24 list with a tolerance of 5.^{′′}0 to obtain the final band-merged list. The matched source is regarded as the same object and the information is merged. The sources not matched remain as independent sources in the list. The number of the matched sources and the distance from the nearest matched source in the merging procedures (1)–(4) are given in the final catalog. If more than one sources in the shorter wavelength list are matched in position, the one with the shortest distance is identified as the same source. In such cases, the number of the position-matched sources is given for the source in question, but the source(s) that is not identified as the same source is regarded as a different source and the number of the matched sources is set as zero. Note that the number of the position-matched sources is always given at the longer wavelength band (Table 2). For each of the matched sources, the position of the shortest wavelength band is adopted as the source position. The band used for the source position determination is indicated by the corresponding code (see §4).

– 17 –

3.5.4. Artifact Identification

Similarly to the Spitzer IRAC images, the N3 images suffer from the “mux-bleed” (signals leaking from bright point sources, making false faint point-like sources every 4 pixels along a row, in which the bright sources are detected) and the “column pulldown” effects (reduction in intensity of the columns in which bright sources are detected). We identify and flag the suspected victims that are located within a belt of ±5 pixels wide along the rows/columns where bright (saturated) sources are detected. We also flag the sources located near very bright sources, using the proximity radius of 20 pixels for N3, and of 15 pixels for the other bands. The flagged sources should be used with care.

The S7 and S11 images suffer from the noticeable artifacts of bright sources due to the internal reflections in the beam splitter (Arimatsu et al. 2011). We flag the source located at the suspected artifact position that can be estimated accurately from the position of the bright source. No artifacts originating from the beamsplitter are appreciated or present at N3, L15 and L24, and thus no flag for the artifact is given at these bands. The format of the codes is described in §4.

3.5.5. Construction of Catalog and Archive

We construct two kinds of catalog, an Archive and a Catalog. The former includes all the detected sources and the latter contains only sources with high reliability.

The Catalog includes only sources that have counterparts in the SAGE-PSC. Although the band profiles of the AKARI IRC and the Spitzer IRAC/MIPS are not exactly the same, a source detected in the IRC band is likely to be detected in the corresponding IRAC/MIPS band because of their similar sensitivities (Fig. 3). We employ the Archive of the SAGE-PSC, which includes more sources than their Catalog, and match the N3 sources

– 18 –

with the [3.6] sources, S7, S11 and L15 with [8.0], and L24 with [24], with a positional tolerance of 3.^{′′}0. The Archive has more and fainter sources than the Catalog, which may contain potential false detection or sources with larger photometric uncertainties. In total, the Catalog contains 660,286 sources and the Archive has 802,285 sources.

4. The Catalog

Table 1 shows the entries for the first 10 sources of the Catalog. The Catalog and the Archive will only be electronically available^4. The record for a source consists of 554 bytes. Descriptions of each entry of the Catalog and the Archive are summarized in Table 2. The first 6 entries are common for all the 5 bands and the rest are the band-specific information. The band-specific entries are bundled together for each band and given in the order of N3, S7, S11, L15, and L24. For the band at which the source is not detected, the band-specific entries are assigned as 99.999 or similar numbers.

The number of the matched sources and the distance from the nearest matched source (Nmat and dis) are given for the longer band. Thus N3 does not have these entries. They are denoted by S7Nmat and S7dis when merging the N3 list with the S7 list. Similarly S11Nmat and S11dis indicate those in merging the N3-S7 list with the S11 list, L15Nmat and L15dis in merging the N3-S7-S11 list with the L15 list, and L24Nmat and L24dis in merging the N3-S7-S11-L15 list with the L24 list.

The flag code consists of 7 characters, one for each flag: “exposure”, “photometry”, “saturation”, “mux bleed”, “column pulldown”, “artifact”, and “multiple” flags, respectively. The description of the flags is summarized in Table 4. Of these, the “saturation”, “mux bleed”, “column pulldown”, and “artifact” flags are set to 1 if the source has a possibility of

4 http://www.ir.isas.jaxa.jp/ASTRO-F/Observation/

– 19 –

being affected by these phenomena (see §3.5.4). The “exposure” flag denotes photometry either from the short (0) or the long (1) exposure data, the “photometry” flag denotes the photometry method employed, 0 for the aperture photometry and 1 for the fit photometry (see §3.5.2), and the “multiple” flag provides the number of nearby sources (see §3.5.1). The code is given for all the bands, but “mux bleed” and “column pulldown” are only given at N3, and “artifact” is assinged only at S7 and S11 (see §3.5.4).

5. General Characteristics of the Catalog

5.1. Accuracy of Photometry and Astrometry

5.1.1. Photometric Accuracy

The photometric accuracy of the present dataset is estimated from the internal consistency of measured flux of the sources in the overlapping regions. Table 5 summarizes the median of the dispersions in the magnitude of the sources observed in more than one pointing observations. The dispersion at N3 (∼ 0.09 mag) is larger than those at S7 and S11 (∼0.06–0.07). Bright sources must include a large number of variable stars. Thus the present dispersions are affected both by the photometric uncertainties and the variability of the sources and indicate upper limits of the photometric uncertainties. Part of the large dispersion at N3 may come from the variability, although a study of the variables based on the SAGE data does not indicate a strong spectral dependence of the variability from 3 to 8 μm (Vijh et al. 2009). It could also be attributed to the variable PSF of the N3 images due to jitters in the AKARI satellite pointing.

– 20 –

5.1.2. Astrometric Accuracy

The median of the dispersions in the positions of the sources detected at multiple pointing observations is summarized in Table 5. The dispersion at shorter wavelengths is smaller than that at longer wavelengths except for N3 (§3.5.3). The dispersion at N3 is slightly worse than those at S7 and S11. This may originate in the distorted PSF at N3, which comes from aberrations of the AKARI telescope on orbit (Kaneda et al. 2007) or tracking errors in the attitude control system since the exposure time of N3 is by three times longer than the MIR band data. The sources detected at multiple bands adopt the position determined in the shortest wavelength band despite the slightly worse dispersion at N3.

We compare the positions in the present catalog with those in the 2MASS-PSC and the SAGE-PSC. The systematic offsets and the standard deviations between the corresponding positions are listed in Table 6. The deviation from the SAGE-PSC is ∼0.^{′′}5, which is slightly larger than that from the 2MASS-PSC of ∼0.^{′′}4. This is attributable to the difference in the astrometric accuracy between the SAGE-PSC of ∼0.^{′′}3 (Sewilo et al. 2009) and the 2MASS-PSC of ∼0.^{′′}07 (Skrutskie et al. 2006). Taking account of these facts, we estimate the uncertainty in the position of the present catalog as ∼0.^{′′}4. This value is in agreement with that of the internal consistency. The offsets from the 2MASS-PSC and the SAGE-PSC are consistent with each other. The systematic offset of the present catalog from the ICRS is estimated to be less than 0.^{′′}1.

– 21 –

5.2. Detection Limit and Completeness

5.2.1. Limiting Magnitude

The distributions of the photometric uncertainty versus magnitude for the sources in the Archive and the Catalog are shown in Figure 2 for each band; the dashed horizontal lines indicate a S/N of 10. The 10-σ limiting magnitude is the faintest magnitude at which the mode of the photometric uncertainties of the sources in the Catalog becomes 0.11 mag. The 10-σ limiting magnitudes are 16.8, 13.4, 11.5, 9.9, and 8.5 mag at N3, S7, S11, L15, and L24, respectively, as listed in Table 7. Figure 2 indicates the presence of two branches in the sources in the Archive except for N3: the one for which σ goes below 0.1 mag at the brightest end and the other in which σ stays above 0.1 mag. The latter branch disappears in the plot of the Catalog sources (left), suggesting that they do not have counterparts in the SAGE catalog. We will discuss this issue in §5.3.

Figure 3 is a diagrammatic representation of the 5-σ limiting magnitudes of the present survey, the Spitzer SAGE survey, and the IRSF/SIRIUS near-infrared survey. The 5-σ limiting magnitudes of the present survey are calculated from the 10-σ limiting magnitudes given in Table 7. We estimate the 10-σ limiting magnitudes for the SAGE survey by the same procedure as described above, then calculate the 5-σ limiting magnitudes. Figure 3 indicates that the limiting magnitudes of the present survey are slightly worse than those of the SAGE survey, while the S11 and L15 bands fill the gap of the SAGE data with comparable sensitivities. Examples of the ISO SWS spectra of stars of known distance (the distances are taken from Crosas & Menten (1997) for IRC +10216 and Perryman et al. (1997) for others) are also plotted after scaling their flux densities at the distance of the LMC. Here, the distance modulus of the LMC is assumed to be 18.5 mag. The figure indicates that all red giants above the tip of the first red giant branch (TRGB) and some fraction of Herbig Ae/Be stars in the LMC can be detected at shorter than 11 μm in the

– 22 –

present survey.

5.2.2. Completeness Limit

The completeness limit is estimated by adding artificial sources of various magnitudes and measuring the detection probability of the sources. Artificial sources with the shape of the PSF-model are added by an IDL software. 90% probability is adopted as the completeness limit. To estimate the completeness limits with different sky-background levels, the following three cases are investigated in each band: (1) “high”: images with the highest sky-background level, (2) “medium”: images with the median of the sky-background level of all images, and (3) “blank”: images with the lowest sky-background level. For each level, 5 images without large masked areas or artifacts are selected and artificial sources are embedded.

The averages and standard deviations of the 90% completeness limits estimated from 5 images at each level are listed in Table 7. In all bands, the 90% completeness limits with the “medium” level are comparable to those with the “blank” level and those with the “high” level are by ∼3 mag shallower than those with the other two. The “high” sky-background level is higher by 3 standard deviations than the median of the sky-background levels of all images in each band. The fraction of the images with the “high” sky-background level is only 1–2%. More than 90% of the images have the sky-background level within two standard deviations from the median of the sky-background level of all the images at each band. Therefore, the typical completeness limits are comparable to those with the “medium” level. The 90% completeness limits with the “medium” level are 14.6, 13.4, 12.6, 10.7, and 9.3 mag at N3, S7, S11, L15, and L24, respectively. They are roughly comparable with the 10-σ limiting magnitudes except at N3, where it is by ∼2 mag shallower than the 10-σ limiting magnitudes. This can be attributed to confusion due to the relatively large

– 23 –

number of sources at N3.

5.3. Comparison with Spitzer SAGE Point Source Catalog

As described in §3.5.5, we construct two kinds of catalog: the Archive, which includes all the detected sources, and the Catalog, which includes sources that have a counterpart(s) in the closest band of the SAGE-PSC. Therefore, the ratio between the number of the sources in the Catalog and that in the Archive in a band is the fraction of the AKARI sources that have a counterpart(s) in the SAGE-PSC. The ratios are 85.0, 56.8, 43.4, 25.1, and 4.8% at N3, S7, S11, L15, and L24, respectively. Since a large fraction of the area of the AKARI survey is covered by the SAGE survey and the sensitivities are comparable (see 5.2.1), the ratios are unexpectedly small except for N3.

The spatial distributions of the Archive and the Catalog sources in S7, S11, L15, and L24 images around bright nebulosity are shown in Figure 4 to investigate the difference in more detail. It indicates that the sources only in the Archive are concentrated along bright nebulosity. Figure 5 shows the relationship between the sharpness and the magnitude for the Archive and Catalog sources at N3, S7, S11, L15, and L24. The sharpness parameter indicates the size of the source compared to the PSF. A positive (negative) sharpness value indicates that the source is more (less) extended than the PSF. The Archive sources at S7, S11, L15, and L24 show distributions around unity, suggesting that they are more extended than point-like sources. These distributions are not seen in the Catalog sources.

Table 8 summarizes the number of the sources with a counterpart in the neighboring shorter wavelength band as well as the number of all the sources in the Archive and the Catalog. The S7 sources are matched with the N3 sources, S11 with S7, L15 with S11, and L24 with L15. A significant fraction of the Archive sources have a counterpart in the

– 24 –

neighboring shortest wavelength band for S7, S11, L15, and L24. These facts suggest that the Archive sources are real, but that they are slightly extended for the beam of Spitzer and thus are not included in the SAGE-PSC as a true point source. Figure 2 indicates that the Archive sources excluded in the SAGE catalog have larger flux uncertainties than those in the Catalog except for N3. The larger uncertainties may be attributable to the nebulosity with which the sources are associated as suggested by the larger sharpness. The associated nebulosity is appreciably seen in the MIR and increases the background fluctuation. The imperfect match with the PSF for slightly extended sources could also increase the uncertainties.

Figure 6 shows the distributions of the difference between the N3, S7, and L24 magnitudes and the [3.6], [8.0], and [24] in the SAGE-PSC for the Catalog sources. Whereas systematic differences are present, which can be attributed to the difference in the relative spectral responses, all the bands show fairly linear correlations, confirming the consistency in the photometric results between the two datasets.

6. Properties of the Sources in the Catalog

In this section, we discuss the following properties of the sources in the present catalog: (1) luminosity functions (LFs), (2) a color-color diagram (CCD), and (3) a color-magnitude diagram (CMD).

6.1. Luminosity Functions

The LFs for the 5 bands are shown in Figure 7. For the magnitudes brighter than 2–4 mag, all of the LFs start to fall rapidly due to the saturation. In the N3 LF, there is a stepwise increase around 12 mag, which corresponds to the flux of TRGB (Ita et al. 2008).

– 25 –

To investigate the populations of the sources that contribute to the LFs at L15 and L24, we also plot the Archive sources that have N3 counterparts brighter and fainter than 12 mag separately by the dotted and dashed lines in Figure 8. In the LFs of S7 and S11, there are no apparent differences depending on the brightness of the N3 counterparts brighter than 11.5 mag, but the sources fainter than 12 mag at N3 become dominant for those fainter than 11.5 mag. In the LFs of L15 and L24, the sources fainter than 12 mag at N3 are dominant irrespective of the magnitude. At the present sensitivities, TRGB without dust shells cannot be detected at L15 and L24 (Figure 3). Therefore, those that contribute to the LFs of L15 and L24 are likely to be dusty AGB stars whose N3 is significantly attenuated. Other types of objects, such as background galaxies, are also supposed to be present.

6.2. Color-Color Diagram

Ita et al. (2008) discuss the characteristics of the CCD of [N3] − [S11] vs. [S11] − [L15] using the preliminary AKARI LMC catalog, where the brackets [ ] indicate the magnitude at the band in question. Based on the same catalog, Siudek et al. (2012) present the distributions of about 2000 sources that are detected at all the IRC 5 bands and have information of the object type on CCDs and CMDs of various combinations. They also discuss the classification of objects using the Support Vector Machine algorithm. These investigations demonstrate the importance of the bands S11 and L15 in the classification, which are unique to AKARI. Ita et al. (2008) suggest that even the N3 data contain different information from the IRAC 3.6 μm band. The short cutoff wavelength of the N3 band is 2.7 μm (Onaka et al. 2007), much shorter than that of the IRAC 3.6 μm band (Fazio et al. 2004) of 3.185 μm. The N3 band is more sensitive to the absorption at 3 μm either of water ice seen in young stellar objects (YSOs) or of C_2H_2 and HCN in carbon stars. Although it contains interesting information, L15 may not have a sufficient depth to probe

– 26 –

low-mass YSOs (Figure 3 and see below). Therefore we investigate the CCD of [N3] − [S7] vs. [S7] − [S11], a combination of the most sensitive 3 bands, here in some detail.

Figure 9 shows the [S7] − [S11] vs. [N3] − [S7] CCD for the Archive sources with S/Ns ≥ 10 at N3, S7, and S11. The sample contains 16446 sources. In the CCD, there are 5 noticeable features, which are labeled as CC1–CC5. Group CC1 forms a clump around ([S7] − [S11], [N3] − [S7]) ∼ (0, 0). Groups CC2 and CC3 constitute sequences extending from CC1 to redder regions; CC2 is a horizontally stretching feature to ([S7] − [S11], [N3] − [S7]) ∼ (3, 1), whereas CC3 is a vertical sequence to ∼ (1, 2.5). CC4 forms a diffuse concentration around ([S7] − [S11], [N3] − [S7]) ∼ (1.5, 2.5) and CC5 is a sequence vertically extending from CC3 further to ([S7] − [S11], [N3] − [S7]) ∼ (0.7, 5.5).

Woods et al. (2011) classify 197 point sources in the LMC based on SAGE-spec observations with the Infrared Spectrograph (IRS) onboard Spitzer (Houck et al. 2004). With a positional tolerance of 10.^{′′}0, 67 sources in Woods et al. (2011) are found to match with the Archive sources. Figure 10a highlights these matched sources by the large symbols. Two naked stars matched (blue circles) are located at CC1 and red supergiants (purple circles) are distributed over CC1 and CC2. O-rich AGB stars (orange diamonds) are located at CC2, while C-rich AGB stars (green diamonds) are located at CC3 and CC5. O-rich post-AGB stars (orange squares) and O-rich planetary nebulae (orange stars) are distributed in the CC4 region. Only one C-rich post-AGB star and one C-rich planetary nebulae are matched with the Archive sources and they are located at CC5 as indicated by the green square and star, respectively. Two H II regions are matched (purple triangles), which are seen in the CC4–CC5 regions. No background galaxies in their sample are matched with the Archive. YSOs (red triangles) are located at CC5. It should be noted that these YSOs are most likely massive ones because of the detection limit of the IRS (Woods et al. 2011). Sources in CC4 and CC5 also include post-AGB stars and planetary

– 27 –

nebulae.

In Figure 10b, background galaxy and YSO candidates selected by Gruendl & Chu (2009) are plotted on the same CCD together with the Archive sources. Gruendl & Chu (2009) select the candidates based on the analysis using the images and photometry of the Spitzer SAGE survey as well as other surveys from optical to NIR wavelengths. With a positional tolerance of 3.^{′′}0, 379 YSO and 239 background galaxy candidates are matched with the Archive sources. Figure 10b shows that CC5 selectively overlaps with YSO candidates, while background galaxies and other YSOs are distributed around the CC4 region. It also indicates a clear separation between YSO and background galaxy candidates around [N3] − [S7] ∼ 3.5, which is roughly consistent with the boundary between CC4 and CC5. The color [N3] − [S7] becomes very red for YSOs because of the water ice absorption at 3 μm (Shimonishi et al. 2008), whereas [S7] − [S11] stays blue due to the silicate absorption (Woods et al. 2011). To confirm the effect of the water ice absorption, the YSOs that show the absorption (Shimonishi et al. 2010; Shimonishi 2012) are also plotted by the green circles in Fig. 10b. 11 of the 14 YSOs are located in the CC5 region, while the rest 3 are in the CC4 region, supporting the above interpretation. The S7 band efficiently probes the unidentified infrared (UIR) bands at 6.2 and 7.7 μm (Onaka et al. 2009), which also accounts partly for the redness of [N3] − [S7]. Therefore, the color [N3] − [S7] is efficient to distinguish YSOs from dusty AGB stars. Further observations of the objects in the CC5 region would be interesting to study their nature and investigate the applicability of this color diagnosis. Background galaxies can have very red [S7] − [S11] color, but their [N3] − [S7] color may not be very red because stellar components contribute to N3. Post-AGB stars or planetary nebulae are also suggested to be distributed in the CC4 region (Siudek et al. 2012).

In summary, the features CC1 to CC5 in the [S7] − [S11] vs. [N3] − [S7] CCD

– 28 –

correspond to the following objects: CC1: naked stars;

CC2: dusty O-rich stars; CC3: dusty C-rich stars;

CC4: YSOs and background galaxy candidates, and post-AGB and planetary nebulae; CC5: YSO candidates with water ice absorption These classifications are also confirmed by the investigation of known objects towards the LMC (Siudek et al. 2012).

Figure 9 shows the distributions of the sources similar to those seen in the [S11] − [L15] vs. [N3] − [S11] CCD based on the previous version of the AKARI LMC catalog (Ita et al. 2008) except for CC5, which is not seen in their diagram. Their classifications of each feature are in agreement with the present results. The absence of CC5 in the [S11] − [L15] vs. [N3] − [S11] CCD may suggest that the present sensitivity of L15 is not sufficient to detect most YSOs in the LMC.

6.3. Color-Magnitude Diagram

Classification based on the CMDs has been extensively discussed for the SAGE-SPC data (e.g., Blum et al. 2006; Whitney et al. 2008). Ita et al. (2008) present CMDs of several combinations of the imaging bands based on the previous version of the AKARI catalog. Here we only briefly discuss a CMD, which shows a well-separated distribution of various objects to confirm the previous results. Figure 11 shows the [N3] − [S11] vs. [S11] CMD for the Archive sources with S/Ns ≥ 10 at N3, S7, and S11. Comparison with the 5 components CC1–CC5 in the CCD indicates:

(1) CC1 sources form a vertically stretching feature along [N3] − [S11] ∼ 0 (CM1) and two separate branches in 0 < [N3] − [S11] < 1.5 (CM1b and CM1c);

– 29 –

(2) CC2 sources form a finger-like feature (CM2) and a clump around ([N3]−[S11], [S11]) ∼ (1.5, 9.5) (CM2b);

(3) CC3 sources form a finger-like structure (CM3); (4) CC4 sources form a clump (CM4);

(5) CC5 sources are distributed to the redder region (CM5).

The sequence CM1b corresponds to a bristle-shape feature, which Ita et al. (2008) attribute to the broad emission feature of aluminum oxide grains around 11.4 μm (e.g., Onaka et al. 1989).

Comparison with their CMD suggests that the distributions of dusty C-rich AGB stars are located at the position of CM3 and those of optical carbon stars correspond to the sequence CM1c (([N3 − S11], S11) ∼ (0.5, 10.5) to (1.0, 8.5)). Other features are also basically seen in the CMD of Ita et al. (2008), confirming the previous results by the improved catalog.

We find a new feature CM2b in Figure 11. The sources of CM2b are found to correspond to CC2 in the CCD (Figure 9), which we assign to dusty O-rich stars (see Figure 10a). According to stellar evolution models (e.g., Herwig 2000; Straniero et al. 2006; Karakas & Lattanzio 2007), the third dredge-up enhances the abundance of carbon relative to oxygen for stars with ≥ 2M_⊙, which leads to the formation of C-rich stars (Lebzelter et al. 2009). For stars with ≥ 4M_⊙, the hot bottom burning decreases the abundance of carbon, which then prevents the formation of C-rich stars (García-Hernández et al. 2006). These suggest that AGB stars with an intermediate-mass (∼2–4 M_⊙) have a high probability of evolving to C-rich stars, and low-mass (≤ 2M_⊙) and high-mass (∼4–8 M_⊙) AGB stars are likely to evolve to O-rich stars. Thus theoretical predictions suggest that CM2 and CM2b in Figure 11 correspond to high-mass and low-mass O-rich stars, respectively. Note that both mass limits depend on the metallicity (Boothroyd et al. 1993) and thus the location

– 30 –

of CM2b may differ in other galaxies.

In Figure 12a, 67 Archive sources classified in Woods et al. (2011) are highlighted as in Figure 10a. The locations of each category source are in agreement with the above discussion. Red supergiants (purple circles) are found to be concentrated on CM2. Post-AGB stars (squares) and planetary nebulae (stars) are distributed over a wide area in the CMD. YSOs with the ice absorption are located at [S11] < 7 mag, while those with the emission features are distributed at [S11] > 6.5 mag.

In Figure 12b, background galaxy and YSO candidates (Gruendl & Chu 2009) are plotted on the CMD together with the Archive sources. Figure 12 indicates that YSO candidates are located around CM5 and background galaxy candidates are distributed over the brighter side of CM4. Gruendl & Chu (2009) exclude faint and red sources from the initial YSO candidates with a criterion of [8.0] > 14 − ([4.5] − [8.0]) to avoid contamination from background galaxies. Faint CM4 sources are likely to be excluded in this selection. Therefore the entire CM4 population can be attributed to background galaxies. These assignments of the features in the CMD are well in agreement with those made in the CCD. The locations of the YSOs with the 3 μm water ice absorption (green circles) reported in Shimonishi et al. (2010) and Shimonishi (2012) are in agreement with those classified by Woods et al. (2011) in Figure 12a.

7. Summary

We present the AKARI LMC Point Source Catalog, which covers a core 10 deg^2 area of the LMC with 5 photometric bands: N3 (3.2 μm), S7 (7 μm), S11 (11 μm), L15 (15 μm) and L24 (24 μm). The 10-σ limiting magnitudes are 17.9, 13.8, 12.4, 9.9, and 8.6 mag at N3, S7, S11, L15 and L24, respectively. They are comparable to those of the Spitzer SAGE

– 31 –

survey and the S11 and L15 data smoothly fill the gap between the IRAC and MIPS bands. The photometric accuracy is estimated to be better than 0.1 mag at N3 and 0.06–0.07 mag in the other bands. The astrometric accuracy is 0.^{′′}3 at N3, S7 and S11, and 1.^{′′}0 at L15 and L24.

We provide a source Catalog and an Archive: The Archive contains all the detected sources, while the Catalog only includes sources that have a counterpart in the Spitzer SAGE point source catalog. Archive contains about 650,000, 140,000, 97,000, 43,000, and 52,000 sources at 3.2, 7, 11, 15, and 24 μm, respectively.

Based on the present catalog, we discuss the LFs at 5 bands, a CCD, and a CMD of the N3, S7, and S11 data for the sources towards the LMC. Several noticeable features are recognized in the CCD and CMD, which can be attributed to naked stars, dusty C-rich and O-rich AGB stars, background galaxies and YSOs. They are distributed at distinct locations on the diagrams, indicating that the present data provide useful information on the classification of the sources towards the LMC.

Acknowledgement

This work is based on observations with AKARI, a JAXA project with the participation of ESA. The authors thank all the members of the AKARI project and the members of the LMC survey for their continuous help and encouragement. They are grateful to F. Egusa for her contribution to the IRC data reduction pipeline. They also thank the Spitzer SAGE team for their help. This work is supported in part by Grants-in-Aid from the Japan Society for the Promotion of Science (JSPS).

Facility: AKARI

– 32 – REFERENCES Alves, D.R. 2004, New A Rev., 48, 659 Arimatsu, K., Onaka, T., Sakon, I., et al. 2011, PASP, 123, 981 Benjamin, R. A., Churchwell, E., Babler, B. L., et al. 2003, PASP, 115, 953 Blum, R. D., Mould, J. R., Olsen, K. A., et al. 2006, AJ, 132, 2034 Boothroyd, A.I., Sackmann, I.J., & Ahern, S.C. 1993, ApJ, 416, 762 Crosas, M., & Menten, K. M. 1997, ApJ, 483, 913 Egan, M. P., Van Dyk, S. F., & Price, S. D. 2001, AJ, 122, 1844 Egan M. P., Price, S. D., Kraemer, K. E., et al. 2003, in Air Force Research Laboratory Technical Report, Vol. AFRL-VS-TR-2003-1589 Fazio, G. G., Hora, J. L., Allen, L. E., et al. 2004, ApJS, 154, 10 García-Hernández, D. A., García-Lario, P., Plez, B., Manchado, A., & D’Antona, F. 2006, IAU Symposium, 234, 87 Gruendl, R., & Chu, Y. 2009, ApJS, 184, 172 Herwig, F. 2000, A&A, 360, 952 Houck, J. R., Roellig, T. L., van Cleve, J., et al. 2004, ApJS, 154, 18 Ishihara, D., Wada, T., Onaka, T., et al. 2006, PASP, 118, 324 Ishihara, D., Onaka, T., Kataza, H. et al., 2010, A&A, 514, A1 Ita, Y., Tanabé, T., Matsunaga, N., et al. 2007, PASJ, 59, S437

– 33 – Ita, Y., Onaka, T., Kato, D., et al. 2008, PASJ, 60, S435 Kaneda, H., Kim, W., Onaka, T., et al. 2007, PASJ, 59, S423 Karakas, A., & Lattanzio, J. 2007, PASA, 24, 103 Kato D., Nagashima, C., Nagayama, T., et al., 2007, PASJ, 59, 615 Kawada M., Baba, H., Barthel, P. D., et al. 2007, PASJ, 59, S389 Kemper, F., Woods, P. M., Antoniou, V., et al. 2010, PASP, 892, 683 Kontizas, E., Dapergolas, A., Morgan, D. H. & Kontizas, M. 2001, A&A, 369, 932 Lebzelter, T., Lederer, M. T., Cristallo, S., Straniero, O., & Hinkle, K. H. 2009, IAU Symposium, 256, 397 Lorente, R., Onaka, T., Ita, Y., et al. 2008, AKARI IRC Data User’s Manual ver. 1.4, http://www.ir.isas.jaxa.jp/AKARI/Observation/ Meixner, M., Gordon, K. D., Indebetouw, R., et al. 2006, AJ, 132, 2288 Meixner, M., Galliano, F., Hony, S., et al. 2010, A&A, 518, L71 Murakami H., Baba, H., Barthel, P., et al. 2007, PASJ,59, S369 Ohyama Y., Onaka, T., Matsuhara, H., et al. 2007, PASJ,, 59, S411 Onaka, T., de Jong, T., & Willems, F. J. 1989, A&A, 218, 169 Onaka T., Matsuhara, H., Wada, T., et al. 2007, PASJ, 59, S401 Onaka, T., Kaneda, H., Sakon, I., & Matsumoto, H. 2009, Proc. of Cosmic Dust – Near and Far, ASP Conf. ser. 414, eds. Th. Henning, E. Grün, & J. Steinacker, (ASP: San Francisco), 227

– 34 – Perryman, M. A. C., Lindegren L., Kovalevsky, J., et al. 1997, A&A, 323, L49 Rieke G. H., Young, E. T., Engelbracht, C. W., et al. 2004, ApJS, 154, 25 Sewilo, M., Meixner, M., Whitney, B., et al. 2009, The SAGE Data Products Description http://ssc.spitzer.caltech.edu/spitzermission/observingprograms/legacy/sage/ Shimonishi, T., 2012, PhD thesis, University of Tokyo Shimonishi, T., Onaka, T., Kato, D., et al. 2008, ApJ, 686, L99 Shimonishi, T., Onaka, T., Kato, D., et al. 2010, A&A, 514, A12 Shimonishi T.,Onaka, T., Kato, D., et al. 2012, submitted to AJ Siudek, M., Pollo, A., Takeuchi, T. T., Ita, Y., Kato, D., & Onaka, T. 2012, Earth, Planets, & Space, in press.

Skrutskie, M. F., Cutri, R. M., Stiening, R., et al. 2006, AJ, 131, 1163 Sloan, G. C., Kathleen, E., Kraemer, K. E., Price, S. D., & Shipman, R. F. 2003, ApJS, 147, 379 Smith, J. D., Draine, B. T., Dale, D. A., et al. 2007, ApJ, 656, 770 Stetson, P. B. 1987, PASP, 99, 191 Straniero, O., Gallino, R., & Cristallo, S. 2006, Nucl. Phys. A, 777, 311 Tabur, V. 2007, PASA, 24, 189 Tanabé, T.,Sakon, I., Cohen, M., et al. 2008, PASJ, 60, S375 van Loon, J. T., Oliverira, J. M., Gordon, K. D., et al. 2010, AJ, 139, 68 Vijh, U. P., Meixner, M., Babler, B., et al. 2009, AJ, 137, 3139

– 35 – Werner M.W., Roellig, T. L., Low, F. J., et al. 2004, ApJS, 154, 1 Whitney B. A., Sewilo, M., Indebetouw, R., et al. 2008, AJ, 136, 18 Woods, P. M., Oliveira, J. M., Kemper, F., et al. 2011, MNRAS, 411, 1597 Yamamura, I., Makiuti, S., Ikeda, N., et al. 2010, VizieR On-line Data Catalog: II/298 Zaritsky, D., Harris, J., Thompson, I. B., & Grebel, E. K. 2004, AJ, 128, 1606

This manuscript was prepared with the AAS L^ATEX macros v5.2.

– 36 –

Table 1. Example of the Catalog Record

ID name ID2 R.A. DEC. pos-flag N3x N3y N3mag N3me N3me2 N3chi N3shrp (1) (2) (3) (4) (5) (6) (7) (8) (9) (10) (11) (12) (13)

56000001 AKARI-LMCC J050737.46-670810.9 76.906067 -67.136353 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000002 AKARI-LMCC J050737.51-670831.8 76.906273 -67.142159 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000003 AKARI-LMCC J050738.23-670640.8 76.909279 -67.111336 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000004 AKARI-LMCC J050745.94-671413.4 76.941399 -67.237053 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000005 AKARI-LMCC J050745.96-670811.4 76.941513 -67.136513 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000006 AKARI-LMCC J050747.82-670821.3 76.949265 -67.139259 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000007 AKARI-LMCC J050749.56-671211.2 76.956482 -67.203102 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000008 AKARI-LMCC J050754.92-665746.1 76.978851 -66.962814 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000009 AKARI-LMCC J050758.73-671218.7 76.994720 -67.205200 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 56000010 AKARI-LMCC J050759.70-670035.7 76.998749 -67.009911 3 999.999 999.999 99.999 99.999 99.999 99.999 99.999 ... ... ... ... ... ... ... ... ... ... ... ... ...

– 37 –

Table 1. continued

N3date N3pid N3flag S7Nmat S7dis S7x S7y S7mag S7me S7me2 S7chi S7shrp S7date (14) (15) (16) (17) (18) (19) (20) (21) (22) (23) (24) (25) (26)

9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 ... ... ... ... ... ... ... ... ... ... ... ... ...

– 38 –

Table 1. continued

S7pid S7flag S11Nmat S11dis S11x S11y S11mag S11me S11me2 S11chi S11shrp S11date S11pid (27) (28) (29) (30) (31) (32) (33) (34) (35) (36) (37) (38) (39)

9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 ... ... ... ... ... ... ... ... ... ... ... ... ...

– 39 –

Table 1. continued

S11flag L15Nmat L15dis L15x L15y L15mag L15me L15me2 L15chi L15shrp L15date L15pid L15flag (40) (41) (42) (43) (44) (45) (46) (47) (48) (49) (50) (51) (52)

9999999 0 99.99 206.406 18.121 10.662 0.207 0.209 0.075 0.052 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 197.784 16.530 9.297 0.072 0.073 0.107 -0.085 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 243.089 27.315 10.074 0.143 0.144 0.114 -0.189 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 53.203 8.753 10.766 0.251 0.253 0.100 0.036 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 202.099 38.444 8.544 0.052 0.053 0.175 -0.077 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 197.140 42.089 10.436 0.197 0.199 0.104 -0.161 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 101.755 27.399 10.834 0.255 0.257 0.090 -0.152 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 237.879 28.323 8.954 0.062 0.063 0.131 0.128 2007-06-02T23:59:44 2213035.1 1100000 9999999 0 99.99 94.249 48.691 9.652 0.097 0.098 0.108 0.015 2007-05-28T11:25:56 2213033.1 1100000 9999999 0 99.99 165.741 32.491 10.831 0.236 0.239 0.067 0.063 2007-06-02T23:59:44 2213035.1 1100000 ... ... ... ... ... ... ... ... ... ... ... ... ...

– 40 –

Table 1. continued

L24Nmat L24dis L24x L24y L24mag L24me L24me2 L24chi L24shrp L24date L24pid L24flag (53) (54) (55) (56) (57) (58) (59) (60) (61) (62) (63) (64)

0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 1 0.27 193.778 11.330 9.226 0.225 0.229 0.154 -0.260 2007-05-28T11:27:37 2213033.1 1100000 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 1 1.23 197.763 33.093 7.008 0.035 0.038 0.161 -0.020 2007-05-28T11:27:37 2213033.1 1100000 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 1 1.10 233.541 22.642 7.041 0.029 0.034 0.096 -0.061 2007-06-03T00:01:26 2213035.1 1100000 1 0.36 90.170 43.412 8.157 0.078 0.081 0.122 0.125 2007-05-28T11:27:37 2213033.1 1100000 0 99.99 999.999 999.999 99.999 99.999 99.999 99.999 99.999 9999-99-99T99:99:99 9999999.9 9999999 ... ... ... ... ... ... ... ... ... ... ... ...

– 41 –

Table 2. Catalog Content

Item format Record position (byte) Content

Common record

ID1 A8 1:8 source ID1: 56****** for Catalog and 51****** for Archive Cname A10 10:19 AKARI-LMCC for Catalog and AKARI-LMCA for Archive ID2 A19 21:39 source ID2 in Jhhmmss.ss-ddmmss.s R.A. F10.6 41:50 right ascension (J2000.0) in degree Decl F10.6 52:61 declination (J2000.0) in degree eq-flag A1 63:63 band at which the position is derived

Band specific N3 S7 S11 L15 L24

x F7.3 65:71 165:171 265:271 365:371 465:471 pixel X-coordinate y F7.3 73:79 173:179 273:279 373:379 473:479 pixel Y-coordinate mag F6.3 81:86 181:186 281:286 381:386 481:486 magnitude in the Vega system uncorrected for extinction me1 F6.3 88:93 188:193 288:293 388:393 488:493 photometric uncertainty from ALLSTAR me2 F6.3 95:100 195:200 295:300 395:400 495:500 total photometric uncertainty^a χ F7.3 102:108 202:208 302:308 402:408 502:508 PSF fit parameter^b sharpness F7.3 110:116 210:216 310:316 410:416 510:516 PSF fit parameter^c

date A19 118:136 218:236 318:336 418:436 518:536 observation date in UT PID A9 138:146 238:246 338:346 438:446 538:546 pointing ID flag A7 148:154 248:254 348:354 448:454 548:554 7-digit code for the object (see text and Table 4) Nmatch I2 — 156:157 256:257 356:357 456:457 number of matched sources (see text for details) distance F5.2 — 159:163 259:263 359:363 459:463 distance from the nearest matched source in arcsec (see text for details)

– 42 –

aIncluding errors in the aperture correction, read-out noise, and conversion factor.

bThe parameter χ increases with the difference in shape between the source and the PSF-profile. The values 99.999 is assigned when the aperture photometry is employed.

cA positive (negative) sharpness indicates that the source is more (less) extended than the PSF-profile, suggesting that the source may be a galaxy, an unresolved multi-star system, a cosmic ray, or image defect. The values 99.999 is assigned when the aperture photometry is employed.

– 43 –

– 44 –

Table 3. Observation Parameters

Properties IRC bands NP N3 S7 S11 L15 L24

Channel NIR NIR MIR-S MIR-S MIR-L MIR-L Bandpass (μm) 1.8–5.5 2.7–3.8 5.9–8.4 8.5–13.1 12.6–19.4 20.3–26.5 Reference wavelength (μm) — 3.2 7.0 11.0 15.0 24.0 Pixel field of view (^{′′} pixel^{−1} ) — 1.446 2.340 2.340 2.384 2.384 Dispersion (μm pixel^{−1} ) 0.06 at 3.5μm — — — — — Exposure time: long exposure^a (s) 133 133 147 147 147 147 Exposure time: short exposure^a (s) 14.0 14.0 1.75 1.75 1.75 1.75 10-σ detection limit^b (mJy) - 0.024 0.226 0.419 1.758 2.921 10-σ detection limit^b (mag) - 17.9 13.8 12.4 9.9 8.6 Saturation limit^{b ,c} (mJy) 12500 at 3.5μm 250 1800 1800 2500 23000 Saturation limit^{b ,c} (mag) 3.6 at 3.5μm 7.8 4.0 3.3 2.0 -1.1 Zero magnitude flux density^d (Jy) - 343 75.0 38.3 16.0 8.0 Number of sources in Archive - 720872 141617 97226 42974 52266 Number of sources in Catalog - 651294 89610 48525 16712 6856

aThese are the nominal values. The total exposure time per pixel depends on the co-adding process. bFor point sources.

cNumbers are taken from ASTRO-F Observer’s Manual version 3.2.2. dFrom Tanabé et al. (2008).

– 45 –

Table 4. Description of Flags

Flag Description

exposure 0: short; 1: long.

photometry 0: aperture photometry; 1: PSF fitting photometry. multiple Number of the nearby sources. mux bleed 1: contamination by mux bleed; only for N3. column pulldown 1: contaminated by column pulldown; only for N3. artifact 1: contaminated by artifact; only for S7 and S11.

Table 5. Internal Dispersion of Photometry and Astrometry

band σ [mag] σ [^{′′}] S/N N_{source}

N3 0.091 0.607 ≥30 10805 S7 0.071 0.413 ≥20 3500 S11 0.058 0.405 ≥20 1314 L15 0.069 0.962 ≥20 497 L24 0.063 1.031 ≥20 455

– 46 –

Table 6. Astrometric Accuracy

catalog offset standard deviation accuracy Δα Δδ Δα Δδ r

2MASS-PSC -0.^{′′}064 0.^{′′}056 0.^{′′}220 0.^{′′}307 0.^{′′}393 ∼0.^{′′}07^a SAGE-PSC -0.^{′′}058 0.^{′′}057 0.^{′′}293 0.^{′′}421 0.^{′′}509 ∼0.^{′′}3^b

aSkrutskie et al. (2006). bSewilo et al. (2009).

Table 7. 10-σ Limiting Magnitude and 90% Completeness Limit

band 10-σ limiting 90% completeness limit magnitude high (mag)^a medium (mag)^b blank (mag)^c

N3 17.9 13.46 ± 0.13 14.58 ± 0.08 15.66 ± 0.08 S7 13.8 10.73 ± 0.41 13.40 ± 0.87 14.06 ± 0.18 S11 12.4 9.12 ± 0.73 12.62 ± 0.08 12.84 ± 0.05 L15 9.9 7.70 ± 1.21 10.68 ± 0.29 11.02 ± 0.13 L24 8.6 5.88 ± 1.12 9.32 ± 0.25 9.50 ± 0.07

aHigh, medium, and blank correspond to the sky background level (see text).

– 47 –

Table 8. Band Merging Results^a

band Archive Catalog N_{all}^b N_{match}^c N_{all}^b N_{match}^c Matching band

S7 141617 101425 89610 85791 N3 S11 97226 67254 48525 43355 S7 L15 42974 27141 16712 12868 S11 L24 52266 23062 6856 5545 L15

aFor merging strategy, see text. bTotal number of sources.

cNumber of sources with a counterpart in the neighboring shorter wavelength band.

– 48 –

Fig. 1.— Observed area of the AKARI IRC survey (solid outline) overlaid on the photographic image kindly provided by Motonori Kamiya. The dashed outline indicates the coverage of the Spitzer SAGE survey (7^∘ × 7^∘: Meixner et al. 2006), the dash-dotted outline shows the coverage of the IRSF/SIRIUS near-infrared survey (6.3^∘ × 6.3^∘: Kato et al. 2007), and the dotted outline represents the coverage of the Magellanic clouds optical photometric survey (8.5^∘ × 7.5^∘: Zaritsky et al. 2004).

– 49 –

Fig. 2.— Photometric uncertainties as a function of magnitude for the Archive sources (left) and the Catalog sources (right) at N3, S7, S11, L15, and L24 from top to bottom. The horizontal dashed lines indicate the S/N levels of 2, 4, and 10, and the vertical dotted lines show the 10-σ limiting magnitudes.

– 50 –

Fig. 3.— Graphic representation of the 5-σ detection limits of the AKARI LMC survey (solid lines). For a comparison, the 5-σ detection limits of the Spitzer SAGE survey and the IRSF/SIRIUS survey are shown by the dashed and dotted lines, respectively. The length of the bars indicates the FWHM of the bandpass. ISO SWS spectra (Sloan et al. 2003) of 3 galactic stars are also plotted after scaling their fluxes at the distance of the LMC as examples of a Herbig Ae/Be star (AB Aur), a red giant with luminosities below the TRGB (β And), and a dusty red giant (IRC +10216).

– 51 –

Fig. 4.— Spatial distributions of Archive (green) and Catalog sources (red) on the S7 (top left), S11 (top right), L15 (bottom left), and L24 (bottom right) images around bright nebulae. The image size is 30^′ × 30^′ and the central position of the image is (5h22m08s, −67d56m12s).

– 52 –

Fig. 5.— Sharpness vs. magnitude. The left figure shows the Archive sources and the right indicates the Catalog sources at N3, S7, S11, L15 and L24 from top to bottom. The numbers in red indicate the 10-σ limiting magnitudes.

– 53 –

Fig. 6.— Comparison of the magnitudes of the AKARI catalog and SAGE-PSC. Residual magnitudes of the sources matched between the AKARI catalog and SAGE-PSC are shown as a function of magnitude at N3 (with SAGE [3.6]), S7, S11, L15 (with [8.0]), and L24 (with [24]) from top to bottom. The numbers in red indicate the 10-σ limiting magnitudes of the AKARI catalog.

– 54 –

Fig. 7.— Luminosity functions. From tom to bottom those at N3, S7, S11, L15, and L24 are shown in 0.1 mag bins. The solid and dashed lines show the Archive and Catalog sources, respectively. The numbers in italic and the vertical dashed lines indicate the 90% completeness limits in “blank” regions.

– 55 –

Fig. 8.— Luminosity functions of the Archive sources. Those at S7, S11, L15, and L24 are shown from top to bottom. The gray lines indicate all Archive sources, the black solid lines those with a counterpart in N3 sources, and the dashed and dotted lines those with a counterpart of N3 brighter and fainter than 12 mag, respectively.

– 56 –

Fig. 9.— Color-color diagram of [N3] − [S7] vs. [S7] − [S11]. The Archive sources with S/Ns ≥ 10 are shown. Each color is binned by 0.025 mag and the number density levels are shown in a logarithmic scale. The dashed line is a locus of the colors for blackbodies from temperatures of 400 to 10000K. Noticeable features are labeled as CC1 to CC5 (see text).

– 57 –

Fig. 10.— Color-color diagram of [N3]−[S7] vs. [S7]−[S11]. The Archive sources with S/Ns ≥ 10 are plotted in a gray-scale together with the sources classified in Woods et al. (2011) in (a) and with the YSO and background galaxy candidates selected by Gruendl & Chu (2009) in (b). In (a), the blue and purple circles indicate naked stars and red supergiants, the orange and green diamonds represent O-rich and C-rich AGB stars, the orange and green squares show O-rich and C-rich post-AGB stars, the orange and green stars indicate O-rich and C-rich planetary nebulae, and the purple and red triangles show H II regions and YSOs, respectively. In (b), the blue and red circles show background galaxy and YSO candidates, respectively. The green circles indicate YSOs with the water ice absorption at 3 μm (Shimonishi et al. 2010; Shimonishi 2012).

– 58 –

Fig. 11.— Color-magnitude diagram of [S11] vs. [N3] − [S11] The Archive sources with S/Ns ≥ 10 are plotted. Each data point is binned by 0.05 mag and the number density levels are shown in a logarithmic scale. Noticeable features are labels as CM1 to CM5 (see text).

– 59 –

Fig. 12.— Color-magnitude diagram of [S11] vs. [N3] − [S11]. The Archive sources with S/Ns ≥ 10 are plotted in a gray-scale together with the sources classified in Woods et al. (2011) (a) and YSO and background galaxy candidates by Gruendl & Chu (2009) (b). The symbols are the same as in Figures 10a and b.