arXiv:1301.0253v1 [astro-ph.GA] 2 Jan 2013

Astronomy & Astrophysics manuscript no. paper˙maser˙pepe © ESO 2017 December 26, 2017

Non–local radiative transfer in strongly inverted masers.

F. Daniel^1 and J. Cernicharo^1

Laboratory of Molecular Astrophysics, Department of Astrophysics, Centro de Astrobiología (CSIC-INTA). Crta. Torrejón a Ajalvir km4. 28840 Torrejón de Ardoz. Madrid. Spain e-mail: danielf@cab-inta.csic.es

ABSTRACT

Context. Maser transitions are commonly observed in media exhibiting a large range of densities and temperatures. They can be used to obtain information on the dynamics and physical conditions of the observed regions. In order to obtain reliable constraints on the physical conditions prevailing in the masing regions, it is necessary to model the excitation mechanisms of the energy levels of the observed molecules.

Aims. We present a numerical method that enables us to obtain self–consistent solutions for both the statistical equilibrium and radiative transfer equations.

Methods. Using the standard maser theory, the method of Short Characteristics is extended to obtain the solution of the integro– differential radiative transfer equation, appropriate to the case of intense masing lines.

Results. We have applied our method to the maser lines of the H_2O molecule and we compare with the results obtained with a less accurate approach. In the regime of large maser opacities we find large differences in the intensity of the maser lines that could be as high as several orders of magnitude. The comparison between the two methods shows, however, that the effect on the thermal lines is modest. Finally, the effect introduced by rate coefficients on the prediction of H_2O masing lines and opacities is discussed, making use of various sets of rate coefficients involving He, o–H_2 and p–H_2. We find that the masing nature of a line is not affected by the selected collisional rates. However, from one set to the other the modelled line opacities and intensities can vary by up to a factor ∼ 2 and ∼10 respectively.

1. Introduction

The first maser signal was detected in 1965 (Weaver et al., 1965). It was due to OH and the intriguing nature of this detection was rapidly attributed to a non–thermal phenomenon (Davies et al., 1967) which originates in the amplification of the radiation due to stimulated emission. Since then, many improvements have been made both in observational facilities and maser theory, leading to an abundant literature on the subject. The main results, both theoretical and observational, have been summarised by, e.g., Elitzur (1992) or Gray (1999). From the observational point of view, major improvements have been obtained in the last 20 years thanks to the rise of sensitive interferometers and VLBI techniques (see e.g. Humphreys, 2007; Fish, 2007, and references therein). The sizes of the regions where maser emission is detected have typical scales of a few AU. Nevertheless, some masers arise from large spatial scales, such as the 183.3 GHz line of water vapour (Cernicharo et al., 1990, 1994). From the point of view of the theory, despite the fact that many improvements have been made in explaining the pumping mechanisms of molecular masers, there are no definitive explanations that could account for all the observations as yet. As an example, the problem of water megamasers observed in the direction of AGN is still a subject of debate (Elitzur et al., 1989; Deguchi & Watson, 1989; Kylafis & Pavlakis, 1999; Cernicharo et al., 2006a).

The basics of the standard maser theory which is widely used in order to interpret masing lines have been reviewed by Elitzur (1992). The main aspect of this theory is to introduce the effect of saturation which puts limits on the amount of energy that can be

Send offprint requests to: F. Daniel radiated by a masing line. As outlined by Collison & Nedoluha (1995), maser theoretical studies adopt two different strategies: i) they solve exactly the radiative transfer in the maser but with a simplified description of the energy levels of the molecule; ii) or deal with an exact description of the molecule but using approximations in the radiative transfer treatment. In the latter case, the escape probability formalism is widely used, despite the fact that the validity of this approximation is questionable in the case of masing lines. Indeed, intense masers require a large amplification path and, therefore, coherence in velocity over relatively large scales. In contrast, the basic principle of the LVG approximation is that the different regions of the cloud are decoupled due to Doppler shifting, hence limiting the coherence path. In this work we present a self–consistent method that aims to go beyond the approximations usually made, i.e. we present a method that enables us to solve exactly the radiative transfer problem and in which we deal with a rigorous description of the molecule.

The theory relevant to the description of masing lines as well as the way the radiative transfer is solved is described in Section 2. An application for the o–H_2O molecule is presented in Section 3 where the method developed in this study is compared to other less accurate approaches. Finally, the current method is used in Section 4 in order to predict which lines of o–H_2O or p–H_2O could be inverted for densities and temperatures typical of AGB circumstellar envelopes. In this section, the predictions based on various sets of collisional rate coefficients involving He, p–H_2 or o–H_2 are also compared.

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

2. Theory

2.1. Absorption coefficient

In the case of intense masers, the radiation field starts to influence the inversion of the population, avoiding a complete frequency redistribution, leading to differing line profiles for absorption and emission. This occurs when the intensity in the masing lines exceeds a certain threshold which depends on the given physical conditions. In this case, the maser is said to be saturated. The way this effect is introduced in the theory is described later in this section.

Moreover, under a particular geometry the amplification path varies with direction, implying that the distribution of molecular velocities should in principle be considered as anisotropic. This problem was first identified by Bettwieser & Kegel (1974). In the case of spherical geometry, a common approximation, known as ”standard theory”, consists of neglecting the anisotropy of the molecular velocities resulting from the existence of directions of different path lengths. The validity of this assumption was tested in various studies (see e.g. Bettwieser, 1976; Neufeld, 1992; Emmering & Watson, 1994; Elitzur, 1994) for spherical geometry. They concluded that considering explicitly the anisotropies of the absorption coefficient could lead to variations in the properties of the emerging maser radiation, in the case of saturated masers. However, it was pointed out that these variations remain unimportant in comparison to the uncertainties that affect maser theory, and that the standard theory should, at least, be a reasonably good first approximation. Given the large number of simplifications adopted by the standard theory in the treatment of the radiative transfer (RT), we assume in the following that the masing line absorption coefficients are isotropic, and we follow a procedure similar to that described by Anderson & Watson (1993). First, we consider the frequency– dependent statistical equilibrium equations (SEE) for the level i: dn_i(v) dt = � j�i � N_j ϕ(v)C_{ji} − n_i(v)C_{i j} � + � N_i ϕ(v) − n_i(v) � C_{ii} + � j�i � n_j(v) R_{ji}(v) − n_i(v) R_{i j}(v) � (1) with

R_{i j}(v) = � � � � � A_{i j} +

B_{i j} 4π � I_v(Ω) dΩ if E_i > E_j B_{i j} 4π � I_v(Ω) dΩ if E_i < E_j (2)

In these equations, N_j represents the total population of level j, n_j(v) is the population of level j at the velocity v. The quantity ϕ(ν) corresponds to the usual Doppler line profile that accounts for both the thermal and turbulent motion of the molecules. A_{i j} and B_{i j} are the Einstein coefficients for spontaneous and induced emission, E_j is the energy of level j, C_{ji} are the collisional rates from level j to level i and I_v(Ω) is the specific intensity in a direction specified by Ω. We note that in equation 1 the elastic collisional rates C_{ii} have to be formally included since they contribute to the relaxation of velocities (Anderson & Watson, 1993). Equation 1 can be re-written so that all levels except those involving the maser transition are included in the so called pump and loss rates. This leads to a phenomenological treatment where the full SEE is artificially reduced to a two level system. In the following, the labels u and l indicate the upper and lower maser levels, respectively. Assuming that for all the other transitions the absorption and emission line profiles are identical and are given by the Doppler line profile ϕ(ν), we obtain from eq. 1:

0 = Λ_u(v) ϕ(v) − n_u(v) [Γ_u(v) + C_{ul} + C_{uu}]

+ ϕ(v) [N_l C_{lu} + N_u C_{uu}] − n_u(v) A_{ul} − Δn(v) R_{lu}(v) (3) 0 = Λ_l(v) ϕ(v) − n_l(v) [Γ_l(v) + C_{lu} + C_{ll}]

+ ϕ(v) [N_u C_{ul} + N_l C_{ll}] + n_u(v) A_{ul} + Δn(v) R_{lu}(v) (4)

where the pump and loss rates, noted Λ_i and Γ_i (with i ∈ {u, l}), are defined by

Λ_i(v) = � j�{u,l}

N_j � C_{ji} + R_{ji}(v) � (5) Γ_i(v) = � j�{u,l} � C_{i j} + R_{i j}(v) � (6) This leads to the usual expression:

Δn(v) = g_l g_u n_u(v) − n_l(v) = n_0(v) � 1 + R_{lu}(v) J̄(v)

�_{−1} ϕ(v) (7)

with

n_0(v) = 1 1 + B(v)^{gu}_{gl} A_{ul} � � �A(v) [Λ_u(v) + N_l C_{lu} + N_u C_{uu}]

− B(v) [Λ_l(v) + N_u C_{ul} + N_l C_{ll}] � � � (8)

J̄(v) =

1 + B(v)^{gu}_{gl} A_{ul}

A(v) + B(v) (9) and A(v) = g_l g_u

[Γ_u(v) + C_{ul} + C_{uu} + A_{ul}]^{−1} (10)

B(v) = � Γ_l(v) + C_{lu} + C_{ll} − g_u g_l

A_{ul}

�_{−1} (11)

The source function of the masing line is given by:

S_{ul}(ν) = −

2hν^3 c^2 g_l g_u n_u(ν) Δn(ν)

(12)

where n_u(ν) can be obtained from eqs 3 and 7. Contrary to the case of thermal lines, the source function is frequency dependent for the maser line.

In order to obtain the source functions and the absorption coefficients from these expressions, we see that the relevant quantities are the specific line intensities (averaged over the angles), and the total level populations, N_j. The latter are obtained by solving the frequency independent SEE expressed by: 0 = � j�i � N_j C_{ji} − N_iC_{i j} � + � j�i � N_j J̄_{ji} − N_i J̄_{i j} � (13)

with

J̄_{kl} = � ϕ_k(ν) R_{kl}(ν) dν (14)

In the latter expression, the velocity profile ϕ_k(ν) = n_k(ν)/N_k accounts for the departure from the Doppler line profile if the line k → l is a masing transition, for consistency with eq. 1. In the case of thermal lines, these profiles are simply given by the Doppler profile and are identical for both levels. In this latter case, the average of the specific intensities over angles and

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

velocities in eq. 13 can be factorized, which is crucial in establishing the preconditioned form of the SEE, as discussed by Rybicki & Hummer (1991). In the case of masing lines and for consistency with eq. 1, we have introduced unequal velocity profiles for the maser levels; consequently the factorisation leading to the preconditioned SEE is no longer feasible. Hence, the usual ALI method cannot be applied.

In most studies treating the radiative transfer in the presence of masers, the pumping rates are taken to be independent of the velocity. In this case the expression for the population difference is similar to eq. 7 except that the velocity dependence of n_0(ν) and J̄(ν) is omitted. Hence, the absorption coefficient will just depend on velocity through the term R_{lu}(ν). In the case of unsaturated masers, this term is always negligible in comparison to J̄(ν) and the absorption coefficient is given by the Doppler line profile. However, for a saturated maser, i.e., for a line with R_{lu}(ν) ∼ J̄, the absorption coefficient decreases at the line centre. This translates to the fact that, for a given pumping scheme, the molecules pumped to the upper level are readily depleted to the lower by stimulated emission since the number of masing photons is large. At this stage, the maser amplification starts to be linear at line centre and the maser line re–broadens.

2.2. Solution of the transfer equation

To solve the transfer equation we have used the short characteristic method (SC) introduced by Olson & Kunasz (1987) . The numerical code based on this method has previously been described in Daniel & Cernicharo (2008) for the case of thermal transitions in 1D spherical geometry. Briefly, in the SC method we assume that the source function can be reproduced numerically by a polynomial function of the opacity in the line (usually of order 1 or 2). At each iteration the absorption coefficients are known from the current populations, and the opacities are evaluated assuming that they behave linearly between consecutive grid points. These assumptions permit us to solve analytically the transfer equation at each spatial grid point. In our models, the radiative transfer deals with both maser and thermal lines. However, the treatment for maser propagation is only switched on when the opacity of a line (i.e. τ_{ul} = N_l − g_l/g_u N_u), at a particular grid point, is negative. For the same line and for the radii where the opacity is positive, the line is treated in a standard way relevant to thermal radiation.

In what follows, we describe a method that allows us to solve the transfer equation for masing lines. It is based on the assumption that the source functions are linearly interpolated. Hence, along a characteristic, specific intensities are derived according to: I_i = I_{i−1} e^{−Δτi} + α_i S_{i−1} + β_i S_i (15)

where the α_i and β_i coefficients depend on the opacity Δ τ_i between points i and i − 1.

In the case of masing lines, a difficulty arises from the fact that the absorption coefficient at point i depends on the angular average R_{lu}(v) of the specific intensities I_i(θ):

κ_{lu}(v) = − hν 4 π B_{lu} n^+_0 (v) � 1 + R_{lu}(v) J̄+(v)

�_{−1} ϕ(v) (16)

where the quantities indexed by a cross (e.g. J̄^+) are obtained with the current estimate for the populations of the energy levels (i.e. the populations obtained at the previous iteration). The same applies to the source functions (see eq. 12). Therefore, the radiative transfer equation becomes integro–differential, whereas in the case of thermal lines, the problem consists in solving a differential equation. Note that the integral part of this integro– differential equation involves an integration of the intensities over 4π steradians. In order to obtain intensities which are fully self-consistent with the level populations used at a given iteration, we thus proceed in three steps.

2.2.1. First iterative scheme

As a first step, we derive specific intensities at each grid point according to eq. 15 assuming that the source functions are independent of the radiation field. In other words, we use eq. 12 in order to express the source function assuming that the average radiation field is R^+_{lu}(ν). For each frequency, we obtain the solution iteratively by calculating I_v(θ) for θ ∈ [0 : π] and then updating κ_{lu}(v) at grid point i. We iterate until the calculated specific intensities are consistent with the initial averaged radiation field.

In the following discussion, R_{lu}(ν) is indexed by i or f whenever it corresponds to the radiation field used in the evaluation of κ_{lu}(ν) or to the one which results from the evaluation of eq. 15 and made use of R^i_{lu}(ν). Additionally, the solutions obtained during the previous steps are indexed with the superscript > if they satisfy R^f_{lu}(ν) > R^i_{lu}(ν) and with the superscript < on the contrary. Once the iterative process has been initialised, a trial value for R_{lu}(v) is obtained according to:

log R_{lu}(ν) = b 1 − a

(17)

with � � � � � � � a = log � � � R^{f >}_{lu} (ν)

R^{f <}_{lu} (ν) � � � / log � � � R^{i>}_{lu} (ν)

R^{i<}_{lu} (ν) � � �

b = log R^{f >}_{lu} (ν) − a log R^{i>}_{lu} (ν)

(18)

The radiation field derived in this way is used to update κ_{lu}(ν). Depending on the resulting specific intensities, one of the pair (R^{i>}_{lu} , R^{f >}_{lu} ) or (R^{i<}_{lu} , R^{f <}_{lu} ) is updated. Finally, the iterative process is stopped when we have R^i_{lu} = R^f_{lu}, within a given accuracy. Figure 1 shows the typical behaviour of R^f_{lu} as a function of R^i_{lu}. The averaged radiation fields determined using our method are marked with squares and are indexed according to the iteration number.

2.2.2. Second iterative scheme

Once this process has been achieved, we perform an update of the source function at point i according to eq. 12, and using the average radiation field R_{lu}(ν) derived during the first iterative scheme. The whole process is then repeated until we obtain convergence for the source function at the current grid point.

2.2.3. Third iterative scheme

As previously stated, in order to derive the absorption coefficient, it is necessary to know the angular average of specific intensities over 4π sr. Using the SC method, the spatial grid is first swept from the outermost grid point (i = N) to the innermost one (i = 1) providing the intensities I_i(θ), with i ∈ [1; N] and θ ∈ [π/2; π]). The grid is then swept in the other direction so that the intensities for θ ∈ [0; π/2]) are then known. This sweeping

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Fig. 1. Variation of the averaged radiation field (solid line) as a function of the initial radiation field entering in the determination of the absorption coefficient. The dashed line corresponds to a straight line of slope unity. The solution of the problem corresponds to the intersection between the two curves. The squares correspond to the averaged radiation field obtained at each iteration.

Fig. 2. Schematic diagram showing the availability of incoming intensities during the inward propagation.

procedure is adopted so that at every moment during the propagation, only the populations used at the current iteration are needed to derive the intensities. In the case of masing lines, an additional complexity arises from the fact that during the inward propagation, the incoming intensities for θ < θ_{lim} have not yet been calculated (c.f. figure 2) with the current populations while they enter in the evaluation of the absorption coefficient.

The third iterative scheme thus consists of obtaining an overall convergence for the intensities I_i(θ), with i ∈ [1; N] and θ ∈ [0; π]. This is done by performing successive sweeping of the spatial grid, each iteration leading to an update of the intensities I_i(θ).

3. Application

In order to test our method, we have performed model calculations for the ortho state of the water molecule and the comparison is made with respect to a simplified treatment that aims to describe the masing lines. This simplified treatment relies on the assumption that the calculation of maser inversion and the resulting intensities can be achieved in a two–step procedure. First, the populations of the molecular levels are determined neglecting the specificity of maser radiative transfer. Secondly, the intensities of the masing lines are calculated using the populations obtained during the first step and taking into account maser propagation. This procedure has been used in previous studies (e.g. Yates et al., 1997; Watson et al., 2002) and the way it is presently implemented is described in the next sections.

The models consist of clouds of uniform H_2 density, temperature (assumed to be 400 K in all models), and o–H_2O abundance (40 levels have been considered). We have adopted a diameter for the cloud of 4.10^{14} cm (2.6 10^{−4} pc) which is the typical size of bright maser spots in the 22 GHz line of water. Moreover, this size provides a maximum amplification path similar to that of the slab depths used in Yates et al. (1997). The collisional rate coefficients are for the collisional system H_2O / He (Green et al., 1993) and are corrected in order to account for the different reduced masses of the H_2O / H_2 and H_2O / He systems. We have selected these rates rather than those of Dubernet et al. (2009) or Faure et al. (2007) as they were the ones used by Yates et al. (1997). These parameters being fixed, we performed the calculations in the (n(H_2),X(H_2O)) plane of parameter space, with respective values in the range [2 10^5; 8 10^9] cm^{−3} and [2 10^{−6}; 8 10^{−4}]. The accuracy of the results will depend on the gridding adopted. Typically, convergence is reached when the spatial sampling is such that the opacity between two consecutive grid points is of the order or less than 1. For all the calculations presented here, we adopted a grid with 500 spatial grid points, which might be inadequate for the highest densities/abundances considered here. However, since we are interested in masing lines which are collisionally quenched at these densities/abundances, the effect of limited convergence accuracy does not affect our conclusions. Moreover, the main goal is to compare the effect of the radiative transfer and both model calculations are performed with the same spatial grid.

As presented in Section 2, elastic collisional rate coefficients for the levels involved in masing lines enter in the definition of the absorption coefficients and source functions. Test calculations have been performed by Anderson & Watson (1993) in order to test the influence of these rates and they concluded that in most cases their inclusion produces rather small effects. Hence, in the present test calculations, we have assumed that the elastic rate coefficients are set to zero. In other words, in the following calculations we assume that C_{ii} = 0 in Eq. ??

3.1. Pumping scheme with/without maser propagation

As a first step, we compare the results of the exact calculation to a simplified treatment that consists of neglecting the amplification inherent to maser propagation when deriving the population of the energy levels of the molecule. To do so, we take the absolute value of the level population difference which then enters in the definition of the absorption coefficients and source functions. These quantities are defined with the usual expressions which are suitable for thermal lines. This permit us to treat masing lines in the same manner as thermal lines. This approach was previously adopted in plane parallel non–local calculations by Yates et al. (1997) with the aim of predicting which water lines could show maser excitation. Their results are discussed in term of the gain in the masing lines (see eq. 3 of Yates et al., 1997)

γ_{ul}(ν) =

Δn(ν)A_{ul}c^2 8πν^2

(19)

which is subsequently averaged over the slab depths (the so– called depth–weighted gain coefficient defined by eq. 7 of Yates et al., 1997). Since γ_{ul}(ν) is proportional to the absorption coefficient κ_{lu}(ν), it is equivalent to consider either the depth– weighted gain coefficient or the opacity in the masing line, and

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

in the following, we choose to discuss the results in terms of line opacities. We emphasise the fact that at this stage, the approximate method described here does not involve any treatment specific to maser radiation and that could account for saturation effects. Thus, the dependence on frequency of the population difference Δn(ν) which enters in the definition of γ_{ul}(ν) [or κ_{lu}(ν)] is just given by the Doppler line profile ϕ(ν).

Fig. 3. Isocontours of the o–H_2O opacities at line centre for the 6_{16} − 5_{23} line at 22 GHz, the 4_{14} − 3_{21} line at 380 GHz and the 4_{23} − 3_{30} line at 448 GHz lines. The left column corresponds to the models where the treatment of maser propagation is omitted and the right one to the current results (see text). The isocontour values as well as the correspondence between grey scale and opacity values are displayed on top of the two columns. The isocontours that correspond to opacities of -4 and -40 are displayed in thick blue lines. Negative values for the opacity correspond to red lines.

Figure 3 shows the opacity at line centre of the 22 GHz (6_{16}- 5_{23}), 380 GHz (4_{14}-3_{21}) and 448 GHz (4_{23}-3_{30}) masing lines, obtained in the two treatments (labelled respectively on or off according to whether maser propagation is accounted for or not). Figure 4 shows the line opacities for the same lines with respect to cuts in density or H_2O abundance. We can see on these figures that including the current maser propagation treatment leads to a substantial decrease in the predicted line opacities for these lines. Indeed, without treating the exact radiation field in the masing lines, we obtain minimum optical depths of the order of -70 for the 22 GHz line and -40 for the 380 and 448 GHz transitions. With our method, the minimum optical depth for the 22 GHz line is reduced to -20 and to -5 for the other two lines.

Fig. 4. Comparison between the opacities derived with (solid lines) or without (dashed lines) accounting for maser propagation for the masers at 22 GHz, 380 GHz and 448 GHz. The left column corresponds to a cut in density at n(H_2) = 2 10^7 cm^{−3} and the differences are shown with respect to variations in X(H_2O). The right column corresponds to a fixed water abundance, i.e. X(H_2O) = 4 10^{−4}.

Fig. 5. Brightness temperatures for the 22 GHz line obtained with the exact treatment (solid lines) and with the approximated treatment (dashed lines). The intensities correspond to a line of sight that crosses the centre of the sphere and are given for the rest frequency of the line.

3.2. Two–level maser propagation

In order to infer the influence of these changes in line opacities, we now consider the resulting masing line intensities. To do so, any reasonable approximated treatment should include a

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Fig. 6. Emerging brightness temperature of the 22 GHz line for the model with n(H_2) = 4 10^7 and X(H_2O) = 6 10^{−4}. The solid line corresponds to the intensity predicted by the exact calculation and the dashed line to the one predicted by the approximated RT (see text).

RT theory that accounts for saturation effects. To obtain a reference point for the current results, we proceed as follows: from the populations previously obtained in the approximate treatment, we compute the pump and loss rates Λ_i(v) and Γ_i(v). These values enter in the definition of the population difference Δn(v) through eq. 7. Then, for a given masing line, the intensities are computed by adjusting R_{lu}(v) as described in section 2.

Using this approximation, we obtain line intensities that differ largely from those obtained with the exact treatment described in section 2. This is illustrated in Fig. 5 for the 22 GHz line. This figure shows the brightness temperatures obtained in the two treatments at a density n(H_2) = 4 10^7 cm^{−3}, for the centre of the line and for a line of sight that passes through the centre of the sphere. This figure shows that for water abundances X(H_2O) > 5 10^{−5} the approximate treatment leads to intensities larger by two orders of magnitude. This originates from the opacity overestimation obtained in the approximate treatment which has been discussed in the previous section. Additionally, Fig. 6 compares the line profiles computed in the two treatments for the model with n(H_2) = 4 10^7 cm^{−3} and X(H_2O) = 6 10^{−4}. In this figure, we see that the higher intensity found in the approximate treatment is accompanied by a broader line profile. This result is produced by the higher line saturation obtained in the approximate treatment with respect to the exact treatment. This fact is illustrated in figure 7 where the ratio R_{lu}(ν)/J̄(ν) is plotted as a function of the velocity offset to line centre and of the normalised radius in the cloud for the 22 GHz line and for the model with n(H_2) = 4 10^7 cm^{−3} and X(H_2O) = 6 10^{−4}, for both the exact and approximated methods. We see in this figure that in the exact calculation the degree of saturation is low, i.e. R_{lu}(ν)/J̄(ν) < 1 at any radii. In contrast, the saturation is high in the approximate calculation with R_{lu}(ν)/J̄(ν) > 10 at most radii.

(a) exact treatment

(b) approximated treatment

Fig. 7. Ratio R_{lu}(ν)/J̄(ν) as a function of the offset to line centre and of the normalized radius in the cloud. This ratio is given for the 22 GHz line and corresponds to the model with n(H_2) = 4 10^7 and X(H_2O) = 6 10^{−4}. The two plots correspond to (a) the exact treatment and (b) an approximated treatment (see text).

In the exact treatment, since the masing line intensities are taken into account when deriving the populations, the population difference between the upper and lower level of the masing line tends to be reduced by induced radiative de–excitation. On the other hand, in the approximate treatment, the averaged radiation field is largely underestimated. This entails that the amount of induced radiative de–excitation events is underestimated, which leads to a greater difference between the populations of the lower and upper levels. Consequently, the derived masing line opacity is larger which is accompanied by a larger degree of saturation of the line. So, the differences encountered in the two treatments originate in the overall flow of population from the upper to lower level, which is induced by radiative de-excitation. The evaluation of this flow of population differs in the two treatments since it relies on the accuracy of the determination of the intensities in the masing line.

We note that in section 2, eq. 7 is derived from the velocity dependent SEE and from this expression it is seen that an increase in the average radiation field leads to a decrease in Δn(ν). From similar considerations dealing with the velocity independent SEE, it can be seen that increasing the value of the radiation

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Fig. 8. The left column corresponds to the opacity of three purely thermal lines which are obtained in a treatment where masing lines are treated explicitly. The right column corresponds to the ratio r_τ = τ^{o f f} /τ^{on} of the opacities obtained with the two treatments (see text).

field for the maser transitions would lead to lower population differences for the levels involved in the maser transitions. This behaviour is not a specific case and we can infer from it that considering explicitly maser propagation will necessarily lead to a decrease in line optical depths in comparison to treatments where the average radiation field would be underestimated.

3.3. Thermal lines

The two treatments for maser propagation differ in the evaluation of the average radiation field of the masing lines. Considering the current maser propagation treatment leads to higher values for the average radiation field which, in turn, when inverting the SEE, leads to a diminution in the population differences between levels involved in maser transitions. The modification of the populations of these levels subsequently modifies the whole energy level populations. This is illustrated in figure 8 for three lines which only show purely thermal emission. In this figure, we see that the opacities of these lines are modified and can show variations up to ∼ 25% between the two treatments in the region of the (n(H_2),X(H_2O)) plane where maser transitions are the most opaque. Nevertheless, for the range of parameters considered here, the number of lines which suffer from optical depth variations greater than 10% is low, and for the majority of the thermal lines the opacities agree within a few percent between the two treatments.

4. Maser prediction

Most of the information that can be extracted from water line observations relies on the modelling of its excitation. From this point of view, water is a difficult molecule to treat since its high dipole moment causes most of its transitions to be sub–thermally excited (see, e.g. Cernicharo et al., 2006b), harbouring very large opacities (see, e.g. González-Alfonso et al., 1998), and many of them being maser in nature (Cheung et al., 1969; Waters et al., 1980; Phillips et al. , 1980; Menten et al. , 1990a,b; Menten & Melnick , 1991; Cernicharo et al., 1990, 1994, 1996, 1999, 2006b; González-Alfonso et al., 1995, 1998). Accurate modeling thus requires, in addition to a good description of the source structure, the availability of collisional rate coefficients. Moreover, as discussed above, special formalisms have to be developed in order to have a realistic treatment of the transfer of radiation in the case of saturated masers. The method developed in the present work for masing lines is used to assess which water lines are expected to show maser excitation as well as the relative opacity of the masers. To do so, we have performed calculations for various gas kinetic temperatures, H_2 and water volume densities. The grid was set up using the boundaries : 100 K < T_k < 1000 K, 10^6 cm^{−3} < n(H_2) < 10^{10} cm^{−3} and n(H_2O) ∈ � 10^2; 10^3; 10^4; 10^5 � cm^{−3}. Additionally, the parameter space is reduced by considering that the water abundance cannot exceed a relative abundance of 10^{−4} with respect to H_2. This range of values for the considered parameters is appropriate to the case of the circumstellar envelopes of evolved stars. The ratios of the line opacities with respect to the maximum 22 GHz opacity are given in Table 1 for o–H_2O and Table 2 for p–H_2O. For the two water symmetries, we compare the opacities obtained with the rate coefficients of Faure et al. (2007) (indexed as SET1), Dubernet et al. (2006, 2009); Daniel et al. (2010, 2011) (indexed as SET2) and Green et al. (1993). In these tables, the ratios obtained with the approximation introduced by Yates et al. (1997) are indicated in parentheses.

The parameter space considered here is a sub–space of the parameter space explored by Yates et al. (1997), since the maximum gas temperature in their calculation is 2000 K and because they include the pumping by dust photons. In the present case we use a lower boundary for the temperature since, in order to go higher, we would have to extrapolate the rate coefficients. Since we aim to compare various sets of collisional rate coefficients, we choose not to introduce artefacts due to the extrapolation procedure in the comparison of the results. Dust can play an important role in deriving the populations of water levels. However, since we report the ratio of the maximum opacity of the masing lines with respect to the maximum opacity of the 22 GHz line, the consideration of dust can only affect the current result for the lines which are radiatively pumped. For these lines, the ratios reported in Tables 1 and 2 have to be considered as lower limits. On the other hand, the ratios reported should be accurate for the lines which are collisionally pumped.

In order to compare the current results with the results reported by Yates et al. (1997), we have to convert the population density ratio of the latter study into opacity ratios. To do so, we start from the definition of the opacity along a ray of length L along which the density populations are uniform. Assuming that the velocity profile ϕ(ν) can be expressed as a gaussian, the opacity at the line i centre is :

τ(i) = 1 8π^32 × c^3 ν^3_i

A(i) g(i) dn(i) × L × � 2k_BT_i m + σ^2_i

�_− 1_2 (20)

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Table 1. Prediction of maser lines for different collisional rate coefficients sets.

Transition Frequency He p-H_2 p-H_2 o-H_2 o-H_2 (GHz) Green SET1 SET2 SET1 SET2 |τ_{22}| 8.2 (10.7) 5.3 (7.1) 9.1 (15.1) 4.9 (6.8) 7.6 (10.1) 6_{1,6} − 5_{2,3} 22 1.00 (1.00) 1.00 (1.00) 1.00 (1.00) 1.00 (1.00) 1.00 (1.00) 10_{2,9} − 9_{3,6} 321 0.73 (0.88) 1.11 (1.16) 0.67 (0.70) 1.17 (1.15) 0.78 (0.89) 4_{1,4} − 3_{2,1} 380 0.53 (1.78) 0.83 (2.14) 0.50 (1.85) 0.93 (2.35) 0.59 (1.63) 6_{4,3} − 5_{5,0} 439 0.48 (0.63) 0.83 (1.03) 0.48 (0.69) 0.91 (1.05) 0.60 (0.93) 7_{5,2} − 6_{6,1} 443 0.02 (0.05) 0.15 (0.21) 0.11 (0.13) 0.16 (0.24) 0.17 (0.25) 4_{2,3} − 3_{3,0} 448 0.42 (1.49) 0.68 (1.89) 0.39 (1.69) 0.74 (1.84) 0.49 (1.55) 1_{1,0} − 1_{0,1} 557 < 0.01 < 0.01 < 0.01 < 0.01 < 0.01 5_{3,2} − 4_{4,1} 621 0.45 (1.69) 0.76 (2.31) 0.42 (1.77) 0.82 (2.13) 0.53 (1.84) 7_{2,5} − 8_{1,8} 1146 N (N) < 0.01 N (N) < 0.01 N (N) 3_{1,2} − 2_{2,1} 1153 0.02 (0.02) 0.17 (0.18) < 0.01 0.20 (0.26) < 0.01 6_{3,4} − 5_{4,1} 1158 0.18 (0.80) 0.36 (1.61) 0.15 (0.56) 0.44 (2.07) 0.24 (1.37) 8_{5,4} − 7_{6,1} 1165 0.09 (0.11) 0.21 (0.35) 0.04 (0.04) 0.21 (0.37) 0.15 (0.24) 7_{4,3} − 6_{5,2} 1278 0.17 (0.49) 0.38 (1.50) 0.14 (0.41) 0.43 (1.70) 0.21 (0.79) 8_{2,7} − 7_{3,4} 1296 0.31 (0.76) 0.54 (1.70) 0.30 (0.90) 0.59 (1.89) 0.34 (0.78) 8_{4,5} − 9_{1,8} 1308 N (N) N (N) N (N) N (N) N (N) 6_{2,5} − 5_{3,2} 1322 0.19 (0.34) 0.41 (0.95) 0.21 (0.27) 0.46 (0.99) 0.26 (0.45) 8_{5,4} − 9_{2,7} 1596 N (N) N (N) N (N) N (N) N (N) 8_{4,5} − 7_{5,2} 1885 0.01 (0.02) 0.06 (0.06) 0.01 (0.01) 0.10 (0.10) 0.03 (0.03) 5_{2,3} − 4_{3,2} 1918 < 0.01 < 0.01 < 0.01 0.01 (0.01) < 0.01 8_{3,6} − 7_{4,3} 2245 < 0.01 0.20 (0.30) 0.01 (0.02) 0.27 (0.43) 0.01 (0.02) 7_{3,4} − 6_{4,3} 2567 < 0.01 < 0.01 N (N) < 0.01 < 0.01 8_{3,6} − 9_{0,9} 2577 N (N) N (N) (N) N (N) N (N) 9_{2,7} − 10_{1,10} 2619 N (N) N (N) (N) N (N) N (N) 9_{4,5} − 8_{5,4} 3150 N (N) N (N) (N) N (N) N (N)

Notes. The first line gives the maximum 22 GHz opacity (τ_{22}) obtained for the density and temperature range covered in this study (see Sec. 4). For each masing line, the ratio of the maximum opacity to τ_{22} is given, making use of the approximate treatment described in Sec. 3 (numbers in parentheses) or with the current method. The transitions in bold correspond to the maser transitions predicted by the present work and not predicted by Yates et al. (1997). The transitions with opacity ratio below 10^{−5} as well as the transitions that do not show population inversion are reported with the N symbol.

Table 2. Same as Table 1 but for p–H_2O

Transition Frequency He p-H_2 p-H_2 o-H_2 o-H_2 (GHz) Green SET1 SET2 SET1 SET2 |τ_{22}| 8.2 (10.7) 5.3 (7.1) 9.1 (15.1) 4.9 (6.8) 7.6 (10.1) 3_{1,3} − 2_{2,0} 183 0.64 (1.22) 0.98 (1.55) 0.59 (1.29) 1.08 (1.63) 0.70 (1.16) 5_{1,5} − 4_{2,2} 325 0.61 (1.24) 0.85 (1.29) 0.57 (1.35) 0.93 (1.32) 0.68 (1.22) 7_{5,3} − 6_{6,0} 437 < 0.01 (0.02) 0.16 (0.23) 0.09 (0.12) 0.15 (0.22) 0.13 (0.21) 6_{4,2} − 5_{5,1} 471 0.46 (0.65) 0.80 (1.15) 0.46 (0.70) 0.83 (1.06) 0.59 (0.97) 5_{3,3} − 4_{4,0} 475 0.49 (1.40) 0.77 (1.79) 0.44 (1.42) 0.86 (1.80) 0.60 (1.60) 6_{2,4} − 7_{1,7} 488 N (N) < 0.01 N (N) < 0.01 < 0.01 2_{1,1} − 2_{0,2} 752 N (N) N (N) N (N) N (N) N (N) 9_{2,8} − 8_{3,5} 906 0.45 (1.07) 0.73 (1.41) 0.43 (1.00) 0.79 (1.32) 0.49 (0.98) 4_{2,2} − 3_{3,1} 916 0.25 (0.56) 0.36 (0.84) 0.25 (0.73) 0.39 (0.92) 0.29 (0.81) 5_{2,4} − 4_{3,1} 970 0.26 (0.80) 0.55 (2.77) 0.21 (0.81) 0.60 (3.06) 0.32 (1.21) 1_{1,1} − 0_{0,0} 1113 N (N) N (N) N (N) N (N) N (N) 7_{4,4} − 6_{5,1} 1173 0.19 (0.41) 0.41 (0.96) 0.18 (0.29) 0.45 (0.98) 0.23 (0.67) 8_{5,3} − 7_{6,2} 1191 0.18 (0.21) 0.15 (0.24) 0.14 (0.18) 0.19 (0.29) 0.24 (0.38) 7_{4,4} − 8_{1,7} 1345 N (N) N (N) N (N) N (N) N (N) 9_{4,6} − 10_{1,9} 1435 N (N) N (N) N (N) N (N) N (N) 7_{2,6} − 6_{3,3} 1441 0.25 (0.41) 0.49 (1.61) 0.23 (0.35) 0.55 (1.88) 0.29 (0.47) 6_{3,3} − 5_{4,2} 1542 0.15 (0.15) 0.28 (0.35) 0.13 (0.11) 0.32 (0.49) 0.20 (0.35) 7_{3,5} − 6_{4,2} 1766 0.06 (0.07) 0.24 (0.39) 0.04 (0.06) 0.30 (0.50) 0.07 (0.11) 8_{4,4} − 7_{5,3} 2162 < 0.01 (N) < 0.01 < 0.01 < 0.01 < 0.01 9_{3,7} − 8_{4,4} 2532 < 0.01 0.16 (0.18) < 0.01 (0.01) 0.20 (0.23) < 0.01 9_{4,6} − 8_{5,3} 2547 N (N) < 0.01 < 0.01 < 0.01 N (N) 6_{2,4} − 5_{3,3} 2962 N (N) < 0.01 N (N) < 0.01 N (N) 8_{3,5} − 7_{4,4} 3670 N (N) < 0.01 N (N) < 0.01 N (N)

Notes. The ratios are still given as a function of the maximum 22 GHz opacity.

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

where ν_i is the rest frequency of line i, A(i) is the Einstein coefficient for spontaneous emission, g(i) is the degeneracy of the upper level of the transition and dn(i) is the population difference per sub–level. This latter quantity is the one considered by Yates et al. (1997) and is defined as :

dn(i) = � n_l g_l − n_u g_u � (21)

where the indexes u and l stand respectively for the upper and lower level of transition i. In Eq. 20, the gas temperature T_i and turbulence velocity σ_i are indexed according to the line, since in the comparison, we only retain the physical parameters that lead to the maximum opacity for this particular line. The opacity ratio thus correlate to the population density ratio considered by Yates et al. (1997) through :

τ_1 τ_2 = � ν_2 ν_1

�_3 A(1) A(2) g(1) g(2) dn(1) dn(2)

(22) × � 2k_BT_1 m + σ^2_1

�_− 1_2 � 2k_BT_2 m + σ^2

� 1_2

Since the temperatures and turbulence of the models for which the ratios are given in Table 2 of Yates et al. (1997) are unknown, we assume T_1 = T_2 and σ_1 = σ_2 while performing the conversion. The maximum error introduced by this assumption is typically of a factor ∼ 2-3 (considering that the 22 GHz has its maximum inversion at 600 K as stated in Yates (1997). ) By considering col. 5 of Table 4, it can be seen that the values currently obtained and the one obtained by Yates et al. (1997) can differ by factors larger than 2-3. The differences might arise from the use of plane–parallel geometry in Yates et al. (1997) against spherical geometry in the current work, or because we do not consider the effect introduced by the pumping by dust photons in the current study. By examining the results of the comparison reported for o–H_2O in Table 4 and for the lines with frequencies higher than 1.3 THz (λ < 230 μm), we can see that the ratios can take high values above this threshold frequency and tend to increase while the frequency increases. Since this behaviour is correlated with the shape of the dust emission, it can be guessed that a quantitative comparison between the two works is plagued by the absence of consideration of dust radiation in the present work.

By comparison to previous calculations (Neufeld & Melnick, 1991; Yates et al., 1997), we find that the 8_{5,4} − 7_{6,1} (1165 GHz), 7_{4,4} − 6_{5,1} (1173 GHz), 8_{5,3} − 7_{6,2} (1191 GHz) lines can show population inversion with substantial opacities, independently of the set of rate coefficients used. These lines were not predicted to be masers in the previous studies. The rest of the lines considered in this work agree with the predictions of Yates et al. (1997) with respect to the possibility of masing action, at least for the lines that show substantial inversion.

Considering the effects introduced by the collisional rate coefficients, we find that the variations from one set to another are moderate. The lines which are found to be inverted are the same, independently of the set considered, and most of the opacities show variations of the order of a factor 2 or less. Our method to treat the RT of the maser lines introduces large differences in the computed line opacities; indeed, for most of the lines, the opacities derived with the exact treatment are lower by up to a factor 4–5 in comparison to the opacities derived with the approximated treatment.

Interestingly, we find that many lines can show substantial inversion. This is in agreement with the observations made by Menten et al. (2008) who report the fluxes of 9 maser transitions of water. Note that the 437 GHz 7_{5,3} − 6_{6,0} whose first detection is reported in the latter study is expected to show a substantial inversion (as was found in Yates et al., 1997) while this line was not found to be inverted by Neufeld & Melnick (1991).

Finally, Humphreys et al. (2001) presented models for the excitation of the 22, 183, 321 and 325 GHz water lines in the circumstellar envelopes (CSE) of AGB stars. They found the different masing lines to be excited in specific regions of the CSE, thus predicting different morphologies of the emission maps for the masing lines they considered. A direct comparison with their results is not possible, since in their study, the model that describes the circumstellar envelope is rather elaborated. Indeed, they first compute the H_2 volume density, gas temperature and expansion velocity from an hydrodynamical code. As a second step, they randomly define masing spots in the envelope and solve the 1D transfer problem for the various spots using the LVG approximation. The physical parameters that concern each emitting spot is defined according to its distance to the star with respect to the parameters obtained from the hydrodynamical model. Finally, the level populations derived from the LVG calculation are then used in a code that propagates the radiation and that takes into account maser saturation in order to calculate the emission of each spot. Performing such a model is out of the scope of the current study, but it is possible to qualitatively discuss their results with the current ones. In Fig. 9, we show the opacities of various water maser lines as a function of the H_2 volume density. The rate coefficients used consider o–H_2 as a collisional partner and are taken from SET2. The opacities are obtained using the treatment for maser propagation and for each line, the opacity is given at 500K and 1000K.

One of the conclusion drawn by Humphreys et al. (2001) is that the 321 and 22 GHz are sensitive to the acceleration zone of the CSE. Additionally, the 321 GHz line is predicted to trace only a region close to the star while the 22 GHz emission extends further outside (see Fig. 9 of Humphreys et al., 2001). Considering the opacities reported in Fig. 9, we can see that the current results support those findings. Indeed, at densities ∼ 10^9 cm^{−3}, the 22 GHz line is the only masing line which is still subsequently inverted. At such a high H_2 density, the other masing lines are found to be collisionaly quenched. Moreover, the 321 GHz line is inverted only at relatively high H_2 densities, ie. n(H_2) > 2 10^7 cm^{−3} which support the fact that this line only traces the innermost part of the CSE. Humphreys et al. (2001) also find that the emission in the 325 GHz line resembles that of the 22 GHz. In the current study, by examining the behaviour of the opacities of those two lines shown in Fig. 9, we can indeed see that these lines have similar excitation conditions. Additionaly Humphreys et al. (2001) predicted the 183 GHz line to be inverted in the outermost part of the CSE. In this region, the H_2 density is too low to produce inversion in the other masers. Referring to Fig. 9, we can see that at n(H_2) ∼ 10^6 cm^{−3}, the 183 GHz line is indeed subsequently inverted while the other lines are not. Finally, considering the behaviour of the opacities reported in Fig. 9, it is possible to qualitatively predict the morphology that the lines not considered by Humphreys et al. (2001) should have. As an example, the emission in the 380 GHz line should resemble the 183 GHz one and the 439 and 470 GHz lines should behave similarly to the 321 GHz line.

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Table 3. Comparison of the current results with Yates et al. (1997)’s results.

o/p–H_2 O Transition Frequency (GHz) Yates97 current Yates97/current 6_{1,6} − 5_{2,3} 22 1.0 1.00 1.00 10_{2,9} − 9_{3,6} 321 0.59 0.88 0.67 4_{1,4} − 3_{2,1} 380 1.46 1.78 0.82 6_{4,3} − 5_{5,0} 439 0.13 0.63 0.20 7_{5,2} − 6_{6,1} 443 0.14 0.05 2.89 4_{2,3} − 3_{3,0} 448 1.12 1.49 0.75 5_{3,2} − 4_{4,1} 621 0.36 1.69 0.21 6_{3,4} − 5_{4,1} 1158 0.89 0.80 1.11 7_{4,3} − 6_{5,2} 1278 0.09 0.49 0.19 8_{2,7} − 7_{3,4} 1296 1.74 0.76 2.29 6_{2,5} − 5_{3,2} 1322 3.11 0.34 9.17 8_{4,5} − 7_{5,2} 1885 0.31 0.02 15.7 5_{2,3} − 4_{3,2} 1918 1.74 < 0.01 > 173 8_{3,6} − 7_{4,3} 2245 0.86 < 0.01 > 85 7_{3,4} − 6_{4,3} 2567 1.17 < 0.01 > 116 3_{1,3} − 2_{2,0} 183 0.83 1.22 0.68 5_{1,5} − 4_{2,2} 325 1.02 1.24 0.82 7_{5,3} − 6_{6,0} 437 0.10 0.02 4.80 6_{4,2} − 5_{5,1} 471 0.07 0.65 0.11 5_{3,3} − 4_{4,0} 475 0.25 1.40 0.18 9_{2,8} − 8_{3,5} 906 0.60 1.07 0.55 4_{2,2} − 3_{3,1} 916 0.48 0.56 0.86 5_{2,4} − 4_{3,1} 970 1.19 0.80 1.49 7_{2,6} − 6_{3,3} 1441 1.07 0.41 2.62 6_{3,3} − 5_{4,2} 1542 0.11 0.15 0.72 7_{3,5} − 6_{4,2} 1766 0.15 0.07 2.21

Notes. Comparison of the opacities obtained in the present work (column 4) to the one estimated from Yates et al. (1997) (column 3). In this latter case, the opacities are obtained from the population density ratio they reported and making use of Eq. 22 (see text for details). The last column gives the opacity ratio obtained in the two studies.

5. Conclusions

The present work deals with obtaining a self–consistent solution for the problem of maser propagation within the scope of non– local radiative transfer. Test cases are presented for the water molecule in which the importance of dealing with maser propagation is emphasised, by comparison to a simplified treatment for the radiative transfer. The main conclusions are :

1. A self-consistent solution for the radiative transfer in masing

lines can be obtained within the scope of the short characteristic method, with subsequent modification of the algorithm used to treat thermal lines due to the integro–differential nature of the transfer equation.

2. The preconditioning of the statistical equilibrium equations

is not feasible using the current method and the Ng acceleration technique cannot be used, so that the algorithm has the convergence rate of the Lambda iterative scheme.

3. The test cases performed for the water molecule have shown

that neglecting maser propagation can lead to substantial errors in the estimate of the masing line opacities, with differences greater than a factor 2. Dealing with strongly inverted masers, it means errors of several orders of magnitude in the prediction of line intensities.

4. In the region where strong masing lines are present, the radiation field in these lines perturbs the whole population of the molecule. Therefore, including maser propagation also modifies the determination of line opacities for purely thermal lines and in the present test cases, maximum differences of the order of a few 10% are found between the two methods adopted. Nevertheless, the number of lines affected is rather low and most of the lines have identical optical depths in the two treatments. Given the larger computational time required to solve the maser propagation, the approximation used in this study is a good alternative if one is concerned with interpreting the emission of non–masing lines.

5. We give predictions of H_2O maser opacities for physical conditions typical of circumstellar envelopes of AGB stars. In addition, the predictions based on various sets of rate coefficients involving He, p–H_2 or o–H_2 are compared. We find that from one set to another, the relative opacities of the masing lines are similar. However, the absolute scale of the opacities are within a factor ∼ 2 depending on the set used.

Acknowledgements. The authors want to thank the referee M.D. Gray for its useful comments that enable to improve the current manuscript. We also want to thank A. Baudry for useful discussions concerning the current study. The authors want to thank J. Roberts and T. Bell for their careful reading of the manuscript. This paper was partially supported within the programme CONSOLIDER INGENIO 2010, under grant Molecular Astrophysics: The Herschel and ALMA Era.- ASTROMOL (Ref.: CSD2009- 00038). We also thank the Spanish MICINN for funding support through grants AYA2006-14876 and AYA2009-07304.

References

Anderson, N., & Watson, W. D. 1993, ApJ, 407, 620 Bettwieser, E. V., & Kegel, W. H. 1974, A&A, 37, 291 Bettwieser, E. 1976, A&A, 50, 231 Cernicharo, J., Thum, C., Hein, H., John, D., Garcia, P., & Mattioco, F. 1990, A&A, 231, L15 Cernicharo, J., Gonzalez-Alfonso, E., Alcolea, J., Bachiller, R., & John, D. 1994, ApJ, 432, L59 Cernicharo, J., González-Alfonso, E., Bachiller, R. 1996, A&A, 305 Cernicharo, J., Pardo, E., Serabyn et al., 1999, ApJ, 520, L131 Cernicharo, J., Pardo, J.R., Weiss, A., 2006, ApJ, 646, L49

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Cernicharo, J., Goicoechea , J., Pardo, J.R., A. Asensio-Ramos, 2006, ApJ, 642, 940 Cheung, A.C., Rank, D.M., Townes, C.H. et al., 1969, Nature, 221, 626 Collison, A. J., & Nedoluha, G. E. 1995, ApJ, 442, 311 Daniel, F., & Cernicharo, J. 2008, A&A, 488, 1237 Daniel, F., Dubernet, M., Pacaud, F., Grosjean, A. 2010, A&A, 517, A13+ Daniel, F., Dubernet, M., Grosjean, A. 2011, A&A Davies, R. D., Rowson, B., Booth, R. S., Cooper, A. J., Gent, H., Adgie, R. L., & Crowther, J. H. 1967, Nature, 213, 1109 Deguchi, S., & Watson, W. D. 1989, ApJ, 340, L17 Dubernet, M.-L., Daniel, F., Grosjean, A., et al. 2006, A&A, 460, 323 Dubernet, M.-L., Daniel, F., Grosjean, A., & Lin, C. Y. 2009, A&A, 497, 911 Elitzur, M., Hollenbach, D. J., & McKee, C. F. 1989, ApJ, 346, 983 Elitzur, M. 1992, Astrophysics and Space Science Library, 170 Elitzur, M. 1994, ApJ, 422, 751 Emmering, R. T., & Watson, W. D. 1994, ApJ, 424, 991 Faure, A., Crimier, N., Ceccarelli, C., Valiron, P., Wiesenfeld, L., & Dubernet, M. L. 2007, A&A, 472, 1029 Fish, V. L. 2007, IAU Symposium, 242, 71 González-Alfonso E., Cernicharo J., Bachiller R., Fuente A., 1995, A&A, 293, L9 González-Alfonso, E., Cernicharo, J., Alcolea, J., Orlandi, M.A. 1998, A&A, 334, 1016 Gray, M. 1999, Royal Society of London Philosophical Transactions Series A, 357, 3277 Green, S., Maluendes, S., & McLean, A. D. 1993, ApJS, 85, 181 Humphreys, E. M. L., Yates, J. A., Gray, M. D., Field, D., & Bowen, G. H. 2001, A&A, 379, 501 Humphreys, E. M. L. 2007, IAU Symposium, 242, 471 Kylafis, N. D., & Pavlakis, K. G. 1999, NATO ASIC Proc. 540: The Origin of Stars and Planetary Systems, 553 Menten, K.L, Melnick, G.J., Phillips, T.G. 1990a, ApJ, 350, L41 Menten, K.L, Melnick, G.J., Phillips, T.G., Neufeld, D.A., 1990b, ApJ, 363, L27 Menten K., & Melnick G.J. 1991, ApJ, 377, 647 Menten, K. M., Lundgren, A., Belloche, A., Thorwirth, S., & Reid, M. J. 2008, A&A, 477, 185 Neufeld, D. A., & Melnick, G. J. 1991, ApJ, 368, 215 Neufeld, D. A. 1992, ApJ, 393, L37 Olson G.L. and Kunasz P.B. 1987,JQSRT, 38, 325 Phillips, T.G., Kwan, J., and Huggins, P.J. 1980, in IAU Symposium 87 :

Interstellar Molecules, ed. B.H. Andrew (Dordrecht: Reidel), p 21. Rybicki, G. B., & Hummer, D. G. 1991, A&A, 245, 171 Waters, J.W., Gustincic, J.J., Kakar, et al., 1980, ApJ, 235, 57 Watson, W. D., Sarma, A. P., & Singleton, M. S. 2002, ApJ, 570, L37 Weaver, H., Williams, D. R. W., Dieter, N. H., & Lum, W. T. 1965, Nature, 208, 29 Yates, J. A., Field, D., & Gray, M. D. 1997, MNRAS, 285, 303

F. Daniel and J. Cernicharo: Non–local radiative transfer in strongly inverted masers.

Fig. 9. Opacity as a function of H_2 volume density, for various o–H_2O and p–H_2O lines which are found to be substantially inverted at T_K = 500 K (red lines) and T_K = 1000 K (black lines).