arXiv:1408.4114v2 [physics.flu-dyn] 13 Oct 2014

AN ENERGETIC VARIATIONAL APPROACH FOR ION TRANSPORT^∗

SHIXIN XU^† , PING SHENG^‡ , AND CHUN LIU^§

Abstract. The transport and distribution of charged particles are crucial in the study of many physical and biological problems. In this paper, we employ an Energy Variational Approach to derive the coupled Poisson-Nernst-Planck-Navier-Stokes system. All physics is included in the choices of corresponding energy law and kinematic transport of particles. The variational derivations give the coupled force balance equations in a unique and deterministic fashion. We also discuss the situations with different types of boundary conditions. Finally, we show that the Onsager’s relation holds for the electrokinetics, near the initial time of a step function applied field.

Key words. Energetic Variational Approach, Poisson-Nernst-Planck (PNP) system, (Least)

Action Principle, (Maximum) Dissipation Principle, Onsager’s relation.

subject classifications. 35Q35, 35Q92, 76W05, 92B05.

1. Introduction and Background The Poisson-Nernst-Planck (PNP) system is one of the most extensively studied models for the transport of charged particles in many physical and biological problems, such as free moving electrons in semiconductors [14, 19, 20], fuel cell [21, 25], ion particles in the electrokinetic fluids [3, 12, 15, 18], and ion channels in cell membranes [2, 6, 22]. Traditionally, the PNP system can be derived by explicit averaging of correlated Brownian trajectories [5], while the actual dynamics of charged particles in water and protein channels are much more complicated [7]. In continuum description, the PNP system can also be viewed as the consequence of both conservation of ion distributions and the Fick’s law. The limitation of this method is that the specific interactions of particles are usually ambiguous or totally neglected. The purpose of this paper is to present an alternative way, an Energetic Variational Approach (EnVarA) [8], in which a consistent, coupled system of equations can be derived for the description of charged particles transport. Our approach is motivated by the seminal work of Lars Onsager [23, 24], that has an attribution to Lord Rayleigh’s 1873 paper [30].

The general framework of EnVarA is the combination of the statistical physics and nonlinear thermodynamics. The First Law of Thermodynamics states that the rate of change of the sum of the kinetic energy K and the internal energy U is equal to the sum of the rates of change of work W and heat Q, so^{d(K+U)}_{dt} =^{dW}_{dt} +^{dQ}_{dt} . From the standard statistical physics, the internal energy U takes into account the particles interactions. Such interactions can be local, such as hard core interactions and nonlocal, such as Coulomb electro static interactions. The Second Law of Thermodynamics, in the isothermal case, is given by, T^{dS}_{dt} =^{dQ}_{dt} +Δ, where T is temperature, S is entropy and Δ ≥ 0 is entropy production. As a reformulation of the linear response assumption, this entropy production functional can be represented as the sum of various rates such as the velocities and the strain rates. By subtracting the Second Law from the First ∗ †Department of Mathematics, University of Science and Technology of China, Hefei 230026, China, (xsxztr@mail.ustc.edu.cn).

‡Department of Physics, Hong Kong University of Science and Technology Clear Water Bay, Kowloon, Hong Kong, China, (sheng@ust.hk).

§Department of Mathematics, Pennsylvania State University, University Park, PA, 16802, USA (liu@psu.edu). 1

Law, under the isothermal assumption, we have, d dt (K +U −T S) = dW dt −Δ, (1.1)

where F := U −T S is the Helmholtz free energy, and K +F is the total energy E^{total}. In case no external forces or fields are applied, i.e.,^{dW}_{dt} = 0, the above expression yields the usual energy dissipation law [8, 9, 26, 27], where the entropy production is the sole contribution to the dissipation, d dt E^{total} +Δ = 0 ⇔ d dt E^{total} = −Δ. (1.2) The (Least) Action Principle (LAP) states that the equation of motion for a Hamiltonian system is the direct result of the variation of the action functional A = ∫_t∗ 0 ∫ Ω(K −F)dxdt with respect to the flow map x(t) = x(X,t) (with x(X,0) = X) [1].

In other words, LAP optimizes the action with respect to all trajectories x(t) = x(X,t) by taking the variation with respect to x, δA = ∫_t∗ 0 ∫ Ω_0 [Fcon]·δxdXdt, where Fcon is the conservative force and Ω_0 is the Lagrangian reference domain of Ω. In particular, in equilibrium, we have the condition F_{con} = 0 for a Hamiltonian dynamics.

Next, we treat the dissipation part with the (Maximum) Dissipation Principle (MDP) [23, 24, 29, 11]. Take the variation with respect to the velocity (rate) in Eulerian coordinates δ(^1_2 Δ) = ∫ Ω[F_{dis}]·δudx, where F_{dis} is dissipative force. Note that the factor^1_2 corresponds to the underlying assumption that Δ is quadratic in the function u. In particular, F_{dis} is linear in u, indicating the fact that we can view MDP as just a reformulation of the linear response assumption of the nonequilibrium thermodynamics [16]. Such postulations are the key to Onsager’s approach [23, 24], as realized by Kubo [16] in the more explicit linear response theory.

The final equation of motion, the balance of all forces, includes both conservative and dissipative components.

The following auxiliary Lemma is crucial in the energetic variational derivation of the system of coupled equations.

Lemma 1.1. Let f satisfy the mass conservation law f_t +∇·(uf) = 0. Define W = ∫ Ω ω(f)dx and Π(ω) = ω_f f −ω , and then δW = ∫ Ω ∇Π·δxdx. Proof: The conservation of mass is equivalent to f(x(X,t),t) =^{f0 (X)}_J , which is a direct consequence of the identity F_t +u·∇F = ∇uF , where f_0(X) is the initial density, J = detF , F (X,t) =^{∂x(X,t)}_{∂X} is the deformation gradient tensor [9]. Rewrite the integration

in the Lagrangian coordinate system and obtain W = ∫ Ω_0 ω( f_0(X) J )JdX. Taking the

variation with respect to flow map x → x+εy, it yields δW = d dε | | |_{ε=0}W (x+εy) = d dε | | |_{ε=0} ∫ Ω_0 ω( f_0(X) J(x+εy) )J(x+εy)dX = − ∫ Ω_0

ω_f ( f_0(X) J ) f_0(X) J^2 ·tr( ∂X ∂x ∂y ∂X )·J^2dX + ∫ Ω_0 ω( f_0(X) J )·J ·tr( ∂X ∂x ∂y ∂X )dX = ∫ Ω −(ω_f f −ω,∇_xỹ)dx = ∫ Ω (∇(ω_f f −ω),ỹ)dx, (1.3) where ỹ(x(X,t),t) = y(X,t). Hence the result holds. ■ Remark 1.2. The above Lemma relates the pressure (the equation of states) to the free energy density. For given energy dissipation law^d_{dt} E^{total} =^d_{dt} ∫ Ω ω(f)dx =

− ∫ Ω f|u|^2dx, if ω(f) = cf lnf only contains the Gibbs entropy, i.e. no particle interactions, hence ideal gas, then Π = ω_f f −ω = cf. In particular, f satisfies f_t = c△f, which is a simple diffusion equation [8].

If ω(f) = af^γ, then Π = ω_f f −ω = a(γ −1)f^γ. In particular, f satisfies f_t = △(a(γ −1)f^γ), which gives the diffusion equation in porous media [31].

Next, we use the compressible Navier-Stokes (NS) equations as an example to illustrate the framework of EnVarA. We start with the kinematic mass conservation,

ρ_t +∇·(ρu) = 0, (1.4)

where ρ is mass density of fluid and u is velocity of fluid. This is equivalent to the

relation ρ(x(X,t),t) = ρ_0(X) J , where J = detF , F (X,t) =^{∂x(X,t)}_{∂X} is the deformation gradient tensor and ρ_0(X) is the initial density [9]. The following energy dissipation law includes all the physics for these Barotropic fluids [28]. d dt ∫ Ω ( 1 2 ρ|u|^2 +ω(ρ) ) dx = − ∫ Ω [ μ_1|∇u|^2 +μ_2|∇·u| ] dx, (1.5) where μ_1 and μ_2 are viscosity constants and ω(ρ) is the Hemholtz free energy density.

By LAP and Lemma 1.1, we obtain the conservative force

F_{con} = −(ρ(u_t +u·∇u)+∇Π(ρ)), (1.6)

with Π(ρ) = ω_ρρ−ω being the pressure. By MDP, the dissipative force is ,

F_{dis} = −(∇·(μ_1∇u)+∇(μ_2∇·u)). (1.7)

Finally, the total force balance gives the Navier-Stokes equation,

ρ(u_t +u·∇u)+∇Π(ρ) = ∇·(μ_1∇u)+∇(μ_2∇·u). (1.8)

The conservative force corresponds to the compressible Euler equation, while the dissipative force corresponds to the Stokes equation. Navier-Stokes equation can be viewed as a hybrid model combining these two independent system.

In this paper, we use the EnVarA to derive the electrokinetic systems by considering the particles interactions in the dissipation part and the corresponding energy law. The outline of paper is as follows: in §2, we present the derivation of the electrokinetic system, Poisson-Nernst-Planck-Navier-Stokes(PNP-NS) system, by using the EnVarA; in §3 we focus on the energy law of the PNP-NS system with different types of boundary conditions; the Onsager relation is proved in §4; conclusion part is given in §5.

2. Derivation of Electrokinetic System Using EnVarA Ion transport in solutions by nature is a multiscale-multiphysics system. With the macroscopic hydrodynamics description, the microscopic dynamics takes account of diffusion and convection as well as electrostatics. The cross scale coupling can be modeled in the general EnVarA framework. The total energy include all the equilibrium physics included in system E^{total} = ∫ Ω ρ 2 |u|^2dx macroscopic + [ K_BT (nln n n_∞ +pln p p_∞ )+ ε 2 |∇ϕ|^2 ]

microscopic dx, (2.1) where ρ is the mass density of fluid, u is the macroscopic velocity of fluid, K_B is the Boltzmann constant, T is the absolute temperature, n_∞(p_∞) is the characteristic negative(positive) charge distribution, n(p) is negative (positive) charge distribution, the dielectrics of solution is chosen to be the constant ε, and ϕ is electric potential. The first term is the macroscopic kinetic energy of the solution fluids. The second and third terms are the thermo-fluctuations (Gibbs entropy) of the ion species. The last term is the electro energy.

In the macroscopic scale, we consider the fluid to be incompressible, i.e. ∇·u = 0. At the same time, we observe the following kinematic conservation of charge distributions,

n_t +∇·(nu_n) = 0, p_t +∇·(pu_p) = 0, (2.2)

where u_n and u_p are the effective velocities of negative and positive charges, respectively. The Gauss’s law yields the Poisson equation, −ε△ϕ = ze(p−n), (2.3) where z is valence of ion and e is the charge for one electron. Equivalently, the potential ϕ can be given by the Green’s kernel G(x,y) in the form of ϕ(x) = ze 1 ε ∫ Ω G(x,y)(n−p)(y)dy. (2.4) By substituting (2.4) into (2.1), the energy can be written in the following form E^{total} = ∫ Ω ρ 2 |u|^2dx+ ∫ Ω K_BT (nln n n_∞ +pln p p_∞ )dx (2.5) + ze 2ε ∫ Ω (p−n)(x) ∫ Ω G(x,y)(n−p)(y)dydx, where the last term, the electrostatic energy, represents the nonlocal Coulomb interactions.

In order to take into account the more detailed interactions of particles, we furthermore consider the dissipation functional Δ as a sum of three parts, which are all quadratic in terms of the ’rates’, the velocities, Δ = ∫ Ω [ K_B T D_n n|u_n −u|^2 + K_B T D_p p|u_p −u|^2 +η|∇u|^2 ] dx, (2.6) where D_n (D_p) is the diffusion constant of negative (positive) ion and η is the viscosity of fluid. The first and second terms represent the frictions between particles and the solvents. The last term is the fraction caused by the viscosity of the solutions.

Now we begin to use the EnVarA to derive the electrokinetic system. In this case, there are three flow maps corresponding to three velocities fields, u, u_n, u_p: macroscopic flow map x(X,t), negative charge map x_n(X,t) and positive charge map x_p(X,t), respectively. For map x_n, Lemma 1.1, Remark 1.2 and the variation yield, F_{n−con} = δA δx_n = δ δx_n [∫_{t∗} 0 (∫ Ω ρ 2 |u|^2dx− ∫ Ω K_B T (nln n n_∞ +pln p p_∞ )dx − ze 2ε ∫ Ω (p−n)(x) ∫ Ω G(x,y)(n−p)(y)dydx ) dt ]

= −(K_BT ∇n−zen∇ϕ) = −n∇μ_n, (2.7) where μ_n :=^δ_{δn} E^{total} = K_BT (1+lnn)−K_B T lnn_∞ −zeϕ is the chemical potential for negative charge distribution n(x,t).

Using MDP, we calculate the variation of^1_2 Δ with respect to the velocity u_n to get the dissipative force, F_{n−dis} = δ δu_n ( 1 2 Δ) = K_B T D_n n(u_n −u). (2.8)

The total force balance for negative charge yields (including (2.7) and (2.8)):

nu_n = nu− D_n K_BT n∇μ_n. (2.9) Substituting (2.9) into (2.2), the mass conservation of negative charge is: n_t +∇·(un) = ∇· ( D_n∇n− ze K_BT D_nn∇ϕ ) . (2.10)

Similarly for positive charge, we can get

pu_p = pu− D_p K_B T p∇μ_p, (2.11) p_t +∇·(up) = ∇· ( D_p∇p+ ze K_BT D_pp∇ϕ ) , (2.12)

where μ_p :=^δ_{δp} E^{total} = K_BT (1+lnp)−K_B T lnp_∞ +zeϕ is the chemical potential for positive charge distribution p(x,t). In the absence of the flow field u, equations (2.10) (2.12) with the Poisson equation (2.3) give the PNP system .

As for the macroscopic flow map x(X,t), considering the incompressible condition, we use 1-parameter family of volume preserving diffeomorphisms to perform the variation, i.e. function x^ε such that x^0 = x, and^{dxε}_{dε} | | |_{ε=0} = y, and for any ε : det^{∂xε}_{∂X} = 1, which in fact leads to a divergence free condition for y(X,t) = ỹ(x(X,t),t), i.e. ∇_x ·ỹ = 0. For LAP, we use the variations x^ε of x as described above and with y satisfying y(X,0) = y(X,t^∗) = 0 for any X ∈ Ω_0. We can calculate the variation of action functional: d dε | | |_{ε=0}A(x^ε) = d dε | | |_{ε=0} ∫_t∗ 0 ∫ Ω_0 1 2 ρ_0(X)|x^ε_t |dXdt (2.13) = ∫_{t∗} 0 ∫ Ω_0 −ρ_0(X)(x_t)_t ·ydXdt = ∫_t∗ 0 ∫ Ω −ρ(x,t)(u_t +u·∇_xu)·ỹdxdt. Hence by the Weyl’s decomposition or Helmholtz’s decomposition, for some Π_1 ∈ W^{1,2}(Ω), we have,

−ρ(x,t)(u_t +u·∇_xu) = ∇_xΠ_1. (2.14)

By MDP and incompressible constrain, we obtain the following equation of motion for the dissipative part, −η△u+ K_B T D_n n(u−u_n)+ K_B T D_p p(u−u_p) = ∇Π̃_2, (2.15) where Π̃_2 is the Lagrange multiplier of incompressible constrain.

Substitute (2.9) and (2.11) into above formula and let Π_2 = Π̃_2 −K_BT ∇n− K_B T ∇p, ∇Π_2 = −η△u−(n−p)ze∇ϕ. (2.16) Then using the force balance, (2.14) and (2.16) yield ρ( ∂u ∂t +(u·∇)u) = η△u−∇Π+(n−p)ze∇ϕ, (2.17) with Π = Π_1 −Π_2. The last term is the Lorentz force induced by the charges in the fluids. It is the reaction to the convected term in (2.10) and (2.12), which is consistent with the Newton’s third Law. Combining (2.3), (2.10), (2.12), (2.17) and incompressibility, we get the coupled Poisson-Nernst-Planck-Navier-Stokes (PNP-NS) system: n_t +∇·(un) = ∇· ( D_n∇n−^{ze}_{KB T} D_nn∇ϕ ) = −∇·J_n, p_t +∇·(up) = ∇· ( D_p∇p+^{ze}_{KB T} D_pp∇ϕ ) = −∇·J_p, −ε△ϕ = ze(p−n), ρ(^{∂u}_{∂t} +(u·∇)u) = η△u−∇Π+(n−p)ze∇ϕ, ∇·u = 0. (2.18)

Finally in this section, we verify the following theorem satisfied by the derived coupled PNP-NS system (2.18).

Theorem 2.1. With the isothermal assumption and vanishing boundary conditions, the system (2.18) satisfies the following energy dissipation law, d dt E^{total} = d dt [∫ Ω ( ρ 2 |u|^2 +K_BT (nln n n_∞ +pln p p_∞ )+ ε 2 |∇ϕ|^2 ) dx ]

= − ∫ Ω [ D_n K_BT n|∇μ_n|^2 + D_p K_BT p|∇μ_p|^2 +η|∇u|^2 ] dx = − ∫ Ω [ K_BT D_n n|u_n −u|^2 + K_BT D_p p|u_p −u|^2 +η|∇u|^2 ] dx = −Δ. (2.19)

Reversely, if we choose the action functional as A = ∫_t∗ 0 ∫ Ω ρ 2 |u|^2dx− ∫ Ω K_B T (nln n n_∞ +pln p p_∞ )dx− ε 2 |∇ϕ|^2dx, and the dissipation functional as (2.6), then by (Least) Action Principle and (Maximum) Dissipation Principle, under the kinematic assumption of distribution (conservation law) (2.2) and Poisson equation, we can obtain the Poisson-Nernst-Planck- Navier-Stokes system (2.18).

Sketch of Proof: From the energy law to PNP-NS system are above derivations. By adding the first equation multiplied by μ_n, second equation multiplied by μ_p, and fourth equation multiplied by u together, and using the weak form of Poisson equation, we can get the energy law. ■ Remark 2.2. Some more complicated models can be derived by including more coupling terms for particle interactions in the total energy E^{total}, such as

1. In [8, 10], it is shown that, by EnVarA, a modified model can be derived naturally for ion particles with finite size effects, through adding interaction term E^{repulsion} = ∑_N i=1 ∑_N j≥i 1 2 ∫ Ω Ψ_{i,j} (|x−y|)c_i(x)c_j (y)dxdy to the total energy, where c_i, c_j mean different species of ions, and Ψ_{i,j} (|x−y|) =^{εij (aj +ai)}_{|x−y|12} is Lennard-Jones (LJ) potential for ith and jth ions located at x and y with the radii a_i, a_j , respectively.

2. If we add E^{surf ace} = ze ∫ Ω(p−n)Ψ_s to the total energy, we can derive the surface potential trap model [32] to describe the electrokinetics induced by the interface of solid and solution, where Ψ_s is a surface potential only depending on the property of material.

3. Boundary Conditions In electrokinetics, most physically interesting properties arise from different boundary conditions [4, 17, 33]. These boundary conditions represent the interactions between particles in the bulk solutions and the particles in or near the boundary [32]. The interactions can also be included into the energy functionals. As in the previous sections, we assume the non-flux boundary condition J_n ·ν = J_p ·ν = 0 for charge density, with ν being out normal vector, and the nonslip boundary condition u = 0 for velocity. We will focus on the boundary effect of potential ϕ which plays an important role in electrodynamics. For the three different boundary conditions, the PNP-NS system has the following theorem. Theorem 3.1. If n, p satisfy J_n ·ν = J_p ·ν = 0, and u = 0 on the boundary ∂Ω, then 1. if ϕ = ϕ_0(x), i.e. Dirichlet boundary, then PNPNS satisfies the energy law, d dt E^{total} = d dt [∫ Ω ρ 2 |u|^2 +K_BT (nln n n_∞ +pln p p_∞ )+ ε 2 |∇ϕ|^2 ] dx (3.1) = − [∫ Ω D_n K_BT n|∇μ_n|^2 + D_p K_BT |∇μ_p|^2 +η|∇u|^2dx ] +ε ∫ ∂Ω ∂ϕ ∂ν ϕ_0dx; 2. if^{∂ϕ}_{∂ν} =^{σ0 (x)}_ε , i.e. Neumann boundary condition, then PNPNS satisfies the energy law, d dt E^{total} = d dt [∫ Ω ρ 2 |u|^2 +K_BT (nln n n_∞ +pln p p_∞ )+ ε 2 |∇ϕ|^2 ] dx (3.2) = − [∫ Ω D_n K_BT |∇μ_n|^2 + D_p K_B T |∇μ_p|^2 +η|∇u|^2dx ] + ∫ ∂Ω σ_0ϕdx; 3. if ϕ+ζ^{∂ϕ}_{∂n} = ϕ_0(x), i.e Robin boundary condition, then PNPNS satisfies the energy law, d dt E^{total} = d dt [∫ Ω ρ 2 |u|^2 +K_B T (nln n n_∞ +pln p p_∞ )+ ε 2 |∇ϕ|^2 + ε 2ζ ∫ ∂Ω |ϕ|^2dx ]

= − [∫ Ω D_n K_B T |∇μ_n|^2 + D_p K_B T |∇μ_p|^2 +η|∇u|^2dx ] . (3.3)

Remark 3.2.

1. When ϕ on the boundary is Robin boundary condition, as time approaches infinity, (3.3) means ∇μ_n = ∇μ_p = ∇u = 0. Considering the boundary condition, it yields J_n = J_p = u = 0, which means there is no fluid flux in the time limit. Then we can derive a Charge Conservation Poisson Boltmann (CCPB) equation [17, 32] −ε△ϕ = zen_∞V ( β exp(−zeϕ/K_BT ) ∫ Ω exp(−zeϕ/K_BT )dx − αexp(zeϕ/K_BT ) ∫ Ω exp(zeϕ/K_BT )dx )

as the time limit of PNPNS system, where α =^{n0}_{n∞} and β =^{p0}_{n∞} with n_0 (p_0) being the initial negative (positive) ion distribution.

2. In the ion transport process, most of time an extra field is added to the domain to generate the electrodynamics phenomena. When there is an external filed added to the PNPNS system, there will be an extra term ∫ Ω(p−n)Ψdx added to the total energy in Theorem 3.1, where −∇Ψ is the extra electric field [13, 32].

4. Onsager’s Relation in Cylindrical Situation The coupling between the flow field and the electric field gives arise to all the important properties and applications of the electrokinetic fluids. For instance, when the fluid-solid interface is charged, the application of an electrical voltage difference can induce a fluid flow. This effect is known as electroosmosis (EO). Conversely, the application of a pressure gradient can generate, besides fluid flow, a voltage difference that is denoted as the streaming potential (SP). The EO and SP coefficients are not independent. They are related by the well-known Onsager’s reciprocal relation [23, 24]. It dictates that the electric current density J_e and the fluid current density J_f be linearly related to the voltage gradient ∇ϕ and the pressure gradient ∇Π : [ J_e J_f ] = − [ L_{11} L_{12} L_{21} L_{22} ][ ∇ϕ ∇Π ] , (4.1)

where L_{11} is the electrical conductivity and L_{21} is the hydrodynamic permeability. In literature [33], the proportional matrix is treated as symmetric and attributed to Onsager’s relation. Onsager’s reciprocal relation, the microscopic reversibility [23, 24] is a stability conditions. It is manifested by specific coupling effects in different physical settings. In (4.1), it is a reformulation of the fact that Lorentz force and the transport of charge are action and reaction.

Onsager’s reciprocal relation has many forms in different settings. Here we take the axisymmetric cylinder coordinate for low Reynolds number situations with constant initial values, i.e. p(·,0) = p_0, n(·,0) = n_0 as an example. Then the PNP-NS system is simplified to be the Poisson-Nernst-Planck-Stokes (PNP-S) system. If an extra filed E_z and a pressure drop^{∂π}_{∂z} are added in z direction, the velocity u_z satisfies ∂Π ∂z −μ [ 1 r ∂ ∂r (r ∂u_z ∂r ) ] = (p−n)ze(− ∂ϕ ∂z +E_z), (4.2)

with u_z(r = a) = ϕ(r = a) = 0 . At the initial several steps,^{∂ϕ}_{∂z} ,^{∂p}_{∂z} ,^{∂n}_{∂z} and^{∂uz}_{∂z} are small and negligible. Then we can get

u_z = εE_zϕ μ + a^2 −r^2 4μ (− ∂Π ∂z ). (4.3)

And the fluxes for the negative and positive charges in z direction are

J_n = − ( D_n ∂n ∂z −D_n ze K_B T ( ∂ϕ ∂z −E_z)n ) = − ze K_BT nD_nE_z (4.4)

J_p = − ( D_p ∂p ∂z +D_p ze K_B T ( ∂ϕ ∂z −E_z )p ) = ze K_BT pD_pE_z . (4.5)

The total electric current in z direction is the sum of the current carried (transported) by the flow field u and the current due to the electric field,

J_e = ∫_L −L ∫_a 0 2(p−n)zeu_zrdrdz + ∫_L −L ∫_a 0 2ze(J_p −J_n)rdrdz 2La^2 = E_z [ ε μa^2 ∫_a 0 rze(p−n)dr + z^2e^2 K_B T E_z(D_pp_0 +D_nn_0) ]

+(− ∂Π ∂z ) 1 2μa^2 ∫_a 0 (p−n)ze(a^2 −r^2)rdr. (4.6) The fluid flux in z direction is

J_f = ∫_L −L ∫_a 0 2u_zrdr 2La^2 = 2εE_z μa^2 ∫_a 0 ϕrdr +(− ∂Π ∂z ) 1 2μa^2 ∫_a 0 (a^2 −r^2)rdr. We may write the Onsager relation as [ J_e J_f ] = [ L_{11} L_{12} L_{21} L_{22} ][ E_z −^{∂Π}_{∂z} ] , (4.7)

where we have introduced the function forms of the coefficients,

L_{12} = 1 2μa^2 ∫_a 0 rze(p−n)(a^2 −r^2)dr, L_{21} = 2ε μa^2 ∫_a 0 ϕrdr. (4.8) But by the Poisson equation, L_{12} can be rewritten as

L_{12} = − ε 2μa^2 ∫_a 0 (a^2 −r^2)( 1 r ∂ϕ ∂r + ∂^2ϕ ∂r^2 )rdr = − ε 2μa^2 [ (−a^2ϕ(0)+2 ∫_a 0 ϕrdr)+(a^2 ϕ(0)− ∫_a 0 6rϕdr) ]

= 2ε μa^2 ∫_a 0 rϕdr = L_{21}, (4.9)

which gives the symmetric property of the matrix.

5. Conclusion In this paper, we derive the electrokinetic system for ion transport in solutions by using an Energy Variational Approach. Taking into consideration of particles interactions in both the free energy functional and the dissipation functional, we obtain the Poisson-Nernst-Planck-Navier-Stokes system. We can extend our theory to include more detailed description of the solutions, such as the finite size effects of the charged particles and various boundary effects. Since the boundary condition of potential play an important role in electrokinetic, we also present the boundary effects to the energy law. The energy laws with an external electric field under different boundary conditions of potential are also obtained. A short demonstration of Onsager’s relation is presented for the Poisson-Nernst-Planck-Stokes system under cylinder axisymmetric coordinate.

6. Acknowledgment P. S. wishes to acknowledge the support of SRFI11/SC02 and RGC grant HKUST604211 for this work. C. L. and S. X wishes to acknowledge the partial support by the NSF grants DMS-1109107, DMS-1216938 and DMS-1159937. S. X. also wishes to acknowledge China Scholarship Council for support.

10 An Energetic Variational Approach for ion transport

REFERENCES

[1] V.I. Arnold, Mathematical methods of classical mechanics, second edition, Springer-Verlag, New York, 1989.

[2] M. Z. Bazant, K. Thornton, and A. Ajdari, Diffuse-charge dynamics in electrochemical systems, Physical Review E, 70, 021506, 2004.

[3] Y. Ben and H. C. Chang, Nonlinear Smoluchowski slip velocity and micro-vortex generation, J. Fluid Mech., 461, 229-238, 2002.

[4] D. L. Chapman, A Contribution to the Theory of Electrocapillarity, Philos. Mag. 25, 475, 1913. [5] Z. Schuss , B. Nadler and R. S. Eisenberg, Derivation of Poisson and Nernst-Planck equations in a bath and channel from a molecular model, Rhys. Rev. E, 64, 1-14, 2001.

[6] R. S. Eisenberg, Computing the field in proteins and channels, J. Mem. Biol., 150, 1- 25, 1996. [7] B. Eisenberg, The value of Einsteins mistakes, Phys. Today (Letter to the Editor), 59(4), 12, 2006.

[8] B. Eisenberg, Y. Hyon, and Chun Liu, Energy variational analysis of ions in water and channels: Field theory for primitive models of complex ionic fluids, J Chem Phys., 133(10), 104104, 2010.

[9] Johannes Forster, Mathematical Modeling of Complex Fluids, master theis, University of Wüurzburg, 2013.

[10] Y. Hyon, J. E. Fonseca, B. Eisenberg and C. Liu, Energy variational approach to study charge inversion(layering) near charged walls, DCDS-B, 17(8), 2725 - 2743, 2012.

[11] Y. Hyon, D. Y. Kwak, and C. Liu, Energtic Variational Approach in Complex Fluids: Maximum Dissipation Principle, 26(4), 1291-1304, 2010.

[12] R. J. Hunter, Foundations of Colloid Science, Oxford University Press, Oxford, 2001. [13] J. D. Jackson, Classical electrodynamics, third version, Wiley, 1999.

[14] J. W. Jerome, Analysis of Charge Transport. Mathematical Theory and Approximation of Semiconductor Models, Springer-Verlag, New York, 1995.

[15] X. Z. Jin, S. Joseph, E. N. Gatimu, P. W. Bohn, and N. R. Aluru, Induced Electrokinetic Transport in Micro-Nanofluidic Interconnect Devices, Langmuir, 23, 13209-13222, 2007.

[16] R. Kubo, Thermodynamics: An advanced course with problems and solutions, North-Holland Pub. Co., 1976.

[17] C. C Lee, H. Lee, Y. K. Hyon, T-C Lin and C. Liu, New Poisson-Boltzmann Type Equations:

One-Dimensional Solutions, Nonlinearity 24, 431, 2011.

[18] J. Lyklema, Fundamentals of Interface and Colloid Science. Volume II: Solid-Liquid Interfaces, Academic Press Limited, San Diego, CA, 1995.

[19] P. A. Markowich, The Stationary Seminconductor Device Equations, Springer-Verlag, Vi- enna, 1986.

[20] P. A. Markowich, C. A. Ringhofer, and C. Schmeiser, Semiconductor Equations, Springer- Verlag, New York, 1990.

[21] I. Nazarov and K. Promislow, The Impact of Membrane Constraint on PEM Fuel Cell Water Mnagement, submitted to J. Electrochem. Soc.

[22] W. Nonner, D. P. Chen, and B. Eisenberg, Progress and prospects in permeation, J. Gen.

Physiol., 113, 773-782, 1999.

[23] L. Onsager, Reciprocal relations in irreversible processes. I., Phys. Rev., II. Ser. 37, 405-426, 1931.

[24] L. Onsager, Reciprocal relations in irreversible processes. II., Phys. Rev., II. Ser. 38, 2265-2279, 1931.

[25] K. Promislow and J. M. Stockie, Adiabatic Relaxation of Convective-Diffusive Gas Transport in a Porous Fuel Cell Electrode, SIAM J. APPL. MATH., 62(1), 180-205, 2001.

[26] T. Z. Qian, X. P. Wang, and P. Sheng, A variational approach to the moving contact line hydrodynamics, J. Fluid Mech. 564, 333-360, 2006.

[27] R. J. Ryham, An energetic variational approach to mathematical modeling of charged fluids:

charge phases,simulation and well posednes, thesis Pennsylvania State University, 2006. [28] I. H.Shames, Mechanics of Fluids, McGraw-Hill, 159, 1962.

[29] P. Sheng, J. Zhang, and C. Liu, Onsager Principle and Electrorheological Fluid Dynamics, Progress of Theoretical Physics Supplement, 175, 131-143, 2008.

[30] J. W. Strutt, Some general theorems relating to vibrations, Proc. of L. M. S. IV, 357-368, 1873. [31] J. L. Vázquez, Nonlinear Diffusion with Fractional Laplacian Operators, Nonlinear Partial Differential Equations Abel Symposia, 7, 271-298, 2012.

[32] L. Wan, S. Xu M. Liao, C. Liu and P. Sheng, New Perspectives on Electrokinetics, submited. [33] Z. Xu, J. Y. Miao, N. Wang, W. Wen, P. Sheng, Digital Flow Control of Electroosmotic Pump:

Onsager Coefficients and Interfacial Parameters Determination, Sol. St. Comm., 151, 440,

2011.