arXiv:1505.06046v1 [astro-ph.CO] 22 May 2015

CONSTRAINING THE DISTANCE TO INSPIRALING NS-NS WITH EINSTEIN TELESCOPE

I. KOWALSKA-LESZCZYNSKA^1, T. BULIK^1 1Astronomical Observatory, University of Warsaw, Al Ujazdowskie 4, 00-478 Warsaw, Poland

1 Introduction

Einstein Telescope (ET) is a planned third generation gravitational waves detector located in Europe1. Its design will be different from currently build interferometers: First, ET will be located underground in order to reduce the seismic noise. The arms length will be 10 km, and the configuration of arms will be different from all interferometers build so far i.e. there will be three tunnels in a triangular shape. ET will consist of three interferometers rotated by a 60deg with respect to each other in one plane. One of the biggest challenges for ET will be to determine sky position and distance to observed sources. If an object is observed in a few interferometers simultaneously one can estimate the position using traingulation from time delays2, but so far there are no plans for a network of third generation detectors. Another possibility to deal with that problem is by using multimessenger approach, because redshift and sky position could be recovered from electromagnetic observations. However, in most cases of ET detection there will be only gravitational signal. In this paper we present a novel method of estimating distance and position in the sky of merging binaries. While our procedure is not as accurate as the multimessenger method, it can be applied to all observations, not just the ones with electromagnetic counterparts.

2 Distance estimation using one interferometer

For simplicity let us consider the case of observation of a double neutron star. In gravitational waves we will be observing directly two quantities: signal to noise ratio (ρ), which is a complicated function of the source properties, as well as the detector characterization, and redshifted chirp mass (M_z = (1 + z)M_{chirp}, M_{chirp} = (M_1M_2)^{3/5}(M_1 + M_2)^{−1/5}). In this particular case we consider only binaries consisting of two neutron stars of equal masses M_1 = M_2 = 1.4 M_⊙, so M_{chirp} = 1.2 M_⊙. The signal to noise ratio in the quadruple approximation for merging double compact objects is well known 3: ρ ∼ Θ d_L(z) (M_z)^{5/6} √ ξ(z), (1) where d_L is the luminosity distance, M_z is the redshifted chirp mass, z is the redshift, Θ is a function of sky position and orientation of the source, and ξ is the function that determines fraction of the sensitivity window filled by a signal (it depends on the chirp mass, and for NSNS binaries its value is close to unity). For a given binary that will be observed in the detector, we can measure ξ directly, by measuring the cutoff frequency when the inspiral ceases.

The function Θ depends on the sky position of the source Ω(ϑ, φ) and on the orientation of the orbit with respect to the line of sight Ω_p(Ψ, i):

Θ = 2 √ (1 + cos^2 i)(F_+)^2 + 4 cos^2 i(F_x)^2, F_+ = 0.5(1 + cos^2 ϑ) cos 2φ cos 2Ψ − cos ϑ sin 2φ sin 2Ψ, F_x = 0.5(1 + cos^2 ϑ) cos 2φ sin 2Ψ + cos ϑ sin 2φ cos 2Ψ. (2)

The density of sources in a unit volume can be expressed by:

d^2n dzdΩdΩ_p = n(z) 1 + z dV dz . (3)

The comoving volume is^{dV}_{dz} = 4π^c_{H0}^{r2(z)}_{E(Ω,z)} , and E(Ω, z) = √ Ω_Λ + Ω_M (1 + z)^3. Then we obtain for a single detector dn dz = ∫ dΩdΩ_p n(z) 1 + z δ(ρ − ρ_m) = 4π n(z) 1 + z c H_0 r^2(z) E(Ω, z) d_L 8r_0 ( 1.2 M_z )_{5/6} 1 √ ξ × P ( ρ^m 8r_0(^{Mz}_{1.2} )^{5/6} √ ξ d_L(z) ) , (4)

where n(z) is the merger rate, r_0 is the characteristic distance for a given detector (see Table 1 in paper by Taylor4 for more details), ρ^m is the actual signal-to-noise ratio measured in the detector.

3 Distance estimation using three co-located interferometers

Design of the Einstein Telescope assumes three co-located interferometers lying in the same plane, so the methods for distance estimation based on triangulation will not be possible. However, a single source will be observed by each of the interferometer with a different orientation. There will be three different measurements of signal to noise ratio. That will provide additional information about the observed source and it allows to constrain the distributions obtained in previous section.

The density of sources per unit volume given by Eq. 3 has to be integrated taking into account that we have three conditions to satisfy.We assume that each signal to noise ratio is measured with perfect accuracy: dn dz = ∫ dΩdΩ_p n(z) 1 + z δ(ρ_1 − ρ^m_1 )δ(ρ_2 − ρ^m_2 )δ(ρ_3 − ρ^m_3 ) = ∫ d^2n dzdΩdΩ_p 4π n(z) 1 + z c H_0 r^2(z) E(Ω, z) d_L 8r_0 ( 1.2 M_z )_{5/6} 1 √ ξ(ρ^m_1 )^2 × δ ( Θ_1 − ρ^m_1 8r_0(^{Mz}_{1.2} )^{5/6} √ ξ d_L(z) ) δ ( Θ_2 Θ1 − ρ^m_2 ρ^m_1 ) δ ( Θ_3 Θ1 − ρ^m_3 ρ^m_1 ) , (5)

Table 1: Physical parameters and observed quantities of four sources. For first three of them (A, B, C) sky position and orientation were chosen randomly from uniform distributions on ththe obtained signal to noise ratio (the binary is optimally oriented).

Physical parameters Observed quantities M_1= M_2 [M_⊙] z ϑ [rad] ϕ [rad] Ψ [rad] i [rad] M_z [M_⊙] ρ^m_1 ρ^m_2 ρ^m_3 A 1.4 0.1 0.53 π 0.82 π 1.30 π 0.70 π 1.34 44.04 94.42 55.95 B 0.5 0.71 π 0.18 π 1.38 π 0.08 π 1.83 41.46 42.42 45.35 C 1.0 0.34 π 1.61 π 0.64 π 0.66 π 2.44 9.99 10.57 12.69 D 1.0 0 π π 0 2.44 36.90 36.90 36.90

For illustration we present four cases of binary neutron stars simulated ET observations. The physical parameters of those sources, as well as the observed quantities are shown in Table 1. The results are shown in Fig. 1. It can be clearly seen that our method can constrain distances to with the accuracy of about 20%.

4 Summary

Distance measurements to merging binaries will be very challenging in the third generation detectors era. So far, there are no plans for any other detector than Einstein Telescope. In this paper, we presented a method that can be used to constrain distance distribution for a given double neutron star observation. We have shown that it is possible to significantly improve distance estimates using the measurements of the signal to noise ratio from all three interferometers .

Acknowledgments

This work was supported by the following Polish NCN grants DEC-2011/01/V/ST9/03171 and 2014/15/Z/ST9/00038.

References

1. M. Punturo et al., Class. Quantum Grav 27, 19 (2010). 2. S. Fairhurst, New J. Phys. 11, 123006 (2009) 3. S. R. Taylor et al., Phys. Rev. D 85, 023536 (2012) 4. S. Taylor and J. R. Gair, Phys. Rev. D 86, 023502 (2012)

Figure 1: Normalized redshift distributions for four NSNS system listed in Table 1. Dashed line represent distribution obtained using only one interferometer, while solid line represent distribution taking into account information from all three interferometers.The arrows indicate the position of the source.