arXiv:1601.06946v1 [physics.plasm-ph] 26 Jan 2016

A compact tunable polarized X-ray source based on laser-plasma helical undulators

Authors:

J. Luo^{1,2}, M. Chen^{1,2∗}, M. Zeng^{1,2}, J. Vieira^3, L.L. Yu^{1,2}, S.M. Weng^{1,2}, L.O. Silva^3, D.A. Jaroszynski^4, Z.M. Sheng^{1,2,4†}, and J. Zhang^{1,2}

Affiliations:

1Key Laboratory for Laser Plasmas (Ministry of Education) and Department of Physics and Astronomy, Shanghai Jiao Tong University, Shanghai, 200240, China.

2Collaborative Innovation Center of IFSA (CICIFSA), Shanghai Jiao Tong University, Shanghai 200240, China.

3GoLP/Instituto de Plasmas e Fusao Nuclear, Instituto Superior Tecnico, Universidade de Lisboa, Lisbon 1049-001, Portugal.

4SUPA, Department of Physics, University of Strathclyde, Glasgow G4 0NG, UK._∗ e-mail: minchen@sjtu.edu.cn †e-mail: zhengming.sheng@strath.ac.uk

Abstract:

Laser wakefield accelerators have great potential as the basis for next generation compact radiation sources because their accelerating gradients are three orders of magnitude larger than traditional accelerators. However, X-ray radiation from such devices still lacks of tunability, especially the intensity and polarization distribution. Here we propose a tunable polarized radiation source from a helical plasma undulator based on plasma channel guided wakefield accelerator. When a laser pulse is initially incident with a skew angle relative to the channel axis, the laser and accelerated electrons experience collective spiral motions, which leads to elliptically polarized synchrotronlike radiation with flexible tunability on radiation intensity, spectra and polarization. We demonstrate that a radiation source with millimeter size and peak brilliance of 2 × 10^{19}photons/s/mm^2/mrad^2/0.1% bandwidth can be made with moderate laser and electron beam parameters. This brilliance is comparable with the third generation of synchrotron radiation facilities running at similar photon energies, suggesting that laser plasma based radiation sources are promising for advanced applications.

Tunable x-ray synchrotron radiation sources have wide applications in natural sciences, medicine and industry [1, 2]. X-rays for such applications are mostly generated from synchrotron radiation facilities, which are usually bulky, costly and not able to satisfy the increasing demand of researchers [3]. Compact, tunable and flexible light sources are ideal for a broad range of applications and many schemes for such sources are under investigation [4, 5]. Among these the laser wakefield accelerator (LWFA) scheme is highly promising due to its tremendous accelerating gradient [6–8]. Electrons can be longitudinally accelerated to GeV energy over centimeters [9]. Besides longitudinal acceleration, electrons also undergo transverse betatron oscillations in wakefields which lead to the emission of electromagnetic radiation in the x-ray range [10–12]. Applications of these radiation sources such as object imaging with high resolution have already been tested [13–15]. Further applications may become possible if some key properties of these radiation sources, including brightness, spectral features and polarization, can be controlled. Among these the polarization is relatively more difficult to control as it relies on the polarization of electron betatron motion. However, it is usually transversely isotropic. Although the polarization can be controlled through electron injection selection or driver pulse tilting techniques [16, 17], the polarization tunability is still not sufficient. Coupling the LWFA with external magnetic undulators would produce tunable radiation. However, both the operation difficulty and the device size increase. External undulators and beam transport systems would enlarge the size of the devices from centimetres to several meters [18].

Making a more compact radiation source with both small acceleration and radiation lengths is challenging. In order to reach this goal, many kinds of plasma based undulators with small period length have been suggested as possible candidates to replace conventional magnetic undulators [19–25]. Here, we provide a pathway that may strongly advance compact plasma based undulator technology, by proposing a compact plasma based helical undulator to generate tunable polarized x-ray radiation, thus paving the way to controlled x-ray generation. Through three dimensional particle-in-cell (3D-PIC) simulations we show that the motion of the laser inside the plasma channel depends on the initial incidence offset and angle between the laser and channel axis. We find conditions where the laser spirals about the channel axis, thereby leading to helical betatron trajectories of accelerated electrons. A post radiation calculation code was then used to study the elliptically shaped hollow x-ray emission in far field. Besides the intensity distribution, we find that the polarization and spectra of the radiation are easily controllable by changing the incidence angle of the driver pulse and channel profiles. Considering typical laser and plasma parameters, currently available in many laboratories, we find that our centimeter scale, plasmabased radiation source is expected to deliver ultra-intense x-rays, with peak brilliance as large as 2 × 10^{19}photons/s/mm^2/mrad^2/0.1% bandwidth. Such high quality flexible and compact radiation source has the potential to impact a wide variety of applications.

Laser and electron beam spiral motions inside the plasma channel

We first study the electron motion inside the plasma channel which resembles that in a helical undulator. Stable laser wakefield accelerators usually use plasma channels to guide the laser pulse over many Rayleigh lengths (i.e. Z_R = k_0w^2_0/2, where k_0 = 2π/λ_0 is the laser wave number in vacuum, w_0 is the focal spot size and λ_0 is the laser wavelength). A plasma channel with a transverse parabolic density profile of n(r) = n_0 + Δnr^2/r^2_0 can guide the laser for long distances, where r represents the transverse coordinate, n_0 is the on-axis electron density, Δn is the channel depth and r_0 is the channel width [7, 22, 23]. For a matched plasma channel (i.e., Δn = Δn_c = (πr_er^2_0)^{−1} and r_0 = w_0, where r_e = e^2/m_ec^2 is the classical electron radius with e and m_e the electron charge and mass at rest, respectively, and c the light speed in vacuum), the laser spot size remains approximately constant during all propagation. If a laser pulse is initially off-axially injected into the plasma channel or at some injection angle, the laser centroid will oscillate transversely in a single plane as it propagates forward [22]. The oscillation period length, given by Λ_{os} = 2πZ_M (Δn_c/Δn)^{1/2}, where Z_M = πr^2_0/λ_0, can be controlled by tuning the channel depth [22]. In addition, when the laser wave number vector is non-collinear with the channel axis, the laser centroid will perform a spiral trajectory around the channel axis as shown in Fig. 1(a). The centroid trajectory of the laser pulse can be simply approximated from the eikonal equations according to the ray tracing method [26] (details can be found in Supplementary Information). In cylindrical coordinates (r, ϕ, z), the laser centroid trajectory is then given by dr dz = ± 1 cosθ_z [1 − n(r) n_c − (1 − n_{e0} n_c ) · (sin^2θ_z b^2 r^2

+ cos^2θ_z)]^{1/2} (1) dϕ dz = bsinθ_z r^2cosθ_z (2) with θ_z = arccos( √ 1 − cos^2θ_x − cos^2θ_y), and where θ_{x, y, z} are the angles between the laser propagation direction and the space coordinate axes x, y, and z. Moreover, n_c is the critical density of plasma, n_{e0} = n_e(r = √ x^2_0 + y^2_0 ) is the plasma density at the laser incidence point (x_0, y_0). The parameter b = (y_0 −x_0cosθ_y/cosθ_x)/( √ (cosθ_y/cosθ_x)^2 + 1) is called striking distance, i.e. the distance between the projection of the incident laser pulse and the plasma channel centre.

When an ultrashort ultraintense laser pulse propagates in such a plasma channel, the background electrons are expelled outward due to the pondermotive force of the driver pulse, generating bubble like wakefields at the back of the laser pulse [27, 28]. If the laser pulse oscillates transversely, the bubble will follow the laser, forcing electrons inside the bubble to follow the motion of the laser centroid [20]. The oscillation period and amplitude can be kept constant until near the laser pump depletion [22]. Thus the plasma may act as a helical undulator and the radiation of the electrons shows typical helical undulator radiation properties, which are dramatically different from those of normal betatron radiation.

We used the massively parallel, fully-relativistic PIC code OSIRIS [29] to investigate the self-consistent three-dimensional dynamics of the laser centroid motion and electron acceleration inside the plasma channel when the laser wave vector is not aligned with the channel axis in the strongly nonlinear blowout regime. Detailed simulation parameters can be found in the Methods. The channel axis is set along the z axis (x = y = 0). In a typical simulation shown in Fig. 1, the initial parameters of laser incidence are x_0 = 1 μm, y_0 = 0, θ_x = 89^∘ and θ_y = 91^∘. Typical bubble cross sections at different laser propagation distances are plotted in Fig. 1(b) to 1(e). Figure 2(a) shows a typical snapshot of the three-dimensional structure of the laser driven blowout region (yellow), with the externally injected electrons at the back of the bubble (light green), and the laser electric fields (blue-red-orange-dark green). Projections of the laser propagation direction on x-y and x-z planes (black dashed arrows) in Fig. 2(a) and a movie of the laser and wake evolution (refer to the Supplementary Information) indicate the spiral motion. The black solid lines in Fig. 2(b) show typical trajectories of the laser centroid obtained from theoretical approximations by solving Eqs. (1) and (2). The red solid lines represent the trajectories from 3D-PIC simulations. The dashed lines on the side planes are the corresponding trajectory projections. The analytical model correctly predicts the wavelength and amplitude of the laser centroid oscillations, both in excellent agreement with PIC simulations. These results show that the eikonal equations can be used to describe the laser propagation for the typical propagation distances in our investigation. The oscillation wavelength from the PIC simulation is about 700 μm closed to the theoretical approximation Λ_{os} = 719.5 μm. In the simulations, because of the laser energy depletion and frequency red shifting as the laser pulse propagates further, the oscillation wavelength and amplitude become smaller than theoretical predictions.

To reduce simulation time and concentrate on the study of the properties of the radiation emitted by the trapped electrons, we consider an external injected scenario, employing a cylindrical electron beam to study the radiation dependance on the intial laser incidence. An illustration of a simulation including ionization injection is given in the Supplementary Information, in order to illustrate the feasibility of our scheme in an all optical setup by only using LWFA. As mentioned before, the trapped and accelerated electron beam experiences spiral motion simutaneously with the acceleration structure following the laser pulse inside the plasma channel. We randomly traced 200 particles from the accelerated electron beam. The centroid position of these electrons (x_c, y_c, z_c) are shown in Fig. 2(b) by the blue solid line. The Root-Mean-Square radius of these electrons (r_{rms} = √ < (x_i − x_c)^2 + (y_i − y_c)^2 >) is less than 0.63 μm during the whole simulation process. As one can see from Fig. 2(b), the period of the spiral motion of the electrons closely follows the period of the laser centroid oscillations. In addition, the amplitude of the oscillations is slightly higher than the laser centroid oscillations, due to its inertia. Electrons are accelerated to nearly 140 MeV in only 1600 μm. The rms deviation of the average energy increases to about 8 MeV, which results from the nonumiformity of the longitudinal acceleration fields in the helically moving bubble. The continous acceleration of electrons with a stable accelerating gradient about 80 GeV/m before x = 1600 μm illustrates that electrons propagate near the back of the bubble. After x > 1600 μm, the accelerating gradient reduces rapidly as electrons enter the dephasing region. So the following calculation of electrons trajectories and radiation stops at x = 1600 μm, which corresponds to using a short capillary in practice.

X-ray radiation from the helical plasma undulator

The spiral motion of the trapped electrons inside the wakefield resembles the electron motion in a traditional helical undulator, which is common in a storage ring of a synchrotron facility for polarized x-ray emission [30]. We studied the radiation properties of these electrons with the numerical radiation post-processing code VDSR [31] (see Methods). This code calculates the radiation distribution according to electrons trajectories obtained from the 3D-PIC OSIRIS simulations. At the beginning of the electron acceleration the normal beam betatron period of the electrons inside the accelerating bubble (λ_β ≈ √ 2γλ_p) is far smaller than the laser oscillation period (Λ_{os}), the radiation properties are more relied on the betatron motion and the emitted photons are low energies which are not the ones we are interested in. In the radiation calculations we cut out these low energy radiation part. Figure 3(a) shows the radiation intensity distribution captured by a virtual radiation detector located in the far-field and centred along the plasma channel axis (see schematic view in Fig. 1(a)). The initial injection parameters of the laser are the same as those in Fig. 1. The far field radiation pattern illustrated in Fig. 3(a) shows a hollow elliptical shape, which is consistent with the electron trajectories whose projection on x-y plane is shown in Fig. 2(b). Key properties of the radiation intensity distribution are described by a fundamental dimensionless radiation parameter, called the strength parameter, given by K = 2πγr_{os}/Λ_{os}, where γ is the Lorentz factor of the electrons, r_{os} is their transverse oscillation amplitude and Λ_{os} is the spiral motion period. In this case the electrons are rapidly accelerated to high energies (γ ≈ 274). Moreover, the minimum oscillation amplitude is (r_{os})_{min} ≈ 1.41 μm, the maximum oscillation amplitude is (r_{os})_{max} ≈ 6.84 μm, and Λ_{os} ≈ 700 μm. These parameters leads to a minimum strength parameter K_{min} ≈ 3.5 and a maximum strength parameter K_{max} ≈ 16.8. Both K_{min} and K_{max} are larger than unity, which means the radiation is in the wiggler regime. As a result, the radiation spectrum is broadband. The x-rays propagate along the emission angles θ ∼ K/γ ≈ 0.73^∘ and 3.51^∘. These angles are larger than the angular width around the emission angle Δ ∼ 1/γ ≈ 0.21^∘, therefore leading to the hollow intensity pattern shown in Fig. 3(a).

To investigate the spectral properties, we have selected two points with the highest radiation intensities and marked them with black circles. As one can see, the maximum radiation intensity comes from the major axis vertices of the radiation ellipse with radiation angle about θ ≈ 3.5^∘, which corresponds to the positions in the electron trajectory projection plane where the electrons have maximum deviation (r_{os} ≈ (r_{os})_{max}) and experience the maximum transverse acceleration. The photon energy spectra of the marked points are shown in Figs. 3(c) and 3(d). The peak position of the spectrum radiated along this direction is about 400 eV which is about the average value of the on-axis radiation where the peak radiation energy is E_p =^3_2 Kγ^2hc/Λ_{os} = 3πγ^3r_{os}hc/Λ^2_{os} with h representing the Plancks constant. [10] For average electron energy (γ̄ = 137) it is E_p = 418.9eV .

In order to discuss the polarization properties of the radiated photons, we define the polarization direction degree of a point as P = I_x/I_t, where I_x is the radiation intensity with photon polarization in the x direction and I_t is the total radiation intensity. When P = 1 the radiation is linearly polarized in the x direction, while when P = 0 the radiation is linearly polarized in the y direction. The polarization direction degree distribution is shown in Fig. 3(b). The two points marked in Fig. 3(a) were also lined out. During the spiral motion, the directions of the electrons’ transverse velocities keep changing, and so does the radiation polarization direction. Because of the positive correlation between radiation polarization and electrons velocity direction, the polarization direction degree appears to change periodically along the elliptical orbit. When electrons move to the upper right marked position, its velocity gradient component in the x direction is lower than that in the y direction, so P < 0.5 and the radiation intensity in the x direction (corresponding to red line in Fig. 3(c)) is weaker than that in the y direction (blue line in Fig. 3(c)). The opposite situation at the lower left marked position is shown in Fig. 3(d).

In addition to the polarization, the radiation intensity is also another important parameter for useful photon sources. The radiation intensity is proportional to the total number of electrons in the beam for incoherent radiation emission. In our typical 3D-PIC simulations, due to the limitation of computational resources, small laser focal spot sizes and injected electron beam radii have been used. The externally injected electron beam charge used in the simulation is thus 4.5 pC, which is close to the ionization induced injection charge measured in the simulation reported in the Supplementary Information. With this charge, the totally number of radiated photons is about 2 × 10^7. A much larger photon number would be radiated if the total number of trapped electrons could be higher. In general, higher charges can be accelerated when using higher energy drivers propagating in lower density plasma in comparison to those considered in our work. Higher accelerated beam charge could also be obtained in ionization injection scenarios by increasing the concentration of the injection gas component. Considering the electron rotation transverse area 15.1 μm^2 and the bunch duration 6.67 fs, in our case the final maximum radiation brightness is about 2×10^{19}photons/s/mm^2/mrad^2/0.1% bandwidth, which is comparable with the highest levels of current third generation of synchrotron radiation facilities at similar x-ray energies.

In our scheme the intensity and polarization distributions of the radiation can be easily controlled by varying the initial laser incidence parameters, i.e. the initial off-axis position (x_0, y_0) and the tilted injection angles (θ_x, θ_y). In Fig. 4(a) the laser centroid trajectories with different initial parameters are shown. The black line corresponds to the one shown in Fig. 2. The radiation shows hollow elliptical shape. An additional simulation was also performed in order to obtain a hollow and circular intensity profile by using laser injection parameters of x_0 = 2.92 μm, y_0 = 0, and θ_x = 90^∘, θ_y = 91.5^∘. The laser performs circular rotation around the channel axis initially. Near laser pump depletion, however, radius of rotation decreases as shown by the red line in Fig. 4(a). Because the emission angle is larger than the angular width of the radiation, the radiation intensity distribution also exhibits a hollow circle pattern, illustrated in Fig. 4(b). The corresponding radiation polarization distribution is shown in Fig. 4(c). As one can see the polarization is strongly angle dependent and it is along the azimuthal direction. This kind of distribution is very convenient for many light-polarization-dependent applications.

Quasi linearly polarized x-rays can also be generated by selecting appropriate initial laser incidence. If one fixes the initial incidence position (x_0 = 1 μm, y_0 = 0), and incidence angle θ_y = 91^∘, but only decreases θ_x from 89^∘ to 88^∘, the ellipticity decrease of the laser centroid trajectory is evident from the blue line in Fig. 4(a). Correspondingly the electron radiation intensity distribution shows a linear structure (shown in Fig. 4(e)) and a bigger radiation polarization degree P is obtained (see Fig. 4(f)), which means that most of the radiated photons are linearly polarized. Furthermore, in this simulation the oscillation amplitude of the electrons has been increased as one can see in Fig. 4(a). The strength parameter (K) is then increased as well. We find that with these parameters the final peak photon energy moves to 1.5 keV, which shows the tunability of radiation energy. Another way to tune the radiation energy is by varying the channel depth since the strength parameter (K) depends on the laser oscillation period (Λ_{os}) in the parabolic plasma channel. The effects of the channel depth on the radiation parameters has already been studied in detail in Refs. 22 and 23.

In general, fine tunability of the distribution of the radiation intensity and polarization can be obtained by controlling the combinations of the initial laser incidence parameters. Here we only show the tunability of the elliptical azimuth angle of the radiation pattern by controlling the combined parameter of cos(θ_x)/cos(θ_y) with fixed incidence position (x_0, y_0). The results are shown in Fig. 4(d). The radiation tilt angle can be tuned from 20 to 70 degrees freely. Because of the coincidence of the electron motion and the laser centroid motion, in practice, one can design the radiation properties by solving the eikonal equations of the laser motion first.

Conclusion

In conclusion, we have studied highly tunable soft x-ray radiation from a helical plasma undulator based on LWFA in a plasma channel. When the initial laser pulse propagation axis is in an arbitrary skew angle relative to the channel axis, theoretical and simulation results illustrate that both the laser pulse and electron beams carry out spiral motion. The plasma acts as a helical undulator modulating electron motion, such that elliptically polarized synchrotron-like radiation can be produced. The distributions of the radiation intensity, polarization and spectrum can all be tuned by controlling the initial laser incidence parameters and the profile of the plasma channel. In general x-ray radiations with hollow elliptical shape and elliptical polarization with brightness comparable to or even higher than the third generation of synchrotron radiation sources can be obtained from these laser plasma based helical undulators. Our studies reveal that such all optical-plasma compact radiation sources can be made highly flexible and are therefore suitable for advanced applications. It deserves to point out that although currently there are still many factors such as average photon flux, spectrum width, stability, making wakefield based radiation sources uncompetitive with traditional SRs, the uniqueness of such sources ( for example brightness, compactness and synchronization with high power laser) make them beneficial complements of SRs. In further, the recent progresses on wakefield acceleration (i.e. electron injection [32], wake diagnosis [33] and high repetition lasers [34]) have shown the potential to make more stable, high quality and high flux radiation sources.

Methods

3D-PIC simulations were performed with OSIRIS code. In the simulations, the profile of the normalized laser vector potential is given by a = eA/m_ec^2 = a_0 × exp(−t^2/L^2_0 − r^2/w^2_0 ) with a_0 = 2.0 (corresponding to the peak intensity of the polarized laser pulse of I = 8.6 × 10^{18} W/cm^2), L_0 = 4.0 T_0, w_0 = 6.75 λ_0 and the laser wavelength λ_0 = 0.8 μm, the laser period T_0 = 2π/ω_0 ≈ 2.67 fs. The plasma density has a parabolic profile with n_0 = 0.001 n_c, Δn = Δn_c, r_0 = w_0, where n_c ≈ 1.7 × 10^{21} cm^{−3} is the critical plasma density for the driver pulse. The injected external electron beam has transverse and longitudinal dimensions with size of L_r = 0.5 μm, L_z = 2.0 μm, and a charge of Q ≈ 4.5 pC. The energy of the beam is E_e = 7.7 MeV or 5.1 MeV in different simulation cases. The size of the simulation box is 40×40×45 μm^3 corresponding to cell size of 200×200×1035. We use 4 super-particles per cell and 8 super-particles per cell for the background electrons and external injected electrons, respectively.

Post process code VDSR was used to perform the radiation calculation. The spatial and velocity vectors of 200 super-particles randomly selected from the accelerated electron beam in 3D-PIC simulations were input into the VDSR code. The time internal of trajectory recording is dt = 0.04 T_0. The code integrates each particle’s radiation along its trajectory. Since the electron beam size is much longer compared with the radiation wavelength interested here, the radiation is essentially incoherent. Because of the computational source limitation, the number of the traced particle is too small for a coherent addition of the electron radiation, we then sum them incoherently to get the final far field spectra on a virtual screen with spatial resolutions. The detected circular region covers a maximum polar angle of 6^∘, which is divided into 24 parts in the radial direction and 72 parts in the azimuthal direction.

References

[1] Huxley, H. E. et al. The use of synchrotron radiation in time-resolved X-ray diffraction studies of myosin layer-line reflections during muscle contraction. Nature 284, 140-143 (1980).

[2] Chen, L., Drr, K. L. & Gouaux, E. X-ray structures of AMPA receptorcone snail toxin complexes illuminate activation mechanism. Science 345, 1021-1026 (2014).

[3] Bilderback, D. H., Elleaume, P. & Weckert, E. Review of third and next generation synchrotron light sources. J. Phys. B At. Mol. Opt. Phys. 38, S773-S797 (2005).

[4] Wong, L. J. et al. Towards grapheme plasmon-based free-electron infrared to X-ray sources. Nature Photon. 10, 46-52 (2016).

[5] Phuoc, K. T. et al. Laser based synchrotron radiation. Phys. Plasmas 12, 023101 (2005).

[6] Tajima, T. & Dawson, J. M. Laser Electron Accelerator. Phys. Rev.

Lett. 43, 267-270 (1979).

[7] Esarey, E., Schroeder, C. B. & Leemans, W. P. Physics of laser-driven plasma-based electron accelerators. Rev. Mod. Phys. 81, 1229-1285 (2009).

[8] Hooker, S. M. Developments in laser-driven plasma accelerators. Nature Photon. 7, 775-782 (2013).

[9] Leemans, W. P. et al. Multi-GeV electron beams from capillarydischarge-guided subpetawatt laser pulses in the self-trapping regime. Phys. Rev. Lett. 113, 245002 (2014).

[10] Corde, S. et al. Femtosecond x rays from laser-plasma accelerators. Rev.

Mod. Phys. 85, 1-48 (2013).

[11] Rousse, A. et al. Production of a keV x-ray beam from synchrotron radiation in relativistic laser-plasma interaction. Phys. Rev. Lett. 93, 135005 (2004).

[12] Cipiccia, S. et al. Gamma-rays from harmonically resonant betatron oscillations in a plasma wake. Nature Phys. 7, 867-871 (2011).

[13] Fourmaux, S. et al. Single shot phase contrast imaging using laserproduced Betatron x-ray beams. Opt. Lett. 36, 2426-2428 (2011).

[14] Kneip, S. et al. X-ray phase contrast imaging of biological specimens with femtosecond pulses of betatron radiation from a compact laser plasma wakefield accelerator. Appl. Phys. Lett. 99, 093701 (2011).

[15] Wenz, J. et al. Quantitative X-ray phase-contrast microtomography from a compact laser-driven betatron source. Nature Commun. 6, 7568 (2015).

[16] Schnell, M. et al. Optical control of hard X-ray polarization by electron injection in a laser wakefield accelerator. Nature Commun. 4, 2421 (2013).

[17] Popp, A. et al. All-optical steering of laser-wakefield-accelerated electron beams. Phys. Rev. Lett. 105, 215001 (2010).

[18] Schlenvoigt, H.-P. et al. A compact synchrotron radiation source driven by a laser-plasma wakefield accelerator. Nature Phys. 4, 130 (2008).

[19] Joshi, C. et al. Plasma wave wigglers for free-electron lasers. IEEE J.

Quantum Electron. 23, 1571-1577 (1987).

[20] Reitsma, A. & Jaroszynski, D. Propagation of a short intense laser pulse in a curve plasma channel. IEEE Trans. Plasma Sci. 36, 1738- 1745 (2008).

[21] Andriyash, I. A. et al. An ultracompact X-ray source based on a laserplasma undulator. Nature. Commun. 5, 4736 (2014).

[22] Chen, M. et al. Tunable synchrotron-like radiation from centimetre scale plasma channels. Light Sci. Appl. 5, e16015 (2016).

[23] Rykovanov, S. G. et al. Plasma undulator based on laser excitation of wakefields in a plasma channel. Phys. Rev. Lett. 114, 145003 (2015).

[24] Vieira, J. et al. Plasma based helical undulator for controlled emission of circularly and elliptically polarised betatron radiation. arXiv:1601.04422v1 (2016).

[25] Hooker, S. M., Gonsalves, A. J., Jaroszynski, D. A. & Leemans, W.

P. Charged particle accelerator and radiation source. U.S. Patent No. 8299713, Oct. 30, 2012.

[26] Born, M. & Wolf, E. Principles of Optics (Oxford Dergamon Press, 1975).

[27] Pukhov, A. and Meyer-ter-Vehn, J. Laser wake field acceleration: the highly non-linear broken-wave regime. Appl. Phys. B 74, 355-361 (2002).

[28] Lu, W. et al. Generating multi-GeV electron bunches using single stage laser wakefield acceleration in a 3D nonlinear regime. Phys. Rev. ST Accel. Beams 10, 061301 (2007).

[29] Fonseca, R. A. et al. OSIRIS: A three-dimensional fully relativistic particle in cell code for modeling plasma based accelerators. Lect. Notes Comp. Sci. 2331, 342-351 (2002).

[30] Wang, C.-X., Schlueter, R. Optimization of circularly-polarized radiation from an elliptical wiggler, asymmetric wiggler, or bending magnet. Nucl. Instr. Meth. In Phys. Rev. A 347, 92-97 (1994).

[31] Chen, M. et al. Modeling classical and quantum radiation from laserplasma accelerators. Phys. Rev. ST Accel. Beams 16, 030701 (2013).

[32] Zeng, M. et al. Multichromatic Narrow-Energy-Spread Electron Bunches from Laser-Wakefield Acceleration with Dual-Color Lasers. Phys. Rev. Lett. 114, 084801 (2015).

[33] Matlis, N. H. et al. Snapshots of laser wakefields. Nature Phys. 2, 749- 753 (2006).

[34] Mourou, G. et al. The future is fibre accelerators. Nature Photon. 4, 258-261 (2013).

Author contributions

M.C. conceived the idea; J.L., M.C. and M.Z. performed the PIC simulations and radiation calculations; J.L., M.C., Z.M.S., J.V. analyzed data; J.L., M.C., Z.M.S. and J.Z. wrote the main manuscript. J.V., L.L.Y., S.M.W., L.O.S. and D.A.J. improved the manuscript. All authors commented on the manuscript and agreed on the contents.

Competing financial interests

The authors declare no competing financial interests.

Acknowledgements

This work is supported in part by the National Basic Research Program of China (2013CBA01504), the National Science Foundation of China (11421064, 11374209, 11374210), a MOST international collaboration project (2014DFG02330), and an EU Horizon 2020 Programme project EuPRAXIA (Grant No. 653782).

M.C. appreciates supports from National 1000 Young Talent Program. Z.M.S. acknowledges the support of a Leverhulme Trust Research Grant. J.V. and L.O.S. acknowledge Laserlab III (Contract No. 284464) and Laserlab IV (Contract No. 654148). D.A.J. acknowledges support of the U.K. EPSRC (Grant No. EP/J018171/1), the EC’s LASERLAB-EUROPE (Grant No. 654148), EuCARD-2 (Grant No. 312453). The authors would like to acknowledge the OSIRIS Consortium for the use of OSIRIS and the visXD framework. Simulations were performed on the Π supercomputer at Shanghai Jiao Tong University and Tianhe II supercomputer at Guangzhou.

Figures

Fig. 1 Sketch of the radiation source from a helical plasma undulator based on LWFA. (a) Spiral motion of laser pulse, wakefield in the plasma channel and the far field x-ray radiation distribution. (b, c, d, e) are the electron density distributions of the transverse slices of the accelerating bubble structure with largest radius at t = 133 fs (b), t = 600 fs (c), t = 1200 fs (d), t = 1800 fs (e).

Fig. 2 Spiral motions of the laser pulse and electron beam in the plasma channel. (a) A snapshot of plasma density (blue background), bubble structure (yellow surface), injected electron beam (light green points), and laser electric fields (blue-red-orange-green iso-surfaces and the projections). The arrows show the laser propagation direction in projection planes. (b) Theoretical (black solid line) and simulation (red solid line) results of the laser pulse centroid trajectory. The blue solid line shows the centroid trajectory of the traced particles. Dashed lines are the projections of the trajectories.

Fig. 3 Intensity and polarization distributions of x-ray radiation. (a) Far field radiation intensity distribution, (b) polarization distribution, (c) radiation spectrum of the marked upper right point and lower left point (d).

Fig. 4 Radiation distributions of intensity and polarization for different laser incidence parameters. (a) Laser centroid trajectories on x-y plane with initial laser incidence parameters of x_0 = 1 μm, θ_x = 89^∘, θ_y = 91^∘ (black), x_0 = 2.92 μm, θ_x = 90^∘, θ_y = 91.5^∘ (red), and x_0 = 1 μm, θ_x = 88^∘, θ_y = 91^∘. Input parameter y_0 is fixed to be 0 μm. The circles and triangles mark the start and end positions of these trajectories, respectively. (b, e) are radiation intensity distributions and (c, f) are radiation polarization distributions. (b, c) correspond to the red line in (a), (e, f) correspond to blue line in (a). (d) The correlation between the azimuth angle of the elliptical radiation region and the ratio of the cosine function of incidence parameters θ_x and θ_y.