arXiv:1707.02500v1 [physics.class-ph] 8 Jul 2017

The 0 to R_1 cylinder radial coordinate transformation can not be used to make cylinder layer electromagnetic cloak

Jianhua Li^∗ and Feng Xie, Lee Xie, Ganquan Xie GL Geophysical Laboratory, USA

Jianhua Li and Ganquan Xie Chinese Dayuling Supercomputational Sciences Center, China Hunan Super Computational Sciences Society, China (Dated: June 8, 2017)

In this paper, we discover and proved that the 0 to R1 cylinder radial coordinate transformation can not be used to make cylinder layer electromagnetic EM cloak. Patent of discover,create method and proof in this paper are reserved by authors in GL Geophysical Laboratory.

PACS numbers: 13.40.-f, 41.20.-q, 41.20.jb,42.25.Bs

I. INTRODUCTION

First in the world, in this paper, we discover and prove that the 0 to R_1 cylinder radial ρ transformation method can not be used for making cylinder layer EM cloak. Because in the 0 to R_1 cylinder radial coordinate transformation, the value area of the electric wave field E_z(ρ, ϕ, z) and magnetic wave field H_z(ρ, ϕ, z) are invariant. After 0 to R_1 cylinder radial transformation,ρ_q = R_1 + Q(ρ), E_z (ρ_q, ϕ, z) = E_z (ρ, ϕ, z),H_z(ρ_q , ϕ, z) = H_z(ρ, ϕ, z) . in the physical inner cylinder boundary , E_z (R_1, ϕ, z) ≠ 0 ,H_z(R_1, ϕ, z) ≠ 0 , The cylinder EM wave field will propagation penetrate into the inner cylinder ρ < R_1, |z| < ∞ .Therefore, the inner cylinder ρ < R_1, |z| < ∞ . can not be cloaked. In many published papers on EM cylinder cloak, the 0 to R_1 cylinder radial transformation is wrongfully used for their EM cylinder layer cloak.

The description of this paper are as follows. Maxwell EM equation in the cylinder coordinate in free space is presented in section 2. 0 to R_1 cylinder radial coordinate transformation can not be used to make EM cloak is proposed in section. 3. Discussion and conclusion is presented in section 4.

II. MAXWELL EM EQUATION IN THE CYLINDER COORDINATE IN FREE SPACE

In this section, let the H_z(ρ, ϕ, z) be magnetic field component in Z direction. We describe magnetic field equation in the cylinder coordinate free space. ∂ ∂ρ ρ^{∂Hz}_{∂ρ} +^{∂2 Hz}_{ρ∂ϕ2} +ρ^{∂2}_{∂z2} H_z + k^2ρH_z = M_s, (1)

∗Also at GL Geophysical Laboratory, USA, glhua@glgeo.com

where ρ is radial coordinate, ϕ is angular coordinate, H_z(ρ, ϕ, z) is the magnetic wave field. k = ω √ εμ is the constant EM wave number in free space , ω is the angular frequency. ε is the basic electric permittivity in free space, μ is the basic magnetic permeability in free space. The magnetic source M_s is induced by the point Delta electric source in ⃗e_x = (1, 0, 0) direction, S(⃗r, ⃗r_s) = δ(ρ − ρ_s)δ(ϕ − ϕ_s)δ(z − z_s)⃗e_x, (2) The incident magnetic wave field H_{z,i}(ρ, ϕ, z) does satisfy the Maxwell magnetic equation (1) in free space, H_{z,i}(ρ, ϕ, z) = − sin ϕ^∂_{∂ρ} g(ρ, ϕ, z) − cos ϕ^1_ρ^∂_{∂ϕ} g(ρ, ϕ, z), (3)

g(ρ, ϕ, z) = − 1 4π e^{ikb} √_{|ρ−ρs |2+(z−zs)2} √ |ρ − ρ_s|^2 + (z − z_s)^2

, (4)

√ |ρ − ρ_s|^2 + (z − z_s)^2 = √ ρ^2 − 2ρρ_s(cos ϕ − ϕ_s) + ρ^2_s + (z − z_s)^2, (5)

H_{z,i} (ρ, ϕ, z) =^1_{4π}^{eik} √_{|ρ−ρs |2+(z−zs)2} (√_{|ρ−ρs |2+(z−zs)2})_2 ( ik −^1 √_{|ρ−ρs |2+(z−zs)2} ) (ρ sin(ϕ) − ρ_s sin(ϕ_s)), (6)

III. 0 TO R1 CYLINDER RADIAL COORDINATE TRANSFORMATION CAN NOT BE USED TO MAKE EM CLOAK

A. Homogeneous magnetic wave equation in the cylinder ρ ≤ R2 and |z| < ∞

For R_2¿ 0 and ρ_s > R_2, in the cylinder ρ ≤ R_2 and |z| < ∞, the homogeneous magnetic wave equation is ∂ ∂ρ ρ^{∂Hz}_{∂ρ} +^{∂2 Hz}_{ρ∂ϕ2} +ρ^{∂2}_{∂z2} H_z + k^2ρH_z = 0, (7) On the cylinder surface boundary ρ = R_2, the magnetic wave field H_z = H_z (ρ, ϕ, z) and its derivative satisfy the continuous boundary conditions

H_z(R^−_2 , ϕ, z) = H_z (R^+_2 , ϕ, z), (8) ∂ ∂ρ H_z(R^−_2 , ϕ, z) = ∂ ∂ρ H_z(R^+_2 , ϕ, z), (9)

B. 0 to R1 cylinder radial coordinate transformation

For R_1 > 0, R_2 > R_1, inside of the cylinder ρ ≤ R_2, the 0 to R_1 cylinder radial continuous coordinate transformation is

ρ_q (r) = R_1 + Q(ρ), 0 ≤ ρ ≤ R_2, (10)

ρ_q(0) = R_1, Q(0) = 0, (11)

ρ_q(R_2) = R_2, Q(R_2) = R_2 − R_1, (12) ∂ ∂ρ ρ_q(R_2) = 1, ∂ ∂ρ Q(R_2) = 1, (13)

The inverse mapping is

ρ = Q^{−1} (ρ_q − R_1) , R_1 ≤ ρ ≤ R_2, (14)

C. Magnetic equation in the cylinder layer R1 ≤ ρ ≤ R2 To substitute 0 to R_1 cylinder radial coordinate transformation (10)-(14) into (7), the magnetic wave equation (7) in the free space cylinder ρ ≤ R_2 and |z| < ∞ is translated to the following anisotropic magnetic wave equation in the cylinder layer R_1 ≤ ρ ≤ R_2, ∂ ∂ρ_q ρ_q ε_ϕ ∂H_z ∂ρ_q + ∂^2 H_z ε_ρ ρ_q ∂ϕ^2

+ρ_qμ_z^{∂2}_{∂z2} H_z + k^2ρ_qμ_z H_z = 0,

(15)

Where the relative parameters induced by the 0 to R_1 cylinder radial transformation (10-14) are

ε_ρ = μ_ρ = ρ ρ_q dρ_q dρ , (16)

ε_ϕ = μ_ϕ = ρ_q ρ dρ dρ_q , (17)

ε_z = μ_z = ρ ρ_q dρ dρ_q , (18)

on the cylinder surface boundary ρ = R_2 the magnetic wave field solution H_z = H_z(ρ, ϕ, z),of equation(15) and its derivative satisfy the following continuous boundary conditions

H_z (R^−_2 , ϕ, z) = H_z(R^+_2 , ϕ, z), (19) 1 ε_ϕ ∂ ∂ρ_q H_z(R^−_2 , ϕ, z) = ∂ ∂ρ H_z (R^+_2 , ϕ, z), (20)

D. 0 to R1 cylinder radial coordinate transformation can not be used to make cylinder layer EM cloak

T heorem 1 : Suppose that the magnetic wave H_z(ρ_q , ϕ, z) does satisfy the magnetic equation (15) with relative anisotropic EM parameters (16-18), and satisfy the field and derivative boundary conditions (19) and (20) that is necessary for no scattering from the cylinder ρ ≤ R_2, |z| < ∞,then H_z (ρ_q , ϕ, z) has the analytic express as follows: H_z (ρ_q, ϕ, z) =^1_{4π}^{eik} √_{|Q−1 (ρq −R1)−ρs|2+(z−zs)2} (√_{|Q−1 (ρq −R1)−ρs |2 +(z−zs)2} )_2 ( ik −^1 √_{|Q−1 (ρq −R1 )−ρs|2+(z−zs)2} ) (Q^{−1} (ρ_q − R_1) sin(ϕ) − ρ_s sin(ϕ_s)),

(21)

Proof: Substitute the analytic magnetic wave field H_z (ρ_q , ϕ, z) in (21) into the equation (15), by inverse transformation, H_z (ρ_q , ϕ, z) is put back to H_z (ρ, ϕ, z) in (6) which is solution of (7). Therefore, H_z (ρ_q, ϕ, z) does satisfy the acoustic equation (15) and does satisfy the no scattering boundary condition (19) and (20), The theorem is proved. In next paper, we will use GLHUA analytical expand method to prove the theorem.

T heorem 2 : Suppose that the relative electric permittivity and magnetic permeability are induced by 0 to

R_1 cylinder radial transformation in (10)-(14),and incident wave is excited by outside electric point source in (2). The magnetic wave does satisfy the necessary no scattering boundary condition on the outer and inner boundary.The magnetic field H_z (ρ, ϕ, z) is propagation penetrate into the inner cylinder ρ ≤ R_1, |z| < ∞. The inner cylinder ρ ≤ R_1, |z| < ∞. can not be cloaked.

Proof: When the point is on the inner cylinder surface boundary ρ_q = R_1, and |z| < ∞. Substitute ρ_q = R_1 into (21), we have H_z (ρ_q , ϕ, z) |_{ρq =R1} = { 1 4π e^{ik} √_{|Q−1(ρq −R1)−ρs|2+(z−zs)2} (√_{|Q−1 (ρq −R1 )−ρs|2+(z−zs)2})_2 ( ik −^1 √_{|Q−1(ρq −R1)−ρs|2+(z−zs)2} ) (Q^{−1} (ρ_q − R_1) sin(ϕ) − ρ_s sin(ϕ_s)) } |_{ρq =R1}

= −^1_{4π} ρ_s sin(ϕ_s)^{eik} √_{|ρs|2 +(z−zs)2} (√_{|ρs|2+(z−zs)2})_2 ( ik −^1 √_{|ρs|2+(z−zs)2} )

(22)

1 ε_ϕ ∂ ∂ρ_q H_z (ρ_q, ϕ, z)|_{rq =R1} = 0. (23)

For simplicity and without confusion, we remove the subscript q in the inner cylinder, it is naturally, we design ε_ρ = μ_ρ = 1, ε_ϕ = μ_ϕ = 1, ε_z = μ_z = 1 in the inner cylinder ρ ≤ R_1 and |z| < ∞ . The magnetic wave H_z (ρ, ϕ, z) , in the inner cylinder does satisfy the following magnetic wave equation ∂ ∂ρ ρ^{∂Hz}_{∂ρ} +^{∂2 Hz}_{ρ∂ϕ2} +ρ^{∂2}_{∂z2} H_z + k^2ρH_z = 0,

(24)

and does satisfy the continuous boundary condition on the cylinder surface boundary ρ = R_1, and |z| < ∞. H_z (ρ, ϕ, z) |_{ρ=R1} = −^1_{4π} ρ_s sin(ϕ_s)^{eik} √_{|ρs|2 +(z−zs)2} (√_{|ρs|2+(z−zs)2})_2 ( ik −^1 √_{|ρs|2+(z−zs)2} ) , (25)

ρ ∂ ∂ρ H_z(ρ, ϕ, z)|_{ρ=R1} = 0, (26)

The continuous boundary conditions (25) and (26) are necessary for no scattering from the inner cylinder ρ ≤ R_1.|z| < ∞ The magnetic wave H_z (ρ, ϕ, z) is cylinder symmetry function only depend on the radial ρ and z, H_z (ρ, ϕ, z) = H_z (ρ, z) , (27) The H_z (ρ, z) does satisfy the following ordinary 0 order Bessel equation ∂ ∂ρ ρ ∂H_z ∂ρ + ρ ∂^2 ∂z^2 H_z + k^2ρH_z = 0, (28) and the following boundary conditions on the ρ = R_1, that is necessary no scattering from inner cylinder ρ ≤ R_1 .|z| < ∞ H_z (R_1, z)

= −^1_{4π} ρ_s sin(ϕ_s)^{eik} √_{|ρs|2+(z−zs)2} (√_{|ρs |2+(z−zs)2})_2 ( ik −^1 √_{|ρs |2 +(z−zs)2} ) (29)

And ∂ ∂ρ H_z(ρ, z)|_{ρ=R1} = 0, (30)

We expand the boundary value of the magnetic wave, H_z (R_1, z) in (29) as

H_z (R_1, z) = ∫_∞ 0 h_g (R_1, k_z ) cos(k_z z)dk_z, (31)

We expand the magnetic wave solution of (28),H_z (ρ, z) as H_z (ρ, z) = ∫_∞ 0 h(ρ, k_z ) cos(k_z z)dk_z, (32)

For any k_z ≥ 0, h(ρ, k_z ) does satisfy the following Bessel equation ∂ ∂ρ ρ ∂h ∂ρ − ρk^2_z h + k^2ρh = 0, (33)

h (R_1, k_z ) = h_g (R_1, k_z ) , (34) ∂ ∂ρ h(ρ, k_z)|_{ρ=R1} = 0, (35)

For 0 ≤ k_z ≤ k, the solution of (33)-(35), h(ρ, k_z) is

h(ρ, k_z) =^π_2 √ k^2 − k^2_z R_1h_g(R_1, k_z) ( N^′_0 ( R_1 √ k^2 − k^2_z ) J_0 ( ρ √ k^2 − k^2_z ) −J^′_0 ( R_1 √ k^2 − k^2_z ) N_0 ( ρ √ k^2 − k^2_z )) , (36)

For k_z ≥ k, the solution of (33)-(35), h(ρ, k_z) is h(ρ, k_z ) = − √ k^2_z − k^2R_1h_g (R_1, k_z ) (K^′_0 ( R_1 √ k^2 − k^2_z ) I_0 ( ρ √ k^2 − k^2_z ) −I^′_0 ( R_1 √ k^2 − k^2_z ) K_0 ( ρ √ k^2 − k^2_z ) ) , (37)

Summary, the magnetic wave solution of (28) C(30) in the inner cylinder, H_z(ρ, z) is H(ρ, z) =^π_2 ∫_k 0 √ k^2 − k^2_z R_1h_g(R_1, k_z) ( N^′_0 ( R_1 √ k^2 − k^2_z ) J_0 ( ρ √ k^2 − k^2_z ) −J^′_0 ( R_1 √ k^2 − k^2_z ) N_0 ( ρ √ k^2 − k^2_z )) dk_z − ∫_∞ k √ k^2_z − k^2R_1h_g(R_1, k_z) (K^′_0 ( R_1 √ k^2 − k^2_z ) I_0 ( ρ √ k^2 − k^2_z ) −I^′_0 ( R_1 √ k^2 − k^2_z ) K_0 ( ρ √ k^2 − k^2_z ) ) dk_z

(38)

The theorem 2 is proved. The magnetic field H_z (ρ, ϕ, z) is propagation penetrate into the inner cylinder ρ ≤ R_1, |z| < ∞. The inner cylinder ρ ≤ R_1, |z| < ∞. can not be cloaked.

Similarly, The electric wave propoagation penetrate into the inner cylinder, The inner cylinder ρ ≤ R_1, |z| < ∞. can not be cloaked.

IV. DISCUSSION AND CONCLUSION

In many published paper[4], authors proposed 0 to R_1 cylinder radial linear transformation for cylinder layer EM cloak,however the EM wave propagation penetrate into their inner cylinder ρ ≤ R_1, |z| < ∞. Their inner cylinder can not be cloaked. The 0 to R_1 cylinder radial coordinate transformation can not be used to make cylinder layer electromagnetic cloak

That necessary no scattering boundary conditions induced that there is unbounded spherical symmetry magnetic wave H(ρ, z) propagation in the inner cylinder ρ < R_1. If the inner magnetic wave H(ρ, z) meet the some EM scattering object in inner sphere, for example a fly, the EM scattering wave will propagation go out outside of the cylinder ρ ≤ R_2. The cylinder ρ ≤ R_2 will be detected. Also, the linear 0 to R_1 cylinder transformation makes the infinite and exceeding light speed propagation. In next papers, we will propose a novel transformation [8] for EM cylinder cloak that will overcome the difficult on the EM wave propagation penetrate into the inner cylinder ρ < R_1. It is totally different from transformation cylinder cloak,our GLHUA double layer cylinder EM incvisible cloak by [1,2,3-5,6,7,8] and GLHUA seismic double cloak and their exact analytical wave propagation will overcome all difficuties in 0 to R_1 transformation cylinder cloak.

Acknowledgments

We wish to acknowledge the support of the GL Geophysical Laboratory and thank the GLGEO Laboratory to approve the paper publication. Authors thank to Professor P. D. Lax for his concern and encouragements Authors thank to Dr. Michael Oristaglio and Professor You Zhong Guo for their encouragments

[1] Jianhua,Li, G. Xie, C, Lin, J. Liu, SEG, Expanded Abstracts, 21, 1, 692-695, (2002), https://www.onepetro.org/conference-paper/SEG-2002- 0692.

[2] Xie, G., F. Xie, L. Xie, and J. Li, “New GL method and its advantages for resolving historical diffculties,” Progress In Electromagnetics Research, PIER 63, 141–152, 2006.

[3] G. Xie, J. Li, L. Xie, F. Xie, arXiv:1005.3999, (2010). [4] D. Schurig,1 J. J. Mock,1 B. J. Justice,1 S. A. Cummer,1 J. B. Pendry,2 A. F. Starr,3 D. R. Smith1* Metamaterial Electromagnetic Cloak at Microwave Frequencies SCIENCE VOL 314 10 NOVEMBER 2006, www.sciencemag.org [5] Xie, G., J.H. Li, E. Majer, D. Zuo, M. Oristaglio “3-D electromagnetic modeling and nonlinear inversion,” Geophysics, Vol. 65, No. 3, 804–822, 2000.

[6] Jianhua,Li, F. Xie, Lee Xie, G. Xie,

GLHUA Electromagnetic Invisible Double Layer Cloak With Relative Parameters Not Less Than 1 and GL No Scattering Inversion, arXiv:1612.02857 [7] Jianhua,Li, F. Xie, Lee Xie, G. Xie, The Theoretical Proof for GLHUA EM Invisible Double Layer Cloak By Using GL No Scattering Modeling and Inversion, arXiv:1701.00534 [8] Jianhua,Li, F. Xie, Lee Xie, G. Xie, ELECTROMAG- NETIC WAVE PROPAGATION IN GLHUA INVISIBLE SPHERE BY GL NO SCATERING FULL WAVE MOD- ELING AND INVERSION, arXiv:1701.02583