arXiv:1712.05337v1 [cond-mat.dis-nn] 14 Dec 2017

Condensed Matter Physics, 2017, Vol. 20, No 4, 43601: 1–9

DOI: 10.5488/CMP.20.43601

http://www.icmp.lviv.ua/journal

The effect of asymmetry of the coil block on self-assembly in ABC coil-rod-coil triblock copolymers

X.-G. Han^1∗, H.-H. Meng^1, Y.-H. Ma^1, S.-L. Ouyang^2

1 School of Science, Inner Mongolia University of Science and Technology, Baotou 014010, China

2 Inner Mongolia Key Laboratory for Utilization of Bayan Obo Multi-Metallic Resources: Elected State Key

Laboratory, Inner Mongolia University of Science and Technology, Baotou 014010, China

Received January 25, 2017, in final form June 5, 2017

Using the self-consistent field approach, the effect of asymmetry of the coil block on the microphase separation is focused in ABC coil-rod-coil triblock copolymers. For different fractions of the rod block f_B, some stable structures are observed, i.e., lamellae, cylinders, gyroid, and core-shell hexagonal lattice, and the phase diagrams are constructed. The calculated results show that the effect of the coil block fraction f_A is dependent on f_B. When

f_B = 0.2, the effect of asymmetry of the coil block is similar to that of the ABC flexible triblock copolymers;

When f_B = 0.4, the self-assembly of ABC coil-rod-coil triblock copolymers behaves like rod-coil diblock copolymers under some condition. When f_B continues to increase, the effect of asymmetry of the coil block reduces.

For f_B = 0.4, under the symmetrical and rather asymmetrical conditions, an increase in the interaction param-

eter between different components leads to different transitions between cylinders and lamellae. The results indicate some remarkable effect of the chain architecture on self-assembly, and can provide the guidance for the design and synthesis of copolymer materials.

Key words: self-consistent field theory, rod-coil block copolymer, self-assembly

PACS: 61.25.Hp, 64.75.+g, 82.60.Fa

1. Introduction

Block copolymers are macromolecules composed of chemically distinct subchains or blocks. The distinct blocks tend to phase separate, whereas the covalent bonds between distinct blocks prevent a macroscopic separation. The competition of these two opposing trends leads to the formation of various ordered phases [1]. From a fundamental point of view, the ordering in block copolymers provides an ideal paradigm for the study of self-organization in soft condensed matter [2]. From a technological point of view, the rich and fascinating ordered structures from block copolymers have found applications ranging from thermoplastic elastomers and high-impact plastics to pressure-sensitive adhesives, and so on. Compared with coil-coil block copolymers, rod-coil block copolymers have received much attention due to their abilities to self-assemble smaller scale structures in the field of novel functional and biomimetic materials [3, 4]. Especially, the rod-coil block copolymers containing conjugated rod building blocks offer opportunities for engineering electronic and optical devices [5–7].

In contrast to coil-coil block copolymers, rod-coil diblock copolymers have rich phase behaviors. Rodcoil block copolymers, as the simplest rod-coil block copolymers, self-assembled into ordered structures, e.g., zigzag lamellae [8], stripes [9], honeycombs [10], and hollow spherical and cylindrical micelles [11]. Compared with AB diblock copolymers, ABC triblock copolymers have more independent parameters controlling their phase behavior. The phase behavior of the two-component rod-coil block copolymers is controlled mainly by three parameters: the volume fraction of the rod block f_A, the Flory-Huggins interaction between different blocks χ_{AB}, and the total degree of polymerization of the copolymer N.

∗xghan0@163.com

This work is licensed under a Creative Commons Attribution 4.0 International License. Further distribution of this work must maintain attribution to the author(s) and the published article’s title, journal citation, and DOI.

43601-1

For ABC triblock copolymers, the number of parameters increases to six, including three interaction parameters χ_{AB}, χ_{BC}, and χ_{AC}; two independent volume fractions f_A and f_B and the total degree of polymerization of the copolymer N. This increased number of molecular variables will impose varieties and complexities on the self-assembly of the rod-coil block copolymers, meanwhile, leading to a great model system for engineering of a large number of intriguing nanostructures.

Some studies have centered on the microphase separation of rodlike-coil three-component block copolymers. Experimentally, Lee and coworkers [12, 13] studied ABC coil-rod-coil triblock molecules, focusing the fraction of coil block on the order-order transition [12]. Zhou et al. [14] reported an ABC coil-coil-rod triblock containing liquid crystal polymer as the rod block, and found the formation of a liquid crystalline phase when the rod block achieved a certain length. Chang et al. [15] found that the rod-rod interaction lead to an order-disorder transition, and the lamellae appeared for f_{rod} ≃ 0.2 in ABC rod-coil-coil triblock copolymers. Theoretically, Xia et al. studied the self-assembly of ABC rod-coil-coil and coil-rod-coil triblock copolymers [16], constructing the phase f_{rod} vs. χ_N phase diagram. Recently, Li et al. concentrated on the order-to-order phase transitions in coil-worm-coil triblock copolymers, suggesting that the tuning of the flexibility parameter provides a promising approach to design the resulting microphase-separated structures in semiflexible copolymer melts [17]. Although some literatures reported the effect of the fraction of end block on self-assembly, a systematic theoretical study on the molecularly asymmetry of the copolymers containing rigid blocks does not exist so far.

Due to the flexibility of adjusting system parameters, theory and simulation provide an ideal approach to explore the phase behavior of block copolymers. Mayes and Olvera de la Cruz [18], as well as Dobrynin and Erukhimovich [19] investigated flexible ABA triblock copolymers in the weak-segregation limit, providing evidence that molecular asymmetry can have a profound effect on both order-disorder and order-order transitions. Later on, Matsen used the self-consistent field theory [20] (SCFT) to show that such molecular asymmetry can alter microdomain dimensions and order-order transitions. Recently, Woloszczuk et al. employed on-lattice Monte Carlo simulations to examine the phase behavior of molecularly flexible asymmetric ABA copolymers in the limit of superstrong segregation, wherein interstitial micelles composed of the minority A endblock were observed to arrange into two-dimensional hexagonal arrays along the midplane of B-rich lamellae. These studies have demonstrated that molecular asymmetry is an important factor for self-assembly of block copolymers. In this work, we will systematically study the effect of the asymmetry of the coil block on self-assembly in the rod-coil block copolymers.

SCFT can be used to study rod-coil block copolymer systems. Pryamitsyn and Ganesan introduced Maier-Saupe theory [18, 19, 21, 22] to really account for the aligning interactions between rods, and the anisotropy interaction between rods presented considerable computational challenges. Some other theoretical models did not consider anisotropic interactions between the rods. For instance, Chen et al. [23], as well as Li and Gersappe [24] performed lattice-based SCFT simulations provided with computational advantage. The work of Chen et al. was the first time that SCFT predicted the hexagonal cylinder phase for rod-coil block copolymers. Subsequently Chen et al. used the SCFT lattice model to study the self-assembly of two-component rod-coil block copolymers [25–28] and studied firstly in theory three-component ones [16]. In this work, using SCFT lattice model, we concentrate on the effect of the volume fraction of the coil block on structure transition in the ABC coil-rod-coil triblock copolymers, providing for different rod block fractions. The paper is organized as follows: In section 2, we present the lattice model SCFT of coil-rod-coil triblock copolymers. The approach employs a two-stage relaxation procedure to evolve a system as rapidly as possible to a free-energy minimum similar to the literature [23]. In section 3, the calculated results are presented. These results are compared with those of previous works, especially with flexible ABC triblock copolymers. A brief conclusion will be given in section 4.

2. Theory

We consider n linear ABC coil-rod-coil triblock copolymers in a lattice, where the degree of polymerization of each chain is N. The A, B and C segments have the same size and each segment occupies one lattice site. Thus, the total number of the lattice sites N_L equals n( f_A + f_B + f_C)N. The system partition function can be expressed as

43601-2

Z = � r(j,s),α(j,s) � � � 1 N^n_L 1 z^n n� j=1 N� s=2 λ^{αj, s −α} ′ j, s−1

r_{j, s} −r^′_{j, s−1} � � � exp � − U k_BT � . (2.1)

Here, r_{j,s} and α_{j,s} denote the position and bond orientation of the s-th segment of the j-th copolymer, respectively. r^′ denotes the nearest neighboring site of r. α_{j,s} can choose all of the possible bond orientations, which depends on the selected lattice model. z denotes lattice coordination number. The transfer matrix lambda depends only on the chain model used. This paper adopts an inflexion chain model. For a coil subchain,

λ^{αj, s −α} ′ j, s−1

r_{j, s} −r^′_{j, s−1} = � 0, α_{j,s} = −α^′_{j,s−1} , 1/(z − 1), otherwise.

(2.2)

For a rigid subchain,

λ^{αj, s −α} ′ j, s−1

r_{j, s} −r^′_{j, s−1} = � 1, α_{j,s} = α^′_{j,s−1} , 0, otherwise.

(2.3)

Following the scheme of Scheutjens and Leemakers [29], the end-segment distribution function G^{αs} (r, s|1) presents a statistical weight of all possible configurations staring from segment 1, which can be located in any position within the lattice, ending at segment s at site r, and satisfies the following recurrence relation:

G^{αs} (r, s|1) = G(r, s) � r^′_{s−1} � α^′_{s−1}

λ^{αs −α′s−1}

r_s −r^′_{s−1} G α_{s−1} (r ′, s − 1|1). (2.4)

For all the values of α_1, the initial condition is G^{α1} (r, 1|1) = G(r, 1), G(r, s) is the weight factor of the free segment. It is expressed as G(r, s) = exp[−ω_β(r_s)], s ∈ β (β = A, B, C). Another end-segment distribution function G^{αs} (r, s|N) satisfies the following recurrence relation:

G^{αs} (r, s|N) = G(r, s) � r^′_{s+1} � α^′_{s+1}

λ^{αs+1−α′s}

r^′_{s+1}−r_s G α_{s+1} (r ′, s + 1|N). (2.5)

With the initial condition G^αN (r, N|N) = G(r, N) for all the values of α_N .

The free energy functional of F (in the unit of k_BT ) in canonical ensemble is defined by F = 1 z � rr^′

[χ_{AB}ϕ_A(r)ϕ_B(r^′) + χ_{AC}ϕ_A(r)ϕ_C(r^′) + χ_{BC}ϕ_B(r)ϕ_C(r^′)] − � r [ω_A(r)ϕ_A(r)

+ ω_B(r)ϕ_B(r) + ω_C(r)ϕ_C(r)] − � r ξ(r)[1 − ϕ_A(r) − ϕ_B(r) − ϕ_C(r)] − n ln Q , (2.6)

where Q = 1 N_L 1 z � r_N � α_N

G^{αN} (r, N|1). (2.7)

Here, χ_{AB}, χ_{AC}, χ_{BC} are the Flory-Huggins interaction parameters between different species. The ϕ_k (r) is the volume fraction field of block specie k, which is independent of the individual polymer configuration, and ω_k (r) is the chemical potential field conjugated to ϕ_k(r). The ξ(r) is the potential field that ensures the incompressibility of the system, also known as a Lagrange multiplier.

Minimizing the free energy functional F with respect to ϕ_A, ϕ_B, ϕ_C, ω_A, ω_B, ω_C and ξ(r) lead to the following SCFT equations:

ω_A(r) = 1 z � r^′

χ_{AB}ϕ_B(r^′) + 1 z � r^′

χ_{AC}ϕ_C(r^′) + ξ(r), (2.8)

ω_B(r) = 1 z � r^′

χ_{BC}ϕ_C(r^′) + 1 z � r^′

χ_{AB}ϕ_A(r^′) + ξ(r), (2.9)

43601-3

ω_C(r) = 1 z � r^′

χ_{AC}ϕ_A(r^′) + 1 z � r^′

χ_{BC}ϕ_B(r^′) + ξ(r), (2.10)

ϕ_A(r) + ϕ_B(r) + ϕ_C(r) = 1, (2.11)

ϕ_A(r) = 1 N_L 1 z n Q � s∈A � α_s

G^{αs} (r, s|1)G^{αs} (r, s|N) G(r, s)

, (2.12)

ϕ_B(r) = 1 N_L 1 z n Q � s∈B � α_s

G^{αs} (r, s|1)G^{αs} (r, s|N) G(r, s)

, (2.13)

ϕ_C(r) = 1 N_L 1 z n Q � s∈C � α_s

G^{αs} (r, s|1)G^{αs} (r, s|N) G(r, s)

. (2.14)

In our calculations, the real-space method is implemented to solve the SCFT equations in a cubic lattice with periodic boundary conditions [16, 23]. The calculations begin from the initial potential fields generated by random functions, and stop when the free energy of the system changes within a tolerance of 10^{−8}. By comparing the system free energies from different initial potential fields, we obtained stable phases in the system of ABC coil-rod-coil triblock copolymers.

3. Result and discussion

In our studies, we explore the effect of the asymmetry of the coil block on structural transition in ABC coil-rod-coil triblock copolymers. The interaction parameters between different species are the same, i.e., χ_{AB} = χ_{BC} = χ_{AC} = χ, and the degree of the polymerization is N = 20. Our calculations are preformed in the lattices of N_L = 60^3 and N_L = 80^3, and the emergence of the self-assembled structures are not constrained by system size. As showed in figure 1, some stable structures are observed, i.e., cylinders, core-shell hexagonal lattice (CSH) phase, lamellae and gyriod, and a perforated lamellae phase appears as a metastable structure. The phase diagrams for copolymers constructed by f_A versus χN are shown in figure 2 for f_B = 0.2, 0.4, 0.6, and most of the regions of all the phase diagrams are occupied by lamellar phase. This indicates that the tolerance of the lamellae to chain architecture asymmetry is the highest of these stable phases in ABC triblock copolymers.

In the case of f_B = 0.2, and when f_A (= 0.05, 0.1) is small, among the three phase, i.e., micelles, CSH phase and lamellae, micelles are the most stable, and the A and B components coexist in the domain of a micelle. With an increase in f_A, CSH phase (0.15 � f_A � 0.20), where the core and shell severally consist of A and B components, firstly becomes more stable, and then lamellae (0.25 � f_A � 0.40) are stable phase. For rod-coil diblock copolymers, at f_B = 0.2, lamellae are not observed, while micelles are observed. Therefore, the existence of a third block leads to the appearance of lamellae, which is confirmed by the flexible triblock copolymer [30]. The CSH phase and lamellae also appear in turn under the similar conditions in flexible ABC ones, but the A and B component-mixed phase is not observed. However, it is expected that micelles will change into CSH phase when the interaction parameter is rather big. Therefore, for f_B = 0.2, the effect of the length of the end block on microphase separation in ABC coil-rod-coil triblock copolymers is similar to that of the flexible ones.

For f_B = 0.4, when the two coil blocks are symmetrical, gyriod and cylinders can be found, gyriod is more stable in the small parameter region of 9 � χN � 13. With an increase in χN, cylinders are more stable than gyriod. With the appearance of the asymmetry of the copolymers (0.20 � f_A � 0.25), gyriod is replaced by lamellar structure. When χN � 14, the free energy of the lamellae is higher than that of cylinders, and thus cylinders remain stable. When f_A = 0.15, 0.10, the cylinder structure is also replaced by lamellae into the larger χN region, and near the order-disorder transition, the copolymers self-assemble into gyriod again. When f_A = 0.05, cylinders are observed in a small χN region, which is different from the case of the large f_A. When χN � 12, lamellae are still observed. In the flexible ABC triblock copolymers, however, the three-color lamellae do not appear when f_A < 0.1. It is obvious that the appearance of lamellae at f_A = 0.05 results from the rigidity of the middle block copolymer of coil-rod-coil triblock copolymer. Accordingly, the chain stiffness is propitious to the occurrence of

43601-4

Figure 1. (Color online) The self-assembled structures of ABC coil-rod-coil triblock copolymers: (a)

cylinder (the components A and C are eliminated for clarity); (b) lamella (the components A and C are eliminated for clarity); (c) gyriod (the components A and B are eliminated for clarity); (d) perforated lamella phase (the components A and C are eliminated for clarity); (e) core-shell hexagonal lattice (the components A and C are eliminated for clarity).

lamellae, which is scrupulously discussed in bottlebrush block copolymers [31]. Furthermore, when 13 � χN � 16, perforated lamellar phase is observed as a metastable structure. When f_A becomes small, the gyriod and cylinders sequentially appear for small χN, indicating that the self-assembly for the asymmetric coil-rod-coil triblock copolymers tends to be that of the coil-rod diblock copolymers, which is in detail discussed below. It is noted that with an increasing χN, the lamellar phase translates into cylinders for large f_A, and vice versa at f_A = 0.05. The effect of the length of the end A block is concerned with the fraction of the middle rod block. For f_B = 0.6, the distribution of the ordered structures in a phase diagram [see figure 2 (c)] is similar to the one of f_B = 0.4 for large f_A. It is shown that the effect of asymmetry of the end coil block on self-assembly will reduce when f_B continues to increase.

In order to clarify the difference of the above two transitions between lamellae and cylinders for f_B = 0.4, as shown in figure 3, the cylindrical phases for different f_A are compared below. When f_A = 0.05 and near the order-disorder transition, both B and C components self-assemble into two cylindrical domains which distribute symmetrically in the space [see figure 3(a)]. The rest of A component appears in the same region of B component as shown in figure 3 (c), since the volume fractions of A component are too small to appear alone in some space positions, where cylinders are similar to those of rod-coil diblock copolymers [23]. When χN increases, the A component is separated from the domain of B component, and the lamellae become stable. In other words, the cylinder/lamella transition appears with an increasing χN. The reason for the formation of cylinders and the explanation for the transition between cylinders and lamellae are in detail discussed by Chremos and Theodorakis [32]. They proposed that a molecular asymmetry is required for the formation of cylindrical domains, and the cylinder/lamella transition results from the entropic penalty, which does apply to diblock copolymers. When f_A = 0.05, the coil-rod-coil triblock copolymers are very asymmetric and are regarded as diblock copolymer, and thus the cylinders form. The appearance of lamellae with χN is due to the behavior of the triblock copolymer. It is obvious that herein the mechanism of the cylinder/lamella is different from the one

43601-5

Figure 2. (Color online) The phase diagram for the ABC coil-rod-coil triblock copolymers with different

length of the end A coil block when f_B = 0.2, 0.4, 0.6, respectively.

proposed by Chremos and Theodorakis. The appearance of the cylinder/lamella transition is to minimize the interaction energy among different components, which is in reasonable agreement with the same transition observed experimentally in rod-coil diblock copolymers [33].

By contrast, when f_A is large, only B component assembles into cylinders, and the A and C components appear alternately in the regions between the series of cylinders [see figure 3 (b) and (c)]. When χN is small, the interface between different component domains is relatively thick, where the system tends to make more room for the coil block to maximize entropy. When χN increases, the interface of lamellae tends to be thin to minimize the interaction energies between different components, and to simultaneously give rise to the configuration entropic penalty. Compared with lamellae, cylinders, where the rods are assembled into interdigitated bilayer structure [23], are favorable to the configuration entropy. Consequently, the cylinders are more stable than lamellar phase for large χN, i.e., the lamella/cylinder transition appears with χN.

4. Conclusion and summary

Using the self-consistent field approach, the effect of asymmetry of the coil block on the microphase separation is focused in ABC coil-rod-coil triblock copolymers. The calculated results show that the effect of the coil block fraction f_A is dependent on f_B. When f_B is small, the effect of asymmetry of the coil block is similar to that of the ABC flexible triblock copolymers; When f_B is an intermediate value, the self-assembly of ABC coil-rod-coil triblock copolymers can behave like rod-coil diblock copolymers under rather asymmetrical conditions. When f_B is large, the effect of asymmetry of the coil block reduces. For intermediate f_B, under the symmetrical and rather asymmetrical conditions, an increase in the interaction parameter between different components leads to different transitions between cylinders

43601-6

Figure 3. (Color online) Figures (a) and (b) are cross sections of the two cylindrical structures with

f_A = 0.05 and f_A = 0.3, respectively. Figure (c) indicates the density changes of three components along the black line in the figures (a) and (b), the hollow and solid symbols correspond to f_A = 0.05 and f_A = 0.3, respectively.

and lamellae. In rod-coil ABC systems, the asymmetric interaction parameters can also be tuned up. It is expected that the interesting morphologies can form in the self-assembly under the conditions of asymmetric interactions, which is demonstrated by the ABC coil-coil-coil triblock copolymers [30, 34]. This investigation will be implemented in the subsequent work.

Acknowledgements

This research is financially supported by the National Nature Science Foundations of China (21564011), the Nature Science Foundations of the Inner Mongolia municipality (2017MS(LH)0211), and the Graduate Education Innovation Program of the Inner Mongolia Autonomous Province (S20161012707).

References

1. Hamley I.W., Developments in Block Copolymer Science and Technology, Wiley, New York, 2004, doi:10.1002/0470093943.fmatter.

2. Hamley I.W., The Physics of Block Copolymers, Oxford University Press, Oxford, 1998. 3. Lecommandoux S., Achard M.F., Langenwalter J.F., Klok H.A., Macromolecules, 2001, 34, 9100–9111, doi:10.1021/ma010940j.

43601-7

4. Łosik M., Kubowicz S., Smarsly B., Schlaad H., Eur. Phys. J. E, 2004, 15, 407–411,

doi:10.1140/epje/i2004-10057-5.

5. Ball Z.T., Sivula K., Fréchet J.M.J., Macromolecules, 2006, 39, 70–72, doi:10.1021/ma052325b. 6. Van De Wetering K., Brochon C., Ngov C., Hadziioannou G., Macromolecules, 2006, 39, 4289–4297, doi:10.1021/ma060497i.

7. Dai C.A., Yen W.C., Lee Y.H., Ho C.C., Su W.F., J. Am. Chem. Soc., 2007, 129, 11036–11038, doi:10.1021/ja0733991.

8. Chen J.T., Thomas E.L., Ober C.K., Hwang S.S., Macromolecules, 1995, 28, 1688–1697, doi:10.1021/ma00109a048.

9. Radzilowski L.H., Carragher B.O., Stupp S.I., Macromolecules, 1997, 30, 2110–2119, doi:10.1021/ma9609700. 10. Lee M., Cho B.K., Ihn K.J., Lee W.K., Oh N.K., Zin W.C., J. Am. Chem. Soc., 2001, 123, 4647–4648, doi:10.1021/ja004071+.

11. Jenekhe S.A., Chen X.L., Science, 1998, 279, No. 5358, 1903–1907, doi:10.1126/science.279.5358.1903. 12. Lee M., Lee D.W., Cho B.K., Yoon J.Y., Zin W.C., J. Am. Chem. Soc., 1998, 120, 13258, doi:10.1021/ja9823619. 13. Oh N.K., Zin W.C., Im J.H., Lee M., Polymer, 2006, 47, 5275–5286, doi:10.1016/j.polymer.2006.05.039. 14. Zhang H., Sun X., Wang X., Zhou Q.F., Macromol. Rapid Commun., 2005, 26, 407–411, doi:10.1002/marc.200400506.

15. Chang C.J., Lee Y.H., Chen H.L., Chiang C.H., Hsu H.F., Ho C.C., Su W.F., Dai C.A., Soft Matter, 2011, 7, 10951–10960, doi:10.1039/c1sm05926b.

16. Xia Y.D., Chen J.Z., Sun Z.Y., Shi T.F., An L.J., Jia Y.X., Polymer, 2010, 51, 3315–3319, doi:10.1016/j.polymer.2010.04.063.

17. Li S.B., Jiang Y., Chen J.Z.Y., J. Chem. Phys., 2016, 145, 184902, doi:10.1063/1.4967423. 18. Gao J., Tang P., Yang Y.L., Soft Matter, 2013, 9, 69–81, doi:10.1039/C2SM26758F. 19. Li S.B., Jiang Y., Chen J.Z.Y., Soft Matter, 2014, 10, 8932–8944, doi:10.1039/C4SM01884B. 20. Matsen M.W., Schick M., Phys. Rev. Lett., 1994, 72, 2660, doi:10.1103/PhysRevLett.72.2660. 21. Pryamitsyn V., Ganesan V., J. Chem. Phys., 2004, 120, 5824–5838, doi:10.1063/1.1649729. 22. Jiang Y., Chen J.Z.Y., Phys. Rev. Lett., 2013, 110, 138305, doi:10.1103/PhysRevLett.110.138305. 23. Chen J.Z., Zhang C.X., Sun Z.Y., Zheng Y.S., An L.J., J. Chem. Phys., 2006, 124, 104907, doi:10.1063/1.2176619.

24. Li W.T., Gersappe D., Macromolecules, 2001, 34, 6783–6789, doi:10.1021/ma010194i. 25. Chen J.Z., Zhang C.X., Sun Z.Y., An L.J., Tong Z., J. Chem. Phys., 2007, 127, 024105,

doi:10.1063/1.2750337.

26. Chen J.Z., Sun Z.Y., Zhang C.X., An L.J., Tong Z., J. Chem. Phys., 2008, 128, 074904, doi:10.1063/1.2831802. 27. Xia Y.D., Sun Z.Y., Shi T.F., Chen J.Z., An L.J., Jia Y.X., Polymer, 2008, 49, 5596–5601, doi:10.1016/j.polymer.2008.09.059.

28. Xia Y.D., Chen J.Z., Sun Z.Y., Shi T.F., An L.J., Jia Y.X., J. Chem. Phys., 2009, 131, 144905, doi:10.1063/1.3247192.

29. Leermakers F.A.M., Scheutjens J.M.H.M., J. Chem. Phys., 1988, 89, 3264, doi:10.1063/1.454931. 30. Tang P., Qiu F., Zhang H.D., Yang Y.L., Phys. Rev. E, 2004, 69, 031803, doi:10.1103/PhysRevE.69.031803. 31. Chremos A., Theodorakis P.E., Polymer, 2016, 97, 191–195, doi:10.1016/j.polymer.2016.05.034. 32. Chremos A., Theodorakis P.E., ACS Macro Lett., 2014, 3, 1096–1100, doi:10.1021/mz500580f. 33. Shi L.Y., Shen Z.H., Fan X.H., Macromolecules, 2011, 44, 2900–2907, doi:10.1021/ma1023704. 34. Tyler C.A., Qin J., Bates F.S., Morse D.C., Macromolecules, 2007, 40, 4654, doi:10.1021/ma062778w.

43601-8

Вплив асиметрiї виткоподiбного блоку на самоскупчення у ABC виток-стержень-виток триблокових кополiмерах

К.-Г. Ґан^1, Ґ.-Ґ. Менг^1, Й.-Ґ. Ма^1, С.-Л. Оуянг^2

1 Вища школа природничих наук, Унiверситет науки i технологiй внутрiшньої Монголiї, Баоту 014010, Китай 2 Головна лабораторiя iнтегрованого використання мультиметалiчних ресурсiв Баян Обо, Унiверситет науки i технологiї внутрiшньої Монголiї, Баоту 014010, Китай

Використовуючи самоузгоджений польовий пiдхiд, описано вплив асиметрiї виткоподiбного блоку на мiкрофазне роздiлення в ABC триблокових кополiмерах виток-стержень-виток. Для рiзних фракцiй стержневого блоку f_B, спостерiгаються стiйкi структури, а саме ламели, цилiндри, гiроїд i гексагональна ґратка сердечник-оболонка, а також побудованi фазовi дiаграми. Результати обчислень показують, що ефект фракцiї виткоподiбного блоку f_A залежить вiд f_B. Коли f_B = 0.2, тодi вплив асиметрiї виткоподiбного блоку є подiбним до ефекту ABC гнучких триблокових кополiмерiв. Коли f_B = 0.4, тодi самоскупчення ABC виток-стержень-виток триблокових кополiмерiв вiдбувається подiбно до двоблокових кополiмерiв стержень-виток за певних умов. Коли f_B продовжує зростати, тодi вплив асиметрiї виткоподiбного блоку зменшується. При f_B = 0.4, за симетричних та доволi асиметричних умов, збiльшення параметра взаємодiї мiж рiзними компонентами призводить до рiзних переходiв мiж цилiндрами та ламелами. Результати вказують на деякий значний вплив ланцюжкової архiтектури на самоскупчення, що може бути керiвництвом для розробки та синтезу кополiмерних матерiалiв.

Ключовi слова: самоузгоджена польова теорiя, стержень-виток блоковий кополiмер, самоскупчення

43601-9