arXiv:1905.12178v1 [cond-mat.mes-hall] 29 May 2019

Optically probing Schwinger angular momenta in a micromechanical resonator

Motoki Asano^{1,∗}, Ryuichi Ohta^1, Takuma Aihara^2, Tai Tsuchizawa^2, Hajime Okamoto^1, and Hiroshi Yamguchi^1 1NTT Basic Research Laboratories, NTT Corporation, 3-1 Morinosato Wakamiya, Atsugi-shi, Kanagawa 243-0198, Japan and 2NTT Device Technology Laboratories, NTT Corporation, 3-1 Morinosato Wakamiya, Atsugi-shi, Kanagawa 243-0198, Japan ( Dated: May 30, 2019)

Abstract

We report an observation of phononic Schwinger angular momenta, which fully represent twomode states in a micromechanical resonator. This observation is based on simultaneous optical detection of the mechanical response at the sum and difference frequency of the two mechanical modes. A post-selection process for the measured signals allows us to extract a component of phononic Schwinger angular momenta. It also enables us to conditionally prepare two-mode squeezed (correlated) states from a randomly excited (uncorrelated) state. The phononic Schwinger angular momenta could be extended to high-dimensional symmetry (e.g. SU(N) group) for studying multipartite correlations in non-equilibrium dynamics with macroscopic objects.

In the theory of quantum angular momentum generalized by Julian Schwinger [1], the angular momentum constructed from two bosonic modes is classified into two groups, SU(2) and SU(1,1). Such Schwinger angular momenta fully represent two-mode states in the system in terms of energy, coherence, and correlations, and allow us to perform state tomography [2, 3], interferometry [4], and test of quantumness [5]. State tomography with angular momentum in the SU(2) group (i.e., Stokes parameters [6]) has been widely demonstrated to identify coherence between various two-mode optical systems [7, 8, 9] in both classical and quantum regime. Interferometry with the angular momenta in the SU(1,1) group has a great potential to enable phase measurements at the Heisenberg limit [10]. Such Schwinger angualr momenta have been well-engineered mainly in optical (photonic) systems but have never been explicitly observed in mechanical (phononic) systems.

A high-Q micromechanical resonator contains multiple non-degenerated mechanical modes and easily shows nonlinearlity induced by opto-mechanical or electro-mechanical interaction [11, 12, 13, 14, 15, 16, 17]. The combination of such nonlinearity with the multiplicity in the mechanical modes opens the door to the observation of phononic Schwinger angular momentum in a mechanical system. In this Letter, we demonstrate optical probing of Schwinger angular momenta in a high-Q micromechanical resonator. The phononic Schwinger angular momenta in the SU(2) and SU(1,1) groups are revealed by probing nonlinear signals via Doppler interferometry and performing a post-selection process. They enable us to conditionally extract two-mode squeezed (correlated) states from a randomly excited (uncorrelated) state because these angular momenta are the function of cross-correlation.

The phononic Schwinger angular momenta in the SU(2) and SU(1,1) groups are represented by vectors S = (S_x, S_y, S_z) and K = (K_x, K_y, K_z) in a sphere and a hyperboloid, respectively [Fig. 1(a) and (b)]. The vertical axis of the sphere is given by S_z = (x^2 + y^2 − x^2_1 − y^2_1)/4 and that of the hyperboloid is given by K_z = (x^2 + y^2 + x^2_1 + y^2_1 )/4, where x_i and y_i are the linear quadrature of ith mechanical modes. The z component of the Schwinger angular momentum corresponds to the energy difference between the two mechanical modes for the SU(2) group and the energy sum for the SU(1,1) group. On the other hand, the x and y components, S_x, S_y and K_x, K_y, include information about the crosscorrelation of the two mechanical modes, where S_x = (x_2y_1 −y_2x_1)/2, S_y = −(x_2x_1 +y_1y_2)/2, K_x = (x_2y_1 + x_1y_2)/2, and K_y = (x_2x_1 − y_2y_1)/2. Each component of angular momenta satisfies a Lie algebra, e.g., {S_i, S_j} = S_k only if i, j, k are cyclic with x, y, z with the Poisson bracket {·} (see supplemental information). These angular momenta represent rotational trajectories in their joint phase space. The rotational trajectory in the SU(2) group is specified with a real angle and that in the SU(1,1) group is specified with an imaginary angle (i.e., hyperbolic trajectory). For instance, the phononic Schwinger angular momentum along the x-direction, i.e., S = (S_x, 0, 0) (K = (K_x, 0, 0)), represents the rotational trajectory with a real angle ϕ (an imaginary angle iϕ) in a joint phase space spanned by x_1 and x_2.

Non-degenerated modes in a micromechanical resonator crucially contain randomness at finite temperature because they are independently actuated by random forces. They lead a random trajectory in their joint phase space, i.e., the phononic Schwinger angular momenta also show a random distribution. The average value of their transverse components becomes zero because of their isotropic distribution. In other words, we can achieve the two-mode mechanical states with the non-zero average of phononic Schwinger angular momenta by directly probing these components and conditionally extracting part of the distribution. To demonstrate these operations, we perform the following two steps.

The first step is to directly probe the nonlinear optical signals generated via higher-order modulation in a Doppler interferometer. These nonlinear optical signals at the sum and difference frequency of two mechanical modes correspond to the response from the transverse components of the phononic Schwinger angular momenta in the SU(2) and SU(1,1) groups, respectively (see supplemental information). A Doppler interferometer was used to simultaneously probe the first-order vibrational mode (Ω_1 = 2π × 0.52 MHz) and thirdorder vibrational mode (Ω_2 = 2π × 1.75 MHz) in a high-tensile silicon-nitride mechanical resonator (150-μm long, 5-μm wide, and 525-nm thick) [Fig. 1(c)]. The high quality factors (∼ 30, 000) in our resonator enhance the measurement sensitivity of the sum and difference frequency signals because the power spectral density of them is proportional to √ n_1n_2Q, where n_i is the number of phonons in the ith mode and Q is the quality factor (see supplemental information). To overcome the measurement noise (∼ 1.4 pm/ √ Hz) in our setup, the mechanical modes were additionally excited to increase n_1 and n_2 via a PZT sheet with artificial white noise. Around the effective temperature T_{eff} > 10^6 K, we observed the noise spectra of sum and difference frequency signals with a spectrum analyzer (the vertical unit is calibrated with thermal motion at room temperature without excitation [18])[Fig. 1(d)]. A random trajectory in the joint phase space was obtained by monitoring the linear quadrature with two lock-in amplifiers with Ω_1 and Ω_2 frequency references [Fig. 1(e)].

The second step involves post-selecting the non-zero average in the transverse components of phononic Schwinger angular momenta. This conditional measurement was performed in quadrature of nonlinear signals from two additional lock-in amplifiers with Ω_2 − Ω_1 and Ω_2 +Ω_1 frequency references. This quadrature contains the response from the two orthogonal transverse components of phononic Schwinger angular momenta (e.g., S_x and S_y). The 10^5 temporal data sets for all signals from the four lock-in amplifiers were recorded within a total of 400 msec. To extract the statistical ensemble which shows the non-zero average of the transverse components, we imposed a condition O_j/max[O_j] ≥ η for a quadrature (i.e., O_j=S_x, S_y, K_x and K_y), where η is a trigger level [Fig. 2(a)]. Although increasing η allows us to extract a large average value of O_j, the number of events which satisfy the condition decreases. We evaluate success probability p_s defined by the number of events satisfying the condition divided by the total number of events [Fig. 2(b)]. When η = 0, only the positive value of the angular momentum is extracted from the random motion, and the average value is trivially non-zero, where p_s = 0.5. Increasing η decreases the success probability because a large amount of the angular momentum only slightly appears in the random motion. The trajectory in the conditional measurement was determined by extracting linear quadratures x_i and y_i only when O_j satisfies the condition. To display the rotational trajectories with respect to the phononic Schwinger angular momenta, the reference frequencies for the lock-in amplifiers were set with a finite detuning so that the detuning δ_i of the ith mode satisfies δ_1 ≈ δ_2 (see supplemental information). The conditional measurement with the finite detuning results in discontinuous rotational motion with a real and imaginary angle [conceptually depicted in Fig.1(a) and (b)] with S_x and K_x, respectively [Fig. 2(c) and 2(d)], whereas a random trajectory was observed without any conditioning [Fig. 1(e)]. This verifies that our conditional measurement allows us to extract the nonzero average of phononic Schwinger angular momenta. For the other components, S_y and K_y, we achieved similar results in the phase space spanned by x_1 and y_2 (see supplemental information).

The transverse components of phononic Schwinger angular momenta also represent a correlation between the two linear quadratures. For instance, the average of S_x and K_x contains the correlation function of x_1 and y_2 (also x_2 and y_1). This implies that the conditional measurement allows us to extract a correlated two-mode state in the randomly actuated mechanical resonator. Here, we evaluate the two-mode correlation in the extracted ensemble with a correlation coefficient matrix. Each element is defined by the correlation factor C_{ij} = Cov[u_i, u_j]/(σ(u_i)σ(u_j)) (u_i = {x_i, y_i}), where Cov[x, y] denotes the covariance between x and y, and σ_i(x) denotes the standard deviation of x. For instance, only self-correlation represented in the diagonal elements appears in the matrix without any conditioning. On the other hand, cross correlation represented in the off-diagonal elements appears with the condition in the phononic Schwinger angular momentum in the SU(2) group [Fig. 3(a)]. Note that the negative average was extracted with the condition O_j/max[O_j ] ≤ −η with a positive η. There totally exist eight types of correlation including the combination of the linear quadrature and the sign of the correlation (four residual correlations were obtained in angular momentum in the SU(1,1) group [see supplemental information]). Moreover, such correlated states show the reduction and amplification of the noise deviation along 45-degree and -45-degree axes in the phase space [Fig. 3(b)]. Increasing η decreases the squeezing level defined by the ratio of the standard deviation between the extracted ensemble and the ensemble without any conditioning [Fig. 3(c)]. The lower limit of the squeezing level reached -3 dB as the two-mode squeezing via parametric nonlinearity does [16, 17]. This means that the conditional measurement of a transverse component suppresses half of the two-mode noise in the phase space. Because the random dynamics of the mechanical modes is determined by a finite time constant, the two-mode squeezed state can survive in the conditional window with a finite time duration τ_w ≡ t_{out} − t_{in}, where t_{in} (t_{out}) is the time when the Schwinger angular momenta enters (leaves) the conditioned window [Fig. 3(d)]. The average of the time duration ⟨τ_w⟩ tells us how fast we should perform the operation by leveraging the squeezed states. Apparently, it exponentially decreases with increasing η [Fig. 3(e)] [19].

Further suppressing the deviation of the Schwinger angular momentum can improve the level of two-mode squeezing. We imposed the second condition, −ϵ ≤ Õ_j/max[Õ_j] ≤ ϵ, where Õ_j is the residual component of the SU(2) [or SU(1,1)] angular momentum, and ϵ is the positive parameter that determines the window for decreasing the appearance of the residual component. Here, we show the case where O_j = S_x and Õ_j = S_y. The squeezing level of the extracted states is improved to over -3 dB with decreasing ϵ [Fig. 4(a)]. There exists a trade-off between the squeezing level and the average of the survival-time duration ⟨τ_w⟩ with decreasing ϵ as well as η [Fig. 4(b)]. Note that the squeezing level is saturated as it approaches -6 dB because the deviation along S_z still exists, and it cannot be accessed in our scheme. Such a double-conditioning scheme can be readily extended to an arbitrary set of the two conditions for both the Schwinger angular momenta in the SU(2) and SU(1,1) groups. Although the other conditions enable us to extract the various ensembles, the squeezing level does not exceed -3 dB (see supplemental information).

In conclusion, we observed phononic Schwinger angular momenta in SU(2) and SU(1,1) groups between two mechanical modes by detecting nonlinear optical signals and performing a conditional measurement. This conditional measurement also enables us to extract twomode correlated (squeezed) states. The concept of Schwinger angular momenta is available for representing not only two-body system but also many-body ones with a higher-order symmetry (e.g., that in the SU(N) group [20]). Such high-dimensional angular momenta can be probed with state-of-the-art cavity nonlinear optomechanical systems [11, 12, 13] integrated with multimode mechanical structures [21, 22]. They open the way to the study of multipartite correlations in non-equilibrium many-body systems affected by various kind of heat baths [23, 24]. Furthermore, as in the scheme of continuous quantum measurement in a mechanical oscillator [25, 26], probing the phononic Schwinger angular momenta in a few-phonon regime could be an interesting challenge for the study of non-equilibrium thermodynamics with macroscopic quantum objects.

We thank Kensaku Chida, Yuichiro Matsuzaki, Tatsuro Hiraki, and Samer Houri for fruitful discussions. This work was partly supported by a MEXT Grant-in-Aid for Scientific Research on Innovative Areas (Grants No. JP15H05869).

FIG. 1. (a) and (b) Illustrations of spherical and pseudo-spherical (hyperboloid) space with vectors S and K of angular momentum in SU(2) and SU(1,1) groups. The typical rotational trajectories in the joint phase space with S = (S_x, 0, 0) and K = (K_x, 0, 0) are described with a real and imaginary angle, ϕ and iϕ, in their insets. (c) Schematic of the experimental setup at room temperature. A doubly-clamped mechanical beam was fabricated from a high tensile (0.2 GPa) silicon-nitride film deposited by thermal chemical vapor deposition (see SEM image). A probe light from He- Ne laser with a wavelength of 633 nm was modulated by an acousto-optic modulator (80 MHz) and detected by an optical heterodyne setup. The detected signals were divided by two: one was connected to a spectrum analyzer to directly measure the power spectral density, the other one was connected to four lock-in amplifiers. Both the linear quadrature and transverse components of phononic Schwinger angular momenta in the SU(2) and SU(1,1) groups were detected by the lock-in amplifiers with phase-synchronized references. Each quadrature was used to perform a conditional measurement. (d) Power spectral density (PSD) of the first-order, third-order, difference frequency, and sum frequency signals measured in the spectrum analyzer. The vertical unit was calibrated to the displacement (pm/ √ Hz) using the thermal motion of the first mechanical mode without random excitation. (e) Random trajectory (black vector) and distribution (black points) in the joint phase space spanned by x_1 and x_2.

FIG. 2. (a) Conceptual illustration of conditional measurement with the input of the linear quadrature of mechanical modes and transverse components of phononic Schwinger angular momenta. Two typical conditions with positive and negative η are depicted. (b) Success probability with respect to η for S_x (the red circles) and K_x (the blue diamonds). The error-bar shows the standard deviation for ten trials with the same condition. (c) and (d) Extracted trajectory (vectors) and distributions (points) with η = 0.3 for S_x and K_x, respectively. The discontinuous trajectories are described while the Schwinger angular momenta satisfy the condition.

FIG. 3. (a) Correlation coefficient matrices with conditional measurements when O_j = {S_x, S_y} and |η| = 0.2 in Schwinger angular momentum in SU(2) group. The absolute value and sign of the correlation coefficient are described by the color maps. (b) Density histogram of the extracted two-mode squeezed state in the joint phase space spanned by x_1 and y_2 with η = 0.2 for S_x. (c) Squeezing level with different η. The red, orange, green and blue plots show the noise reduction ratio along diagonal axes x_1 − y_2, y_1 + x_2, y_1 − x_2, and y_1 + x_2, respectively. The black dashed line corresponds to the squeezing level of -3 dB. (d) Schematic image of the survival-time duration. The red vectors describe the random motion projected to the space spanned by S_x and S_y. (e) Average of the survival time duration with respect to η. The numerical results show the good agreement with the experimental time duration. The purple and black plots corresponds to the experimental and numerical results. All error-bars were calculated as the standard deviation for ten trials.

FIG. 4. (a) Squeezing level with respect to η and three different ϵ with O_j = S_x and Õ_j = S_y. The red plots show the level with the single conditional measurement, and the blue and green plots show the case with ϵ = 0.2 and ϵ = 0.1. The blue-shaded area corresponds to the level over -3 B that is never obtained in the single conditioning. (b) Average of the survival-time duration (blue plots) and squeezing level (red plots) with η = 0.2 and different ϵ. All error-bars were calculated as the standard deviation for ten trials.

Supplemental Information: Optically probing Schwinger angular momenta in a micromechanical resonator

SCHWINGER ANGULAR MOMENTA BETWEEN TWO BOSONIC MODES

The components of Schwinger angular momenta S_i in SU(2) and K_i in SU(1,1) (i = x, y, z) are defined as quadratic forms of linear phase quadratures x_j and y_j (j = 1, 2) as follows: S_x =(x_2y_1 − y_2x_1)/2, (S1) S_y = − (x_2x_1 + y_1y_2)/2, (S2) S_z =(x^2 + y^2 − x^2_1 − y^2_1 )/4, (S3) K_x =(x_2y_1 + x_1y_2)/2, (S4) K_y =(x_2x_1 − y_2y_1)/2, (S5) K_z =(x^2 + y^2 + x^2_1 + y^2_1 )/4, (S6) Because x_i and y_i are canonical conjugate with each other, the algebra among the angular momenta can be examined by taking account of the Poisson bracket {A, B} ≡

∑_2 i=1 ∂A ∂x_i ∂B ∂y_i − ∂A ∂y_i ∂B ∂x_i . For Sx and Sy, we obtain the following cyclic algebra {S_x, S_y} = S_z , {S_y, S_z} = S_x , {S_z, S_x} = S_y, (S7) {K_x, K_y} = −K_z , {K_y, K_z} = K_x , {K_z, K_x} = K_y. (S8) The z components of SU(2) [SU(1,1)] angular momentum commute with the transverse components of SU(1,1) [SU(2)] angular momentum as {S_x, K_z} = {S_y, K_z} = {K_x, S_z} = {K_y, S_z} = 0. (S9) Moreover, the combination of S_i and K_j (i, j = x, y) is no longer closed in the algebra of angular momentum, such that {S_x, K_x} =(x_1y_1 − x_2y_2)/2 (S10) {S_x, K_y} = − (x^2_1 − y^2_1 − x^2 + y^2)/4 (S11) {S_y, K_x} = − (x^2_1 − y^2_1 + x^2 − y^2)/4. (S12) {S_y, K_y} = − (x_1y_1 + x_2y_2)/2 (S13) (S14)

The observables in the right-hand-side are achieved in the second harmonics of mechanical modes from the measurement nonlinearity (experimentally observed in [12]). All observables including the second harmonics and the Schwinger angular momenta constructs sp(4)-algebra, as discussed in [27]. Note that the quantization of these angular momenta immediately derives the commutation relationship including the Planck constant with the same algebra.

PHONONIC SCHWINGER ANGULAR MOMENTA IN DOPPLER EFFECT

The Doppler effect causes the frequency modulation of light with respect to the velocity of vibrational objects. Here, we consider that the light simultaneously probes two mechanical vibrations with different angular frequencies, Ω_1 and Ω_2, at finite temperature. In our heterodyne setup, the probe light a(t) is given by

a(t) = √ P e^{iΩAOMt} exp [i(β_1v_1(t) + β_2v_2(t))] + c.c. (S15)

where P is the probe power, Ω_{AOM} is the angular frequency shifted by the acousto-optic modulator, and β_i and v_i are the modulation index and the vibrational velocity of ith mechanical mode. The velocity driven by random force is represented by v_i(t) = x_i cos Ω_it + y_i sin Ω_it, where Ω_i is the angular frequency, x_i(t) and y_i(t) are orthogonal linear quadratures. Using Jacobi-Anger expansion, we obtain

a(t) = √ P e^{iΩAOMt} ∑ k ∑ l ∑ m ∑ n i^{(k+l)}J_k (β_1x_1) J_l (β_2x_2)

J_m (β_1y_1) J_n (β_2y_2) e^{i((k+m)Ω1 +(l+n)Ω2)t} + c.c., (S16)

where J_m(x) is the mth order Bessel function of the first kind. This can be expanded in terms of optical sideband frequencies (including the difference frequency Ω_D ≡ Ω_2 − Ω_1 and sum frequency Ω_S ≡ Ω_2 + Ω_1) as follows:

a(t) = √ P [ a_0(t) + a_{ΩAOM±Ω1} (t) + a_{ΩAOM±Ω2} (t)

+ a_{ΩAOM±ΩD} (t) + a_{ΩAOM±ΩS} (t) + . . . ] (S17) where each term is given by

a_{ΩAOM±Ωi} (t) =β_ix_i(t) sin [(Ω_{AOM} ± Ω_i)t] ± β_iy_i(t) cos [(Ω_{AOM} ± Ω_i)t] (S18) a_{ΩAOM±ΩD} (t) = ± β_1β_2S_x(t) sin [(Ω_{AOM} ± Ω_D)t] + β_1β_2S_y(t) cos [(Ω_{AOM} ± Ω_D)t] (S19) a_{ΩAOM±ΩS} (t) = ∓ β_1β_2K_x(t) sin [(Ω_{AOM} ± Ω_S )t] − β_1β_2K_y(t) cos [(Ω_{AOM} ± Ω_S )t] . (S20)

Here, we assume that β_ix_i ≪ 1 and β_iy_i ≪ 1 for approximating the Bessel function as J_q(z) ≈ (z/2)^q/q!. Obviously, the difference (sum) frequency signal contains the transverse components of phononic Schwinger angular momentum in the SU(2) [SU(1,1)] group.

SIGNAL LEVEL FOR PHONONIC SCHWINGER ANGULAR MOMENTA

To discuss the signal level of phononic Schwinger angular momenta, we introduce the power spectral density, which is defined by the Fourier transform of the statistical average, ⟨z(t)z(0)⟩, of thermal noise at the mechanical frequency:

S_{vi} (Ω_i) = √ 2k_BT m_iΓ_i = 2 √ n_iQ_iΩ_ix^{zp}_i (i = 1, 2) (S21)

with a unit of (m/s)/ √ Hz where k_B is the Boltzmann factor, T is the temperature, and m_i, Γ_i, n_i, Q_i, and x^{zp}_i are the effective mass, linewidth, number of thermal phonons, quality factor, and zero-point fluctuation of mechanical displacement of the ith mechanical mode, respectively. In the same manner, the sensitivity of O_j = {S_x, S_y, K_x, K_y} is represented by

S_{Oj} (Ω_i) = √ 2(k_BT )^2 m_1m_2Ω^2_1Ω^2(Γ_1 + Γ_2) = 2 √ 2 √ n_1n_2Q_1Q_2Ω^2_1Ω^2 Ω_1Q_2 + Ω_2Q_1 x^{zp}_1 x^{zp}_2 (i = D, S) (S22)

with a unit of (m/s)^2/ √ Hz. Here, we assume that ⟨x_i(t)x_i(0)y_i(t)y_i(0)⟩ = ⟨x_i(t)x_i(0)⟩⟨y_i(t)y_i(0)⟩.

Because the modulation index in the Doppler effect is represented by β_i = 2π/(λ_LΩ_i), where λ_L is the wavelength of the probe light, the power spectral densities of measured photocur-

TABLE I. Parameters for power spectral density Symbol Value Unit Ω_1 2π × 0.52 MHz Ω_2 2π × 1.74 MHz x^{ZP}_1 5.6 fm x^{ZP}_2 2.9 fm Q_1, Q_2 3.0 × 10^4 λ_L 632.8 nm

rent for linear and nonlinear terms are given by

I_L(Ω_i) =4πξ_Dx^{zp}_i √ P P_Ln_iQ_i Ω_iλ^2_L

(i = 1, 2) (S23)

I_{NL}(Ω_i) =8 √ 2π^2ξ_Dx^{zp}_1 x^{zp}_2 √ P P_Ln_1n_2Q_1Q_2 (Ω_1Q_2 + Ω_2Q_1)λ^4_L

(i = D, S) (S24)

where P_L is the power of the local oscillator, ξ_D is the factor of opto-electric conversion in the photodetector. To discuss the signal-to-noise ratio for nonlinear signals, the nonlinear power spectral density S̃_{Oj} (Ω_i) converted as the unit of (m/s)/ √ Hz is defined by S̃_{Oj} (Ω_i) ≡I^{NL}(Ω^i) I_L(Ω_1)

S_1(Ω_1). (S25)

In our experiment, the noise floor level in the Doppler interferometer was estimated to 1.4 pm/ √ Hz. This value was calibrated by a thermal noise spectrum at room temperature in the first mechanical mode. The nonlinear signals were obtained when the effective temperature T_{eff} ≡ n_1ℏΩ_1/(k_BT ) ∼ 10^6 with the artificial noise amplitude V_{noise} ∼ 2 V. The experimental power spectral density shows good agreement with the theoretical value [Fig. S1(a)] calculated with the parameters in Table I. Mechanical resonators with a high Q factor and small effective mass enable us to observe the Schwinger angular momenta at room temperature without any artificial noise [Fig. S1(b)]. For instance, mechanical resonators with two-dimensional materials [28, 29] and nanowire mechanical resonators [30, 31] have extremely small effective mass, and silicon-nitride resonators with a phononic shield [32, 33] show Q > 10^6. They will be good candidates for observing and engineering phononic Schwinger angular momenta.

FIG. S1. (a) Power spectral density of the first mechanical modes (red circle) and the sum and difference frequency signals (blue circle: sum frequency signal, and blue square: difference frequency signal). The red and blue lines show the theoretically calculated values with the parameters in Table I. The effective temperature T_{eff} is calibrated with the first mechanical modes. The yellowshaded area corresponds to V_{noise} = 2 V, at which we performed all experiments shown in the main text. The black dashed line shows the noise floor level in the Doppler interferometer. (b) Density color plots of the converted nonlinear power spectral density as a function of mechanical Q factor and effective mass at room temperature (300 K). The white point is the parameter in our experiment.

ROTATIONAL TRAJECTORY WITH A FINITE DETUNING

The dynamics of two-mode mechanical system in a rotational reference frame is represented by the Hamiltonian H = ∑ i δ_i(x^2_i + y^2_i )/2, where δ_i is a detuning between the frequency of the reference frame and resonance of the ith mode. By taking into account the random mechanical force, the linear quadratures follow the Langevin equations

ẋ_i = − γ_i 2 x_i + δ_i 2 y_i + √ γ_ix_{th,i} (S26)

ẏ_i = − γ_i 2 y_i − δ_i 2 x_i + √ γ_iy_{th,i} (S27) (S28)

where γ_i is the damping factor and ξ_{th,i} (ξ = x, y) is the random fluctuation with ⟨ξ_{th,i}(t)ξ_{th,i}(t^′)⟩ = 4k_BT_{eff} δ(t − t^′).

Rotational trajectory in the joint phase space is specified by an angular momentum defined by the vector product of coordinates and their velocity fields (momentum). To discuss the detuning dependence of the rotational trajectory, here we define statistical averages of rotational angular momenta S ≡ ⟨ẋ_2x_1 − ẋ_1x_2⟩_η and K ≡ ⟨ẋ_2x_1 + ẋ_1x_2⟩_η, where ⟨·⟩_η denotes the ensemble average with the conditional measurement with η. S quantifies the rotational trajectory with a real angle, and K does so with a imaginary angle. By considering the conditional measurement with S_x and K_x (i.e. ⟨S_y⟩_η = ⟨K_y⟩_η = 0) and substituting the Langevin equations into the definition of the rotational angular momenta, we obtain relationships

S = − δ_2 + δ_1 2 ⟨S_x⟩_η + δ_2 − δ_1 2 ⟨K_x⟩_η, (S29) K = δ_2 + δ_1 2 ⟨K_x⟩_η − δ_2 − δ_1 2 ⟨S_x⟩. (S30)

A finite detuning crucially determines the rotational trajectory with respect to the conditional average of Schwinger angular momenta. In the case where δ = δ_1 = δ_2, the rotational trajectory with a real (imaginary) angle is determined by the phononic Schwinger angular momentum in the SU(2) [SU(1,1)] group. This corresponds to the fact that the phonoinc Schwinger angular momentum in the SU(2) [SU(1,1)] group is a generator of rotation with a real (imaginary) angle. S and K obtained in numerical simulation of the Langevin equation with γ = γ_1 = γ_2 shows good agreements with their dependence proportional to δ/γ (see Fig. S2). On the other hand, in the case where δ = δ_1 = −δ_2, there exists the opposite relationships, S ∝ K_x and K ∝ S_x. This reference frame effectively makes a partial timereversal operation which reverses the time evolution only in the second mechanical mode (i.e., y_2 → −y_2). Because this operation swaps the function of K_x and S_x, the rotational trajectory with a real (imaginary) angle is extracted via the conditional measurement of K_x (S_x).

CONDITIONAL MEASUREMENT WITH THE OTHER COMPONENTS OF ANGULAR MOMENTA

Here, we show the results of the conditional measurement of S_y and K_x, which corresponds to the real and imaginary rotation in the phase space spanned by x_1 and y_2 [Fig. S1(a) and (b)]. Moreover, the correlation coefficient matrix in the conditional measurement of SU(1,1) Schwinger angular momenta also contains the non-diagonal elements as the case of angular momenta in the SU(2) group do [Fig. S1(c)].

FIG. S2. (a) and (b) Rotational angular momenta S and K calculated with results of numerical simulation of Langevin equations with δ = δ_1 = δ_2. The square plots show rotational angular momentum with η = 0.3 in the condition O_j /max[O_j ] ≥ η, and the circle plots show that with η = −0.3 in the condition O_j/max[O_j ] ≤ η where O_j = {S_x, K_x}. The error-bars represent the standard deviation for ten trials. All numerical results fitted to linear functions (shown by the dashed lines) show good agreement with the analytical expressions (S29) and (S30).

CONDITIONAL MEASUREMENT WITH THE OTHER DOUBLE CONDI- TIONS

By fixing the first condition S_x/max[S_x] ≤ 0.2, the squeezed conditional distribution with respect to the angular momenta for the second conditions, S_y, K_x, and K_y are compared with ϵ = 0.1 [Fig. S2(a)-(c)]. Obviously, the multi-modal non-Gaussian distribution appears by conditioning the angular momenta in the SU(1,1) group while the first condition is selected from the angular momentum in the SU(2) group (S_x). The squeezed levels along the x_1 − y_2 axis are −4.5 ± 0.4, −3.0 ± 0.4, and −3.0 ± 0.3 dB in the second condition with S_y, K_x, and K_y, respectively. Note that the rotational trajectory in the phase space spanned by x_1 and x_2 also shows the multi-modal distribution in the case of K_x and K_y [Fig. S2(d)-(f)].

FIG. S3. (a) and (b) Extracted trajectory (vectors) and distributions (points) with η = 0.3 for S_y and K_y, respectively. The discontinuous trajectories are described while the Schwinger angular momenta satisfy the condition. (c) Correlation coefficient matrix with conditional measurement when O_j = {K_x, K_y} and |η| = 0.2 in SU(1,1) Schwinger angular momentum. The value including the sign of the correlation coefficient is described by the color maps.

FIG. S4. (a), (b), and (c) Density histograms of the extracted two-mode thermal squeezed state with the double conditioning in S_y, K_x, and K_y. (d), (e), and (f) Conditioned distributions and trajectories extracted by the second conditions in S_y, K_x and K_y, respectively. The trajectories (vector) are described while the Schwinger angular momenta satisfy each condition.

[1] J. Schwinger, in: L. C. Biedenharn, H. van Dam (Eds.), Academic, New York, pp. 229?279, (1965).

[2] A. G. White, D. F. V. James, P. H. Eberhard, and P. G. Kwiat, Phys. Rev. Lett. 83, 3103 (1999).

[3] J. Řeháček, B.-G. Englert, and D. Kaszlikowski, Phys. Rev. A 70, 052321 (2004). [4] B. Yurke, S. L. McCall, and J. R. Klauder, Phys. Rev. A 33, 4033 (1986). [5] H. Nha, and J. Kim, Phys. Rev. A 74, 012317 (2006). [6] G. G. Stokes. Trans. Cambridge Phil. Soc. 9, 399?416 (1852).

[7] G. Milione, H. I. Sztul, D. A. Nolan, and R. R. Alfano, Phys. Rev. Lett. 107, 053601 (2011). [8] W. P. Bowen, R. Schnabel, H-A. Bachor, and P. K. Lam, Phys. Rev. Lett. 88, 093601 (2002). [9] M. Lassen, G. Leuchs, and U. L. Andersen, Phys. Rev. Lett. 102, 163602 (2009). [10] D. Li, B. T. Gard, Y. Gao, C-H. Yuan, W. Zhang, H. Lee, and J. P. Dowling, Phys. Rev. A 94, 063840 (2016).

[11] J. C. Sankey, C. Yang, B. M. Zwickl, A. M. Jayich, and J. G. E. Harris, Nat. Phys. 6, 707 (2010).

[12] G. A. Brawley, M. R. Vanner, P. E. Larsen, S. Schmid, A. Boisen, and W. P. Bowen, Nat.

Commun. 7, 10988 (2016).

[13] R. Leijssen, G. R. La Gala, L. Freisem, J. T. Muhonen, and E. Verhagen, Nat. Commun. 8, 16024 (2017).

[14] H. Okamoto, A. Gourgout, C-Y Chang, K. Onomitsu, I. Mahboob, E. Y. Chang, and H.

Yamaguchi , Nat. Phys. 9, 480 (2013).

[15] T. Faust, J. Rieger, M. J. Seitner, J. P. Kotthous, and E. M. Weig, Nat. Phys. 9, 485 (2013). [16] I. Mahboob, H. Okamoto, K. Onomitsu, and H. Yamaguchi , Phys. Rev. Lett. 113, 167203 (2014).

[17] A. Pontin, M. Bonaldi, A. Borrielli, L. Marconi, F. Marino, G. Pandraud, G.?A. Prodi, P.?M.

Sarro, E. Serra, and F. Marin, Phys. Rev. Lett. 116, 103601 (2016).

[18] R. B. Karabalin, M. H. Matheny, X. L. Feng, E. Defaÿ, G. L. Rhun, C. Marcoux, S. Hentz, P. Andreucci, and M. L. Roukes, Appl. Phys. Lett. 95, 103111 (2009).

[19] Although ⟨τ_w(η)⟩ (here we explicitly denote it as the function of η) defines a simple time-scale for our state preparation scheme, it is not suitable to stably prepare the squeezed states with squeezing level ξ_{sq}(η) because of the large deviation, σ(τ_w(η)) ∼ ⟨τ_w(η)⟩. To efficiently use the two-mode thermal squeezed states for sensing or interferometry, we have to set τ_w(η̃) so that the trajectory enters the deeper conditional window spanned by η̃ > η with respect to the expected squeezing level ξ_{sq}(η).

[20] M. Mathur, I. Raychowdhury, and R. Anishetty, J. Math. Phys. (N.Y.) 51, 093504 (2010) [21] I. Mahboob, M. Mounaix, K. Nishiguchi, A. Fujiwara, and H. Yamaguchi , Sci. Rep. 4, 4448 (2014).

[22] W. Hvidtfelt P. Nielsen, Y. Tsaturyan, C. B. Moller, E. S. Polzik, A. Schliesser, Proc. Natl.

Acad. Sci. 114, 62 (2017).

[23] S. Gröblacher, A. Trubarov, N. Prigge, G. D. Cole, M. Aspelmeyer, and J. Eisert, Nat.

Commun. 6, 7606 (2015).

[24] J. Klaers, S. Faelt, A. Imamoglu, and E. Togan, Phys. Rev. X 7, 031044 (2017). [25] K. Jacobs, L. Tian, and J. Finn, Phys. Rev. Lett. 102, 057208 (2009). [26] M. R. Vanner, Phys. Rev. X 1, 021011 (2011). [27] A. Vourdas, Phys. Rev. A 46, 442 (1992).

[28] J. S. Bunch, A. M. van der Zande, S. S. Verbridge, I. W. Frank, D. M. Tanenbaum, J. M.

Parpia, H. G. Craighead, P. L. McEuen, Science 315, 490 (2007).

[29] M. Will, M. Hamer, M. Moller, A. Noury, P. Weber, A. Bachtold, R. V. Gorbachev, C.

Stampfer, and J. Gttinger, Nano Lett. 17, 5950 (2017).

[30] R. He, X. L. Feng, M. L. Roukes, and P. Yang, Nano Lett. 8, 1756 (2008). [31] T. S. Abhilash, J. P. Mathew, S. Sengupta, M. R. Gokhale, A. Bhattacharya, and M. M.

Deshmukh, Nano Lett. 12, 6432 (2012).

[32] Y. Tsaturyan, A. Barg, E. S. Polzik, and A. Schliesser, Nat. Nanotech. 12, 776 (2017). [33] A. H. Ghadimi, S. A. Fedorov, N. J. Engelsen, M. J. Bereyhi, R. Schilling, D. J. Wilson, and T. J. Kippenberg, Science 360, 764 (2018).