arXiv:1909.08524v1 [physics.atom-ph] 18 Sep 2019

Proceedings of the Eighth Meeting on CPT and Lorentz Symmetry (CPT’19), Indiana University, Bloomington, May 12–16, 2019

1

Matter Wave Interferometry for Inertial Sensing and Tests of Fundamental Physics

D. Schlippert,^1 C. Meiners,^1 R.J. Rengelink,^1 C. Schubert,^1 D. Tell,^1 É. Wodey,^1 K.H. Zipfel,^1 W. Ertmer,^1 and E.M. Rasel^1

1Institut für Quantenoptik, Leibniz Universität Hannover, Welfengarten 1, 30167 Hannover, Germany

Very Long Baseline Atom Interferometry (VLBAI) corresponds to groundbased atomic matter-wave interferometry on large scales in space and time, letting the atomic wave functions interfere after free evolution times of several seconds or wave packet separation at the scale of meters. As inertial sensors, e.g., accelerometers, these devices take advantage of the quadratic scaling of the leading order phase shift with the free evolution time to enhance their sensitivity, giving rise to compelling experiments. With shot noise-limited instabilities better than 1 × 10^{−9} m/s^2 at 1 s at the horizon, VLBAI may compete with state-of-the-art superconducting gravimeters, while providing absolute instead of relative measurements. When operated with several atomic states, isotopes, or species simultaneously, tests of the universality of free fall at a level of parts in 10^{13} and beyond are in reach. Finally, the large spatial extent of the interferometer allows one to probe the limits of coherence at macroscopic scales as well as the interplay of quantum mechanics and gravity. We report on the status of the VLBAI facility, its key features, and future prospects in fundamental science.

1. Introduction

Nearly half a century after the seminal observation of gravity-induced phase shifts on matter waves,^1 coherent control in atom interferometers is now a standard technique used around the world to perform inertial measurements^2, determine fundamental constants,^{3,4} and to test the laws of fundamental physics.^5 At a given phase noise the intrinsic sensitivity of an atom accelerometer in the common Mach-Zehnder-type configuration^6 scales with the leading order phase shift,

Δϕ = ⃗k_{eff} · ⃗a T^2 (1)

where ℏ⃗k_{eff} is the momentum transferred during atom-light interaction, ⃗a is the acting acceleration, and 2T is the wave packets’ free evolution time. One can therefore increase the scale factor of the instrument k_{eff}T^2 by exploiting

Proceedings of the Eighth Meeting on CPT and Lorentz Symmetry (CPT’19), Indiana University, Bloomington, May 12–16, 2019

2 its linear scaling in atomic recoil ℏk_{eff} but also the quadratic dependency on the free evolution time T . To that end, besides initiatives for operation in microgravity,^{7–9} increasing the free fall distance of ground-based devices towards long free fall tubes is a path pursued by groups around the world.^{10,11} Indeed, combined with an exquisite control over external fields and other deteriorating effects, extending the baseline of gravimeters from tens of centimeters to several meters opens the way for competition with state of the art superconducting gravimeters or quantum tests of the universality of free fall (UFF) at an unprecedented level,^{12} competitive with those achieved by the best classical methods.^{13–15} In these proceedings we report on the status and key features of the Very Long Baseline Atom Interferometry (VLBAI) facility implemented in the Hannover Institute of Technology (HITec) of Leibniz Universität Hannover.

2. The VLBAI facility

2.1. Design

The VLBAI facility in Hannover is currently in its final stage of construction and consists of three main components:

(1) At the heart of the device is a 10 m long, vertically oriented ultrahigh vacuum tube with a 10 cm diameter in clearance for the atom optics light fields. In order to shield the experiment from magnetic stray fields mimicking inertial forces, the tube is enclosed in a highperformance dual layer magnetic shield reducing magnetic field gradients below 10 nT/m. Additionally, the full baseline is equipped with a network of temperature probes for detecting and subsequently correcting errors due to temperature gradients.^{16} (2) Both ends of the vacuum tube will be equipped with dual-species sources^a providing the operator with (near-)quantum degenerate ensembles of stable bosonic and fermionic ytterbium isotopes as well as 87Rb.^{12} Making use of hybrid magnetic and optical trapping techniques as well as delta-kick collimation,^{17} we anticipate an atom flux on the order of 10^6 at/s with temperatures in the picokelvin regime.^{18} (3) For absolute measurements, we will utilize a seismic attenuation system (SAS) to suspend a retro reflection mirror that serves as the atom interferometer’s inertial reference. Based on geometric anti-springs,^{19}

aAs such, the facility can be operated either in drop mode (2 T = 0.8 s) or with atoms being launched (2 T = 2.8 s).

Proceedings of the Eighth Meeting on CPT and Lorentz Symmetry (CPT’19), Indiana University, Bloomington, May 12–16, 2019

3 our SAS features a passive resonance frequency of hundreds of millihertz and provides means of 6-degrees-of-freedom active stabilization via electromagnetic actuation using the signals of on-board broadband seismometers as well as novel opto-mechanical devices.^{20}

The VLBAI facility aims to use rubidium, which is well-established as a standard choice for inertial sensors using readily available source and laser technology, as well as the heavy lanthanide ytterbium which offers its own benefits. Indeed, as an effective two-electron system it has broad lines to apply strong cooling forces, as well as narrow intercombination transitions with a low Doppler-limit. Furthermore, the bosonic isotopes all share the property of having a vanishing first order magnetic susceptibility, making systematic effects and environmental decoherence mechanisms easier to control. Finally, the internal composition of our species offers enhanced sensitivity when searching for new physics beyond the standard model.^{21,22}

2.2. Performance estimation

With the SAS and the magnetic shield tackling the dominant external noise sources, we expect an improvement in absolute gravimetry beyond the state of the art. The performance of the device will however ultimately be limited by quantum projection, i.e., shot noise. In a simple drop configuration with 2 × 10^5 at per cycle, 3 s preparation time, and a free evolution time 2T = 800 ms, the shot noise-limited sensitivity of the VLBAI facility is 1.7 nm s^{−2} at 1 s. In a more advanced configuration, launching 1 × 10^6 at per cycle to reach a free evolution time of 2T = 2.8 s and using 4-photon atom optics yields a shot noise-limited acceleration sensitivity of 40 pm s^{−2} at 1 s. For a gradiometric configuration^{3,23} with a baseline L = 5 m between the two atom interferometers with 1 × 10^5 at per cycle, 3 s preparation time, and 2T = 800 ms, the shot noise-limited sensitivity is 5 × 10^{−10} s^{−1} at 1 s.

A simultaneous comparison measurement with^{87}Rb and^{170}Yb has the perspective for testing the UFF^{12} by determining the Eötvös ratio between the two species to better than one part in 10^{13}.

2.3. Fundamental physics

Beyond these metrological goals, the apparatus will also serve as a test bed for interferometry with very large scale factors as necessary for gravitational wave detection^{23} and is intrinsically sensitive to fundamental decoherence mechanisms^{24} and limitations of the quantum superposition principle.^{25}

Proceedings of the Eighth Meeting on CPT and Lorentz Symmetry (CPT’19), Indiana University, Bloomington, May 12–16, 2019

4 3. Conclusion & Outlook

The VLBAI facility will enable highly sensitive absolute gravimetry and tests of the Universality of Free Fall. It therefore offers a world-wide unique environment, both for cutting edge inertial sensing and to test our understanding of General Relativity, quantum mechanics and their interplay, possibly leading to a future reconciliation of the two.^{12}

Acknowledgments

This project is supported through the CRCs 1128 “geo-Q”, 1227 “DQmat”, “Niedersächsisches Vorab” in the “Quantum- and Nano-Metrology (QUANOMET)” initiative. D.S. gratefully acknowledges funding by the Federal Ministry of Education and Research (BMBF) through the funding program Photonics Research Germany under contract number 13N14875.

References 1. R. Colella et al., Phys. Rev. Lett. 34, 1472 (1975). 2. A. Peters, K.Y. Chung, and S. Chu, Nature 400, 849 (1999). 3. G. Rosi et al., Nature 510, 518 (2014). 4. R.H. Parker et al., Science 360, 191 (2018).

5. M. Jaffe et al., Nat. Phys. 13, 938 (2017); D.O. Sabulsky et al., Phys. Rev.

Lett. 123, 061102 (2019).

6. M. Kasevich and S. Chu, Phys. Rev. Lett. 67, 181 (1991). 7. D.N. Aguilera et al., Classical Quant. Grav. 31, 115010 (2014). 8. D. Becker et al., Nature 562, 391 (2018).

9. L. Wörner et al., In: Proceedings of International Astronautic Congress 2018, IAC-18,A2,1,13,x45004 (2018).

10. C. Overstreet et al., Phys. Rev. Lett. 120, 183604 (2018) 11. L. Zhou et al., Gen. Relativ. Gravit. 43, 1931 (2011). 12. J. Hartwig et al., New J. Phys. 17, 035011 (2015). 13. P. Touboul et al., Phys. Rev. Lett. 119, 231101 (2017). 14. F. Hofmann and J. Müller, Classical Quant. Grav. 35, 035015 (2018). 15. S. Schlamminger et al., Phys. Rev. Lett. 100, 041101 (2008). 16. P. Haslinger et al., Nat. Phys. 14, 1745 (2017). 17. H. Müntinga et al., Phys. Rev. Lett. 110, 093602 (2013). 18. S. Loriani et al., New J. Phys. 21, 063030 (2019). 19. A. Bertolini et al., Nucl. Instrum. Meth. A 435, 475 (1999). 20. L.L. Richardson et al., arXiv:1902.02867.

21. M.A. Hohensee et al., Phys. Rev. Lett. 111, 151102 (2013). 22. V.A. Kostelecký and J.D. Tasson, Phys. Rev. D 83, 016013 (2011). 23. S. Dimopoulos et al., Phys. Rev. D 78, 122002 (2008). 24. A. Bassi et al., Class. Quantum Grav. 34, 193002 (2017). 25. T. Kovachy et al., Nature 528, 530 (2015).