arXiv:2010.05136v1 [cond-mat.mes-hall] 11 Oct 2020

Theory of Transport in Ferroelectric Capacitors

Gerrit E. W. Bauer^{1−5,∗} and Ryo Iguchi^3 and Ken-ichi Uchida^{2−4} 1WPI-AIMR, Tohoku University, Sendai 980-8577, Japan 2Institute for Materials Research,Tohoku University, Sendai 980-8577, Japan 3National Institute for Materials Science, Tsukuba 305-0047, Japan 4Center for Spintronics Research Network, Tohoku University, Sendai 980-8577, Japan and 5Zernike Institute for Advanced Materials, Groningen University, Netherlands (Dated: October 13, 2020)

We present a time-dependent diffusion theory for heat and polarization transport in a planar ferroelectric capacitor with parameters derived from a one-dimensional phonon model. We predict steady-state Seebeck and transient Peltier effects.

Magnetism and ferroelectricity are caused by the spontaneous ordering of magnetic and electric dipoles, respectively, and have much in common [1]. Electro- and magnetocaloric phenomena are similar entropic effects caused by a transient non-equilibrium in the electric and magnetic dipole ensembles [2]. Transport phenomena attracted more attention in magnetic structures [3, 4]. In ferroelectrics, a thermopolarization [5–7] and dielectric Peltier effect [8, 9] have been reported, but the associated theory inappropriately mixes caloric and transport (or caloritronic) phenomena.

Here we formulate a linear-response theory of transport in electrically insulating ordered ferroelectrics (FE) for the most basic device, i.e. a slab of a FE between metallic contacts. We solve the diffusion problem with emphasis on the time response to an abrupt perturbation. A microscopic theory of polarization and heat currents based on a one-dimensional phonon model for a displacive FE leads to numerical parameter estimates. The analogies and differences with magnon transport are illuminating [10, 11].

Linear response - We consider a FE with metal contacts in a planar configuration with polarization density p (x) normal to the interfaces, which interacts with an electric field E(x) as H = − ∫ p (x) E (x) dx. (1) Temperature (∂T ) and electric field (∂E) gradients generate heat j_q and polarization j_p current densities. In the linear response regime, “currents” and “forces” are related by a matrix of material and device-dependent transport coefficients [12, 13]. The caloritronic relations can be summarized by a 2 × 2 linear response matrix ( j_p j_q ) = σ ( 1 S Π κ/σ ) ( ∂E −∂T ) , (2)

where σ (κ) is the polarization (thermal) conductivity with units m/Ω (W/m/K), while S (Π) is the ferroelectric Seebeck (Peltier) coefficient with units V/K/m (V/m). The dissipation rate ḟ = j_p∂E + j_q ∂T/T implies the Onsager-Kelvin relation Π = T S. For a mono-domain simple ferroelectric all transport coefficients should be positive.

The electrocaloric properties are governed by the temperature and field dependent thermal equilibrium polarization p_0 (E, T ) and heat/energy q_0 (E, T ) densities with susceptibilities χ_E = (∂p_0/∂E)_T and χ_T = (∂p_0/∂T )_E .

Metallic contacts efficiently screen the surface charges. When shorted, the electric field in the FE vanishes except for small corrections due to a finite screening length [15]. A constant applied voltage △V_{ext} generates an electric field E_{ext} = △V_{ext}/L, but since ∂E_{ext} = 0 there can be no DC Peltier effect. A temperature difference △T_{ext} between the contacts generates a gradient ∂T_{ext} = △T_{ext}/L. The polarization current into a metal contact is dissipated quickly without measurable effects. The principle observables are the electric field-induced Peltier heat current and the Seebeck thermovoltage over the contacts induced by a polarization change △V = − ∫ p − p_0 ϵ dx, (3) where ϵ is the dielectric constant.

Diffusion - The conservation relation for the FE polarization reads ∂j_p = −ṗ − p − p_0 τ (4) in terms of the relaxation time τ. A similar equation holds for the heat accumulation, but we assume from the outset that its relaxation is much faster than that of the polarization, so the local temperature instantaneously adapts to the external one. We also assume that thermalization of the non-equilibrium ferroelectric order can be modelled by an equilibrium distribution with a local temperature T_{ext} (x, t) and a non-equilibrium chemical potential μ (x, t) [10]. It is convenient to define μ_{tot} = μ−P E_{ext}, where P is the electric dipole of the unit cell such that the driving force in Eq. (2) E → −μ_{tot}/P. With p − p_0 = χ_E μ/P + χ_T (T − T_0) , we arrive at the diffusion equation for the non-equilibrium chemical potential ∂^2μ − 1 λ^2 μ = τ λ^2 ( μ̇_{tot} + P χ_T χ_E Ṫ_{ext} ) (5) with diffusion length λ = √ στ/χ_E . In frequency (ω) space ∂^2μ − μ λ̄2 = − iωτ λ^2

Ḟ_{ext} (x, ω) (6)

where F_{ext} = μ_{ext} + P χ_T T_{ext}/χ_E and λ^2/λ̄^2 = 1 − iωτ. For a capacitor with contacts at x_1 = 0, x_2 = L, using ∂^2F_{ext} = 0 and short diffusion lengths λ ≪ L, μ (x, ω) = A (ω) e^{−x/λ̄} + B (ω) e^{−(x−L)/λ̄} + iωτ 1 − iωτ F_{ext} (x, ω) , (7)

Interfaces - The boundary conditions to the contacts fix the integration constants A and B. The interface transport coefficients obey an Onsager relation similar to Eq. (2). Demanding continuity of the polarization current, the boundary conditions for the chemical potential are governed by an interface conductance G Gμ ( 0^+ ) = σ∂μ ( 0^+ ) ; Gμ ( L^− ) = −σ∂μ ( L^− ) . (8)

We focus below on two limiting cases. A good metal contact efficiently screens the polarization dynamics and suppresses the chemical potential at the interface. This is the transparent interface limit G ≫ σ/λ. The opposite limit of an opaque interface with G ≪ σ/λ represents, e.g., a contact with a thin non-FE spacer between FE and the metal.

Solutions - Close to the left interface μ (x, ω) = λ λG σ + √ 1 − iωτ + iωτ 1 − iωτ [ ∂F_{ext} (ω) − G σ F_{ext} (0, ω) ] (9) In the DC limit ω → 0

μ_{DC} (x) = λ λG σ + 1 e^{−x/λ}P S∂T_{ext} (10)

The thermovoltage generated by a temperature difference

△V_{DC} = − λ λG σ + 1 χ_E ϵ λ L S△T_{ext} (11)

is maximized for an opaque interface G/σ → 0. In a symmetric capacitor the contributions from both interfaces cancel, so the total △V_{DC} increases with the contrast of the interface conductances. The theoretically possible maximal thermovoltage in the weakly dissipative limit (L ≪ λ) for one transparent and one opaque interface is △V_{max} = −χ_E LS△T_{ext}/ (2ϵ) .

At finite frequencies the length and time scales λ and τ govern the dynamics. We consider the transients generated by switching on the external perturbation F_{ext} = F^{(Θ)}_{ext} Θ (t) , where Θ is the step function, on a time scale faster than τ. The Fourier transform back to the time domain can be obtained by contour integration.

For a transparent (left) interface we arrive at a transient accumulation in the FE caused by an electric field pulse of

μ (x, t > 0) = −e^{−t/τ} P E^{(Θ)}_{ext} erf ( 1 2 √ τ t x λ ) . (12)

We recover the pure electrocaloric term in the bulk of the FE μ (x ≫ λ, t > 0) = −e^{−t/τ} P E^{(Θ)}_{ext} , which dominates the observable thermovoltage. The polarization current in the absence of a temperature gradient is generated by the leakage of the electrocaloric accumulation into the contact, on the left side of the form j_p (x, t > 0) = σ √ τ πt e^{− tτ − τt} (^{x2λ} )^2

E^{(Θ)}_{ext} λ , (13)

while that for the right contact has the opposite sign. The associated Peltier heat current j_q = Πj_p cools the FE and heats the contacts or vice versa, with a possible interface contribution.

In the opaque interface limit

μ (x, t > 0) = P Sλ∂T^Θ_{ext} ( e^{−x/λ} − 1 2 [ e^{−x/λ}erfc (√ t τ − x 2λ √ τ t ) + e^{x/λ}erfc (√ t τ + x 2λ √ τ t )])

+ e^{−t/τ} [ −F^{(Θ)}_{ext} + P χ_T χ_E ∂T^{(Θ)}_{ext} ( x erf ( 1 2 √ τ t x λ ) + 2λ √ π √ t τ e^{− τEt} (^{x2λ} )^2 )] (14)

The polarization current vanishes at the interface x = 0, but

μ (0, t > 0) = P Sλ erf (√ t/τ ) ∂T^{(Θ)}_{ext} + e^{−t/τ} [ −F^{(Θ)}_{ext} (0) + P χ_T χ_E ∂T^{(Θ)}_{ext} 2λ √ π √ t τ ] (15)

We recognize a Seebeck contribution caused by the buildup of a polarization accumulation/depletion at the interface that approaches the DC limit Eq. (10) for long times. The second term is purely caloric but corrected by diffusion via the third term.

Phonon model - The caloritronic parameters σ and Π depend on the nature of the ferroelectricity and material, but their magnitude is not known. Here we derive estimates by a simple model of one-dimensional diatomic chains at temperatures below a displacive phase transition that generates a permanent electric dipole P = δQ in each unit cell, where δ is the deformation and Q the ionic charge. at finite temperature the polarization is affected by transverse phonons with maximum frequency ω_{op} = 2 √ C/M, where M is the ionic mass and C the force constant. We adopt the “ferron” approximation that the thermal fluctuations leave P invariant, but reduce its projection along the FE order. For high temperatures k_B T ≫ ℏω_{op} the Boltzmann equation for a constant scattering relaxation time τ_r ≪ τ then leads to a Peltier coefficient Π = J_q J_p | | |_{∂T =0} = Cδ^2 P , (16)

and the conductivities σ = τ_r Π^2 ω^2_{op} 8a k_B T, (17)

κ = σΠ^2/T, (18)

where a is the lattice constant. In this model, the electrocaloric properties also depend on the Peltier coefficient

χ_E = k_B T a^3Π^2

; χ_T = k_B a^3Π ( 1 − E Π ) . (19)

A stiffer material increases the heat relative to the polarization current, suppressing the calorics and enhancing caloritronics. The figure of merit ZT = (σ/κ) ( Π^2/T ) = 1 (20)

does not depend on the model parameters and temperature (even when k_B T ≯ ℏω_{op}).

Estimates - Room-temperature material constants close to barium titanate of ω_{op} = 5 THz, a = 0.4 nm, P = 2 × 10^{−29} Cm, δ = 0.03 nm, C = 25 J/m^2, τ_r = 1 ps, and τ = 1 ns lead to Π = 10 MV/cm, χ_E = 7 × 10^{−11} C/(Vm), χ_T = −2 × 10^{−4} C/(Km^2), κ = 4 W/(Km), σ = 10^{−15} m/Ω, and λ = 130 nm. With ϵ/ϵ_0 = 2000 in terms of the vacuum dielectric constant ϵ_0 the predicted DC thermovoltage induced by a temperature gradient of ∂T = 10 K/μm at an opaque interface is △V = 2 mV. The integrated heat flow through a transparent interface ∫ j_p (0, t) dt excited by an electric field pulse of E^{(Θ)}_{ext} = 1 MV/cm is 9 J/m^2. Because of the uncertainties in the parameters and simplicity of the model these numbers should be taken with a grain of salt.

Summary - We predict caloritronic effects in planar capacitors filled with an electrically insulating ferroelectric that may interfere with normal operation or used for energy applications.

Acknowledgments - The authors thank T. Teranishi, J. Kano, K. Yamamoto, and W. Yu for valuable discussions. G.B. is supported by JSPS KAKENHI Grant No. 19H00645. R.I. and K.U. are supported by JSPS KAK- ENHI Grant No. 20H02609, JST CREST “Creation of Innovative Core Technologies for Nano-enabled Thermal Management” Grant No. JPMJCR17I1, and the Canon Foundation.

∗ g.e.w.bauer@imr.tohoku.ac.jp [1] N. A. Spaldin, Topics Appl. Phys. 105, 175 (2007). [2] S. Crossley, N. D. Mathur, and X. Moya, AIP Advances 5, 067153 (2015).

[3] G.E.W. Bauer, E. Saitoh, and B. van Wees, Nat. Mat.

11, 391 (2011).

[4] C.H. Back, G.E.W. Bauer, and B.L. Zink, J. Phys. D 52 230301 (2019).

[5] M. Marvan, Czech. J. Phys. B, 19, 1240 (1969). [6] V.L. Gurevich and A. K. Tagantsev, Pis’ma Zh. Eksp.

Teor. Fiz. 35, 106 (1982) [JETP Lett. 35,128 (1982)]. [7] V. A. Trepakov, M. Nurievak, and Tagantseav, Ferroelectrics 94, 377 (1989).

[8] A. K. Tagantsev, Usp. Fiz. Nauk 152, 423 (1987) [Sov.

Phys.—Usp. 30, 588 (1987)].

[9] V. A. Trepakov, T. Raftkov, M. Marvan, L. Jastrabik, and P. Divin, Europhys. Lett. 21, 891 (1993).

[10] L.J. Cornelissen, K.J.H. Peters, G.E.W. Bauer, R.A.

Duine, and B.J. van Wees, Phys. Rev. B 94. 014412 (2016) [11] B. Flebus, K. Shen, T. Kikkawa, K. Uchida, Z. Qiu, E.

Saitoh, R.A. Duine, and G. E. W. Bauer, Phys. Rev. B 95, 144420 (2017).

[12] S. R. de Groot, Thermodynamics of Irreversible Processes, (North-Holland Publ., 1963) [13] L. D. Landau and E.M. Lifshitz, Statistical Physics, Part 1 (Oxford, UK: Butterworth-Heinemann, 1975).

[14] P. Chandra and P. B. Littlewood, Topics Appl. Physics 105, 69 (2007).

[15] R. R. Mehta, B. D. Silverman, and J. T. Jacobs, J. Appl.

Phys. 44, 3379 (1973).