arXiv:2104.07432v1 [cs.IT] 15 Apr 2021

On the existence of quaternary Hermitian LCD codes with Hermitian dual distance 1

Keita Ishizuka^∗, Ken Saito^†

Abstract

For k ≥ 2 and a positive integer d_0, we show that if there exists no quaternary Hermitian linear complementary dual [n, k, d] code with d ≥ d_0 and Hermitian dual distance greater than or equal to 2, then there exists no quaternary Hermitian linear complementary dual [n, k, d] code with d ≥ d_0 and Hermitian dual distance 1. As a consequence, we generalize a result by Araya, Harada and Saito on the nonexistence of some quaternary Hermitian linear complementary dual codes.

Keywords. Linear code, Linear complementary dual code, Hermitian linear complementary dual code. 2010 AMS Classification. 94B05

1 Introduction

Let F_q be the finite field of order q, where q is a prime power. Let F^n_q be the vector space of all n-tuples over F_q and let x = (x_1, x_2, . . . , x_n) be a vector of F^n_q . The Hamming weight of x is defined as wt(x) = #{i | x_i ≠ 0}. In this note, we are concerned only with linear codes. Thus we omit the term “linear” and simply write “code”. A k-dimensional subspace C of F^n_q is said to be an [n, k] code over F_q . The parameters n, k are said to be the length, dimension of C respectively. A vector of C is said to be a codeword of C. The codes over F_2 , F_3 , F_4 are said to be the binary, ternary, quaternary codes respectively. Let C be an [n, k] code over F_q and let 0_n be the zero vector of F^n_q . The minimum weight of C is defined as d(C) = min{wt(x) | x ∈ C, x ≠ 0_n}. If the minimum weight of C equals to d, then C is said to be an [n, k, d] code over F_q .

∗Corresponding author. Research Center for Pure and Applied Mathematics Graduate School of Information Sciences, Tohoku University, Sendai 980–8579, Japan. email:

keita.ishizuka.p5@dc.tohoku.ac.jp

†Research Center for Pure and Applied Mathematics Graduate School of Information Sciences, Tohoku University, Sendai 980–8579, Japan. email:

kensaito@ims.is.tohoku.ac.jp

Let x = (x_1, x_2, . . . , x_n), y = (y_1, y_2, . . . , y_n) ∈ F^n_q . For F^n_q , the Euclidean inner product is defined as (x, y) = ∑_n i=1 x_iy_i. The Euclidean dual code C^⊥ of an [n, k] code C over F_q is defined as C^⊥ = {x ∈ F^n_q | (x, y) = 0 for all y ∈ C}. Let x = (x_1, x_2, . . . , x_n), y = (y_1, y_2, . . . , y_n) ∈ F^n_{q2} . For F^n_{q2} , the Hermitian inner product is defined as (x, y)_h = ∑_n i=1 x_iy_i, where y_i = y^q_i . The Hermitian dual code C^{⊥h} of an [n, k] code C over F_q2 is defined as C^{⊥h} = {x ∈ F^n_{q2} | (x, y)_h = 0 for all y ∈ C}. A code C is said to be a Euclidean (resp. Hermitian) linear complementary dual code, a Euclidean (resp. Hermitian) LCD code for short, if C ∩ C^⊥ = {0_n} (resp. C ∩ C^{⊥h} = {0_n}). The Euclidean (resp. Hermitian) dual distance d^⊥ (resp. d^{⊥h}) of C is the minimum weight of the Euclidean (resp. Hermitian) dual code.

Carlet, Mesnager, Tang, Qi and Pellikaan [3] proved that any code over F_q2 (q > 2) is equivalent to a quaternary Hermitian LCD code. Lu, Li, Guo and Fu [6] proved that a quaternary Hermitian LCD code leads to a construction of a maximal-entanglement entanglement-assisted quantum error correcting code. For k ≥ 2 and a positive integer d_0, Araya, Harada and Saito proved that if there exists no binary (resp. ternary) Euclidean LCD [n, k, d] code with d ≥ d_0 and d^⊥ ≥ 2, then there exists no binary (resp. ternary) Euclidean LCD [n, k, d] code with d ≥ d_0 and d^⊥ = 1 [1, Proposition 3.3]. This motivates us to study the existence of quaternary Hermitian LCD codes with d^{⊥h} = 1. In this note, it is shown that a result analogous to [1, Proposition 3.3] holds for quaternary Hermitian LCD codes.

The remaining of this note is organized as follows. In Section 2, we recall preliminary results and prove a lemma needed later. In Section 3, for k ≥ 2 and a positive integer d_0, it is shown that if there exists no quaternary Hermitian LCD [n, k, d] code with d ≥ d_0 and d^{⊥h} ≥ 2, then there exists no quaternary Hermitian LCD [n, k, d] code with d ≥ d_0 and d^{⊥h} = 1. Furthermore, we apply the result and obtain a generalized version of [2, Theorem 9].

2 Preliminaries

A generator matrix of a code C is any matrix whose rows form a basis of C. Given a matrix G, we denote the transpose, conjugate of G by G^T , G respectively. The following characterization on Hermitian LCD codes is due to Güneri, B. Özkaya and P. Solé [4].

Lemma 1 ([4, Proposition 3.5]). Let C be an [n, k] code over F_q2 and let G be a generator matrix of C. Then C is a Hermitian LCD code if and only if the k × k matrix GG^T is nonsingular.

Lemma 2. Let k ≥ 2. If there exists a quaternary Hermitian LCD [n, k, d_0] code with d^{⊥h} ≥ 2, then there exists a quaternary Hermitian LCD [n+1, k, d] code with d^{⊥h} ≥ 2 and d ∈ {d_0, d_0 + 1}.

Proof. Let C_0 be a quaternary Hermitian LCD [n, k, d_0] code with d^{⊥h} ≥ 2. From the proof of [5, Proposition 4], C_0 has a generator matrix of the form G_0 = ( x G_1 ) , satisfying that (x, x)_h ≠ 0 and xG_1^T = 0_{k−1}. The code C_1 with generator matrix G_1 is a quaternary Hermitian LCD [n, k − 1] code.

(i) k = 2: G_1 is regarded as a codeword c_1 ∈ C_1 with (c_1, c_1)_h ≠ 0 since C_1 is a Hermitian LCD code.

(ii) k ≥ 3: From the proof of [5, Proposition 4], C_1 has a generator matrix of the form G^′_1 = ( x^′ G^′_2 ) , satisfying that (x^′, x^′)_h ≠ 0 and x^′G^′_2^T = 0_{k−2}. The code C^′_2 with generator matrix G^′_2 is a quaternary Hermitian LCD [n, k − 2] code. Since both G_1 and G^′_1 are generator matrices of C_1,

G^′_0 = ( x G^′_1 ) = x x^′ G^′_2

is also a generator matrix of C_0. Since x ∈ C^{⊥h}_1 , we have (x, x^′)_h = 0 and xG^{′T}_2 = 0_{k−2}.

Consider the following k × (n + 1) matrix G:

G = ( G_0 h^T ) if k = 2, ( G^′_0 h^T ) if k ≥ 3, where h = { (1, 1) if k = 2, (1, 1, 0_{k−2}) if k ≥ 3.

Let C be the code with generator matrix G.

(i) k = 2: it holds that

det GG^T = det ( xx^T + 1 xG_1^T + 1 G_1x^T + 1 G_1G_1^T + 1 ) = 1.

(ii) k ≥ 3: it holds that

det GG^T = det xx^T + 1 xx^{′T} + 1 xG^′_2^T x^′x^T + 1 x^′x^{′T} + 1 x^′G^′_2^T G^′_2x^T G^′_2x^{′T} G^′_2G^′_2^T

= det G^′_2G^′_2^T ≠ 0.

In any case, GG^T is nonsingular. By Lemma 1, C is a Hermitian LCD code. Furthermore, it holds that for all nonzero codeword c ∈ C there exists a nonzero codeword c_0 ∈ C_0 and a ∈ F_4 such that c = (c_0, a). Therefore, it follows that d(C) ∈ {d_0, d_0 + 1}. It is clear that d^{⊥h} ≥ 2. Hence C is a quaternary Hermitian LCD [n + 1, k, d] code with d^{⊥h} ≥ 2 and d ∈ {d_0, d_0 + 1}.

3 The existence of quaternary Hermitian LCD codes with Hermitian dual distance 1

Theorem 1. Let k ≥ 2 and let d_0 be a positive integer. If there exists no quaternary Hermitian LCD [n, k, d] code with d ≥ d_0 and d^{⊥h} ≥ 2, then there exists no quaternary Hermitian LCD [n, k, d] code with d ≥ d_0 and d^{⊥h} = 1.

Proof. Suppose that there exists a quaternary Hermitian LCD [n, k, d] code C with d ≥ d_0 and d^{⊥h} = 1. Let l be the number of zero coordinates of C. Puncturing C on the zero coordinates gives a quaternary Hermitian LCD [n − l, k, d] code with d^{⊥h} ≥ 2. Then a quaternary Hermitian LCD [n, k, d] code with d ≥ d_0 and d^{⊥h} ≥ 2 is constructed by Lemma 2. This contradicts the assumption.

For positive integers n, k, α, define r_4(n, k, α) = 4^{k−1}n −^{4k−1}_3 α. Araya, Harada and Saito [2] gave the following result on the nonexistence of some quaternary Hermitian LCD codes with d^{⊥h} ≥ 2.

Theorem 2 ([2, Theorem 9]). Let k ≥ 3 and 4α − 3n ≥ 1.

(i) Suppose that 4r_4(n, k, α) < k. Then there exists no quaternary Hermitian LCD [n, k, α] code with d^{⊥h} ≥ 2.

(ii) Suppose that 4r_4(n, k, α) ≥ k. If there exists no quaternary Hermitian LCD [4r_4(n, k, α), 3r_4(n, k, α)] code with d^{⊥h} ≥ 2, then there exists no quaternary Hermitian LCD [n, k, α] code with d^{⊥h} ≥ 2.

By Theorem 1, we remove the condition on the Hermitian dual distance as follows.

Corollary 1. Let k ≥ 3 and 4α − 3n ≥ 1.

(i) Suppose that 4r_4(n, k, α) < k. Then there exists no quaternary Hermitian LCD [n, k, α] code.

(ii) Suppose that 4r_4(n, k, α) ≥ k. If there exists no quaternary Hermitian LCD [4r_4(n, k, α), 3r_4(n, k, α)] code with d^{⊥h} ≥ 2, then there exists no quaternary Hermitian LCD [n, k, α] code.

Araya, Harada and Saito determined the largest minimum weight among all quaternary Hermitian LCD [n, 3] codes [2, Theorem 12]. In the proof of [2, Theorem 12], the nonexistence of some quaternary Hermitian LCD [n, 3] codes with d^{⊥h} ≥ 2 was established by Theorem 2. On the other hand, the nonexistence of some quaternary Hermitian LCD [n, 3] codes with d^{⊥h} = 1 was established by case-by-case analyses. By Corollary 1, we only have to consider quaternary Hermitian LCD [n, 3] codes with d^{⊥h} ≥ 2. This simplifies the proof.

Acknowledgement

The authors are grateful to Professor Masaaki Harada for bringing this problem to their attention.

References

[1] M. Araya, M. Harada and K. Saito, Characterization and classification of optimal LCD codes, Des. Codes Cryptogr. 89 (2021), 617–640.

[2] M. Araya, M. Harada and K. Saito, Quaternary Hermitian linear complementary dual codes, IEEE Trans. Inform. Theory 66 (2020), 2751– 2759.

[3] C. Carlet, S. Mesnager, C. Tang, Y. Qi and R. Pellikaan, Linear codes over F_q are equivalent to LCD codes for q > 3, IEEE Trans. Inform. Theory 64 (2018), 3010–3017.

[4] C. Güneri, B. Özkaya and P. Solé, Quasi-cyclic complementary dual codes, Finite Fields Appl. 42 (2016), 67–80.

[5] M. Harada and K. Saito, Remark on subcodes of linear complementary dual codes, Inform. Process. Lett. 159 (2020), 105963, 3 pp.

[6] L. Lu, R. Li, L. Guo and Q. Fu, Maximal entanglement entanglementassisted quantum codes constructed from linear codes, Quantum Inf. Process. 13 (2015), 165–182.