arXiv:2201.05240v1 [cs.IT] 13 Jan 2022

Integrated Sensing and Communication with Millimeter Wave Full Duplex Hybrid Beamforming

Md Atiqul Islam^†, George C. Alexandropoulos^§, and Besma Smida^† †Department of Electrical and Computer Engineering, University of Illinois at Chicago, USA §Department of Informatics and Telecommunications, National and Kapodistrian University of Athens, Greece emails: {mislam23,smida}@uic.edu, alexandg@di.uoa.gr

Abstract—Integrated Sensing and Communication (ISAC) has attracted substantial attraction in recent years for spectral efficiency improvement, enabling hardware and spectrum sharing for simultaneous sensing and signaling operations. In-band Full Duplex (FD) is being considered as a key enabling technology for ISAC applications due to its simultaneous transmission and reception capability. In this paper, we present an FDbased ISAC system operating at millimeter Wave (mmWave) frequencies, where a massive Multiple-Input Multiple-Output (MIMO) Base Station (BS) node employing hybrid Analog and Digital (A/D) beamforming is communicating with a DownLink (DL) multi-antenna user and the same waveform is utilized at the BS receiver for sensing the radar targets in its coverage environment. We develop a sensing algorithm that is capable of estimating Direction of Arrival (DoA), range, and relative velocity of the radar targets. A joint optimization framework for designing the A/D transmit and receive beamformers as well as the Self-Interference (SI) cancellation is presented with the objective to maximize the achievable DL rate and the accuracy of the radar target sensing performance. Our simulation results, considering fifth Generation (5G) Orthogonal Frequency Division Multiplexing (OFDM) waveforms, verify our approach’s high precision in estimating DoA, range, and velocity of multiple radar targets, while maximizing the DL communication rate.

Index Terms—Full duplex, millimeter wave, direction estimation, range-Doppler estimation, joint communication and sensing.

I. INTRODUCTION

Integrated Sensing and Communication (ISAC) is an emerging concept for future wireless networks, where the previously competing sensing and communication operations are jointly optimized in the same hardware platform using a unified signal processing framework [1]–[5]. Recently, Full Duplex (FD) massive Multiple-Input Multiple-Output (MIMO) communications have been considered a key enabler for ISAC applications due to their simultaneous UpLink (UL) and DownLink (DL) transmission capability within the entire frequency band [6]– [9]. Furthermore, FD massive MIMO ISAC applications at millimeter Wave (mmWave) frequencies have the potential to provide high capacity communication links while simultaneously achieving high-resolution sensing, e.g., Direction of Arrival (DoA), range, and relative speed of radar targets/scatterers.

The performance of the FD ISAC systems relies on the in-band Self-Interference (SI) signal suppression capability that stems from the Transmitter (TX) to the Receiver (RX) side during FD operation. Recently in [7], [8], [10], [11], SI cancellation was achieved for the FD massive MIMO systems operating at mmWave, utilizing a combination of propagation domain isolation, analog domain suppression, and digital SI cancellation techniques. To alleviate the hardware cost in mmWave massive MIMO transceivers, hybrid Analog and Digital (A/D) beamformers are usually employed, where largescale antenna arrays are usually connected to a small number of Radio Frequency (RF) chains via analog preprocessing networks comprised of phase shifters [12]. Such systems require appropriate beam selection for analog TX/RX beamformers, chosen from predefined codebooks, to maximize DL rate and sensing accuracy. Moreover, in the envisioned FD ISAC with massive MIMO radios, the transmit waveform will be utilized for both DL data transmission and sensing of the radar targets [1]. Therefore, a joint design of the A/D beamformers and SI cancellation along with sensing techniques is required for maximizing the performance of FD ISAC systems.

Very recently in [13], [14], joint radar communication and sensing frameworks, leveraging FD operation, were considered for single-antenna systems, where both communication and radar waveforms were optimized for sensing performance. In [15], [16], the FD ISAC operation was proposed for mmWave frequency bands considering a massive MIMO FD Base Station (BS), where the signal power is maximized in the radar target direction, while maintaining a threshold DL rate performance. Although the considered FD ISAC approach estimated the DoA two radar targets, the range was only calculated for one target due to its disassociated DoA and range estimation technique.

In this paper, we present a novel FD massive MIMO ISAC system operating at mmWave frequencies and realizing hybrid A/D beamforming, where Orthogonal Frequency Division Multiplexing (OFDM) waveforms are utilized for both DL communication and radar target sensing. Unlike state-of-the-art works, we devise an ISAC optimization framework that is capable of estimating the DoA, range, and relative velocity of multiple radar targets, while maximizing the DL communication rate. Our numerical results, considering the fifth Generation (5G) New Radio (NR) OFDM waveform, verify the high sensing accuracy and the increased communication rate of the proposed optimization design.

II. SYSTEM AND SIGNAL MODELS We consider an FD ISAC system comprising of an FD mmWave massive MIMO Base Station (BS) node b equipped

Fig. 1. The considered FD massive MIMO ISAC system: the FD hybrid A/D beamforming Base Station (BS) communicates in the downlink with a mobile single-antenna half-duplex User Equipment (UE), while its reflected transmitted signals from radar targets/scatterers in the environment are received via hybrid combining and processed for DoA, range, and relative velocity estimations of the radar targets/scatterers.

with N_b TX and M_b RX antenna elements communicating in the DL direction with an RX User Equipment (UE) node u with M_u antenna elements, while the reflected DL signal is utilized to detect radar targets/scatterers randomly distributed within the communication/sensing environment at the RX of BS node b, as depicted in Fig. 1. To reduce the number of RF chains and phase shifters, the BS node b employs a partially-connected Hybrid BeamForming (HBF) structure with A/D TX and RX beamformers, where each of the N^{RF}_b and M^{RF}_b TX/RX RF chains is connected to a Uniform Linear Arrays (ULA) of N^A_b and M^A_b antenna elements, respectively, via phase shifters. Therefore, it holds N_b = N^A_b N^{RF}_b and M_b = M^A_b M^{RF}_b for total number of TX and RX antennas, respectively, at the BS node b. Since the size of the antenna array at the UE node u is typically much smaller than at the FD massive MIMO BS b, we assume that the UE adopts a fully digital beamforming structure.

It is assumed that BS node b transmits mmWave OFDM waveforms in the DL direction containing Q OFDM symbols with P active subcarriers. In the BaseBand (BB), the unit power frequency-domain symbol vector s_{p,q} ∈ C^{db×1} at the pth subcarrier of qth OFDM symbol is precoded using digital beamforming matrix V^{BB}_b ∈ C^{N RFb ×db} , where d_b ≤ min{N^{RF}_b , M_u}. Following the BB precoder, the DL signal is processed by the analog beamformer V^{RF}_b ∈ C^{Nb×N RFb} containing the configurations of the phase shifters as follows:

V^{RF}_b ≜ v_1 0_N A_{b ×1} · · · 0_N A_{b ×1} 0_N A_{b ×1} v_2 · · · 0_N A_{b ×1} . . . . .. . . . 0_N A_{b ×1} 0_N A_{b ×1} · · · v_N (RF)_b

. (1)

The elements of each v_i are assumed to have constant magnitude, i.e., |[v_i]_n|^2 = 1/N^A_b ∀n = 1, 2, . . . , N^A_b . We also assume that v_i ∈ F_{TX} ∀i = 1, 2, . . . , N^{RF}_b , which means that all analog TX precoding vectors belong in a predefined beam codebook F_{TX} including card(F_{TX} ) distinct vectors (or analog beams). Applying both A/D beamforming, the TX frequencydomain symbols at the antenna elements are expressed as

x_{p,q} ≜ V^{RF}_b V^{BB}_b s_{p,q} , (2)

where x_{p,q} ∈ C^{Nb×1}. The signal transmissions at node b is power limited according to E{‖V^{RF}_b V^{BB}_b s_{p,q} ‖^2} ≤ P_b.

A. Radar Signal Reception Model

For sensing operation, we consider that a collection of K radar targets/scatterers are randomly distributed within the communication/sensing environment and are to be detected by the BS node b. All the K targets reflect DL signal back to the RX of the BS node, while only a subset of them (L out of K) contributes to the DL communication scattering paths between the BS node b and the RX UE node u. The purpose of the sensing operation is to estimate the DoA, range, and relative velocity of each radar targets.

We consider that the DoAs of the K targets are defined as Θ = [θ_1, θ_2, · · · , θ_K ], while the distance and the relative speed of kth target correspond to a delay τ_k and a Doppler shift f_{D,k}, respectively. Enabled by FD, the received signal y_{p,q} ∈ C^{Mb ×1} at the RX of the BS node b combining the SI and the reflected signal by the Radar targets is expressed as y_{p,q} ≜ K∑ k=1 α_ke^{j2π(qTs fD,k −pτk Δf )}a_{Mb} (θ_k)a^H_{Nb} (θ_k )x_{p,q} + H_{b,b}x_{p,q} + n_{p,q}, (3)

where α_k ∈ C and n_{p,q} ∼ CN (0, σ^2_b I_{Mb} ) represent the reflection coefficient of the kth radar target and the receiver noise floor, respectively. Here, Δf and T_s ≜ 1/Δf + T_{cp} denote the subcarrier spacing and the total OFDM symbol duration (including the cyclic prefix). The propagation delay causes the phase shift e^{−j2πpτk Δf} across subcarriers, while the Doppler shift contributes a row-wise oscillation across different OFDM symbols [17]. Considering ULA, the steering vector a_{Nb} (θ) for N_b antenna elements and any DoA θ is formulated as [18] a_{Mb} (θ)≜ 1 √ N_b [ 1, e^{j 2πλ d sin(θ)}, . . . , e^{j 2πλ (Nb−1)d sin(θ)}]^T, (4)

where λ is the propagation signal wavelength and d denotes the distance between adjacent antenna elements. Here, H_{b,b} ∈ C^{Mb ×Nb} is the SI channel path at the BS node b, which is modeled as a Rician fading mmWave channel as [19, eq. (9)].

The received signal at the node b RX is first processed by the RF combiner W^{RF}_b ∈ C^{Mb ×M RFb} , where the structure of the combiner is formulated similarly as (1). Here, the analog RX combining vectors belong in a predefined beam codebook F_{RX} including card(F_{RX} ) distinct vectors. After RF combination and A/D SI cancellation, the received signal is expressed as

~y_{p,q} ≜(W^{RF}_b )^H K∑ k=1 α_ke^{j2π(qTs fD,k −pτk Δf )}a_{Mb}(θ_k)a^H_{Nb}(θ_k)x_{p,q} + ( ~H_{b,b} +C_b +D_b)V^{BB}_b s_{p,q} +(W^{RF}_b )^Hn_{p,q}, (5)

where ~H_{b,b} ≜ (W^{RF}_b )^HH_{b,b}V^{RF}_b is the effective SI channel after analog TX/RX beamforming. Here, C_b and D_b represent the analog and digital SI cancellation, respectively, that are designed following the structure presented in [7].

B. DL Signal Reception Model

As mentioned above, L out of K scatterers contributes to the DL channel H_{u,b} ∈ C^{Mu×Nb} . As the principal focus of the paper is to estimate Radar target parameters, we ignore the delay and Doppler shift parameters for the DL channel. Now, the received DL signal vector r_{p,q} ∈ C^{Mu×db} at the UE RX is expressed as

r_{p,q} ≜ W^H_u (^L∑ ℓ=1 β_ℓa_{Mu} (θ_ℓ)a^H_{Nb} (θ_ℓ)x_{p,q} + z_{p,q} )

= W^H_u ( H_{u,b}x_{p,q} + z_{p,q} ) , (6)

where β_ℓ ∈ C and z_{p,q} ∼ CN (0, σ^2_uI_{Mu} ) represent the complex reflection coefficient of ℓth scatter path and the noise floor at RX node u, respectively.

The achievable DL rate of the FD ISAC system can be expressed as

R_{DL} ≜ log_2 ( det ( I_{db} + W^H_u H_{u,b}V^{RF}_b V^{BB}_b (V^{RF}_b V^{BB}_b )^H

× H^H_{u,b}W_u(W^H_u W_uσ^2_u)^{−1} )) , (7)

III. DOA, DELAY, AND DOPPLER SHIFT ESTIMATION

In this section, we present the estimations of the DoA, delay, and Doppler shift parameters of the Radar targets, which are realized by the BS’s RX using the reflected signals.

A. Radar Target DoA Estimation

For DoA estimation, we deploy the MUltiple SIgnal Classification (MUSIC) algorithm; other DoA estimation techniques can be used as well [20]. First, we estimate the covariance matrix of the radar target reflected signal. Across all subcarriers

Algorithm 1 Delay and Doppler Shift Estimation

Input: x_{p,q} , ~y_{p,q} ,∀p, q, W^{RF}_b , and ^θ_k ∀k. Output: ^τ_k, ^f_{D,k}, ∀k. 1: Set n = 0, · · · , P − 1 and m = −^Q_2 , · · · ,^Q_2 − 1. 2: for k = 1, 2, . . . , K do 3: Set g_{p,q} ≜ a_{Mb} (^θ_k)a^H_{Nb} (^θ_k)x_{p,q} .

4: Set z_{p,q} ≜^1_{Mb}^{Mb} ∑ i=1 [W^{RF}_b ~y_{p,q} ]_i/[g_{p,q}]_i, ∀p, q.

5: Set A(n, m) ≜^{P −1} ∑ p=0 (_{Q−1} ∑ q=0 z_{p,q} e^{−j2π qmQ} ) e^{j2π pnP} . 6: Set (n^∗, m^∗) = arg max_{n,m} |A(n, m)|^2.

7: Set the estimated delay ^τ_k =^{n∗}_{P Δf} .

8: Set the Doppler frequency of kth target ^f_{D,k} =^{m∗}_{QTs} . 9: end for

and OFDM symbols of the communication slot, the covariance matrix R_b ∈ C^{M RFb ×M RFb} can be estimated as R_b ≜E{~y_{p,q} ~y^H_{p,q} }, ^R_b ≜ 1 P Q Q−1∑ q=0

P −1∑

p=0 ~y_{p,q} ~y^H_{p,q} . (8)

By taking the eigenvalue decomposition of the estimated sample covariance matrix ^R_b, it is deduced that:

^R_b ≜ Udiag{η_1, η_2, . . . , η_{Mb} }U^H, (9)

where η_1 ≥ η_2 ≥ . . . ≥ η_M RF_b are the eigenvalues of ^R_b and U ∈ C^{M RFb ×M RFb} contains their corresponding eigenvectors. Since we are interested in estimating the DoAs of K radar targets, the matrix U can be partitioned as U = [U_s|U_n], where the columns in U_n ∈ C^{M RFb ×M RFb −K} are the eigenvectors spanning the noise subspace and U_s ∈ C^{M RFb ×K} contains the signal space eigenvectors. The MUSIC spectrum for the considered HBF architecture can be thus formulated as: S(θ) ≜ ( a^H_{Mb} (θ)W^{RF}_b U_nU^H_n (W^{RF}_b )^Ha_{Mb} (θ) )_{−1} , (10)

whose K peaks correspond to the K estimated DoAs ^θ_k, ∀k.

B. Delay and Doppler Shift Estimation

The next step is to estimate the delay and Doppler shift parameters associated with the K estimated DoAs. Using the estimate DoA ^θ_k and the known transmit signal x_{p,q} , we formulate a reference signal in the DoA direction as

g_{p,q} ≜ a_{Mb} (^θ_k)a^H_{Nb} (^θ_k)x_{p,q} . (11)

Now, we utilize the received signal ~y_{p,q} to derive the quotient averaged across all RX antennas that includes the effect of delay and Doppler shift in the direction of ^θ_k as z_{p,q} ≜ 1 M_b M_b∑

i=1 [W^{RF}_b ~y_{p,q} ]_i/[g_{p,q}]_i, ∀p, q. (12)

To estimate ^τ_k and ^f_{D,k}, we formulate the likelihood function: A(n, m) ≜ P −1∑

p=0 (_{Q−1} ∑ q=0 z_{p,q}e^{−j2π qmQ} ) e^{j2π pnP} , (13) where n = 0, · · · , P − 1 and m = −Q/2, · · · , Q/2 − 1. Finally, we find the best quantized delay and Doppler shift that maximizes the likelihood function norm. The delay and Doppler shift estimation procedure is provided in Algorithm 1. IV. PROPOSED ISAC OPTIMIZATION FRAMEWORK In this section, we present a joint optimization framework deriving A/D beamformers and SI cancellation matrices with the objective to maximize the DL rate and the radar estimation accuracy.

We consider a time division duplexing communication protocol, where the DoAs estimated in one communication time slot is utilized to derive the beamformers and SI cancellation matrices for the successive slot. To optimize the DL rate and radar target parameter estimation accuracy, we propose to maximize the SNR in both the DL and radar target direction. Given the estimated DoAs ^θ_k, ∀k, the SNR in the direction of all radar targets can be written as

^Γ_{Radar} ≜ ‖ ‖ ‖(W^{RF}_b )^H K∑ k=1 a_{Mb} (^θ_k)a^H_{Nb} (^θ_k)V^{RF}_b V^{BB}_b ‖ ‖ ‖^2Σ^{−1}_b ,

(14)

where Σ_b = ‖( ^~H_{b,b} + C_b + D_b)V^{BB}_b ‖^2 + ‖ ‖W^{RF}_b ‖ ‖^2 σ^2_b is the interference plus noise covariance matrix at the RX of node b. Similarly, the estimated DL SNR is expressed as

^Γ_{DL} = ‖ ‖ ‖W^H_u L∑ ℓ=1 a_{Mu} (^θ_ℓ)a^H_{Nb} (^θ_ℓ)V^{RF}_b V^{BB}_b ‖ ‖ ‖^2Σ^{−1}_u , (15)

where Σ_u = ‖W_u‖^2 σ^2_u is the noise covariance matrix at the RX node u.

The optimization problem to maximize the Radar target and DL SNR can be written as

OP : max

V^{RF}_b ,V^{BB}_b ,W^{RF}_b

C_b,D_b ,W_u

^Γ_{Radar} + ^Γ_{DL}

s.t. ‖ ‖ ‖ ‖[( ^~H_{b,b} +C_b)V_{BBb} ]_{(j,:)} ‖ ‖ ‖ ‖ 2 ≤λ_b,∀j = 1, . . . , M^{RF}_b , E{‖V^{RF}_b V^{BB}_b ‖^2} ≤ P_b, (16)

w_j ∈ F_{RX} ∀j and v_n ∈ F_{TX} ∀n = 1, 2, . . . , N^{(RF)}_b

The optimization problem in (16) is a non-convex problem with coupling variables, hence, quite difficult to tackle. In this work, we solve it suboptimally using alternating optimization, leaving other possibilities for future work.

First, using the estimated DoAs, we formulate a virtual channel of in the radar target direction as ^H_R ≜ K∑ k=1 a_{Mb} (^θ_k)a^H_{Nb} (^θ_k). Now to maximize the radar SNR, we

find the TX analog beams solving the following suboptimization problem:

OP1 : V^{RF}_b ≜ argmax_{vj ∈FTX} ‖ ^H_RV^{RF}_b ‖^2 (17)

The solution of OP1 requires a simple search through the beam codebook F_{TX} . Using the TX analog beamformer V^{RF}_b ,

Algorithm 2 FD ISAC Optimization

Input: ^H_{b,b}, N, P_b and ^θ_k ∀k.

Output: V^{RF}_b , V^{BB}_b , W^{RF}_b , C_b, D_b, and W_u.

1: Set ^H_R ≜^K ∑ k=1 a_{Mb} (^θ_k)a^H_{Nb} (^θ_k).

2: Set ^H_{u,b} ≜^L ∑ ℓ=1 a_{Mu} (^θ_ℓ)a^H_{Nb} (^θ_ℓ).

3: Set W_u as the d_b left-singular vectors of ^H_{u,b} corresponding to the singular values in descending order.

4: Set V^{RF}_b ≜ arg max

v_j ∈F_{TX}

‖ ^H_RV^{RF}_b ‖^2.

5: Set W^{RF}_b ≜ arg max

w_j ∈F_{TX}

‖(W^{RF}_b )^H ^H_R V^{RF}_b ‖^2 ‖(W^{RF}_b )^H ^H_{b,b}V^{RF}_b ‖^2 .

6: Set ^~H_{b,b} = (W^{RF}_b )^H ^H_{b,b}V^{RF}_b and ^~H_{u,b} = ^H_{u,b}V^{RF}_b .

7: Set C_b = [ −[ ^~H_{b,b}]_{:,1:} N_{M RFb} 0_{:,(N} RF_{b −} N_{M RFb :N} RF_{b )} ] and D_b = −( ^~H_{b,b} + C_b).

8: Obtain B with the N^{RF}_b right-singular vectors of ( ^~H_{b,b} + C_b) corresponding to the singular values in descending order.

9: for α = N^{RF}_b , N^{RF}_b − 1, . . . , 2 do 10: Set F = [B]_{(:,N} RF_{b −α+1:N} RF_{b )}.

11: Set G as the optimum precoding for the effective DL MIMO channel ^~H_{u,b}F given P_b.

12: if ‖ ‖ ‖[( ^~H_{b,b} +C_b)FG]_{(j,:)} ‖ ‖ ‖ 2 ≤λ_b,∀j = 1, . . . , M^{RF}_b , then

13: Output V^{BB}_b = FG and stop the algorithm. 14: else 15: Output that the C_b realization does not meet the residual SI constraint.

16: end if 17: end for

we derive the analog combiner solving the suboptimization problem OP1, where we simultaneously maximize the radar SNR and suppress SI signal as follows:

OP2 : W^{RF}_b ≜ argmax_{wj ∈FTX}

‖(W^{RF}_b )^H ^H_RV^{RF}_b ‖^2 ‖(W^{RF}_b )^H ^H_{b,b}V^{RF}_b ‖^2

(18)

Similar to OP1, the solution of OP2 requires a simple search through the available beam codebook F_{RX} . Given the analog SI cancellation taps N ≤ N^{RF}_b M^{RF}_b and the analog TX/RX beamformer at the BS, we follow a similar procedure to [7], aiming to find the digital beamforming matrix V^{BB}_b and the SI cancellation matrices maximizing the DL rate and suppressing the SI signal power below the RF saturation level of λ_b. The latter will ensure proper reception of the Radar target reflected signal. Our solution for the optimization problem (16) is summarized in Algorithm 2.

V. NUMERICAL RESULTS

In this section, we present numerical results for the radar sensing and DL rate performance of the proposed FD massive MIMO ISAC system operating at mmWave frequencies.

Fig. 2. Sensing parameter estimation performance for 6 radar targets with N^{RF}_b = M^{RF}_b = 8, N^A_b = N^A_b = 16 and transmit power of 30dBm. (a) DoA and range estimation, (b) Range and relative velocity estimation.

A. Simulation Parameters

We perform an extensive waveform simulation following the FD massive MIMO architecture illustrated in Fig. 1 when operating at mmWave frequencies, where a 128 × 128 FD massive MIMO node b is communicating in the DL direction with 4 antenna RX UE node u. The BS node b employs N^{RF}_b = M^{RF}_b = 8 TX/RX RF chains with each of them connected to a ULA of N^A_b = M^A_b = 16 antenna elements via phase shifters. The communication is performed using mmWave frequency of 28GHz and a 5G NR OFDM waveform with 100MHz BandWidth (BW) and Δf = 120KHz subcarrier spacing. According to the 5G NR specifications, we have 66 Physical Resource Blocks (PRBs) resulting in P = 792 active subcarriers and Q = 14 OFDM symbols in each communication slot. Total OFDM symbol duration is defined as T_s = 8.92μs. We have considered a radio subframe of 1ms for DL communication. The RX noise floors at all nodes were assumed to be −90dBm for 100MHz BW OFDM signal. To this end, the RXs have an effective dynamic range of 60dB provided by 14-bit Analog-to-Digital Converters (ADC) for a Peak-to-Average-Power-Ratio (PAPR) of 10 dB. Therefore, the residual SI power after analog SI cancellation at the input of each RX RF chain has to be below −30dBm to avoid signal saturation. The pathloss of the clustered DL channel is assumed to be 100dB, whereas the SI channels are modeled as Rician fading channels with a κ-factor of 35dB and pathloss 40dB [21]. For the BS analog TX/RX beamformer, we consider a 5-bit beam codebook based on the Discrete Fourier Transform (DFT) matrix. We have used 1000 independent Monte Carlo simulation runs to calculate the Radar sensing and DL rate performance.

Fig. 3. Sensing parameter estimation performance for 6 radar targets with N^{RF}_b = M^{RF}_b = 8, N^A_b = N^A_b = 16 and DL transmit power of 10dBm. (a) DoA and range estimation, (b) Range and relative velocity estimation.

B. Radar Target Parameters

We have considered K = 6 radar targets randomly distributed in the sensing/communication environment with DoAs θ_k ∈ [−90^∘ 90^∘], ∀k. For communication scatters, L = 2 out of K = 6 targets are chosen randomly. Each of the radar targets the range and relative velocity is selected randomly with a maximum range of 80m and maximum velocity of 100km/h.

C. Radar Target Sensing performance

In Fig. 2, We have depicted the sensing performance of the proposed FD ISAC system with a 128 × 128 massive MIMO node transmitting DL signal with a transmit power of 30dBm. The DoA and range estimation is plotted in contrast to the true target parameters in Fig. 2(a), where it is evident that the proposed FD ISAC system can detect all 6 targets successfully with high precision. Even for really close target (10^∘ and 12^∘) with only 2^∘ angle and less than 5m range difference, the estimation performance is highly accurate. The superior sensing performance is provided by the proposed associated delay estimation approach with high-resolution MUSIC DoA estimation unlike previous FD ISAC work in [16], where range estimation for such close targets was not possible. In Fig. 2(b), the relative velocity is plotted with respect to the range estimation for 30dBm DL transmit power. The figure shows that the proposed FD ISAC system is capable of estimating the relative velocity of all 6 targets with less than 1.5% estimation error.

In Fig. 3, radar target sensing performance of the proposed FD ISAC system is presented for 10dBm DL transmit power. It is evident from Fig. 3(a) that the DoA estimation is almost accurate even at a low transmit power of 10dBm. However, for

Fig. 4. DL rate with respect to transmit power in dBm for the 128 × 128 massive MIMO FD BS communicating with a 4 antenna UE RX node.

the target at 3^∘, the estimated range is around 3m away the actual value of 80m. This is due to the low transmit power and higher path loss of the furthest target. In Fig. 3(b), the relative velocity estimation is showcased, where the proposed approach achieved sensing performance with less than 5% estimation error for a low transmit power of 10dBm.

The DL rate performance of the proposed FD ISAC system with a 128 × 128 massive MIMO BS node transmitting to a 4 antenna UE RX node is depicted in Fig. 4 with respect to transmit power. It is evident from the figure that the proposed FD ISAC approach is capable of providing DL rate very close (1.5bps/Hz) to the ideal rate in addition to the high radar sensing performance at the RX of BS node for N = 16 (25%) analog SI cancellation taps at the FD massive MIMO node. For even smaller hardware complexity (12.5%) taps, the DL rate performance is comparable up to 20 dB transmit power. However, as transmit power increases the impact of SI signal worsens, for DL transmit power of 30dBm, the FD ISAC system is capable of providing 75% of the ideal DL rate with only N = 8 SI cancellation taps. VI. CONCLUSION

In this paper, we presented an FD-based ISAC optimization framework, where an FD massive MIMO BS node is transmitting DL signals and concurrently performing radar target sensing utilizing the reflected signals. We devised a DoA, delay, and Doppler shift estimation algorithm for multiple radar target sensing considering hybrid A/D beamforming at the BS node. Adopting a limited complexity analog SI cancellation architecture, we presented a joint design of the A/D beamformer and SI cancellation that maximizes the DL rate together with the target sensing performance. Our performance results for a mmWave channel model demonstrated the high precision DoA, range, velocity estimation of multiple radar targets while providing maximized DL rate. In future work, the proposed FD ISAC approach will be considered for sensing and communication demanding practical applications, such as autonomous vehicles and flight control systems.

ACKNOWLEDGMENTS This work was partially funded by the National Science Foundation CAREER award #1620902.

REFERENCES

[1] F. Liu, C. Masouros, A. P. Petropulu, H. Griffiths, and L. Hanzo, “Joint radar and communication design: Applications, state-of-the-art, and the road ahead,” IEEE Trans. Commun., vol. 68, no. 6, pp. 3834–3862, Feb. 2020.

[2] I. Alamzadeh, G. C. Alexandropoulos, N. Shlezinger, and M. F. Imani, “A reconfigurable intelligent surface with integrated sensing capability,” Scientific Reports, vol. 11, no. 20737, pp. 1–10, Oct. 2021.

[3] G. C. Alexandropoulos, N. Shlezinger, I. Alamzadeh, M. F. Imani, H. Zhang, and Y. C. Eldar, “Hybrid reconfigurable intelligent metasurfaces: Enabling simultaneous tunable reflections and sensing for 6G wireless communications,” [online] https://arxiv.org/abs/2104.04690, 2021.

[4] K. V. Mishra, M. B. Shankar, V. Koivunen, B. Ottersten, and S. A.

Vorobyov, “Toward millimeter-wave joint radar communications: A signal processing perspective,” IEEE Signal Process. Mag., vol. 36, no. 5, pp. 100–114, Sep. 2019.

[5] B. Paul, A. R. Chiriyath, and D. W. Bliss, “Survey of RF communications and sensing convergence research,” IEEE Access, vol. 5, pp. 252–270, Jan. 2016.

[6] H. Alves, T. Riihonen, and H. A. Suraweera, Full-Duplex Communications for Future Wireless Networks. Singapore: Springer, 2020.

[7] G. C. Alexandropoulos, M. A. Islam, and B. Smida, “Full duplex hybrid A/D beamforming with reduced complexity multi-tap analog cancellation,” in Proc. IEEE SPAWC, Atlanta, USA, May 2020.

[8] M. A. Islam, G. C. Alexandropoulos, and B. Smida, “Direction-assisted beam management in full duplex millimeter wave massive MIMO systems,” in Proc. IEEE GLOBECOM, Madrid, Spain, Dec. 2021.

[9] ——, “Simultaneous data communication and channel estimation in multi-user full duplex MIMO systems,” in Proc. IEEE ASILOMAR, Pacific Grove, USA, Nov. 2020.

[10] Z. Xiao, P. Xia, and X.-G. Xia, “Full-duplex millimeter-wave communication,” IEEE Wireless Commun., vol. 24, no. 6, pp. 136–143, Dec. 2017.

[11] I. P. Roberts, H. B. Jain, and S. Vishwanath, “Equipping millimeterwave full-duplex with analog self-interference cancellation,” in Proc. IEEE ICC, Dublin, Ireland, Jun. 2020.

[12] V. Venkateswaran and A.-J. van der Veen, “Analog beamforming in MIMO communications with phase shift networks and online channel estimation,” IEEE Trans. Signal Process., vol. 58, no. 8, pp. 4131–4143, Aug. 2010.

[13] C. B. Barneto, T. Riihonen, M. Turunen, L. Anttila, M. Fleischer, K. Stadius, J. Ryynänen, and M. Valkama, “Full-duplex OFDM radar with LTE and 5G NR waveforms: Challenges, solutions, and measurements,” IEEE Trans. Microw. Theory Techn., vol. 67, no. 10, pp. 4042–4054, Aug. 2019.

[14] S. D. Liyanaarachchi, T. Riihonen, C. B. Barneto, and M. Valkama, “Optimized waveforms for 5G–6G communication with sensing: Theory, simulations and experiments,” IEEE Trans. Wireless Commun., Jun. 2021.

[15] C. B. Barneto, S. D. Liyanaarachchi, T. Riihonen, M. Heino, L. Anttila, and M. Valkama, “Beamforming and waveform optimization for OFDMbased joint communications and sensing at mm-waves,” in Proc. IEEE ASILOMAR, Pacific Grove, USA, Nov. 2020, pp. 895–899.

[16] S. D. Liyanaarachchi, C. B. Barneto, T. Riihonen, M. Heino, and M. Valkama, “Joint multi-user communication and MIMO radar through full-duplex hybrid beamforming,” in IEEE Int. Symp. Joint Commun. & Sensing (JC&S), Feb. 2021, pp. 1–5.

[17] M. Braun, C. Sturm, and F. K. Jondral, “Maximum likelihood speed and distance estimation for OFDM radar,” in IEEE Radar Conf., May 2010, pp. 256–261.

[18] J. P. González-Coma et al., “Channel estimation and hybrid precoding for frequency selective multiuser mmWave MIMO systems,” IEEE J. Sel. Topics Signal Proces., vol. 12, no. 2, pp. 353–367, Mar. 2018.

[19] K. Satyanarayana et al., “Hybrid beamforming design for full-duplex millimeter wave communication,” IEEE Trans. Veh. Technol., vol. 68, no. 2, pp. 1394–1404, Dec. 2018.

[20] H. Krim and M. Viberg, “Two decades of array signal processing research: the parametric approach,” IEEE Signal Process. Mag., vol. 13, no. 4, pp. 67–94, Jul. 1996.

[21] G. C. Alexandropoulos and M. Duarte, “Joint design of multi-tap analog cancellation and digital beamforming for reduced complexity full duplex MIMO systems,” in Proc. IEEE ICC, Paris, France, May 2017.