arXiv:2203.07693v1 [astro-ph.IM] 15 Mar 2022

J. Astrophys. Astr. (0000) 000: DOI

An Automated Pipeline for Ultra-Violet Imaging Telescope (UVIT)

S. K. Ghosh^{1,4,*}, S. N. Tandon^{2,5}, S. K. Singh^3, D. S. Shelat^{3,4}, P. Tahlani^3, A. K. Singh^3, T. P. Srinivasan^3,P. Joseph^5, A. Devaraj^5, K. George^{5,6}, R. Mohan^5, J. Postma^7, C. S. Stalin^5

1Tata Institute of Fundamental Research, Mumbai 400005, India 2Inter-University Centre for Astronomy & Astrophysics, Pune 411007, India 3Space Application Centre (ISRO), Ahmedabad 380015, India 4National Centre for Radio-Astrophysics (NCRA-TIFR), Pune 411007, India 5Indian Institute of Astrophysics, Bangalore 560034, India 6Ludwig-Maximilians-Universität, Munich, Germany 7University of Calgary, Calgary, Canada

*Corresponding author. E-mail: swarna@tifr.res.in

Received: date / Accepted: date

Abstract.

We describe a versatile pipeline for processing the data collected by the Ultra-Violet Imaging Telescope (UVIT) on board Indian Multi-wavelength astronomical satellite ASTROSAT.The UVIT instrument carries out simultaneous astronomical imaging through selected filters / gratings in Far-Ultra-Violet (FUV), Near-Ultra-Violet & visible (VIS) bands of the targeted circular sky field (∼ 0.5 deg dia). This pipeline converts the data (Level-1) emanating from UVIT in their raw primitive format supplemented by inputs from the spacecraft sub-systems into UV sky images (& slitless grating spectra) and associated products readily usable by astronomers (Level-2). The primary products include maps of Intensity (rate of photon arrival), error on Intensity and effective Exposure. The pipeline is open source, extensively user configurable with many selectable parameters and its execution is fully automated. The key ingredients of the pipeline includes – extraction of drift in pointing of the spacecraft, and disturbances in pointing due to internal movements; application of various corrections to measured position in the detector for each photon - e.g. differential pointing with respect to a reference frame for shift and add operation, systematic effects and artifacts in the optics of the telescopes and detectors, exposure tracking on the sky, alignment of sky products from multi-episode exposures to generate a consolidated set and astrometry. Detailed logs of operations and intermediate products for every processing stage are accessible via user selectable options. While large number of selectable parameters are available for the user, a well characterized “standard default” set is used for executing this pipeline at the Payload Operation Centre (POC) for UVIT and selected products are archived and disseminated by the Indian Space Research Organization (ISRO) through its ISSDC portal.

Keywords. telescopes: UVIT — instrumentation: pipeline

MS received 04 October 2021; accepted

1. Introduction

The ASTROSAT is the first Indian astronomical space mission which covers a wide range of the electromagnetic spectrum (Agrawal, 2006; Singh et al., 2014). This satellite carried five major scientific instruments to provide a platform for multiwavelength astronomy from a low earth orbit with a small inclination to the equator. Four instruments covered different energies of soft to hard X-ray astronomy while the fifth one, Ultra-Violet Imaging Telescope (UVIT), enabled astronomical measurements over wide instantaneous field of view with high angular resolution, in the ultraviolet region. A summary of characteristics for each of these 5 instruments on board ASTROSAT are presented in Table 1. The primary aim of UVIT is to simul-

© Indian Academy of Sciences 1

Page 2 of J. Astrophys. Astr. (0000) 000:

taneously image the desired region of the sky in Far-Ultra-Violet (FUV; 1300 – 1800 Å) and Near- Ultra-Violet (NUV; 2000 – 3000 Å) bands for a field of ∼ 28^′ diameter with a resolution ∼ 1.5^{′′} (Tandon et al 2017a & 2017b). The telescope for NUV band also provided for imaging in optical / visible band (VIS; 3200 – 5500 Å), whose primary aim was to provide improved aspect of the telescope bore site every second. All three bands simultaneously view almost identical region of the sky. More details of UVIT and its in-orbit performance are presented in Tandon et al. (2017c) and references therein. The NUV band went non-functional on March 30, 2018 and remained so despite multiple attempts to revive it.

The subject matter of this paper is the automated pipeline for processing of the raw data received from the instrument and the spacecraft to produce images for FUV and NUV in standard units. The processing involves two separate steps. The first step, called L1 (Level-1), processes the telemetery data to provide a bundle of data for each target of observation. The L1 data bundle for UVIT consists of Science (Imaging) data from all 3 Detectors and Auxilliary (Aux) data containing inputs regarding UVIT Filters and various information from Spacecraft Systems, e.g. time calibration, attitude of satellite reference axes, position in orbit, gyro signals, and house keeping information. The second process, called L2 (Level-2), uses the bundle provided by L1 to make images for FUV and NUV in standard units for use by astronomers. The process L1 is implemented at a centre of Indian Space Research Organization (ISRO), while the process L2, which is theme of this paper, is implemented at UVIT-Payload Operation Centre (UVIT-POC) at Indian Institute of Astrophysics, Bangalore. It is ISRO’s exclusive right & responsibility to operate, maintain and upgrade the archives for disseminating all scientific data products from UVIT (which includes both L1 & L2).

The motivation for this paper is as follows. It provides an authentic description of processes involved in the translation from the Level-1 to the Level-2, which uses this pipeline. The ISRO’s archive hosts the L2 products generated using a “default” set of selectable parameters which are optimal for catering to most general users. The present work not only explains the implications of these selections, but also provides details about various additional options some of which could be useful to researchers with specific science aim. In addition, for future refinements of the pipeline, this work provides the basic reference.

Structure of this paper is as follows. In Section 2, we present a brief overview of imaging operations with UVIT and the complete end-to-end flow of data beginning from their collection to the final products that are ready for scientific analysis and interpretation by astronomers. In Section 3, detailed description of all the processing steps involved in generating Level-2 starting from Level-1 data is presented (hereafter referred to as UVIT Level-2 Pipeline, UL2P). This section first describes the higher level structure of the software, and details of the lower level structure follow subsequently. Section 4 contains experience during commissioning the pipeline, selected sample results, success rates and yields of UL2P and their general archiving details. Section 5 presents a summary along with comments on possible further improvements for future.

2. Overview

2.1 Imaging with UVIT

The imaging components of UVIT include optics, detectors and filter wheels. The optics consists of twin identical Ritchey-Chretian telescopes as shown in Fig. 1. (more details can be found in Kumar et al 2012 a).

The detector system for each of the 3 bands consist of intensified C-MOS imager (Star-250; 512×512 pixels), whose gain can be configured through its high voltage settings. While a high gain deploys Photon Counting mode (PC; ∼ 29 frames/s for the full field) used for the two UV bands, a low gain effects Integration mode (INT; ∼ 1 frame/s) used for the VIS band. Details of these modes are available in the Appendix-1 (Sec. A1.1).

A single clock (among the 3 bands) is selected for the operational ease of inter-band time alignment.

The Filter Wheel Drive system of each band positions the selected filter (or grating) and is parked at a light blocking position when not in use.

The electronic controller for each band configures and operates the detector read out system. The key selections include : (a) size of the sky field - full field (512×512 pixels) or a smaller square window (100×100 / 150×150 / 200×200 / 300×300 / 350×350) for obtaining higher frame-rates, roughly in inverse proportion the number of pixels read ; & (b) the imaging mode (PC / INT).

The imaging sessions are scheduled only during dark part of any orbit to avoid scattered solar radiation. Every planned sky field undergoes

J. Astrophys. Astr. (0000)000: Page 3 of

Figure 1. Optical layout of the two UVIT Telescopes, UT-1 and UT- 2, each employing a pair of Primary & Secondary mirrors. The UT-1 is dedicated for the Far-UV (FUV) band. The UT-2 feeds the Near-UV (NUV) band via reflection of a beam-splitter and the Optical (VIS) band through it.

detailed checks for its safety against overexposure due to any unacceptably bright object in the field or moon within a cone of defined half angle from the axis. Additionally, onboard safety measures with autonomous swift action ensure detector safety against accidental exposure to bright field.

The spacecraft operations usually translate observations of a specific astronomical target, with the filter and window size, of a typical science proposal into a sequence of smaller segments of imaging sessions, i.e. Episodes, spread over multiple orbits, as a single orbit can support imaging for a maximum of ∼ 2000 seconds, primarily due to the requirement of dark side of the orbit, and other factors like angle constraint to avoid earth occultation, South Atlantic Anomaly etc can further curtail this duration.

2.2 End to end data flow

The Fig. 2 shows the scheme of onboard interfaces between the ASTROSAT spacecraft and UVIT for control of operations using commands as well as collection of data to be communicated to the ground station. In addition to planned operations, the spacecraft systems also process emergency situations and guides UVIT to a safe condition. The data collected correspond to sky images, status & settings of various parameters of subsystems and health monitoring.

A block diagram displaying data flow and interconnections on ground is presented in Fig. 3. After the required processing at the ISRO’s ground segment systems, the data for UVIT are provided as FITS files called Level-1 data. These includes Science Data from the three detectors, and all the additional information on UVIT and the SC (named Aux Data) necessary for the next processing step. All the parameters of the detectors are made available in the Science Data, and the Aux Data provides status & positions of the three filter wheels, time calibration table, orbital position, velocity, attitude information of the reference axes of the satellite, data from Gyros, and housekeeping information, at appropriate sampling rates.

Each observing session (Episode, for a specific band, filter & window setting), is no longer than ∼ 2000 s, i.e. dark part of an orbit. All the Level-1 data products (Science Data & Aux Data) for all the Episodes for a target are organized into a single bundle named as “merged Level-1”. In the merged bundle Science Data for each band are assembled in individual directories and all the Aux Data are assembled in another directory. The Level-2 pipelines uses the directories of Science Data and Aux Data along with the calibration data base for generating the final images in standard units and coordinates. The data on raw images are provided by Science Data, data on the filters and orientation of the satellite are provided by Aux Data. Data on variation of sensitivity over the field and geometrical distortions are taken from the calibration data base. Details of operations executed in the pipeline are described in Section 3.

Page 4 of J. Astrophys. Astr. (0000) 000:

Figure 2. Schematic of the UVIT Payload. The telescope UT1 (UT2 & a Beam Splitter) feeds all sub-systems for the FUV (NUV & VIS) band/(s). The sub-systems represent functionalities including the selection of desired Filter (or Grating), configuration of Detector read out & settings of its High Voltages, and two way data communications with the spacecraft.

3. Level-2 Pipeline

This section gives a full description of the pipeline. The section is divided in two parts: in the first part functionality of the pipeline is described fully, and in the second part the actual implementation is described. A list of acronyms used in this document as well as frequently used names for a few key user selectable parameters is presented in Table 2. Additionally, a complete list of all parameters are available at the very end (Appendix-11). For most readers the functionality of the pipeline would suffice without going into the detailed description, which is full of many intricate technical details, unless they want to use / run the pipeline themselves for generation of the images.

3.1 Functionality

This sub-section provides a qualitative description of the operations carried out by the pipeline for generating the astronomer ready output products. This includes the primary aim, various inputs and the key processing steps. The terminology used here are as follows. The term “Step” has been introduced at the very highest level of description for ease of comprehension. A “Chain” refers to a completely stand alone sequence of smaller processing “Block”-s. The functionality of several Blocks used for different imaging modes and/ or Chains are similar, hence they have been implemented as “Modules” callable with appropriate selection of switches. The codes for remaining Blocks are embodied within respective Chains. Individual Chains are described in later sections 3.2.1, 3.2.2 & 3.2.3. While a few brief generic comments about Modules appear in section 3.2.7, individual Modules are described in Appendix 1 (Sec A1.1, to A1.20). The functionality of Blocks that are not Modules are given within the description of Chains.

3.1.1 Primary Aim of Level-2 Pipeline The UVIT Level-2 Pipeline (UL2P) is designed to translate ISSDC /ISRO provided Level-1 data (mL1) into science ready products in astronomer friendly format, utilizing instrument calibration database (CAL DB) as well as user settings of selectable parameters & switches (PIL) (see Fig 3). The pri-

J. Astrophys. Astr. (0000)000: Page 5 of

Figure 3. UVIT / ASTROSAT Ground Segment Systems. The UVIT Payload Operation Centre (POC) executes the Level-2 Pipeline using various inputs and generates the astronomer ready Sky Image Products & other outputs for archiving and dissemination.

mary products include the two UV sky image arrays as detected photon count rates in standard coordinate system (Right Ascension – Declination J2000) as well as primitive detector coordinate system (X-Y axes of the sensor) for every imaging Episode. The corresponding Uncertainty Arrays and sky Exposure Arrays are also generated. The subsidiary products include time series of spacecraft drift, photon centroid list for the image with flat field weight, etc. In addition to the above products for every Episode of observation, similar products are generated, by combining data for all the Episodes, for the total exposure (in all the orbits) with identical Filter-Window combination. The above is achieved through an one time run of a fully automated Driver Scheme, using a single configuration file for user selections.

3.1.2 Input Data There are three types of inputs required for running the pipeline, viz., the bundled Level-1 data (merged Level-1; mL1), the calibration database (CAL DB) and the user settings of all selectable parameters and switches (Parameter

Interface Library; PIL).

The mL1 represents collection of all data pertaining to one specific pointing of the spacecraft to the astronomical target (referred to by an unique Observation ID, ObsID). It consists of science data from all sky exposures executed by UVIT during that pointing as well as auxiliary data from the spacecraft systems (e.g. orbit & attitude information). The science data are packed as a sequence of “frame”-s, one for each individual short exposure. Their content depend on the mode of operation of the detector, viz., Integration (INT; used for VIS band; ∼ 1 frame per sec) or Photon Counting (PC; used for NUV & FUV bands; ∼ 29 fps). While the raw pixel values of the entire field (512x512) are preserved for INT mode, centroids (computed onboard) of individual detected photons constitute the frame for the PC mode. More details about exact contents of these data are available elsewhere (Appendix-1, Sec. A1.1).

An “Episode” of exposure in any band is defined as one continuous imaging session with a specific selection of filter and window size. Thus,

Page 6 of J. Astrophys. Astr. (0000) 000:

an Episode can either last the whole usable darkside of an orbit or a fraction of it in case the settings are changed. There is an option in the pipeline to divide the imaging duration of one Episode into multiple equal segments for processing independently. These segments are referred to as “Pseudo-Episode” individually. The nomenclature of grouping of science data used here is displayed in Fig. 4. The CAL DB contains organized datasets representing calibration arrays for each band (FUV, NUV & VIS) quantifying flat field correction across the detector, distortions, bad pixels, etc. The complete details of CAL DB are presented in Appendix-5.

The PIL is a single configuration file containing numerical values of all selectable parameters and ON/OFF settings of various switches. While complete details are available in Appendix-11, a few key parameters are also listed in Table-2.

3.1.3 The Processing Steps The generation of UV images from the inputs described above, involve the following main processing steps which are identical for NUV and FUV bands. 1) At first the drift of spacecraft pointing is estimated using stars detected in images captured in VIS frames (sampled ∼ 1 frame-per-sec, fps). There is an alternate provision for finding drift from NUV / FUV band data also in absence of VIS band data. 2) Next, individual UV frames are added to generate a cumulative image in the detector coordinates, after applying drift corrections and various instrumental corrections (which varies across the field of view) to the detected photons of each individual frame. Appropriate transformation is applied to generate the image in RA-Dec coordinates also. The corresponding Uncertainty to the UV image (from photon statistics) and the Exposure on the sky are also generated, which complete the set of image products. The above description is applicable for each single imaging session (Episode) lasting ∼ 2000 sec or less (see Fig. 5). 3) Image products from successive imaging sessions with identical combination of filter and window size (for the same UV band), are combined to generate the products for the total exposure by applying corrections for the relative shift and rotation determined using brigher UV stars detected in individual Episodes (described in a later sub-section named Driver Scheme, Sec 3.2.4; see Fig. 9).

The first two steps, #1 & #2 above are stand alone processing chains named - (i) the Relative Aspect chain which generates a time series of drift relative to position at some reference time as defined by the corresponding Reference Frame; (ii) the Sky Image chain which generates astronomical images & associated products. As the exposures can be taken either in photon counting (PC) mode or in integration (INT) mode, each of the chains has two versions (accordingly the chains are designated as : RA INT / RA PC & L2 PC / L2 INT). The last step (#3) is called Driver Scheme which combines images & associated products (Exposure & Uncertainty Arrays) obtained from all the Episodes, corresponding to the same combination of filter and window, after aligning them to correct for relative shift and rotation.

The key functionalities of these chains and the Driver Scheme are summarized along with their implementation in the next section (Sec. 3.2). The chains in turn call various processing Modules, whose technical descriptions appear in Appendix-1.

3.2 Implementation

This subsection provides various details of implementation of the pipeline. First the processing chains RA INT, RA PC & L2 PC and the Driver Scheme are summarized, followed by the strategy for addressing the situation of data loss in the input bundle as well as handling of special situations. Finally general concepts behind the design of modules are presented (details of individual modules can be found in Appendix-1).

The figures displaying the processing blocks of various chains follow a convention to distinguish Modules from rest by shading the latter (Fig.s 6, 7 & 8). In addition the blocks which have rarely been turned on are identified in the respective captions for the figure.

3.2.1 Relative Aspect chain for Integration mode (RA INT) : The purpose of this chain is to obtain time series of instantaneous shift and rotation of the field, relative to the position at any chosen time or set of frames, every second or so. This chain operates on VIS band data which are collected in INT mode. The typical accuracy obtained is ∼ 0.1^{′′} for the full field. The chain operates on data of one Episode at a time. Various steps of the processing are shown in Fig. 6 (RA INT) and are described below in the sequence in which they are executed and the numbers in parenthesis refer to the block numbers in that figure.

Data Ingest (1) : Import of all the user selected switch settings and values from a parameter file. Relevant data on calibration and on the exposure are taken from CAL DB and mL1 respec-

J. Astrophys. Astr. (0000)000: Page 7 of

Figure 4. Nomenclature for data groupings. Each “orbit” corresponds ∼ 100 minutes - the time taken by the spacecraft to go around the Earth once. The term “eclipse” refers to that part of every orbit when the spacecraft is in the Earth’s shadow blocking the Sun. UVIT observations are mandatorily scheduled during eclipses for instrument safety. The entire eclipse duration could either be used for sky exposure with a fixed settings for data collection leading to a single “Episode” or the time can be sub-divided into 2 or more exposures (with different settings) as per scientific needs. The pipeline has an option to sub-divide the data collected during one Episode into multiple pseudo-Episodes. The imaging data collection during an Episode involves repeated read outs of the detector - data corresponding to an individual read out is called a “Frame”.

tively. These data are: a) from calibration: the tables /arrays of bad pixels, distortions, flat-field, dark & exposure template; b) from mL1: i) science data originating from the instrument: frames of INT mode images in selected band, and ii) auxiliary data from the S/C: aspect of S/C, time calibration, house keeping information on instrument health, good-time /bad-time flags. Handling of discontinuities and abnormal data. Removal of engineering grade science data collected during gradual ramping up of the highvoltages at the beginning of the Episode, as per safety protocol. Extraction of individual image frames.

Artifact Handler (2) : The unexpected artifacts in the image and saturated pixels are flagged here enabling further processing to ignore them.

Dark Subtraction & Unit Conversion (3) : Subtraction of ‘dark’ frame from each individual image frame followed by conversion of the signal values from “count per exposure” to “count per second” unit.

Masking of Bad Pixels (4) : Flagging of the locations corresponding to ‘Bad Pixel’-s in every image frame.

Flagging Cosmic Ray affected pixels (5) : Identification of Cosmic Ray affected pixels (in every image frame) and their flagging.

Flat Fielding (6) : Multiplicative correction for non-uniform response across the field applied to all image frames.

Pixel Padding (8) : Expansion of all images from 512×512 to 600×600 size by symmetrically adding pixels along all four sides populated with a flag. This enlargement allows accommodation of movement of the instantaneous sky field due to spacecraft drift over the duration of the Episode. While this functionality is not explicitly required in this Chain, the corresponding Module (& also the following processing steps) being common with the Sky Imaging Chain, this step is retained to keep the array dimensions compatible.

Image Accumulation (9) : Selection of time step for drift computation by accumulating and averaging selected number, N acc, of successive image frames generating a series of accumulated frames, Acc frame.

Detection of stars & finding Centroids (11) : Analysis of individual image Acc frames to identify stars using an algorithm which uses dynamic

Page 8 of J. Astrophys. Astr. (0000) 000:

Figure 5. Schematic diagram showing generation of UV sky image corresponding to a single uninterrupted observing session called Episode. Starting with Level-1 data for the Episode along with UVIT calibration data (CAL DB) & user selected options (PIL), two stand alone processing chains (Relative Aspect chain, RA INT or RA PC; & L2 PC) generate the output products. Actions in the first block (Relative Aspect chain to extract drift of the spacecraft) include : correcting for artifacts & detection of stars in raw VIS images for RA INT (& similarly from UV images generated by stacking photon centroids, in case of RA PC) applying corrections to star centroids for instrument effects (distortions), determine drift (shift & rotation) as a function of time (from centroids) in Detector coordinates and finally convert to spacecraft coordinates. The second block (Sky Imaging chain to generate UV sky image & other products) begins with input UV data (list of centroids of photon events), flags affected events for rejection, computes event weight to include flat field, applies corrections to centroids for various systematic effects of the instrument & drift (applicable for corresponding time instance) determined in the first block, to obtain true sky arrival directions of individual UV photons. The UV sky image is generated by accumulating individual photons in both the Detector and Astronomical coordinates directly. Corresponding Uncertainty (from photon statistics) as well as sky Exposure maps are also generated.

threshold, distribution of light around local maxima and neighbourhood criteria. Computation of X & Y centroids for every detected star and intensity ordered tabulation.

Correction for Detector Distortion (12) : Application of additive corrections to the centroids of stars for the detector distortion.

Correction for Optics Distortion (13) : Application of additive corrections to the centroids of stars for the distortion due to telescope optics.

Identification of Reference Frame & Binning of time step (14) : Selection of timing reference for drift computation process, by identifying a particular Acc frame to be the Reference Frame, RF (by skipping the initial N skip number of Acc frames). Beginning with the RF and till the end of the Episode, an additional level of binning of time step is carried out optionally, by averaging star centroids exytracted from N avg number of successive

Acc frame-s. (For default usage, N avg = 1).

Drift Computation (15) : Computation of time series of relative drifts (shifts along X & Y axes and a rotation about the central pixel) from the differences in centroids of matching stars tabulated for successive time samples. The centroids for multiple stars are used in a least square fitting scheme having a choice of either equal or intensity based weighting. A manual mode of inter active selection of stars is also available to mitigate rare situations arising due to residual artifacts in the image data unaddressed by the handler block (#2). Subsequent translation of these drifts for every time sample to the integral drifts, with respect to the timing reference corresponding to the Reference Frame.

Time Domain Filtering (16) : The time series of drift in three variables (x_{shift}, y_{shift} & θ) are lowpass filtered in time domain, with user selectable parameters for smoothening them.

J. Astrophys. Astr. (0000)000: Page 9 of

Figure 6. Schematic block diagram of the Relative Aspect chain for Integration mode (RA INT). The block numbers 7 and 10 have never been turned on (except for testing & validation). The manual mode of star selection is not shown. The shaded blocks do not belong to any Module.

Generation of Relative Aspect Series (17) : The time series of drifts are tabulated as Relative Aspect Series, RAS, in Detector (X, Y , θ) as well as Spacecraft (Roll,Yaw,Pitch) coordinates systems as finalproduct from this RA INT chain.

The Appendix-8 presents the directory structure of final products from the RA INT chain.

3.2.2 Relative Aspect chain for Photon Counting mode (RA PC) : The aim of the RA PC chain is identical to that for the RA INT chain, but its functional details are different since it operates on the data collected in Photon Counting mode (e.g. when NUV or FUV data is used to obtain the time series of drift, Relative Aspect Series). This chain also operates on data of one Episode at a time. Various steps of the processing are shown in Fig. 7 (RA PC) and are described below in the sequence in which they are executed.

Data Ingest (1) : Similar to the case of RA INT (see above), except that the science data originating from selected band of the instrument operated in PC mode consist of a table with details of individual photon events detected in successive exposed frames in the Episode. These details (e.g. centroids) are generated from the raw frames, through on board processing. In this step, a master table of photon events along with relevant data is created.

Flagging of events in Bad Pixels (2) : A column is appended to the master table which holds the Bad Pixel flag. The events with their X & Y centroid coordinates overlapping with any of the bad pixels are flagged. Later processing steps ignores the flagged events.

Pixel Padding (3) : The centroid coordinates are modified to translate their range from (1 to 512) to (1 to 600) along each axis thereby effectively incorporating symmetric padding along all four sides. This allows accommodation of movement of the instantaneous sky field due to spacecraft drift over the duration of the Episode. Here again, this step is retained for compatibility of the shared Modules between the Relative Aspect & Sky Imaging Chains.

Rejection of Cosmic Ray affected frames (4) : Identification of individual frames affected by showers due to Cosmic Ray events and discarding all events in them. The process uses statistical distribution of number of events in all frames of the Episode and user selected parameters to arrive at

Page 10 of J. Astrophys. Astr. (0000) 000:

Figure 7. Schematic block diagram of the Relative Aspect chain for Photon Counting mode (RA PC) The block number 8 has never been turned on (except for testing & validation). The shaded blocks do not belong to any Module.

the threshold value for flagging. This rejection is useful for dark fields where contribution of showers to the background of photon events can be a large fraction of the total. If the rejection is not desired, the parameters can be set accordingly.

Centroid Bias correction (5) : Application of corrections for systematic bias, due to use of a simple algorithm on board, to the centroid values.

Flat Fielding (6) : The ‘Effective Number of Photon’ (ENP) for every event is changed from its initial value of unity by application of multiplicative correction for non-uniform response across the field.

Unit Conversion (7) : The entries for all events are modified from ‘ENP per frame’ to ‘ENP per second’ unit.

Correction for Detector Distortion (9) : Application of additive corrections to the centroids of photon events for the detector distortion.

Correction for Optics Distortion (10) : Application of additive corrections to the centroids of photon events for the distortion due to telescope optics.

Frame Integration (11) : Transformation of centroid coordinates for all photons from (600, 600) range to (4800, 4800) to implement pixel subdivision. Generation of a time series of two dimensional sky image arrays, Comb frame (4800×4800), by accumulating photon events from selected number of consecutive frames (N combine). The functionality of this selectable parameter N combine for this RA PC chain is equivalent to the parameter N acc for RA INT chain. The distinct nomenclature is chosen to emphasize the large difference in their typical values (N acc ∼ 1; N combine ∼ 30).

At this stage of processing of the RA PC chain, 2-D sky images are available starting from PC modedata. Accordingly, the subsequent steps leading to extraction of drift are very similar to the corresponding steps of RA INT.

Detection of stars & finding Centroids (12) : Similar to that for RA INT chain (step #11) above.

Identification of Reference Frame & Binning of time step (13) : Similar to that for RA INT chain (step #14) above.

Drift Computation (14) : Similar to that for RA INT chain (step #15) above.

Time Domain Filtering (15) : Similar to that for RA INT chain (step #16) above.

Generation of Relative Aspect Series (16) :

J. Astrophys. Astr. (0000)000: Page 11 of

Similar to that for RA INT chain (step #17) above.

3.2.3 Sky Image chain for Photon Counting mode (L2 PC) : The Sky Image chains L2 PC and L2 INT generate astronomical images for observations carried out in Photon Counting and Integration mode respectively . Primary aim of UVIT is to image in NUV and FUV bands, both of which are observed in the PC mode. Hence, the functionality of only the L2 PC chain is presented here, which is the more significant among the two versions.

The L2 PC chain processes data from one Episode and one band (NUV / FUV) at each instance. The Fig. 8 displays the schematic block diagram for this chain. Its steps are described below in the sequence of their execution. Certain steps here are similar to corresponding steps in the RA PC chain described earlier.

Data Ingest (1) : Importing selected switch settings and parameters, calibration and exposure data, spacecraft aspect, time calibration, etc. as well as science data (see step #1 of RA INT & RA PC for details). Generation a master table of all photons along with their details for the entire Episode.

Creation of Exposure Template (2) : The master templates of sky exposure are created for every combination of band, mode and window size by carrying out pixel sub-division of corresponding arrays available from the CAL DB. The resulting sky Exposure Template arrays are of 4800×4800 size. In order to track true exposure of the sky on the detector, the relevant master array will be offset according to drift corrections applicable for the time instances and stacked together in a later processing block.

Flagging of events in Bad Pixels; & with Multi- Photon signature (3) : Flagging of events with centroids located within a Bad Pixel (similar to step #2 of RA PC). Identification of potential multiphoton cases from event details along with user selected parameters and flagging them- this selection has never been used.

Pixel Padding (4) : Modification of the centroid coordinates of photon events by translating their range from (1 to 512) to (1 to 600) to accommodate spacecraft drift (similar to step #3 of RA PC).

Pixel Sub-Division of centroids (5) : Transformation of centroid coordinates for all photons from (600, 600) range to (4800, 4800) by pixel subdivision.

Rejection of Cosmic Ray affected frames (6) : Identification and rejection of frames affected by Cosmic Ray showers (similar to step #4 of

RA PC).

Centroid Bias correction (7) : Application of corrections for systematic bias to the centroid values (similar to step #5 of RA PC).

Flat Fielding (9) : Application of multiplicative correction for non-uniform response across the field (similar to step #6 of RA PC).

Unit Conversion (11) : The entries for all events are modified from ‘ENP per frame’ to ‘ENP per second’ unit (similar to step #7 of RA PC).

Correction for Detector Distortion (12) : Application of additive corrections to the centroids of photonevents for the detector distortion (similar to step #9 of RA PC).

Correction for Optics Distortion (13) : Application of additive corrections to the centroids of photon events for the distortion due to telescope optics (similar to step #10 of RA PC).

Corrections for drift (14) : Extraction of corrections for spacecraft drift applicable to individual frames by time interpolation of the corresponding Relative Aspect Series, RAS. The RAS should be available from a prior run of the Relative Aspect chain (RA INT or RA PC) covering the time duration of the Episode. Application of drift correction (involving 2 shifts & a rotation) to centroids of the individual photons.

Generation of drift corrected Exposure Array/(s) (15) : Application of drift corrections to a time series of Exposure Template (generated in step #2 earlier) arrays, one each corresponding to every frame of the Episode or pseudo-Episode, and their accumulation leading to ‘Exposure’ array/(s).

Frame Integration (16) : Consideration of the entire Episode or division into multiple pseudo- Episodes each consisting of N combine consecutive frames, Comb frame (after discarding initial N discard frames). Generation of 2-D UV sky image/(s) by gridding every un-flagged photon of the Episode / (pseudo-Episode) onto 4800×4800 ‘Signal’ array/(s) as per its (X, Y) centroids in the detector coordinate system. Generation of corresponding statistical ‘Uncertainty’ array/(s), which ideally should be based on counting of photon events in each pixel but here it has been computed from the ‘Signal’ & corresponding ‘Exposure’ arrays. This approximation leads to a systematic error in the ‘Uncertainty’ due to variation of the Detector’s response across the field, which is <10% for central 24^′ diameter circle of the field (see Tandon et al 2017c, 2020).

Registration & Averaging (17) : Combination of multiple ‘Signal’, ‘Exposure’ & ‘Uncertainty’ arrays from pseudo-Episodes after aligning them for

Page 12 of J. Astrophys. Astr. (0000) 000:

Figure 8. Schematic block diagram of the Sky Imaging chain for Photon Counting mode (L2 PC) The block numbers 8 and 10 have never been turned on (except for testing & validation). The shaded blocks do not belong to any Module.

any relative shifts and rotation determined using brightest point sources detected in ‘Signal’ arrays. Conversion to physical units for entries in the final combined set of ‘Signal’ (count/second), ‘Exposure’ (second) & ‘Uncertainty’ (count/ second) arrays. All these arrays are of 4800×4800 size in the detector (X, Y) coordinate system.

It is noteworthy that this block is effective only if ‘pseudo-Episode’ option has been selected, in which the data from an Episode is divided into parts of selected size (default configuration of the pipeline does not exercise this option). The process of combining images involves transformation of individual sub-pixels (at 9600×9600, followed by 2x2 binning), unlike the use of individual photon centroids while combining multiple Episodes in the Driver Scheme described later (Sec. 3.2.4).

Image Flipping (NUV) (18) : Flipping the set of image arrays - ‘Signal’, ‘Exposure’ & ‘Uncertainty’, for the NUV band only, about X-axis to undo the effect of the folding plane mirror (see Fig. 1).

Transformation to astronomical RA-Dec coordinates (19) : Conversion from detector to astronomical coordinate system Right Ascension, Declination (ICRS J2000) using attitude information of the spacecraft, for all 3 image arrays. The UV image (‘Signal’) is re-generated by coordinate transformation of individual photon centroids to minimize any loss of angular resolution (in case pseudo-Episode option has not been exercised; else image sub-pixels are transformed). At this stage, the outermost regions of the nearly circular field is truncated based on sky exposure less than 10% of the peak exposure. The process of this truncation for all the three image arrays, viz., ‘Signal’, ‘Exposure’ & ‘Uncertainty’ are carried out consistently.

Astrometry using optical catalogue (20) : Correlation of bright stars detected in the UV image with USNO A2 optical star catalogue to determine astrometric corrections (shifts and rotation). Application of these corrections to all the 3 arrays, viz., ‘Signal’, ‘Exposure’ & ‘Uncertainty’, with improved absolute aspect. The probability of success for the astrometry step in this chain (for an individual Episode) is lower than that for the similar operation on the multi-Episode combined image in

J. Astrophys. Astr. (0000)000: Page 13 of

Driver Scheme (Section 3.2.4) with higher total sky exposure.

The Appendix-9 presents the directory structure of final products from the L2 PC chain.

3.2.4 Driver Scheme The Driver Scheme operates at the highest level of hierarchy of the data processing in the pipeline. It handles the entire merged Level-1 dataset (‘mL1’) at one go and carries out all necessary processing to finally generate the full set of final deliverable products for all 3 bands, for different pairs of filters and window sizes used in each band. Often to achieve a long exposure under identical configuration, the observations are carried out as a series of Episodes. The observations with same combination of filter & window size need to be segregated together to generate a single set of products consolidating the total integration time planned. The method employed to combine Episodes requires that individual Episodes are considered as single data chunks (& not sub-divided into pseudo-Episodes). This requires a few processing steps in addition to those handling individual Episodes, which are also executed in a systematic manner by the Driver Scheme. The Driver Scheme internally calls the Relative Aspect and Sky Imaging chains (described in Sec. 3.2.1 / 3.2.2 & 3.2.3) multiple times as required for any specific mL1 dataset. The Fig. 9 displays the functional details of operations of the Driver Scheme. The top level directories for the final products from this Driver Scheme along with additional information regarding next level contents corresponding to the multi- Episode “group”-s are presented in Appendix-10. Given a merged dataset (‘mL1’), the Driver Scheme identifies science data segments for the 3 bands which correspond to the same Episode (from time stamps). It is pertinent to note the role Reference Frame (described earlier in step #14 of RA INT; Sec. 3.2.1) plays in connecting data from the band used to extract the drift, usually VIS, but NUV in absence of VIS, and the band in which sky images are to be generated (NUV / FUV). It provides the critical timing reference for calculating drifts for each Frame of the UV bands from the time series of drifts generated by Relative Aspect chains.

Default configuration :

1) Identification of time ordered sequence of available Episodes of VIS band data (say, V1, V2, ... Vn).

2) Running of Relative Aspect chain for Integration mode, RA INT, using VIS band for tracking on each of these individual Episodes to generate corresponding drift series (RAS V, Relative Aspect Series from VIS). Label these drift series as RAS V1, RAS V2, ... RAS Vn and the corresponding time ranges to be TR1, TR2, .... TRn. All these RAS V products are available in individual sub-directories corresponding to each Episode, inside the directory “/uvit” (see Appendix-10).

3) Identification of data sets for individual Episodes of NUV band and any combination of Filter & Window size (N1, N2, .... Np), which have time overlap with any of the time ranges (TRi : i=1,2, ...n) for which RAS Vs are available from the previous step. Running of Sky Imaging chain L2 PC on each of these ‘p’ Episodes of NUV data. Flagging of the remaining Episodes of NUV band data (if any) which do not have time overlap with any of the time ranges (TRi : i=1,2, ...n), and label them as NF1, NF2, ... NFm. Products for individual Episodes are stored under unique directories (“/ NUV 1” etc; Appendix-10).

4) Similar to previous step #2 but for FUV band data. Identification of individual Episodes of FUV band and any combination of Filter & Window size (F1, F2, .... Fq), which have time overlap with any of the time ranges (TRi : i=1,2, ...n) for which RAS Vs are available from the step #1. Running of Sky Imaging chain L2 PC on these ‘q’ Episodes of FUV data. Flagging of the remaining Episodes of FUV band data (if any) which do not have time overlap with any of the time ranges (TRi : i=1,2, ...n), and label them as FF1, FF2, ... FFk. Products for individual Episodes are stored under unique directories (“/ FUV 1” etc; Appendix-10).

5) Execution of Relative Aspect chain for Photon Counting mode, RA PC, using NUV band for tracking on each of the flagged Episodes of NUV band data NF1, NF2, ... NFm (identified in step #2) to generate corresponding drift series RAS NF1, RAS NF2, ... RAS NFm. Label the corresponding time ranges of these RAS NFs to be TR NF1, TR NF2, .... TR NFm. All these RAS NF products are available in individual subdirectories corresponding to each Episode, inside the directory “/ RAPC” (see Appendix-10).

6) Execution of Sky Imaging chain L2 PC on each of the flagged Episodes (total ‘m’) of NUV band data NF1, NF2, ... using the corresponding drift series RAS NF1, RAS NF2, ... (generated in step #4). Products from this step are stored in additional directories in continuation with those generated at the step #2 above.

7) Execution of Sky Imaging chain L2 PC on those flagged Episodes of FUV band data among FF1, FF2, ... FFk, which have time overlap with any of the time ranges TR NF1, TR NF2,

Page 14 of J. Astrophys. Astr. (0000) 000:

Figure 9. Schematic diagram showing sequence of steps of Driver Scheme (Default case) which operates autonomously on the entire dataset for a specific ObsID (mL1; consists of many Episodes) and generates all requisite products in one go. An Episode represents the dataset from a single imaging session whereas collection of all imaging sessions during that particular pointing of the spacecraft to the target constitutes an ObsID. The two processing chains (each operating for a single Episode at a time), viz., Relative Aspect (RA INT /RA PC) and Sky Imaging (L2 PC) are used repeatatively. The former derives the spacecraft drift relative to a chosen reference direction. The latter generates UV images from detected photons after applying corrections for drift and instrument systematics. The Relative Aspect chain, RA INT, uses VIS data and in its absence, the RA PC version for NUV/ FUV data. Sky Image Products (UV, Uncertainty & Exposure arrays) corresponding to multiple Episodes with identical filter & window size are generated by combining data from individual Episodes.

.... TR NFm using the drift series generated using NUV data in step #4, viz., RAS NF1, RAS NF2, ... RAS NFm. Products from this step are stored in additional directories in continuation with those generated at the step #3 above.

8) After the executions of the Sky Imaging chain has been completed for all Episodes (completing all the 7 steps described above), their products are segregated for identical combinations of the 3 key parameters, viz., UV band, filter & window size, into “group”-s. A process attempts to combine all images in RA-Dec (ICRS) system from individual Episodes (with no subdivision into pseudo- Episodes) belonging to a particular group using the following steps : (i) Identify the Reference Episode, RE, with largest sky exposure, EXP TIME; (ii) Order the remaining ‘Other Episode’-s (OE 1, OE 2, ... OE n) in descending order of EXP TIME; (iii) Attempt to match brightest stars (avoiding outer annular region with sky exposure < 20% of peak) from RE with brightest stars from other orbits (OE 1, OE 2, ...) one by one. Let ‘k’ cases be successful (k ≤ n); (iv) Centroid coordinates of individual bright stars are used to determine relative Shifts & Rotation between each pair of (RE & OE j; j : 1, 2, ... k); (v) Application of identical shifts & rotation corrections to the centroids of to all photon events of the particular individual Episode (“OE j”); (vi) Application of shifts & rotation corrections to the corresponding Exposure arrays, which involve transformation of individual sub-pixels at 9600×9600 level and regridding. Generation of a combined Exposure array by stacking all ‘k’ components; (vii) Populating photon events into ‘aligned to RE’ arrays and convertion to combined Signal array (“count / second”) by pixel by pixel arithmetic operations including corresponding aligned and combined Exposure array; One important caveat deserves mention here : while the Exposure arrays from indi-

J. Astrophys. Astr. (0000)000: Page 15 of

vidual Episodes carry the 10% cut, the table of photons which populate ‘aligned to RE’ arrays do not. This leads to significantly erroneous values for Signal at the outer regions. For accurate photometry of stars /targets in such affected outer regions the three arrays, i.e. Signal array, Exposure array and Uncertainty array, from each Episode should be added with the shifts and rotations as applicable. (viii) Generation of the combined Uncertainty array. All products resulting from combining of multiple Episodes record in their headers a log identifying the Episode selected as RE, complete list of all the OE-s as well as the Episodes which contributed to these multi-Episode products. It is noteworthy that the final combined multi-Episode UV image (Signal array) is generated directly from transformed centroids of individual photons, just like for individual Episodes, thereby retaining their angular precision despite undergoing alignment operations involving rotation. However, the generation of Exposure and Uncertainty arrays do face some loss of precision, even though their impact is significantly reduced by employing pixel sub-division as described above. The process of combining observations from multiple Episodes includes a check on the difference in the Roll angle values (which is a slowly varying function of time) between the Reference Episode & each of the Other Episodes in order to mitigate their occasional incorrect entries for attitude noticed in the L1 data. This difference is required to be less than 2 degrees for the Episode to be considered for the combining step.

Products generated by this step, corresponding to individual “group” of multi-Episodes are stored under a directory name uniquely identifying that “group” (e.g. “/NUV Final F1 W511”; Appendix- 10).

9) Execution of Astrometry Module to determine finer corrections & apply them, to the sky coordinates of the multi-Episode combined image products (Signal, Exposure & Uncertainty arrays) for each “group” generated in the previous step. Astrometric corrections are determined by correlating stars identified from the Signal array with standard astronomical catalogues of stars. If successful, identical corrections (involving shifts and rotation of arrays through pixel sub-division, transformation & binning scheme) are applied to each of the set of 3 arrays. For more technical details about this Astrometry Module see Appendix- 1 (Sec. A1.20). Products generated by this final step for astrometry, for every “group” of multi- Episodes are stored under an unique directory (e.g. “/NUV FullFrameAst F1 W511”; Appendix-10).

Forced NUV tracking configuration : There is an additional option in the Driver Scheme to completely ignore the VIS datasets & use only NUV data for generating the drift series (RAS) & then make UV images of the sky (both NUV & FUV). In absence of NUV data, the FUV itself can also be used to generate RAS followed by making FUV images of the sky. The Fig. 10 shows possible cases arising due to different kinds of time overlaps between VIS & UV band Level-1 data. Normal situation as per observation planning is case ‘A’, which is ideal and handled using VIS data for tracking. However, sometimes other cases with partial (‘B’ / ‘C’) or no overlap (‘D’) are also noticed which occur due to details of data flow up to the generation of Level-1 data. While the ‘default’ setting of the Driver Scheme (tracking by VIS when any amount of time overlap exists, & force UV tracking when none exists) handles the cases A & D optimally, the remaining cases (B & C) lead to sub-optimal usage of data (limited the overlap part only). This is mitigated by forcing drift tracking with UV data on all the data (ignoring VIS completely). Of course, success with UV tracking critically depends on existence of at least one UV bright star within the field of view. Accordingly, the strategy followed at the UVIT-POC is to execute the Driver Scheme twice, once each with the two options (default & forced NUV tracking) and provide two sets of Level-2 products generated by them, allowing users the choice.

3.2.5 Strategy for missing data In the design of the pipeline, special emphasis has been given to incorporate graceful degradation in view of occasional loss of data at various stages of communication between UVIT and ground station as well as errors encountered in the input products from Level-1. For example – (a) in case of incomplete extraction of drift (e.g. due to large chunk of missing data), images are generated using products for whatever duration they could be salvaged); (b) in complete absence of VIS data for any Episode, the drift extraction is automatically attempted using the NUV data itself; (c) the scheme for combining multiple Episodes, employs a logic which leads to best possible outcomes in the event of sub-optimal signal to noise situation; (d) crash situations of individual processes / chains do not hamper the pipeline from full exploration of the entire data set. The pipeline attempts to maximize the sky exposure translating to scientifically useful products in spite of the limitations in the input data and artifacts therein. The pipeline has been implemented

Page 16 of J. Astrophys. Astr. (0000) 000:

Figure 10. The extraction of spacecraft Drift using VIS & NUV data under different situations of time overlap between sky exposures of VIS and NUV bands. The logic used under “Default” settings of the Driver Scheme, viz., use VIS when any time overlap with UV imaging exists, leads to sub-optimal results for Cases ‘B’ & ‘C’. This is avoided with “forced” NUV tracking. Accordingly, pipeline products generated using both these strategies are provided for the users (when NUV data are available).

primarily in C++ with total ∼ 30,000 lines of code.

3.2.6 Handling special situation An Episode of observation has been defined earlier as an uninterrupted period of data collection. The input Level-1 science data for an Episode consisting of time sequence of image frames however often show multiple types of anomalies – e.g. missing part / full frames, discontinuities in frame number, frame time & other artifacts. Most such issues have been addressed by gradually improved algorithms incorporated in the Data Ingest block of the pipeline during early in orbit Performance Verification phase of ASTROSAT & UVIT (see Appendix-1, Sec. A1.1 for details). The term pseudo-Episode has also been introduced as the user chooses to divide the data from a normal Episode into multiple parts, Comb frames (N combine frames each), to technically address possible misalignments at shorter time scales. For example, when the temporal evolution of spacecraft drift in a particular Episode includes discrete large and fast drifts components, division into pseudo-Episodes is useful. Another example of forced use of pseudo-Episode due to a different reason follows. Under some specific situation arising out of design of UVIT hardware as well as software preceding the pipeline, even a single uninterrupted data collection needs to be subdivided into smaller pseudo-Episodes (for example : 16-bit Frame Counter overflow in ∼ 100 s, during PC mode imaging with the smallest window size 100×100), each holding consecutive 2^{16} frames. The last pseudo-Episode would in general contain a smaller number of frames. The pipeline treats each pseudo-Episode at par with a normal Episode.

3.2.7 Modules The pipeline has been implemented in a modular fashion keeping in mind several blocks of processing are common to different chains and their versions based on imaging mode. Accordingly these are implemented as stand alone Modules for flexibility of being called by different chains. Whenever relevant, these Modules internally support both the imaging modes, viz., Integration (INT) & Photon Counting (PC). Many of them can be turned ON or OFF depending on the user need and / or enabling testing, diagnosing and evaluation. The resulting products from each Module follow a naming convention with name suffix embedded in them. A master list of all the Modules, their functionality and linkages to different chains are presented in Table 3. The large number of selectable switches and variable parameters used by these Modules are provided in Appendix-11.

J. Astrophys. Astr. (0000)000: Page 17 of

Some generic comments on Modules follow prior to their description. Every Module has several primitive switches regarding overwriting of existing file structure (‘clobber’), inclusion of complete log of operations on product headers (‘history’), choice for timing reference - using the Universal Time Clock or UVIT’s Master Clock (‘utcFlag’), storing outputs from individual block (‘Write to disk’ flags), etc. The headers of every product from individual Modules record settings of all selectable switches and parameters. In addition, values of various corrections factors (e.g. events rejected due to parity error, CRC, etc), frames affected by Cosmic Ray showers & discarded, frames affected by artifacts in data, initial frames affected by mandatory safety checks which are discarded, etc. are logged in the headers. Every failure to achieve convergence or successful completion of any block is recorded in a master log with a message (including the text string “CRASH”) which helps to track it and relevant details for its later investigation and diagnosis. Individual Modules are described with full technical details in Appendix-1. They are presented in an order following their sequence of appearance in the chains for drift extraction – Relative Aspect (RA INT & RA PC; section 3.1.4.1) followed by the Modules exclusively for the chains for Sky Imaging (L2 PC & L2 INT; section 3.1.4.2). In general, within every Chain, almost all Modules process all the frames of an Episode before transferring control to the next Module (only exceptions being the sequence of blocks 10, 11, 12 & 13 in RA INT chain which form a looping segment; see Fig. 6).

There is also a library of utilities that are commonly used by several Modules & processing blocks.

4. Commissioning experience, operation

and performance of the pipeline

Extensive testing of each Module / algorithm as well as the four chains have been carried out over an extended period. This began with data collected in the laboratory in the year 2015, well before the launch of UVIT/ ASTROSAT. The spacecraft drifts were simulated with jigs created to generate relative motion between a UV source and the detector assembly. Most debugging could be completed only after launch with in-orbit data from Performance Verification phase. Some tweaking of strategies and choices of algorithms were also needed. Many of the parameters related to instrument characteristics were refined based on the data from in-orbit calibration, whose starting values were from lab tests. Two noteworthy parameters which needed most careful and laborious analyses are : (i) Relative shifts between time stamps of the frames in the three bands – these are required for translating time-series of the drift derived from one band, e.g. VIS, to the other bands, e.g. NUV and FUV, & (ii) relative angles between the coordinate system (X-Y axes) among the three detectors as well as with respect to the spacecraft coordinates (Yaw-Pitch). A common Master Clock (from the selected band) is used by all the bands for time stamping individual frames. The time offsets between the NUV (or FUV) band (irrespective of window size selection) with respective to the VIS band (as well as between NUV & FUV bands, which is needed in case of drift tracking using NUV) have been calibrated. These are presented in Appendix- 2. The details of relative angles between coordinate systems are presented in Appendix-3.

The UL2P described above have been in regular use at the UVIT Payload Operation Centre (POC) for generating standard bundle of products for archiving and dissemination to the community of astronomers by the ISSDC. The UVIT Driver Module is executed twice on each merged Level-1 data set – once using VIS band for drift extraction (RA INT chain) and the other time forcing the use of NUV band for extracting drift (RA PC chain). A nominal set of default parameters are used for both the runs. The standard bundle of products for dissemination is selected by the POC & ISSDC, which includes the most important items required by common end users (astronomers). The Table 4 list all contents of this bundle. It includes products for each combination of UV Band, Filter & Window size from individual episode as well as combined over multiple episodes (for details see Appendices 2, 3 & 10). For the single episode case, constituents are : Drift series (RAS; final output of RA INT/ RA PC chain; from ‘uvt- ComputeDrift’ directory; Event list (including final centroids in both Detector & Astronomical coordinates; from ‘uvtShiftRot’ directory; one final post-Astrometry UV sky map (Signal; RA-Dec; ICRS; J2000; from ‘uvtFullFrameAst’ directory), and three pre-Astrometry sky maps of UV (Signal), Exposure & Uncertainty (all in Detector X- Y coordinates; from ‘uvtFlippedRegImage’ directory). For the combined multi-episode case the constituents are : one final post-Astrometry UV sky map (Signal; RA-Dec; ICRS; from the directory like - ‘XUV FullFrameAst F1 W511’, where X=F

Page 18 of J. Astrophys. Astr. (0000) 000:

or N for FUV and NUV respectively), and three pre-Astrometry sky maps of UV (Signal), Exposure & Uncertainty (all in Detector X-Y coordinates; from the directory like ‘XUV Final F1 W511’). There are two sets of these above constituents – one set each for drift extraction using VIS & NUV. The above is further repeated for each combination of UV Band, Filter & Window size. The complete details of all products (including the standard bundle) from the pipeline are presented in Appendices 2, 3 & 10. The current version (v6.3) of UL2P described here has been in use at the POC since mid 2018. Prior to that, an earlier version (v5.7) was in use.

The UL2P is completely open source and its distribution has been simplified by creating an “Installer” compatible with most Unix operating systems. Relevant instructions for installation and other related information are publicly available for download from multiple sites (https://uvit.iiap.res.in/Downloads; http://astrosat-ssc.iucaa.in/?q=uvitData; https://www.tifr.res.in/~uvit/). Two caveats must be noted by users of this pipeline. 1) As has been mentioned earlier (Sections 3.2.3 & 3.2.4) the precision of photometry in multi-Episode UV images for the outmost regions, are compromised by the fact that Exposure arrays from individual Episodes undergo a cut (< 10%) but not the corresponding photons while combining Episodes; 2) The scheme of applying large angle rotation to the Exposure array (e.g. from Detector X-Y system to astronomical RA-Dec coordinate system) leads to small but detectable artifacts of repeated patterns with amplitude ∼ few percent. Both these issues have been discovered rather recently and they will be addressed in the next upgrade of the pipeline. The corrective measure for #1 will include applying the exposure based cut (< 10% of peak) on the Signal (unit : count /second) array only (i.e. leaving Exposure & Uncertainty arrays without any cut) at the individual Episode processing level. This will preserve photometric precision of the multi-Episode arrays generated by the Driver Scheme. For the #2, an improved logic for mapping pixels from pre- to post-rotation Exposure arrays will be employed.

Next, some typical examples of results are presented. Figure 11 displays two typical examples of drifts extracted (along Detector X & Y axes) by the Relative Aspect chain RA INT using VIS band data. It spans ∼ 1200 / 1500 seconds of time. The peak to peak variation of drift is around ∼ 160 arc seconds. The sharp spikes (positive in one & negative in another) observed in these plots appear at regular intervals corresponding to systematic jerks imparted by planned mechanical movement of the payload Scanning X-ray Sky Monitor (SSM). The drift extraction process has been able to successfully mitigate any major adverse effect of such rather harsh disturbances on the PSF.

Next, as an example we present UV images of an astronomical source, viz., the nearby spiral galaxy NGC 300 at a distance of ∼ 1.9 Mpc, processed by the pipeline to demonstrate its efficacy. The Far- UV image is displayed in Fig. 12, which uses 14,300 s exposure with in the filter F148W (λ_{mean} = 148.1 nm, Δλ = 50 nm). The Fig. 13 shows a colour composite Near-UV image of NGC 300 using observations with exposures of 20,000 s in filter N242W (blue; λ_{mean} = 241.8 nm, Δλ = 78.5 nm) & 2,500 s in filter N263M (green; λ_{mean} = 263.2 nm, Δλ = 27.5 nm).

While these sample images show the utility and success of the pipeline in extracting astronomically significant high quality images qualitatively, the POC carries out systematic analyses of the products to quantify their quality objectively. The performance of this Level-2 pipeline has been reported by Ghosh et al. (2021), which had used UVIT observations carried out till mid-2020. Here we have updated it including the latest status.

The FUV and NUV images generated by the pipeline are analyzed for Point Spread Function, PSF, for a minimum of three stars (point sources) spread over the entirefield of view. The extensive in-orbit calibrations have characterized the PSFs for both the FUV and NUV bands by a compact central core and an extended pedestal (Tandon et al 2017c, 2020). Based on these anticipated structure of the PSFs a quality score has been defined. The criteria followed to assign the quality score are : the best score of ‘10’ is assigned if the pedestal is < 20% and the full width at half maxima, FWHM, of the PSF is < 1.6 arc-sec; similarly ‘9’ & ‘8’ correspond to FWHM being < 1.8 arc-sec & < 2.0 arcsec, respectively. For every increase in the pedestal by 5% (beyond 20%), the quality score is reduces by 2. This score is estimated for both the bands (FUV and NUV) and the mean of these values is quoted in the quality report which always accompanies the UL2P product bundle. The distributions of quality score in FUV & NUV bands for all observations carried out till recently (09-Dec- 2021) are shown in Table 5. As can be seen, the pipeline products for NUV band achieve a quality factor of 9 or above for ∼ 90% of observations. For the FUV band, this fraction is relatively lower at ∼ 54%, which increases to ∼ 66% if the quality

J. Astrophys. Astr. (0000)000: Page 19 of

Figure 11. Two examples of drifts extracted by the Relative Aspect chain RA INT from VIS data spanning 1200 / 1500 sec. The peak to peak movements are ∼ 160^{′′} (1 pixel ∼ 3.3^{′′}).

factor of 8 or above are considered. The relative superiority of the quality score of images in NUV over FUV is related to the fact that the UVIT instrument achieved better angular resolution in the NUV band. Since the NUV band shares the same telescope with VIS band and FUV uses a separate dedicated telescope (see Fig. 2), a possible cause could be temporal changes in the relative angle between the two telescope structures within the time scale of an orbit. Activating the ‘pseudo-Episode’ option for L2 PC chain for the FUV band may improve its quality score.

One of the key parameters quantifying eventual success rate of the UL2P is the fraction of total on sky exposure finally contributing to the UV image product. The ASTROSAT operations group schedules sky exposures based on approved time allocated (say T MCAP), for a particular target from a scientific Proposal. Let the Level-1 data successfully generated at the ground station of ISRO be for duration T L1. This forms the input for the UL2P. Let the final UV image product generated by UL2P be T L2 (somewhat like EXP TIME keyword in header). Then yield of UL2P (for that particular episode of observation) can be defined by the ratio - (T L2 / T L1). The distribution of this yield for both NUV & FUV observations carried out till recently (09-Dec-2021) are presented in Table 6. The fraction of all pointings in this sample achieving yield above 0.9 (0.8) is ∼ 72% (86%) for the NUV band. The corresponding fraction for the FUV band is ∼ 75% (88%). These values indicate that there is scope for improvements in the pipeline.

5. Summary and possible future improvements

A versatile data processing pipeline (UL2P) has been developed for the UVIT payload on board ASTROSAT satellite. This pipeline runs in a fully automated mode and is ideally suited for the Payload Operation Centre, where huge amounts of data collected from UVIT need to be processed swiftly without human intervention. The pipeline generates astronomer ready sky images in UV. Its main components are : handling of occasional artifacts and anomalies in Level-1 data, extraction of spacecraft drifts, and disturbances due to internal movements; application of various corrections to measured direction of arrival for each photon – e.g. spacecraft motion (with respect to planned inertial pointing towards target direction), systematic

Page 20 of J. Astrophys. Astr. (0000) 000:

Figure 12. Far-UV image of the Spiral galaxy NGC 300 generated by the pipeline using exposure of 14,300 s with the filter F148W (λ_{mean} = 148.1 nm, Δλ = 50 nm).

effects and artifacts in the optics of the telescopes and detectors, exposure tracking on the sky, alignment of sky products from multi-episode exposures to generate a consolidated set and astrometry. Detailed logs of operations are maintained on headers of products and intermediate products for every processing stage are accessible via user selectable options. This pipeline has been tested extensively before releasing for regular use at the Payload Operation Centre (POC) located at the Indian Institute of Astrophysics (IIA), Bangalore. Every UVIT dataset from ISRO/ISSDC is received by the POC which after processing sends the corresponding standard products back to ISRO/ISSDC for archiving and dissemination. The current version of UL2P described here has been in use since February 2018 and has continued to successfully generate relevant products for the astronomer community leading to scientific results world wide. While large number of selectable parameters are available for the user, a well characterized “standard default” set is used for executing this pipeline at the Payload Operation Centre (POC) for UVIT and selected products are archived and disseminated by the Indian Space Research Organization (ISRO) through its ISSDC portal. Users preferring to use selections of parameters different from the “standard default”, can download, install and run UL2P themselves following instructions provided online. There are a few areas where improvements to this pipeline would help the end users. These include - (1) improvement in efficiency of combining multi-orbit images, (2) improvement in success rate for astrometry correction and (3) improvement in the precision of astrometry. Each of these improvements are linked to use of optical stars (from VIS images) instead of the current scheme of using UV stars detected in UVIT images with significant signal to noise ratio. The scientifically important research areas involving extremely faint fields will benefit most from these.

Appendix-1 : Modules used in the UVIT Level-2 Pipeline

This appendix provides complete technical details of the processing blocks used by the UVIT Level-2 pipeline. Given the two different available modes of imaging operations the processing chains have distinct versions for each of these modes. There are several computational blocks with commonality in their function among the chains / versions. Hence, such processes are captured as Modules with selectable switches and parameters to meet the requirements of all similar applications (see Table 3 for a list of all Modules and their linkages to different chains). A complete list of switches and parameters for these Modules is available in Appendix-11. The Modules are called by the chains and the resulting products from each Module follow a naming convention with name suffix embedded in them for ease of tracking as well as higher

J. Astrophys. Astr. (0000)000: Page 21 of

Figure 13. Colour composite NUV image of the Spiral galaxy NGC 300 generated by the pipeline using exposures of 20,000 s in filter N242W (blue; λ_{mean} = 241.8 nm, Δλ = 78.5 nm) and 2,500 s in filter N263M (green; λ_{mean} = 263.2 nm, Δλ = 27.5 nm).

level of scripting for autonomous operations. Individual Modules are described next, in a natural order of their sequence of appearance in the chains for drift extraction : Relative Aspect (RA INT & RA PC) followed by those exclusively for the Sky Imaging (L2 PC & L2 INT). There are 20 Modules presented below in sub-sections numbered : A1.1, A1.2, ... to A1.20. Every Module consists of several blocks operating in a sequence, and in general, each block operates on all the frames of an Episode before transferring control to the next block (with only exception of a few in the RA INT chain).

A1.1 DataIngest

The Data Ingest is the very first block for any of the processing chains and it prepares all inputs data for processing in the subsequent Modules. Its key functionality is to import input data, check its integrity, sort them into various groups / tables and carry out certain computations. It directly interfaces with the “merged Level-1” (mL1) data bundle which is the primary input to the pipeline, the Calibration Database, CAL DB, as well as the user selected parameter set (Parameter Interface Library; PIL).

First a brief description of the contents of input data bundle mL1 is presented. The mL1 contains all the Level-1 data products Science Data

& Aux Data for the same Observation ID (ObsID; it includes Proposal ID, Target serial number & Pointing sequence number) in an organized manner. Generally the observations corresponding to a specific ObsID lasts multiple successive orbits. The directory structure of a representative data set (mL1) is shown in Appendix-4. The Appendix- 5 shows the directory structure of the Calibration Database, CAL DB. The notation followed to represent multi-level directory structure in Appendix-4 as well as similar other Appendices (5 to 10) is as follows : a normal dash symbol represents files in current directory and a longer horizontal shift or dash represents the next lower sub-directory (followed by the sub-directory name) & the lines immediately following it give contents of that subdirectory. A few files with very long names are broken into two lines with the second line beginning with a large number of dots.

The Science Data are segregated into the three band wise directories. These directories in turn host multiple sub-directories, each of which correspond to one specific “Episode” of data collection. Each sub-directory is populated by 3 files (FITS tables), the imaging data and two files (GTI & BTI) containing flags for a large number of parameters pertaining to the spacecraft & UVIT.

The imaging data are packed as a sequence of

Page 22 of J. Astrophys. Astr. (0000) 000:

“frame”-s, one for each individual exposure, preserving their time order. Each frame comprises of an integral number of fixed size “packets” (2048 bytes) whose contents and format depend on the imaging mode (INT/PC) configured. Each packet begins with the Synchronization Mark, Primary Header and a Secondary Header (includes an Image Frame Counter & various other Counters with timing information) followed by 2016 bytes of image data & ending with a parity-code (CRC). The very first packet of every frame always holds the data for all settings for the Detector Module and the data for system status and health monitoring only. The second packet onwards contains image data. The total number of packets in any frame, N_p depends on the imaging mode. The last packet for the frame usually needs padding to complete the stipulated fixed size (2048 bytes). In case of Integration mode (INT), the raw pixel ADUs (2- bytes per pixel) are packed in the usual sequence of 2-D array covering the entire selected window region. Hence, the value of N_p is always predictable for INT mode, e.g. maximum value of 262 corresponds to full 512×512 window setting. On the other hand, in Photon Counting mode (PC), the raw pixel signals are processed on board to identify individual photon event and compute its centroid along two detector based axes (X, Y). After this processing, the data from the frame comprises of all extracted photon events packed as a sequence, with each photon event contributing 6 contiguous bytes. Accordingly, each packet can accommodate up to 336 photons. As a result, the value of N_p in PC mode may vary from frame to frame, since it depends on the total number of photon events identified. The contents of the 6 bytes for every detected photon event are : centroid along X (2 bytes), centroid along Y (2 bytes), measures of asymmetry in the raw event foot-print & local background (2 bytes).

The Auxiliary (Aux) data correspond to the entire time duration covering the full merged data set. They are FITS tables containing uninterrupted continuous time series of various measured / derived parameters mostly originating in spacecraft sub-systems. Examples of Aux data that are used directly by the pipeline follow. The time correlation between the spacecraft’s clock (raw & calibrated) and internal clocks of UVIT (‘*.tct’). The attitude of the spacecraft : tabulated as quaternions representing rotation angles with respect to reference coordinate system - Roll, Yaw & Pitch (‘*.att’). The signals from the angular rate sensors (Gyros) for the 3 axes (Roll, Yaw & Pitch) which are tabulated separately (‘*.gyr’).

The Fig. 14 provides the sequence of operations carried out by Data Ingest. DataIngest initially carries out the following functions - (i) import mL1 data, (ii) set up structured paths for Science data and AUX data, (iii) establish links to Calibration Database, (iv) import and interpret settings of various user selectable switches and values of parameters, from Parameter Interface Library, PIL, queries.

As a part of check on data integrity at a primitive level, the user selected action is carried out on individual data packets which failed the CRC test. Next, the headers of individual science data blocks corresponding to distinct Episodes are interpreted for various settings : respective observing Band, imaging Mode, Filter, the band selected for Master Clock. For each Episode, a time correlation between UVIT’s Master Clock and the absolute time (Universal Time Clock, UTC, stamped by the Level-1 process) is constructed. Occasionally, the UTC shows erratic behaviour. Even when user selects to use the UVIT clock (i.e. with ‘utcFlag’ switch is OFF), a robust error tolerant scheme has been employed to establish a scheme capable of predicting Modified Julian Date (MJD) from UVIT clock, albeit with limited precision (∼ 1 s).

Next step deals with identification and treatment of corrupt and unusable data. The frame number and its corresponding time stamp must always increment in a regular fashion as per the selected parameters related to the frame read-out rate (with the exception of natural return to zero on overflow of the respective counters). This provides a good handle for identifying certain kinds of data corruption. The nature of unusual data patch includes the following occurrences noticed in most Level-1 data sets (in PC mode) : mismatch between Frame Number and Frame Time (one of them being in the correct sequence correct and the other showing a JUMP ‘spike’, which can be positive or negative); completely discontinuous Frame Number & Frame Time inserted within normal good data sequence; data from a particular frame repeated elsewhere in the same data set (i.e. for the same observing Episode); abrupt discontinuity in Frame Number which violates monotonicity, etc. These issues have come to light progressively during the mission and appropriate logic incorporated within this DataIngest Module. As a result this Module has evolved over longer time. The identified ‘outlier’ frames are discarded from further consideration. The fraction of input Level-1 data successfully translated by DataIngest Module to reorga-

J. Astrophys. Astr. (0000)000: Page 23 of

Figure 14. Block Diagram for DataIngest Module. This module first collects all relevant input data from observations, calibration and user selections of configurable parameters. It checks integrity and quality of observational data and separates them bandwise in suitable formats (as per imaging mode : INT / PC) for processing by the later stages. It carries out time correlation and certain other functions as described in the text.

nized output usable for the subsequent Modules depends on frequency of occurrences of unusual data patches. Some statistical information based on past ∼ 4 years’ operation of UVIT are provided in Section 4.

Initial part of every Episode of observation includes data collected during ramping up of high voltages for detector safety, which is not scientifically useful since the gain is changing with time. These time stretched are identified and discarded. The primary time variable to be used extensively by the subsequent steps of the pipeline is generated by applying UTC correction to UVIT’s Master Clock (only if ‘utcFlag’ is selected to be ON). In case the Good Time Interval (GTI) filtering is turned ON, the time stretches of data not meeting the criteria selected by the user are discarded. The precise value for exposure time per frame is computed and recorded. In actual processing so far, GTI filtering has never been used.

The next phase of processing in DataIngest depends on the imaging Mode. For INT, individual frames containing raw pixel counts are extracted and stored in separate 2-D FITS image files in a directory named ‘SignalFrames’ with nomenclature of each file having Frame number and Time stamp embedded in it. This directory also stores a list of extracted images.

For PC, sequence of individual frames with centroid coordinates in detector X-Y coordinate system and other details like Frame number, UVIT Master clock time, UTC time, diagnostic measures of event’s raw 5x5 pixel footprint - ‘Max-Min’ & ‘Min’ values of the 4 corners for every detected photon are all packed into a single ‘events’ file. It holds the data from the specific imaging Episode as one master list of photon events in chronological order as FITS table.

For both the Modes, the following products are included : UVIT-UTC time correlation table, log of data loss and an ‘info’ file for passing various computed & PIL parameters to the subsequent Modules.

Some long term effects of exposure to radiation (SEE) on the on board electronic components were noticed midway through the mission life. They were recoverable by hardware RESET to the system at periodic intervals. However, some fraction

Page 24 of J. Astrophys. Astr. (0000) 000:

of the data collected were affected beyond the designed immunity in the pipeline. As a result additional software patches were developed and applied at a later stage to mitigate these effects. While nature of these fixes belongs to the DataIngest module, they were accommodated in the envelope code for the chain (RA INT) and described in Section 3.2.1.

A few general remarks follows, on the convention followed throughout the pipeline for flagging of unusal data / locations. First about flagging pixels /elements of a 2-D image / array, which need not be considered for processing due to either considered as “bad” due to any defect or representing a region outside the active area of the detector. An unique value (-9999) is assigned to such pixels / elements for their easy recognition as an “invalid” pixel / element by all processing blocks. No arithmetic operation is carried out on such flagged pixels / invalid elements & their values are left unaltered. On the other hand, the flagging of individual photons in the master event list are carried out by appending an additional column with an entry with a value ‘1’ (= good) / ‘0’ (=bad) indicating their inclusion / exclusion for consideration in further processing (e.g. event located outside the detector’s active area; asymmetry in footprint signifying multi-photon event).

Directory structures of the products of DataIngest Module for INT and PC modes are provided in Appendix-6 & Appendix-7 respectively.

A1.2 uvtUnitConversion

Aim of this Module, (called by all the versions of the chains) is to translate the image data into physical unit, making it independent of the frame integration time, selected for the observation. For INT mode data, first a dark frame, D(ix,jy), taken from CAL DB is subtracted from the raw frame, RI(ix, jy), and then divided by the frame integration time, T_i, (earlier computed by DataIngest Module) making the pixel values to be ‘signal/s’. (The code is designed to derive this dark frame by linear interpolation in time between dark frames taken before the sky-exposure and after the sky- exposure. But, in practice this dark frame is taken from the CAL DB of ground calibration.) This process is repeated for every image frame.

I_uc(ix,jy)= [RI(ix,jy)-D(ix,jy)]/(T_i);

for all pixels (ix, jy) of the image, & repeated for all images; For PC mode data, each photon event is assigned a value of ‘event/sec’ (1 divided by the frame integration time) and recorded in an additional column of the master table of events. This column is referred to as Effective Number of Photons per second (ENP).

ENP_uc(k) = [ 1 /(T_i) ];

for all events in master table ‘k’ = 0 to ‘k max’ Note the suffix ‘uc’ which identifies the outputs with the Module. Similar naming convention is followed for all other Modules also.

A1.3 uvtMaskBadPix

This Module is called by all versions of the processing chains. The functionality of this Module includes identifying and flagging of : (1) bad pixels in INT mode image arrays, & (2) events in PC mode master table with centroids located in bad pixels as well as those satisfying criteria for being classified as multi-photon event. BAD PIXELS files, for each of the three bands, are arranged as per the mode of observations and the chosen window size, in the CAL DB. All the inactive pixels, either because of being outside the detector’s circular field of view or beacause of selection of one of the smaller window options, are represented as ‘bad pixels’ by populating ‘0’ entries (rest with ‘1’ entries), in the corresponding BAD PIXELS file BP(ix, jy). For INT mode the flagging is effected on all bad pixels of each image frame.

if BP(ix, jy) = 0, then
I_bp(ix, jy) = INVALID_PIX_VALUE;
else I_bp(ix, jy) = I_uc(ix, jy);

As stated earlier (Sec A1.1), a value of ‘-9999’ is assigned for the ‘INVALID PIX VALUE’ flag. For PC mode, every photon event is assigned a value for the variable ‘BAD FLAG’ depending on the integral parts of its centroid coordinates. The centroid coordinates, (x, y), are real numbers represented by an integer part (in the range : 0 - 511) and a fractional part. Consider the integer parts of the centroids (x, y) to be (ix, jy). A new column for ‘BAD FLAG’ is appended to the master table of events, which is populated with :

BAD_FLAG(k) = BP(ix, jy),

where centroid coordinates for the event ‘k’ are (x, y);for all events in master table ‘k’ = 0 to ‘k max’ This Module carries out another function for the PC mode, viz., flagging for Multi-photon events. The option for discarding events having two neighbouring photons was introduced with the

J. Astrophys. Astr. (0000)000: Page 25 of

aim of achieving higher angular resolution. On board processing in PC, mode for detecting individual photon events from raw frames, also extract diagnostic information as stated earlier. The identification of a imulti-photon event is based on this diagnostic data, ( ‘Max-Min’ & ‘Min’ among the raw counts from 4 corners of the 5x5 photon event footprint, ) and the selected threshold value, ‘mult photon thrsld’. For events meeting the above condition are flagged for potential rejection (= ‘0’) in the ‘MULTI PHOTON’ column appended in the master table of events.

if [Max-Min](k) > mult_photon_thrsld,
 then MULTI_PHOTON(k) = 0;
else MULTI_PHOTON(k) = 1;

for all events in master list ‘k’ = 0 to ‘k max’ Subsequent processing has the option to discard every frame with even one event with multi-photon flag set for rejection from further consideration. However, this option has never been used.

A1.4 uvtCosmicRayCorr

This Module handles the effects of Cosmic Rays and is called by all versions of the processing chains. There is a provision for by passing this Module.

This Module attempts to mitigate the effects of individual primary Cosmic Ray (CR) hits as well as shower of secondary charged particles generated by interaction of CR within and near the detector. Some of the charged particles would pass through the CMOS imager leading to a large signal in individual pixels, while other charged particles and photons would generate light pulses some of which look like photon events in the PC mode. In the INT mode, the former can be detected as unusually large signals in individual pixels the latter cannot be isolated as these would be similar to genuine photon events. In the PC mode, some of the hits would generate a large shower of events in a frame which can be distinguished statistically from the normal frames. For INT data, pixels with values above a selected threshold, CR thrshld, are flagged and the process is applied on all the frames.

if I_bp(ix, jy) > CR_thrshld, then
  I_cr(ix, jy) = INVALID_PIX_VALUE;
else I_cr(ix, jy) = I_bp(ix, jy);

for all pixels (ix, jy) of the frame.

For PC mode data, CR affected frames are first identified based on their event count being larger than a dynamically determined

‘event count threshold’ and then flagged. All events from these flagged frames are ignored for further processing. The value of ‘event count threshold’ is computed using two user selected parameters (p & q) as follows : event count threshold = AV G + p ∗ (AV G)^{0.5} + q/((AV G)^{0.5}) where, AVG is an estimate for the average number of true photon events per frame determined from the entire data set for that observation episode. The statistical scheme employed for finding AVG iteratively removes the CR affected frames from the sample as “outliers”. The second term in the equation addresses fluctuations in case of very low values of event counts encountered for fields very dark in the UV. At first the CR affected frames are identified using their unique frame numbers and then all photon events from those CR affected frames are removed from the master list of events (& separately recorded in the log of CR affected frames). As a result, the total number of useful frames is reduced. The loss would depend on the orbit and distribution of matter in the spacecraft, and for UVIT it is ∼ 5 frames/s. Therefore, for optimal results this correction is only useful for dark fields where contribution of the Cosmic Rays to the photon counts is not much less than the contribution of the background.

A1.5 uvtFlatFieldCorr

This Module, called by all the versions of the chains, applies a multiplicative correction for variations of response of the detector and transmission of the selected filter across the field. The correction factor arrays are available from the CAL DB (FLAT FIELDS FILTER). The array appropriate for the band, mode and filter is selected to apply this correction. For INT mode this 2-D correction array, FF(ix, jy), is multiplied to every image frame, leaving flagged pixels (flagging process assigned an unique ‘invalid’ value for its easy identification) unaltered.

if I_cr(ix,jy)=INVALID_PIX_VALUE, then
 I_ff(ix,jy) = INVALID_PIX_VALUE;
else I_ff(ix,jy)=I_cr(ix,jy)*FF(ix,jy);

for all pixels (ix, jy) of the frame.

In case of PC mode data, the value in ENP column for each event is replaced after multiplying it with the correction value from the array element corresponding to that event’s centroid coordinates.

Page 26 of J. Astrophys. Astr. (0000) 000:

ENP_ff(k :ix,jy)= ENP_uc(k)*FF(ix,jy);

where integer part of the centroid coordinates of the event ‘k’ are (ix, jy); for all events in master list ‘k’ = 0 to ‘l max’

A1.6 uvtQEMCPCorr

This Module corrects for the thermal effects on the detector’s response - through variation of Quantum Efficiency and gain of the Micro Channel Plate assembly. This Module is called by all the versions of the chains and it can be turned off. It uses Aux (LBT) data for reading the instantaneous temperature of the detector Module (Camera Proximity Unit, CPU) and estimates corresponding multiplicative correction factor by interpolating the relevant table from CAL DB (QE TEMP). The in orbit thermal stability of the CPUs have been so good that so far this correction was never required.

A1.7 uvtPixPadding

This Module is called by all versions of the processing chains. In order to accommodate movements of the UVIT field on sky due to spacecraft drift over the duration of Episode, it is necessary to enlarge the size of the 2-D arrays representing the sky images. For INT mode all image frames are expanded from 512×512 to 600×600 size, I pp(ix, jy), by introducing a 44 pixel wide boundary on all four sides and assigning each of these added pixels with the value of ‘Bad Pixel’ flag. For the PC mode data, centroid coordinates (cx, cy) for all photon events are incremented by (+44, +44) along both axes :

cx_pp= cx + 44; & cy_pp= cy + 44;

for all events in master list ‘k’ = 0 to ‘l max’. It may be noted that the size of the padding chosen leads to a natural limitation of inclusion of the sky exposure data corresponding to spacecraft drifts at one go. However, a data set with unusually large total drift can still be handled by sub-dividing it into multiple (non-overlapping) time ranges chosen intelligently based on the drift profiles along the two axes (X, Y). Its implementation involves selections of parameters for the Module uvtRefFrameCal described later on (see Sec. A1.13). The pipeline will then need to be executed as many times as the number of sub-divided datasets.

A1.8 uvtAccEveryTsec

This Module is called only by the Relative Aspect chain for Integration mode data (RA INT). Functionality of this Module is to accumulate selected number, ‘N acc’, of successive INT mode frames to enhance the signal for detection of faint stars with a good S/N ratio. A pixel by pixel averaging is carried out resulting in accumulated frames, Acc frame-s. This Module does not handle PC mode (instead this functionality is embedded within the RA PC chain directly).

A1.9 uvtSubDivision

This Module is called by all versions of the processing chains, with the functionality of dividing the image pixels or their coordinates in to subpixels.

The target angular resolution for UV bands of UVIT was < 1.8^{′′}, while the pixel scale for the final 512×512 CMOS sensor is ∼ 3.3^{′′}. The detector system and on board processing for PC mode ensures precision of determining event centroid coordinates (X, Y) to 1/32 of each pixel (∼ 0.1^{′′}). As a result, there is a need for sub-dividing various arrays. A subdivision by 8x8 has been used to get more than 4 effective pixels within the required resolution (i.e. mapping 600×600 to 4800×4800). For PC mode, photon event centroids :

cx_sd= cx_pp*8; & cy_sd= cy_pp*8;

for all events in master list ‘k’ = 0 to ‘l max’. For INT mode processing, an user selectable factor, sub div factor, m (= 2 / 4 / 8) has been introduced for sub-division. This Module implements this sub-division where, original contents of the individual pixels are equally divided among the corresponding sub-divided pixels depending on value of sub div factor, m. The sub-pixels corresponding to flagged pixels are retained as flagged.

if I_acc(ix, jy) = INVALID_PIX_VALUE, then
   I_sd(i_m_x, j_m_y) = INVALID_PIX_VALUE;
else I_sd(i_m_x,j_m_y)=I_acc(ix,jy)/(m^2);

over (m x m) sub-pixels;

for all pixels (ix, jy) of the image, & repeated for all the images;

A1.10 uvtDetectStar

This Module is for identifying stars in an image and quantifying coordinates of their geometric centroids. It is called by all versions of the chains.

This Module processes individual sky images to identify candidate stars from local maxima in light

J. Astrophys. Astr. (0000)000: Page 27 of

distribution, confirm them to be stars from refined analyses of neighbourhood pixels and compute the centroid coordinates. Finally an intensity ordered table of stars is generated. This Module supports both INT and PC mode data. The functionality of this Module is very basic & general purpose, accordinglyit is called explicitly by the two chains extracting spacecraft aspect (RA INT & RA PC) and implicitly by the remaining two chains for their larger Modules : uvtRegAvg (Sec. A1.19), uvt- FullFrameAst (Sec. A1.20), which are described later. Fig. 15 presents a schematic flowchart for this Module. In brief, the implementation is as follows. The values of all valid pixels in the input sky image frame are used to determine the ‘mean (MN)’ & ‘standard deviation (SD)’ for the background, after removing ‘outliers’ (due to presence of stars) by using an iterative scheme. An initial starting ‘threshold’ for detecting a star is defined as (MN + p * SD), where ‘p’ is user selectable and is initially kept at a conservatively high value (∼ 10 - 50). At first all pixels with values above this threshold are considered to be associated with potential stars. If their number is lower than the user selected value for minimum number of stars, ‘min stars’, then the value of ‘p’ is reduced gradually and the process repeated, till the requirement is met.

Multiple neighbouring pixels at this stage could correspond to the same star. In the next step, a neighbourhood criterion using a square box foot print for the star image is used to identify the brightest pixel in each box to get a refined list of pixels (rp ix, rp jy). Size of the box is user selectable but the optimal size is found to be 15x15. Whether the candidate mimics signatures of a genuine star is tested by an elaborate logic using the values of the neighbouring pixels, thus providing immunity against noise spikes. If the number in this refined list does not meet the ‘min stars’ condition, then the value of ‘p’ is reduced further and both the steps described above are repeated till the condition is met (or ‘p’ reaches a value < 5 & the process aborts with appropriate error log).

In the final step, intensity weighted centroid and background corrected total intensity in the box are computed. They are computed as :

c_l_x=[sum{sig(ix,jy)*ix}/sum{sig(ix,jy)}]
c_l_y=[sum{sig(ix,jy)*jy}/sum{sig(ix,jy)}]
  int_l = [sum{sig(ix,jy)}]

where sum is evaluated for ‘ix’ & ‘jy’ running through [rp ix – (k+1)/2] to [rp ix + (k+1)/2] & [rp jy – (k+1)/2] to [rp jy + (k+1)/2], respectively

, where ‘k+2’ is size of the box and ‘sig’ are background corrected values of signal.

Finally, an intensity ordered (descending) table of intensities (int l) and centroids (c l x, c l y) is generated.

A1.11 uvtDetectDistCorr

This Module is called by both INT & PC versions of the Relative Aspect chain and the PC version of the Sky Imaging chain.

This Module applies corrections for the distortion inherent to the detector Module (primarily due to the fibre optic taper). This distortion modifies the expected linear relation between location of electronic detection of a photon event and its original location of arrival on the photo-cathode. Hence, in order to determine the true position for each photon event, a correction needs to be applied. This correction has been quantified by extensive calibrations in the laboratory and confirmed in orbit using well studied astronomical targets. The corrections are identical for all the filters of the band and are available in the CAL DB (DISTORTION/ DETECTOR/ band) as 512×512 arrays. For PC mode, the correction is applied to centroids of every individual photon event & for INT mode to the centroids of each detected star tabulated by the uvt- DetectStar Module (Sec. A1.10). The correction values applicable to the nearest pixel coordinates for each centroid (c x, c y) are applied :

c_x_ddc = c_x -
det_dist_corr_x{nint(c_x-44),nint(c_y-44)};
c_y_ddc = c_y -
det_dist_corr_y{nint(c_x-44),nint(c_y-44)}

where the arrays ‘det dist corr x’ & ‘det dist corr y’ are from CAL DB (for appropriate band FUV / NUV / VIS). An offset in indexing (by 44; see Sec A1.7) is needed since the arrays in CAL DB are in 512×512 system (& all coordinates subsequent to uvtPixPadding Module have them translated to 600x600 system to accommodate spacecraft drift).

A1.12 uvtOpticAssDistCorr

This Module is called by both INT & PC versions of the Relative Aspect chain and the PC version of the Sky Imaging chain.

This Module corrects for distortion due to the Telescope Optical Assembly and is very similar to that discussed above (uvtDetectDistCorr in Sec. A1.11). This distortion has been estimated from

Page 28 of J. Astrophys. Astr. (0000) 000:

Figure 15. Flow chart for star detection (uvtDetectStar module). The algorithm for detecting stars is based on identifying local peaks above a threshold which is sum of average background and the standard deviation multiplied by a factor, ‘p’. The value of ‘p’ is tweaked iteratively (initially starting with a high value) till the desired number of stars are identified. Centroid positions and intensity for the stars are tabulated.

design of the telescope and is very small. The corrections to be applied are available in the CAL DB (DISTORTION /OPTICS /band/filter). It may be noted that since this particular correction originates from design of the telescope optics alone, the CAL DB arrays are identical for all filter-band combinations. For PC mode, the correction is applied to centroids of every individual photon event & for INT mode to the centroids of each detected star tabulated by the uvtDetectStar Module (Sec. A1.10). The correction values applicable to the nearest pixel coordinates for each centroid (from the earlier Module, say, c x ddc, c y ddc) are applied :

c_x_oadc = c_x_ddc -
 optic_assm_dist_corr_x{nint(c_x_ddc-44),
                      nint(c_y_ddc-44)};
c_y_oadc = c_y_ddc -
 optic_assm_dist_corr_y{nint(c_x_ddc-44),
                      nint(c_y_ddc-44)}

where the arrays ‘optic assm dist corr x’ & ‘optic assm dist corr y’ are from CAL DB (for appropriate band FUV / NUV / VIS & filter F1/ F2 / ...) in 512×512 system.

A1.13 uvtRefFrameCal

This Module selects timing reference and step size for subsequent extraction of drift series. It is called by both INT & PC versions of the Relative Aspect chain. This Module is responsible for two functionalities : (1) generate the Reference Frame defined by an ensemble of centroids and intensities of the detected stars with respect to which all relative aspects for future instances of time will be computed, & (2) to prepare tables, similar to the preceding “(1)”, of detected stars for all subsequent time samples. These are then used to find the drifts in a later processing Module (uvtComputeDrift in Sec. A1.14). It begins with the tabulated lists of distortion corrected centroids of stars detected. Each table represents one time sample. The sequence tables as a time series have been generated earlier from individual Acc frame-s (by uvt- DetectStar in Sec. A1.10). There are two user selected parameters for this Module, viz., number of initial time samples to be ignored, N skip, & the number of successive time samples to be combined as a block, N avg, to effectively widen the time bin for computing the average positions of the stars. The resulting time series from the sequence

J. Astrophys. Astr. (0000)000: Page 29 of

of blocks will subsequently be used for computation of the drift. The very first block is used to generate the Reference Frame by associating stars using neighbourhood criteria on the centroids from N avg number of individual Acc frame-s. This is followed by recording the average values for centroid along X, centroid along Y, Intensity & Time. This process is repeated for the subsequent blocks. The selectable parameter N skip provides a scheme to handle data set withunusually large drift, by breaking down the full time range into multiple parts.

A1.14 uvtComputeDrift

This Module is called by both INT & PC versions of the Relative Aspect chain. It supports both INT & PC mode input data and carries out the following tasks : (1) compute the drift which includes shifts and rotation of the field of selected UVIT band as a function of time in Detector coordinate system to generate Relative Aspect Series (RAS); (2) time domain digital low pass filtering of the RAS using selectable parameters; & (3) to translate the filtered RAS to the spacecraft coordinate system, viz., Roll, Yaw & Pitch using mechanical and optical mounting details of the bands on the spacecraft. The Fig. 16 presents the schematic flow of processing in this uvtComputeDrift Module.

The drift computation involves at first reading in all the tables of centroids & intensities for stars, from products of the earlier Module uvtRefFrame- Cal (Sec. A1.13). In the next step, within a loop, two consecutive tables are considered which are referred to using subscripts ‘p’ & ‘c’ for ‘previous’ and ‘current’ respectively. The stars common to both the tables are identified and associated as pairs using their centroid coordinates and an user selected neighbourhood criterion representing maximum expected relative drift.

The generation of the RAS involves computation of best estimates the three variables ‘δx shift’, ‘δy shift’ & ‘δθ’ in detector coordinate system, representing the best fit for transformation of centroids from ‘table p’ to ‘table c’. This best estimation is carried out using the centroids and a selectable algorithm (3 choices available). The most commonly used algorithm finds solution for least sum of squares of deviations, while giving equal weight to all the stars to avoid bias due to some bright stars in few locations. The algorithm is linearised by use of the approximation “sin δθ = δθ and cos δθ =1” which is valid as the relative rotations within any Episode are < 0.1 degree.

In order to limit the error propagation through addition of multiple incremental corrections over multiple time steps, the above scheme is repeated again between the star centroids in the Reference Frame (time RF) and the drift corrected centroids for any time sample time c obtained above. The additional corrections obtained now (say, δθ2, δx2 shift & δy2 shift) are used to compute the final drift values valid for time c, as :

θ RF fin(time c) = θ RF est(time c) + δθ2 x shift RF fin(time c) = x shift RF est(time c) + δx2 shift y shift RF fin(time c) = y shift RF est(time c) + δy2 shift

The complete process described above is repeated for the entire time range by advancing the time by steps of one in a loop. The resulting time series of θ RF fin, x shift RF fin & y shift RF fin are the Relative Aspect Series in Detector coordinate system. Other choices of algorithm for extraction of drift parameters include : (a) dropping the assumption about ‘θ’ to be small; & (b) assigning intensity based weights to individual stars (weight proportional to intensity). In all the 3 algorithms, user has a choice to drop the parameter ‘θ’ from drift extraction (i.e. consider only shifts and no rotation).

The time domain low pass filtering is carried out to minimise errors in the drift parameters . A sliding time window (ΔT) selects the samples over (t- ΔT/2) to (t + ΔT/2) duration. They are then fitted with a polynomial of degree ‘n poly’ using a least square method. The value for fittedpolynomial at mid-point of the time window is assigned as the filtered result for time instance ‘t’. This process is repeated through the complete time series. While ΔT and n poly are selectable by the user the most commonly used values for these have been 4 seconds & 1 respectively.

Finally the drift parameters are transformed from the Detector coordinate system to the spacecraft coordinate system using available transformation matrices. The convention followed for mapping them are : θ⇒ Roll, X ⇒ Pitch & Y ⇒ Yaw. Details of the two way transformations between the Detector and spacecraft coordinate systems are available in Appendix-3. The final Relative Aspect Series, RAS, are made available in both the detector as well as spacecraft coordinate systems, which are required by both versions of the Sky Imaging chains (L2 PC & L2 INT). The standard bundle of the pipeline products includes the two RAS tables for every individual Episode, one each from RA INT and RA PC chains. The tables show the drifts at regular intervals of time.

Page 30 of J. Astrophys. Astr. (0000) 000:

Figure 16. Flow chart for extraction of drift (uvtComputeDrift module). Using centroids of detected stars in successive frames (sampled every ∼ 1 sec for VIS tracking) the incremental relative drift local in time is estimated first. The quantified drift includes 2 shifts along the detector axes and a possible rotation. Subsequently they are translated to cumulative total drift as a function of time, with respect to the Reference Frame. Time domain filtering is used for smoothen the 3 drift variables. Finally they are transformed to spacecraft coordinate system (for use by any of the bands).

A1.15 uvtCentroidCorr

This Module was planned for the PC mode version of the Sky Imaging chain. It corrects for a subtle effect which introduces shift in the centroid of a photon event computed on board. It can arise if estimate of the background signal, which is equated to the lowest value of the four corner signals of 5X5 window around centre of the event, used for onboard calculations of centroid differs significantly from the actual value due to a large noise. The mitigation scheme employed use of median filtered background from measured dark frames in orbit. During early operations in orbit, the noise in background was found to be insignificant. Accordingly, need for activating this Module has not arisen. This correction must precede the correction for centroid bias (uvtCentroidBias, Sec. A1.16) described next.

A1.16 uvtCentroidBias

This Module is called by both the Relative Aspect & Sky Imaging chains for the PC mode. It applies corrections for bias introduced on the centroids of photon events computed by on board signal processing. This systematic bias is inherent to the scheme adopted for obtaining the centroids from raw pixel values in the event foot print (3x3 or 5x5), which slightly modifies the fractional part of the computed centroid value from the corresponding true value. Sometimes this effect is also referred to as Fixed Pattern Noise. The effects of this bias have been quantified from the extensive laboratory calibrations which have been translated into look up tables correlating the measured with the true values for the fractional part of the centroids along both the axes (X, Y). The CAL DB provides these look up tables. This uvtCentroidBias Module recovers the true value from the measured one by applying the corresponding correction (for the appropriate band FUV / NUV / VIS & selected foot print 3x3 / 5x5; e.g. BIAS CORR/FUV/3x3) to all centroids in the master table of events.

A1.17 uvtShiftRot module & further updating of event table

J. Astrophys. Astr. (0000)000: Page 31 of

This Module is called by both INT & PC versions of the Sky Imaging chain. The uvtShiftRot Module carries out the following two tasks for INT mode observations : (A) apply the drift to individual images - single frame or ‘N acc’ frames clubbed together as Acc frame in the Module uvtAccEveryTsec, to align these with the Reference Frame; (B) create Exposure Arrays corresponding to each individual image taking into account the active areas of the detector and aligning them to the Reference Frame by applying drift corrections. For the PC mode, only the first of these two functionalities is incorporated by applying the drift to the centroids of photons. In the PC mode, instead of Exposure Arrays for individual exposure an integrated Exposure Array is created by adding the Exposure Arrays corresponding to individual images. This has been done as the number of individual images in an Episode could be about a million storing these individually would be too expensive in memory space.

A1.17.1 Task-A :

The drift parameters for every image are calculated by a linear interpolation of the entries in the table of drifts for the band, provided by A1.14 uvtComputeDrift, at the relevant time.

A1.17.1a PC mode - For PC mode data, these interpolated drift parameters are used to apply identical corrections to centroids of all photon events of the specific frame.

c x snr= x shift + (c x -x0)*cosθ - (c y -y0)*sinθ + x0 c y snr= y shift + (c x -x0)*sinθ - (c y -y0)*cosθ + y0

where x0 = x size/2 & y0 = y size/2; where the ‘snr’ subscript refers to the shift and rotation corrected centroids & the (c x, c y) are the most recently updated centroids from the master photon event list from the module “uvtOpticAssDistCorr” (Sec A1.12). These drift corrected centroid values (c x snr, c y snr) for each photon event replace the earlier entries for centroid values in the master table of events and remain available for subsequent processing blocks till the very end of execution of the chain. In case the RAS does not cover the entire time range for the Episode, only the part with time overlap is retained and the remaining events are discarded since the drift corrections can not be applied to them. This updated table is preserved in the sub-directory labeled ‘uvtShiftRot 6.3’ within the product bundle for the corresponding Episode, in a file named with the suffix ‘ snr’ (see Appendix- 9).

Further updating by a later processing (uvtFull- FrameAst Module) :

The photon event table finally updated by this uvtShiftRot Module (described above) gets further refined by a later processing Module carrying out astrometric corrections by matching detected stars with those in an existing standard catalogue (module uvtFullFrameAst; Sec. A1.20). A new event table is generated which adds fresh information regarding coordinates and time while retaining all the past details, located in the same sub-directory with the file name having the suffix ‘ radec’.

Five additional columns are appended, which are named ‘RA’, ‘DEC’, ‘MJD L2’, ‘RA-aaaaa’ & ‘DEC-aaaaa’. The first pair contains the best estimate of the event coordinates in RA, Dec (ICRS; J2000) system relative to the map centre, which are the final values obtained from the pipeline run for the corresponding Episode including Astrometry. The last pair correspond to the RA, Dec obtained through transformation of event centroids from Detector (X, Y) system to RA, Dec system using the aspect information from the spacecraft. In the event of failure of the astrometry block, both sets of coordinates would be identical.

The column named ‘TIME’ was planned to provide the primary timing information for each photon event. It is normally populated with SPS MJD, the absolute time provided by L1 through calibration of the spacecraft’s on board clock, through selection of the ‘utcFlag’ to be ON. Alternately, if the UTC switch is selected to be OFF (when SPS MJD showed erratic values occasionally), this ‘TIME’ column is populated with the UVIT’s Master clock, and the ‘MJD L2’ column in the table would still provide estimated absolute time with about ∼ 1 sec accuracy, using local calibration of the UVIT’s Master clock (carried out within the L2 pipeline, in DataIngest Module – Sec. A1.1). This enables astronomical variability analysis at time scales shorter than typical duration of observation episodes which is ∼ 2000 seconds under all circumstances.

The standard bundle of the pipeline products disseminated by the ISSDC includes this final resulting table (with suffix ‘ radec’), as the event list table, corresponding to every data set from individual Episodes.

A1.17.1b INT mode - For INT mode data, individual image frames are first transformed by pixel sub-division from original size 4800×4800 to 9600×9600. Then contents of each of these finer sub-pixels are moved to a new location after application of the shift and rota-

Page 32 of J. Astrophys. Astr. (0000) 000:

tion correction using relations similar to the above. Finally, a 2x2 binning is carried out to bring the array dimensions back to original level. The process ensures local ‘conservation’ of signals and adequate handling of ‘Bad Pixels’. At the end, as many drift corrected image frame products are generated as were available at the input. They are all in Detector coordinate system (X, Y).

A1.17.2 Task-B :

For the second task of generating Exposure Arrays, at first the relevant “Template Exposure Array” is accessed from CAL DB (EXPO- SURE TEMPLATE / band / mode / window size). Primarily, entries in this array are ‘1’ for all subpixels corresponding to the good pixels within the selected window and ‘0’ for the rest. For every image qualified for inclusion in making sky image, a corresponding Exposure Array is generated by applying drift corrections (on the template array) appropriate for that time instance following the procedure described in Task-A (A1.17.1b INT mode).

A1.18 uvtFrameIntegration

This Module is called by both the Relative Aspect and Sky Imaging chains for PC mode data. It is responsible for gridding the photon centroids from multiple (N combine) successive frames onto 2-D array/(s). For the RA PC chain, a time series of images, Comb frames, are generated which are used for identifying individual stars in a subsequent processing stage. For the L2 PC chain this module is either used to combine all the frames for the Episode into a single image or construct multiple images by sub- dividing the full data into smaller time intervals corresponding to ‘pseudo-Episode’- s. The latter option enables application of corrections for small mis-alignments due to any temporal effects, in a subsequent processing step (module uvtRegAvg; Sec. A1.19).

The typical values of the time step ‘T’ corresponding to the selectable parameter, N combine, are ∼ 1 s and ∼ 300 s for RA PC and L2 PC chains respectively. Time sequence of images, Comb frames, are referred to as 4800×4800 “Sig” arrays. The last image would be made with < N combine frames in case the Total number of frames is not integer multiple of N combine. There is a provision to skip N discard initial frames to discard the initial frames either due to any starting disturbance or during a rapid drift of the pointing. Corresponding sole / sequence of “Exposure” array/s and “Uncertainty” array/s are also generated in the L2 PC chain. The “Signal” array/s are obtained by pixel by pixel division of the “Sig” array/s by the corresponding “Exposure” array/s and the statistical “Uncertainty” array/s are generated using the “Signal” and “Exposure” array/s (based on square-root of estimated number of total EFFECTIVE photon events, corrected for the variation of responsivity on the detector, in each individual pixel and not the actual number of photon events). The “Exposure” products from this module are stored in the directory ‘uvtExposure- Frames 6.3’ and the rest (Sig, Signal & Uncertainty) in sub-directories under the directory ‘uvt- FrameIntegration 6.3’.

A1.19 uvtRegAvg

This Module is called by both INT & PC versions of the Sky Imaging chain. It may be noted that in an earlier processing block (PC : uvtFrameIntegration Module; Sec. A1.18; INT : uvtFindWtdMean for L2 INT (not described here), the dataset from a specific Episode has either been treated as a whole (‘Episode’) or in smaller parts (‘pseudo-Episode’) as per user’s choice. Here, the Module uvtRegAvg, combines the multiple Signal (“Sig”) and Exposure (“Exposure”) arrays in case ‘pseudo-Episode’ option was exercised in that earlier bloc. These multiple ‘Sig’ & ‘Exposure’ arrays are combined after determining relative Shifts and Rotation between them using an algorithm to align detected brightest point sources from successive ‘Sig’ arrays which were generated earlier on. The alignment operations are identical for each pair of ‘Sig’ & ‘Exposure’ arrays.

Additionally, for PC mode UV imaging, these combined ‘Sig’ & ‘Exposure’ arrays are used to generate the output ‘Signal’ & ‘Uncertainty’ arrays in true “count/second” unit, using the same scheme as described earlier (uvtFrameIntegration Module; Section A1.18). The same operation is carried out on the sole pair of ‘Sig’ & ‘Exposure’ arrays in case the ‘Episode’ option was exercised in the preceding processing block to generate all 3 final products, viz., ‘Signal’, ‘Exposure’ & ‘Uncertainty’.

At the end of this uvtRegAvg process (irrespective of the choice between pseudo-Episode / Episode), a single set of sky image, exposure & uncertainty products are generated which utilize the entire data set for the particular observation Episode (for a particular combination of Band, Filter & Window size in one orbit). These final array products Signal (counts/sec), Exposure (no of frames) & Uncertainty (counts/sec) are of 4800×4800 size and in Detector coordinate (X, Y) system and stored in the ‘uvtRegAvg 6.3’ directory (see Appendix-9).

J. Astrophys. Astr. (0000)000: Page 33 of

Since the algorithms used in this uvtRegAvg Module for 3 different steps of processing are identical to those described earlier for other Modules, only their references are mentioned here. The scheme to find bright point sources in individual component images (from pseudo-Episodes) is similar to that used for the Module uvtDetectStar (Sec. A1.10) & to determine relative offset (shifts and rotation) between them uses the scheme followed for the Module uvtComputeDrift (Sec. A1.14). Finally, the scheme employed for aligning these individual images based on the locations of detected point sources, is the same as followed for the Module uvtShiftRot (Sec. A1.17.1b; Task-A, for INT mode). It may be noted that the alignment of pseudo-Episodes involves transformation of image sub-pixels resulting in some loss of angular precision, unlike alignment among Episodes carried out in the Driver Scheme (Sec. 3.2.4) in which individual photon centroids are transformed.

A1.20 uvtFullFrameAst

This Module is called by both INT & PC versions of the Sky Imaging chain as well as the Driver- Scheme, which determines finer corrections to the sky coordinates of image products by correlating stars detected in the UV image with standard astronomical catalogues of stars.

The Module uvtFullFrameAst attempts to improve the accuracy of the aspect of the UV sky image products generated prior to invoking this Module. The input images have their sky coordinates determined based on information of spacecraft attitude (Roll RA, Roll DEC, Roll ROT; ICRS J2000) provided in the Level-1 Aux data (‘*.att’ file in ‘mL1’ dataset). The typical accuracy of these coordinates is ∼ 45 arc-sec RMS and up to 3 arcmin peak-to-peak. Hence, there is a large scope for improvement by correlating stars detected in the image products with standard star catalogues to first determine the offsets and then applying corresponding corrections.

The algorithm followed is described here. First identify brightest point like sources detected from the UVIT image (NUV/FUV) and record their RA- Dec (ICRS) coordinates. They are then correlated with brightest entries in the USNO A2 optical star catalogue within a selected search radius (∼ 3 arc minutes). The USNO catalogue was reformatted by – (a) retaining stars brighter than 16 magnitude & (b) embedding an indexing scheme to enable very fast search by the pipeline. ‘Good’ or ‘accidental’ matches of UVIT-USNO pairs are classified based on a sequence of statistical tests carried out iteratively. At first the brightest pairs are considered and progressively less bright pairs are also included for this analysis. If successful in identifying confirmed matches, a least square method is employed to extract the 3 parameters – shifts along RA & Dec and a rotation around the centre of the image (similar to the algorithm described for the Module uvtComputeDrift, Sec. A1.14). The next step is to apply these corrections (shifts & rotation) to the 3 standard products, viz., UV image (‘Signal’), Exposure and Uncertainty arrays. The scheme for application of these astrometric corrections to the UV image differs between the case for individual Episode (when sub-division into pseudo-Episodes is not selected), from that for multi-Episode case. While the astrometric corrections are applied to centroids of individual photons in the former case, the shift & rotational transformations are applied on the sub-divided array elements for the latter.

In the Sky Imaging Chain L2 PC - When this uvtFullFrameAst Module is called by the Sky Imaging chain L2 PC for an individual Episode, the corrections are applied to the centroids (RA, Dec) of each photon event and the master table of events is updated. Two additional columns are introduced in this master table, which hold the astrometry corrected coordinates (details given in Sec. A1.17 for Module uvt- ShiftRot, Task-A, PC mode). The final UV image is generated by populating these photons in Signal array of 4800×4800 size. This process ensures minimal loss of precision (angular resolution) while applying astrometric corrections. Similar corrections for the Exposure and Uncertainty arrays are implemented by physical movements of pixel contents as described for Module uvtShiftRot (Sec. A1.17, Task-A, INT mode; first pixel sub-division from 4800×4800 to 9600×9600; re-gridding individual sub-pixels by applying transformation; & finally 2x2 binning).

In the Driver Scheme - When this uvtFullFrameAst Module is called by the Driver Scheme to apply astrometric corrections to the combined multi-Episode products, all 3 arrays viz., Signal, Exposure and Uncertainty are handled identically. In this case, Signal array also undergoes the same scheme of corrections for the two shifts and the rotation, as implemented for the Exposure and Uncertainty arrays in the case for individual Episodes described in the preceding para.

In addition to using the optical catalogue USNO A2, bright NUV & FUV source catalogues from GALEX mission are also used to correlate bright point like sources from UVIT images. The good

Page 34 of J. Astrophys. Astr. (0000) 000:

matches of UVIT-GALEX pairs are also used to extract the offset corrections, but they are only recorded in a log file. The details of star match ‘success’ / ‘failure’ with Optical & UV catalogues are recorded as HISTORY / COMMENT entries on image HEADERs.

All the image products Signal (counts/sec), Exposure (no of frames) & Uncertainty (counts/sec) are of 4800×4800 size and in RA-Dec (ICRS; J2000) coordinate system. They all are stored in the sub- directory named ‘uvtFullFrameAst 6.3’ either below a directory labeled by the specific Episode (see Appendix-9) or a directory identifying the “group” (Band/ Filter/ Window) for multi- Episode case (see Appendix-10). In case of failure of this astrometry block, the set of resulting products contain arrays identical to pre-astrometry images with adequate qualification in header keywords of the failure.

The standard bundle of pipeline products archived and disseminated by ISSDC includes the Signal image product from this Module as final UV sky image in Astronomical coordinates, corresponding to every Episode generated by the Sky Imaging chain (L2 PC), as well as combined multi- Episode images generated by the Driver Scheme for every “group”. The corresponding Exposure and Uncertainty products are also included.

Appendix 2 : Relative time shifts between the three Bands In spite of a common Master Clock used by all three Bands of UVIT, the timing details of detector read out electronics lead to systematic shifts in the time stamps recorded on individual frames. These shifts depend on the imaging parameters configured. The relative time shifts most relevant for the pipeline are between the band used to obtain Relative Aspect Series and the Imaging UV bands. This has been calibrated (in seconds unit) to be :

t RAS - t img = t0 RAS - (-T Img frame/ 2)

where ‘t0 RAS’ depends on the band generating RAS, its imaging mode & parameters; & ‘T Img frame’ is the frame integration time of the imaging Band (NUV / FUV); t0 RAS =-0.427; for drift tracking by VIS band in INT mode; full 512×512 field; t0 RAS = -(T RAS frame/2); for drift tracking by NUV band in PC mode; any window size; where ‘T RAS frame’ is the frame integration time of the tracking Band (NUV).

Appendix 3 : Transformations between the Detector and Spacecraft coordinate systems

The Detector coordinate system for each band is defined by the X-Y axes of its electronic sensor (Star-250), and the axis normal to this plane corresponds to the optic axis of the telescope (either directly as for the FUV & VIS bands, or via one reflection with a plane surface; see Fig. 1). The rotation angle about the optic axis is denoted by ‘θ’ in the detector system. The Spacecraft coordinate system comprise of the axes Roll, Yaw & Pitch which is defined by the structure of the spacecraft. These two systems are interconnected through the details of mounting of sub-systems of UVIT on to the spacecraft’s mechanical interface. Nominally, the optic axis is aligned parallel to the Roll axis and the (X, Y) and (Yaw, Pitch) are connected through a single angle of rotation about an axis normal to all these 4 axes. Similarly, one rotation angle connects any pair of detectors for two bands. All these angles were initially measured during optical alignment tests in the laboratory. These were subsequently validated andrefined by in orbit measurements during the Performance Verification phase.

The transformations between detector (X, Y, θ) and spacecraft (Roll, Yaw & Pitch) are implemented as matrices for band, BND, as RPYTOXY- THETA BND, {BND : FUV / NUV / VIS}, populated with numerical values, along with a corresponding plate scale. The reverse transformations, XYTHETATORPY BND, are generated internally by matrix inversion.

RPYTOXYTHETA FUV : -0.00249798, 0.29636841, 0.29636841, 0.00249798

RPYTOXYTHETA NUV : 0.15423, 0.25153, -0.25153, 0.15423

RPYTOXYTHETA VIS : 0.1627, 0.2400, 0.2400, -0.1627

The above are consistent with the angles between +Y and the -Yaw (measured CCW) to be +0.483, +31.515 and +34.134 degrees for the FUV, NUV & VIS bands respectively. They are also consistent with the following directly observable relations which connect image coordinates of a star in the NUV & VIS detectors (accounting for slightly different plate scale for VIS; dX & dY are referenced with respect to the respective array centres) : dX NUV = 1.01652 * dX VIS - 0.04649 * dY VIS

dY NUV = - 0.04649 * dX VIS - 1.01652 * dY VIS

The corresponding relations connecting image coordinates of a star in the FUV & VIS detectors are :

dX FUV = -0.85093 * dX VIS + 0.56645 * dY VIS

dY FUV = 0.56645 * dX VIS - 0.85093 * dY VIS

Appendix-4 : Directory structure of merged Level-1 data set (mL1)

J. Astrophys. Astr. (0000)000: Page 35 of

-AS1G06 157T01 9000000772uvt level1 mcap.xml -AS1G06 157T01 9000000772uvt level1.mkf

—aux -AS1G06 157T01 9000000772uvt level1.tct —aux1 -AS1G06 157T01 9000000772uvt level1.att -AS1G06 157T01 9000000772uvt level1.gyr -AS1G06 157T01 9000000772uvt level1.orb —aux2 -AS1G06 157T01 9000000772uvt level1.lbt —aux3 —AS1G06 157T01 9000000772uvt level1.orb -hk -AS1G06 157T01 9000000772uvt level1.hk

—uvtF ——DarkF ——uvtF.01 -AS1G06 157T01 9000000772uvtFIIPC00F2 level1.bti -AS1G06 157T01 9000000772uvtFIIPC00F2 level1.fits -AS1G06 157T01 9000000772uvtFIIPC00F2 level1.gti ——uvtF.02 -AS1G06 157T01 9000000772uvtFIIPC00F0 level1.bti -AS1G06 157T01 9000000772uvtFIIPC00F0 level1.fits -AS1G06 157T01 9000000772uvtFIIPC00F0 level1.gti ——uvtF.03 ... —uvtN ——DarkN ——uvtN.01 -AS1G06 157T01 9000000772uvtNIIPC00F5 level1.bti -AS1G06 157T01 9000000772uvtNIIPC00F5 level1.fits -AS1G06 157T01 9000000772uvtNIIPC00F5 level1.gti ——uvtN.02 -AS1G06 157T01 9000000772uvtNIIPC00F0 level1.bti -AS1G06 157T01 9000000772uvtNIIPC00F0 level1.fits -AS1G06 157T01 9000000772uvtNIIPC00F0 level1.gti ——uvtN.03 ... —uvtV ——DarkV ——uvtV.01 -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.bti -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.fits -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.gti ——uvtV.02 -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.bti -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.fits -AS1G06 157T01 9000000772uvtVIIIM00F2 level1.gti ——uvtV.03

... Appendix-5 : Directory structure of UVIT Calibration Database (CAL DB)

-change.log -readme.txt

-AV PH ENERGY (scalar) –FUV -calibfile.fits –NUV -calibfile.fits –VIS -calibfile.fits

-BAD PIXELS (2-D array 512 x 512) –FUV —IM —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

–NUV —IM

—-100X100 -calibfile.fits ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

–VIS —IM —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

-BIAS CORR (table : 3 col x 4097 row) –FUV —3X3 -calibfile.fits —5X5 -calibfile.fits

–NUV —3X3 -calibfile.fits —5X5 -calibfile.fits

–VIS —3X3 -calibfile.fits —5X5 -calibfile.fits

-DARK (2-D array 512 x 512) -darkend.fits -darkstart.fits

-DISTORTION (Two 2-D arrays 512 x 512; ........ first for X axis & second for Y axis) –DETECTOR —FUV -calibfile.fits

—NUV -calibfile.fits

—VIS -calibfile.fits

–OPTICS —FUV —–F0 -calibfile.fits ... —–F7 -calibfile.fits

—NUV —–F0 -calibfile.fits ... —–F7 -calibfile.fits

—VIS —–F0 -calibfile.fits ... —–F5 -calibfile.fits

-EXPOSURE TEMPLATE (2-D array 1200 x 1200) –FUV —IM —-100X100 -calibfile.fits

Page 36 of J. Astrophys. Astr. (0000) 000: ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

–NUV —IM —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

–VIS —IM —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits —PC —-100X100 -calibfile.fits ... —-512X512 -calibfile.fits

-FLAT FIELDS FILTER (2-D array 512 x 512) –FUV —IM —-F0 -calibfile.fits ... —-F7 -calibfile.fits —PC —-F0 -calibfile.fits ... —-F7 -calibfile.fits

–NUV —IM —-F0 -calibfile.fits ... —-F7 -calibfile.fits —PC —-F0 -calibfile.fits ... —-F7 -calibfile.fits

–VIS —IM —-F0 -calibfile.fits ... —-F5 -calibfile.fits —PC —-F0 -calibfile.fits ... —-F5 -calibfile.fits

-QE TEMP (table : 9 col x 20 row) –FUV —IM -calibfile.fits —PC -calibfile.fits

–NUV —IM -calibfile.fits —PC -calibfile.fits

–VIS —IM -calibfile.fits —PC -calibfile.fits

Appendix-6 Directory structure for DataIngest output (Integration mode; INT)

-AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.crcFailedList -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.dataIngestOut -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.info -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.missingFrameList -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.timeCorrection

-Dark –AS1A03 103T01 9000001132uvtVIIIM00F4 l2 darkbegin.fits –AS1A03 103T01 9000001132uvtVIIIM00F4 l2 darkend.fits

-SignalFrames –AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734052.8140 f16 di.fits –AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734053.7900 f32 di.fits –AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734054.7670 f48 di.fits ... ... Appendix-7 Directory structure for DataIngest output (Photon Counting mode; PC) -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.crcFailedList -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.dataIngestOut -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.events -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.image -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.info -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.missingFrameList -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 di.timeCorrection

–Dark -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 darkbegin.fits -AS1G06 157T01 9000000772uvtFIIPC00F6 l2 darkend.fits

Appendix 8 Directory structure for the outputs from the Relativistic Aspect Chain for Integration Mode (RA INT)

DataIngest 6.3 -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.crcFailedList -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.crcFailedList -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.dataIngestOut -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.info -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.missingFrameList -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 di.timeCorrection

-Dark -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 darkbegin.fits -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 darkend.fits

-SignalFrames -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734052.8140 f16 di.fits -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734053.7900 f32 di.fits ... ... -uvtComputeDrift 6.3 -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 dr.fits -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 dr.info

J. Astrophys. Astr. (0000)000: Page 37 of

-observation.txt

-uvtRefFrameCal 6.3 -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 rfc.info

-Centroid -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734053.790000 f1 rf centroid.fits -AS1A03 103T01 9000001132uvtVIIIM00F4 l2 t2734054.767000 f2 rf centroid.fits ... ... Appendix 9 : Directory structure for the outputs from the Level-2 Sky Imaging Chain for Photon Counting Mode (L2 PC)

DataIngest 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.crcFailedList -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.dataIngestOut -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.events -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.image -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.info -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.missingFrameList -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 di.timeCorrection

-Dark -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 darkbegin.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 darkend.fits

-uvtExposureFrames 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 f1 exp fi.fits

-uvtFlippedRegImage 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 f1 10Per rg.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 ............................ f1 expFlipped rg.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 ............................ f1 NoiseMapFlipped rg.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 ............................ f1 sigFlipped rg.fits

-uvtFrameIntegration 6.3 –NOISE MAP -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t2734148.0000 ........................... f1 sig noise map sig.fits –SignalFrames -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t2734148.0000 ........................... f1 sig fi.fits –SignalFrames DividedWithExposure -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t2734148.0000 ........................... f1 sig Sig DividedWithExp.fits

-uvtFullFrameAst 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 as Exp.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 as NoiseMap.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 as Sig.fits -star raDec frmOptics catalogueWith 10Stars.txt -star raDec frmOptics catalogueWith 5Stars.txt -star radec.txt

-uvtRADECImage 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 .............................. f1 noise ra-decnoise.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 .............................. f1 sig ra-decexp.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 f1 sig ra-dec.fits

-uvtRegAvg 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 f1 exp regAvg.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 .............................. f1 noiseMap regAvg.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t0.0000 f1 sig regAvg.fits

-uvtShiftRot 6.3 -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 radec.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 snr.fits -AS1A03 103T01 9000001132uvtNIIPC00F1 l2 t9999.0000 f1 img fi.fits

Appendix-10 : Top level directories for products from Driver Scheme (with some additional details for Combined multi- Episode products)

-/FUV FullFrameAst F3 W511 –uvtFullFrameAst 6.3 -AS1A03 103T01 9000001132uvtFIIPC00F3 l2 as Exp.fits -AS1A03 103T01 9000001132uvtFIIPC00F3 l2 as NoiseMap.fits

-AS1A03 103T01 9000001132uvtFIIPC00F3 l2 as Sig.fits -star raDec frmOptics catalogueWith 5Stars.txt -star radec.txt

–/FUV Final F3 W511 -F3 W511 FinalImage Exp.fits -F3 W511 FinalImage NoiseMap.fits -F3 W511 FinalImage Sig.fits

-/FUV FullFrameAst F2 W511 -/FUV Final F2 W511 -/NUV FullFrameAst F6 W511 -/NUV Final F6 W511 -/NUV FullFrameAst F3 W511 -/NUV Final F3 W511 -/NUV FullFrameAst F2 W511 -/NUV Final F2 W511 -/NUV FullFrameAst F1 W511 -/NUV Final F1 W511 -/ RAPC -/ FUV 10 -/ NUV 10 -/ FUV 9 -/ NUV 9 -/ FUV 8 -/ NUV 8 -/ FUV 7 -/ NUV 7 -/ FUV 6 -/ NUV 6 -/ FUV 5 -/ NUV 5 -/ FUV 4 -/ NUV 4 -/ FUV 3 -/ NUV 3 -/ FUV 2 -/ NUV 2 -/ FUV 1 -/ NUV 1 -/uvit

Appendix-11 : All user selectable parameters

List of all user selectable switch settings and parameters for the pipeline (through Parameter Interface Library, PIL), are presented in a tabular form (see Table 7). The sequence of parameters are grouped by : DRIVER SCHEME and RA INT, RA PC & L2 PC chains. Parameter names in bold font indicate them to be tweaked frequently by users.

Acknowledgements

We thank the anonymous referees for their useful suggestions which led to improvements. The UVIT project is a result of collaboration between IIA, Bangalore, IUCAA, Pune, TIFR, Mumbai, many centers of the Indian Space Research Organization (ISRO), and the Canadian Space Agency. We thank these organizations for their general support. We thank D Bhattacharya for his role in organizing the pipeline requirements. The Ground Segment software teams of ISRO at ISAC/URSC, Banglaore, ISTRAC, Bangalore & SAC, Ahmedabad have provided significant support throughout the development of the pipeline. We gratefully thank all the members of these teams for their support. We also thank members of the ASTROSAT Project & the ASTROSAT Science Working Group

Page 38 of J. Astrophys. Astr. (0000) 000:

for their critical feedbacks. Finally, we thank numerous users of early versions of this pipeline for their feedbacks.

References

Ghosh, S. K., Tandon, S. N., Joseph, P., et al., 2021, JApA, 42, 29

Kumar, A., Ghosh, S. K., Hutchings, J., et al., 2012, SPIE, 8443, 84431N

Tandon, S. N., Ghosh, S. K., Hutchings, J. B., et al., 2017a, CSci, 113, 583

Tandon, S. N., Hutchings, J. B., Ghosh, S. K., et al., 2017b, JApA, 38, 28

Tandon, S. N., Postma, J., Joseph, P., et al., 2020, AJ, 159, 158

Tandon, S. N., Subramaniam, A., Girish, V., et al., 2017c, AJ, 154, 128

J. Astrophys. Astr. (0000)000: Page 39 of

Table 1. Scientific experiments on board Indian multi-wavelength astronomical satellite ASTROSAT Instrument Ultra-Violet Soft Xray Large Area Cadmium-Zinc- Scanning Sky Imaging Telescope Xenon Telluride Monitor Telescope (SXT) Proportional Imaging (SSM) UVIT Counter Telescope (LAXPC) CZTI) Waveband Far UV: 130-180 nm Soft X-ray: Soft & Hard Hard X-ray: Soft & Hard Near UV: 200-300 nm 0.3 - 8 keV X-ray: 25 - 150 keV X-ray : Visible: 320-550 nm 3 - 100 keV 2.5 - 10 keV Field of View ∼28 arc-min ∼40 arc-min 0.9 deg×0.9 deg 4.6 deg×4.6 deg 22-27 deg× 100 deg Optics Twin Ritchie Chretian Conical foil Collimator 2-D coded 1-D coded 2-mirror system (Wolter-I) mask mask Mirrors Detector Photon X-ray CCD Proportional CdZnTe Position Counting at the Counter Arrays sensitive (Intensified) focal plane Proportional CMOS imagers Counter Angular 1.2-1.5 arc-sec 2 arc-min ∼1-5 arc-min 8 arc-min ∼10-13 arc-min Resolution (in Far & (in scan along coding Near UV) mode) axis & 2.5 deg across Energy 10-50 nm 90 eV at 1.5 keV 12-15% 6% at 25% Resolution as per filter 136 eV at 5.9 keV in 22-60 keV 100 keV at 6 keV selection Geometrical 1250 250 10,800 (total 976 173 Collection for each of the for 3 (total for Area (cm^2) 3 wavebands identical 3 units) units) Effective ∼10 for Far 90 at 1.5 keV 6000 415 11 Area (cm^2) UV band; at 5-20 keV photometric; at 2.5 keV; ∼10 for Near (total for 3 335 51 UV band; identical spectroscopic at 5 keV; ∼40 for Visible units) (total for band; 3 units) Time 2 milli-sec ∼2.4 sec for 10 micro-sec 20 micro-sec 0.1 milli-sec Resolution full field; ∼0.28 sec for central area Sensitivity 20 mag (5σ) ∼10^{−13} erg cm^{−2} 1 milli-Crab 20 milli-Crab ∼28-40 milliin 160 sec for sec^{−1} (5σ) (3σ) in (5σ) in Crab (3σ) for Far UV in 20,000 sec 1,000 sec 10,000 sec in 600 sec Total Mass (kg) 230 70 419 56 65.5

Page 40 of J. Astrophys. Astr. (0000) 000:

Table 2. List of frequently used acronyms, names and selectable parameters referred to in this document.

Serial Acronym / Name Expanded form / No. / Selectable parameter Description Acronym :

1 CAL DB Calibration Database 2 CR Cosmic Rays 3 CRC Cyclic Redundancy Check 4 ENT Effective Number of Photon 5 FITS Flexible Image Transport System 6 FUV Far-UltraViolet band of UVIT 7 GTI Good Time Interval 8 ICRS International Celestial Reference System 9 INT INTegration Mode of imaging 10 ISRO Indian Space Research Organization 11 ISSDC Indian Space Science Data Centre 12 L1 Level-1 data (input for the pipeline) 13 L2 Level-2 data (output of the pipeline) 14 L2 PC Level-2 Sky Imaging chain for data collected in Photon Counting (PC) mode 15 L2 INT Level-2 Sky Imaging chain for data collected in Integration (INT) mode 16 MCP Micro-Channel Plates (used as Intensifier in the Detector Module) 17 MJD Modified Julian Date 18 mL1 Merged Level-1 data bundle (input for the pipeline; provided by ISRO / ISSDC) 19 NUV Near-UltraViolet band of UVIT 20 OE Other Episode/s (other than the Reference Episode among the “group” of Episodes to be combined, with identical Band, Filter & Window configuration) 21 PC Photon Counting Mode of imaging 22 PIL Parameter Interface Library 23 POC Payload Operation Centre (located at the Indian Institute of Astrophysics, Bangalore) 24 PSF Point Spread Function 25 RA INT Level-2 Relative Aspect chain for data collected in Integration (INT) mode 26 RA PC Level-2 Relative Aspect chain for data collected in Photon Counting (PC) mode 27 RAS Relative Aspect Series (time series of 3 variables quantifying drift; Roll-Pitch-Yaw / X-Y-θ) 28 RE Reference Episode (with longest exposure time) among the “group” of Episodes to be combined, each with identical Band, Filter & Window configuration 29 RF Reference Frame; defines the instance of time for an Episode, with respect to which drift corrections are measured & applied to frames at future times 30 SAA South Atlantic Anomaly 31 SC Spacecraft 32 SSM Scanning X-ray Sky Monitor 33 UL2P UVIT Level-2 Pipeline 34 USNO United States Naval Observatory (catalogue of stars) 35 UTC Universal Time Clock 36 UV Ultra-Violet 37 UVIT Ultra-Violet Imaging Telescope 38 VIS Visible (VIS) band of UVIT Name / Selectable parameter :

1 Aux Auxiliary data (from spacecraft sub-systems) 2 Episode Smallest unit of imaging session as per mission operations; corresponding data consist of time series of frames read out at a planned rate 3 EXP TIME Total effective Exposure Time (seconds) based on no. of frames contributing to the product 4 Exposure 2-D Array, its elements hold no. of frames exposed with valid pixels of the detector 5 N acc No. of successive VIS frames to be stacked for generating individual accumulated images, ‘Acc frame’ (from which star are identified for drift tracking; used in RA INT chain) 6 N avg Centroids of detected stars from N avg successive accumulated images (Acc frames) are combined to select a wider time bin for drift computation (used in RA INT chain) 7 N combine (1) No. of successive NUV /FUV frames to be accumulated for generating time series of images, ‘Comb frame’, from which drift is extracted (used in RA PC chain);

(2)Division of Episode into multiple pseudo- Episodes, each consisting of N combine consecutive frames (when “pseudo-Episode” option is used in L2 PC chain);

8 N p No. of packets containing image data in a frame 9 ObsID Observation ID identifies an unique sky pointing towards a target 10 pseudo-Episode Part of an Episode when divided into multiple data chunks (each with N combine frames) 11 Sig 2-D array, with elements holding accumulated ENPs from drift corrected frames 12 Signal 2-D array, sky image in “counts/sec” unit 13 Uncertainty 2-D array, with elements holding statistical uncertainty from no. of photon of events contributing to the pixel (in “counts/sec” unit) 14 utcFlag Switch to select either Universal Time Clock or UVIT’s Master Clock for timing

J. Astrophys. Astr. (0000)000: Page 41 of

Table 3. List of Modules used in the Pipeline and their linkages to Chains

Serial Functionality of the Module Name of the References to Usage No. Module Module description of the Module (Appendix 1) (Chains) 1 Ingest the observational data DataIngest A1.1; RA INT, RA PC, as well as calibration databases Fig.14 L2 PC, L2 INT 2 Unit conversion from ‘event’ to uvtUnitConversion A1.2 RA INT, RA PC, ‘event-per-second’ L2 PC, L2 INT 3 Flagging of pixels / events uvtMaskBadPix A1.3 RA INT, RA PC, corresponding to unusable regions of L2 PC, L2 INT the detector 4 Identifying frames affected by uvtCosmicRayCorr A1.4 RA INT, RA PC, Cosmic Ray showers L2 PC, L2 INT 5 Applying correction for response uvtFlatFieldCorr A1.5 RA INT, RA PC, variation over the detector area L2 PC, L2 INT 6 Correction for temperature uvtQEMCPCorr A1.6 RA INT, RA PC, dependence of : Quantum Efficiency L2 PC, L2 INT (QE) of detector gain of Micro- Channel-Plate (MCP) 7 Symmetric expansion of 2-D arrays to uvtPixPadding A1.7 RA INT, RA PC, accommodate spacecraft drifts L2 PC, L2 INT 8 Frame Accumulation by stackings uvtAccEveryTsec A1.8 RA INT of successive frames 9 Generating finer grid of 2-D arrays to uvtSubDivision A1.9 RA INT, RA PC, achieve / preserve higher resolution L2 PC, L2 INT 10 Star Detection - identify brighter uvtDetectStar A1.10; RA INT, sources in the sky image Fig.15 RA PC 11 Correction for Detector Distortion - uvtDetectDistCorr A1.11 RA INT, RA PC, photon event / star centroids corrected L2 PC for local defects inherent in the Detector 12 Correction for Distortion in the uvtOpticAssDistCorr A1.12 RA INT, optical assembly - photon event / star RA PC, L2 PC centroids corrected for local distortions in the Telescope optics 13 Identification of a Reference Frame uvtRefFrameCal A1.13 RA INT, with respect to which all ‘relative’ RA PC shifts and / or rotations etc are computed 14 Computation of drift (for temporal uvtComputeDrift A1.14; RA INT, scale of several seconds) from VIS / Fig.16 RA PC NUV images to generate Relative Aspect Series (RAS) 15 Computation of jitter (for sub-second/ uvtComputeJitter RA INT, second time scale) from Gyro signals RA PC 16 Computation of inter-band alignment uvtComputeThermal RA INT, due to thermal effects RA PC 17 Correction to the photon event uvtCentroidCorr A1.15 L2 PC centroids for error in on board estimation of dark counts of the CMOS sensor 18 Correction for the Fixed Pattern uvtCentroidBias A1.16 RA PC, Noise to the photon event centroids L2 PC 19 Correction for drift by applying Shift uvtShiftRot A1.17 L2 PC, & Rotation L2 INT 20 Frame Integration - dividing the full uvtFrameIntegration A1.18 RA PC, dataset into smaller sub-sets, as an option L2 PC 21 Generation of Exposure Weighted uvtFindWtdMean L2 INT Mean Images & Exposure Arrays 22 Registration & Averaging - aligning uvtRegAvg A1.19 L2 PC, images from sub-sets of an episode L2 INT and combining into a single image 23 Establishing absolute aspect of the uvtFullFrameAst A1.20 L2 PC, image by matching catalogued stars L2 INT, Driver Scheme

Page 42 of J. Astrophys. Astr. (0000) 000:

Table 4. Standard set of pipeline data products bundled by UVIT POC for dissemination and archiving by the ISRO /ISSDC

Product Description Drift Drift Drift Drift Total type extraction extraction extraction extraction No. using VIS using VIS using NUV using NUV of (RAS VIS) (RAS VIS) (RAS NUV)* (RAS NUV)* files

Sky Image Sky Image Sky Image Sky Image in NUV band in FUV band in NUV band in FUV band

*for obsn. till *for obsn. till March 30, 2018 March 30, 2018 Products for each Individual Episode :

Sky Image FITS image 1 1 1 1 4 (Detector coordinates; X-Y) (4800x4800 pixels) Sky Image, post Astrometry FITS image 1 1 1 1 4 (Astronomical coordinates; (4800x4800 pixels) RA-Dec, ICRS) Exposure Map FITS image 1 1 1 1 4 (Detector coordinates; X-Y) (4800x4800 pixels) Uncertainty Map FITS image 1 1 1 1 4 (Detector coordinates; X-Y) (4800x4800 pixels) Photon Events List FITS binary table 1 1 1 1 4 (Photon centroids in both Detector & Astronomical coordinates) Drift Series (RAS file) FITS binary table 1 1 1 1 2 (In Detector & Spacecraft coordinates) Products for each “Group” of Multi-Episodes :

Sky Image, post Astrometry FITS image 1 1 1 1 4 (Astronomical coordinates; (4800x4800 pixels) RA-Dec, ICRS) Sky Image, pre Astrometry FITS image 1 1 1 1 4 (Astronomical coordinates; (4800x4800 pixels) RA-Dec, ICRS) Exposure Map, post FITS image 1 1 1 1 4 Astrometry (Astronomical (4800x4800 pixels) coordinates; RA-Dec, ICRS) Uncertainty Map, post FITS image 1 1 1 1 4 Astrometry (Astronomical (4800x4800 pixels) coordinates; RA-Dec, ICRS) Common Products :

Data Quality Report XML 1 README TXT 1 ChangeLog TXT 1 DISCLAIMER TXT 1 Pipeline Parameter Files TXT 2

Table 5. Distribution of the quality values (from achieved PSF size & amount of pedestal) for FUV and NUV band images.

Quality bin (range) (1-2) (2-3) (3-4) (4-5) (5-6) (6-7) (7-8) (8-9) (9-10) NUV band (No. of ObsIDs) 0 0 0 3 6 5 7 18 335 FUV band (No. of ObsIDs) 15 22 30 41 58 84 84 118 527

Table 6. Distribution of the yield values (percentage of input Level-1 data translated to Level-2 image products, for FUV & NUV bands) achieved by the pipeline.

Yield bin (%) 10 20 30 40 50 60 70 80 90 100 NUV band (No. of ObsIDs) 3 0 1 0 7 4 11 27 54 275 FUV band (No. of ObsIDs) 9 5 3 5 9 24 28 72 149 797

J. Astrophys. Astr. (0000)000: Page 43 of

Table 7. List of all user selectable switch settings and parameters available through Parameter Interface Library (PIL). The sequence of items are grouped in the following order : (a) DRIVER SCHEME and (b) RA INT, RA PC & L2 PC chains. Parameters frequently tweaked by the users are highlighted by bold font.

Serial Parameter name Processing Suggested Description Comments No. (bold indicates Chain Default (switch logic:

frequently value ‘1’/‘y’ for ON; tweaked ones) ‘0’/‘n’ for OFF) Parameters for Processing Driver Scheme Chain 1 NUVonNUVflag DRIVER SCHEME n Switch for forcing all drift generations Turn ON only if using NUV only (i.e. ignore all VIS) VIS data NOT reliable 2 FUVonFUVflag DRIVER SCHEME n Switch for forcing all drift generation Turn ON only if using FUV only (i.e. ignore all VIS & VIS & NUV NUV data). Useful for generating NOT available FUV images only 3 thresholdpc DRIVER SCHEME 50 Parameter related to threshold for star ‘AVG’ & (& L2PC-NUV) detection (starting value of ‘p’ in : ‘SIGMA’ are Threshold = AVG + p * SIGMA; ‘p’ is average and gradually decreased iteratively till standard demanded no. of stars are achieved). deviation of Used (1) for aligning UV images from values (only nondifferent Episodes; & (2) in Astrometry zero entries module. considered) in pixels of image array. Only for PC mode.

4 minimumTargetedStars DRIVER SCHEME 6 Targeted minimum no. of stars (1) For PC mode (& RA INT) (iterations proceed with lower ‘p’ & & (2) for INT detection threshold, till target is mode. achieved) : (1) to align images from different Episodes; & (2) detection of stars in ‘uvtDetectStar’ module (INT mode) 5 minimum targetedstarspc DRIVER SCHEME 5 Success Criterion for Astrometry stage : (& L2PC-NUV) minimum no. of star matches with Catalogue required;

Parameters Processing common to Chains multiple chains 6 level1indir RA INT, RA PC, - Path to the directory holding Input L2 PC, L2 INT Level-1 data 7 caldbdir RA INT, RA PC, - Path to the directory holding Calibration L2 PC, L2 INT Database (CAL DB) 8 level2outdir RA INT, RA PC, - Path to the directory holding Calibration L2 PC, L2 INT from the Driver Scheme (top level location, below which products appear in a structured manner) 9 ZipFlag RA INT, RA PC, y Switch to indicate type of L1 data set : ISSDC L2 PC, L2 INT ‘tar’ (select ‘n’) or ‘zip’ (select ‘y’) disseminates in ‘zip’ format 10 utcFlag RA INT, RA PC, n Switch to select clock for time reference Must be ‘n’ L2 PC, L2 INT - ‘y’ : use calibrated Universal Time Clock (UTC); ‘n’ : use UVIT’s Master clock

... Continued

Page 44 of J. Astrophys. Astr. (0000) 000:

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value Parameters for RA INT For ‘drift’ extraction Relative Aspect from VIS images Series Chain (INT) (in Integration Mode) 11 history RA INT y Switch for history to be written (‘y’) or Records the not (‘n’). History contains all the settings settings : #11 to of the selectable switches & input #39 as listed in parameters with which the Chain has this table) ran.

12 clobber RA INT y Action in case the output directory Default to erase chosen by the user is already existing. If past contents (if clobber is YES (‘y’) then this directory any) will be removed and created afresh by pipeline. If clobber is NO (‘n’) then pipeline will exit with an appropriate error message 13 GTI FLAG RA INT 0 GTI filtering to be done(1) or not(0). Must be ’0’ (i.e. not using GTI filter) 14 crcflag RA INT n Switch to select if CRC check to be CRC check is carried out (‘y’), or not (‘n’). If ‘y’ is ignored. Bit error selected, another switch (‘dropframe’, rate in general is see #20) selects the action : to drop the very low. affected packet alone or all packets for that image frame.

15 ManualMode RA INT n Switch for Manual Mode operation to Useful only when select stars - On(‘y’) or Off(‘n’); either star field [used in “uvtComputeDrift” block]; very complex or enters interactive mode for this block severe detector alone, and the rest of the processes run artifacts (& automatically]. normal run with ‘n’ has FAILED) 16 channel RA INT VIS Selection of Band for which to run Normally only VIS band is used in Integration (INT) Mode 17 junkfileflag RA INT 1 Switch for handling artifacts of VIS VIS artifact detector (‘horizontal stripes’ etc. in VIS handler must be images) - ‘1’ : ON; ‘0’ : OFF ON 18 thresholdforjunkFrame RA INT 5000 Threshold (pixel ADU) value for Pixel threshold identifying ‘artifacts’ in VIS images value of VIS (Threshold for artifact detection) artifacts from experience 19 darkframeFlag RA INT 1 Switch for Dark Subtraction: ‘1’ Dark subtraction =substract Dark; ‘0’ = no action must be ON (‘1’) 20 dropframe RA INT-DataIngest 0 Switch to select action if CRC check Relevant only if fails : ‘1’ = entire image frame to be switch for CRC discarded; or ‘0’ = only the individual test is turned ON failed packets (2048 bytes) to be (‘crcflag’ = ‘y’; discarded. see #14 above) 21 ThresholdValue RA INT 400000 Threshold value to identify pixel with Cosmic Ray Cosmic Ray hit (for INT mode) detection is effectively OFF 22 flatfieldFlag RA INT 1 Flat Field correction Switch : ‘1’= apply Flat Field Flat Field correction; ‘0’= no action correction must be ON (‘1’) 23 Nacc RA INT 1 Effectively selects the size of the Time Allowed values bin for drift extraction; ‘Nacc’ is the no. include any of successive raw INT mode frames integer : 1 / 2 / 3 / accumulated to generate a single image 4 ... etc. The (from which stars are identified) & value of 1 is processed further optimal for typical spacecraft drift.

24 refineWindow RA INT 15 Size (pixel unit) of the square window Selection MUST considered (centered on each star be ‘15’ candidate in the First-cut list) to further shortlist identifying local maxima (leading to generate Refined list);

... Continued

J. Astrophys. Astr. (0000)000: Page 45 of

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 25 centroidWindow RA INT 3 Size (pixel unit) of the square window Selection MUST used to compute Centroid values (along be ‘3’ X & Y axes) for each entry in the Refined list;

26 threshold RA INT 10 Parameter related to threshold for star ‘AVG’ & detection - starting value of ‘p’ in : ‘SIGMA’ are Threshold = AVG + p * SIGMA; ‘p’ is average and gradually decreased iteratively till standard required no. of stars are found. deviation of values in pixels (with outliers removed) in dark substracted image array (for INT mode only).

27 framesToBeDiscard RA INT 1 Number of initial images (each obtained Valid range of by accumulating ‘Nacc’ raw images) to values : 0/ 1/ 2/ be ignored (skipped) prior to identifying ... less than the the Reference Frame (or its beginning total no. of sample) images. Can be used to skip data patch with unusually large drift.

28 averageFactor RA INT 1 A second level of Time bin selection : Valid range of centroids of detected stars from selected values : 1/ 2/ 3/... number of successive ‘accumulated’ etc. frames (each comprising of ‘Nacc’ raw Optimal value for frames) are averaged to define the typical drift is Reference Frame & similarly averaged ‘1’. centroid tables for future time bins;

29 freqDomainFilterFlag RA INT 2 Switch to select kind of filtering on the Default value is Drift Series (low pass filtering) : ‘0’= conservative (by- Time domain; ‘1’= Frequency domain; passing the & ‘2’= no Filtering; filter). Under special circumstances, the filter can be useful.

30 freq value RA INT 0.2 Cut-off frequency (Hz); Default is max. Relevant only if Frequency domain allowed, filtering is selected; (i.e. corresponding to ‘freqDomainFilterFlag’=‘1’, see #29 the bandwidth for above) drift extraction from VIS. Lower values are valid.

31 orderPitch RA INT 1 Polynomial order for filtering time series Choice is of PITCH component of drift appropriate for default Time Window (4 sec).

32 orderYaw RA INT 1 Polynomial order for filtering time series See #31 of YAW component of drift 33 orderRoll RA INT 1 Polynomial order for filtering time series See #31 of ROLL component of drift 34 typeFiltering RA INT 2 Switch for selection among 3 options in Global option fits Time domain filtering : ‘0’= global; the entire time 1=polynomial; 2= local (sliding series of drift at polynomial) ; once. Local option fits many times, using a sliding Time Window (‘deltaTime’ = 4 sec, see #35 below).

35 deltaTime RA INT 4 Selection of Time Window for the ‘local’ (seconds) option of Time domain filtering; (Relevant only if ‘typeFiltering’=2, see #34 above)

... Continued

Page 46 of J. Astrophys. Astr. (0000) 000:

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 36 diffDist RA INT 1 Parameter for drift computation. Search distance Selection of initial search distance (pixel is gradually unit) for identifying star matches among increased if no images from successive time bins; match is found. (up to a fixed max. value).

37 GenMatchStarsFile flag RA INT 0 Switch regarding writing record of star matched star-pair lists from two successive time bins; ‘1’= write & ‘0’= do not write;

38 shiftRotDetAlgoFlag RA INT 1 Switch to select (among 3 available Equal weights options) the scheme for computation of to each star drift. The 3 choices are : (1) Equal provides uniform weight to each star & rotation angle representation to d theta, between successive time the full sky field, bins is small; (2) Intensity based improving weight; (3) d theta can be large. precision of the extracted drift.

39 flag thetaComp RA INT 0 Switch to include or exclude ‘rotation’ (d theta), in drift computation; ‘1’ = d theta parameter is included along with ‘Xshift’ & ‘Yshift’; & ‘0’ = only ‘Xshift’ & ‘Yshift’ to be extracted;

Parameters for RA PC For ‘drift’ extraction from Relative Aspect NUV /FUV photon event list Series Chain (PC) (in Photon Counting Mode) 40 historyrapc RA PC y Switch to retain history or not; (similar Records settings to ‘history’, see #11 above); of all switches & parameters for the RA PC Chain (#40 to #66 as listed in this table) 41 clobberrapc RA PC y Action in case the output directory chosen by the user is already existing; (similar to ‘clobber’, see #12 above);

42 GTI FLAGrapc RA PC-DataIngest 0 GTI filtering to be done(1) or not(0) Not using GTI filter 43 crcflagrapc RA PC n Switch to select if CRC check to be CRC check is carried out (‘y’), or not (‘n’). If ‘y’ is ignored. Bit error selected, another switch rate in general is (‘dropframerapc’, see #44) selects the very low. action : to drop the affected packet alone or all packets for that image frame.

44 dropframerapc RA PC-DataIngest 0 Switch to select action if CRC check Relevant only if fails : ‘1’ = entire image frame to be switch for CRC discarded; or ‘0’ = only the individual test is turned ON failed packets (2048 bytes) to be (‘crcflagrapc’ = discarded ‘y’; see #43 above).

45 parityFlagrapc RA PC 2 Switch for qualifying criteria of photon Default option events based on their parity tests; ‘1’= tests the 2 crucial all three words for the event must have words. The 3-rd correct parity, ‘2’= the two words word holds event holding X & Y centroids must have asymmetry. correct parity. Statistics of The option ‘0’ by-passes parity tests rejected events completely. based correction is applied to retain photometric accuracy.

... Continued

J. Astrophys. Astr. (0000)000: Page 47 of

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 46 thresholdMultphrapc RA PC 9999 Threshold for identifying multiple Test to identify photon events (from asymmetry in the multi-photon event’s 5x5 pixel footprint); events is turned Event with ‘Max-Min’ among 4 corners OFF. above selected ‘thresholdMultphrapc’ Recommended are flagged as multi-photon event. value to turn the test ON is ‘100’.

47 flatfieldFlagrapc RA PC 0 Switch for applying Flat field correction : ‘1’ = apply; ‘0’ = no action;

48 thresholdrapc RA PC 10 Parameter related to threshold for star Similar to detection (first-cut peaks); Starting value ‘thresholdpc’, see of ‘p’ in : Threshold = AVG + p * #3 above. SIGMA; ‘p’ is gradually decreased iteratively till required no. of stars are found.

49 GenMatchStarsFile flagrapc RA PC 0 Switch regarding writing record of star Similar to matched star-pair lists; ‘1’= write & ‘GenMatchStarsF ‘0’= do not write; ile flag’, see #37 above.

50 refinedWinSizerapc RA PC 15 Neighbourhood criteria for identifying Selection MUST stars; (pixel unit) be ‘15’. Similar to ‘refineWindow’, see #24 above.

51 centroidWinSizerapc RA PC 3 Size of square box to compute Centroids Selection MUST for detected stars (pixel unit); be ‘3’. Similar to ‘centroidWindow’, see #25 above.

52 framesDiscardrapc RA PC 2 Number of initial frames to be discarded Default choice of before initiating accumulation of frames; ‘2’ is optimal, Valid values : 0 / 1 / 2/ ... less than total since only the frames. very first frame is found to be ‘disturbed’.

53 framesComputerapc RA PC 90 ( 3 Number of successive frames to be Selection sec per combined (accumulated) for generating depends on NUV image) every image to be used for extracting brightness of drift; (effectively selects the Time bin) field stars 54 framesToBeDiscardrapc RA PC 1 Number of initial ‘combined’ The default value (accumulated) frames to be discarded ‘1’, ignores prior to identifying the Reference Frame initial 3 sec, (or its beginning sample). which is Valid choices are 0 /1 / 2/ 3 ...etc., less appropriate. than total data set. Can be used to skip data patch with unusually large drift.

55 averageFactorrapc RA PC 1 A second level of selection to widen the Optimal value Time bin : number of successive for typical drift is ’combined’ (accumulated) frames, whose ‘1’. Similar to star centroids need to be averaged to ‘averageFactor’, construct Reference Frame (& also for see #28 above. subsequent future Time bins) Valid range of numbers : 1/ 2/ 3/... etc. Larger number implies cruder time sampling of drift.

56 flag thetaComprapc RA PC 0 Switch to include (‘1’) or exclude (‘0’) Similar to ‘rotation’ (d theta) in drift ‘flag thetaComp’, computation; see #39 above.

57 diffDistrapc RA PC 1 Parameter for drift computation. Search distance is Selection of initial search distance (pixel gradually unit) for identifying star matches among increased if no centroids from successive time bins; match is found. (up to a fixed max. value). Similar to ‘diffDist’; see #36 above.

... Continued

Page 48 of J. Astrophys. Astr. (0000) 000:

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 58 freqDomainFilterFlag RA PC 2 Switch to select kind of low pass Similar to rapc filtering on the Drift Series; ‘freqDomainFilter Flag’, see #29 above.

59 freqValuerapc RA PC 0.2 Cut-off frequency (Hz); (Only for Similar to Frequency domain filtering selection) ‘freq value’, see see #30 above.

60 orderPitchrapc RA PC 1 Polynomial order for filtering PITCH Similar to component of drift ‘orderPitch’, see see #31 above.

61 orderYawrapc RA PC 1 Polynomial order for filtering YAW See #60 component of drift 62 orderRollrapc RA PC 1 Polynomial order for filtering ROLL See #60 component of drift 63 typeFilteringrapc RA PC 2 Switch for selection among 3 options in Similar to Time domain filtering; ‘typeFiltering’, see #34 above.

64 deltaTimerapc RA PC 4 Selection of Time Window for the ‘local’ (seconds) option of Time domain filtering; (Relevant only if ‘typeFilteringrapc’=2, see #63 above) 65 shiftRotDetAlgoFlag RA PC 3 Switch to select (among 3 available The 3 algorithms rapc options) the scheme for computation of are described for drift ‘shiftRotDetAlgo Flag’, see #38 above 66 minimumTargetedStars RA PC 4 Minimum no. of stars demanded in the Similar to rapc module for star detection ‘minimumTargeted (uvtDetectStar; PC mode) Stars’, see #4 above;

Parameters for L2 PC (for For generating NUV /FUV sky Sky Imaging chain NUV /FUV) images from photon event list (Level2PC) : (in Photon Counting Mode) 67 historypc L2 PC-NUV y Switch to write history or not; Records settings /68 /historypcfuv /L2 PC-FUV (similar to ‘history’ in #11 above); of all switches & parameters for the L2 PC Chain for NUV/ FUV; (#67/68 to #119/120 as listed in this table) 69 clobberpc L2 PC-NUV y Action in case the output directory /70 /clobberpcfuv /L2 PC-FUV chosen by the user is already existing; (similar to ‘clobber’ in #12 above);

71 GTI FLAGpc L2 PC-NUV 0 GTI filtering to be done(1) or not(0) Not using GTI /72 /GTI FLAGpcfuv DataIngest filter /L2 PC-FUV DataIngest 73 crcflagpc L2 PC-NUV n Switch to select if CRC check to be CRC check is /74 /crcflagpcfuv /L2 PC-FUV carried out (‘y’), or not (‘n’). If ‘y’ is ignored. Bit error selected, another switch (‘dropframepc’ rate in general is /‘dropframepcfuv’, see #81/82 below) very low. selects the action : to drop the affected packet alone or all packets for that image frame.

75 pathToOutputTarpc L2 PC-NUV - path for storing the output products of Not relevant /76 /pathToOutputTarpc /L2 PC-FUV L2 PC chain, when run as a stand alone when running full fuv chain; Driver Scheme 77 parityFlagpc L2 PC-NUV 2 Switch for qualifying criteria of photon Details similar to /78 /parityFlagpcfuv /L2 PC-FUV events based on their parity tests; ‘parityFlagrapc’, see #45 above.

79 thresholdMultphpc L2 PC-NUV 9999 Threshold for identifying multiple Test to identify /80 /thresholdMultphpcfuv /L2 PC-FUV photon events. multi-photon Similar to ‘thresholdMultphrapc’, events is turned OFF in #46 above; Recommended value to turn it ON is ‘100’.

... Continued

J. Astrophys. Astr. (0000)000: Page 49 of

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 81 dropframepc L2 PC-NUV 0 Switch to select action if CRC check Relevant only if /82 /dropframepcfuv DataIngest fails : ‘1’ = entire image frame to be switch for CRC /L2 PC-FUV discarded; or ‘0’ = only the individual test is turned ON DataIngest failed packets (2048 bytes) to be (‘crcflagpc’ / discarded ‘crcflagpcfuv’ = ‘y’; see #73/ #74 above).

83 thr One crpc L2 PC-NUV 9999 Value of the parameter no. 1 for Cosmic Ray /84 /thr One crpcfuv /L2 PC-FUV identifying Cosmic Ray affected frames, affected frame “N”, in equation : threshold = AVG + identification is N*sqrt (AVG) + ST/(sqrt(AVG)) ; effectively turned where AVG= average no of events per OFF. frame; Recommended value to turn it ON is ‘3’.

85 thr Two crpc L2 PC-NUV 9999 Value of the parameter no. 2 for Cosmic Ray /86 /thr Two crpcfuv /L2 PC-FUV identifying Cosmic Ray affected frames, affected frame “ST”; (see ‘thr One crpc’ / detection is ‘thr One crpcfuv’, #83/ #84 above); turned OFF. Recommended value to turn it ON is ‘10’.

87 CentCorr tobedonepc L2 PC-NUV 0 Switch regarding application of /88 /CentCorr tobedonepc /L2 PC-FUV corrections to event centroids due to

fuv Dark : ‘1’ = apply; ‘0’ = no action 89 CentBias tobedonepc L2 PC-NUV 0 Switch regarding application of /90 /CentBias tobedonepc /L2 PC-FUV corrections to event centroids due to

fuv Bias (FPN) : ‘1’ = apply; ‘0’ = no action 91 DetectDist tobedone L2 PC-NUV 1 Switch for Detector Distortion /92 pc /L2 PC-FUV correction : ‘1’ = apply;

/DetectDist tobedone ‘0’ = no action pcfuv 93 OpticDist tobedone L2 PC-NUV 1 Switch for Detector Distortion /94 pc /L2 PC-FUV correction : ‘1’ = apply;

/OpticDist tobedone ‘0’ = no action pcfuv 95 frameIntFlagpc L2 PC-NUV 0 Switch selection for ’Frame Integration’ Default is /96 /frameIntFlagpcfuv /L2 PC-FUV block : to divide the full data from the ‘Episode’ case, to ‘Episode’ into smaller parts (‘pseudo- use the full data Episode’-s) or not; ‘1’ = divide into together (i.e. no multiple parts (‘pseudo-Episode’ case); division into ‘0’ = all data used together as a ‘pseudosingle set (‘Episode’ case); Episode’-s).

97 framesDiscardpc L2 PC-NUV 2 Number of initial frames to be discarded Valid range of /98 /framesDiscardpcfuv /L2 PC-FUV (prior to gridding photon events into values : 0/ 1/ 2/ 2-D array/(s) in ‘Frame Integration’ block) ... less than the total no. of images.

Choice optimal, since only the very first frame is found to be ‘disturbed’.

99 framesComputepc L2 PC-NUV 9400 Number of successive frames to be Relevant only if /100 /framesComputepcfuv /L2 PC-FUV (say) combined together to form a ‘pseudo- ‘pseudo-Episode’ Episode’, in the ‘Frame Integration’ case is selected block. for dividing the Should not exceed the total no. of full data from the frames in the full Episode. ‘Episode’ into In general, the last ‘pseudo-Episode’ multiple parts will consist of fewer no. of frames, when (i.e.‘frameIntFlagpc’ total no. is not an integral multiple of /‘frameIntFlagpcfuv’ this selection. =‘1’; see #95 /#96)

... Continued

Page 50 of J. Astrophys. Astr. (0000) 000:

Table 7. (Continued) : List of all user selectable switch settings and parameters available through Parameter Interface Library, PIL.

Serial Parameter name Processing Suggested Description Comments No. Chain Default value 101 refinedWinSizepc L2 PC-NUV 15 Neighbourhood criteria for identifying Selection MUST /102 /refinedWinSize /L2 PC-FUV stars (pixel unit); be ‘15’ (similar to pcfuv ‘refineWindow’, see #24 above);

103 centroidWinSizepc L2 PC-NUV 3 Size of square box to compute Centroids Selection MUST /104 /centroidWinSize /L2 PC-FUV for detected stars (pixel unit); be ‘3’ (similar to pcfuv ‘centroidWindow’, see #25 above);

105 diffDistpc L2 PC-NUV 1 Selection of initial search distance (pixel Search distance is /106 /diffDistpcfuv /L2 PC-FUV unit) for identifying star matches gradually between a pair of images from ‘pseudo- increased if no Episode’-s; (used for ‘pseudo-Episode’ match is found case in Frame Integration block) (up to a fixed max. value).

107 shiftRotDetAlgo L2 PC-NUV 1 Switch to select (among 3 available The 3 algorithms /108 Flagpc /L2 PC-FUV options) the algorithm for determining are similar to /shiftRotDetAlgo offsets (shift & rotation) between images those described for Flagpcfuv from a pair of ‘pseudo-Episode’-s; ‘shiftRotDetAlgoFlag’, (used for ‘pseudo-Episode’ case in see #38 above Frame Integration block) 109 flag thetaComppc L2 PC-NUV 0 Switch to include (‘1’) or exclude (‘0’) Similar to /110 /flag thetaComp /L2 PC-FUV ‘rotation’ (d theta) in computation ‘flag thetaComp’, pcfuv of offset; (used for ‘pseudo-Episode’ see #39 above; case in Frame Integration block) 111 thresholdpc L2 PC-NUV (& 50 Threshold for star detection (first-cut See details in #3 /112 /thresholdpcfuv DRIVER SCHEME) /10 peaks) - starting multiplier, ‘p’, of sigma above. /L2 PC-FUV in : Threshold = AVG + p * SIGMA; The parameter [used by Astrometry block; and ‘thresholdpc’ is used for ‘pseudo-Episode’ case in Frame common to Integration block] Driver Scheme & L2 PC Chain for NUV.

113 database namepc L2 PC-NUV - Path pointing to star catalogue (USNO /114 /database name /L2 PC-FUV A2) database; used for matching stars in pcfuv Astrometry block.

115 search algo for L2 PC-NUV 2 Switch to select type of Search area in /116 FullFrameAstpc /L2 PC-FUV the star Catalog : ‘1’ = Square box;

/search algo for ‘2’ = Circular; FullFrameAstpcfuv 117 Radi searchpc L2 PC-NUV 0.05 Dimension of Search area (length of Default choice is /118 Radi searchpcfuv /L2 PC-FUV square box or radius of circle) to find based on matching stars from Catalogue; accuracy of (in degrees) spacecraft’s attitude.

119 minimum targeted L2 PC-NUV 5 Success Criterion for Astrometry stage : The parameter /120 starspc /L2 PC-FUV minimum no. of star matches with ‘minimum /minimum targeted Catalogue demanded; targetedstarspc’ is starspcfuv common to Driver Scheme & L2 PC Chain for NUV (see #5 above).