arXiv:2203.16061v1 [cond-mat.mtrl-sci] 30 Mar 2022

Origin of Perpendicular Magnetic Anisotropy in Co_xFe_{3−x}O_{4+δ} Thin Films Studied by X-ray Magnetic Circular and Linear Dichroisms

Jun Okabayashi^{1,∗}, Masaaki A. Tanaka^2, Masaya Morishita^2, Hideto Yanagihara^3, and Ko Mibu^2 1Research Center for Spectrochemistry, The University of Tokyo, Bunkyo-ku, Tokyo 113-0033, Japan 2Graduate School of Engineering, Nagoya Institute of Technology, Nagoya 466-8555, Japan 3Institute of Applied Physics, University of Tsukuba, Tsukuba 305-8573, Japan (Dated: March 31, 2022)

We investigate the element-specific spin and orbital states and their roles on magnetic anisotropy in the Co-ferrite (CoxFe3−xO_{4+δ} (001)) thin films which exhibit perpendicular magnetic anisotropy (PMA). The origin of PMA in the low x region (x < 1) can be mainly explained by the large perpendicular orbital magnetic moments in the Co^{2+} (3d^7) states detected by X-ray magnetic circular and linear dichroisms (XMCD/XMLD). The XMLD for a PMA film (x = 0.2) with square hysteresis curve shows the oblate charge distribution in the Co^{2+} site, which is consistent with the change in local nearest neighbor distance in Co detected by extended X-ray absorption fine structure analysis. Our finding reveals that the microscopic origin of PMA in Co-ferrite comes from the enhanced orbital magnetic moments along out-of-plane [001] direction through in-plane charge distribution by tensile strain, which adds the material functionalities in spinel ferrite thin films from the viewpoint of strain and orbital magnetic moments.

Perpendicular magnetic anisotropy (PMA) is one of the crucial issues in the spintronics research field from the viewpoints of thermal stability enhancement and highdensity storage technology with the low current magnetization switching. Until now, tremendous efforts have been devoted to design the materials with large PMA to add the novel functionalities and external field controlling of magnetic properties [1–5]. Among them, the magnetic oxides possess a number of attractive advantages for the spintronics devices because of their semiconducting or insulating behavior with high spin polarization. These magnetic oxides can be utilized as spin-filtering effects, resulting in high tunnel magnetoresistance with multiferroic properties by controlling the tensile or compressive strains in the thin films [6–8].

Most famous spinel-type compounds for spintronics application might be Co-ferrites (CoFe_2O_4: CFO) epitaxial thin films because of their insulating advantages as spin-filtering, high-frequency performance, and magnetostrictive properties [9–16]. Further, the interfacial proximity effect, emerging on films with non-magnetic heavymetal elements which possess a large atomic spin-orbit interaction [17–19], also develops as the spin-orbitronics researches through the interfacial spin-orbit coupling. Recent development appends further functionality of large PMA in CFO in the order of 10^6 J/m^3 by tuning the Co compositions [20–23]. Since CFO exhibits high magnetostriction coefficient (λ_{100} = –590 × 10^{−6}), the strain from the substrates propagates into the CFO layer, which brings the local distortion around the transition-metal (TM) cation sites. In fact, the lattice mismatching between MgO (4.21 Å) and CFO (8.38 Å) forming almost the double period brings the epitaxial crystalline growth with a few percentages of tensile strain into CFO thin layer. Depending on the Co compositions, the lattice constants of CFO can be tuned systematically. Structural and magnetic properties in the CFO thin films can be controlled by the cation vacancies and anti-phase boundaries which are generated during the crystalline growth and suppress the saturation magnetization values through the antiparallel spin coupling [24–27]. Historically, magnetic anisotropy in bulk CFO has been understood as an effect that the average of <111> easy axes direction produces cubic anisotropy in Co^{2+} [28– 30]. Recent theoretical and experimental investigations for CFO thin films suggest that the tensile strain into CFO layer produces the PMA [31–38]. Squareness of outof-plane hysteresis curves depends on the growth mode, such as molecular-beam epitaxy, pulsed-laser deposition (PLD), or sputter deposition. It is also reported that the PMA increases in off-stoichiometric CFO films with low Co compositions [22, 23]. Although the PMA in CFO is strongly demanded for spinel-type oxide spintronics and spin-orbitronics by controlling the orbital states [39], the microscopic origin of the PMA appearing in the low Co compositions of CFO has not been clarified yet.

In order to understand the PMA in CFO, the elementspecific orbital magnetic moments (m_{orb}) and their orbital anisotropy have to be examined explicitly. In particular, m_{orb} is expected to be sensitive to the strain and local symmetry from the ligand fields around the TM ions. X-ray magnetic circular and linear dichroisms (XMCD / XMLD) with their magneto-optical sum rules are powerful tools to detect the element-specific spin and orbital states in each site with the charge asphericity [40]. Especially, XMLD sum rules can probe the orbital anisotropy (Q = 3L^2_z − L^2) in the notation of orbital angular momentum (L) and electric quadrupoles (Q). Furthermore, since the Fe L-edge spectra consist of the signals of three kinds of Fe^{2+} or Fe^{3+} states with octahedral O_h and tetrahedral T_d symmetries, the XMCD and XMLD magneto-optical sum rules for the integrals of Fe L-edge spectra cannot be adopted without separating each contribution. Site- and state-resolved analyses become a crucial role for understanding the origin of PMA. For the analysis of XMCD and XMLD spectra, the ligand-field multiplet (LFM) cluster-model simulations including the configuration interaction (CI) approach are used to determine the site-specific electronic structure parameters accompanied by spin and orbital magnetic moments and their anisotropies [41]. Until now, the XMCD and XMLD for CFO with in-plane anisotropy have been extensively studied with angular dependence between incident polarized beam, magnetic field, and sample surface normal [42–45]. However, the X-ray magnetic spectroscopy investigations for the PMA films with square magnetization–magnetic field (M-H) hysteresis shape in low Co compositions have not been pursued. We have proceeded the XMLD measurements for probing the orbital anisotropy in several PMA systems by using remanent magnetization states in the polar Kerr geometry [46, 47]. On the other hand, recent operando-XMCD technique enables manipulation of out-of-plane and inplane m_{orb} by controlling strain in the magnetic multilayers, which is a microscopic origin of magneto-striction; that leads to the observation of an effect proposed as ”orbital-striction effect” [48]. The PMA in strained CFO can be also categorized as a novel orbital-controlled material system by using the orbital degeneracy in Co^{2+} 3d^7 system in O_h ligand field. Furthermore, extended x-ray absorption fine structure (EXAFS) analysis through the multiple-scattering process is also employed to determine the element-specific structural characterization. The precise determinations of spin and orbital states become a key solution to develop a strain-induced orbital physics and their applications using CFO.

In this study, considering above research motivations, we aim to investigate the origin of PMA in CFO from the viewpoint of element-specific spin and orbital magnetic moments and their anisotropy using XMCD and XMLD with LFM calculations and local structure detection by EXAFS analysis.

The Co_xFe_{3−x}O_{4+δ} (001) samples (x=0.2 and 0.6) were prepared by PLD on the MgO (001) substrates with the similar recipe of reference [23]. The PLD was performed under the conditions of the substrate temperature of 300^∘C, the background oxygen pressure of 6.0 Pa, and the deposition rate of 0.03 nm/s. A neodymium-doped yttrium-aluminum-garnet laser at the double frequency (532 nm) with the pulse width of 6 ns and the repetition rate of 30 Hz was used. The energy density of the laser beam was controlled to 1 J/cm^2 by an optical lens. The 13-nm-thick CFO (001) layer with 1-nm-thick Cu capping layer was deposited for various Co compositions (x). Excess oxygens accompanied by possible cation vacancies are described as δ. The case of x=0.2 and 0.6 exhibits the PMA and in-plane anisotropy, respectively. The in-plane anisotropy in Co_{0.6}Fe_{2.4}O_{4+δ} is produced by the post annealing at 400^∘C after the growth by releasing the strain. The results of sample characterization by Xray diffraction (XRD) and magnetization measurements are shown in Supplemental Material (Fig. S1) [49].

The XMCD and XMLD were performed at BL-7A and 16A in the Photon Factory at the High-Energy Accelerator Research Organization (KEK-PF). For the XMCD measurements, the photon helicity was fixed, and a magnetic field of ±1.2 T was applied parallel to the incident polarized soft x-ray beam, to obtain signals defined as μ+ and μ− spectra. The total electron yield mode was adopted, and all measurements were performed at room temperature. The X-ray absorption spectroscopy (XAS) and XMCD measurement geometries were set to normal incidence, so that the directions of photon helicity axis and the magnetic field were parallel and normal to the surface, enabling measurement of the absorption processes involving the normal components of the spin and orbital magnetic moments. In the XMLD measurements, the remanent states magnetized out-of-plane were adopted. For grazing incident measurements in XMLD, the tilting angle between incident beam and sample surface normal was kept at 60^∘. The direction of the electric field (E) of the incident linearly polarized synchrotron beam was tuned horizontally and vertically by undulator. We define the sign of XMLD by the subtraction of the (M‖E)−(M⊥E) spectra with respect to the magnetization M. The EXAFS measurements at Co K-edge were performed at BL-12C in KEK-PF using the florescence yield mode with a 19-element solid-state detector at room temperature.

Figure 1 shows the XAS and XMCD of Co_{0.2}Fe_{2.8}O_{4+δ} for Fe and Co L-edges at the normal incidence setup. Spectra are normalized at each absorption edge. Because of the composition ratio of Co:Fe=1:14, the XAS intensities of Co are suppressed. XMCD intensity ratio to XAS is estimated to be 5% and 47% for Fe and Co L_3 edge, respectively. The raw data are displayed at the Supplemental Material (Fig. S2). XAS and XMCD line shapes for Fe L-edges show distinctive features due to the three kinds of Fe states (Fe^{3+} in O_h, Fe^{3+} in T_d, and Fe^{2+} in O_h). For the Fe L-edges, although the difference in XAS is small, clear differential XMCD line shapes are detected. The Fe^{3+} state with T_d symmetry exhibits opposite sign, which is common for the spinel ferrite compounds. On the other hand, in the case of Fe_3O_4, the Fe^{2+} component is more enhanced [50]. Large XMCD signals in Co L-edge correspond to the saturated magnetized states. Within the orbital sum rule, the large m_{orb} gives rise to the asymmetric XMCD line shapes. Since the Co site is almost identical as Co^{2+}(O_h) symmetry, the sum rules can be applicable for the Co XMCD spectra. The spin and orbital magnetic moments for Co^{2+} sites are estimated as 1.32±0.20 and 0.63±0.09 μ_B, respectively, using an electron number of 7.1. The error bars mainly originate from the estimation of background in XAS which is used for the sum rule analysis. Large m_{orb} originates from the orbital degeneracy in d^7 electron system in the strained Co site. The multiplet structures are almost similar to the previous report by the LFM calculations along the easy-axis direction [44, 45]. In order to confirm the PMA, the element-specific magnetic hysteresis curves are measured at each peak in Fe and Co L_3 edge. As shown in Fig. 1(c), clear square shapes are detected at each photon energies due to the out-of-plane easy axis, which is almost consistent with the magnetization measurement shown in Fig. S1 [49]. The square M-H curves for all energies suggest the strong exchange coupling among each site. The opposite sign in the M-H curves at Fe^{3+} T_d site and Fe^{2+}/Co^{2+} O_h sites originates from the antiferromagnetic super-exchange interaction among these sites. These suggest that the small amounts of anisotropic Co sites with large m_{orb} govern the easy axis direction of Fe sites and stabilize the PMA.

Figure 2 shows the E vector polarization dependent XAS, where the electric field E is parallel and perpendicular to the out-of-plane magnetization direction. The differential line shapes were similar to those of previously reported spectra [44]. Because of small difference in XAS by the horizontal (parallel) and vertical (perpendicular) beams as shown in the inset of Fig. 2, XMLD intensities are also suppressed and displayed in the different scales. For Fe L-edge XMLD, the overlapping of three kinds of components brings complex differential line shape. We note that the integrals of the XMLD line shapes are proportional to the charge asphericity within the XMLD sum rule [51]. For Co L-edge XMLD of the Co^{2+} O_h site, we confirmed that the integral of XMLD converges to a negative value, deducing that the sign of Q_{zz}, where Q_{zz} is the diagonal tensor component of electric quadrupole moment describing the charge distribution asphericity as Q_{xx} + Q_{yy} + Q_{zz} = 0, is negative with the order of 10^{−1}. The result means the in-plane orbital states are strongly coupled with E. This value can be also estimated from the XMCD spin sum rule considering the magnetic dipole m_{Tz} term. Since the measurement geometry of 60^∘ tilted from the sample surface normal cannot detect precise orthogonal direction, the oblique angle suppresses the linear dichroism intensity to √ 3/2. The orbital polarization of Co 3d states means the pancake-type oblate charge distribution, which enhances out-of-plane component of m_{orb}. Therefore, with both XMCD and XMLD combined, it can be concluded the in-plane tensile strain triggers the changes of charge distribution along in-plane direction, resulting in the large out-of-plane m_{orb} and the PMA.

For the analysis of XMCD and XMLD spectra, we employed cluster-model calculations including the CI for Co^{2+} and Fe sites in Co_{0.2}Fe_{2.8}O_{4+δ} as tetrahedral (T_d) TMO_4 and octahedral (O_h) TMO_6 clusters, modeled as a fragment of the spinel-type structures. The Hamiltonian included the electronic structure parameters of full on-site TM 3d–3d (valence–valence) and 2p–3d (core–valence) Coulomb interactions (U) and the T_d or O_h crystal fields (10Dq) in the TMs, along with the hybridization between the TM 3d and O 2p wave functions. The charge-transfer energy was defined as Δ=E(3d^{n+1}L) − E(3d^n), where L denotes a hole in a ligand p orbital. The hybridization between the TM 3d and O 2p states was also parameterized in terms of the Slater–Koster parameters (pdσ) and (pdπ), where the relation (pdσ) = –1/2(pdπ) was used [52]. The parameters (ppσ) and (ppπ) were always set to zero. In all cases, a Gaussian broadening was used to simulate spectral broadening.

As shown in Fig. 3, spectral line shapes of XMCD and XMLD can be reproduced by the LFM calculations qualitatively, at least the peak positions, with three Fe states and uniformed Co state. The fitting parameters are listed in Table I. We emphasize the same adjusted parameters of Δ, U and pdσ and intensity ratios of each component for XMCD and XMLD are applicable for the fitting. In comparison with the previous first-principles calculations of CFO, the values of U = 5 eV are also plausible from the viewpoints of LFM calculations [53– 56]. The multiplet parameter values are almost similar to the previous report [57]. For the Co^{2+} 3d^7 case, the t_{2g} states are split into two levels by the tetragonal distortion, and the lowest xy states are occupied by one of the down spin electrons. The other electron occupies the degenerated yz or zx states [35]. We determined the tetragonal distortion for the Co 3d states (D_{tet}) to be 0.02 eV in order to reproduce the XMCD and XMLD spectral line shapes qualitatively. However, the best fitted parameter sets shown in Table I are not sensitive to the parameters caused by the strain. The intensity ratio of Fe^{3+} T_d, Fe^{3+} O_h, and Fe^{2+} O_h is deconvoluted to be 1:1.3:0.25 in the fitting of Fe L_3-edge XMCD and XMLD affecting the decrease of Fe^{2+} states in the inverse spinel structure. The Co L-edge line shapes are reproduced with only a single Co^{2+} site, except the peak at 779.5 eV in XMLD.

In order to confirm the local environment around the Co atoms, XAFS measurements with EXAFS analysis in the Co K-edge were performed to deduce the nearest neighbor distance through the Fourier transform. As shown in Fig. 4, the Co K-edge absorption spectra with EXAFS oscillatory behaviors are observed for x = 0.2 (PMA) and x=0.6 (in-plane anisotropy). We note that the Fe K-edge XAFS cannot be separated in the Fourier transform without some assumption because of the contributions of three kinds of states. Clear XAFS oscillation is detected and plotted in the wave number k in the inset of Fig. 4(a). XAFS oscillation functon k^3χ(k) can be fitted by FEFF8 program [58] and the Fourier transformed EXAFS profile is also displayed in Fig. 4(b) considering the information up to second nearest neighbor from the Co site. By using the fitting procedure, the nearest Co-O bond length in the Co sites is 2.09 and 2.08 Åfor PMA and in-plane cases, respectively, which is almost identical with the previous study [59]. The expansion of nearest neighbor in the PMA film is qualitatively consistent with the XRD shown in Fig. S1 [49]. Because of the effect of phase shift, the peak position in EXAFS is not related to the bond length directly. Coordination number also becomes large in the case of PMA because of the distorted local environment around Co site, which corresponds to the intensity of EXAFS profile in Fig. 4(b). These suggest the tensile local distortion triggers the PMA in the Co site of strained CFO.

Considering the above results, we discuss the electronic structures of CFO. First, we discuss the suppression of Fe^{2+} with increasing the Co composition. The previous report of Mössbauer spectra for related CFO with PMA suggests the suppression of Fe^{2+} [23], where ∼100 nm from the interface was probed using incident γ-rays and emitted conversion electrons. Since the probing depth region of XMCD is beneath 3 nm from the surface, finite Fe^{2+} states in XMCD is located at the surface region. The previous report suggests that the Fe^{2+} state is located at the surface region with inevitable lateral inhomogeneity [60].

Second, we discuss the occupation of cation sites by the charge neutrality and the number of cation elements. Using the Co concentration and charge neutrality in the inverse spinel structure of the formation of spinel structure of AB_2O_4 formula unit; Fe^{3+(Td)}(Co^{2+(Oh )}Fe^{2+(Oh )}Fe^{3+(Oh )})O_4, the following two equations are deduced for Co_{0.2}Fe_{2.8}O_{4+δ}; 14n_{Co}2+ =n_{Fe}2+ +n_{Fe}3+ , and 2n_{Co}2+ +2n_{Fe}2+ +3n_{Fe}3+ =8, where n is the number of each element and the cation vacancy is implicitly incorporated as δ. Since the ratio of n_{Fe}3+_{(Td)}, n_{Fe}2+_{(Oh)}, and n_{Fe}3+_{(Oh )} is estimated from the XMCD and XMLD analyses, these four parameters are calculated to be n_{Fe}3+_{(Oh )}=1.34, n_{Fe}3+_{(Td)}=1.03, n_{Fe}2+_{(Oh )}=0.26, and n_{Co}2+_{(Oh )}=0.19. These suggest that the existence of excess cation vacancies (n_v) can be estimated to be 0.185 from the equation for the cation site, n_v = 3 − n_{Fe}3+_{(Oh )} − n_{Fe}3+_{(Td)} − n_{Fe}2+_{(Oh )} − n_{Co}2+_{(Oh )}. We emphasize that the cation vacancy can be estimated quantitatively from the analysis of XMCD.

Third, we discuss the relationship between strain and orbital magnetic moments. For the Co^{2+} 3d^7 system, the ground state^4F multiplet energy split by the cubic crystal field to Γ_4 state, and further effects by trigonal or tetragonal field and exchange coupling stabilize the lowest 3d^7 states. The splitting of t_{2g} state promotes the degeneracy for spins as analogous to the 3d^2 system of spinel-type V^{3+} compounds [61, 62]. Large m_{orb} is recovered by the spin-orbit coupling ξ_{Co} of 70 meV. Since the uniaxial anisotropy in spinel-type Co ferrite is inevitably formed from the structural and electronic configuration, the out-of-plane easy axis can originate from the tensile strain effect. In the theoretical model calculation, the PMA energy (K) deduced from the energy difference along the axis direction can be expressed as K = E(100) − E(001) = −B_1χ, where B_1 and χ is the magneto-elastic coefficient and strain, respectively [34]. Phenomenological B_1 of 1.4×10^8 J/m^3 consists of the elastic constant and magneto-striction coefficient at room temperature for CoFe_2O_4. In the case of x=0.2, B_1x is applied to estimate K. Considering the lattice constants of a_‖ = 8.42Å and a_⊥ = 8.29Å estimated from the XRD, the strain of (a_‖ − a_⊥)/a_0∼1.5 % was deduced using the bulk CFO value a_0 = 8.38Å [32]. Therefore, the PMA energy is roughly estimated to 0.51 × 10^6 J/m^3. On the other hand, microscopic estimation of the PMA energy can be performed using anisotropic m_{orb} as

K = 1/4ξΔm_{orb}, where spin-orbit coupling constant is ξ and Δm_{orb} is the difference between out-of-plane and in-plane m_{orb}. Although the in-plane m_{orb} cannot be detected unless applying high magnetic field to saturate the magnetization along the hard axis, we used the value in the reference with extrapolation in low Co concentration [44]. Assuming the value of Δm_{orb} to be 0.2 μ_B, the PMA energy of Co can be estimated to be 1.6 × 10^6 J/m^3 with the assumption of the Co composition x=0.2 and strained CFO volume. The value of K from XMCD is overestimated compared with that from magnetization measurements, in general, by a pre-factor of 0.1 [63]. These estimations suggest that the PMA energy can be explained mainly by the contribution of small amount of anisotropic Co sites. Furthermore, the macroscopic magnetostriction effect, which the relation between strain and K, can be recognized including the m_{orb} from the viewpoint of electron theory as orbital-elastic effect. The contributions from the Fe^{3+} (3d^5) sites are negligible because of halffilled quenched orbital magnetic moments. The contribution from the Fe^{2+} (3d^6) sites is also quenched since the strained undegenerated level is occupied. Therefore, the origin of PMA in Co_{0.2}Fe_{2.8}O_{4+δ} can be predominantly explained by the enhanced m_{orb} of 1/14 Co compositions through the strained charge distributions, which can be recognized as diluted doped magnetic oxide systems.

Finally, we discuss the origin of PMA in the spinel-type oxides from the viewpoint of tensile or compressive strain and m_{orb}. The strain in CFO is derived from the tensile strain in the film, which is detected by the EXAFS analysis and confirmed by the sign of XMLD. Recent report shows that the PMA in spinel-type NiCo_2O_4 originates from the compressive strain in the film [64, 65] and that the enhancement of m_{orb} in XMCD measurements is not distinctive with the 2+ and 3+ mixed valence states of both Co and Ni sites [66]. Therefore, the PMA in spineltype oxides can be categorized by the tensile or compressive strain. Because of tensile strain, oblate-type charge distribution induces m_{orb} along out-of-plane direction, which is similar to the case of enhanced m_{orb} in Co/Pd multilayer [67]. On the other hand, in-plane compression or out-of-plane elongation modulates the proratetype charge distributions, which induces the quadrupole moments without enhancing m_{orb} as discussed in strained Mn_{3−x}Ga system [47].

In summary, using XMCD and XMLD, we investigated the element-specific orbital magnetic moments and their anisotropy in Co-ferrite thin films with low Co concentration which exhibit the PMA. The origin of PMA in CFO is explained by the large m_{orb} in the Co^{2+} (3d^7) states. The tensile lattice strain, which is deduced from EXAFS, induces the out-of-plane m_{orb} through the anisotropic inplane charge distribution. Furthermore, a novel method to estimate the number of cation vacancy from XMCD line shapes was also proposed. Our finding clearly reveals that the controlling strain modulates m_{orb}, which opens up the material functionalities in the oxide spinorbitronics by strain engineering, especially in the TM d^7 systems.

ACKNOWLEDGMENTS

This work was partially supported by JSPS KAKENHI (Grant No. 16H06332), the Kato Science and Technology

Foundation, the Izumi Science and Technology Foundation, and the Telecommunications Advancement Foundation. Parts of the synchrotron radiation experiments were performed under the approval of the Photon Factory Program Advisory Committee, KEK (Nos. 2019G028 and 2021G069).

[1] S. Mangin, D. Ravelosona, J. A. Katine, M. J. Carey, B. D. Terris, and Eric E. Fullerton Nature Materials 5, 210 (2006). Current-induced magnetization reversal in nanopillars with perpendicular anisotropy [2] S. Ikeda, K. Miura, H. Yamamoto, K. Mizunuma, H. D.

Gan, M. Endo, S. Kanai, J. Hayakawa, F. Matsukura, and H. Ohno, Nature Materials 9, 721 (2010), A perpendicular anisotropy CoFeB/MgO magnetic tunnel junction [3] Wei-Gang Wang, Mingen Li, Stephen Hageman, and C.

L. Chien, Nature Materials 11, 64 (2012), Electric-field-assisted switching in magnetic tunnel junctions [4] Takayuki Nozaki, Anna Koziol-Rachwal, Masahito Tsujikawa, Yoichi Shiota, Xiandong Xu, Tadakatsu Ohkubo, Takuya Tsukahara, Shinji Miwa, Motohiro Suzuki, Shingo Tamaru, Hitoshi Kubota, Akio Fukushima, Kazuhiro Hono, Masafumi Shirai, Yoshishige Suzuki, and Shinji Yuasa, NPG Asia Materials 9, 451 (2017). Highly efficient voltage control of spin and enhanced interfacial perpendicular magnetic anisotropy in iridium-doped Fe/MgO magnetic tunnel junctions [5] B. Dieny and M. Chshiev, Rev. Mod. Phys. 89, 025008 (2017). Perpendicular magnetic anisotropy at transition metal/oxide interfaces and applications [6] C A F Vaz,J. Phys.: Condens. Matter 24, 333201 (2012), Electric field control of magnetism in multiferroic heterostructures [7] Tomoyasu Taniyama, J. Phys.: Condens. Matter 27, 504001 (2015), Electric-field control of magnetism via strain transfer across ferromagnetic/ferroelectric interfaces [8] Diogo Castro Vaz, Agnes Barthelemy, and Manuel Bibes, Jpn.J. Appl. Phys. 57, 0902A4 (2018). Oxide spinorbitronics: New routes towards low-power electrical control of magnetization in oxide heterostructures [9] A. V. Ramos, M.-J. Guittet, and J.-B. Moussy, R. Mattana, C. Deranlot, and F. Petroff, and C. Gatel, Appl. Phys. Lett. 91, 122107 (2007), Room temperature spin filtering in epitaxial cobalt-ferrite tunnel barriers [10] Y. K. Takahashi, S. Kasai, T. Furubayashi, S. Mitani, K. Inomata, and K. Hono, Appl. Phys. Lett. 96, 072512 (2010), High spin-filter efficiency in a Co ferrite fabricated by a thermal oxidation [11] Nuala M. Caffrey, Daniel Fritsch, Thomas Archer, Stefano Sanvito, and Claude Ederer, Phys. Rev. B 87, 024419 (2013), Spin-filtering efficiency of ferrimagnetic spinels CoFe2O4 and NiFe2O4 [12] Michael Foerster, Milko Iliev, Nico Dix, Xavier Marti, Mykhailo Barchuk, Florencio Sanchez, and Josep Fontcuberta, Adv. Funct. Mater. 22, 4344 (2012), The Poisson Ratio in CoFe2 O4 Spinel Thin Films [13] Mateusz Scigaj, Nico Dix, Jaume Gazquez, Maria Varela,

Ignasi Fina, Neus Domingo, Gervasi Herranz, Vassil Skumryev, Josep Fontcuberta, and Florencio Sanchez, Scientific Reports 6, 31870 (2016), Monolithic integration of room temperature multifunctional BaTiO3 -CoFe2O4 epitaxial heterostructures on Si(001) [14] Yong Zhang, Lvkang Shen, Ming Liu, Xin Li, Xiaoli Lu, Lu Lu, Chunrui Ma, Caiyin You, Aiping Chen, Chuanwei Huang, Lang Chen, Marin Alexe, and Chun-Lin Jia, ACS Nano 11, 8002 (2017), Flexible Quasi-Two-Dimensional CoFe2 O4 Epitaxial Thin Films for Continuous Strain Tuning of Magnetic Properties [15] K. Prabahar, R. Ranjith, P. Saravanana, A. Srinivasa, Journal of Magnetism and Magnetic Materials 475, 276 (2019), Effect of magnetic field annealing on the magnetostriction and deflection properties of CoFe2O4 thin films grown by PLD [16] Hiroshige Onoda, Hiroaki Sukegawa, Jun-Ichiro Inoue, and Hideto Yanagihara, Adv. Mater. Interfaces 8, 2101034 (2021), Strain Engineering of Magnetic Anisotropy in Epitaxial Films of Cobalt Ferrite [17] Yajuan Hui, Weiming Cheng, Zhaobing Zhang, Haiwei Wang, Changsheng Xie, and Xiangshui Miao, Appl. Phys. Lett. 110, 192404 (2017), Transport mechanism of the magnetoresistance effects in Ta/CoFe2 O4 nanostructures [18] Hari Babu Vasili, Matheus Gamino, Jaume Gazquez, Florencio Sanchez, Manuel Valvidares, Pierluigi Gargiani, Eric Pellegrin, and Josep Fontcuberta, ACS Appl. Mater. Interfaces 10, 12031 (2018), Magnetoresistance in Hybrid Pt/CoFe2O4 Bilayers Controlled by Competing Spin Accumulation and Interfacial Chemical Reconstruction [19] Walid Amamou, Igor V. Pinchuk, Amanda H. Trout, Robert E. A. Williams, Nikolas Antolin, Adam Goad, Dante J. O’Hara, Adam S. Ahmed, Wolfgang Windl, David W. McComb, and Roland K. Kawakami, Phys. Rev. Mater. 2, 011401(R) (2018), Magnetic proximity effect in Pt/CoFe2 O4 bilayers [20] H. Yanagihara, K. Uwabo, M. Minagawa, Eiji Kita, and Noriyuki Hirota, J. Appl. Phys. 109, 07C122 (2011), Perpendicular magnetic anisotropy in CoFe2 O4 (001) films epitaxially grown on MgO(001) [21] Ryan Comes, Man Gu, Mikhail Khokhlov, Jiwei Lu, Stuart A.Wolf, J. Magn. Magn. Mater. 324, 524 (2012), Microstructural and domain effects in epitaxial CoFe2 O4 films on MgO with perpendicular magnetic anisotropy [22] Tomohiko Niizeki, Yuji Utsumi, Ryohei Aoyama, Hideto Yanagihara, Jun-ichiro Inoue, Yuichi Yamasaki, Hironori Nakao, Kazuyuki Koike, and Eiji Kita, Appl. Phys. Lett. 103, 162407 (2013), Extraordinarily large perpendicular magnetic anisotropy in epitaxially strained cobalt-ferrite CoxFe3−2xO4 (001) (x=0.75, 1.0) thin films

[23] Katsuyoshi Naruse, Masaaki Tanaka, Kosuke Nomura, Takuya Taniguchi, Syuta Honda, Teruo Ono, and Ko Mibu, J. Magn. Magn. Mater. 475, 721 (2019), Perpendicular magnetic anisotropy and tunneling conductivity of epitaxial cobalt-ferrite (001) films grown on nonmagnetic metal films [24] S. Celotto, W. Eerenstein, and T. Hibma, Eur. Phys. J.

B 36, 271 (2003). Characterization of anti-phase boundaries in epitaxial magnetite films [25] Amit V. Singh, Behrouz Khodadadi, Jamileh Beik Mohammadi, Sahar Keshavarz, Tim Mewes, Devendra Singh Negi, Ranjan Datta, Zbigniew Galazka, Reinhard Uecker, and Arunava Gupta, Adv. Mater. 29, 1701222 (2017), Bulk Single Crystal-Like Structural and Magnetic Characteristics of Epitaxial Spinel Ferrite Thin Films with Elimination of Antiphase Boundaries [26] Xiao Wang, Zhiwei Hu, Stefano Agrestini, Javier Herrero-Martín, Manuel Valvidares, Raman Sankar, Fang-Cheng Chou, Ying-Hao Chu, Arata Tanaka, Liu Hao Tjeng, Eric Pellegrin, Journal of Magnetism and Magnetic Materials 530, 167940 (2021). Evidence for largest room temperature magnetic signal from Co^{2+} in antiphase-free and fully inverted CoFe2 O4 in multiferroic-ferrimagnetic BiFeO3- CoFe2O4 nanopillar thin films [27] Zhuo Li, Jinlian Lu, Lei Jin, Jan Rusz, Vancho Kocevski, Hideto Yanagihara, Eiji Kita, Joachim Mayer, Rafal E. Dunin-Borkowski, Hongjun Xiang, and Xiaoyan Zhong, Adv. Funct. Mater. 31, 2008306 (2021), Atomic Structure and Electron Magnetic Circular Dichroism of Individual Rock Salt Structure Antiphase Boundaries in Spinel Ferrites [28] J. Slonczewski, Phys. Rev. 110, 1341 (1958). Origin of Magnetic Anisotropy in Cobalt-Substituted Magnetite [29] Masashi Tachiki, Progress of Theoretical Physics, 23, 1055 (1960). Origin of the Magnetic Anisotropy Energy of Cobalt Ferrite [30] John B. Goodenough, Magnetism and the Chemical Bond (John Wiley & Sons, 1963) [31] Y. Suzuki, G. Hu, R.B. van Dover, R.J. Cava, J. Magn.

Magn. Mater. 191, 1D8 (1999), Magnetic anisotropy of epitaxial cobalt ferrite thin films [32] A. Lisfi, C. M. Williams, L. T. Nguyen, J. C. Lodder, A. Coleman, H. Corcoran, A.Johnson, P. Chang, A. Kumar, and W. Morgan, Phys. Rev. B 76, 054405 (2007), Reorientation of magnetic anisotropy in epitaxial cobalt ferrite thin films [33] J. Inoue, H. Itoh, M. A. Tanaka, K.Mibu, T. Niizeki, H.

Yanagihara, and E. Kita, IEEE Trans. Magn. 49, 3269 (2013), Study of Perpendicular Magnetic Anisotropy and Magneto-Elastic Coupling in the First Principles and Phenomenology [34] Jun-ichiro Inoue, Hideto Yanagihara and Eiji Kita, Materials Research Express 1, 046106 (2014) , Magnetic anisotropy and magnetostriction in cobalt ferrite with lattice deformation [35] Jun-ichiro Inoue, Tomohiko Niizeki, Hideto Yanagihara, Hiroyoshi Itoh, and Eiji Kita, AIP Advances 4, 027111 (2014), Electron theory of perpendicular magnetic anisotropy of Co-ferrite thin films [36] M. A. Tanaka, K. Harada, M. Takemura, K. Mibu, and J. Inoue, J. Appl. Phys. 115, 17C101 (2014), Nonlinear strain dependence of magnetic anisotropy in CoFe2O4 films on MgO(001) substrates

[37] Takeshi Tainosho, Jun-ichiro Inoue, Sonia Sharmin, Masaki Takeguchi, Eiji Kita, and Hideto Yanagihara, Appl. Phys. Lett. 114, 092408 (2019), Large negative uniaxial magnetic anisotropy in highly distorted Coferrite thin films [38] Junichiro Inoue, Hiroshige Onoda and Hideto Yanagihara, J. Phys. D: Appl. Phys. 53, 195003 (2020), Uniaxial magnetic anisotropy of transition metal oxides: role of local lattice deformation [39] Aurelien Manchon and Abderrezak Belabbes, Solid State Phys. 68, 1 (2018). Spin-Orbitronics at Transition Metal Interfaces [40] J. Stöhr, J. Magn. Magn. Mater. 200, 470 (1999). Exploring the microscopic origin of magnetic anisotropies with X-ray magnetic circular dichroism (XMCD) spectroscopy [41] Frank de Groot and Akio Kotani, Core Level Spectroscopy of Solids, (CRC Press, Boca Raton, FL, 2008).

[42] Gerrit van der Laan, Elke Arenholz, Rajesh V.

Chopdekar and Yuri Suzuki, Phys. Rev. B 77, 064407 (2008), Influence of crystal field on anisotropic x-ray magnetic linear dichroism at the Co^{2+} L2,3 edges [43] J. A. Moyer, C. A. F. Vaz, E. Negusse, D. A. Arena, and V. E. Henrich, Phys. Rev. B 83, 035121 (2011), Controlling the electronic structure of Co1−xFe2+xO4 thin films through iron doping [44] J. A. Moyer, C. A. F. Vaz, D. A. Arena, D. Kumah, E.

Negusse, and V. E. Henrich. Phys. Rev. B 84, 054447 (2011), Magnetic structure of Fe-doped CoFe2 O4 probed by x-ray magnetic spectroscopies [45] Yuki K. Wakabayashi, Yosuke Nonaka, Yukiharu Takeda, Shoya Sakamoto, Keisuke Ikeda, Zhendong Chi, Goro Shibata, Arata Tanaka, Yuji Saitoh, Hiroshi Yamagami, Masaaki Tanaka, Atsushi Fujimori, and Ryosho Nakane, Phys. Rev. B 96, 104410 (2017), Electronic structure and magnetic properties of magnetically dead layers in epitaxial CoFe2O4/Al2O3/Si(111) films studied by x-ray magnetic circular dichroism [46] Jun Okabayashi, Yuki Iida, Qingyi Xiang , Hiroaki Sukegawa , and Seiji Mitani, Appl. Phys. Lett. 115, 252402 (2019), Perpendicular orbital and quadrupole anisotropies at Fe/MgO interfaces detected by x-ray magnetic circular and linear dichroisms [47] Jun Okabayashi, Yoshio Miura, Yohei Kota, Kazuya Z.

Suzuki, Akimasa Sakuma, and Shigemi Mizukami, Scientific Reports 10, 9744 (2020), Detecting quadrupole: a hidden source of magnetic anisotropy for Manganese alloys [48] Jun Okabayashi, Yoshio Miura and Tomoyasu Taniyama, npj Quantum Materials 4, 21 (2019), Strain-induced reversible manipulation of orbital magnetic moments in Ni/Cu multilayers on ferroelectric BaTiO3 [49] See Supplemental Material at [URL] for XRD, magnetization measurements, and wide-range XAS and XMCD spectra of CoxFe3−xO_{4+δ} (x =0.2 and 0.6).

[50] Shoma Yasui, Syuta Honda, Jun Okabayashi, Takashi Yanase, Toshihiro Shimada, and Taro Nagahama, Phys.Rev. Appl. 15, 034042 (2021), Large Inverse Tunnel Magnetoresistance in Magnetic Tunnel Junctions with an Fe3O4 Electrode [51] S. S. Dhesi, G. van der Laan and E. Dudzik, Appl. Phys.

Lett. 80, 1613 (2002), Determining element-specific magnetocrystalline anisotropies using x-ray magnetic linear dichroism [52] W. A. Harrison, Electronic Structure and the Properties of Solids (Dover, New York, 1989).

[53] Z. Szotek, W. M. Temmerman, D. Kodderitzsch, A.

Svane, L. Petit, and H. Winter, Phys. Rev. B 74, 174431 (2006), Electronic structures of normal and inverse spinel ferrites from first principles [54] Y.H. Hou, Y.J. Zhao, Z.W. Liu, H.Y. Yu, X.C. Zhong, W.Q. Qiu, D.C. Zeng, and L.S. Wen, J. Phys. D: Appl. Phys. 43, 445003 (2010), Structural, electronic and magnetic properties of partially inverse spinel CoFe2O4: a first-principles study [55] Debashish Das, Rajkumar Biswas and Subhradip Ghosh, J. Phys.: Condens. Matter 28, 446001 (2016) , Systematic analysis of structural and magnetic properties of spinel CoFe2O4 (B = Cr, Mn and Fe) compounds from their electronic structures [56] Sumayya M. Ansari, Vikas Kashid, Hemant Salunke, Debasis Sen, Yesh D. Kolekar, and C. V. Ramana, Phys. Rev. B 102, 035446 (2020), First-principles calculations of the electronic structure and magnetism of nanostructured CoFe2O4 microgranules and nanoparticles [57] Hebatalla Elnaggar, Maurits W. Haverkort, Mai Hussein Hamed, Sarnjeet S. Dhesi and Frank M. F. de Groot, J. Synchrotron Rad. 28, 247 (2021), Tensor description of X-ray magnetic dichroism at the Fe L2,3-edges of Fe3O4 [58] A.L. Ankudinov, B. Ravel, J.J. Rehr, and S.D. Conradson, Phys. Rev. B 58, 7565 (1998). Real Space Multiple Scattering Calculation of XANES [59] S.A. Chambers, R.F.C. Farrow, S. Maat, M.F. Toney, L.

Folks, J.G. Catalanoc T.P. Trainor, G.E. Brown Jr., J. Magn. Magn. Mater. 246, 124 (2002), Molecular beam epitaxial growth and properties of CoFe2 O4 on MgO(001) [60] Makoto Minagawa, Hideto Yanagihara, Kazuyuki Uwabo, Eiji Kita, and Ko Mibu, Jap. J. Appl. Phys. 49, 080216 (2010). Composition Shift as a Function of Thickness in Fe_{3−δ} O4 (001) Epitaxial Films [61] Jun Okabayashi, Shigeki Miyasaka, Kazuhiro Hemmi, Kiyohisa Tanaka, Setsuko Tajima, Hiroki Wadati, Arata Tanaka, Yasumasa Takagi, and Toshihiko Yokoyama, J. Phys. Soc. Jpn. 84, 104703 (2015). Investigating Orbital Magnetic Moments in Spinel-Type MnV2O4 Using X-ray Magnetic Circular Dichroism

[62] Jun Okabayashi, Shigeki Miyasaka, Masashi Takahashi, and Setsuko Tajima, Jpn. J. Appl. Phys. 57, 0902BD (2018). Local electronic and magnetic properties of ferroorbital-ordered FeV2O4 [63] Jun Okabayashi, Songtian Li, Seiji Sakai, Yasuhiro Kobayashi, Takaya Mitsui, Kiyohisa Tanaka, Yoshio Miura, and Seiji Mitani, Phys. Rev. B 103, 104435 (2021), Perpendicular magnetic anisotropy at the Fe/Au(111) interface studied by Mössbauer, x-ray absorption, and photoemission spectroscopies [64] Xuegang Chen, Xiaozhe Zhang, Myung-Geun Han, Le Zhang, Yimei Zhu, Xiaoshan Xu, and Xia Hong, Adv. Mater. 31, 1805260 (2019), Magnetotransport Anomaly in Room-Temperature Ferrimagnetic NiCo2 O4 Thin Films [65] Hiroki Koizumi, Ikumi Suzuki, Daisuke Kan, Jun-ichiro Inoue, Yusuke Wakabayashi, Yuichi Shimakawa, and Hideto Yanagihara, Phys. Rev. B 104, 014422 (2021), Spin reorientation in tetragonally distorted spinel oxide NiCo2 O4 epitaxial films [66] Daisuke Kan, Masaichiro Mizumaki, Miho Kitamura, Yoshinori Kotani, Yufan Shen, Ikumi Suzuki, Koji Horiba, and Yuichi Shimakawa, Phys. Rev. B 101, 224434 (2020), Spin and orbital magnetic moments in perpendicularly magnetized Ni1−xCo2+y O4−z epitaxial thin films: Effects of site-dependent cation valence states [67] Jun Okabayashi, Yoshio Miura, and Hiro Munekata, Sci.

Rep. 8, 8303 (2018). Anatomy of interfacial spin-orbit coupling in Co/Pd multilayers using X-ray magnetic circular dichroism and first-principles calculations

TABLE I. The Electronic structure parameters used in the LFM cluster calculation. The units of each value is in eV. Δ U (pdσ) 10Dq Fe^{2+} (O_h) 6.5 6.0 1.2 0.9 Fe^{3+} (O_h) 0.5 6.0 1.2 0.9 Fe^{3+} (T_d) 4.5 6.0 2.0 -0.5 Co^{2+} (O_h) 6.5 6.0 1.3 0.5

FIG. 1. XAS and XMCD of Co0.2 Fe2.8O_{4+δ} film. μ+ and μ− in XAS denote the magnetic field direction along the incident photon beams at normal incident geometry. Difference of μ^+ − μ^− is defined as XMCD spectra for (a) Fe L-edge and (b) Co L-edge. Both XAS and XMCD intensities are normalized by photon flux. (c) Magnetic-field dependence at each fixed photon energy; 708, 709, and 778 eV corresponding to Fe^{2+} (O_h), Fe^{3+} (T_d), and Co^{2+} (O_h) peaks, respectively.

FIG. 2. XAS and XMLD of Co0.2 Fe2.8O_{4+δ} film of (a) Fe and (b) Co L-edges. Spectra were taken at the grazing incident setup where E of the incident beam and direction of magnetization M were parallel (horizontal) and perpendicular (vertical), respectively. The inset displays an illustration of the XMLD measurement geometry.

FIG. 3. Calculated XMCD and XMLD spectra for (a,b) Fe and (c,d) Co L-edges. For Fe L-edge, three components of Fe^{2+} (O_h), Fe^{3+} (O_h), and Fe^{3+} (T_d) sites are also shown. Total spectra are shown in black solid line. Open dotted curves are experimental XMCD and XMLD shown in Figs. 1 and 2.

FIG. 4. XAFS and EXAFS of Co0.2Fe2.8O_{4+δ} (PMA) and Co0.6 Fe2.4O_{4+δ} (in-plane anisotropy). (a) Co K-edge XAFS. Inset shows corresponding k oscillation in k^3χ(k) for x = 0.2. Dot curve shows the fitting result. (b) EXAFS profile after the Fourier transform. Inset shows the fitting result in x = 0.2.