arXiv:2210.16007v1 [cs.IT] 28 Oct 2022

Design of Protograph LDPC-Coded MIMO-VLC Systems with Generalized Spatial Modulation

Lin Dai, Yi Fang, Member, IEEE, Yong Liang Guan, Senior Member, IEEE, Mohsen Guizani, Fellow, IEEE

Abstract

This paper investigates the bit-interleaved coded generalized spatial modulation (BICGSM) with iterative decoding (BICGSM-ID) for multiple-input multiple-output (MIMO) visible light communications (VLC). In the BICGSM-ID scheme, the information bits conveyed by the signal-domain (SiD) symbols and the spatial-domain (SpD) light emitting diode (LED)-index patterns are coded by a protograph low-density parity-check (P-LDPC) code. Specifically, we propose a signal-domain symbol expanding and re-allocating (SSER) method for constructing a type of novel generalized spatial modulation (GSM) constellations, referred to as SSERGSM constellations, so as to boost the performance of the BICGSM-ID MIMO-VLC systems. Moreover, by applying a modified PEXIT (MPEXIT) algorithm, we further design a family of rate-compatible P-LDPC codes, referred to as enhanced accumulate-repeat-accumulate (EARA) codes, which possess both excellent decoding thresholds and linear-minimum-distance-growth property. Both analysis and simulation results illustrate that the proposed SSERGSM constellations and P-LDPC codes can remarkably improve the convergence and decoding performance of MIMO-VLC systems. Therefore, the proposed P-LDPC-coded SSERGSM-mapped BICGSM-ID configuration is envisioned as a promising transmission solution to satisfy the high-throughput requirement of MIMO-VLC applications.

Index terms— Visible light communication, multiple-input multiple-output, protograph LDPC codes, generalized spatial modulation, bit-interleaved coded modulation.

L. Dai, and Y. Fang are with the School of Information Engineering, Guangdong University of Technology, Guangzhou 510006, China (email: bs0109dl@163.com; fangyi@gdut.edu.cn).

Y. L. Guan is with the School of Electrical and Electronic Engineering, Nanyang Technological University, Singapore (e-mail: eylguan@ntu.edu.sg).

M. Guizani is with the Machine Learning, Mohamed Bin Zayed University of Artificial Intelligence (MBZUAI), Abu Dhabi, UAE (e-mail: mguizani@ieee.org).

I. INTRODUCTION As a promising complementary solution to alleviate the shortage of wireless spectrum resources, optical wireless communication (OWC) is an attractive technology which has drawn a great deal of attention from both the academic and industrial communities [1]. Particularly, visible light communication (VLC) technology has been standardized in IEEE 802.15.7 [2], and hence could become a commercialized method for indoor communication scenarios due to the low infrastructure cost. VLC technology enjoys the characteristic that lighting and communication can coexist without causing interference for each other [3]. Moreover, advantages in the terms of energy efficiency, wide bandwidth, license-free application and higher security make VLC a promising solution to be part of the 5G wireless networks [4]. In indoor VLC systems, the light emitting diodes (LEDs) are the main medium used for data transmission by modulating the intensity of the emitted light because of their superior switching capabilities. However, the LEDs have quite low modulation bandwidth (i.e., about 20 MHz) [5], which greatly limits the transmission rate of the VLC systems. Meanwhile, the conventional transmission framework typically adopts single-input-single-output (SISO) technique, which cannot provide spatial diversity gain. To deal with this problem, some technologies such as multiple-input multiple-output (MIMO) [6], [7] have been applied to the VLC systems.

The conventional MIMO technology activates all LED emitters at every time slot and transmits the same information simultaneously, which results in the inter-channel interference (ICI). For averting ICI, a multiple-LED modulation scheme, called spatial modulation (SM), has been proposed in [8], [9]. However, SM would lead to low spectral efficiency (SE) because it does not efficiently utilize the transmitted resources. Therefore, some other schemes such as generalized spatial modulation (GSM) [10], quad-LED complex modulation (QCM) [11] and dual-LED complex modulation (DCM) [12] have been developed. As a spectral-efficient multiple-input multiple-output visible light communication (MIMO-VLC) transmission scheme, the conventional GSM (ConGSM) simultaneously activates multiple LEDs and every activated LED is allowed to carry the different unipolar pulse amplitude modulated (UPAM) intensity level during each transmission instant [10]. However, due to the channel correlation of the static MIMO-VLC channels under the line-of-sight (LOS) condition, the signal-domain (SiD) symbol design for the ConGSM is not the optimal. In [13], a new SiD symbol-design method for activate-space collaborative constellation GSM (ASCCGSM) has been proposed by minimizing the power of the SiD symbols to improve the error performance of MIMO- VLC system. Beyond that, it is well known that the coded modulation (CM) scheme [14]–[17] plays an important role in improving the overall system performance.

In [15], a trellis coded spatial modulation (TCSM) scheme was proposed, in which only SiD bits are protected by a trellis code to improve the performance over correlated channels. After that, the authors in [18] have extended the TCSM scheme to an enhanced coded SM (ECSM) scheme which jointly encodes the bits conveyed in the spatial-domain (SpD) and SiD so as to achieve a higher coding gain in the indoor OWC systems. Furthermore, it has been pointed out in [19] that a trellis coded GSM (TGCSM) scheme is spectrally efficient and robust against the correlated MIMO channels. Additionally, a bit-interleaved coded modulation (BICM) combined with SM has been proposed as a promising solution, which provides performance improvements against the channel correlation effect [16]. However, the BICM is not the optimal transmission scheme due to the independent demapping and decoding procedures. To compensate for the performance loss arising from separated demapping and decoding, iterative decoding (ID) is introduced at the receiver to enhance the BICM performance [20]. In this paper, we consider the transmission scheme for BICM combined with GSM and ID, referred to as BICGSM-ID. Nevertheless, there exist some challenges in the design of the bit-interleaved coded generalized spatial modulation with iterative decoding (BICGSM-ID) scheme for the MIMO-VLC systems.

In communication systems, error-correction codes (ECCs) play a critical role in improving the system performance. In [18], the convolutional codes have been applied in the ECSM-aided indoor OWC systems. The non-binary low-density parity-check (LDPC) codes and polar codes have been presented in coded spatial modulation (CSM) scheme in the SM-MIMO systems [21], [22]. As a class of capacity-approaching codes, protograph low-density parity-check (P-LDPC) codes [23] have been widely exploited in the wireless communication systems due to their noticeable performance and simple implementation. Especially, the accumulate-repeat-by-4-jagged-accumulate (AR4JA) code [24], which possesses simple protograph structures to realize linear encoding and decoding, can achieve very desirable error performance in both low and high signal-noise-ratio (SNR) regions over additive white Gaussian noise (AWGN) channels. However, the conventional P-LDPC codes may not perform well in specific BICM-ID VLC systems.

To facilitate the design and analysis of the P-LDPC-coded BICM systems, a variety of protographbased extrinsic information transfer (PEXIT) algorithms [25]–[28] have been developed to predict the system performance in the low SNR region. On the other hand, in [24], [29], the asymptotic weight distribution (AWD) has been formulated to estimate the typical minimum distance ratio (TMDR), i.e., the linear-minimum-distance growth property, of a P-LDPC code so as to predict the system performance in the high SNR region. Although the performance of the P-LDPC-coded BICM

Fig. 1. Block diagram of a P-LDPC-coded BICGSM-ID MIMO-VLC system.

systems has been intensively studied, there is still a lack of design methodology for P-LDPC-coded BICGSM-ID scheme, especially in the MIMO-VLC systems.

Driven by the aforementioned motivations, we investigate the performance of the P-LDPC-coded BICGSM-ID MIMO-VLC systems. The main contributions are in two-fold and can be summarized as follows. 1) A type of novel GSM constellations, referred to as symbol expanding and re-allocating GSM (SSERGSM) constellations, is proposed through an SSER method. Meanwhile, we utilize the constellation-constrained average mutual information (AMI) to evaluate the achievable capacity of the proposed SSERGSM constellations in the MIMO-VLC systems. 2) Based on the modified protograph extrinsic information transfer (MPEXIT) algorithm, we put forward a novel family of rate-compatible P-LDPC codes, called enhanced accumulate-repeat-accumulate (EARA) codes. The proposed EARA codes can not only benefit from desirable decoding thresholds, but also possess the linear-minimum-distance-growth property in the BICGSM-ID MIMO-VLC systems. Simulations are carried out to verify that the proposed P-LDPC-coded BICGSM-ID schemes with the SSERGSM constellations outperform the state-of-the-art counterparts in the MIMO-VLC systems.

The remainder of this paper is organized as follows. Section II introduces the P-LDPC-coded BICGSM-ID MIMO-VLC system model and presents the information-theoretic methodology to calculate the AMIs of the GSM constellations. This section also describes the proposed an MPEXIT algorithm for the PLDPC-coded BICGSM-ID MIMO-VLC system. Section III proposes the SSERGSM constellation design, in which a new SSER method is exploited to design the SiD symbols. Section IV constructs a new family of rate-compatible P-LDPC codes. Section V provides various simulated results and discussions. Finally, Section VI concludes the contributions of this paper.

Notations: Boldface lowercase and uppercase letters denote vectors and matrices, respectively. Let (·)^T, ⌊·⌋, ‖ · ‖ and ! denote the transpose operation, floor function, Frobenius norm and factorial operation, respectively. Besides, | · | represents the cardinality of a set.

II. SYSTEM MODEL AND PRELIMINARIES A. Conventional GSM

In a conventional GSM (ConGSM) [10], we assume N_t and N_a (i.e., N_a ≥ 2) are the numbers of transmit LEDs and active LEDs at each transmission instant, respectively. It is apparent that the number of all possible LED activation patterns is Δ = N_t!/(N_t −N_a)!N_a!. To ensure that the number of LED activation patterns is a power of two, 2^{ρd} effective LED activation patterns are selected for the M-ary unipolar PAM (M-UPAM) intensity level transmission, where ρ_d = ⌊log_2 Δ⌋. The M-UPAM intensity levels can be formulated as [10], [30]

I_t = (2I_at)/(M + 1), ∀t = 1, 2, · · · , M, (1)

where I_a is the average intensity level of each LED.

Consequently, there are two different types of constellations, i.e., spatial-domain (SpD) constellation and signal-domain (SiD) constellation, involved in GSM. The SpD constellation set Ω is dependent on the effective LED activation patterns (i.e., |Ω| = 2^{ρd} ) and the SiD constellation set Λ is dependent on the order M of UPAM and N_a (i.e., |Λ| = M · N_a). As a result, at each transmission instant, the number of coded bits can be written as

ρ = ρ_d + N_a · log_2 M. (2)

More details of the ConGSM can be referred to [10].

B. System Model

The block diagram of a P-LDPC-coded BICGSM-ID MIMO-VLC system is shown in Fig. 1, in which an indoor LOS MIMO-VLC link with N_t LEDs and N_r photodetectors (PDs) at the transmitter and receiver, respectively, are considered. In such a scenario, we assume that N_a (i.e., N_a ≥ 2) is the number of active LEDs at each transmission instant. In Fig. 1, the input information-bit stream c = (c_1, c_2, . . . , c_k) is first encoded to a length-n codeword u (i.e., coded-bit stream) by exploiting a P-LDPC code. Further, the code-bit stream u = (u_1, u_2, . . . , u_n) is permuted by a random interleaver. Subsequently, every ρ consecutive coded bits are processed by a GSM mapper. More specifically, the ρ consecutive coded bits are divided into two parts in a sequential order. The first part including ρ_d bits is used to select the effective LED activation patterns, while the second part contains ρ_s = N_a log_2 M bits, and every log_2 M component bits are independently mapped to an M-UPAM intensity level.

After the GSM mapper, every ρ (i.e., ρ = ρ_d +ρ_s) coded bits are carried by a GSM signal, and thus a length-(n/ρ) GSM symbol sequence v̂ = (v̂_1, v̂_2, · · · , v̂_k, · · · , v̂_{n/ρ}) can be yieled. Finally, each GSM symbol is converted into a transmission vector x = [x_1, x_2, · · · , x_{Nt} ]^T, which is propagated through a MIMO-VLC channel. The received signal can be given as

y = Hx + w, (3)

where y = [y_1, y_2, · · · , y_{Nr} ]^T is a vector with size of N_r × 1, and x = [x_1, x_2, · · · , x_{Nt} ]^T is the transmitted GSM signal vector. In particular, x consists of the N_t − N_a zero elements representing the inactive LEDs, and the N_a positive, real-valued elements choosing from the UPAM intensity symbol set. Moreover, w is the noise vector with size of N_r × 1, each of which can be modeled as the independent and identically distributed (i.i.d) additive white Gaussian noise (AWGN) with zero mean and variance σ^2 = N_0/2, where N_0 is the single sided noise power spectral density. H is the LOS channel gain matrix with size of N_r × N_t, and the entries of the H matrix can be determined by [18] h_{ij} = ε(η+1)A 2πd^2_{ij} cos

η(ϕ_{ij} ) cos(ψ_{ij} ), 0 ≤ ψ_{ij} ≤ Ψ_{1/2} 0, ψ_{ij} > Ψ_{1/2}, (4) where d_{ij} represents the distance between the j-th transmit LED and the i-th receive PD, i ∈ (1, 2, · · · , N_r) and j ∈ (1, 2, · · · , N_t). ϕ_{ij} and ψ_{ij} are the angle of irradiance and incidence from the jth transmit LED to the i-th receive PD, respectively. η = − ln 2/ ln(cos Φ_{1/2}) represents the Lambert’s mode number, where Φ_{1/2} is the transmit semi-angle of the LED. Also, ε, A and Ψ_{1/2} represent the PD responsivity, PD area and half-power field-of-view (FOV) angle of the PD, respectively. In this paper, the average optical signal-to-noise ratio (OSNR) is defined as follows [31], [32]

OSNR = P_{rx}/( √ 2Rρσ), (5) where R denotes the code rate and P_{rx} =^1_{Nr} ∑_{Nr} i=1 ∑_{Nt} j=1 h_{ij}I is the average received optical power, and I is the average optical intensity being emitted.

At the receiver, each received GSM symbol is processed by a serially concatenated ID framework, which includes a GSM demapper and a P-LDPC decoder. Specifically, given the k-th received symbol y_k and its corresponding bit sequence v̂_k = (v^k_1 , v^k_2 , · · · , v^k_{ρd} , · · · , v^k_ρ ), in which the first consecutive ρ_d bits are used for selecting effective LED activation patterns with the set Ω and the remaining ρ_s bits are mapped to the SiD constellation with the set Λ, we conveniently denote the SpD and SiD bit sequences as v̂_{d,k} = (v^k_{d,1}, v^k_{d,2}, · · · , v^k_{d,l}, · · · , v^k_{d,ρd} ) and v̂_{s,k} = (v^k_{s,1}, v^k_{s,2}, · · · , v^k_{s,q}, · · · , v^k_{s,ρs} ), respectively. Based on the k-th received symbol and its corresponding a-priori log-likelihood-ratios

(LLRs) L^a_{dem}, the corresponding a-posteriori LLRs L^p_{dem} output from the GSM demapper can be derived by [33] L^p_{dem}(v^k_{d,l}) =L^a_{dem}(v^k_{d,l}) + max_{x∈Λbq ,x∈Ω0l} [−‖y − Hx‖^2/2σ^2

+ Q_1] − max

x∈Λ^b_q ,x∈Ω^1_l

[−‖y − Hx‖^2/2σ^2 + Q_1], (6)

L^p_{dem}(v^k_{s,q}) =L^a_{dem}(v^k_{s,q}) + max_{x∈Ωbl ,x∈Λ0q} [−‖y − Hx‖^2/2σ^2

+ Q_2] − max

x∈Ω^b_l ,x∈Λ^1_q

[−‖y − Hx‖^2/2σ^2 + Q_2], (7)

where l = 1, 2, · · · , ρ_d, q = 1, 2, · · · , ρ_s, Q_1 = ∑_ρ τ =1,τ ≠l(1−v k τ )L^a_{dem}(v^k_τ ), and Q_2 = ∑_ρ τ =1,τ ≠ρ_d+q(1− v^k_τ )L^a_{dem}(v^k_τ ). Additionally, Ω^b_l is the subset of Ω with the l-th labeling bit having value b ∈ {0, 1} and Λ^b_q is the subset of Λ with the q-th labeling bit having value b ∈ {0, 1}. Hence, the extrinsic LLRs L^e_{dem} ( i.e., L^e_{dem} = L^p_{dem} − L^a_{dem} ) gleaned from the GSM demapper are deinterleaved and are viewed as the a-priori LLRs L^a_{dec} into the P-LDPC decoder. Through a decoding procedure, the extrinsic LLRs L^e_{dec} ( i.e., L^e_{dec} = L^p_{dec} − L^a_{dec} ) output from the P-LDPC decoder are re-interleaved and fed back as the updated a-priori LLRs L^a_{dem} for the next iteration. In such an iterative demapping and decoding framework, the extrinsic LLRs and a-priori LLRs are iteratively updated between the demapper and the decoder so as to improve the reliability of the a-posteriori LLRs and enhance the MIMO-VLC system performance.

C. Achievable Average Mutual Information

Here, we discuss the AMI for the BICGSM transmission scheme in the MIMO-VLC systems. For the BICGSM scheme, the transmitted GSM symbol vector x is determined jointly by the effective LED activation pattern d ∈ Ω and the SiD constellation symbol s ∈ Λ, in which each symbol s contains N_a UPAM intensity levels.

From the perspective of equivalent parallel channels, at each transmitted instant, the joint mapping for the ρ bits in the set Ω and Λ can be viewed as ρ parallel binary sub-channels which are independent and memoryless. Suppose that the receiver has ideal channel state information (CSI). The AMI can reflect the maximum information rate for error-free transmission, and thus the AMI can be used as a criterion for evaluating the channel transmission performance. We assume that d and s are the independent uniformly distributed random variables in the sets Ω and Λ, respectively. The spatialdomain AMI (SiD-AMI) and signal-domain AMI (SpD-AMI), denoted by I_{SpD} and I_{SiD} respectively, can be calculated as [34]

I_{SpD} =

ρ_d∑

i=1 I(v_{d,i}; y|H)

= ρ_d −

ρ_d∑

i=1 E_{vd,i ,y,H} [ log_2 ∑ d∈Λ,s∈Ω p(y|d, s, H) ∑ d∈Λ,s∈Ω^{vd,i}_i p(y|d, s, H) ] , (8)

I_{SiD} =

ρ_s∑

j=1 I(v_{s,j}; y|H)

= ρ_s −

ρ_s∑

j=1 E_{vs,j ,y,H} [ log_2 ∑ d∈Λ,s∈Ω p(y|d, s, H) ∑ s∈Ω,d∈Λ^{vs,j}_i p(y|d, s, H) ] , (9)

where v_{d,i} (i = 1, 2, · · · , ρ_d) and v_{s,j} (j = 1, 2, · · · , ρ_s) are the i-th SpD labeling bit and the j-th SiD labeling bit, respectively. Moreover, Ω^{vd,i}_i and Λ^{vs,j}_j are the subset of Ω with the i-th bit v_{d,i} (v_{d,i} ∈ {0, 1}) and the subset of Λ with the j-th bit v_{s,j} (v_{s,j} ∈ {0, 1}), respectively. Additionally, p(y|d, s, H) denotes the probability density function (PDF) of the receiver vector y conditioned on the effective LED activation pattern d ∈ Ω and the SiD constellation symbol s ∈ Λ. Therefore, the constrained AMI for a BICGSM scheme in the MIMO-VLC systems, called BICGSM-AMI is given by I_{BICGSM} = I_{SpD} + I_{SiD}. (10)

D. Modified PEXIT Algorithm

To the best of our knowledge, PEXIT algorithm can be used to track the evolution of the mutualinformation between the variable-node (VN) decoder and the check-node (CN) decoder [23]. Through such a manner, PEXIT algorithm is able to evaluate the decoding threshold of a P-LDPC code so as to reveal the error performance at low SNR region under an iterative decoder. By modifying the traditional PEXIT algorithm [35], one can evaluate the convergence performance of the P-LDPC-coded BICGSM-ID scheme in MIMO-VLC systems.

To facilitate the treatment of the modified PEXIT (MPEXIT) algorithm for the P-LDPC-coded BICGSM-ID scheme, we first introduce the concept of P-LDPC codes. A protograph can be seen as a Tanner graph [36] containing a few variable nodes, check nodes and edges. In the Tanner graph, each edge connects a variable node and a check node and the parallel edges are allowed. Assume that a protograph possesses n_v variable nodes and n_c check nodes, which can be represented by an n_c × n_v base matrix B = (b_{i,j} ), b_{i,j} is the number of edges connecting C_i with V_j. Furthermore, a

TABLE I MAPPING TABLE OF THE CONGSM CONSTELLATION WITH Nt = Nr = 4, Na = 2 AND ρ = 4 (I.E., M = 2).

Label

Effective LED SiD modulated Transmitted activation pattern symbol vector x 0000 (1, 2) (2I_a/3, 2I_a/3) [2I_a /3, 2I_a/3, 0, 0]^T 0001 (1, 2) (2I_a/3, 4I_a/3) [2I_a/3, 4I_a/3, 0, 0]^T 0011 (1, 2) (4I_a/3, 4I_a/3) [4I_a/3, 4I_a/3, 0, 0]^T 0010 (1, 2) (4I_a/3, 2I_a/3) [4I_a/3, 2I_a/3, 0, 0]^T 0100 (1, 3) (2I_a/3, 2I_a/3) [2I_a/3, 0, 2I_a/3, 0]^T 0101 (1, 3) (2I_a/3, 4I_a/3) [2I_a/3, 0, 4I_a/3, 0]^T 0111 (1, 3) (4I_a/3, 4I_a/3) [4I_a/3, 0, 4I_a/3, 0]^T 0110 (1, 3) (4I_a/3, 2I_a/3) [4I_a/3, 0, 2I_a/3, 0]^T 1000 (1, 4) (2I_a/3, 2I_a/3) [2I_a/3, 0, 0, 2I_a/3]^T 1001 (1, 4) (2I_a/3, 4I_a/3) [2I_a/3, 0, 0, 4I_a/3]^T 1011 (1, 4) (4I_a/3, 4I_a/3) [4I_a/3, 0, 0, 4I_a/3]^T 1010 (1, 4) (4I_a/3, 2I_a/3) [4I_a/3, 0, 0, 2I_a/3]^T 1100 (2, 3) (2I_a/3, 2I_a/3) [0, 2I_a/3, 2I_a/3, 0]^T 1101 (2, 3) (2I_a/3, 4I_a/3) [0, 2I_a/3, 4I_a/3, 0]^T 1111 (2, 3) (4I_a/3, 4I_a/3) [0, 4I_a/3, 4I_a/3, 0]^T 1110 (2, 3) (4I_a/3, 2I_a/3) [0, 4I_a/3, 2I_a/3, 0]^T

larger protograph graph corresponding to a P-LDPC code can be obtained from a given protograph (resp. base matrix) by a “copy-and-permute (lifting)” operation which is usually implemented by a modified progressive-edge-growth (PEG) algorithm [37].

In the BICGSM-ID MIMO-VLC system, Suppose that G_1 is the maximum number of inner iteration for the P-LDPC decoder while G_2 is the maximum number of outer iteration between the GSM demapper and the P-LDPC decoder. The MPEXIT algorithm is shown as follows. 1) Initialization: Given an OSNR, initialize the incoming a-priori MI from the i-th variable node to the j-th check node I_{av}(i, j) = 0.

2) Extrinsic MI calculation of GSM demapper: For the k-th channel output symbol v̂_k, and the corresponding the SpD bits v̂_{d,k} = (v^k_{d,1}, v^k_{d,2}, · · · , v^k_{d,i}, · · · , v^k_{d,ρd} ) and the SiD bits v̂_{s,k} = (v^k_{s,1}, v^k_{s,2}, · · · , v^k_{s,i}, · · · , v^k_{s,ρs} ), the extrinsic MI I^{α,k}_{e,dem} between v̂_{α,k} and L^p_{dem}(v^k_α) in the GSM demapper can be calculated by Monte-Carlo simulation, where L^p_{dem}(v^k_α) is expressed by equations (6) and (7), and α = {d, s}.

3) Channel MI calculation of variable nodes: The channel MI of the i-th variable node I_{ch}(i) is calculated by I_{ch}(i) = 1 n n/ρ∑ k=1 (I^{d,k}_{e,dem} · ρ_d + I^{s,k}_{e,dem} · ρ_s). (11)

Fig. 2. Design principle of the proposed SSERGSM constellation with Nt = Nr = 4, Na = 2 and ρ = 4 (i.e., M = 2).

Specially, I_{ch}(i) = 0 if the i-th variable node is punctured in a protograph. 4) Extrinsic MI update between variable nodes and check nodes: In the inner iteration process, the extrinsic MIs are iteratively updated between the variable nodes and the check nodes, where the detailed process is given in [35].

5) A-priori MI update for GSM demapper: Exploiting the a-priori MI passed from check nodes to variable nodes, a-priori MI I^a_{dem} for the GSM dmapper can be measured by

I^a_{dem}(j) = J ((_{nc}∑ i=1 b_{i,j} [J^{−1}(I^a_{vn}(i, j))]^2 )_{1/2}) , (12)

where I^a_{vn}(i, j) is the a-priori MI passed from the j-th check node to the i-th variable node, and J(.) function is derived in [27]. Then I^a_{dem} can be further used for the next outer iteration.

Through this way, we can get the lowest OSNR value for which all a-posteriori MIs of the variable nodes converges to 1 by repeating Steps 2) ∼ 5) with different OSNR values.

Remark 1: To ensure the accuracy of the evaluated result, the proposed MPEXIT algorithm assumes that a finite binary codeword including both 0 and 1 bits is transmitted when calculating the MI, while the traditional PEXIT algorithm assumes an infinite-length all-zero codeword to do so. In addition, the proposed MPEXIT algorithm considering the silent features of GSM and indoor MIMO-VLC channel has a different channel MI expression I_{ch}(i) from that in the traditional PEXIT algorithm.

III. DESIGN OF PROPOSED SSERGSM FOR BICGSM-ID MIMO-VLC SYSTEMS In the MIMO-VLC systems, SiD modulated symbols are the critical parameter for formulating the GSM constellation, which can be designed and optimized so as to boost the system performance.

In the ConGSM, the SiD bits are modulated using the M-UPAM intensity levels for all effective LED activation patterns. In other words, the intensity levels are selected from an M-UPAM symbol

TABLE II MAPPING TABLE OF THE PROPOSED SSERGSM CONSTELLATION WITH Nt = Nr = 4, Na = 2 AND ρ = 4 (I.E., M = 2).

Label

Effective LED SiD modulated Transmitted activation pattern symbol vector x 0000 (1, 2) (I_a/6, I_a/6) [I_a /6, I_a/6, 0, 0]^T 0001 (1, 2) (I_a/6, 7I_a/6) [I_a/6, 7I_a/6, 0, 0]^T 0011 (1, 2) (7I_a/6, 7I_a/6) [7I_a/6, 7I_a/6, 0, 0]^T 0010 (1, 2) (7I_a/6, I_a/6) [7I_a/6, I_a/6, 0, 0]^T 0100 (1, 3) (2I_a/6, 2I_a/6) [2I_a/6, 0, 2I_a/6, 0]^T 0101 (1, 3) (2I_a/6, 8I_a/6) [2I_a/6, 0, 8I_a/6, 0]^T 0111 (1, 3) (8I_a/6, 8I_a/6) [8I_a/6, 0, 8I_a/6, 0]^T 0110 (1, 3) (8I_a/6, 2I_a/6) [8I_a/6, 0, 2I_a/6, 0]^T 1000 (1, 4) (4I_a/6, 4I_a/6) [4I_a/6, 0, 0, 4I_a/6]^T 1001 (1, 4) (4I_a/6, 10I_a/6) [4I_a/6, 0, 0, 10I_a/6]^T 1011 (1, 4) (10I_a /6, 10I_a/6) [10I_a/6, 0, 0, 10I_a/6]^T 1010 (1, 4) (10I_a/6, 4I_a/6) [10I_a/6, 0, 0, 4I_a/6]^T 1100 (2, 3) (5I_a/6, 5I_a/6) [0, 5I_a/6, 5I_a/6, 0]^T 1101 (2, 3) (5I_a/6, 11I_a/6) [0, 5I_a/6, 11I_a/6, 0]^T 1111 (2, 3) (11I_a /6, 11I_a/6) [0, 11I_a/6, 11I_a/6, 0]^T 1110 (2, 3) (11I_a/6, 5I_a/6) [0, 11I_a/6, 5I_a/6, 0]^T

set S = {I_1, I_2, · · · , I_M }, the SpD bits allocated for all effective LED activation pattern share the same M-UPAM symbol set S. As a example, the mapping table of ConGSM constellation for a 4×4 MIMO-VLC system with N_a = 2 and ρ = 4 (i.e., M = 2) is shown in Table I, where we choose (1, 2), (1, 3), (1, 4) and (2, 3) as the effective LED activation patterns, and the numbers 1, 2, 3 and 4 respectively represent the 1-th, 2-nd, 3-rd and 4-th LED indices. Given a MIMO-VLC channel (i.e., a channel matrix H), the correlation property of each effective LED activation pattern can be measured by the corresponding normalized instantaneous channel correlation matrix (NICCM) [38]. The larger the value of elements in NICCM is, the stronger the correlation of the corresponding LED activation pattern possesses. Due to the correlation property of the effective LED activation patterns, the ConGSM with all effective LED activation patterns sharing the same M-UPAM symbol set S may make the extrinsic MIs output from the demapper unreliable, which degrades the system performance. Therefore, we put forward a signal-domain symbol expanding and re-allocating (SSER) method for constructing a type of novel GSM constellations to improve the performance of the BICGSM-ID MIMO-VLC system. The detailed SSER design method is described as follows. 1) Expanding the number of the UPAM symbols: Given an M-ary UPAM symbol set S = {I_1, I_2, · · · , I_M }, which must satisfy I_t ∈ (0, 2I_a], ∀t ∈ 1, 2, · · · , M, and the number of effective

LED activation patterns β = 2^{ρd} . First, we evenly divide the entire symbol space (0, 2I_a] into β symbol subspaces, i.e., (2I_aτ/β, 2I_a(τ + 1)/β], ∀τ ∈ 0, 1, · · · , β − 1. Subsequently, we choose M UPAM symbols from each symbol subspace, and define the selection principle as Ĩ_{n′+Mτ} = 2I^an^′ β(M + 1) + 2I_aτ β , ∀τ ∈ 0, 1, · · · , β − 1, (13) where n^′ = 1, 2, · · · , M. Therefore, the new UPAM symbol set S̃ = {Ĩ_1, Ĩ_2, · · · , Ĩ_{βM} } is generated. Taking the case of ρ = 4 (i.e., M = 2) as a example, and the detailed design principle are shown in Fig. 2. Referring to this figure, one can obtain 4 symbol subspaces, i.e., (0, I_a/2], (I_a/2, I_a], (I_a, 3I_a/2] and (3I_a/2, 2I_a]. Then, we choose 2 UPAM symbols from each symbol subspace to form the new UPAM symbol set S̃ = {I_a/6, 2I_a/6, 4I_a/6, 5I_a/6, 7I_a/6, 8I_a/6, 10I_a/6, 11I_a/6}. Through this way, it is possible for all effective LED activation patterns to possess different UPAM symbol subsets.

2) Re-allocating the UPAM symbols for β effective LED activation patterns: For the expanded βM UPAM modulation symbols obtained from the first-step design, we first rank the βM symbols in an ascending order of their corresponding intensity values. Then, we select M different UPAM modulation symbols at maximum equal-intensity interval for each effective LED activation patterns. For example, the effective LED activation patterns (1, 2), (1, 3), (1, 4) and (2, 3) possess the UPAM symbol subsets {I_a/6, 7I_a/6}, {2I_a/6, 8I_a/6}, {4I_a/6, 10I_a/6} and {5I_a/6, 11I_a/6}, respectively. Finally, the SiD bits in each effective LED activation pattern are mapped to the corresponding UPAM modulation symbols.

Based on the above two steps, one can construct the SSERGSM constellation according to a given modulation order M and the number of effective LED activation patterns β, which can significantly enhance the demapper reliability so as to ensure excellent BICGSM-ID performance. As an example, the mapping table of SSERGSM constellation for a 4 × 4 MIMO-VLC system with N_a = 2 and ρ = 4 (i.e., M = 2) is shown in Table II. To verify the superiority of the proposed SSERGSM constellation, the convergence performance of BICGSM-ID will be investigated in the forthcoming subsections.

A. Simulation Settings and BICGSM-AMI Analysis

1) Simulation Settings: Unless otherwise mentioned, we consider a 4 × 4 indoor LOS MIMO- VLC channel and assume that the geometric setup of the channel model is shown in Fig 3. In this figure, the LEDs and PDs are aligned in a quadratically 2 × 2 array which is located in the middle of a 5.0m × 5.0m × 3.0m room, thus the four LEDs and four PDs construct two squares of lengths

TABLE III PARAMETER SETTING FOR THE TRANSCEIVER OF AN INDOOR MIMO-VLC SYSTEM.

Room

Length, i.e., x 5m Width, i.e., y 5m Height, i.e., z 3m

Transmitter

Number of LEDs, i.e., N_t 4 Number of the activated LEDs, i.e., N_a 2 Height from the floor 3m LED semi-angle, i.e., Φ_{1/2} 8^o d_{tx} 0.3m, 0.5m, 0.7m

Receiver

Number of PDs, i.e., N_r 4 Height from the floor 0.75m PD responsivity, i.e., ε 0.434A/W PD area, i.e., A 7mm^2 FOV angle of PD, i.e., Ψ_{1/2} 55^o d_{rx} 0.1m

Fig. 3. Geometric setup of the channel model for a 4 × 4 indoor LOS MIMO-VLC system.

d_{tx} and d_{rx}, respectively. Moreover, the PDs are placed at the plane z = 0.75m (e.g., the height of a table). Besides, the parameters utilized for transceiver are summarized in Table III. Based on this model, we investigate different MIMO-VLC channel setups by varying the spacing between two neighboring LEDs (i.e., d_{tx}), while the other system parameters remain unchanged. In this paper, the setting about the values of d_{tx} is the same as those in [18], i.e., d_{tx} = 0.3m, 0.5m, and 0.7m. Note that three different values of d_{tx} represent three different channel matrices, and the smaller the value of d_{tx} is, the stronger the correlation of the corresponding channel is.

2) BICGSM-AMI Analysis: According to Sect. II-C, the achievable BICGSM-AMI (i.e., I_{BICGSM}), SpD-AMI (i.e., I_{SpD}) and SiD-AMI (i.e., I_{SiD}) for a given GSM constellation can be measured. Assuming that the numbers of coded bit at each transmitted instant are set as ρ = 4 (i.e., M = 2) and ρ = 6 (i.e., M = 4), the AMIs for the proposed SSERGSM, ConGSM [10], and ASCCGSM [13]

(a) (b) Fig. 4. IBICGSM, ISpD and ISiD for the proposed SSERGSM, ConGSM, and ASCCGSM over a MIMO-VLC channel with dtx = 0.5m, where the numbers of coded bits at each transmission instant are set as: (a) ρ = 4 (i.e., M = 2) and (b) ρ = 6 (i.e., M = 4).

over a MIMO-VLC channel with d_{tx} = 0.5m are depicted in Fig. 4(a) and Fig. 4(b), respectively. As observed from Fig. 4(a), the proposed SSERGSM exhibits a significantly larger I_{BICGSM} with respect to the ConGSM and ASCCGSM. Meanwhile, I_{SpD} and I_{SiD} of the proposed SSERGSM are larger than their corresponding counterparts. Therefore, it can be concluded that the BICGSM scheme with the proposed SSERGSM mapper can obtain better performance compared with ConGSM and ASCCGSM mappers. Similar phenomenon also occurs in the case of ρ = 6 (i.e., M = 4).

In order to show the influence of the spacing between two neighboring LEDs on the BICGSM capacity, we set three different values of d_{tx}, i.e., d_{tx} = 0.3m, 0.5m, 0.7m in the cases of ρ = 4 (i.e., M = 2) and ρ = 6 (i.e., M = 4). Then, the corresponding BICGSM capacities for the proposed SSERGSM are illustrated in Fig. 5. One can observe that the proposed SSERGSM has the largest BICGSM capacity when d_{tx} = 0.7m, while it can achieve the lowest BICGSM capacity when d_{tx} = 0.3m whether the case of ρ = 4 or ρ = 6. This indicates that the proposed SSERGSM with d_{tx} = 0.7m can achieve the best performance among the three different cases of d_{tx}.

B. Convergence-Performance Analysis

1) Decoding Thresholds: In order to further demonstrate the merit of the proposed SSERGSM in the BICGSM-ID MIMO-VLC systems, we conduct the convergence-performance analysis by means of the MPEXIT algorithm. Suppose that all information bits used in the above scenarios are encoded by the rate-1/2 AR4JA code [24]. Unless otherwise stated, the information block length is 3600 bits, and the maximum numbers of inner and outer iterations are assumed as G_1 = 20 and G_2 = 4, respectively. Furthermore, we consider three different values of d_{tx}, i.e., d_{tx} = 0.3m, 0.5m, 0.7m, in the BICGSM-ID MIMO-VLC systems, where the cases of ρ = 4 and ρ = 6 are involved.

Fig. 5. IBICGSM for the proposed SSERGSM over MIMO-VLC channels with dtx = 0.3m, dtx = 0.5m and dtx = 0.7m, where the cases of ρ = 4 (i.e., M = 2) and ρ = 6 (i.e., M = 4) are considered.

In Table IV, we analyze the decoding thresholds of rate-1/2 AR4JA code [24] in the BICGSM- ID MIMO-VLC systems with three different GSM constellations, i.e., the proposed SSERGSM, ConGSM [10] and ASCCGSM [13]. As can be seen from Table IV, in the case of ρ = 4, the P- LDPC-coded BICGSM-ID MIMO-VLC system with the proposed SSERGSM constellation achieves the smaller decoding threshold compared with other two GSM constellations, i.e., ConGSM [10] and ASCCGSM [13] constellations, when d_{tx} are respectively set to be 0.3m, 0.5m and 0.7m. Moreover, the decoding thresholds of the AR4JA-coded BICGSM-ID schemes with the three different GSM constellations are reduced as d_{tx} varies from 0.3m to 0.7m, which indicates that system performance is optimal when d_{tx} = 0.7m. Similar conclusions can be drawn from the case of ρ = 6. We have also analyzed the decoding thresholds for the proposed SSERGSM constellation in the AR4JA-coded BICMGSM systems without ID, and have found that the ID framework converges faster than the non-ID framework. Thus, the SSERGSM constellation can obtain better performance than other two GSM constellations in the P-LDPC-coded BICGSM-ID MIMO-VLC systems.

2) Extrinsic MI of GSM Demapper: To elaborate a little further, we analyze the extrinsic MIs output from the demappers corresponding to three different GSM constellations in the cases of ρ = 4 and ρ = 6 for the AR4JA-coded BICGSM-ID MIMO-VLC systems with d_{tx} = 0.5m, and show the results in Fig. 6. As observed, in the case of ρ = 4 (see Fig. 6(a)), when OSNR is varying from 4.05 dB to 4.75 dB, the proposed SSERGSM constellation obtains greater extrinsic MI compared with other two GSM constellations, implying that using the SSERGSM constellation can provide more reliable information for the demapper during the iterative process with respect to other two GSM constellations. It is well known that more reliable demapping information can accelerate the convergence of the P-LDPC-coded BICM-ID scheme. Similar conclusion can be found in Fig. 6(b)

TABLE IV DECODING THRESHOLDS (DB) OF THE AR4JA-CODED BICGSM-ID SCHEMES WITH THREE DIFFERENT GSM CONSTELLATIONS

OVER MIMO-VLC CHANNELS WITH THREE DIFFERENT VALUES OF dtx , WHERE THE CASES OF ρ = 4 AND ρ = 6 ARE CONSIDERED. THE MAXIMUM NUMBERS OF INNER AND OUTER ITERATIONS ARE ASSUMED AS G1 = 20 AND G2 = 4, RESPECTIVELY.

d_{tx} (m) ρ = 4 SSERGSM ConGSM [10] ASCCGSM [13]

0.3 5.731 9.225 8.623 0.5 4.746 6.846 6.472 0.7 3.804 5.322 5.215

d_{tx} (m) ρ = 6 SSERGSM ConGSM [10] ASCCGSM [13]

0.3 7.603 10.612 10.027 0.5 6.585 8.324 7.749 0.7 5.278 6.196 6.014

(a) (b) Fig. 6. Extrinsic MIs for the proposed SSERGSM, ConGSM and ASCCGSM in a P-LDPC-coded BICGSM-ID MIMO-VLC system with dtx = 0.5m, where the numbers of coded bits at each transmission instant are set as: (a) ρ = 4 (i.e., M = 2) and (b) ρ = 6 (i.e., M = 4).

with the case of ρ = 6. It can be easily observed that the extrinsic-MI analyses agree well with their corresponding decoding-threshold analyses. Therefore, given an OSNR range, the extrinsic MI of the GSM demapper can serve as a useful performance metric of a GSM constellation over the MIMO-VLC channels.

IV. DESIGN OF P-LDPC CODES FOR BICGSM-ID MIMO-VLC SYSTEMS In order to improve the error correction performance of the BICGSM-ID MIMO-VLC systems, a type of rate-compatible P-LDPC codes is designed in this section.

Fig. 7. Protograph structure of the proposed EARA P-LDPC code

A. Design of P-LDPC Codes

It is well known that the conventional AR4JA code [24] has excellent error performance over the AWGN channels because it enjoys two desirable properties, i.e., low decoding threshold and linear minimum distance growth (the minimum Hamming distance growing linearly with the codeword length) [39]. The base matrix corresponding to a rate-(e + 1)/(e + 2) AR4JA code is given by

B_{AR4JA} =

1 2 0 0 0 0 3 1 1 1 0 1 2 2 1

2e 0 0 · · · 0 0 1 3 · · · 1 3 3 1 · · · 3 1

, (14)

where e is the number of extension patterns (i.e., e = 0, 1, 2, · · · ), the matrix size is 3 × (2e + 5), and the degree-6 variable node (i.e., the second column of B) is punctured.

Typically, the performance of P-LDPC codes depends on not only the structure of codes, but also the type of channel. The conventional P-LDPC codes, such as AR4JA code, that performs well over AWGN channels are not suitable for the usage in the BICGSM-ID MIMO-VLC systems. Besides, by using the PEXIT analysis, we found that the P-LDPC codes with the lowest-degree variable node punctured can achieve better convergence performance with respect to the counterparts with other puncturing rules in the BICGSM-ID MIMO-VLC systems. Therefore, we aim to design a type of rate-compatible P-LDPC code with puncturing the lowest degree variable node.

Considering a given codeword length, the lifting factor (i.e., “copy-and-permuting” times) for P- LDPC code will becomes smaller if the protograph size increases, which makes it more difficult to avoid error floor. Furthermore, the larger the protograph is, the more complex the corresponding optimization algorithm will be. Therefore, we first consider a rate-1/2 mother base matrix with the same size as that of the conventional AR4JA code, which includes a punctured variable node. To facilitate the code design, we impose some constraints on the rate-1/2 P-LDPC code in order to guarantee that its mother base matrix possesses the linear-minimum-distance-growth property and a relatively low decoding threshold, as follows.

1) Initialize a protograph with a degree-1 variable node being the punctured variable node, which corresponds to the second column in the mother base matrix.

2) Impose empirical constraints for the linear-minimum-distance-growth property on the base matrix, i.e., only one degree-2 variable node is allowed in the mother base matrix.

3) Set the maximum number of parallel edge to be 3 in the mother base matrix so as to maintain the low encoding and decoding complexity. This is because the encoding and decoding complexity of a P-LDPC code can be reflected by the number of edges in its corresponding protograph. Besides, for a fixed codeword length, if the number of parallel edges increases, the likelihood of short cycles will increase.

Based on the above rules, the mother base-matrix structure of the proposed rate-1/2 P-LDPC code can be formulated as

B_{1/2} = b_{1,1} 1 b_{1,3} b_{1,4} 0 b_{2,1} 0 b_{2,3} b_{2,4} 1 b_{3,1} 0 b_{3,3} b_{3,4} 1

. (15)

To assign the first column in the mother base matrix B_{1/2} as the largest degree variable node, we add an additional constraint, i.e., b_{1,1}+b_{2,1}+b_{3,1} > b_{1,3}+b_{2,3}+b_{3,3} and b_{1,1}+b_{2,1}+b_{3,1} > b_{1,4}+b_{2,4}+b_{3,4}. After a exhaustive search using the proposed MPEXIT algorithm, one can obtain the optimal mother base matrix with lowest decoding threshold and linear-minimum-distance-growth property, as

B_{1/2} =

1 1 1 0 0 3 0 2 1 1 1 0 1 2 1

. (16)

However, for higher-rate P-LDPC code design, the search space becomes larger, hence the corresponding exhaustive-search method is more complex. Therefore, we resort to a pattern-extension method, which is similar to the construction of the AR4JA codes, to design the higher-rate P- LDPC code. In particular, the pattern-extension method can be realized by repeatedly adding two variable nodes into the resultant mother protograph (i.e., base matrix). It has been demonstrated in

[24], [29] that adding degree-3 variable node into a rate- 1/2 protograph can maintain the lowestcomplexity feature for its corresponding higher-rate counterparts without deteriorating the linearminimum-distance-growth property.

For the above reason, a type of enhanced rate-compatible P-LDPC codes with the code rate R = (e + 1)/(e + 2) (e = 0, 1, 2, · · · ), referred to EARA codes, is obtained. The protograph structure of the proposed EARA code is illustrated in Fig. 7, where the dark circles denote transmitted variable nodes, the white circle denotes the punctured variable node, and the plus circle are check nodes. As a result, the corresponding base matrix is given as

B_{EARA} =

1 1 1 0 0 3 0 2 1 1 1 0 1 2 1

2e 0 0 · · · 0 0 2 1 · · · 2 1 1 2 · · · 1 2

. (17)

B. Asymptotic Performance Metrics

1) Decoding-Threshold Analysis: To verify the convergence performance of the proposed EARA P-LDPC code, we take the rate-2/3 AR4JA code [24], accumulate-repeat-by-4-accumulate (AR4A) code [40], improved-AR4JA (IAR4JA) code, improved-AR4A (IAR4A) code and regular-(3, 9) code [24] as benchmarks in the proposed SSERGSM-aided BICGSM-ID MIMO-VLC systems with d_{tx} = 0.3m, and show their corresponding decoding thresholds in Table V. It is noted that the IAR4JA code and IAR4A code respectively represent two modified P-LDPC codes possessing the same base matrix as the AR4JA code and the AR4A code, but only with puncturing the lowest degree variable nodes. As shown, the proposed EARA P-LDPC code possesses the lowest decoding threshold among the six types of P-LDPC codes in the cases of ρ = 4 and ρ = 6. This implies that the proposed EARA P-LDPC code can achieve better error performance in low-OSNR region compared with its counterparts in the proposed SSERGSM-aided BICGSM-ID MIMO-VLC systems with d_{tx} = 0.3m.

2) AWD Analysis: By exploiting AWD function [24], [29], we measure the TMDRs for rate-2/3 P-LDPC codes, i.e., the proposed EARA code, AR4JA code, AR4A code, IAR4JA code, IAR4A code and regular-(3, 9) code and give the corresponding results in Table VI. Referring to this table, except that the AR4A code and IAR4A code, the other four types of P-LDPC codes possess effective TMDR values (i.e., positive TMDR values).

Based on the above decoding-threshold and AWD analyses, it is affirmed that the proposed EARA code not only possesses the lowest threshold but also exhibits a linear-minimum-distance property. This demonstrates that the proposed EARA code achieves better convergence performance compared

TABLE V DECODING THRESHOLDS OF P-LDPC CODES, I.E., THE PROPOSED EARA CODE, AR4JA CODE, AR4A CODE, IAR4JA CODE, IAR4A CODE AND REGULAR-(3, 9) CODE, IN THE PROPOSED SSERGSM-AIDED BICGSM-ID MIMO-VLC SYSTEMS WITH dtx = 0.3m, WHERE ρ = 4 AND ρ = 6 ARE CONSIDERED. THE MAXIMUM NUMBERS OF INNER AND OUTER ITERATIONS ARE

ASSUMED AS G1 = 20 AND G2 = 4, RESPECTIVELY.

ρ = 4 EARA AR4JA AR4A IAR4JA IAR4A Regular OSNR(dB) 5.314 7.226 7.145 6.214 6.157 6.012 ρ = 6 EARA AR4JA AR4A IAR4JA IAR4A Regular OSNR(dB) 7.108 8.625 8.512 8.028 7.964 7.813

TABLE VI TMDRS OF RATE-2/3 P-LDPC CODES, I.E., THE PROPOSED EARA CODE, AR4JA CODE, AR4A CODE, IAR4JA CODE, IAR4A

CODE AND THE REGULAR-(3, 9) CODE, IN THE BICGSM-ID MIMO-VLC SYSTEMS.

Code Type EARA AR4JA AR4A IAR4JA IAR4A Regular TMDR 0.004 0.009 N.A 0.008 N.A 0.006

with its counterparts in the low-OSNR region and provides a desirable error performance in the high- OSNR region in the proposed SSERGSM-aided BICGSM-ID MIMO-VLC systems.

Remark 2: We have also evaluated the six types of P-LDPC codes with other code rates (e.g., R = 1/2, 3/4) and have observed that the EARA codes also obtain the lowest decoding threshold and have effective TMDR values.

C. Complexity Analysis

In this subsection, we analyze the computational complexity of the P-LDPC codes for successful decoding under the serially concatenated ID framework. In this ID framework, GSM demapper and P-LDPC decoder impose the main computational complexity. Therefore, based on the log-domain maximum a-posteriori probability (Log-Map) demapping algorithm [33] and the LLR-based belief propagation (LLR-BP) decoding algorithm [41], we evaluate the numbers of real addition (RA) and real multiplication (RM) operations of a P-LDPC code for successful decoding under the ID framework. The results are shown in Table VII, where n and m are the number of VNs and CNs, respectively; p is the number of punctured VNs; ḡ_v and ḡ_c denote the average degrees of VNs and CNs, respectively; T̄_1 and T̄_2 denote the average numbers of inner and outer iterations. As a further investigation, Table VIII presents the average numbers of RA and RM operations of different P- LDPC codes for successful decoding in the SSERGSM-aided BIGSM-ID MIMO-VLC systems with

TABLE VII AVERAGE NUMBER OF OPERATIONS OF A P-LDPC CODE FOR SUCCESSFUL DECODING UNDER THE ID FRAMEWORK.

Component

Operation RA RM

Log-Map demapping (n − p)[2^ρ((Nt + 1)Nr + 2ρ − 4) + 2]T̄2 2^ρ(n − p)[(Nt + 1)Nr + ρ + 2]T̄2 LLR-BP decoding m(ḡv − 1)T̄1 2nḡcT̄1

d_{tx} = 0.3m and ρ = 4. As can be seen from this table, the proposed EARA P-LDPC code possesses a lower computational complexity compared with its counterparts under the ID framework.

V. SIMULATION RESULTS To validate our proposed SSERGSM constellation and constructed EARA P-LDPC code, we present various simulation results on the BICGSM-ID MIMO-VLC systems in this section. To be specific, a 4×4 indoor LOS MIMO-VLC channel model is considered. Furthermore, we assume that the information block length of P-LDPC codes is 3600 bits. In addition, unless otherwise stated, the maximum numbers of inner iterations and outer iterations are G_1 = 20 and G_2 = 4, respectively.

A. BER Performance of Proposed SSERGSM Constellation

Fig. 8 depicts the bit-error-rate (BER) curves of rate-1/2 the AR4JA-coded BICGSM-ID schemes with three different types of GSM constellations, i.e., the proposed SSERGSM constellations, Con- GSM [10], and ASCCGSM [13] over a MIMO-VLC channel with d_{tx} = 0.5m, where the maximum numbers of outer iterations are set as G_2 = 0, 2, 4. For the case of ρ = 4 (i.e., M = 2), as observed from Fig. 8(a), the proposed SSERGSM constellation can achieve better error performance compared with the two counterparts in the BICGSM-ID MIMO-VLC systems. To be specific, when G_2 = 4, the proposed SSERGSM constellation exhibits remarkable gains of about 1.9 dB and 2.4 dB over the ASCCGSM and the ConGSM constellations, respectively, at a BER of 7 × 10^{−6}. Furthermore, when G_2 = 0 (i.e., BICGSM system), it is evident that the proposed SSERGSM constellation can also obtain larger gains compared with its counterparts, indicating that the proposed SSERGSM constellation is suitable for not only ID scenario but also non-ID scenario. Additionally, it can be easily observed that, at a BER 5 × 10^{−6}, the proposed SSERGSM constellation with G_2 = 4 obtains about 0.3-dB gain over that with G_2 = 2, while the latter obtains about 0.56-dB gain over that with G_2 = 0. Similar observations can be also found in the case of ρ = 6 (i.e., M = 4) (see Fig. 8(b)). Based on the above discussions, the proposed SSERGSM constellation will become better as the

(a)

(b) Fig. 8. BER curves of the AR4JA-coded BICGSM-ID schemes with the proposed SSERGSM, ASCCGSM, and ConGSM constellations over a MIMO-VLC channel with dtx = 0.5m, where (a) ρ = 4 (i.e., M = 2) and (b) ρ = 6 (i.e., M = 4) are considered. The maximum numbers of outer iterations are set as G2 = 0, 2, 4.

maximum number of out iterations (i.e., the value of G_2) increases, while the relative performance between the proposed SSERGSM constellation and the benchmarks remains the same.

As a further investigation, we perform the BER performance for three different types of GSM constellations, i.e., the proposed SSERGSM constellations, ConGSM [10], ASCCGSM [13] in the AR4JA-coded BICGSM-ID MIMO-VLC systems with three different values of d_{tx} (i.e., d_{tx} = 0.3m, 0.5m, and 0.7m) in Fig. 9. Referring to Fig. 9(a) corresponding to the case of ρ = 4 (i.e., M = 2), at a BER of 7 × 10^{−6}, the proposed SSERGSM constellation only requires about a 4.8- dB OSNR when d_{tx} = 0.7m, while it needs about 5.68-dB and 6.88-dB OSNR when d_{tx} = 0.5m

TABLE VIII AVERAGE NUMBERS OF RA AND RM OPERATIONS OF DIFFERENT P-LDPC CODES FOR SUCCESSFUL DECODING UNDER THE ID

FRAMEWORK.

Code Type

Operation RA RM

EARA 2.642 × 10^6 6.602 × 10^6 AR4JA 8.853 × 10^6 2.205 × 10^7 AR4A 8.762 × 10^6 2.173 × 10^7 IAR4JA 4.565 × 10^6 1.123 × 10^7 IAR4A 4.241 × 10^6 1.025 × 10^7 Regular 2.819 × 10^6 7.789 × 10^6

and 0.3m, respectively. We also observe that, aiming to achieve a BER of 7 × 10^{−6}, the proposed SSERGSM constellation benefits from performance gains of about 3 dB and 3.64 dB compared with the ASCCGSM and ConGSM constellations when d_{tx} = 0.3m. When d_{tx} = 0.5m, the proposed SSERGSM constellation also significantly outperforms the ASCCGSM and ConGSM constellations about 1.9-dB and 2.4-dB gains, respectively. When d_{tx} = 0.7m, this performance gains of the proposed SSERGSM constellation with respect to the ASCCGSM and ConGSM constellations are only about 0.45 dB and 0.6 dB, respectively. Likewise, one can observe from Fig. 9(b) that the relative performance among the three different types of GSM constellations in the case of ρ = 6 (i.e., M = 4) is identical to that in the case of ρ = 4 (i.e., M = 2). These phenomenons suggest that the P-LDPC-coded BICGSM-ID MIMO-VLC system performance is continuously improved as d_{tx} increases from 0.3m to 0.7m, while the relative performance-gain between the proposed SSERGSM constellation and the benchmarks becomes smaller simultaneously. The reason is the fact that the parameter d_{tx} plays an important role in affecting the correlation of the MIMO-VLC channel. Specifically, a smaller d_{tx} produces a higher correlated MIMO-VLC channel. It manifests that the proposed SSERGSM constellation has greater advantage in the highly-correlated MIMO- VLC channels.

B. BER/FER Performance of Proposed EARA P-LDPC Code

Here, we carry out some BER/frame-error-rate (FER) performance simulations on the rate-2/3 proposed EARA code, the AR4JA code [24], AR4A code [40], IAR4JA code, IAR4A code and the regular-(3, 9) code [24] in the SSERGSM-aided BICGSM-ID MIMO-VLC systems with d_{tx} = 0.3m, where the cases of ρ = 4 (i.e., M = 2) and ρ = 6 (i.e., M = 6) are considered. The results are

(a)

(b) Fig. 9. BER curves of the AR4JA-coded BICGSM-ID schemes with the proposed SSERGSM, ASCCGSM, and ConGSM constellations over MIMO-VLC channels with (a) ρ = 4 (i.e., M = 2) and (b) ρ = 6 (i.e., M = 4). The spacings between two neighboring LEDs of are set as dtx = 0.3m, 0.5m, and 0.7m.

illustrated in Fig. 10. According to Fig. 10(a), at a BER of 7 × 10^{−6}, the proposed EARA P-LDPC code outperforms the IAR4A code and the IAR4JA code by about 0.67 dB and 0.78 dB, respectively. Moreover, the proposed EARA P-LDPC code achieves more than 0.4-dB gain over the regular-(3, 9) code, while the regular-(3, 9) code further respectively performs better than the AR4A code and the AR4JA code by about 1.15 dB and 1.69 dB in the case of ρ = 4 (i.e., M = 2). Referring to Fig. 10(b) for the case of ρ = 6 (i.e., M = 4), at OSNR = 9.0 dB, the proposed EARA P-LDPC code can achieve a BER of 6 × 10^{−6}, while the AR4JA code, AR4A code, IAR4JA code, IAR4A code and the regular-(3, 9) code accomplish BERs of 7.4 × 10^{−2}, 5.2 × 10^{−2}, 5.8 × 10^{−3}, 4.1 × 10^{−3}

(a)

(b) Fig. 10. BER/FER curves of six types of P-LDPC codes in the SSERGSM-aided BICGSM-ID MIMO-VLC systems with dtx = 0.3m, where (a) ρ = 4 (i.e., M = 2) and (b) ρ = 6 (i.e., M = 4) are considered.

and 3.7×10^{−4}, respectively. Importantly, there is no error-floor phenomenon for the proposed EARA P-LDPC code when the BER reduces to 10^{−6}. Based on the above observations, the proposed EARA P-LDPC code exhibits the best performance among the six types of P-LDPC codes.

Remark 3: We have also carried out simulations with other system setups (e.g., different values of N_t, N_r, N_a, G_1, G_2 and ρ), and have found that the relative performance between the proposed SSERGSM constellation and the benchmarks remains the same, which verifies the robustness of our proposed design.

VI. CONCLUSION In this paper, we presented a new BICGSM-ID transmission scheme over the MIMO-VLC channels. The design and optimization of GSM constellations and P-LDPC codes for use in the BICGSM- ID have been carefully investigated. To be specific, we modified the PEXIT algorithm according to the characteristics of GSM and MIMO-VLC channel. Next, we put forward an SSER design method to formulate a type of SSERGSM constellations tailored for the P-LDPC-coded BICGSM-ID MIMO- VLC systems, which exhibits better performance than other GSM constellations in this scenario. By exploiting the MPEXIT algorithm, we also constructed a family of EARA P-LDPC codes, which possess lower decoding thresholds than other P-LDPC codes and desirable linear-minimum-distance-growth property in the SSERGSM-aided BICGSM-ID MIMO-VLC systems. Simulation results validated that the joint deployment of SSERGSM constellations and EARA P-LDPC codes allow the BICGSM-ID MIMO-VLC systems to achieve very desirable error performance. In addition, we analyzed the effect of the correlation of MIMO-VLC channel on the system performance. Owing to these advantages, the proposed P-LDPC-coded BICGSM-ID is expected to promise a good solution for high-throughput MIMO-VLC applications.

REFERENCES

[1] M. Z. Chowdhury, M. K. Hasan, M. Shahjalal, M. T.Hossan, and Y. M. Jang, “Optical wireless hybrid networks: Trends, opportunities, challenges, and research directions,” IEEE Commun. Surveys Tuts., vol. 22, no. 2, pp. 930–966, 2nd Quart. 2020.

[2] IEEE Standard for Local and Metropolitan Area Networks-Part 15.7: Short-Range Wireless Optical Communication Using Visible Light, IEEE Standard 802.15.7-2011, Sep. 2011.

[3] T. Koonen, “Indoor optical wireless systems: Technology, trends, and applications,” J. Lightw. Technol., vol. 36, no. 8, pp.

1459–1467, Apr. 2018.

[4] H. Yang, W.-D. Zhong, C. Chen, and A. Alphones, “Integration of visible light communication and positioning within 5G networks for Internet of Things,” IEEE Netw., vol. 34, no. 5, pp. 134–140, Sep./Oct. 2020.

[5] F. Zafar, M. Bakaul, and R. Parthiban, “Laser-diode-based visible light communication: Toward gigabit class communication,” IEEE Commun. Mag., vol. 55, no. 2, pp. 144–151, Feb. 2017.

[6] C. Chen, W. Zhong, and D. Wu, “On the coverage of multiple-input multiple-output visible light communications,” IEEE Trans.

Green Commun. Netw., vol. 9, no. 9, pp. D31–D41, Sep. 2017.

[7] C. Chen, W. Zhong, H. Yang, and P. Du, “On the performance of MIMO-NOMA-based visible light communication systems,” IEEE Photon. Technol. Lett., vol. 30, no. 4, pp. 307–310, Feb. 2018.

[8] R. Mesleh, H. Elgala, and H. Haas, “Optical spatial modulation,” IEEE/OSAJ. Opt. Commun. Netw., vol. 3, no. 3, pp. 234–244, Mar. 2011.

[9] L. Wu, J. Cheng, Z. Zhang, J. Dang, and H. Liu, “Low-complexity spatial modulation for IM/DD optical wireless communications,” IEEE Photon. Technol. Lett., vol. 31, no. 6, pp. 475–478, Mar. 2019.

[10] S. P. Alaka, T. L. Narasimhan, and A. Chockalingam, “Generalized spatial modulation in indoor wireless visible light communication,” in Proc. IEEE Global Commun. Conf. (GLOBECOM), San Diego, CA, USA, Dec. 2015, pp. 1–7.

[11] R. Tejaswi, T. L. Narasimhan, and A. Chockalingam, “Quad-LED complex modulation (QCM) for visible light wireless communication,” in Proc. IEEE WCNC Wkshps, Doha, Qatar, Apr. 2016, pp. 18–23.

[12] Y. Celik, “On the performance of dual-LED complex modulation for VLC,” in Proc. IEEE 11th Int. Conf. Electrical and Electronics Engineering (ICEEE), Nov. 2019, pp. 707–711.

[13] C. R. Kumar and R. K. Jeyachitra, “Power efficient generalized spatial modulation MIMO for indoor visible light communications,” IEEE Photon. Technol. Lett., vol. 29, no. 11, pp. 921–924, Jun. 2017.

[14] U. Wachsmann, R. F. H. Fischer, and J. B. Huber, “Multilevel codes: Theoretical concepts and practical design rules,” IEEE Trans. Inf. Theory, vol. 45, no. 5, pp. 1361–1391, Jul. 1999.

[15] R. Mesleh, M. D. Renzo, H. Haas, and P. M. Grant, “Trellis coded spatial modulation,” IEEE Trans. Wireless Commun. Lett., vol. 9, no. 7, pp. 2349–2361, Jul. 2010.

[16] M. Koca and H. Sari, “Bit-interleaved coded spatial modulation,” in Proc. IEEE 23rd Int. Symp. Pers. Indoor Mobile Radio Commun. (PIMRC), Sydney, NSW, Australia, Sep. 2012, pp. 1949–1954.

[17] Y. Liao, M. Qiu, and J. Yuan, “Design and analysis of delayed bit-interleaved coded modulation with LDPC codes,” IEEE Trans.

Commun., vol. 69, no. 6, pp. 3556–3571, Jun. 2021.

[18] T. Fath, J. Klaue, and H. Haas, “Coded spatial modulation applied to optical wireless communications in indoor environments,” in Proc. IEEE Wireless Commun. Netw. Conf. (WCNC), Shanghai, China, Apr. 2012, pp. 1000–1004.

[19] Y. Zhou, D. Yuan, X. Zhou, and H. Zhang, “Trellis coded generalized spatial modulation,” in Proc. IEEE 79th Veh. Technol.

Conf. (VTC Spring), May. 2014, pp. 1–5.

[20] Z. Yang, Y. Fang, G. Zhang, F. C. M. Lau, S. Mumtaz, and D. B. da Costa, “Analysis and optimization of tail-biting spatially coupled protograph LDPC codes for BICM-ID systems,” IEEE Trans. Veh. Technol., vol. 69, no. 1, pp. 390–404, Jan. 2020.

[21] D. Feng, H. Xu, J. Zheng, and B. Bai, “Nonbinary LDPC-coded spatial modulation,” IEEE Trans. Wireless Commun., vol. 17, no. 4, pp. 2786–2799, Apr. 2018.

[22] J. Dai, K. Niu, Z. Si, and D. Zhang, “Polar-coded spatial modulation,” IEEE Trans. Signal Process., vol. 69, pp. 2203–2217, 2021.

[23] Y. Fang, G. Han, G. Cai, F. C. M. Lau, et al., “Design guidelines of low-density parity-check codes for magnetic recording systems,” IEEE Commun. Surveys Tuts., vol. 20, no. 2, pp. 1574–1606, 4th Quart. 2018.

[24] D. Divsalar, S. Dolinar, C. R. Jones, and K. Andrews, “Capaccity-approaching protograph codes,” IEEE J. Sel. Areas Commun., vol. 27, no. 6, pp. 876–888, Aug. 2009.

[25] T. V. Nguyen, A. Nosratinia, and D. Divsalar, “Threshold of protograph-based LDPC coded BICM for Rayleigh fading,” in Proc. IEEE Global Telecommun. Conf. (GLOBECOM), Dec. 2011, pp. 1–5.

[26] P. Chen, C. Kui, L. Kong, Z. Chen, and M. Zhang, “Non-binary protograph-based LDPC codes for 2-D ISI magnetic recording channels,” IEEE Trans. Trans. Magn., vol. 53, no. 11, pp. 1–5, Nov. 2017.

[27] Y. Fang, G. Zhang, G. Cai, F. C. M. Lau, P. Chen, and G.Han, “Root-protograph-based BICM-ID: A reliable and efficient transmission solution for block-fading channels,” IEEE Trans. Commun., vol. 67, no. 9, pp. 5921–5939, Sep. 2019.

[28] Y. Bu, Y. Fang, G. Han, S. Mumtaz, and M. Guizani, “Design of protograph-LDPC-based BICM-ID for multi-level-cell (MLC) NAND flash memory,” IEEE Commun. Lett., vol. 23, no. 7, pp. 1127–1131, Jul. 2019.

[29] Y. Fang, G. Bi, Y. L. Guan, and F. C. M. Lau, “A survey on protograph LDPC codes and their application,” IEEE Commun.

Surveys Tuts., vol. 17, no. 4, pp. 1989–2016, 4th Quart. 2015.

[30] A. K. Gupta and A. Chockalingam, “Performance of MIMO modulation schemes with imaging receivers in visible light communication,” J. Lightw. Technol., vol. 36, no. 10, pp. 1912–1927, May. 2018.

[31] C. Tang, M. Jiang, H. Shen, and C. M. Zhao, “Optimized constellation design for P-LDPC coded multi-color visible light communications,” in Proc. Int. Conf. Telecommun (ICT)., May. 2016, pp. 1–5.

[32] A. Yesilkaya, E. Basar, F. Miramirkhani, E. Panayirci, M. Uysal, and H. Haas, “Optical MIMO-OFDM with generalized LED index modulation,” IEEE Trans. Commun., vol. 65, no. 8, pp. 3429–3441, Aug. 2017.

[33] L. Hanzo, O. Alamri, M. E1-Hajjar, and N. Wu, Near capacity multi-functional MIMO systems. Hoboken, NJ, USA: Wiley, 2009.

[34] Z. Wu, X. Gao, and C. Jiang, “Nonbinary LDPC-coded spatial multiplexing for rate-2 MIMO of DVB-NGH system,” IEEE Trans. Broadcast., vol. 64, no. 2, pp. 201–210, Jun. 2018.

[35] G. Liva and M. Chiani, “Protograph LDPC codes design based on EXIT analysis,” in Proc. IEEE Global Commun. Conf., Nov.

2007, pp. 3250–3254.

[36] J. Thorpe, “Low-density parity-check (LDPC) codes constructed from protographs,” in Proc. IPN Progr. Rep., vol. 154, Aug.

2003, pp. 1–7.

[37] T. V. Nguyen, “Design of capacity-approaching protograph-based LDPC coding systems,” Ph.D. dissertation, Dept. Electr. Eng.

Univ. Texas at Dallas, Dallas, TX, USA, Dec. 2012.

[38] X. Gao, Z. Bai, P. Gong, and D. O. Wu, “Design and performance analysis of LED-grouping based spatial modulation in the visible light communication system,” IEEE Trans. Veh. Technol., vol. 69, no. 7, pp. 7317–7324, Jul. 2020.

[39] T. V. Nguyen, A. Nosratinia, and D. Divsalar, “The design of rate-compatible protograph LDPC codes,” IEEE Trans. Commun., vol. 60, no. 10, pp. 2841–2850, Oct. 2012.

[40] C. Tang, M. Jiang, H. Shen, and C. M. Zhao, “Analysis and optimization of P-LDPC coded RGB-LED-based VLC systems,” IEEE Photon. J., vol. 7, no. 6, pp. 1–13, Dec. 2015.

[41] J. Chen, A. Dholakia, E. Eleftheriou, M. P. C. Fossorier, and X. Y. Hu, “Reduced-complexity decoding of LDPC codes,” IEEE Trans. Commun., vol. 53, no. 8, pp. 1288–1299, Aug. 2005.