arXiv:2308.11955v1 [physics.flu-dyn] 23 Aug 2023

Stability of variable density rotating flows: Inviscid case and viscous effects in the limit of large Reynolds numbers

C. Jacques, B. Di Pierro,^∗ F. Alizard, and M. Buffat Univ Lyon, Université Claude Bernard Lyon I, Ecole Centrale de Lyon, INSA Lyon, CNRS, Laboratoire de Mécanique des Fluides et d’Acoustique, UMR 5509, 43 boulevard du 11 novembre 1918, F-69100, VILLEURBANNE, France

A. Cadiou and L. Le Penven Univ Lyon, Ecole Centrale de Lyon, INSA Lyon, Université Claude Bernard Lyon I, CNRS, Laboratoire de Mécanique des Fluides et d’Acoustique, UMR 5509, 36 Avenue Guy de Collongue, F-69134, ECULLY, France

Abstract

Linear stability of solid body rotating flows with axisymmetric density variations is addressed analytically. Considering inviscid disturbances, a non trivial dispersion relation is obtained and it is shown that the instability is of Rayleigh–Taylor type in cylindrical frame. The viscous correction is derived, in the limit of large Reynolds numbers and large azimuthal wave numbers, allowing the determination of the most unstable mode. Theoretical predictions are checked by comparing them to (spectrally accurate) computed eigenvalues and direct numerical simulations.

I. INTRODUCTION

Rotating and swirling flows of gas mixtures (i.e. variable density flows) are encountered in a wide variety of industrial and geophysical flows. Rotating injectors and hurricanes are two examples illustrating the special case of solid-body rotation [15]. Understanding the dynamics of these flows is not only of fundamental interest but is also relevant for the development of control and optimisation strategies.

It is well known that solid body rotation of a homogeneous fluid is a marginally stable configuration of Euler’s equations [9, 10], while viscosity has only a stabilizing influence. Hence, the so-called inertial waves have been experimentally observed only when the excitation source is sustained [16]. Considering three dimensional disturbances of a two-dimensional axisymetric basic configuration, the flow exhibits an instability if the Rayleigh-discriminant Φ = 2V (dV/dr + V/r)/r is negative somewhere in the flow [14] (r being the distance from rotation center and V (r) the azimuthal velocity).

If density variations within the fluid are considered, an equivalent to the Brünt-Vaïssalla frequency G is usually defined by G^2 = −(Ω^2r/ρ)dρ/dr (ρ being the density and Ω = V/r). Leibovith [13] and Howard [8] have shown independently that the flow is stable to axisymmetric disturbances if G^2 < Φ, for both incompressible and compressible flows. For rotating flows with axial jet, Leibovitch and Stewartson [14] have been able to theoretically derive the discrete spectrum of the instability near the point where the Doppler frequency kW + mΩ − ω admits an extremum (ω, k, m, W being the pulsation, axial wavenumber, azimuthal wavenumber and axial velocity, respectively). Subsequently, Eckhoff [4] derived a

∗ corresponding author: bastien.di-pierro@univ-lyon1.fr

sufficient condition for instability using a WKB expansion. Those results have been extended by Leblanc and Le Duc [12], who established a link between the eigenfrequencies of [4] and [14]. Di Pierro and Abid [1] have proposed an asymptotic expression for the eigenfrequency associated with rotating flow with axial jet, assuming large wavenumbers. Along with that, Gans [6] has shown that the flow is unstable with respect to any non axisymmetric two-dimensional disturbances if G^2 is slightly positive. Additionally, considering an equivalent configuration, Sipp et al. [20] have shown through numerical experiments that G^2 > 0 is a necessary condition for such an instability. The authors argued that the underlying mechanism was associated with a Rayleigh–Taylor instability. More recently, Scase and Hill [18] investigated both theoretically and numerically the effect of rotation on confined two liquid layers, with different density and viscosity, that form concentric cylinders. Their axis of rotation is confused with central axes of these cylinders. The authors have also discussed the effect of rotation of both miscible and immiscible fluids. For all flow cases, the equilibrium state is associated with the two-layers initially separated by a sharp interface. An Orr-Sommerfeld like equation is derived that successfully reproduces Direct Numerical Simulations as far as the linear approximation is still valid. Especially, they have shown that the system may be unstable when the inner fluid is denser than the outer one driven by the centrifugal force. The instability takes the form of mushroom like perturbations in the nonlinear regime as observed in Rayleigh–Taylor configuration. Scase and Sengupta [19] extended these results to a three dimensional configuration. They showed that the disturbances growth is essentially driven by geometrical parameters in the absence of surface tension: domain aspect ratio and initial position of the interface. While the above findings provide a good understanding of the amplification of Rayleigh–Taylor like instability in a centrifugally driven configuration, it does not discuss the case of initial gas mixtures and spatially extended configuration in the radial direction. Finally, an equivalent configuration of a cylindrical biphasic flow with uniform radial acceleration has been studied by Zeng et al. [21]. They observed both two and three-dimensional disturbances and particularly, they showed that the growth rate of the two-dimensional mode varies as ν^{1/3} (ν the kinematic viscosity), while the three dimensional regime is very dependent of the viscosity ratio. The purpose of this paper is then to investigate certain aspects of Rayleigh–Taylor instability in rotating flows and to extend previously mentionned studies. The studied configuration is a steady, solid-body rotation and incompressible flow in the presence of a radial smooth density gradient. Two results are obtained : i) an analytical dispersion relation without any asymptotic consideration in the inviscid case and ii) a viscous correction in the limit of large Reynolds numbers. The present study allows an extension of some conclusions in [1], which are limited to a large wavenumber and inviscid analysis. This paper also extends the study of [20] which numerically deals with the stability of inviscid Gaussian vortex with heavy cores. The present study corresponds to the case of non axial flow W (r) = 0 of [1] and small density core length b → 0 of [20]. In particular, it is shown that a sufficient condition for instability is G^2 > 0 somewhere in the flow for any density ratio, and that the viscous correction has a purely stabilizing effect, allowing the determination of the most unstable mode. A very good agreement between the analytical dispersion relation and (linear/nonlinear) numerical simulations is obtained.

The paper is organized as follows. In section II, the problem formulation is stated with mathematical and numerical considerations. Section III establishes the inviscid dispersion relation, and section IV deals with the viscous correction. Both are validated by comparison with computed eigenvalues in these two sections. Finally, those results are compared with direct numerical simulations in section V, and the last section provides some physical discussion and concluding remarks.

II. PROBLEM FORMULATION

A. Governing equations

The incompressible, variable-density Navier-Stokes equations are considered, neglecting molecular diffusion [7]: ∂u ∂t = −(u · ∇)u − 1 ρ ∇P + μ ρ Δu, (1) ∂ρ ∂t = −u · ∇ρ, (2) ∇ · u = 0, (3)

with u the vector velocity field, ρ the density and P the pressure. The dynamic viscosity μ is assumed to be constant, which is representative of gazeous or liquid mixtures, and the surface tension is neglected. We investigate a steady solid-body rotation base flow with rotation rate Ω and an axisymmetric density profile, as sketched in figure 1. By introducing

FIG. 1. Sketch of the basic flow.

R, the density core length, as the length scale and Ω^{−1} as the time scale, one can define the Reynolds number Re = ρ_∞ΩR^2/μ where ρ_∞ is the density far from the rotating center. The velocity, pressure and density fields of the base flow are expressed in polar coordinates (r, θ) as U_0(r) = Ωre_θ, P_0(r) and ρ_0(r) , respectively. We consider two-dimensional disturbances of the form : (u_r(x, t), u_θ(x, t), ρ(x, t), P (x, t))^T = (u(r), v(r), ρ(r), p(r))^T exp(i(mθ − ωt)), (4) with m the azimuthal wavenumber and ω the unknown complex pulsation. Linearization of equations (1, 2, 3) leads to the following eigensystem : i ( mΩ − ω + i L Reρ_0 ) u − 2 ( Ω − im Reρ_0r^2 ) v + 1 ρ_0 dP dr − Ω^2r ρ_0 ρ = 0, 2 ( Ω − im Reρ_0r^2 ) u + i ( mΩ − ω + i L Reρ_0 ) v + im rρ_0 P = 0, i (mΩ − ω) ρ + u dρ_0 dr = 0, 1 r dru dr + im r v = 0, (5)

with L = d^2 dr^2 + 1 r d dr − m^2 + 1 r^2 .

B. Numerical resolution

The eigenvalues and eigenfunctions (u, v, ρ, p) are computed with spectral accuracy by using Chebyshev polynomial expansions. The infinite domain r ∈ [−∞, ∞] is mapped to the interval γ ∈ [−1, 1] containing the Gauss-Lobato points (γ_i = cos(iπ/(N − 1)), i = 0..N − 1) using the transformation r = tan(πγ/2). This transformation avoid the expression of a boundary condition at r = 0, which depend on the disturbance symmetry. The number of modes N is even such that the singular point r = 0 is avoided. In the following , the radial derivative operators of order n will be denoted by D^n_r [17].

Since the equation associated with the pressure is independant of ω, the system 5 is numerically ill-conditioned. This leads to the computation of non physical oscillating modes [17]. To avoid the occurence of these spurious modes when solving the eigensystem, the pressure is eliminated from (5) by taking the divergence of the momentum equations and using the inverse of an elliptic operator: D = [ m^2 r^2ρ_0 − ( D_r + 1 r ) 1 ρ_0 D_r ]_{−1} . (6)

Now, the eigenvalue problem can be recast as:

A u v ρ = iω u v ρ , (7)

with

A = imΩ −^1_{Reρ0} L +^1_{ρ0} D_rD C_u −2 ( Ω −^{im}_{Reρ0r2} ) +^1_{ρ0} D_rD C_v^{−Ω2r}_{ρ0} +^1_{ρ0} D_rD C_ρ 2 ( Ω −^{im}_{Reρ0r2} ) +^{im}_{ρ0r} D C_u imΩ −^1_{Reρ0} L +^{im}_{ρ0r} D C_v^{im}_{ρ0r} D C_ρ dρ_0 dr 0 imΩ ,

C_u = ( D_r +^1_r ) ( imΩ −^1_{Reρ0} L ) + 2^{im}_r ( Ω −^{im}_{r2Reρ0} ) C_v = −2 ( D_r +^1_r ) ( Ω −^{im}_{r2Reρ0} ) +^{im}_r ( imΩ −^1_{Reρ0} L ) C_ρ = − ( D_r +^1_r

)_{Ω2r}

ρ_0

and L = D^2_r + (1/r)D_r − (m^2 + 1)/r^2. In addition to eliminating spurious modes, elimination of the pressure improves operator conditionning and accelerates the computation of eigenvalues. The last eigensystem (7) is solved using LAPACK routines.

For numerical validation, the following basic density profile is used :

ρ_0(r) = 1 + s − 1 2 ( 1 − tanh ( r − 1 e )) , (8)

which mimics heavy (or light) vortex core with smooth density variations; e being the variation length of density profile and s being the density ratio between the rotating center and the far field.

III. INVISCID INSTABILITY

In the limit of an infinite Reynolds number, the system (5) can be rewritten as a single equation of the variable ϕ = ru, as:

d^2ϕ dr^2 + 1 ρ_0r dρ_0r dr dϕ dr − [ 2mΩ rρ_0Σ dρ_0 dr + m^2 r^2 ( 1 + G^2 Σ^2 )] ϕ = 0, (9)

with:

G^2 = −

Ω^2r ρ_0 dρ_0 dr , Σ = mΩ − ω. (10)

Introducing ψ = √ rρ_0ϕ, equation (9) becomes:

d^2ψ dr^2 + [ ζ − 2mΩ rρ_0Σ dρ_0 dr − m^2 r^2 ( 1 + G^2 Σ^2 )] ψ = 0, (11)

with: ζ = [ 1 2ρ_0r dρ_0r dr ]_2 − 1 2ρ_0r d^2ρ_0r dr^2 . (12)

From (11), we assume that the unstable dynamics occurs at the location r^∗, such that G^2(r^∗) is a local extremum. Introducing, r̃ = r − r^∗ and ψ̃(r̃) = ψ(r), a second order Taylor expansion of (11) gives: d^2ψ̃ dr̃^2 + Θ(r̃)ψ̃ = 0 (13)

with:

Θ(r̃) = ζ(r^∗) − χ(r^∗) r^{∗2} + ( dζ dr (r^∗) +

2χ(r^∗) r^{∗3} ) r̃ + ( d^2ζ dr^2 (r^∗) − 1 r^{∗2} d^2χ dr^2 (r^∗) −

6χ(r^∗) r^{∗4} ) r̃^2 2 , χ(r) = 2m G^2 ΩΣ + m^2 ( 1 + G^2 Σ^2 ) . (14)

Equation (13) is a parabolic cylinder equation. Assuming that ψ vanishes far from r^∗, equation (13) admits solutions in the form of Weber-Hermite polynomials ψ̃(r̃) = H_n(αr̃+β) with: α = √ 2 ( 3 χ(r^∗) r^{∗4} + 1 2r^{∗2} d^2χ dr^2 (r^∗) − 1 2 d^2ζ dr^2 (r^∗) )_{1/4} , β = 2 α^3 ( dζ dr (r^∗) +

2χ(r^∗) r^{∗3} ) , (15)

if and only if:

− 1 α^2 χ(r^∗) r^{∗2} − ζ(r^∗) + (_{dζ} dr (r^∗) +^{2χ(r∗)}_{r∗3} )_2

2^{d2ζ}_{dr2} (r^∗) − 2^1_{r∗2}^{d2χ}_{dr2} (r^∗) −^{12χ(r∗)}_{r∗3} = n + 1 2 , (16)

FIG. 2. Inviscid dispersion relation Im(ω) versus azimuthal wavenumber m for density ratio s = 2 and mass thickness e = 0.2 (Dotted: eigenvalue of system (7), line: root of dispersion relation (16), dashed: Asymptotical solution (17)).

where n is an integer. This inviscid dispersion relation corresponds to the case studied numerically in [20] for small density distribution widths (defined as “b” in their paper). Note that it is not based on the assumption of a weakly varying base flow [1] or large wavenumbers. In the limit of large azimuthal wavenumbers, the following growth rate is obtained by expansion of (16) with respect to m:

ω_n = mΩ +

G^2 mΩ + i ( √ G^2(r^∗) + n +^1_2 m √ − r^{∗2} 2 d^2G^2 dr^2 (r^∗) ) . (17)

Here, the expression (17) is identical to the one obtained in [1], except for the correction G^2/mΩ to the real part. Equation (16) has no explicit solution, and is numerically solved using the Muller’s root finding algorithm [11].

Figure 2 compares the dispersion relation obtained using the full system (7) to the solution of (16) and the asymptotic expression (17). A very good agreement is found: the solutions of system (7) and equation (16) are almost undistinguishable, and the relative error is less than 10% if m ≥ 6 when comparing the solution of (7) and (17).

IV. ASYMPTOTIC VISCOUS INSTABILITY

The viscous case is considered here in the limit of large Reynolds numbers as well as large wave numbers, such that 1 ≪ m^2 ≪ Re. Hence, m^2Re^{−1} is treated as a small parameter.

FIG. 3. Growth rate Im(ω) versus azimuthal wavenumber m for s = 10, e = 0.2 and Re = 1000

(Dotted: eigenvalue of system (7), line: Asymptotical solution (22)).

In this limit, the viscous operator behaves to leading order as 1 Re L ≈ −m^2 r^2Re . (18)

The differential system (5) can then be rewritten as a second order differential equation:

d^2ϕ dr^2 + [ 1 ρ_0r dρ_0r dr + 1 Σ + iN dN dr ] dϕ dr − [ 2m(Ω − iM) rρ_0(Σ + iN ) dρ_0 dr + m^2 r^2 ( 1 + G^2 Σ(Σ + iN ) ) − 2im r 1 Σ + iN dM dr ] ϕ = 0, (19)

with: N = −m^2 r^2Re , M = m r^2Re . (20)

Proceeding in the same way as in previous section, one gets to leading order in m and m^2/Re: d^2ψ dr^2 − [ 2mG^2 r^2Ω(Σ + iN ) + m^2 r^2 ( 1 + G^2 Σ(Σ + iN ) )] ψ = 0, (21)

with ψ = √ ρ_0r(Σ + iN )ϕ. Here again, a parabolic cylinder equation is found, whose solutions are Weber-Hermite polynomials associated with the following dispersion relation:

ω_n = mΩ +

G^2(r^∗) Ωm + i ( √ G^2(r^∗) − n + 1/2 m √ − r^{∗2} 2 d^2G^2 dr^2 (r^∗) − m^2 2Reρ_0(r^∗)r^{∗2} ) . (22)

Figure 3 shows the imaginary part of the eigenfrequencies obtained numerically in compar-

FIG. 4. Numerical and asymptotical growth rate Im(ω_{n,max}) versus m_{max} for the most unstable mode for e = 0.2. Left: Re = 10^4 and s = 2, 3, 4, 5, 6, 7, 8, 9, 10. Right: s = 8 and Re = 10^2, 10^3, 10^4, 10^5, 10^6 (Dotted: eigenvalue of system (7), line: Asymptotical solution (23- 24)).

ison with the asymptotic solution (the real parts being undistinguishable). It appears that equation (22) is a good approximation when 12 ≤ m ≤ 50 (the error is less than 2.5%); i.e. in the limit of large m and m^2Re^{−1} ≲ O(1). Moreover, one can see that the maximum of the dispersion curve (see figure 3) is correctly represented by this last approximation. This allows the identification of the most unstable mode as well as the corresponding azimuthal wavenumber:

ω_{n,max} = mΩ + G^2(r^∗) Ωm + i √ G^2 − 3i 2

(( n +^1_2 ) √ −^{r∗2}_2^{d2G2}_{dr2} (r^∗)

) 2_3

(r^{∗2}ρ_0(r^∗)Re)^13

, (23)

m_{max} = (( n + 1 2 ) Reρ_0(r^∗)r^{∗2} ) 1_3 ( − r^{∗2} 2 d^2G^2(r^∗) dr^2 ) 1_6 . (24)

A comparison between these approximations and numerical solutions is shown in figure 4. Very good agreement is found for the most amplified mode ω_{n,max} as well as for the selected azimuthal mode m_{n,max}.

V. NONLINEAR INSTABILITY

To analyse the instability dynamics towards the non linear stage, the variable density Navier–Stokes equations (1, 2, 3) are solved numerically using the method presented in

[3]. Here is a brief review. The spatial discretisation is based on a two-dimensional Fourier expansion, with periodic boundary conditions. Time integration is performed using a second order Runge-Kutta scheme, while the pressure is computed using a fixed point method to ensure the incompressiblity constraint. The time step is choosen as 10^{−2} in order to satisfy stability criterion, and the computational domain is a square of size 6π × 6π discretized with 512 × 512 grid points. The initial density profile (8) is used. The velocity initial condition is a Lamb–Oseen like vortex: Δ(U_θe_θ) = −∇ × (Ω_{LO}(r)e_z), with Ω_{LO}(r) = Ω exp(−r^2/a^2) the vorticity and a = 5. The latter velocity field is then compatible with periodic boundary conditions [2]. A plot of the initial distribution is shown in figure 5 (top left). Note that the dynamics within the vortex core (r ≲ 0.3a) is close to a solid body rotation. In the case of constant density, the Lamb-Oseen vortex does not satisfy the instability conditions of Leibovich & Stewarson [14]. Its linear stability has been proven numerically by [5]. Finally, the flow is initially disturbed with a random noise of amplitude O(10^{−3}). The disturbance amplitudes A_m of each mode m are extracted from the Fourier expansion ρ̂_m(r, t) of the density field ρ(r, θ, t) interpolated from the Cartesian grid (x, y), and are defined as: A_m(t) = √∫_R 0 |ρ̂_m(r, t)|^2rdr. (25) Figure 5 shows a contour plot of the density field at times t ≈ 3.7, 5.5 and 7.4 for Re = 1000 and s = 2. At the earliest times, many azimutal modes are growing (figure 5 top right), while the azimutal mode m ≈ 17 emerges a little later on (figure 5 bottom left). This last mode is the most unstable, that is predicted by the asymptotic expression m_{max} (24).

Figure 6 shows the amplitude of the m = 17 mode versus time and the asymptotic prediction exp(−iω_{n,max}t)(see equations 23, 24); Im(ω_{n,max}) ≈ 1.04 with the considered parameters for this mode. After a transient time, one can see that the exponential growth is well represented by the asymptotic theory. For t ≈ 7, figure 5 (bottom right) shows that the instability reaches a non-linear stage where modal interactions can no longer be neglected. The study of these nonlinear interactions is left for future work. A last simulation where e/R = O(1) has been performed, with the basic flow:

ρ_0(r) = 1 + (s − 1) exp(−r^2) (26)

The comparison between direct numerical simulation and prediction of (23) is shown on figure (7). Once again, a very good agreement is found.

FIG. 5. Direct numerical simulation of the variable density rotating flow with s = 2 and Re = 1000. Initial radial distribution (top left), Iso-contours of density field at time t ≈ 3.7 (top right),t ≈ 5.5 (bottom left) and t ≈ 7.4 (bottom right). x and y are here the Cartesian coordinates.

FIG. 6. Amplitude of the azimutal mode m = 17 versus time, for Re = 1000 and s = 2 and the asymptotic prediction (23,24).

FIG. 7. Left: dispersion relation of base flow (26). Right: Amplitude of the azimutal mode m = 10 versus time, for Re = 1000 and s = 2 and the asymptotic prediction (23, 24), for base flow (26).

VI. DISCUSSION AND CONCLUSION

The paper presents a linear temporal stability analysis of an axisymmetric, variabledensity, uniformly rotating flow evolving under the incompressibility constraint. The problem solutions are validated by comparison to spectrally accurate numerical methods. In the inviscid case, which is considered first, the problem is governed by a second order differential equation. It is shown that the instability dynamics is characterized by an analog to the Brünt-Vaïssalla frequency G(r) (with G^2(r) = (−Ω^2r/ρ_0)dρ_0/dr ). It is also shown that disturbances reach a maximum near the location where G^2(r) admits an extremum. A non trivial dispersion relation is obtained. However, in the limit of large azimuthal wavenumbers, an approximation of eigenfrequency can be analytically obtained. It can be seen that an instability can occur if and only if G^2 > 0 (i.e. if dρ_0/dr < 0). In that sense, it completes results given by Scase and Hill [18] restricted to the sharp initial density profile case and confined within a given radial distance from the rotating center. One deduces that the instability is triggered when the local centrifugal acceleration (a_c = Ω^2re_r) and the reduced density gradient ( ¯∇ρ = (∇ρ_0)/ρ_0) are in opposite directions. This shows that the resulting instability is a cylindrical Rayleigh–Taylor one, the disturbance growth rate being proportional to the maximum of √ −a_c · ¯∇ρ. This is very similar to the classical planar Rayleigh–Taylor growth rate √ gkA_t (g, k and A_t being the gravitational acceleration, the wavenumber and the Atwood number respectively). When comparing the expression of the eigenfrequencies at large m for solid-body rotation to the asymptotic result of [1] obtained assuming weakly-varying velocity profiles, it appears that the instability growth rates are the sames up to order 1/m. The only difference being that a change is observed in the the real frequency of order 1/m. In the inviscid case, all modes are unstable and the instability growth rate is an increasing function of the azimuthal wavenumber approaching the asymptotic value √ G^2 for large m. Hence, no mode selection is observed. To correctly represent the mode selection, viscous effects have been studied in the limit of large Reynolds numbers as well as large m. The resulting dynamics equation is very similar to the inviscid one and viscosity appears as a purely stabilizing effect. Indeed, the real frequency is not affected by the viscous drag while the growth rate varies as −m^2/(ρ_0Re). Once again, this is remarkably similar to the planar Rayleigh–Taylor viscous correction proportional to −k^2/(ρ_mRe) (ρ_m being an average density). Thus, the resulting instability exhibits competitive mechanisms between the inviscid Rayleigh–Taylor instability and to viscous damping. The most unstable mode has a growth rate varying as Re^{−1/3} while the corresponding azimuthal wavenumber grows as Re^{1/3}. The latter scaling is very similar to the planar Rayleigh–Taylor instability for which the growth rate varies as Re^{−1/3}, while the corresponding longitudinal wavenumber grows as Re^{2/3}.

Considering three dimensional disturbances for the same base flow ( i.e. a columnar vortex), one notes that the dynamics equation remains the same when considering the modified wave number l^2 = m^2 + k^2r^2, where k the axial wave number. In particular, in the limit of large wavenumbers l → ∞ and large Reynolds numbers, equation (19) remains invariant by substituting m with l. Hence, the same instability characteristics are obtained. Such three-dimensional disturbances are helical Rayleigh-Taylor instabilities. Such disturbances has been observed by Zeng et al. [21] for biphasic radially accelerated flows. Finally, these results have been validated using nonlinear direct numerical simulations where the instability is triggered by superimposing random noise of small amplitude onto the base flow. The most unstable mode observed in these simulations is in very good agreement with asymptotic theory. In the later times of the simulation, while nonlinearities appear, a strong modal interaction leads to the formation of mushroom-shaped disturbances, which are characteristics of a Rayleigh–Taylor instability. The resulting flow pattern is very similar to the one observed by Scase and Hill [18] in confined configuration.

ACKNOWLEDGEMENT

The authors acknowledge the “Fédération Lyonnaise de Modélisation et Sciences Numériques” for providing numerical facilities on the cluster P2CHPD.

[1] Di Pierro, B. & Abid, M. 2010 Instabilities of variable-density swirling flows. Physical Review E 82 (4), 046312.

[2] Di Pierro, B. & Abid, M. 2012 Rayleigh–Taylor instability in variable density swirling flows. The European Physical Journal B 85, 1–8.

[3] Di Pierro, B. & Abid, M. 2013 A projection method for the spectral solution of nonhomogeneous and incompressible Navier–Stokes equations. International Journal for Numerical Methods in Fluids 71 (8), 1029–1054.

[4] Eckhoff, K. S. 1984 A note on the instability of columnar vortices. Journal of Fluid Mechanics 145, 417–421.

[5] Fabre, D., Sipp, D. & Jacquin, L. 2006 Kelvin waves and the singular modes of the lamb-oseen vortex. Journal of Fluid Mechanics 551, 235.

[6] Gans, R. F. 1975 On the stability of shear flow in a rotating gas. Journal of Fluid Mechanics 68 (2), 403–412.

[7] Guillén-González, F., Damázio, P. & Rojas-Medar, M. A. 2007 Approximation by an iterative method for regular solutions for incompressible fluids with mass diffusion. Journal of mathematical analysis and applications 326, 468–487.

[8] Howard, L. N. 1973 On the stability of compressible swirling flow. Studies in Applied Mathematics 52 (1), 39–43.

[9] Kelvin 1910 Mathematical and physical papers, IV. Hydrodynamics and General Dynamics, Cambridge, England 69.

[10] Landau, L. D. & Lifchitz, E. 1987 Course of theoretical Physics, Fluid Mechanics, , vol. 6.

Pergamon.

[11] Lang, M. & Frenzel, B.-C. 1994 Polynomial root finding. IEEE Signal Processing Letters 1 (10), 141–143.

[12] Leblanc, S. & Le Duc, A. 2005 The unstable spectrum of swirling gas flows. Journal of

Fluid Mechanics 537, 433–442.

[13] Leibovich, S. 1969 Stability of density stratified rotating flows. AIAA Journal 7 (1), 177– 178.

[14] Leibovich, S. & Stewartson, K. 1983 A sufficient condition for the instability of columnar vortices. Journal of Fluid Mechanics 126, 335–356.

[15] Lumley, J. L. 1999 Engines: An Introduction. Cambridge University Press. [16] McEwan, A. D. 1970 Inertial oscillations in a rotating fluid cylinder. Journal of Fluid Mechanics 40 (3), 603–640.

[17] Peyret, R. 2013 Spectral methods for incompressible viscous flow, , vol. 148. Springer Science & Business Media.

[18] Scase, M. M. & Hill, R. J. A. 2018 Centrifugally forced Rayleigh–Taylor instability.

Journal of Fluid Mechanics 852, 543–577.

[19] Scase, M. M. & S., Sengupta 2021 Cylindrical rotating Rayleigh–Taylor instability. Journal of Fluid Mechanics 907, A33.

[20] Sipp, D., Fabre, D., Michelin, S. & Jacquin, L. 2005 Stability of a vortex with a heavy core. Journal of Fluid Mechanics 526, 67–76.

[21] Zeng, R. H., Tao, J. J. & Sun, Y.B. 2020 Three-dimensional viscous Rayleigh–Taylor instability at the cylindrical interface. Physical review E 102, 023112.