arXiv:2308.12019v2 [physics.optics] 21 Jun 2024

Negative Refraction in isotropic achiral and chiral materials

Y. B. Band^1, Igor Kuzmenko^1, Marek Trippenbach^2 1 Department of Chemistry, Department of Physics, Department of Electro-Optics, and the Ilse Katz Center for Nano-Science, Ben-Gurion University, Beer-Sheva 84105, Israel 2 Faculty of Physics, University of Warsaw, ul. Pasteura 5, 02-093 Warszawa, Poland

We show that negative refraction in materials can occur at frequencies ω where the real parts of the permittivity ε(ω) and the permeability μ(ω) have different sign, and that light with such frequencies can propagate just as well as light with frequencies where they have equal sign. Therefore, for negative refraction one does not need to be in the “double-negative” regime. We consider negative refractive index achiral materials using the Drude-Lorentz model and chiral materials using the Drude-Born-Fedorov model. We find that the time-averaged Poynting vector always points along the wave vector, the time-averaged energy-flux density is always positive, and the time-averaged energy density is positive (negative) when the refractive index is positive (negative). The phase velocity is negative when the real part of the refractive index is negative, and the group velocity generally changes sign several times as a function of frequency near resonance.

I. INTRODUCTION

Negative refraction (NR) is a phenomenon in which electromagnetic waves are refracted at an interface with NR angle [1–5]. It is believed that in order for NR to occur, the real part of the (electric) permittivity (ε) and real part of the (magnetic) permeability (μ) must both be negative at a particular frequency [1–9]. Such materials are sometimes called “double-negative” materials. NR meta-materials, i.e., specially designed NR materials made from assemblies of multiple elements fashioned from composite materials have been developed [3, 6–9]. It is furthermore believed that light at frequencies such that {Re[ε(ω)] > 0 and Re[μ(ω)] < 0} or {Re[ε(ω)] < 0 and Re[μ(ω)] > 0}, is not able to propagate in materials [1–9]. Both beliefs are predicated on the assumption that the permittivity and the permeability are real. However, this “double-negative” criterion does not apply for frequencies close to resonance, where the permittivity and the permeability are complex. If the permittivity and the permeability are real and have different signs, the average energy flux density (average Poynting vector) vanishes (see Sec. II C). However, if the permittivity and the permeability are complex, the average energy flux density is non-zero (the same is true for the chiral case treated in Sec. IV A). Here we use the amplitudephase representation of the permittivity and permeability within the Drude-Lorentz model for achiral media [10] and the Drude-Born-Fedorov model [11] for chiral media to calculate the complex refractive index. We then analyze and categorize the wealth of phenomena that occur when optical waves are in frequency ranges near resonant optical transitions where NR is possible. The analysis presented here breaks the old paradigm for NR and creates a new one in which the frequency regime for NR is significantly broader when compared with previously deduced frequency ranges.

References [12, 13] are exceptions; they used the amplitude-phase representation of the permittivity, permeability and refractive index. They consider two resultant complex refractive indices, n(ω) = ± √ ε(ω)μ(ω)/(ε_0μ_0). While the resultant complex refractive index n(ω) with the minus sign is not a physical solution, because it gives negative absorption (i.e., gain), the refractive index n(ω) with the plus sign has the right properties.

To date, NR materials have been fabricated using manmade meta-materials, but Ref. [14] argued that naturally occurring NR materials exist; the NR of n(?) were calculated. NR meta-materials have led to significant technological advancements [4–9] including: (1) superlensing, i.e., overcoming the diffraction limit of conventional lenses, allowing for sub-wavelength imaging for high-resolution microscopy [15, 16], (2) cloaking using devices that can manipulate the flow of light around an object, rendering it invisible to observers [4, 17, 18], (3) terahertz imaging, spectroscopy, and communication systems, enabling non-invasive inspections in biomedical imaging and security screening [19], and (4) antennas incorporating NR meta-materials that can enhance the radiated power of the antenna NR by focusing electromagnetic radiation by a flat lens versus dispersion [20–22].

II. THEORY

For an electromagnetic plane wave, with electric field E(r, t) = Re(E_0 e^{i(k·r−ωt)}) and magnetic field H(r, t) = Re(H_0 e^{i(k·r−ωt)}), the Faraday and Ampère equations, together with the constitutive equations in an isotropic homogeneous material, D = εE and B = μH yield, in SI units,

k × E_0 = ω μ(ω)H_0, k × H_0 = −ω ε(ω)E_0. (1)

Substituting k =^{n(ω) ω}_c k̂ we obtain

n(ω) k̂ × E_0 = c μ(ω)H_0, (2)

n(ω) k̂ × H_0 = −c ε(ω)E_0, (3) which yields [noting that in vacuum, c^2 = (ε_0μ_0)^{−1}],

n^2(ω) = c^2ε(ω)μ(ω) =^{ε(ω)μ(ω)}_{ε0 μ0} . (4)

A. Drude-Lorentz model

The Drude-Lorentz model [10] is a widely used theoretical framework for describing the behavior of electromagnetic waves in materials. It provides a phenomenological approach to model ε and μ of materials, including those with NR. In the Drude-Lorentz model, the equation of motion for an electron in a meta-atom can be expressed as: m d^2r dt^2 = −mω^2_0r − mγ dr dt + (−e)E(ω)e^{−iωt}, (5) where m is the effective mass of the electron, r(t) is the displacement of the electron, ω_0 is the resonance frequency, γ is the damping coefficient, e is the elementary charge, and E(ω) is the electric field of the incident electromagnetic wave at frequency ω. Substituting r(t) = r_0(ω)e^{−iωt}, into Eq. (5), we find r_0(ω) = (_{−e/m} ω^2_0 −ω^2−iγω ) E(ω). The polarization P(ω) related to the induced dipole moment per unit volume, can be written as P(ω) = −Ner_0(ω) ≡ χ(ω)E(ω), where χ(ω) is the electric susceptibility of the material. Substituting the expression for r_0 into P(ω), we can obtain the electric susceptibility as χ(ω) = −^{Ne2}_{m(ω2−ω20 +iγω)} where N is the number density of electric dipole moments. The electric permittivity ε(ω) of the material can then be calculated as ε(ω) = ε_0(1 + χ(ω)) = ε_0(1 − ω^2_p ω^2 − ω^2_0 + iγω

), (6)

where the plasma frequency is defined as ω^2_p =^{Ne2}_{ε0 m} [25]. [If we make use of the Clausius-Mossotti relation [23],

then ε(ω) = ε_0(1 −^{ω2p}_{ω2−ω̃20 +iγω} ) where ω̃^2_0 = ω^2_0 − ω^2_p/3, but the correction to the resonance frequency is usually small.] Similarly, a magnetic dipole transition with resonance frequency ω_{0m} and width γ_m yields the magnetic permeability,

μ(ω) = μ_0(1 − ω^2_{pm} ω^2 − ω^2_{0m} + iγ_mω

), (7)

where the magnetic plasma frequency squared ω^2_{pm} is a constant related to the magnetic properties of the material and is proportional to the transition magnetic dipole moment squared.

B. Negative refractive index

In order to develop the theory of NR, Veselago [1]

wrote, n(ω) = ± √_{ε(ω)μ(ω)} ε_0μ_0 , where the minus sign is re-

quired for the case when the real parts of both ε(ω) and μ(ω) are negative. This is the standard approach for dealing with double-negative materials [1–9]. Instead we follow a more direct and mathematically appealing procedure. We write the complex refractive index as n(ω) = √ |ε(ω)||μ(ω)| √ ε_0μ_0 e^{i(θε(ω)+θμ(ω))/2}, (8) where θ_ε and θ_μ are the complex phases of ε and μ, respectively, i.e., ε = |ε|e^{iθε} and μ = |μ|e^{iθμ} . The real (imaginary) part of n(ω) is the refractive index (optical absorption coefficient divided by ω/c). The imaginary part of n(ω), n^{′′}(ω), must be non-negative since otherwise the plane wave for the electric field, E(r, t) = Re(E_0 e^{i(k·r−ωt)}) = Re(E_0 e^{iω[(n′ (ω)+in′′ (ω))k̂·r/c−t]}), would have gain, which is impossible. This form of the refractive index is unique (there are no branch point problems because of the square root in the definition of the refractive index, and because the imaginary part of n(ω) cannot be negative since that would imply gain). Therefore, adding an angle π to θ_n = (θ_ε + θ_μ)/2 in Eq. (8) would yield an unphysical complex refractive index.

C. Poynting vector

The Poynting vector (which gives the electromagnetic energy transfer per unit area per unit time) is defined as S = E × H. For a linearly polarized plane wave with E(r, t) = Re(E_0 e^{i(k·r−ωt)}) and H(r, t) = Re(H_0 e^{i(k·r−ωt)}), where E_0 and H_0 obey the Eqs. (2) and (3) with ε, μ and n being complex, the three orthogonal vectors {E_0, H_0, k} can be written as E_0 = E_0 x̂, H_0 = H_0 ŷ and k = k ẑ, where k = ωn(ω)/c, H_0 = √ |ε|/|μ| E_0e^{iθH} , and θ_H = (θ_ε − θ_μ)/2. The orthogonal vectors {E_0, H_0, k} form a right- (left)-handed coordinate system if Re(n) > 0 (Re(n) < 0). Taking E_0 to be real and positive, we obtain

S = ẑ √ |ε|/|μ| E^2_0 cos(ζ) cos(ζ + θ_H )e^{−2k′′ z} . (9) Here ζ = k^′z − ωt, and k^′ = n^′(ω)ω/c (k^{′′} = n^{′′}(ω)ω/c) is the real (imaginary) part of k, and n^′ (n^{′′}) is the real (imaginary) part of n. When θ_H vanishes, S is proportional to cos^2(ζ) and is directed along ẑ. When θ_H ≠ 0, the magnetic field has phase shift θ_H with respect to the electric field. Hence, there are intervals of ζ where both cos(ζ) and cos(ζ + θ_H ) have the same sign and S is along ẑ, and there are intervals of ζ where cos(ζ) and cos(ζ + θ_H ) have different signs. In the latter case, S is along −ẑ. Hence the energy transfer per unit area per unit time is time-dependent and can be either positive or negative. The time-averaged energy flux density is

S̄ ≡^1_T ∫_T 0 S(z, t)dt = ẑ √ |ε|/|μ| (E^2_0 /2) cos(θ_H )e^{−2k′′ z}, (10) where T = 2π/ω is the wave period. If ε and μ are real and have different signs, satisfying the Faraday and Ampère equations requires |θ_H | = π/2 and S̄ = 0. If ε and μ are complex, 0 < θ_ε < π and 0 < θ_μ < π, and |θ_H | < π/2, which is clear from the Drude-Lorentz model; S̄(ω) is always directed along ẑ.

D. Electromagnetic energy density and power dissipation density

The time rate of change of the electromagnetic energy density is given by [24] ∂u ∂t = E · ∂D ∂t + H · ∂B ∂t . (11)

Moreover, the rate of change of the energy density can be written as^{∂u}_{∂t} = Q +^{∂ueff}_{∂t} , where Q is the power dissipation density, and^{∂ueff}_{∂t} is the energy density rate due to energy transfer, i.e., the difference between incoming and outgoing electromagnetic energies. For a narrow wave packet, the time-averaged power dissipation Q̄ and the energy density ū_{eff} averaged over a period 2π/ω are [24, 27] Q̄ = ω 2 [ ε^{′′}(ω) | |E_0 | |^2 + μ^{′′}(ω) | |H_0 | |^2]e^{−2k′′ z} = ω 2 { ε^{′′}(ω) + μ^{′′}(ω) | | ε(ω) μ(ω) | |} | |E_0 | |^2e^{−2k′′ z}, (12) ū_{eff} = 1 2 { d(ω ε^′(ω)) dω | E_0 |_2 + d(ω μ^′(ω)) dω | H_0 |_2} e^{−2k′′ z} = 1 2 { d(ω ε^′(ω)) dω + d(ω μ^′(ω)) dω | | ε(ω) μ(ω) | | }| |E_0 | |^2e^{−2k′′ z} . (13)

Note that if ω_p > √ γ(2ω_0 + γ), then ε^′(ω_±) = 0, where

ω_± = ω_{20} + ω^2p − γ^2 2 ± √( ω^2_p − γ^2 2 )_2

− ω^2_0 γ^2.

For ω_− < ω < ω_+, ε^′(ω) is negative. If ω is close to ω_−, ε^′(ω) is small and^{∂ε′ (ω)}_{∂ω} < 0, then^{d(ω ε′ (ω))}_{dω} < 0, and the electric energy density^1_2^{d(ω ε′ (ω))}_{dω} | |E_0 | |^2 is negative.

Moreover, if ω_{pm} > √ γ_m (2ω_{0m} + γ_m), there is a range of ω where^{d(ω μ′(ω))}_{dω} < 0, and the magnetic energy density 1 2 d(ω μ^′(ω)) dω | |H_0 | |^2 is negative.

E. Phase velocity and group velocity

The phase velocity of light is v_p = ω/k^′, and the group velocity is v_g = (∂k^′/∂ω)^{−1}. Hence, v_p = c/n^′, and v_g = c/(n^′+ω∂_ωn^′). Note that when n^′ < 0, the phase velocity is negative, and when n^′ + ω∂_ωn^′ < 0, the group velocity is negative. In other words, if a pulse propagates through a material with a negative group velocity, the peak of the pulse propagates in the direction opposite to the energy flow direction [28, 29]. Moreover, near a resonance, n^′ + ω∂_ωn^′ can be small, and the group velocity can exceed the speed of light [30]. Experiments have verified that it is possible for the group velocity to exceed the speed of light in vacuum [29, 31–33]. From our calculations we see that the group velocity can become singular at as many as four frequencies.

A circular-polarization representation for achiral materials will be discussed following the chiral case below. It turns out to be simpler than the linearly polarized analysis above.

III. NUMERICAL RESULTS FOR THE ACHIRAL CASE

Using the Drude-Lorentz model for an electric dipole transition and a magnetic dipole transition with resonance frequencies that are close to one another (see the caption of Fig. 1 for the set of parameters used), we calculate the complex permittivity ε(ω) and complex permeability μ(ω) versus frequency, and the complex refractive index n(ω) (whose real part is the index of refraction and imaginary part is the absorption coefficient) using Eq. (8). Figure 1 shows the complex ε(ω) and μ(ω) versus frequency calculated with the Drude-Lorentz model. The region of frequencies where both of the real parts of ε(ω) and μ(ω) are negative is shown in Fig. 1, but there are also frequency regions where the real parts of ε(ω) and μ(ω) are of opposite sign. Figure 2 plots the real and imaginary parts n(ω), defined in Eq. (8), versus ω. Note that the absorption coefficient α ≡ Im[n(ω)] ≥ 0 for all frequencies [hence there is absorption (no gain) for all frequencies]. Moreover, there are frequency regions where Re[n(ω)] < 0 and in part of this frequency range the real parts of ε(ω) and μ(ω) are of opposite sign.

Note that all the figures in this paper appear in the Supplemental Material (SM) [26], which is a Mathematica notebook, that allows the reader to modify all the material parameters using the sliders.

For comparison, Fig. 3 shows n(ω) versus ω calculated assuming the light can propagate only if the real parts of ε and μ are of the same sign, as assumed in much of the literature. Where they are of opposite sign, n(ω) has been set to zero in Fig. 3. With the set of parameters used, there are two frequency regions where n(ω) has been set to zero; the frequency regions [3.01, 3.24] and [3.73, 5.82]. Readers can compare Fig. 3 with Fig. 2 to see the behavior of the correct refractive index in these regions. The large region where n(ω) is zeroed to the right of ω = 3.7 is where the real part of ε is negative but the real part of μ is positive, and the same is true in the small region near ω = 3.0 (see Fig. 1).

Figure 4 plots the frequency dependence of the timeaveraged Poynting vector,^{S̄(ω)}_{E 20 e−2k}′′_z [which is equivalent

FIG. 1. The complex relative electric permittivity (ε/ε0) and complex magnetic permeability (μ/μ0) plotted versus ω (in arbitrary units) for Drude-Lorentz parameters, ω0 = 3, ω0m = 3.2, γ = 0.3, γm = 0.2, ωp = 5, andωpm = 2. The dashed curves are the imaginary parts of ε(ω) and μ(ω).

FIG. 2. The real (magenta) and imaginary (black) parts of the complex refractive index n(ω) versus ω (in arbitrary units) for the same Drude-Lorentz parameters as used in Fig. 1. The NR region is to the right of the resonance frequency. The imaginary part shows absorption over a large region about the resonance frequency.

to the non-averaged quantity^{S±(ω)}_{E 2±e−2k}′′_{σ z} for right and left

polarized light in the chiral case, as discussed in Sec. IV]. The average Poynting vector is positive (i.e., in the z direction) for all frequencies. The peaks of S̄ appear at the frequencies of the maximum and minimum of n(ω), respectively. Figure 5 plots both the average energy density ū(ω) and the imaginary parts of the permittivity and permeability, ε^{′′}(ω) ≡ Im[ε(ω)] and μ^{′′}(ω) ≡ Im[μ(ω)], versus frequency. ū(ω) is negative in the frequency region near the maximum of ε^{′′}, and in a region near the maximum of μ^{′′}.

Figure 6 shows the time-averaged power dissipation density Q̄(ω) versus ω given in Eq. (12). The major peak near ω = 3 is due to the peak of the imaginary part of n(ω) and the minor peak near ω = 3.8 is near the small peak of the imaginary part of n(ω) near ω = 3.9. In

FIG. 3. The real and imaginary parts of the complex refractive index versus ω (in arbitrary units) for the same Drude-Lorentz parameters as used in Fig. 1 using the “doublenegative” criterion that propagation cannot occur if the real parts of ε and μ have different signs. In the these frequency regions the real and imaginary parts of n(ω) have been set to zero, which is necessary according to the commonly held view.

FIG. 4. The time-averaged Poynting vector S̄ plotted versus ω (in arbitrary units) for the same Drude-Lorentz parameters as used in Fig. 1.

Fig. 1 we can see that the imaginary part of μ(ω) has a peak at ω = 3.2 which contributes to the peak of Q̄(ω) but is shifted due to the factor of | |^{ε(ω)}_{μ(ω)} | | multiplying it

[see Eq. (12)].

Figure 7 plots the phase velocity v_p = ω/k^′ versus frequency. There are two resonances in the phase velocity that originate from the two zeros in Re[n(ω)] ≡ n^′(ω). Figure 8 plots the group velocity v_g = (∂k^′/∂ω)^{−1} versus frequency. There are four resonances for the group velocity that originate from four zeros in ∂[ωn^′(ω)]/∂ω.

Figure 9 simulates a plane wave which is polarized along the x-axis as it propagates along the z-axis. The figure shows the electric field E(r, t) = x̂ Re[e^{i(kz−ωt)}], where k = n(ω)ω/c, versus z at five different times. At a frequency ω = 3.8 (arb. units), the phase of the electric field propagates in the −z direction (the curves shift left with increasing time), hence the real part of the refractive index is negative (see below). For

FIG. 5. The time-averaged energy density ū(ω) (black), the imaginary part of the permittivity, Im(ε) ≡ ε^{′′} (red) and the imaginary part of the permeability, Im(μ) ≡ μ^{′′} (blue) versus ω (in arbitrary units) for the same Drude-Lorentz parameters as used in Fig. 1.

FIG. 6. The time-averaged power dissipation density Q̄(ω) versus ω (in arbitrary units) for the same Drude-Lorentz parameters as used in Fig. 1.

the Drude-Lorentz parameters used here, the permittivity is ε(ω) = −3.402 + 0.923 i, and the permeability is μ(ω) = 0.078 + 0.167 i, i.e., ε^′(ω) and μ^′(ω) have different signs (so according to the “double-negative” criterion that propagation cannot occur if the real parts of ε and μ have different sign, propagation cannot occur at this frequency), and the refractive index is n(ω) = −0.339 + 0.731i. In the section titled “Simulation of the propagation of a plane wave in an achiral medium” of the SM [26] you can run a movie of the propagation of the electric field and watch it propagate by opening the time slider and playing the movie. In the SM [26] you can also change the frequency ω as well as other Drude-Lorentz parameters to see how the propagation changes as the parameters are varied.

IV. CHIRAL MEDIA

The constitutive equations for isotropic chiral media must be modified to allow for optical activity. One form

FIG. 7. Phase velocity vp = ω/k^′ versus frequency, for the same Drude-Lorentz parameters as used in Fig. 1.

FIG. 8. Group velocity vg = (∂k^′/∂ω)^{−1} versus frequency, for the same Drude-Lorentz parameters as used in Fig. 1.

of the modified constitutive equations, called the Drude- Born-Fedorov model [10, 11], is as follows: D = ε[E + β ∇ × E], (14) B = μ[H + β ∇ × H], (15) where the electric permittivity ε(ω) is given in Eq. (6), and the magnetic permeability μ(ω) is given in Eq. (7). This form is symmetric under time-reversal. The pseudoscalar β, sometimes called the chiral admittance, has the units of length and is a measure of the optical activity. Let us consider a plane wave electromagnetic field, E(r, t) = Re[E(r, t)] = Re[E_0e^{i(k·r−ω t)}], and similarly for B(r, t), D(r, t) and H(r, t), and determine the consequences of Eqs. (14)-(15). Using the Faraday and Ampère laws in a nonconducting medium, ∇ × E = iωB, ∇ × H = −iωD, the Drude-Born-Fedorov equation in frequency space takes the form

D_0 = ε(ω) [E_0 + iωβ(ω)B_0] , (16) B_0 = μ(ω) [H_0 − iωβ(ω)D_0] .

These equations can be written in matrix form as ( E_0 H_0 ) = ( ε^{−1}(ω) −iωβ(ω) iωβ(ω) μ^{−1}(ω) ) ( D_0 B_0 ) . (17)

FIG. 9. Simulation of the electric field Ex(z, t) = Re[Ex(z, t)] of the plane wave propagating along the z-axis plotted versus z at five times, t = 0, 0.1, 0.2, 0.3, 0.4 (arb. units), where the period τ = 2π/ω = 1. Here we took ω = 3.8 (arb. units) and the same Drude-Lorentz parameters as used in Fig. 1, so n(ω) = −0.339 + 0.731i.

Substituting into the Faraday and Ampère equations gives

k × E_0 = ωB_0, k × H_0 = −ωD_0, (18)

which, upon writing k =^{ñ(ω)ω}_c k̂, can be written in terms of the refractive index as ñ(ω) c k̂ × (ε^{−1}D_0 − iωβB_0) = B_0, ñ(ω) c k̂ × (μ^{−1}B_0 + iωβD_0) = −D_0. (19)

Solving for ñ(ω) in the determinant obtained using these equations yields two degenerate solutions for the rightand left-handed circularly polarized light fields,

ñ(ω) ≡ n_±(ω) = n(ω) 1 ∓^{βω}_c n(ω) , (20)

where n(ω) is given in Eq. (8).

A. Non-resonant chiral admittance

In this subsection we consider a chiral medium containing impurity atoms with an electric dipole transition and impurity atoms with a magnetic dipole transition. The chiral admittance β of the chiral medium has resonances that are very far from the resonance frequencies of the atoms, so it is reasonable to take β as frequencyindependent [34]. In the next subsection we investigate the case where the chiral admittance has a resonance form [35–38].

Using a circular polarization basis we write

E_0 = E_+ e_+ + E_− e_−, (21)

FIG. 10. In a medium that is chiral, the real and imaginary parts of the complex refractive index n±(ω) versus ω (in arbitrary units) are different for right-circular polarization (solid curves) and left (dashed). The same Drude parameters as used in Fig. 1 are used here, and β = 0.02 (arb. units).

(similarly for D_0, B_0 and H_0) where the subscript ± refers to right-polarized (left-polarized) waves, e_+ = −1√ 2 ( x̂ + iŷ ) , and e_− =^{1√}_2 ( x̂ − iŷ ) . We find that

D_± = n_±(ω) n(ω) ε(ω)E_±, B_± = ∓ in_±(ω) c E_±,

H_± = ∓i √ |ε(ω)| |μ(ω)| e^{iθH} E_±. (22) The real part of the complex wavenumber of a circularly polarized wave is k^′_σ = ωn^′_σ(ω)/c, where σ = ±, and n^′_σ (ω) is the real part of n_σ(ω). The rotation angle of the polarization of linearly polarized light is given by θ_{rot} ≡ Re[Δn]l = (n^′_+ − n^′_−)l, where l is the length of the NR material traversed. Moreover, differential absorption Δα_± ≡ Im[Δn]ω/c = (n^{′′}_+ − n^{′′}_−)ω/c (i.e.,the circular dichroism) ensues, hence the light will generally be elliptically polarized upon propagation through the material, and θ_{rot}(ω) will be the rotation of the major and minor axes.

Figure 10 plots the real (magenta) and imaginary (black) parts of n_±(ω) versus ω for right-circular polarized (+) (solid curves) and left-circular polarized (−) light (dashed curves). The resonance frequency and the entire curves for the complex refractive index are shifted to higher (lower) frequencies for the right-circular polarized (left-circular polarized) light in the chiral medium (finite β) relative to those in Fig. 2 (which is for β = 0). Moreover, both Re(n_+) and Im(n_+) are smaller in magnitude than Re(n_−) and Im(n_−), respectively. Both Re(n_+) and Re(n_−) have regions of NR, and these regions partly overlap. Both Im(n_±) are positive (absorptive) for all frequencies. The absorption of both right and left circular polarized light have minima near ω ≈ 3.8.

Figure 11 plots the circular birefringence Re[Δn(ω)] = n^′_+(ω) − n^′_−(ω), which is promotional to the polarization rotation angle θ_{rot}(ω) = [n^′_+rot(ω) − n^′_−rot(ω)]l ver-

FIG. 11. In a chiral medium, the real and imaginary parts of the complex refractive index n±(ω) versus ω (in arbitrary units) are different for right-circular polarization (solid curves) and left (dashed). The same Drude-Born-Fedorov parameters are used here as in Fig. 10.

sus frequency, and the circular dichroism Im[Δn(ω)] = n^{′′}_+(ω) − n^{′′}_−(ω), which is proportional to the differential absorption Δα(ω) ≡ (n^{′′}_+(ω) − n^{′′}_−(ω))ω/c versus frequency. Both the circular birefringence and the circular dichroism change sign as a function of frequency near the resonance, but the real part changes sign twice whereas the imaginary part changes sign only once. For frequencies larger than ω ≈ 3.8, both the circular birefringence and the circular dichroism are very small (the solid and dashed curves in Fig. 10 are very close to overlapping).

The possibility of obtaining negative refraction in a chiral medium due to a resonance in the permittivity only (and not in the permeability) was first suggested by Pendry [39]; see also Refs. [40, 41]. This can be understood from Eq. (20) by noting that if the real part of the second term in the denominator is larger than unity, n_+ would be negative (while n_− would be positive). In Fig. 10 we see that there are frequency ranges where both n_+ and n_− are negative due to the resonance structure of ε and μ. The resonance in n_+ occurs at smaller frequency than the resonance in n_−.

The Poynting vector is given by

S_±(ω) = k̂ √ |ε(ω)| |μ(ω)| E^2_± 2 cos θ_H e^{−2k′′σ z}. (23) Since |θ_H | ≤ π/2, S_± points in the k̂ direction. Note that the energy flux density^{S±}_{e−2k}′′_{σ z} does not depend on r or t (as opposed to the non-time averaged achiral case). The Poynting vector^{S±(ω)}_{E 2±e−2k}′′_{σ z} , is independent of the polariza-

tion σ and the chiral admittance β, there is no need to present a figure for this case since the results are identical to Fig. 4 which shows the average energy flux density S̄ obtained in the achiral case discussed in Sec. II.

Following a similar line of reasoning as used by Jackson [24] for the achiral case, we find that the energy density u_± and the power dissipation density Q_± are given by

FIG. 12. In a chiral medium, the phase velocities vp,±(ω) versus ω are different for right-circular polarization (solid curves) and left (dashed). The same Drude-Born-Fedorov parameters are used here as in Fig. 10.

[42]

u_± = 1 16π { d [ ωε̃^′(ω)] dω | |E_±(ω) | |^2 + d [ ωμ̃^′(ω)] dω | |H_±(ω) | |^2

+2 d [ ω^2β̃^′(ω)] dω Im [ H_±(ω) · E^∗_±(ω) ] }

= | |E_±(ω) | |^2 16π { d [ ωε̃^′(ω)] dω + d [ ωμ̃^′(ω)] dω | | | ε(ω) μ(ω) | | |

∓2 d [ ω^2β̃^′(ω)] dω Re [√ ε(ω) μ(ω) ]} , (24)

Q_± = ω 8π { ε̃^{′′}(ω) | |E_±(ω) | |^2 + μ̃^{′′}(ω) | |H_±(ω) | |^2

+2ωβ̃^{′′}(ω) Im [ H_±(ω) · E^∗_±(ω) ]}

= ω | E_±(ω) |_2 8π { ε̃^{′′}(ω) + μ̃^{′′}(ω) | | | ε(ω) μ(ω) | | |

∓2 ωβ̃^{′′}(ω) Re [√ ε(ω) μ(ω) ]} . (25)

Note that circularly polarized light has a constant magnitude, hence time-averaging the energy density and power dissipation density is not necessary when a circular polarization basis is used (unlike the linearly polarization basis used in the achiral section).

In the limit β → 0, the phase velocities v_{p,σ} (ω) and group velocities v_{p,σ} (ω) go to the achiral ones, and, as already stated, the energy flux density and the energy density go to the achiral average energy flux density and the average energy density, respectively.

The phase velocity is v_{p,σ} (ω) = ω/k^′_σ =^c_{n′σ (ω)} , and the group velocity is v_{g,σ} (ω) = (∂k^′_σ/∂ω)^{−1} = c n^′_σ (ω)+ω∂_ω n^′_σ (ω) . Figure 12 plots the phase velocities

v_{p,±}(ω) versus ω and Fig. 13 plots the group velocities v_{g,±}(ω). The resonance behavior of the phase and group

FIG. 13. In a medium that is chiral, the phase velocities vg,±(ω) versus ω are different for right-circular polarization (solid curves) and left (dashed). The same Drude-Born- Fedorov parameters are used here as in Fig. 10.

velocities are similar to the achiral case; the phase velocities have two resonances and the group velocities have four. The SM notebook [26] allows you vary the β parameter (and other parameters) to see the dramatic changes in the frequency dependence of θ_{rot}(ω), Δα_± and other quantities such as the phase and group velocities.

Figure 14 plots u_+(ω) and u_−(ω) versus frequency. The right and left polarization curves are hard to distinguish but the inset plots the difference Δu_±(ω) =

u_+(ω)(ω) E^2_+e^{−2k′′+ z} −^{u− (ω)(ω)} E^2_−e^{−2k′′− z} . Figure 15 shows the power dis-

sipation density Q_±(ω) versus ω for right-circular (red) and left-circular polarization (dashed blue). The power dissipation is always positive, and resonance behavior has two local maxima in this case, and the difference ΔQ_±(ω) =^{Q+(ω)(ω)} E^2_+e^{−2k′′+ z} −^{Q−(ω)(ω)} E^2_−e^{−2k′′− z} = 0 for all frequencies

if β is real (as we shall see in Sec. IV B, for complex β, ΔQ_±(ω) is in general not zero).

FIG. 14. In a chiral medium, the energy density u±(ω) versus ω for right-circular (red) and left-circular polarization (dashed blue). The same Drude-Born-Fedorov parameters are used here as in Fig. 10. The inset shows the difference Δu±(ω) = u+(ω)(ω) E2+e−2k ′′ σ z −^{u−(ω)(ω)} E2−e−2k ′′ σ z .

FIG. 15. In a chiral medium, the power dissipation density Q±(ω) versus ω for right-circular (red) and left-circular polarization (dashed blue). The difference ΔQ±(ω) =^{Q+(ω)(ω)}_{E2+ e−2k′′σ z} − Q−(ω)(ω) E2−e−2k ′′ σ z is identically zero. The same Drude-Born-Fedorov

parameters are used here as in Fig. 10.

Finally, Fig. 16 shows the electric field E(z, t) of a plane wave propagating along the z-axis plotted versus z (in the SM [26] you can run a movie which shows the time-dependence of E(z, t), and you can also change the material parameters). The light field at z = 0 is linearly polarized (see orange line at the front face of the material in the figure). The polarization becomes elliptical as the field propagates in z. The electric field can be represented as

E(z, t) = 2^{−1/2}E_0Re[(−e_+e^{ik+ z} + e_−e^{ik− z})e^{−iωt}]. (26)

In addition to the electric field inside the material, the linear polarization of the incident field at the front face of the medium is determined by the intersection of the blue curve with the orange line at the front face, and the polarization ellipse of the field at z = z_{max} is shown at the back face as the intersection of the blue curve with the green line and the orange ellipse. To better understand the plane wave polarization dynamics, the reader is strongly encouraged to use the Manipulate command in the SM [26].

B. Resonant chiral admittance

The chiral admittance β(ω) can be frequency dependent [35, 36]; it can even have a resonance form (that can be modeled by a Lorentzian function) [37, 38], β(ω) = c ω_{pβ} ω^2 − ω^2_{0β} + iωγ_β

. (27)

Here ω_{0β} is the resonance frequency, γ_β is the resonance width, and ω_{pβ} is the chiral admittance strength parameter. We use a model similar to Ref. [35] wherein we have a chiral medium which has an electric dipole transition with susceptibility χ_β (ω) having resonance frequency ω_{0β}

FIG. 16. The electric field E(z, t) of the plane wave (26) propagating along the z-axis plotted as a function of z for t = 0. The orange line at the front face of the material shows the linear polarization of the incident light. The intersection of the blue curve with the orange line gives the instantaneous polarization at t = 0. The orange ellipse shows the polarization states of the light at the back face of the material as a function of time, and the intersection of the blue curve with the orange ellipse gives the instantaneous polarization at t = 0. The same Drude-Born-Fedorov parameters are used here as in Fig. 10. In the SM [26] you can run a movie showing the time-dependence of the polarization.

that results in a contribution to the permittivity with resonance frequency ω_{0β} and resonance width γ_β , and the chiral medium has impurity atoms. The impurity atoms have resonant electric susceptibility χ(ω) = ε(ω)/ε_0 − 1, where ε(ω) is given in Eq. (6). Furthermore, the chiral medium (without impurity atoms) has susceptibility

χ_b(ω) = − ω^2_{pb} ω^2 − ω^2_{0β} + iωγ_β

, (28)

where ω_{pb} is a plasma frequency of the medium without impurity atoms. The total permittivity of the chiral medium with impurity atoms is

ε̃(ω) = ε_0 [1 + χ(ω) + χ_β(ω)]. (29)

The permeability μ(ω) of impurity atoms is given in Eq. (7). Note that if ω_{0β} is of the same order of magnitude as ω_0 and ω_{0m}, the optical characteristics of the resonant chiral materials can be very different than the constant β case. Specifically, if ω is close to ω_{0β} , the chiral admittance can be large. Appendix A discusses the conditions that restrict the parameters appearing in the resonance chiral admittance given in Eq. (27).

Figure 17 shows the real and imaginary parts of the refractive index in Eq. (20), with β on the right hand

FIG. 17. Refractive index for a medium with resonant chiral admittance. The real and imaginary parts of the complex refractive index n±(ω) versus ω (in arbitrary units) are different for right-circular polarization (solid curves) and left (dashed). The same Drude parameters for ε and μ as used in Fig. 1 are used here, and the parameter for β(ω) are ω_{0β} = 3.3, ω_{pβ} = 0.4, γ_β = 4.3.

FIG. 18. Blowup of the ordinate in Fig. 17 showing the real and imaginary parts of n−(ω) versus frequency.

side of the equation replaced by β(ω) given by Eq. (27) for a medium with a resonance in the chiral admittance very close to the resonance frequencies of the permittivity and permeability. The right circularly polarized light has huge n^′_+(ω) which changes sign at ω ≈ 3.15 and a gigantic n^{′′}_+(ω) (hence absorption) with a maximum at the same frequency. For left circularly polarized light, both n^′_−(ω) and n^{′′}_−(ω) cannot be seen on the ordinate scale of the figure, therefore we plot these quantities in Fig. 18. The refractive index n^′_−(ω) is negative in the frequency region 3.12 < ω < 3.98, and the absorption has a maximum at ω ≈ 3.03. Comparing the refractive index here with that shown in Fig. 10 for the non-resonance β case, we see that the scale of the right-circularly polarized refractive index is roughly two orders of magnitude larger here, but the left-circularly polarized refractive index is the same order of magnitude here.

Figure 19 shows the energy densities u_±(ω) versus ω for right-circularly and left-circularly polarized light. There are two maxima and one minimum in the energy density. In comparing with the energy density in Fig. 14 we see that again there is a region where the energy density is negative, but the shape of the energy density curve as a function of frequency is very different here. Because of the resonance in β, the minimum is three orders of magnitude deeper than in the non-resonance case. The inset shows that Δu(ω) =^{u+(ω)(ω)}_{E 2+e−2k}′′_{+ z} −^{u−(ω)(ω)}_{E 2−e−2k}′′_{− z} is four

orders of magnitude larger than the non-resonant β case.

FIG. 19. Energy density u±(ω) versus ω for right-circular (red) and left-circular polarization (dashed blue) for a chiral medium with resonant β(ω). The inset shows a blowup of difference Δu±(ω) =^{u+(ω)(ω)} E2+ e−2k ′′ σ z −^{u−(ω)(ω)} E2− e−2k ′′ σ z . The same Drude-

Born-Fedorov parameters as used in Fig. 17 are used here.

FIG. 20. In a chiral medium with resonant β(ω), the power dissipation densities Q±(ω) versus ω for right-circular (red) and left-circular polarization (dashed blue). The difference ΔQ±(ω) =^{Q+(ω)(ω)} E2+e−2k ′′ σ z −^{Q−(ω)(ω)} E2−e−2k ′′ σ z is very small and positive in

this case; the difference is largest at ω ≈ 3.152 where ΔQ± = 4.05. The same Drude-Born-Fedorov parameters as used in Fig. 17 are used here.

Figure 20 shows the power dissipation densities Q_±(ω) versus ω. The maxima for Q_±(ω) occur at ω ≈ 3.152, but the Q_+(ω) maximum is a little larger and at a slightly higher frequency that for Q_−(ω). The power dissipation densities here are roughly a factor of 40 larger than for the non-resonant β case shown in Fig. 15.

V. SUMMARY

We calculated the complex ε, μ and refractive index n versus frequency using a Drude-Lorentz model for a material having electric dipole and magnetic dipole transition resonances that are near one another, using the amplitude-phase representation for complex functions in Eq. (8) to define √ εμ. We then evaluated the phase velocity, group velocity, Poynting vector (energy flux density), energy density and power dissipation density, and discussed their surprising behavior for frequencies near the resonances. We then treated chiral media using the Drude-Born-Fedorov model. The circular polarized representation used to treat the chiral case determines the optical rotation activity and circular dichroism of the light given incident linearly polarized light, and yields the Poynting vector (energy flux density) and energy density which are independent of position and time (this is true for the time-averaged quantities in the achiral case too). In the limit as the chiral admittance β → 0, the energy flux density and energy density are identical to the temporally averaged energy flux density and energy density calculated with the linear polarized representation in the achiral case. We then considered the case when the chiral admittance β depends on frequency and has a resonance near the resonance frequencies of the permittivity and permeability of the media, and saw that the results can vary dramatically from those obtained when the chiral admittance is almost constant near the resonance frequencies of the permittivity and permeability. We intend to generalize the theory to treat non-isotropic condensed matter systems in a future publication.

Appendix A: Conditions on the parameters appearing in the resonant chiral admittance

Let us now consider a medium without any impurity atoms in order to determine the conditions the restrict the parameter values appearing in β(ω). The electric susceptibility of the medium is given in Eq. (28), the medium permittivity is ε_b(ω) = ε_0(1 + χ_b(ω)), and the chiral admittance is given by Eq. (27). The refractive index of the chiral medium without impurity atoms is n_{b±}(ω) = n_b(ω) 1 ∓^{β(ω) ω}_c n_b(ω)

. (A1)

where

n_b(ω) = √ ε_b(ω). (A2)

The imaginary part of the refractive index must be positive, n^{′′}_{β±}(ω) ≥ 0, which implies

n^{′′}_b (ω) > ω β^{′′}(ω) |n_b(ω)|^2. (A3)

Assuming that γ_β is large, γ_β ≫ ω_{oβ}, and applying the condition (A3) to the range ω ≪ γβ we get the inequality

ω_{pβ} < ω^2_{pb} 2ω . (A4)

This inequality is satisfied in the frequency range ω < ω_{max} = ω^2_{pb}/(2ω_{pβ}). On the other hand, when ω_{max} ≫ ω_{0β}, ω^2_{pb} 2ω_{pβ} ≫ ω_{0β} .

[1] V. G. Veselago, “The electrodynamics of substances with simultaneously negative values of ε and μ”. Soviet Physics Uspekhi 10, 509 (1968).

[2] J. B. Pendry, D. R. Smith, “Reversing Light With Negative Refraction”, Physics Today 57, 37 (2004).

[3] D. R. Smith, J. B. Pendry, M. C. K. Wiltshire, “Metamaterials and Negative Refractive Index’, Science 305, 788 (2004).

[4] J. B. Pendry, D. Schurig, D. R. Smith, “Controlling Electromagnetic Fields”, Science 312, 1780 (2006).

[5] V. Veselago, L. Braginsky, V. Shklover, C. Hafner, “Negative Refractive Index Materials”, J. Computat. Theor. Nanosci. 3, 1 (2006).

[6] C. M. Krowne, Y. Zhang (Eds.), Physics of Negative Refraction and Negative Index Materials, (Springer, Berlin, 2007), see for example, p. 357, Fig. 12.15.

[7] G. V. Eleftheriades, K. G. Balmain (Eds.), Negative- Refraction Metamaterials, Fundamental Principles and Applications, (John Wiley & Sons, Hoboken, 2005). See the paper by D. Schurig and D. R. Smith, “Negative Index Lenses”, Chapter 5, p. 221, after Eq. (5.15).

[8] S. A. Ramakrishna, T. M. Grzegorczyk (Eds.), Physics and Applications of Negative Refractive Index Materials, (CRC Press, Boca Raton, 2009), see for example, p. 121, Fig. 3.21.

[9] F. Capolino (Ed.), Theory and Phenomena of Metamaterials (CRC Press, Boca Raton, 2009). See for example the paper by C-W Qiu, S. Zouhdi and A. Sihvola, “A Review of Chiral and Bianisotropic Composite Materials Providing Backward Waves and Negative Refractive Indices”; Section 24.2 states: “In order to realize the negative refraction [16, 17], the composite material must have effective permittivity and permeability that are negative over the same frequency band. When the real parts of permittivity and permeability possess the same sign, the electromagnetic waves can propagate.”

[10] P. Drude, Lehrbuchder Optik, (S.Hirzel, Leipzig, 1912);

H. Lorentz, “The motion of electrons in metallic bodies I”. KNAW, Proceedings. 7, 438-453 (1905).

https://dwc.knaw.nl/DL/publications/PU00013989.pdf.

[11] M. Born, Optik, Ein Lehrbuch der Elektromagnetischen Lichttheorie, (Springer, Heidelberg, 1933); F. I. Fedorov, “The Theory of the Optical Activity of Crystals”, Sov. Phys. Usp. 15, 849 (1973).

[12] R. W. Ziolkowski and E. Heyman, “Wave propagation in media having negative permittivity and permeability”, Phys. Rev. E64, 056625 (2001).

[13] M. W. McCall1, A. Lakhtakia and W. S. Weiglhofer, “The negative index of refraction demystified”, Eur. J. Phys. 23 353 (2002).

[14] C-Y Chen, M-C Hsu, C. D. Hu, Y C. Lin, “Natural Negative-Refractive-Index Materials”, Phys. Rev. Lett. 127, 237401 (2021).

[15] J. B. Pendry, “Negative Refraction Makes a Perfect Lens”, Phys. Rev. Lett. 85, 3966 (2000).

[16] X. Zhang, Z. Liu, “Superlenses to overcome the diffraction limit”, Nature Materials 7, 435 (2008).

[17] U. Leonhardt, T. Philbin, Geometry and Light: The Science of Invisibility, Dover Books on Physics (Dover, 2010).

[18] M. Kim and J. Rho, “Metamaterials and imaging”, Nano Convergence 2, (2015). DOI 10.1186/s40580-015-0053-7.

[19] F. Ling, Z. Zhong, R. Huang and B. Zhang, “A broadband tunable terahertz negative refractive index metamaterial”, Sci. Rep. 8, 9843 (2018).

[20] G. V. Eleftheriades, A. Grbic, and M. Antoniades, “Negative-refractive-index metamaterials and enabling electromagnetic applications”, Proc. IEEE Int. Symp. Antennas and Propagation 2, 1399-1402 (2004).

[21] R. W. Ziolkowski and A. D. Kipple, “Application of double negative materials to increase the power radiated by electrically small antennas”, IEEE Trans Antennas and Propagation 51, 2626-2640, (2003).

[22] A. Rennings, S. Otto, C. Caloz, and P. Waldow, “Enlarged half-wavelength resonator antenna with enhanced gain”, Proc. IEEE Int. Symp. Antennas and Propagation 3A, 683 (2005).

[23] C. J. F. Böttcher, “Theory of Electric Polarization”, (Elsevier, 1973); A. Lakhtakia, Selected papers on linear optical composite materials. Bellingham, Wash., USA: SPIE Optical Engineering Press (1996). See also

https://en.wikipedia.org/wiki/Clausius%E2%80%93Mossotti_relation.

[24] J. D. Jackson, Classical Electrodynamics, 3rd Ed., (John Wiley & Sons, Hoboken, 1999), Eqs. (6.126a) and (6.126b).

[25] Quantum mechanical treatments include the transition electric dipole moment of the transition divided by the Bohr radius, d/a0, to give ε(ω) = ε0(1 + χ(ω)) = 1 − ω2p(d2/a20) ω2−ω20 +iγω . Often one incorporates the factor d

2/a^2_0 into

the plasma frequency as follows: ω^2_p =^{Ne2 (d2 /a20)}_{ε0m} . [26] The supplementary material contains the Mathematica notebook Negative-refractive_index.nb.

[27] Shivanand, and K. J. Webb, “Electromagnetic field energy density in homogeneous negative index materials”, Opt. Express 20, 11370 (2012).

[28] G. M. Gehring, A. Schweinsberg, C. Barsi, N. Kostinski and R. W. Boyd, “Observation of Backward Pulse Propagation Through a Medium with a Negative Group Velocity”, Science 312, 895 (2006).

[29] G. Dolling, C. Enkrich, M. Wegener, C. M. Soukoulis and S. Linden, “Simultaneous Negative Phase and Group Velocity of Light in a Metamaterial”, Science 312, 892 (2006).

[30] B. Segev, P. W. Milonni, J. F. Babb and R. Y. Chiao, “Quantum noise and superluminal propagation”, Phys. Rev. A 62, 022114 (2000).

[31] R W. Boyd and D J. Gauthier, “Controlling the Velocity of Light Pulses”, Science 326, 1074 (2009).

[32] M. S. Bigelow, N. N. Lepeshkin, H. Shin and R. W.

Boyd, “Propagation of smooth and discontinuous pulses through materials with very large or very small group velocities”, J. Phys.: Condens. Matter 18, 3117 (2006).

[33] A. Schweinsberg, N. N. Lepeshkin, M. S. Bigelow, R. W.

Boyd, and S. Jarabo, “Observation of superluminal and slow light propagation in erbium-doped optical fiber”, Euro. Phys. Lett. 73, 218 (2006).

[34] V. V. Varadan, R. Ro, and V. K. Varadan, “Measurement of the electromagnetic properties of chiral composite materials in the 8-40 GHz range”, Radio Science 29, 9 (1994).

[35] E. U. Condon, “Theories of Optical Rotatory Power” Rev. Mod. Phys. 9, 432 (1937).

[36] M C K Wiltshire, J. B. Pendry and J. V. Hajnal, J. Phys.:

Condens. Matter 21 292201, (2009).

[37] R. Zhao, T. Koschny and C. M. Soukoulis, “Chiral metamaterials: retrieval of the effective parameters with and without substrate”, Optics Express 18, 14553 (2010).

[38] S. S. Oh and O. Hess, “Chiral metamaterials: enhancement and control of optical activity and circular dichroism”, Nano Convergence 2, 24 (2015).

[39] J. B. Pendry, “A Chiral Route to Negative Refraction”, Science 306, 1353-1355 (2004).

[40] C. Monzon and D. W. Forester, “Negative Refraction and Focusing of Circularly Polarized Waves in Optically Active Media”, Phys. Rev. Lett. 95, 123904 (2005).

[41] S. Tretyakov, A. Sihvola, L. Jylhä, “Backward-wave regime and negative refraction in chiral composites”, Photonics and Nanostructures–Fundamentals and Applications 3, 107-115 (2005).

[42] The energy density expression here differs from that in L.

V. Poulikakos, P. Gutsche, K. M. McPeak, S. Burger, J. Niegemann, C. Hafner, D. J. Norris, “Optical Chirality Flux as a Useful Far-Field Probe of Chiral Near Fields”, ACS Photonics 3, 1619 (2016). The expression used here includes dispersion terms for the permittivity and permeability that are not included in this reference.