arXiv:2309.00808v1 [physics.acc-ph] 2 Sep 2023

POTENTIAL-WELL BUNCH LENGTHENING IN ELECTRON STORAGE RINGS

Demin Zhou^∗, Gaku Mitsuka, Takuya Ishibashi, KEK Accelerator Laboratory, 1-1 Oho, Tsukuba 305-0801, Japan Karl Bane, SLAC National Accelerator Laboratory, Menlo Park, California 94025, USA

Abstract

The cubic equation derived by B. Zotter has been popularly used for electron storage rings to describe the scaling law of potential-well bunch lengthening. This equation has also often been used to calculate the effective impedance when the bunch lengthening is measured or simulated. This paper discusses the validity of Zotter’s equation and presents an alternative but self-consistent equation for potential-well bunch lengthening. Its applications to predicting bunch lengthening and extracting effective impedance from bunch length measurements are also addressed.

INTRODUCTION

Individual electrons oscillate around a fixed point in the longitudinal phase space in electron storage rings. The RF system creates a potential well that confines the beam in a bucket. When the oscillations are of small amplitude, the motion of the electrons is linear. Using the longitudinal coordinate 𝑧 and momentum deviation 𝛿, the linear equations of motion are [1] 𝑑𝑧 𝑑𝑠 = −𝜂𝛿, 𝑑𝛿 𝑑𝑠 = − 𝑒𝑉_{rf}𝜔_{rf} cos 𝜙_s 𝐸𝐶𝑐 𝑧. (1)

The following quantities are used: the electron charge 𝑒, the speed of light 𝑐, the slip factor 𝜂, the RF voltage 𝑉_{rf}, the RF frequency 𝜔_{rf}, the electron energy 𝐸, the circumference of the ring 𝐶 and the synchronous phase 𝜙_s. We assume that the reference particle is moving at the speed of light, 𝑐. In the presence of radiation damping and quantum excitation, the beam reaches a stable equilibrium distribution in the longitudinal phase space, which is Gaussian [2]. The momentum spread 𝜎_{𝛿0} in an electron storage ring at equilibrium is determined by the beam energy and the bending radii of the dipole magnets but is not affected by the RF parameters 𝑉_{rf} and 𝜔_{rf} (see Eq. (7.94) of [1]). Radiation effects cause the beam to bunch, with an rms length of 𝜎_{z0} = −𝑐𝜂𝜎_{𝛿0}/𝜔_{z0}. From Eqs. (1), the synchrotron frequency 𝜔_{z0} is defined by

𝜔_{z0} ≡ sgn[𝜂] � − 𝑒𝑐𝑉_{rf}𝜂𝜔_{rf} cos 𝜙_s 𝐸𝐶 , (2)

where sgn[] is the sign function. We define 𝜔_{z0} to have the opposite sign of 𝜂 (this is the choice of the SAD code [3]) so that 𝜎_{z0} is always positive.

The longitudinal wakefields deform the potential well created by the RF system. As a result, the equations of motion

∗ dmzhou@post.kek.jp

are modified to: 𝑑𝑧 𝑑𝑠 = −𝜂𝛿, 𝑑𝛿 𝑑𝑠 = 𝜔^2_{z0} 𝜂𝑐^2 𝑧 − 𝐹(𝑧, 𝑠). (3)

The wakefield term 𝐹(𝑧, 𝑠) is calculated from the convolution of charge density and longitudinal wake function

𝐹(𝑧, 𝑠) = 𝐼_𝑛

∫_∞ −∞ 𝑊_‖ (𝑧 − 𝑧^′)𝜆(𝑧^′, 𝑠)𝑑𝑧^′, (4)

with the scaling factor 𝐼_𝑛 = 𝑁𝑒^2/(𝐸𝐶) = 𝐼_𝑏/(𝑐(𝐸/𝑒)), the line density distribution 𝜆(𝑧, 𝑠), and the wake function 𝑊_‖ (𝑧). Here, 𝑁 is the bunch population, and 𝐼_𝑏 = 𝑁𝑒/(𝐶/𝑐) is the bunch current. The wake function and the corresponding impedance are Fourier transforms of each other: 𝑊_‖ (𝑧) =^𝑐_{2𝜋}

∫_∞ −∞ 𝑍_‖ (𝑘)𝑒^{𝑖𝑘𝑧} 𝑑𝑘 and 𝑍_‖ (𝑘) = 1 𝑐 ∫_∞ −∞ 𝑊_‖ (𝑧)𝑒^{−𝑖𝑘𝑧} 𝑑𝑧 with 𝑘 ≡ 𝜔/𝑐. Using the impedance, 𝐹(𝑧, 𝑠) can be rewritten as

𝐹(𝑧, 𝑠) = 𝑐𝐼_𝑛 2𝜋 ∫_∞ −∞ 𝑑𝑘𝑍_‖ (𝑘)𝜆̃(𝑘, 𝑠)𝑒^{𝑖𝑘𝑧} , (5)

with the beam spectrum 𝜆̃(𝑘, 𝑠) =

∫_∞ −∞ 𝜆(𝑧, 𝑠)𝑒^{−𝑖𝑘𝑧} 𝑑𝑧.

Since 𝑊_‖ (𝑧) and 𝜆(𝑧, 𝑠) are real, the reality condition applies: 𝜆̃^∗ (𝑘, 𝑠) = 𝜆̃(−𝑘, 𝑠) and 𝑍^∗_‖ (𝑘) = 𝑍_‖ (−𝑘).

THE CUBIC EQUATION FOR BUNCH LENGTHENING

In [4], Zotter solved the equations of motion for a single particle as described by Eqs. (3). The leading-order perturbation from the longitudinal wakefields was found to shift the incoherent synchrotron frequency. For electron storage rings, Eq. (5.10) of [4] is of interest to us:

𝜔^2_z = 𝜔^2_{z0} (1 − 𝜉𝑍_1) , (6)

with 𝜉 = 𝜂𝜔^2_0𝐼_𝑏/(2𝜋𝜔^2_{z0}(𝐸/𝑒)) and

𝑍_1 (𝜎_z) = − √ 2𝜋𝑐^3 𝜔^3_0𝜎^3_z Im � 𝑍_‖ 𝑛 �_{𝑚=1} eff . (7)

Here 𝜔_z is the incoherent synchrotron frequency after bunch lengthening, 𝜎_z is the rms length of the lengthened bunch, 𝜔_0 = 2𝜋𝑐/𝐶 is the revolution frequency, and � 𝑍_‖ /𝑛

�_{𝑚=1} eff is the effective impedance for azimuthal mode 𝑚 = 1. The effective impedance is a quantity used in collective instability theories [5]. It is defined as follows: � 𝑍_‖ 𝑛 �_𝑚 eff = ∞� 𝑝=−∞

𝑍_‖ ( 𝜔_{𝑚𝑝} )

𝑝 ℎ_𝑚 (𝜔_{𝑚𝑝}) ∞� 𝑝=−∞

ℎ_𝑚 (𝜔_{𝑚𝑝})

, (8) where 𝑛 = 𝜔/𝜔_0, 𝜔_{𝑚𝑝} = 𝑝𝜔_0 + 𝑚𝜔_z the mode frequencies. The power density of the 𝑚-th mode is defined as

ℎ_𝑚 (𝜔) = 𝜆̃_𝑚 (𝜔) · 𝜆̃^∗_𝑚 (𝜔), (9)

with 𝜆̃_𝑚 (𝜔) the Fourier transform of the line density of the 𝑚-th azimuthal mode. It was suggested in [4] that, when using Eq. (8) to calculate 𝑍_1, 𝜔_{𝑚𝑝} should be evaluated with 𝜔_z = 0.

Usually, the ring length is much larger than the bunch length, suggesting that the sampling frequency step 𝜔_0 in Eq. (8) is much smaller than the typical frequency of the beam spectrum, that is, 𝑐/𝜎_{z0}. With this condition, the summations over 𝑝 in Eq. (8) can be fairly replaced by integrals, yielding � 𝑍_‖ 𝑛 �_𝑚 eff = ∫_∞ −∞ 𝑍_‖ (𝜔)^{𝜔0}_𝜔 ℎ_𝑚 (𝜔)𝑑𝜔 ∫_∞ −∞ ℎ_𝑚 (𝜔)𝑑𝜔

. (10)

For a Gaussian bunch, the power densities ℎ_𝑚 (𝜔) for 𝑚mode is given by

ℎ_𝑚(𝜔) = (𝜔𝜎_z/𝑐)^{2𝑚}𝑒^{−𝜔2 𝜎2z /𝑐2} . (11)

For the case of potential-well bunch lengthening, 𝜎_z can be replaced by 𝜎_{z0} so that � 𝑍_‖ /𝑛

�_{𝑚=1} eff is a constant machine parameter independent of the bunch current. Note that the effective impedance depends on the beam properties, but the original impedance 𝑍_‖ (𝜔) only depends on the beam’s surroundings [5].

For electron storage rings, the energy spread is constant below the microwave instability threshold, resulting in

𝜎_z𝜔_z = 𝜎_{z0}𝜔_{z0} = −𝑐𝜂𝜎_{𝛿0}. (12)

Combining Eqs. (6) and (12), we arrive at Zotter’s cubic equation for potential-well bunch lengthening:

𝑥^3 − 𝑥 + 𝑐𝐼_𝑏 𝜅𝜂𝜔_0𝜎_{z0}𝜎^2_{𝛿0} (𝐸/𝑒) Im � 𝑍_‖ 𝑛 �_{𝑚=1} eff = 0, (13)

where 𝑥 = 𝜎_z/𝜎_{z0} and 𝜅 = √ 2𝜋. Note that from Eq. (6) to Eq. (13), 𝜉𝑍_1 (𝜎_z) is replaced by 𝜉𝑍_1 (𝜎_{z0})/𝑥^3.

There are alternative ways of deriving the cubic equation similar to Eq. (13) (for example, see Refs. [5–7]). Here, we present a simple way that does not need the effective impedance defined by Eq. (8). From Eqs. (3), we can obtain the second-order differential equation of longitudinal coordinate as

𝑑^2𝑧 𝑑𝑠^2 = − 𝜔^2_{z0} 𝑐^2 𝑧 + 𝜂𝐹(𝑧, 𝑠) (14)

We assume the incoherent synchrotron frequency with wakefield perturbation is given by

𝑑^2𝑧 𝑑𝑠^2 = − 𝜔^2_z 𝑐^2 𝑧. (15)

To find the explicit form of 𝜔_z, we can approximate 𝐹(𝑧, 𝑠) by taking the leading term that is linear to 𝑧. To do so, we take the derivative over 𝑧 on the right side of Eq. (5) and then average over the line density:

𝐹_1 =

∫_∞ −∞ 𝑑𝑧𝜆(𝑧, 𝑠)

𝜕𝐹(𝑧, 𝑠) 𝜕𝑧 = 𝑖𝑐𝐼_𝑛 2𝜋 ∫_∞ −∞ 𝑑𝑘𝑘𝑍_‖ (𝑘)𝜆̃(𝑘, 𝑠)𝜆̃^∗ (𝑘, 𝑠).

(16)

From the reality condition of the impedance and beam spectrum, it follows that only the imaginary part of 𝑍_‖ (𝑘) contributes to 𝐹_1. Taking a Gaussian bunch and pure inductive impedance 𝑍_‖ (𝑘) = −𝑖𝑘𝑐𝐿, one can obtain

𝐹_1 = 𝑐𝐼_𝑛 2𝜋 √ 𝜋𝑐𝐿 2𝜎^3_z

. (17)

Alternatively, for an absolute impedance, the effective inductance can be defined as follows [8]:

𝐿_{eff} = 1 𝑐 ∫_∞ −∞ 𝑑𝑘𝑘𝑍_‖ (𝑘)𝜆̃(𝑘, 𝑠)𝜆̃^∗ (𝑘, 𝑠) ∫_∞ −∞ 𝑑𝑘𝑘^2𝜆̃(𝑘, 𝑠)𝜆̃^∗ (𝑘, 𝑠)

. (18)

For a Gaussian bunch, it becomes

𝐿_{eff} =

2𝑖𝜎^3_z √ 𝜋𝑐 ∫_∞ −∞ 𝑑𝑘𝑘𝑍_‖ (𝑘)𝜆̃(𝑘, 𝑠)𝜆̃^∗ (𝑘, 𝑠), (19)

which is equivalent to

𝐿_{eff} = − 1 𝜔_0 Im � 𝑍_‖ 𝑛 �_{𝑚=1} eff (20)

with the effective impedance calculated by Eqs. (10) and (11). The concept of effective inductance was first introduced by K. Bane in [8].

If we replace 𝐹(𝑧, 𝑠) with 𝐹_1𝑧 in Eq. (14) and compare the resulting equation with Eq. (15), we can obtain

𝜔^2_z 𝑐^2 = 𝜔^2_{z0} 𝑐^2 − 𝑐^2𝜂𝐼_𝑛 𝐿_{eff} 4 √ 𝜋𝜎^3_z

. (21)

Using the relation given in Eq. (12), we arrive at a cubic equation of bunch lengthening factor 𝑥:

𝑥^3 − 𝑥 − 𝑐𝐼_𝑏 𝜅𝜂𝜎_{z0}𝜎^2_{𝛿0} (𝐸/𝑒)

𝐿_{eff} = 0, (22)

with 𝜅 = 4 √ 𝜋. It can be seen that Eqs. (13) and (22) are identical except for the constant 𝜅 in the denominator. We conclude that the factor of √ 2𝜋/(𝜔_0𝜏)^3 for 𝑍_1 in Eq. (5.9) of [4] is incorrect and should be replaced by √ 𝜋/(2(𝜔_0𝜏)^3).

This conclusion will be justified in the following section.

The cubic equations (13) and (22) have been widely used in electron storage rings. During the design and construction phases, an impedance database can be created and used to calculate the effective impedance. This can then be used to predict the potential-well bunch lengthening using Eq. (22). During beam commissioning phases, beambased measurements are typically performed to extrapolate the effective impedance or effective inductance, which is used to verify the accuracy of the impedance database. A comprehensive review can be found in [9]. The author of [9] suggests that Eq. (22) is a model more consistent with the prediction of the Haissinski equation [10] and with the measurements in the electron storage rings. However, it is important to emphasize that this consistency is conditional on the following factors: (1) The total longitudinal impedance of the ring can be well approximated by a pure inductance, 𝑍_‖ (𝑘) = −𝑖𝑘𝑐𝐿, with the impact of its real part negligible. (2) The potential well, which is distorted by wakefields, remains well quadratic so that the lengthened bunch is close to Gaussian. These factors allow us to replace 𝜂𝐹 in Eq. (14) with 𝜂𝐹_1𝑧, where 𝐹_1 is given by Eq. (17). This leads to the cubic equation (22). Typically, important sources of inductive impedance include small 3D discontinuities, such as obstacles or cavities with longitudinal dimensions comparable to or smaller than the rms bunch length (𝜎_{z0}), on beam pipes; small angle transitions, such as collimators in colliders or tapers sandwiching small-gap insertion devices in light sources, in flat chambers. Small 3D discontinuities from the flanges and bellows are common in all storage rings.

The cubic equation (22) may not apply well in some cases. One example is damping rings, where small-angle transitions are usually unnecessary. A good example is the SLC damping ring with the improved chamber [11], where the resistive part dominates the total impedance [12]. Another example is future circular colliders (FCCs), where the resistive-wall impedance is dominant because of their large circumferences.

A SELF-CONSISTENT EQUATION FOR BUNCH LENGTHENING

For electron storage rings, the circulating beam can be modeled as a continuous distribution 𝜓(𝑧, 𝛿, 𝑠), with its evolution governed by the Vlasov-Fokker-Planck (VFP) equation [13]. Specifically, when considering the synchrotron motion, the VFP equation is [14] 𝜕𝜓 𝜕𝑠 + 𝑑𝑧 𝑑𝑠 𝜕𝜓 𝜕𝑧 + 𝑑𝛿 𝑑𝑠 𝜕𝜓 𝜕𝛿 = 2 𝑐𝑡_𝑑 𝜕 𝜕𝛿 � 𝛿𝜓 + 𝜎^2_{𝛿0} 𝜕𝜓 𝜕𝛿 � , (23)

with 𝑡_𝑑 the longitudinal damping time. The equations of motion are given by Eqs. (3), with the line density distribution 𝜆(𝑧, 𝑠) =

∫_∞ −∞ 𝜓(𝑧, 𝛿, 𝑠)𝑑𝛿.

The VFP equation has an 𝑠-independent stationary solution 𝜓_0 (𝑧, 𝛿) in the form of 𝜓_0 (𝑧, 𝛿) = 𝜓̂_0 (𝛿)𝜆_0 (𝑧) below the microwave instability threshold. The momentum distribution 𝜓̂_0 (𝛿) is Gaussian with rms spread 𝜎_{𝛿0}, and the spatial distribution satisfies

𝑑𝜆_0 (𝑧) 𝑑𝑧 + � 𝑧 𝜎^2_{z0} − 1 𝜂𝜎^2_{𝛿0}

𝐹_0 (𝑧) � 𝜆_0 (𝑧) = 0. (24)

Here 𝐹_0 (𝑧, 𝑠) is from Eq. (4) with 𝜆(𝑧, 𝑠) replaced by the equilibrium distribution 𝜆_0 (𝑧). The solution of Eq. (24) is the so-called Haissinski equation [10]

𝜆_0 (𝑧) = 𝐴𝑒^− 𝑧2 2𝜎2z0 − 𝐼 𝜎z0 ∫_∞ 𝑧 𝑑𝑧^′ W_‖ (𝑧^′ )

, (25)

with the new scaling parameter 𝐼 = 𝐼_𝑛𝜎_{z0}/(𝜂𝜎^2_{𝛿0}) and the wake potential of the bunch

W_‖ (𝑧) =

∫_∞ −∞ 𝑊_‖ (𝑧 − 𝑧^′)𝜆_0 (𝑧^′)𝑑𝑧^′, (26)

With the synchrotron tune defined by 𝜈_{z0} = 𝜔_{z0}/𝜔_0, there is 𝐼 = −𝑁𝑒^2/(2𝜋𝜈_{z0}𝐸𝜎_{𝛿0}) [12, 15]. The stability of the Hassinski equation is beyond the scope of this paper, and the reader is referred to [16] and references therein.

Integrating over 𝑧 on both sides of Eq. (24) and recognizing that the center of mass of the bunch is

𝑧_𝑐 =

∫_∞ −∞ 𝑧𝜆_0 (𝑧)𝑑𝑧, (27)

we obtain 𝑧_𝑐 = 𝐼𝜎_{z0}𝜅_‖ , with the well-known loss factor

𝜅_‖ (𝐼) =

∫_∞ −∞ 𝑑𝑧𝜆_0 (𝑧)W_‖ (𝑧). (28)

In terms of impedance, it is

𝜅_‖ = 𝑐 𝜋 ∫_∞ 0 Re[𝑍_‖ (𝑘)]ℎ(𝑘)𝑑𝑘 (29)

with the spectral power density ℎ(𝑘) = 𝜆̃_0 (𝑘)𝜆̃^∗_0 (𝑘).

Given the bunch profile 𝜆_0 (𝑧), by definition, the rms bunch length is calculated by

𝜎^2_z =

∫_∞ −∞ (𝑧 − 𝑧_𝑐)^2𝜆_0 (𝑧)𝑑𝑧 =

∫_∞ −∞ 𝑧^2𝜆_0 (𝑧)𝑑𝑧 − 𝑧^2_𝑐 . (30)

We show how to calculate 𝜎_z from Eq. (24). We can obtain three terms by multiplying 𝑧 on both sides of this equation and performing integration over 𝑧. The first term is a constant -1 (consider that 𝜆_0 (𝑧) decays exponentially as 𝑒^{−𝑧2/(2𝜎2z0 )} when 𝑧 → ±∞, according to the Haissinski equation). The second term equals 𝜎^2_z +𝑧^2_𝑐. The third term is an integration that contains the wake function. Combining the three terms, we can arrive at an equation that describes the potential-well bunch lengthening

𝑥^2 − 1 − 𝑐𝐼 2𝜋𝜎_{z0}

𝑍^{eff}_‖ (𝑥) = 0, (31)

where 𝑍^{eff}_‖ is formulated by

𝑍^{eff}_‖ = 2𝜋 𝑐 ∫_∞ −∞ 𝑑𝑧(𝑧 − 𝑧_𝑐)𝜆_0 (𝑧)W_‖ (𝑧). (32)

In terms of impedance, it is equivalent to

𝑍^{eff}_‖ = −

∫_∞ −∞ 𝑑𝑘𝑍_‖ (𝑘)𝜆̃_0 (𝑘) � 𝑖 𝑑 𝑑𝑘 𝜆̃^∗_0 (𝑘) + 𝑧_𝑐𝜆̃^∗_0 (𝑘) � . (33)

Here, we define 𝑍^{eff}_‖ as an effective impedance, which is always real but not complex, to indicate bunch lengthening. Equation (31) shows that the term 𝑍^{eff}_‖ is a quadratic function of 𝑥, where 𝑥 is a function of the normalized current 𝐼 (i.e., 𝑥 = 𝑥(𝐼)). Since Eq. (31) is derived from the Haissinski equation without any approximations and the Haissinski equation is the exact stationary solution of the VFP equation, we conclude that it is a self-consistent equation for the potential well lengthening applicable to electron storage rings. We emphasize that Eq. (31) is not valid at beam currents above the microwave instability threshold, where the beam energy spread will increase.

Equation (32) shows that the effective impedance 𝑍^{eff}_‖ is a measure of the average stretching force over the whole bunch. From the impedance viewpoint, Eq. (33) states that both the real and imaginary parts of the impedance contribute to the bunch lengthening when the density distribution is deformed, although the imaginary part is usually the dominant source.

At 𝐼 = 0, the density distribution is Gaussian with 𝑧_𝑐 = 0 and 𝑥(0) = 1. The bunch lengthening rate at 𝐼 = 0 is given by 𝑥^′_0 ≡ 𝑑𝑥/𝑑𝐼|_{𝐼=0} =^𝑐_{4𝜋 𝜎z0} 𝑍^{eff}_‖ (1). Here, the effective impedance 𝑍^{eff}_‖ (1) is given by Eq. (33) with 𝑧_𝑐 = 0 and 𝜆̃_0 (𝑘) = 𝑒^{−𝑘2 𝜎2}z0^{/2}. It only depends on the imaginary part of 𝑍_‖ (𝑘), suggesting that the inductive part of the impedance solely determines the lengthening rate of the bunch at zero current. The relation between 𝑍^{eff}_‖ and the normalized current 𝐼 is complicated. Here, we only give the slope at 𝐼 = 0 as 𝑑𝑍^{eff}_‖ /𝑑𝐼|_{𝐼→0} =^{2𝜋 𝜎z0}_𝑐 � 𝑥^{′2}_0 + 𝑥^{′′} � with 𝑥^{′′} = 𝑑^2𝑥/𝑑𝐼^2 to be determined.

Further calculations can be carried out when a Gaussian distribution with rms length 𝜎_z and center of mass 𝑧_𝑐 is used to approximate the Haissinski distribution Eq. (25). From Eqs. (28) and (33), the center of mass and effective impedance are explicitly written as follows:

𝑧_𝑐 =

𝐼𝜎_{z0}𝑐 𝜋 ∫_∞ 0 𝑑𝑘Re[𝑍_‖ (𝑘)]𝑒^{−𝑘2 𝜎2z} , (34)

𝑍^{eff}_‖ = −2𝜎^2_z

∫_∞ 0 𝑑𝑘𝑘Im[𝑍_‖ (𝑘)]𝑒^{−𝑘2 𝜎2z} . (35)

The above quantities can be formulated explicitly for some well-defined impedances in the literature. For more details, the reader is referred to [17], where it is shown that 𝑍^{eff}_‖ (𝑥) has different scaling laws, depending on the properties of specific impedances. In particular, when the ring impedance is approximated by 𝑍_‖ (𝑘) = −𝑖𝑘𝑐𝐿_{eff}, we immediately obtain the cubic equation (22) from Eqs. (31) and (35). This justifies Eq. (22) and leads us to conclude that the original Zotter’s equation (13) should be recast with 𝜅 = 4 √ 𝜋, as suggested in [9]. Meanwhile, the conventional effective impedance and inductance are connected to the newly defined effective impedance 𝑍^{eff}_‖ by

𝐿_{eff} = − 1 𝜔_0 Im � 𝑍_‖ 𝑛 �_{𝑚=1} eff = 2𝜎_{𝑧0} √ 𝜋𝑐 𝑍^{eff}_‖ , (36)

Figure 1: Pseudo-Green’s function wake and corresponding impedance without CSR for SuperKEKB HER.

and these quantities should be evaluated at zero bunch current.

BUNCH LENGTHENING IN SUPERKEKB

As a specific example, we consider the high-energy ring (HER) of SuperKEKB (the case of LER was discussed in [17]). Longitudinal wakes for various components have been calculated using a Gaussian driving bunch with length 𝜎̂_𝑧 =0.5 mm and summed to create the pseudo-Green function wake [18] as shown in Fig. 1. The corresponding impedance shown in the same figure is calculated by Fourier transforming the wake data (indeed, the chirp-Z transform is used to improve the frequency revolution). The decay of impedance data at high frequencies is due to the chosen 0.5mm Gaussian bunch, which acts as a Gaussian window function of 𝑒^{−𝑘2 𝜎̂2𝑧 /2}. This is justified when the ratio of the nominal length of the bunch 𝜎_{z0} to the length of the driving bunch 𝜎̂_𝑧 is very large (for our example, 10). The bunch should not be strongly deformed or microbunched, so the high-frequency impedances are not sampled. The beam parameters used to solve the Haissinski equation are beam energy 𝐸=7.00729 GeV, ring circumference 𝐶=3016.315 m, slip factor 𝜂=4.543 × 10^{−4}, bunch length at zero current 𝜎_{z0}=5.05 mm, momentum spread 𝜎_{𝛿0}=6.3 × 10^{−4}, and synchrotron tune 𝜈_{z0}=-0.0272. The scaling parameter at 𝑁 = 10^{11} is 𝐼 = 0.0212 pC/V. The numerically obtained Haissinski solutions with bunch populations 𝑁 = (0.0471, 4.71, 9.42, 14.1) × 10^{10} (corresponding to 𝐼=(0.0001, 0.01, 0.02, 0.03) pC/V) are shown in Fig. 2. The lengthening of the bunch and the centroid

Figure 2: Haissinski solution for SuperKEKB HER with 𝑁 = (0.0471, 4.71, 9.42, 14.1) × 10^{10}.

Figure 3: Bunch centroid and rms bunch length as a function of normalized current for SuperKEKB HER.

shift as a function of the normalized current are shown in Fig. 3. Using the bunch length data from Fig. 3, the effective impedance 𝑍^{eff}_‖ is calculated by Eq. (31), as shown in Fig. 4. In this figure, we also plot the 𝑥𝑍^{eff}_‖ data, which corresponds to Zotter’s cubic equation. According to the cubic equation, the inductance impedance dominates the total impedance, and 𝑥𝑍^{eff}_‖ should be a constant or have a weak dependence on the bunch current. Figure 4 shows that this is not the case for SuperKEKB HER. Therefore, we conclude that Zotter’s equation does not apply well to this ring. However, the same analysis for SuperKEKB LER showed that 𝑥𝑍^{eff}_‖ is fairly constant [17], suggesting that a pure inductance is good enough to describe the lengthening of the bundle in LER.

SUMMARY

Zotter’s equation is valid under the following conditions: The longitudinal total impedance of the ring can be well approximated by a pure inductance, and the impact of the real part of the total impedance is negligible. The Haissinski equation, a self-consistent solution of the VFP equation below the microwave instability threshold, has been used to derive a new equation to describe potential-well bunch lengthening. The effective impedance used to describe bunch lengthening has simply been redefined. This new equation is useful for comparing impedance calculations with beambased measurements in electron storage rings.

Figure 4: Effective impedance as a function of normalized current calculated from simulated bunch lengths for SuperKEKB HER.

ACKNOWLEDGEMENTS

The author D.Z. thanks many colleagues, including G. Bassi, A. Blednykh, A. Chao, Y. Cai, L. Carver, K. Hirata, R. Lindberg, M. Migliorati, T. Nakamura, K. Ohmi, K. Oide, B. Podobedov, Y. Shobuda, V. Smaluk, M. Tobiyama, and L. Zhang for inspiring discussions on various aspects of impedance issues in electron storage rings.

REFERENCES

[1] A. Wolski, Beam dynamics in high energy particle accelerators, Imperial College Press, 2014.

[2] A. Chao, Lectures on accelerator physics, World Scientific, 2020.

[3] SAD homepage, https://acc-physics.kek.jp/SAD/.

[4] B. Zotter, CERN SPS/81-14 (1981).

[5] A. Chao, Physics of collective beam instabilities in high energy accelerators, Wiley series in beam physics and accelerator technology (1993).

[6] K.-Y. Ng, Physics of intensity dependent beam instabilities, World Scientific, 2006.

[7] A. Chao, Special Topics in Accelerator Physics, World Scientific, 2022.

[8] K. Bane, SLAC-PUB-5177 (1990).

[9] V. Smaluk, NIMA 888, 22 (2018).

[10] J. Haissinski, Neural Comput. 18B (1) (1973).

[11] K. Bane and C.-K. Ng, Impedance calculations for the improved SLC damping rings, in Proceedings of the 15th Particle Accelerator Conference (1993).

[12] R. Warnock and K. Bane, Phys. Rev. Accel. Beams 21, 124401 (2018).

[13] T. D. Frank, Linear and nonlinear fokker-planck equations, Synergetics, 149 (2020).

[14] J. M. Jowett, in AIP Conference Proceedings, Vol. 153 (1987).

[15] K. Oide and K. Yokoya, KEK-Preprint-90-10 (1990).

[16] Y. Cai, Physical Review Special Topics-Accelerators and Beams 14, 061002 (2011).

[17] D. Zhou, T. Ishibashi, and G. Mitsuka, arXiv:2307.01286 (2023).

[18] T. Ishibashi, et al., Impedance modelling and single-bunch collective instability simulations for the SuperKEKB mainrings, to be published in Journal of Instrumentation.