arXiv:2406.07308v1 [astro-ph.IM] 11 Jun 2024

Revealing Predictive Maintenance Strategies from Comprehensive Data Analysis of ASTRI-Horn Historical Monitoring Data

Federico Incardona,^1 Alessandro Costa,^1 Giuseppe Leto,^1 Kevin Munari,^1 Giovanni Pareschi,^2 Salvatore Scuderi,^3 and Gino Tosti^4 for the ASTRI project^∗

1INAF, Osservatorio Astrofisico di Catania, I-95123 Catania, Italy;

federico.incardona@inaf.it

2INAF, Osservatorio Astronomico di Brera, I-23807 Merate, Italy

3INAF, Istituto di Astrofisica Spaziale e Fisica Cosmica, I-20133 Milano, Italy

4Universià di Perugia, Istituto di Astrofisica Spaziale e Fisica Cosmica, I-20133 Milano, Italy

∗http://www.astri.inaf.it/en/library/

Abstract. Modern telescope facilities generate data from various sources, including sensors, weather stations, LiDARs, and FRAMs. Sophisticated software architectures using the Internet of Things (IoT) and big data technologies are required to manage this data. This study explores the potential of sensor data for innovative maintenance techniques, such as predictive maintenance (PdM), to prevent downtime that can affect research. We analyzed historical data from the ASTRI-Horn Cherenkov telescope, spanning seven years, examining data patterns and variable correlations. The findings offer insights for triggering predictive maintenance model development in telescope facilities.

1. Introduction

ASTRI-Horn (Pareschi 2016) is an Italian telescope designed to detect gamma rays as a prototype of the Small-Sized Telescopes of the Cherenkov Telescope Array (CTA) project (The CTA Consortium 2018). It was developed in the context of ASTRI (“Astrofisica con Specchi a Tecnologia Replicante Italiana”, Vercellone et al. 2013), a project that aims at deploying an array of nine ASTRI-like telescopes (named the ASTRI Mini- Array) at the Observatorio del Teide in Tenerife (Spain) for the study of high-energy gamma-ray emissions from astrophysical sources (Vercellone et al. 2022; Scuderi et al. 2022). As a whole, the system will be an Internet of Things environment, requiring a complex software architecture to address data collection and storage (Incardona et al. 2022b; Costa et al. 2021). 1

2. Telescope activity windows

The ASTRI-Horn prototype was installed in 2014 at the observing station of the INAF Astrophysical Observatory of Catania (Serra La Nave, Mt. Etna).

We analyzed the monitoring time series collected by the Telescope Control Unit (TCU) and the Telescope Health Control Unit (THCU) (Tanci et al. 2016), which are in charge of monitoring the ASTRI-Horn housekeeping data, and by a Weather Station (WS) located in the proximity of the telescope.

The data spans from June 2017 to October 2023, but we selected only intervals when the motors were active. We obtained 1307 intervals, for which we estimated an average time duration of about 90 minutes. Fig.1 reports the interval amplitude distribution in seconds.

Figure 1. Distribution of the activity windows duration of the ASTRI-Horn telescope since 2017.

3. Variables correlation and principal component analysis

The set of available monitored properties for TCU, THCU, and WS was composed of more than 200 time series, each of which was sampled with a frequency of about 15 seconds, even if, in many cases, the sampling rate was not uniform.

We focused on a subset of monitored properties composed of 19, 27, and 4 variables, respectively, for TCU, THCU, and WS. These features report information about the currents, voltages, phases, positions, temperatures, torques, and statuses of the telescope components, as well as the environmental temperature, humidity, wind speed, and solar radiation.

To reduce the number of data points, we resampled each active interval of the dataset at a rate of 1 minute and computed the correlation matrix (Fig.2). We also used larger time scales (1, 6, 12 hours, one day, and one week) to resample the dataset and every time we computed the correlation matrix.

We found tens of correlations with the larger values of the Pearson coefficient^1 (r > 0.9) at every time-scale. On the time scale of the week, we observed a moder-

1The Pearson coefficient r is the ratio between the covariance of two variables and the product of their standard deviations and measures the linear correlation between two variables (Johnson & Wichern 1988).

Predictive Maintenance Strategies for ASTRI-Horn 3

Figure 2. Correlation matrix for a subset of TCU, THCU, and WS variables collected from 2017 to 2023 and resampled at one minute.

ate correlation with r ≈ 0.53 between the Azimuth master motor current and encoder initialization status. This correlation strengthened to r ≈ 0.75 when we focused on the time frame just before the encoder replacement, which happened in April 2022 due to wear. This finding suggests a potential wear signature in the time series data that warrants further investigation.

Finally, we performed a Principal Component Analysis (PCA, Johnson & Wichern 1988) on the dataset. The scree plot^2 reported in Fig.3 shows that about 16 principal components retain about 80% of the total dataset variance.

4. Insights for predictive maintenance models

Predictive maintenance (PdM, Mobley 2002) is a data-driven approach to maintenance that improves the life cycle of a system by predicting just in time potential equipment malfunction, reducing its downtime. Such an innovative approach can be applied to telescope facilities (Incardona et al. 2022a) in combination with some of the most advanced Machine Learning models (Gambadoro et al. 2023).

We aim to develop a model that constantly compares, for each target feature, the actual measured values and the predicted ones and raises an alarm every time a deviation from the model is detected. We will exploit the stronger correlations and principal components to reduce model overfitting. Confirmed correlations due to wear will be used to identify the correct prediction window for that kind of damage. Finally, we plan to repeat this analysis by considering a wider set of monitored properties.

2A scree plot is a graph of eigenvalues against the corresponding principal component number (Johnson & Wichern 1988).

4 Incardona et al.

Figure 3. Amount of dataset variance explained by each principal component (bars) and cumulatively (line with markers).

Acknowledgments. This work was conducted in the context of the ASTRI Project. We gratefully acknowledge support from the people, agencies, and organizations listed here: http://www.astri.inaf.it/en/library/. This paper went through the internal ASTRI review process. This work is also supported by the “Istituto Nazionale di Astrofisica” (INAF) Mini-Grant.

References

Costa, A., Munari, K., Incardona, F., et al. 2021, in Proceedings of 37th International Cosmic Ray Conference — PoS(ICRC2021), vol. 395, 700 Gambadoro, S., et al. 2023, in Machine Learning for Astrophysics (Cham: Springer International Publishing), 205 Incardona, F., Costa, A., & Munari, K. 2022a, Failure type detection and predictive maintenance for the next generation of imaging atmospheric cherenkov telescopes. 2212.12381 Incardona, F., et al. 2022b, The monitoring logging and alarm system of the astri mini-array gamma-ray air-cherenkov experiment at the observatorio del teide. 2207.06372 Johnson, R. A., & Wichern, D. W. 1988, Applied Multivariate Statistical Analysis (USA:

Prentice-Hall, Inc.)

Mobley, R. K. 2002, in An Introduction to Predictive Maintenance (Second Edition), edited by R. K. Mobley (Butterworth-Heinemann), 1–438 Pareschi, G. 2016, in Ground-based and Airborne Telescopes VI, vol. 9906 of Society of Photo- Optical Instrumentation Engineers (SPIE) Conference Series, 99065T Scuderi, S., et al. 2022, Journal of High Energy Astrophysics, 35, 52. 2208.04571 Tanci, C., et al. 2016, in Software and Cyberinfrastructure for Astronomy IV, vol. 9913 of Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series, 99133L The CTA Consortium 2018, Science with the Cherenkov Telescope Array (WORLD SCIEN- TIFIC). URL https://doi.org/10.1142/10986 Vercellone, S., et al. (ASTRI) 2013, in 33rd International Cosmic Ray Conference, 0109. 1307.

5671 Vercellone, S., et al. 2022, Journal of High Energy Astrophysics, 35, 1. 2208.03177