arXiv:2406.09058v1 [cs.IT] 13 Jun 2024

Environment-Aware Codebook Design for RIS-Assisted MU-MISO Communications: Implementation and Performance Analysis

Zhiheng Yu, Jiancheng An, Member, IEEE, Ertugrul Basar, Fellow, IEEE, Lu Gan, and Chau Yuen, Fellow, IEEE

Abstract

Reconfigurable intelligent surface (RIS) provides a new electromagnetic response control solution, which can proactively reshape the characteristics of wireless channel environments. In RIS-assisted communication systems, the acquisition of channel state information (CSI) and the optimization of reflecting coefficients constitute major design challenges. To address these issues, codebook-based solutions have been developed recently, which, however, are mostly environment-agnostic. In this paper, a novel environment-aware codebook protocol is proposed, which can significantly reduce both pilot overhead and computational complexity, while maintaining expected communication performance. Specifically, first of all, a channel training framework is introduced to divide the training phase into several blocks. In each block, we directly estimate the composite end-to-end channel and focus only on the transmit beamforming. Second, we propose an environment-aware codebook generation scheme, which first generates a group of channels based on statistical CSI, and then obtains their corresponding RIS configuration by utilizing the alternating optimization (AO) method offline. In each online training

This article was presented in part at the IEEE VTC2024-Spring [1]. This work was partially supported by Sichuan Science and Technology Program under Grant 2023YFSY0008 and 2023YFG0291. The work of Ertugrul Basar was supported by TUBITAK under Grant 120E401. The work of Chau Yuen was supported in part by the Ministry of Education, Singapore, under its Ministry of Education (MOE) Tier 2 under Award MOE-T2EP50220-0019; and in part by the Science and Engineering Research Council of Agency for Science, Technology and Research (A*STAR) Singapore, under Grant M22L1b0110.

Z. Yu and L. Gan are with the national key laboratory on blind signal processing. School of Information and Communication Engineering, University of Electronic Science and Technology of China (UESTC), Chengdu 611731, China, and also with the Yibin Institute of UESTC, Yibin 644000, China (e-mail: zhihengyu2000@163.com; ganlu@uestc.edu.cn).

J. An and C. Yuen are with the School of Electrical and Electronics Engineering, Nanyang Technological University, Singapore 639798 (e-mail: jiancheng an@163.com; chau.yuen@ntu.edu.sg).

E. Basar is with the Communications Research and Innovation Laboratory (CoreLab), Department of Electrical and Electronics Engineering, Koç University, Sariyer, Istanbul 34450, Turkey. (e-mail: ebasar@ku.edu.tr).

block, the RIS is configured based on the corresponding codeword in the environment-aware codebook, and the optimal codeword resulting in the highest sum rate is adopted for assisting in the downlink data transmission. Third, we analyze the theoretical performance of the environment-aware codebookbased protocol taking into account the channel estimation errors. Finally, numerical simulations are provided to verify our theoretical analysis and the performance of the proposed scheme. In particular, the simulation results demonstrate that our protocol is more competitive than conventional environmentagnostic codebooks.

Index Terms

Reconfigurable intelligent surface (RIS), channel training, environment-aware codebook, multiuser downlink beamforming.

I. INTRODUCTION Reconfigurable intelligent surface (RIS) is an artificial electromagnetic (EM) material with programmable EM properties [2]. Essentially, an RIS is composed of numerous sophisticatedly designed EM meta-atoms. By dynamically adjusting the control signals for each RIS element, it becomes possible to intelligently manipulate the EM characteristics, including the amplitude, phase, polarization, and frequency of the incident signal in a programming manner [3], [4]. In contrast to conventional wireless technologies such as massive multiple-input multiple-output (MIMO) and millimeter wave (mmWave) communications [5] that have to grapple with issues related to network energy consumption and hardware costs, the RIS elements are passive and simply reflect incident signals, mitigating the power-thirsty radio frequency (RF) chains and forward delay in traditional relays [6]–[8]. Remarkably, an RIS can operate in full-duplex mode without encountering self-interference problems [9]. By adjusting the phase shifts at the RIS, various functionalities such as secure communications, focused beam emission, and enhanced indoor coverage can be achieved [10]–[12]. In addition to the single-layer RIS, the application of stacked intelligent metasurfaces (SIM) in different scenarios has also begun to emerge for performing signal processing tasks in the wave domain [13]–[15]. Besides, integrating RIS with transceivers also attracts increased attention [16]. Given these advantages, RIS-empowered communication is considered to be a key technology enabling future wireless networks [2], [17]–[20].

Nevertheless, RIS-assisted wireless communication systems also present some challenges. On the one hand, obtaining accurate channel state information (CSI) is much more difficult due to the fact that most RISs are composed of passive elements or only equipped with a small number of onboard signal processing units [21], [22]. More specifically, it becomes impractical to separately estimate base station (BS)-RIS and RIS-user channels using traditional pilot-based methods. Therefore, several advanced channel estimation techniques have been proposed to estimate cascaded or composite end-to-end channels [23]–[30]. For instance, Mishra et al. introduced a simple ON/OFF method capable of estimating the cascaded BS-RIS-user channels one by one [25]. Subsequently, Xu et al. proposed a novel ON/OFF based minimum mean square error (MMSE) channel estimation method for RIS-assisted high mobility systems, which mitigates the Doppler-induced error floor [26]. In order to reduce the pilot overhead required for estimating the cascaded BS-RIS-user channels, Wang et al. leveraged the similarity of the BS-RIS link between multiple users [24]. Furthermore, in [27], Wei et al. considered the double-structured sparsity of the cascaded channels to estimate the angle parameters, while [23] proposed a channel trainingbased scheme to directly estimate the composite channels. More recently, Guo et al. developed a new channel estimator leveraging the unitary approximate message passing (UAMP) technique [28], and Chen et al. proposed a new compressed sensing-based channel estimation protocol to estimate the cascaded channels [29], [31]. Combined with deep learning, Xu et al. proposed a three-stage joint channel decomposition and prediction framework that exploits the quasi-static property of BS-RIS channel and the fast time-varying property of RIS-user channels [30].

On the other hand, the optimization of reflecting coefficients (RCs) at the RIS constitutes another challenge [32]–[40]. More specifically, in [34], Wu and Zhang concentrated on minimizing the total transmit power under specific signal-to-interference-plus-noise ratio (SINR) constraints, they adopted alternating optimization (AO) method based on semidefinite relaxation (SDR) to obtain approximate solutions of transmit precoding matrix and RIS RCs. In [32], Yan et al. devised RCs based on the statistical CSI to maximize spectral efficiency. In [37], Di et al. proposed a hybrid beamforming scheme to maximize the sum rate of RIS-aided multi-

TABLE I COMPARISON OF PROPOSED SCHEME WITH RECENT RIS SOLUTIONS

Reference MIMO setup Phase shift model Optimization objective Channel Complexity Imperfect CSI PBF design Proposed MU-MISO Discrete Sum rate Composite Low ✓ ✓ [23] MU-MIMO Discrete Transmit power Composite Low ✓ ✓ [33] MIMO Discrete Throughput Composite Low ✓ ✓ [34] MU-MISO Continuous Transmit power Separate High × × [17] MIMO Continuous Throughput Separate High × ✓ [41] MIMO Discrete Received signal power Separate Moderate × ✓ [42] MISO Discrete Achievable rate Composite Low ✓ ✓ [27] MU-MISO Continuous NMSE Separate Moderate × × [38] MIMO Discrete ASE Separate Moderate ✓ ✓ [28] MIMO Continuous NMSE Separate Low × × [24] MU-MISO Continuous NMSE Separate Moderate ✓ × ASE: Average spectral efficiency NMSE: Normalized mean square error PBF: Passive beamforming

user multiple-input single-output (MU-MISO) systems. For beyond-diagonal (BD) RIS-aided multi-user systems, Fang and Mao proposed a closed-form solution for passive beamforming to maximize the sum of the effective channel gains [40]. Besides, [36] proposed a heuristic algorithm to optimize continuous phase shifts of RIS-aided massive MIMO systems. In an RISaided mmWave MIMO system, Xu et al. developed a novel deep reinforcement learning (DRL) algorithm to design joint beamforming according to a location-aware imitation environment [39]. However, it is important to note that the schemes mentioned above assume the perfect CSI, which is generally unavailable in practical scenarios. Considering the imperfect CSI, in [33], An et al. conceived a low-complexity framework for maximizing the achievable rate of RIS-aided MIMO system with discrete phase shifts. The RCs are pre-designed and the effective composite channel is estimated. Moreover, [35] considered an imperfect CSI scenario and solved the max-min SINR problem considering a continuous phase shift. In [38], Nikolaos et al. proposed two phase shift design schemes whose complexity is linear to the number of RIS elements and receive antennas.

In addition, considering the complexity and overhead, [45] proposed a low-complexity antenna selection algorithm to avoid the joint optimization problem with the transceiver, which is capable of supporting arbitrary MIMO configuration. Moreover, several group-/fully-connected schemes are introduced to reduce the pilot overhead. More specifically, in [43], Shen et al. proposed a novel RIS architecture based on group- and fully-connected reconfigurable impedance networks

A [34]: Optimal configuration B [42]: Statistic CSI-based scheme C [41]: Scalar/Vector RIS design D [43]: Optimal RIS grouping E [44]: Group connected RIS F [34]: Random configuration B-A curve: Proposed environment-aware codebook scheme Fr : Rician factor of the RIS-user channel C : Euler-Mascheroni constant θ1 : RC angle of the reactance matrix’s non-zero eigenvalues γ : Transmit SNR Γ : Gamma function NG: Number of RIS elements in each group β_l : Large-scale path loss coefficient of the cascaded link

Fig. 1. The performance versus overhead diagram, where the proposed scheme strikes a flexible tradeoff between the statistical CSI-based scheme and the optimal RIS configuration.

and derived the scaling law for received signals in RIS-aided MIMO systems. Adopting a similar RIS structure, [41] analyzed the scaling law for received signal power using BD RISs in case of discrete phase shifts. Additionally, in [44], Kundu et al. adopted a grouping strategy to optimize the RIS and derived a tight closed-form upper bound for the achievable rate.

Recently, various codebook-based schemes have emerged to enhance RIS-based systems’ performance with moderate overhead. For instance, [46] proposed a codebook-based framework and introduced three codebook generation schemes. Further in [22] and [23], An et al. employed a low complexity framework to maximize the achievable rate. They analyzed the theoretical performance of the random and uniform codebooks. Beyond generating codebooks offline, in [42], Jia et al. proposed an environment-aware codebook design to flexibly adapt to different channel conditions. Moreover, [47] proposed a discrete Fourier transform (DFT) codebook, which, however, experiences significant SINR loss in the near-field region of RIS [48]. To solve this problem, a ring-type codebook based on the Fresnel principle was further proposed to determine the phase distribution by employing the location information of the user and an RIS.

Besides, in [49], Abdallah et al. developed a multi-agent DRL-based beamforming codebook design that relies only on receiving power measurements.

Nevertheless, the above codebook-based schemes usually entail substantial training overhead and lack adaptability to channel environment variations. Against this background, in this paper, we introduce a novel codebook-based protocol for RIS-assisted MU-MISO systems and propose an environment-aware scheme to obtain a discrete RIS RC configuration codebook. Specifically, we first generate virtual channels in each training block according to the statistical CSI, and then perform AO of RC configuration and transmit power allocation to obtain the corresponding RIS RC codeword. In the on-line stage, we configure the RIS according to the predesigned codebook and estimate the composite end-to-end channel for each codeword, which reduces the performance loss caused by imperfect CSI. Then, we theoretically analyze the received power scaling law in a single-user scenario considering both the perfect and imperfect CSI to gain valuable insights into the proposed environment-aware codebook scheme. Comparing with the existing work [42], we derive a tighter upper bound of the achievable rate in perfect CSI scenario. Moreover, the influence of channel estimation errors in the environment-aware codebook-based schemes has been theoretically analyzed in Proposition 2. For illustration, we contrast the proposed scheme to its existing channel estimation and passive beamforming counterparts in Table I. In addition, as shown in Fig. 1, we show the performance vs. overhead tradeoff of the proposed scheme and contrast it to existing schemes. To summarize, our contributions are outlined as follows.

1) We propose a channel training-based protocol for RIS-assisted MU-MISO systems. In contrast to conventional schemes, we develop a novel environment-aware codebook design scheme, where we generate a set of virtual channels with the same distribution as practical channels. For each virtual channel, we employ the AO method to solve the sum rate maximization problem. Specifically, we adopt a successive refinement method to optimize the RC at the RIS and a classic water-filling power allocation algorithm to allocate transmit power at the BS when one of them is fixed. By doing so for Q virtual channels, we generate an environment-aware RC codebook.

2) Then, in the on-line stage, we configure the RIS using each codeword in the environmentaware codebook and thus obtain Q candidate composite end-to-end channels. The optimal index that maximizes the sum rate is determined to obtain the corresponding discrete RIS configuration and transmit power allocation.

3) Next, the theoretical achievable rate adopting the proposed environment-aware channel training-based protocol is analyzed under both the perfect and imperfect CSI scenarios. To the best of our knowledge, this is the first work to analyze the influence of channel estimation errors on codeword index selection.

4) Finally, numerical simulation results are provided to validate our performance analysis. Both the theoretical analysis and simulation results demonstrate that the proposed environmentaware codebook scheme strikes a flexible trade-off between the achievable performance and pilot overhead.

The rest of this paper is organized as follows. Section II introduces the RIS-assisted multiuser system model. In Section III, we introduce the proposed codebook-based protocol and environment-aware codebook generation scheme. Then, the theoretical performance of the proposed scheme is analyzed in Section IV, where the effects of channel estimation errors are also considered. Section V provides numerical simulations to evaluate the performance of the proposed scheme. Finally, Section VI concludes the paper.

Notations: Scalars are denoted by italic letters, vectors and matrices are denoted by lower and upper bold-face letters, respectively; C^{x×y} denotes the space of x × y complex-valued matrices; For any general matrix A, A^T , A^H , A^∗, rank(A) represent its transpose, Hermitian transpose, conjugate and rank, respectively; For a complex-valued vector x, ‖x‖ denotes its Euclidean norm, |x| denotes its magnitude, and diag(x) denotes a diagonal matrix with each diagonal element being the corresponding entry in x; We denote the N × N identity matrix as I_N ; log(·) and ⌊·⌋ represent the logarithmic function and floor operator, respectively; The distribution of a circularly symmetric complex Gaussian (CSCG) random vector with mean vector x and covariance matrix Σ is denoted by ∼ CN (x, Σ), where ∼ stands for “distributed as”; For a square matrix S, tr(S) and S^{−1} denote its trace and inverse, respectively; E {·} denotes the statistical expectation. ℜ {·} and ℑ {·} denotes the real part and imagine part of a complex number, respectively. For clarity, we summarize the main symbols used in this paper and their meanings in Table II.

TABLE II MAJOR SYMBOLS AND THEIR MEANINGS

Symbol Meaning

M The number of BS antennas N The number of RIS elements K The number of users Q Training overhead G The BS-RIS channel h^H_{d,k} The BS-user k channel h^H_{r,k} The RIS-user k channel h^H_k The composite channel of user k Φ RC configuration of the RIS w Transmit precoding vector θ Phase shift of RIS element R Sum rate of multiple users T_c The channel coherence time P Transmit power allocation matrix ε Composite channel estimation error P_d Transmit power at the BS P_{ul} Average power of the pilot signals σ^2_z Average noise power at the BS σ^2_k Average noise power at the users

II. SYSTEM MODEL

Let us consider an RIS-assisted multi-user communication system in a single cell as shown in Fig. 2, where an RIS with N reflecting elements is deployed to enhance the downlink (DL) signal transmission between a multi-antenna BS and K single-antenna users. The number of transmit antennas at the BS is denoted by M. The RIS is equipped with a smart controller capable of adjusting the RCs according to the real-time CSI [21]. In this paper, we adopt a quasi-static flat-fading channel model for all links. Besides, we consider a time-division duplexing (TDD) protocol for both uplink (UL) as well as DL transmissions and assume the channel’s reciprocity for the CSI acquisition in the DL based on the UL training. The baseband equivalent channels

Fig. 2. An RIS-assisted multiuser communication system.

spanning from the BS to the RIS, from the RIS to user k, and from the BS to user k are denoted by G ∈ C^{N×M} , h^H_{r,k} ∈ C^{1×N} , h^H_{d,k} ∈ C^{1×M} , respectively, with k = 1, 2, · · · , K.

Let the diagonal matrix Φ = diag (φ_1, φ_2, · · · , φ_N ) represent the RC configuration of the RIS, where φ_n denotes the RC of the nth RIS element, following |φ_n| = 1 for n = 1, 2, · · · , N. In this paper, we use discrete phase shifts to control signal reflection. In order to facilitate the practical implementation, we consider that the discrete phase shifts are obtained by uniformly quantizing the interval [0, 2π) and let b represent the number of bits used for quantizing the phase shift levels. Hence the phase shift of each RIS element is assumed to be one of B = 2^b discrete phase shift values. The phase shift set B is given by B = {0, Δθ, · · · , (B − 1)Δθ} , (1) where Δθ = 2π/B. Thus, the RC of the nth element at the RIS can be expressed as φ_n = e^{jθn} , θ_n ∈ B, n = 1, 2, · · · , N and the composite end-to-end channel for user k is given by

h^H_k = h^H_{r,k}ΦG + h^H_{d,k}, k = 1, 2, · · · , K. (2)

Let H = [h_1, h_2, · · · , h_K ] ∈ C^{M×K} represent the UL channels associated with K users.

During the channel estimation process in the UL phase, the pilot signal received at the BS is given by y = K∑ k=1 h_k √ P_{ul}x_k + z, (3)

where P_{ul} is the average power of the pilot symbols, which is assumed to be identical for all users, x_k denotes the pilot symbol transmitted from user k to BS with zero mean and unit variance, z ∈ C^{M×1} denotes the additive white Gaussian noise (AWGN) at the BS obeying z ∼ CN (0, σ^2_z I_M ).

Next, we consider the DL of data transmission and use linear transmit precoding at the BS. As a result, the complex baseband signal received at user k is given by

r_k = h^H_k K∑ i=1 w_is_i + n_k, (4)

where s_k denotes the transmitted information symbol of user k, w_k ∈ C^{M×1} denotes the corresponding transmit beamforming vector and n_k ∼ CN (0, σ^2_k) , k = 1, 2, · · · , K denotes the AWGN at the kth user’s receiver.

Meanwhile, we adopt the Rician channel in this paper. Specifically, the RIS-user k channel can be expressed as

h_{r,k} = √ β_r (√ F_r F_r + 1 h^{LoS}_{r,k} + √ 1 F_r + 1 h^{NLoS}_{r,k} ) , (5)

where β_r and F_r are the path loss and the Rician factor of RIS-user channel, respectively; h^{LoS}_{r,k} and h^{NLoS}_{r,k} represent the line-of-sight (LoS) and non-line-of-sight (NLoS) components of RISuser channel, respectively. The NLoS components are i.i.d. complex Gaussian variables with zero mean and unit variance, satisfying h^{NLoS}_{r,k} ∼ CN (0, I_N ). Similarly, the BS-user channel and BS-RIS channel are modeled by using (5).

Moreover, we consider a uniform linear array (ULA) of M antennas at the BS and a uniform planar array (UPA) of N antennas at the RIS. Let a_{BS} (δ) ∈ C^{M×1} and a_R (ζ, γ) ∈ C^{N×1} denote the steering vector of the BS and the RIS, respectively. Specifically, the mth entry of a_{BS} is denoted as e^{j 2π}λ^{(m−1)dBS sin(δ)}, m = 1, 2, · · · , M, where d_{BS} denotes the element spacing of the BS, λ denotes the wavelength of the signal, and δ ∈ [−π/2, π/2) de-

Fig. 3. The frame structure of the proposed protocol.

notes the angle of departure (AoD) or the angle of arrival (AoA). The nth entry of a_R is denoted as e^{j 2πλ dR sin(γ)}[^{⌊ n−1N}x^{⌋ sin(ζ)+((n−1)−⌊ n−1N}x^{⌋Nx) cos(ζ)}]^{/λ}, n = 1, 2, · · · , N, where d_R denotes the element spacing of the RIS. N_x is the number of reflecting elements deployed at each row of the RIS. Moreover, ζ ∈ [0, π) and γ ∈ [−π/2, π/2) denote the azimuth and elevation AoA/AoD, respectively. Thus, the LoS component of the G, h_r and h_d are given by a_{BS} ( δ^{AoA}_d ) , a_R ( ζ^{AoA}_g , γ^{AoA}_g ) a_{BS} ( δ^{AoD}_g )_H and a_R ( ζ^{AoA}_r , γ^{AoA}_r ) , respectively, where δ^{AoA}_d and δ^{AoD}_g represent the AoA from the user to the BS and the AoD from the BS to the RIS, respectively; ζ^{AoA}_g and γ^{AoA}_g represent the azimuth and elevation AoA from the BS to the RIS, respectively; ζ^{AoA}_r and γ^{AoA}_r represent the azimuth and elevation AoA from the user to the RIS, respectively.

III. THE PROPOSED CHANNEL TRAINING PROTOCOL In this section, we outline the proposed codebook-based scheme by first introducing our channel training-based protocol in Section III-A. Then, our bespoke environment-aware codebook generation scheme is proposed in Section III-B. In Section III-C, we introduce the on-line codebook configuration stage.

A. Channel Training-Based Protocol

As shown in Fig. 3, our channel training-based protocol consists of off-line and on-line stages.

In the off-line stage, we generate a group of virtual channels based on the statistical CSI. Then, we use the AO algorithm to obtain the optimal RC configuration corresponding to each virtual channel. Repeating for Q virtual channels generates the RC codebook.

In the on-line stage, the transmission protocol is divided into two phases: • The UL channel training phase: During the UL channel training phase, we adjust the RIS configuration over training blocks according to the environment-aware codebook. Then, we repeat carrying out the composite channel estimation and the transmit precoding design to obtain Q candidate channels;

• The DL data transmission phase: During the DL signal transmission phase, we select the optimal channel maximizing the sum rate from Q candidates, and get the corresponding RIS configuration and transmit power allocation to assist in the DL communications.

B. Off-Line Codebook Design Stage

Next, we elaborate on the detailed steps to generate the environment-aware codebook. 1) Virtual Channel Generation Based on Statistical CSI: Note that the statistical CSI of all channels is easier to obtain by measurement or averaging historical observations, and it has a longer channel coherence time [32], [50]. In this paper, we utilize the statistical CSI, which includes the path loss, the LoS component and the distribution of the NLoS component of the practical channels to design the environment-aware codebook offline. Specifically, we generate Q virtual channels off-line for the RIS-user k link according to (5), yielding h_{r,k,q} = √ β_r (√ F_r F_r + 1 h^{LoS}_{r,k} + √ 1 F_r + 1 h̃^{NLoS}_{r,k,q} ) , (6)

where h^{LoS}_{r,k} is the LoS component of the virtual channel and it remains unchanged within each channel coherence block, h̃^{NLoS}_{r,k,q} represents the NLoS component of the qth virtual channel which is randomly generated following the same distribution with h^{NLoS}_{r,k} during each training block. In addition, the virtual channels for BS-RIS and BS-user k links are generated in the same way.

2) Alternating Optimization Algorithm: For each tentative virtual channel, we endeavor to maximize the sum rate for all users by jointly optimizing the transmit precoding at the BS and the RC configuration at the RIS, subject to the total transmit power. Specifically, the optimization problem is formulated as max W_q ,Φ_q K∑ k=1 log_2 ( 1 + | |hH_{k,q}w_{k,q} | |^2 ∑_K l≠k | |hH_{k,q}w_{l,q} | |^2 + σ2_k )

s.t.Φ_q = diag (φ_{q,1}, φ_{q,2}, · · · , φ_{q,N} ) , φ_{q,n} = e^{jθq,n} , θ_{q,n} ∈ B, ∀n ∈ N , K∑ k=1 ‖w_{k,q}‖^2 ≤ P_d, (7)

for q = 1, 2, · · · , Q, where h^H_{k,q} = h^H_{r,k}Φ_qG + h^H_{d,k} ∈ C^{1×M} and w_{k,q} are the composite channel and the transmit precoding vector for user k during the qth training block, respectively. W_q = [w_{1,q}, w_{2,q}, · · · , w_{K,q}] ∈ C^{M×K} denotes the transmit precoding matrix. P_d is the total transmit power at the BS.

In this paper, we adopt zero-forcing (ZF) beamforming at the BS to eliminate interference between different users, yielding h^H_{k,q}w_{k,q} = √ p_{k,q}, k = 1, 2, · · · , K, h^H_{k,q}w_{l,q} = 0, ∀l ≠ k, l = 1, 2, · · · , K, (8) where p_{k,q} denotes the received power of user k in the qth training block.

Let H^H_q = [h_{1,q}, h_{2,q}, · · · , h_{K,q}]^H ∈ C^{K×M} , q = 1, 2, · · · , Q represent the DL composite channels in the qth training block, the optimal transmit precoding matrix W_q is given by a pseudo-inverse of H^H_q with an appropriate power allocation among users. More specifically, the transmit precoding matrix can be expressed as

W_q = H_q ( H^H_q H_q )_{−1} P^{12}q , (9)

where P_q = diag (p_{1,q}, p_{2,q}, · · · , p_{K,q}) denotes the received power matrix in the qth training block.

As a result, the sum rate R_q can be simplified as

R_q = K∑ k=1 log_2 ( 1 + p_{k,q} σ^2_k ) . (10)

Next, we utilize the AO algorithm to obtain the optimal transmit power allocation and RC solution, which consists of the following two parts:

a) Transmit Power Allocation: Given a tentative RIS RC configuration matrix Φ_q, the transmit power allocated to user k is p_{k,q} = ‖w_{k,q}‖^2. Let U_q = ( H^H_q H_q )_{−1} ∈ C^{K×K} , P_q = diag ( p_{1,q}, p_{2,q}, · · · , p_{K,q} ) denotes the transmit power allocation matrix. By applying the classic water-filling power allocation algorithm [33], the transmit power allocated to the kth user can be expressed as

p_{k,q} = max { 1 η_q − σ^2_ku_{k,q}, 0 } , (11)

where u_{k,q} is the kth diagonal element of U_q and η_q is a threshold that satisfies ∑_K k=1 max

{_1 η_q − σ 2 ku_{k,q}, 0 } = P_d. Once the transmit power allocation among users is obtained, the received power of user k can be expressed as p_{k,q} = p_{k,q}/u_{k,q}.

b) RIS RC Optimization: Given the transmit power allocation matrix P_q, problem (7) is reduced to

max_{θq,n} R_q (θ) = K∑ k=1 log_2 ( 1 + p_{k,q} u_{k,q}σ^2_k )

s.t. θ_{q,n} ∈ B, ∀n ∈ N . (12) In this paper, we adopt a successive refinement method to optimize RIS RCs one by one. Specifically, when fixing other (N − 1) RCs, we calculate the objective function value R_q (θ) for all potential values of θ_{q,n} in B and choose the phase shift corresponding to the maximum value. After repeating this one-dimensional search process several times, we obtain the optimal RIS configuration Φ_q corresponding to the transmit power allocation P_q.

Moreover, we use random phase shifts to initialize power allocation. Then we alternately optimize the power allocation and RIS configuration until the objective function R_q reaches

Algorithm 1 Environment-Aware Codebook Design. Input: Statistical CSI.

Output: Φ_q and P_q, q = 1, 2, · · · , Q. 1: for q ∈ {1, 2, · · · , Q} do 2: Generate h_{r,k,q}, h_{d,k,q}, k = 1, 2, · · · , K and G_q according to (6). 3: Set r = 1.

4: Initialize the random RC matrix Φ^r_q. 5: repeat 6: Optimize P^r_q according to (11). 7: for n ∈ {1, 2, · · · , N} do 8: Optimize φ^r_{q,n} = e^{jθrq,n} according to (12). 9: end for 10: Update r = r + 1.

11: until The fractional decrease of R_q is below a threshold ϵ > 0. 12: Φ_q = Φ^r_q and P_q = P^r_q. 13: end for 14: return Φ_q and P_q.

convergence.

By carrying out the virtual channel generation in (6) and the AO method for all Q training

blocks, we obtain Q candidate channels and their corresponding P_q and Φ_q. Note that our chan-

nels are generated offline according to the statistical CSI, the corresponding RIS configuration

and power allocation are also performed offline.

C. On-Line RIS Configuration Stage

In the on-line stage, we complete the RIS configuration by selecting the optimal codeword

in the environment-aware codebook to assist in the DL transmission. Specifically, we adjust the

RIS RC in different training blocks and obtain Q objective function values. The decision center

will select the optimal codeword maximizing the sum rate to assist in the DL data transmission.

Accordingly, the transmit precoding matrix is also determined.

1) Composite Channel Estimation: Specifically, given the RC configuration of the qth training

block Φ_q, q = 1, 2, · · · , Q the received signal at the tth time slot (TS) of the qth training block is given by

y_{q,t} = K∑ k=1 h_{k,q} √ P_{ul}x_{k,t} + z_{q,t} = √ P_{ul}H_qx_t + z_{q,t}, (13)

where h_{k,q} denotes the composite channel spanning from the kth user to the BS in the qth training block, x_{k,t} is the pilot symbol transmitted from user k to the BS in TS t, which remains identical for all Q training blocks, x_t = [x_{1,t}, x_{2,t}, · · · , x_{K,t}]^T is the pilot vector of the tth TS.

Upon collecting the signals of T TSs in the qth training block, the signal received at the BS in this block is given by

Y_q = [y_{q,1}, y_{q,2}, · · · , y_{q,T} ] = √ P_{ul}H_qX + Z_q, (14)

where X = [x_1, x_2, · · · , x_T ] ∈ C^{K×T} is the pilot matrix used for estimating the composite channels spanning from the K users to the BS. Z_q = [z_{q,1}, z_{q,2}, · · · , z_{q,T} ] ∈ C^{M×T} denotes the noise matrix at the BS during the qth training block.

The composite channel estimation during each block is equivalent to the channel estimation for conventional MU-MISO systems. We employ the mutually orthogonal pilot design to mitigate the interference between multiple users. In order to generate K groups of mutually orthogonal pilot sequences for separating the pilot signals transmitted by K users, the length of the pilot sequence T must satisfy T ≥ K. Furthermore, to minimize the pilot overhead, we consider T = K [51]. The least squares (LS) estimate of the composite channel H_q of the qth training block can be expressed as

~H_q = 1 K √ P_{ul}

Y_qX^H . (15)

2) Transmit Precoding: Based on the estimate of the composite channel in the qth training block, BS performs multi-user transmit precoding by utilizing the ZF precoder:

~W_q = ~H_q ( ~H^H_q ~H_q )_{−1} ~P^12_q , (16) where ~P_q = diag (~p_{1,q}, ~p_{2,q}, · · · , ~p_{K,q}) is the received power allocation matrix and ~p_{k,q} =^{pk,q}_{~uk,q} is the received power of user k when configuring the qth codeword, ~u_{k,q} is the kth diagonal element of ~U_q = ( ~HH_q ~H_q )_{−1} . 3) Optimal Index Selection: Then, after obtaining Q candidate channels and their corresponding transmit precoding matrices, the RIS RC configuration problem can be expressed as

max_q R_q = K∑ k=1 log_2 ( 1 + 1 σ^2_k | |~h_{Hk,q} ~w_{k,q} | |^2 )

s.t. 1 ≤ q ≤ Q. (17) Once the index q̂ of the optimal training block is obtained, we get the RIS RC configuration Φ̂ = Φ_{q̂}, and the corresponding transmit precoding matrix accordingly1.

IV. THEORETICAL ANALYSIS OF THE PROPOSED SCHEME In this section, we analyze the performance of the proposed environment-aware scheme by considering a single user case. We first analyze the theoretical achievable rate considering the noiseless channels in Section IV-A. Then, in Section IV-B, we analyze the influence of channel estimation errors on the proposed channel training scheme.

A. Perfect CSI

Firstly, we examine the scenario where there is no channel estimation error at each training block. For brevity, we assume that the direct BS-user link is blocked and the BS-RIS channel remains only the LoS component which is likely to happen in practical scenarios. Based on the above assumptions, the theoretical received power scaling law is summarized in Proposition 1.

Proposition 1: Assume h_{r,n} following the Rician channel model with Rician factor of F_r , n = 1, 2, · · · , N. For N ≫ 1, the average signal power received by the user is given by P_r =P_dβ_rβ_gMN ( F^2_1 N + F^2_2 (logQ + C) + √ πF_1F_2 ) , (18)

1Note that the RIS configuration is completed by selecting the optimal codeword that maximizes the sum rate. To further boost the performance, one can design appropriate codeword weighting methods to obtain better RIS configuration, which constitutes our future work.

(a) Perfect CSI (b) Imperfect CSI Fig. 4. Conventional channel estimation and passive beamforming scheme. (Red arrow: cascaded channel including the RC configuration)

where P_d is the total transmit power of BS, Q is training overhead, F_1 = √_{Fr} F_r+1 , F2 =

√_1

F_r+1

and C ≈ 0.57722 is the Euler-Mascheroni constant.

Proof: Please refer to Appendix A.

Next, we provide some useful insights into Proposition 1 by considering four special cases: 1) As the Rician factor F_r → 0, the RIS-user channel turns into the Rayleigh channel. In this case, the proposed scheme degenerates to the random phase-shift codebook scheme [22] and the received power P_r → P_dβ_rβ_gMN (logQ + C).

2) As the Rician factor F_r approaches infinity, the RIS-user channel turns into the deterministic LoS channel, which is perfectly aligned according to the statistical CSI. In this case, we have P_r → P_dβ_rβ_gMN^2 which characterizes the quadratic power scaling law versus the number of RIS elements [34].

3) When considering the training overhead of Q = 1, the environment-aware algorithm reduces to the statistical CSI-based scheme [32]. In particular, if F_r → 0, we have P_r = P_dβ_rβ_gMNC, which is equivalent to a random phase shift configuration scenario. If F_r → +∞, we can achieve the power scaling law relying on the optimal RIS configuration, i.e. P_r = P_dβ_rβ_gMN^2.

4) When the training overhead reaches the maximum overhead Q_{max} = 2^{bN} , we arrive at the quadratic scaling law of the average received power at the user with respect to the number of RIS elements N [22], which is comparable to the optimal RIS configuration.

As such, the proposed environment-aware codebook scheme strikes favorable tradeoffs be-

(a) Perfect CSI scenario. (Red arrow: cascaded channel including the RC configuration)

(b) Imperfect CSI scenario. (Green arrow: composite end-to-end channel; Blue dotted arrow: composite channel with error) Fig. 5. The proposed channel training-based protocol.

tween the statistical CSI-based RIS configuration and the optimal RIS configuration method by flexibly adapting the codebook size Q.

B. Imperfect CSI

In this subsection, we analyze the theoretical achievable rate while considering the imperfect CSI. As shown in Fig. 4 and Fig. 5, we provide a scenario of four RIS elements to show the effects of the channel estimation errors.

Firstly, Fig. 4 shows the influence of channel estimation errors on conventional channel estimation and passive beamforming schemes. Observe from Fig. 4(a) that all four cascaded channels with optimal RC configuration, which are denoted by solid red arrows, are aligned when there are no channel estimation errors. In this context, the optimal achievable rate is shown in Eq. (30) of [34]. When taking into account the practical channel estimation errors, we can observe from Fig. 4(b) that the optimal phase shift associated with each RIS element is rotated, which results in the deviation from the perfect case. This results in a loss of achievable rate characterized by Eq. (29) of [23].

By contrast, the influence of channel estimation errors on the proposed environment-aware codebook scheme is shown in Fig. 5, where Fig. 5(a) represents four training blocks in the perfect CSI scenario and the corresponding cases in the imperfect CSI scenario are shown in Fig. 5(b).

Specifically, as shown in Fig. 5, φ_{q,n}, q = 1, · · · , Q, n = 1, 2, 3, 4 represents the RC of the nth RIS element at the qth training block. They rotate the cascaded channels with the corresponding angle to get the results shown by the red arrows. In this case, the achievable rate maximization problem is equivalent to the problem

max_{q∈Q} Y_q = | | | | N∑ n=1 h^∗_{r,n}φ_{q,n}g_{n,m} | | | | 2 . (19)

We calculate Y_q for all Q training blocks and obtain the optimal index i whose theoretical performance is analysed in Proposition 1.

When considering the practical channel estimation errors, it is important to note that for our channel training protocol, the effect of channel estimation errors is not reflected separately at each phase shift. Instead, it distorts the composite end-to-end channels, which is shown by the green arrow. Based on the estimated composite channels (i.e., the dotted blue arrow in Fig. 5(b)), maximizing the achievable rate problem is equivalent to

max_{q∈Q} Ŷ_q = | | | | N∑ n=1 h^∗_{r,n}φ_{q,n}g_{n,m} + ε_q | | | | 2 , (20)

where ε_q ∼ CN ( 0, σ^2_q ) denotes the estimation error of the composite channel in the qth training block. It is noted that the optimal codeword index may not be correctly selected when considering channel estimation errors. In the proposed codebook scheme, the influence of the channel estimation errors is implicitly reflected in the selection of the codeword index, whose impacts are difficult to be accurately characterized. In this paper, a tight upper bound of the achievable rate is derived in Proposition 2.

Proposition 2: Assume h_{r,n} following the Rician channel model with Rician factor of F_r , n = 1, 2, · · · , N. ε_q ∼ CN ( 0, σ^2_q ) , q = 1, 2, · · · , Q is the composite channel estimation error during the qth training block. For N ≫ 1, the average signal power received by the user is given

Fig. 6. Schematic of an RIS-aided multi-user communication scenario.

by P_r = P_dMβ_rβ_g ( N^2F^2_1 + NF_1F_2 √ π

+NF^2_2

N +^π_2 (N − 1) √_{βr βg} (N−1)β_r β_g+σ^2_q

N +^π_2 √ N − 1 (logQ + C) . (21)

Proof: Please refer to Appendix B.

V. SIMULATION RESULTS In this section, we provide numerical simulation results to validate the performance of the proposed scheme. All results are obtained by averaging 1,000 independent experiments. As shown in Fig. 6, we consider an RIS-aided multi-user system. Specifically, the antenna array at the BS is modeled by a ULA and deployed on the z-axis with antenna spacing of d_{BS} = λ/2. The number of the BS antennas is set to M = 8. The RIS is modeled by a UPA and deployed on the y-z plane with 10 × 10 array structure (N = 100) with element spacing of d_R = λ/8. Moreover, the Rician factor of the BS-RIS, RIS-user, and BS-user channels are F_g = 4 dB, F_r = 3 dB, and F_d = −3 dB, respectively. The quantization number of the discrete phase shift set is set to b = 1. The distance from BS to RIS, from each user to the BS-RIS line and between two adjacent users are set to d_{BR} = 100 m, d_0 = 2 m and d_1 = 10 m, respectively. Both the BS and RIS are situated at a height of h_{BS} = h_R = 5 m.

Fig. 7. Achievable rate R of the single user versus training overhead Q, where we consider perfect CSI (The.: theoretical result; Sim.: simulation result).

The path loss of each channel is modeled as [33]

β = C_0(d/d_m)^{−α}, (22)

where d is the distance of the corresponding link, C_0 = −20 dB denotes the path loss of the reference distance d_m = 1 m and α denotes the path loss factor.

We assume that the path loss factor of BS-RIS, RIS-user and BS-user links are α_g = 2.4, α_r = 2.5 and α_d = 3.5, respectively. Moreover, we consider the transmit power at the BS is set to P_d = 40 dBm, the average power of the pilot signals is P_{ul} = −23 dBm, the average noise power at the BS and the user are σ^2_z = −110 dBm and σ^2_k = −90 dBm, respectively.

Firstly, we verify the performance analysis in a single user scenario by only considering User 8 in Fig. 6. As shown in Fig. 7, we verify our analytical results in Section IV-A under different RIS-user channel conditions, where we set F_r = −15 dB, 3 dB, and 15 dB, respectively. It can be seen that the proposed codebook scheme gains an improved achievable rate as the codebook size increases. Moreover, the theoretical result offers a tight upper bound of the simulation result when confronting with diverse channel conditions.

Moreover, Fig. 8 verifies our analytical results in Section IV-B considering the channel estimation errors. It can be seen that the theoretical bound accurately characterizes the environment-

Fig. 8. Achievable rate R of the single user versus training overhead Q, where we consider imperfect CSI (Err.: simulation result with imperfect CSI).

aware codebook scheme for a high Rician factor, e.g., F_r = 15 dB. Besides, in the case of F_r = 3 dB and −15 dB, the theoretical results provide a tight upper bound. Compared to Fig. 7, the performance degradation at F_r = 15 dB is negligible, which implies that the codebook based on statistical CSI achieves optimal performance at high Rician factors. At F_r = 3 dB and −15 dB, there exists moderate performance degradation in the proposed scheme, indicating strong robustness against noise.

Next, as shown in Fig. 9, we compare the sum rate versus total transmit power at BS while activating Users 6 and 8. The Rician factor of the RIS-user link is set to F_r = 10 dB. The training overhead is set to Q = 100. Note that the sum rate is improved as the transmit power increases, and exhibits a logarithmic growth trend. In addition, the proposed scheme outperforms the random codebook scheme in both the perfect and imperfect CSI scenarios. Specifically, a sum rate gain of 1.78 bps/Hz is observed under perfect CSI. This is because the proposed scheme generates the RIS RC codebook by leveraging the statistical CSI.

Next, we evaluate the robustness of the proposed environment-aware codebook-based scheme by considering four different setups in Fig. 10. Note that under all setups, the achievable sum rate increases with the training overhead. Besides, observe from Fig. 10 that the proposed scheme always outperforms the random codebook scheme corresponding to the training overhead Q = 1,

Fig. 9. Sum rate R versus transmit power P_d at the BS (RanC.: random codebook; Pro.: proposed scheme; Random: random configuration; Optimal: optimal configuration).

(a) User k, k = 5, 6, 7, 8. (b) User k, k = 2, 4, 6, 8.

(c) User k, k = 2, 4, 5, 6, 7, 8. (d) User k, k = 6, 8. Fig. 10. Sum rate R versus training overhead Q.

due to the fact that the proposed scheme utilizes the statistical CSI to design the phase shift codebook. Further comparing Figs. 10(a)-10(c) that activating more users results in an improved sum rate, thanks to the multi-user multiplexing gain. For instance, the sum rate increases by 24.90 bps/Hz from activating users 6 and 8 to activating users 5, 6, 7 and 8. Furthermore, we

Fig. 11. Sum rate R versus the number of RIS elements N.

note that the advantage of the proposed scheme over the random codebook scheme is more significant in Figs. 10(a) and 10(d). Both these two cases correspond to activating users near the RIS. Moreover, Fig. 10 shows that the influence caused by the channel estimation errors becomes severe as the training overhead increases, which is consistent with our analysis accounting for the imperfect CSI in Section IV-B.

Next, Fig. 11 compares the sum rate versus the number of RIS elements, considering users 6 and 8 and setting the training overhead to Q = 50. It can be observed that the proposed scheme outperforms the random codebook scheme under all setups. Besides, as the number of RIS elements increases from N = 10 to N = 100, the proposed scheme results in a more significant sum rate improvement with diminishing return, which is due to the fact that a larger number of reflecting elements could reap more radiating energy by coherently superimposing all cascaded links.

Finally, Fig. 12 evaluates the effective sum rate versus the channel coherence time, where we only activate users 6 and 8 and consider four different training overhead scenarios. Here, the effective sum rate is defined by

R_e = T_c − τ T_c E {_K ∑ k=1 log_2 ( 1 + | |h^H_k w_k | |^2 ∑_K l≠k |h H k w_l|^2 + σ^2_k )} , (23)

Fig. 12. The effective sum rate Re versus the channel coherence time Tc.

where T_c is the channel coherence time and τ is the pilot overhead. It can be seen that the proposed scheme can flexibly adapt the pilot overhead in the face of different values of channel coherence time. Specifically, for a rapidly time-varying channel (e.g., T_c ≤ 200), the effective sum rate of the proposed scheme with training overhead Q = 1 attains the best performance. However, as the channel coherence time becomes longer, the increased training overhead can lead to a higher effective sum rate. Therefore, based on the specific coherence time, the proposed scheme can flexibly adjust the training overhead, thus maximizing the effective sum rate.

VI. CONCLUSION In this paper, we have proposed a channel training-based protocol for RIS-assisted MU-MISO systems, where an environment-aware RC codebook is designed. Specifically, during the off-line stage, the proposed scheme generates a set of virtual channels based on the statistical CSI and obtains an environment-aware codebook according to the off-line AO algorithm. Then, during the on-line stage, we have configured the RIS based on the environment-aware codebook and have directly estimated the composite end-to-end channels. Subsequently, we have performed the ZF precoding design at the BS to obtain candidate channels. Finally, the optimal codeword resulting in the highest sum rate has been adopted to configure the RIS for assisting in the data transmission. Furthermore, we have analyzed the performance of the proposed scheme accounting for both the perfect and the imperfect CSI scenarios and have evaluated the achievable

rate of the environment-aware codebook scheme through simulation results. It has been shown

that the proposed scheme has better performance than traditional codebook schemes, and can

strike a favorable trade-off between performance and the training overhead. We highlight that

the proposed scheme can be applied to a wider range of wireless systems including cell-free

massive MIMO systems and OFDM systems by leveraging the statistical CSI therein [19], [46],

[52], [53].

APPENDIX A

PROOF OF PROPOSITION 1

By applying the assumptions of Proposition 1, let Q = {1, 2, · · · , Q}, the average received

power P_r at the single user with codebook based RC configuration can be expressed as

P_r = P_dE { max_{q∈Q} ‖h^H_r Φ_qG‖^2 } . (24)

Due to the fact that the maximum value of the sum does not exceed the sum of the maximum

values, (24) can be further written as

P_r = P_dE max_{q∈Q} ‖ ‖ ‖ ‖ N∑ n=1 h^∗_{r,n}φ_{q,n}g^T_n ‖ ‖ ‖ ‖ 2

≤ P_dE M∑ m=1 max_{q∈Q} | | | | N∑ n=1 h^∗_{r,n}φ_{q,n}g_{n,m} | | | | 2

= P_dβ_rβ_gME max_{q∈Q} | | | | N∑ n=1 h^∗_{r,n}φ_{q,n}g_{n,m} | | | | 2 , (25)

where g^T_n is the nth row of G and ‘≤’ reduces to ‘=’ if and only if rank(G) = 1; h_{r,n} and

g_{n,m} are the nth entry of h_r and g_m, respectively; h^∗_{r,n} and g_{n,m} denote their normalized results,

respectively. φ_{q,n} is the nth entry on the diagonal of Φ_q.

Since we have h^∗_{r,n} = F_1 ( h^{LoS}_{r,n} )_∗ + F_2 ( h^{NLoS}_{r,n} )_∗ and g_{n,m} = g^{LoS}_{n,m}, | | | ∑_N n=1 h^∗_{r,n}φ_{q,n}g_{n,m} | | |^2 can be further written as | | | | N∑ n=1 h^∗_{r,n}φ_{q,n}g_{n,m} | | | | 2

= | | | | N∑ n=1 ( F_1 ( h^{LoS}_{r,n} )_∗ + F_2 ( h^{NLoS}_{r,n} )_∗) φ_{q,n}g^{LoS}_{n,m} | | | | 2

= | | | | N∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} | | | | 2 + | | | | N∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} | | | | 2

+ 2ℜ {(_N ∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} )_∗

× (_N ∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} )} . (26)

Note that we adopt the environment-aware scheme relying on the statistical CSI. In each

channel training block, we generate the NLoS component of the RIS-user channel and configure

the phase shift of the nth RIS element as θ_{q,n} = ∠ (√ F_rh^{LoS}_{r,n} + h̃^{NLoS}_{r,q,n} ) − ∠ ( g^{LoS}_{n,m} ) , (27)

where h̃^{NLoS}_{r,q,n} is the random NLoS component generated off-line. Thus when considering the

Rayleigh fading in the proposed scheme, it is equivalent to adopting a random phase-shift

configuration codebook.

Then, we consider the three terms of (26) separately. Specifically, for the first entry of (26),

the LoS component of multiple reflected channels is largely aligned thus it can be expressed as

E max_{q∈Q} | | | | N∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} | | | | 2

= F^2_1 | | | | N∑ n=1 | |(h^{LoS}_{r,n} )^∗ | | | |g^{LoS}_{n,m} | | | | | | 2 = F^2_1 N^2. (28)

The other two entries of (26) are related to the NLoS component, where we can obtain ∑_N n=1 φ_{q,n} ( h^{NLoS}_{r,n} )_∗ g^{LoS}_{n,m} ∼ CN (0, N) as N → ∞ based on Lindeberg-Levy central limit

theorem [34].

Specifically, the second entry reflects the effects on the NLoS component of the channel.

According to Lemma 1 in [22], we have

max_{q∈Q} | | | | N∑ n=1 φ_{q,n} ( h^{NLoS}_{r,n} )_∗ g^{LoS}_{n,m} | | | | 2 d= N Q∑ j=1 1 Q − j + 1 ρ_j , (29)

where ρ_j are i.i.d. standard exponential random variables with a rate parameter of 1. Thus we

have E {ρ_j } = 1 and it can be obtained that

E max_{q∈Q} | | | | N∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} | | | | 2

=F^2_2 E { N Q∑ j=1 1 Q − j + 1 ρ_j }

=F^2_2 N (logQ + C) . (30)

Since we have E {∑_N n=1 φ_{q,n} ( h^{NLoS}_{r,n} )_∗ g^{LoS}_{n,m} } = 0, the third entry of (26) can be further derived as E { max_{q∈Q} 2ℜ {(_N ∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} )_∗

× (_N ∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} )}}

=2F_1F_2ℜ { E { max_{q∈Q} {_N ∑ n=1 |φ_{q,n}|^2 h^{LoS}_{r,n} ( h^{NLoS}_{r,n} )_∗ | g^{LoS}_{n,m} | |^2 + (_N ∑ i=1 φ_{q,i} ( h^{NLoS}_{r,i} )_∗ g^{LoS}_{i,m} ) (_N ∑ j≠i φ^∗_{q,j}h^{LoS}_{r,j} (g^{LoS}_{j,m})^∗ )}}}

(a) =2F_1F_2ℜ { E {_N ∑ n=1 h^{LoS}_{r,n} ( h^{NLoS}_{r,n} )_∗ }}

(b) <2F_1F_2 N∑ n=1 (| h^{LoS}_{r,n} | E {| (h^{NLoS}_{r,n} )^∗ |})

(c) = √ πF_1F_2N, (31)

where (a) holds because we have E {∑_N i=1 φ_{q,i} ( h^{NLoS}_{r,i} )_∗ g^{LoS}_{i,m} } = 0, | |g^{LoS}_{n,m} | | = 1 and |φ_{q,n}| = 1;

(b) holds as we have ℜ { E {∑_N n=1 h^{LoS}_{r,n} ( h^{NLoS}_{r,n} )_∗}} < ∑_N n=1 E { ℜ { h^{LoS}_{r,n} }} E { ℜ {( h^{NLoS}_{r,n} )_∗}} , ℜ { h^{LoS}_{r,n} } ≤ | |hLoS_{r,n} | | and ℜ {(hNLoS_{r,n} )^∗} ≤ | |(hNLoS_{r,n} )∗ | |; Moreover, equality (c) holds due to the fact

that | |(hNLoS_{r,n} )^∗ | | follows Rayleigh distribution with mean value of √π/2.

Substituting (28), (30) and (31) into (26), the proof is completed. ■

APPENDIX B

PROOF OF PROPOSITION 2

Similar to (26), the average received power P_r of the single user when considering channel

estimation errors is given by

P_r = P_dβ_rβ_gME | | | | N∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q̂,n}g^{LoS}_{n,m} | | | | 2

+ | | | | N∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q̂,n}g^{LoS}_{n,m} | | | | 2

+2ℜ {(_N ∑ n=1 F_1 ( h^{LoS}_{r,n} )_∗ φ_{q̂,n}g^{LoS}_{n,m} )_∗

× (_N ∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q̂,n}g^{LoS}_{n,m} )}} , (32)

where φ_{q̂,n} is the RC with selected index q̂ for the nth RIS element in the presence of channel

estimation errors, which is obtained by

φ_{q̂,n} = arg max_{q∈Q} | | | | N∑ i≠n h^∗_{r,i}φ_{q,i}g_{i,m} + h^∗_{r,n}φ_{q,n}g_{n,m} + ε_q | | | | 2 , (33)

where φ_{q,n} represents the RC of the nth RIS element at the qth training block, and φ_{q,i}, i ≠ n

represent the fixed (N −1) RCs when optimizing φ_{q,n}. ε_q ∼ CN ( 0, σ^2_q ) is the composite channel

estimation error in the qth training block.

Then, as illustrated in Fig. 5, we select the optimal RC configuration maximizing the sum

rate in the imperfect CSI scenario. Since the codewords are obtained based on the statistical

CSI, the first entry of (32) is equal to that without channel estimation errors. Moreover, as we

have E {∑_N i=1 ( h^{NLoS}_{r,n} )_∗ φ_{q̂,i}g^{LoS}_{i,m} } = 0, the result of the third part remains the same with that

considering perfect CSI, i.e., (31).

Under imperfect CSI conditions, the second entry of (32) still follows an exponential distribu-

tion at each training block. However, the Qth order statistics is a scaling version of that in (32).

Let u denote the scaling factor. Specifically, we first consider the effect of the channel estimation

errors on a single RC, keeping the remaining (N−1) terms fixed, i.e., ∑_N i≠n √ β_r(h^{NLoS}_{r,i} )^∗φ_{q,i} √ β_gg^{LoS}_{i,m} ∼ CN (0, (N − 1)β_rβ_g). Next, we derive the scaling factor to characterize the influence of the

channel estimation errors.

Let h^∗_{c,n} = √ β_r(h^{NLoS}_{r,n} )^∗ √ β_gg^{LoS}_{n,m} represent the NLoS component of the cascaded channel

spanning from the user to the BS through the nth RIS element. Hence, by solving (19), it is

straightforward to obtain the optimal RC for the nth RIS element φ̄_{q,n} =^{hc,n}|_{h∗c,n}| ∑_N i≠n h ∗ c,iφ_{q,i} |^{∑N}_{i≠n} h^∗_{c,i}φq,i|, and the second term in (32) can be simplified to

u_o ≜ | | | | N∑ i≠n h^∗_{c,i}φ_{q,i} + h^∗_{c,n}φ̄_{q,n} | | | | 2

= | | | | N∑ i≠n h^∗_{c,i}φ_{q,i} | | | | 2 + |h_{c,n}|^2 + 2ℜ {| | | N∑ i≠n h_{c,i}φ^∗_{q,i} | | | | | h^∗_{c,n} | } . (34)

Moreover, we obtain the optimal RC under imperfect CSI by solving (20), i.e., φ̂_{q,n} = h_{c,n} |h^∗c,n| ∑_N i≠n h ∗ c,iφ_{q,i}+ε_q |^{∑N}_{i≠n} h^∗_{c,i}φq,i+εq|, we have

u_e ≜ | | | | | N∑ i≠n h^∗_{c,i}φ_{q,i} + h^∗_{c,n}φ̂_{q,n} | | | | | 2

= | | | | | N∑ i≠n h^∗_{c,i}φ_{q,i} | | | | | 2 + | |h^∗_{c,n} | |^2

+2ℜ N∑ i≠n h_{c,i}φ^∗_{q,i} | |h^∗_{c,n} | | ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | |∑N_{i≠n} h_{∗c,i}φ_{q,i} + ε_q | | . (35)

The expectation of the third entry in (35) can be expressed as

E 2ℜ N∑ i≠n h_{c,i}φ^∗_{q,i} | |h^∗_{c,n} | | ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | | ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | | = 2E | |h^∗_{c,n} | | ℜ N∑ i≠n h_{c,i}φ^∗_{q,i} ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | | ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | | . (36)

According to the assumptions of h^∗_{c,n} ∼ CN (0, β_rβ_g) , n = 1, 2, · · · , N, ∑_N i≠n hc,iφ ∗ q,i ∼ CN (0, (N − 1)β_rβ_g), ε_q ∼ CN ( 0, σ^2_q ) , q = 1, 2, · · · , Q, we have

E | | | | N∑ i≠n h^∗_{c,i}φ_{q,i} | | | | 2 = (N − 1)β_rβ_g,

E {| |h^∗_{c,n}|^2 } = β_rβ_g, E {| h^∗_{c,n} |} = √ π 2 √ β_rβ_g, E { ℜ {| | | | N∑ i≠n h_{c,i}φ^∗_{q,i} | | | | | |h^∗_{c,n} | | }} = π 4 √ N − 1β_rβ_g,

E ℜ N∑ i≠n h_{c,i}φ^∗_{q,i} ∑_N i≠n h ∗ c,iφ_{q,i} + ε_q | |∑N_{i≠n} h_{∗c,i}φ_{q,i} + ε_q | | = √ π(N − 1)β_rβ_g 2 √ (N − 1)β_rβ_g + σ^2_q

. (37)

As a result, the scaling factor is obtained by u ≜ E {u_e} E {u_o} = N +^π_2 (N − 1) √_{βrβg} (N−1)β_r β_g +σ^2_q

N +^π_2 √ N − 1 . (38)

Applying (38) to the second entry of (32), we arrive at

E | | | | N∑ n=1 F_2 ( h^{NLoS}_{r,n} )_∗ φ_{q̂,n}g^{LoS}_{n,m} | | | | 2

< F^2_2 uE max_{q∈Q} | | | | N∑ n=1 ( h^{NLoS}_{r,n} )_∗ φ_{q,n}g^{LoS}_{n,m} | | | | 2

= F^2_2

N +^π_2 (N − 1) √_{βrβg} (N−1)β_r β_g +σ^2_q

N +^π_2 √ N − 1 N(logQ + C). (39)

Combining the three entries in (32), the proof is completed. ■

REFERENCES

[1] Z. Yu, J. An, L. Gan, and C. Yuen, “Environment-aware codebook for RIS-assisted MU-MISO communications:

Implementation and performance analysis,” arXiv preprint arXiv:2404.00265, 2024.

[2] T. Cui, S. Jin, J. Zhang et al., “Research report on reconfigurable intelligent surface (RIS),” IMT-2030 (6G) Promotion Group, Sep. 2021.

[3] Y. Liu, X. Liu, X. Mu, T. Hou, J. Xu, M. Di Renzo, and N. Al-Dhahir, “Reconfigurable intelligent surfaces: Principles and opportunities,” IEEE Commun. Surv. Tutor., vol. 23, no. 3, pp. 1546–1577, May. 2021.

[4] E. Basar, M. Di Renzo, J. De Rosny, M. Debbah, M.-S. Alouini, and R. Zhang, “Wireless communications through reconfigurable intelligent surfaces,” IEEE Access, vol. 7, pp. 116 753–116 773, Aug. 2019.

[5] F. Boccardi, R. W. Heath, A. Lozano, T. L. Marzetta, and P. Popovski, “Five disruptive technology directions for 5G,” IEEE Commun. Mag., vol. 52, no. 2, pp. 74–80, Feb. 2014.

[6] Q. Wu and R. Zhang, “Towards smart and reconfigurable environment: Intelligent reflecting surface aided wireless network,” IEEE Commun. Mag., vol. 58, no. 1, pp. 106–112, Aug. 2019.

[7] E. Björnson, Ö. Özdogan, and E. G. Larsson, “Intelligent reflecting surface versus decode-and-forward: How large surfaces are needed to beat relaying?” IEEE Wireless Commun. Lett., vol. 9, no. 2, pp. 244–248, Nov. 2019.

[8] E. Shi, J. Zhang, H. Du, B. Ai, C. Yuen, D. Niyato, K. B. Letaief et al., “RIS-aided cell-free massive MIMO systems for 6G: Fundamentals, system design, and applications,” arXiv preprint arXiv:2310.00263, 2023.

[9] M. Di Renzo, A. Zappone, M. Debbah, M.-S. Alouini, C. Yuen, J. De Rosny, and S. Tretyakov, “Smart radio environments empowered by reconfigurable intelligent surfaces: How it works, state of research, and the road ahead,” IEEE J. Sel. Areas Commun., vol. 38, no. 11, pp. 2450–2525, Apr. 2020.

[10] S. Li, B. Duo, M. Di Renzo, M. Tao, and X. Yuan, “Robust secure UAV communications with the aid of reconfigurable intelligent surfaces,” IEEE Trans. Wireless Commun., vol. 20, no. 10, pp. 6402–6417, Apr. 2021.

[11] W. Tang, J. Y. Dai, M. Z. Chen, K.-K. Wong, X. Li, X. Zhao, S. Jin, Q. Cheng, and T. J. Cui, “MIMO transmission through reconfigurable intelligent surface: System design, analysis, and implementation,” IEEE J. Sel. Areas Commun., vol. 38, no. 11, pp. 2683–2699, Nov. 2020.

[12] S. Kayraklık, I. Yildirim, Y. Gevez, E. Basar, and A. Görçin, “Indoor coverage enhancement for RIS-assisted communication systems: Practical measurements and efficient grouping,” in Proc. 2023 IEEE Int. Conf. Commun. (ICC), May. 2023, pp. 1–6.

[13] J. An, C. Yuen, C. Xu, H. Li, D. W. K. Ng, M. D. Renzo, M. Debbah, and L. Hanzo, “Stacked intelligent metasurface-aided MIMO transceiver design,” IEEE Wireless Commun., pp. 1–9, 2024, Early Access.

[14] J. An, C. Xu, D. W. K. Ng, G. C. Alexandropoulos, C. Huang, C. Yuen, and L. Hanzo, “Stacked intelligent metasurfaces for efficient holographic MIMO communications in 6G,” IEEE J. Sel. Areas Commun., Aug. 2023.

[15] J. An, M. Di Renzo, M. Debbah, H. V. Poor, and C. Yuen, “Stacked intelligent metasurfaces for multiuser downlink beamforming in the wave domain,” arXiv preprint arXiv:2309.02687, May. 2023.

[16] J. An, C. Yuen, C. Huang, M. Debbah, H. Vincent Poor, and L. Hanzo, “A tutorial on holographic MIMO communications—part I: Channel modeling and channel estimation,” IEEE Commun. Lett., vol. 27, no. 7, pp. 1664–1668, May. 2023.

[17] S. Zhang and R. Zhang, “Capacity characterization for intelligent reflecting surface aided MIMO communication,” IEEE J. Sel. Areas Commun., vol. 38, no. 8, pp. 1823–1838, Aug. 2020.

[18] C. Huang, A. Zappone, G. C. Alexandropoulos, M. Debbah, and C. Yuen, “Reconfigurable intelligent surfaces for energy efficiency in wireless communication,” IEEE Trans. Wireless Commun., vol. 18, no. 8, pp. 4157–4170, Jun. 2019.

[19] E. Shi, J. Zhang, R. He, H. Jiao, Z. Wang, B. Ai, and D. W. K. Ng, “Spatially correlated reconfigurable intelligent surfaces-aided cell-free massive MIMO systems,” IEEE Trans. Veh. Technol., vol. 71, no. 8, pp. 9073–9077, Aug. 2022.

[20] E. Shi, J. Zhang, D. W. K. Ng, and B. Ai, “Uplink performance of RIS-aided cell-free massive MIMO system with electromagnetic interference,” IEEE J. Sel. Areas Commun., vol. 41, no. 8, pp. 2431–2445, Jun. 2023.

[21] C. You, B. Zheng, and R. Zhang, “Channel estimation and passive beamforming for intelligent reflecting surface: Discrete phase shift and progressive refinement,” IEEE J. Sel. Areas Commun., vol. 38, no. 11, pp. 2604–2620, Mar. 2020.

[22] J. An and L. Gan, “The low-complexity design and optimal training overhead for IRS-assisted MISO systems,” IEEE Wireless Commun. Lett., vol. 10, no. 8, pp. 1820–1824, May. 2021.

[23] J. An, C. Xu, L. Wang, Y. Liu, L. Gan, and L. Hanzo, “Joint training of the superimposed direct and reflected links in reconfigurable intelligent surface assisted multiuser communications,” IEEE Trans. Green Commun. Netw., vol. 6, no. 2, pp. 739–754, Jun. 2022.

[24] Z. Wang, L. Liu, and S. Cui, “Channel estimation for intelligent reflecting surface assisted multiuser communications:

Framework, algorithms, and analysis,” IEEE Trans. Wireless Commun., vol. 19, no. 10, pp. 6607–6620, Jun. 2020. [25] D. Mishra and H. Johansson, “Channel estimation and low-complexity beamforming design for passive intelligent surface assisted MISO wireless energy transfer,” in Proc. IEEE Int. Conf. on Acoust., Speech and Signal Process. (ICASSP). IEEE, Apr. 2019, pp. 4659–4663.

[26] C. Xu, J. An, T. Bai, S. Sugiura, R. G. Maunder, Z. Wang, L.-L. Yang, and L. Hanzo, “Channel estimation for reconfigurable intelligent surface assisted high-mobility wireless systems,” IEEE Trans. Veh. Technol., vol. 72, no. 1, pp. 718–734, Jan. 2023.

[27] X. Wei, D. Shen, and L. Dai, “Channel estimation for RIS assisted wireless communications—part II: An improved solution based on double-structured sparsity,” IEEE Commun. Lett., vol. 25, no. 5, pp. 1403–1407, May. 2021.

[28] Y. Guo, P. Sun, Z. Yuan, C. Huang, Q. Guo, Z. Wang, and C. Yuen, “Efficient channel estimation for RIS-aided MIMO communications with unitary approximate message passing,” IEEE Trans. Wireless Commun., Feb. 2023.

[29] J. Chen, Y.-C. Liang, H. V. Cheng, and W. Yu, “Channel estimation for reconfigurable intelligent surface aided multi-user mmWave MIMO systems,” IEEE Trans. Wireless Commun., Oct. 2023.

[30] W. Xu, J. An, Y. Xu, C. Huang, L. Gan, and C. Yuen, “Time-varying channel prediction for RIS-assisted MU-MISO networks via deep learning,” IEEE Trans. Cogn. Commun. Netw., vol. 8, no. 4, pp. 1802–1815, Dec. 2022.

[31] J. An, H. Li, D. W. K. Ng, and C. Yuen, “Fundamental detection probability vs. achievable rate tradeoff in integrated sensing and communication systems,” IEEE Trans. Wireless Commun., vol. 22, no. 12, pp. 9835–9853, Dec. 2023.

[32] Y. Han, W. Tang, S. Jin, C.-K. Wen, and X. Ma, “Large intelligent surface-assisted wireless communication exploiting statistical CSI,” IEEE Trans. Veh. Technol., vol. 68, no. 8, pp. 8238–8242, Aug. 2019.

[33] J. An, C. Xu, L. Gan, and L. Hanzo, “Low-complexity channel estimation and passive beamforming for RIS-assisted MIMO systems relying on discrete phase shifts,” IEEE Trans. Wireless Commun., vol. 70, no. 2, pp. 1245–1260, Feb. 2022.

[34] Q. Wu and R. Zhang, “Intelligent reflecting surface enhanced wireless network via joint active and passive beamforming,” IEEE Trans. Wireless Commun., vol. 18, no. 11, pp. 5394–5409, Nov. 2019.

[35] H. Alwazani, A. Kammoun, A. Chaaban, M. Debbah, M.-S. Alouini et al., “Intelligent reflecting surface-assisted multi-user MISO communication: Channel estimation and beamforming design,” IEEE Open J. Commun. Soc., vol. 1, pp. 661–680, May. 2020.

[36] K. Zhi, C. Pan, H. Ren, and K. Wang, “Statistical CSI-based design for reconfigurable intelligent surface-aided massive MIMO systems with direct links,” IEEE Wireless Commun. Lett., vol. 10, no. 5, pp. 1128–1132, May. 2021.

[37] B. Di, H. Zhang, L. Song, Y. Li, Z. Han, and H. V. Poor, “Hybrid beamforming for reconfigurable intelligent surface based multi-user communications: Achievable rates with limited discrete phase shifts,” IEEE J. Sel. Areas Commun., vol. 38, no. 8, pp. 1809–1822, Jun. 2020.

[38] N. I. Miridakis, T. A. Tsiftsis, and R. Yao, “Zero forcing uplink detection through large-scale RIS: System performance and phase shift design,” IEEE Trans Commun, Jan. 2023.

[39] W. Xu, J. An, C. Huang, L. Gan, and C. Yuen, “Deep reinforcement learning based on location-aware imitation environment for RIS-aided mmWave MIMO systems,” IEEE Wireless Commun. Lett., vol. 11, no. 7, pp. 1493–1497, Jul. 2022.

[40] T. Fang and Y. Mao, “A low-complexity beamforming design for beyond-diagonal RIS aided multi-user networks,” IEEE Commun. Lett., Nov. 2023.

[41] M. Nerini, S. Shen, and B. Clerckx, “Discrete-value group and fully connected architectures for beyond diagonal reconfigurable intelligent surfaces,” IEEE Trans. Veh. Technol., Jul. 2023.

[42] X. Jia, J. An, H. Liu, H. Liao, L. Gan, and C. Yuen, “Environment-aware codebook for reconfigurable intelligent surfaceaided MISO communications,” IEEE Wireless Commun. Lett., vol. 12, no. 7, pp. 1174–1178, Jul. 2023.

[43] S. Shen, B. Clerckx, and R. Murch, “Modeling and architecture design of reconfigurable intelligent surfaces using scattering parameter network analysis,” IEEE Trans. Wireless Commun., vol. 21, no. 2, pp. 1229–1243, Feb. 2022.

[44] N. K. Kundu, Z. Li, J. Rao, S. Shen, M. R. McKay, and R. Murch, “Optimal grouping strategy for reconfigurable intelligent surface assisted wireless communications,” IEEE Wireless Commun. Lett., vol. 11, no. 5, pp. 1082–1086, Nov. 2021.

[45] C. Xu, J. An, T. Bai, S. Sugiura, R. G. Maunder, L.-L. Yang, M. Di Renzo, and L. Hanzo, “Antenna selection for reconfigurable intelligent surfaces: A transceiver-agnostic passive beamforming configuration,” IEEE Trans. Wirel. Commun., vol. 22, no. 11, pp. 7756–7774, Nov. 2023.

[46] J. An, C. Xu, Q. Wu, D. W. K. Ng, M. Di Renzo, C. Yuen, and L. Hanzo, “Codebook-based solutions for reconfigurable intelligent surfaces and their open challenges,” IEEE Wirel Commun, Nov. 2022.

[47] F. Wang, X. Wang, X. Li, X. Hou, L. Chen, S. Suyama, and T. Asai, “Ring-type codebook design for reconfigurable intelligent surface near-field beamforming,” in Proc. IEEE 33rd Annual International Symposium on Personal, Indoor and Mobile Radio Communications (PIMRC). IEEE, Sep. 2022, pp. 391–396.

[48] J. An, C. Yuen, L. Dai, M. D. Renzo, M. Debbah, and L. Hanzo, “Near-field communications: Research advances, potential, and challenges,” IEEE Wireless Commun., 2024.

[49] A. Abdallah, A. Celik, M. M. Mansour, and A. M. Eltawil, “Deep reinforcement learning based beamforming codebook design for RIS-aided mmWave systems,” in Proc. IEEE 20th Consumer Commun. Netw. Conf. (CCNC). IEEE, Mar. 2023, pp. 1020–1026.

[50] G. Wang, W. Peng, D. Li, T. Jiang, and F. Adachi, “Statistical CSI acquisition in the nonstationary massive MIMO environment,” IEEE Trans. Veh. Technol., vol. 67, no. 8, pp. 7181–7190, Aug. 2018.

[51] H. Yin, D. Gesbert, M. Filippou, and Y. Liu, “A coordinated approach to channel estimation in large-scale multiple-antenna systems,” IEEE J. Sel. Areas Commun., vol. 31, no. 2, pp. 264–273, Jan. 2013.

[52] J. An, C. Xu, D. W. K. Ng, C. Yuen, and L. Hanzo, “Adjustable-delay RIS is capable of improving OFDM systems,” IEEE Trans. Veh. Technol., pp. 1–16, 2024, Early Access.

[53] W. Xu et al., “Algorithm-unrolling-based distributed optimization for RIS-assisted cell-free networks,” IEEE Int. Things J., vol. 11, no. 1, pp. 944–957, Jan. 2024.