arXiv:2409.02000v1 [physics.optics] 3 Sep 2024

The Non-reciprocity of Multi-mode Optical Directional Amplifier Realized by Non-Hermitian Resonator Arrays

Jin-Xiang Xue^1, Chuan-Xun Du^{1,3},^∗ Chengchao Liu^1, Liu Yang^1, and Yong-Long Wang^{1,2,3†} 1 School of Physics and Electronic Engineering, Linyi University, Linyi, 276005, China 2 Department of Physics, Nanjing University, Nanjing 210093, China and 3 National Laboratory of Solid State Microstructures, Department of Materials Science and Engineering, Nanjing University, Nanjing, 210093, China

In the present paper, a multi-frequency optical non-reciprocal transmission is first realized by using a non-Hermitian multi-mode resonator array.We find that the non-reciprocity can be used to route optical signals, to prevent the reverse flow of noise, and find that the multi-frequency can be used to enhance information processing. In terms of the Scully-Lamb model and gain saturation effect, we accomplish a dual-frequency non-reciprocal transmission by introducing nonlinearity into a linear array of four-mode resonators. For example, a directional cyclic amplifier is constructed with non-reciprocal units. As potential applications, the non-reciprocity optical systems can be employed in dual-frequency control, parallel information processing, photonic integrated circuits, optical devices and so on.

PACS Numbers: XXXXXXX

I. INTRODUCTION

Optical systems can be widely applied in scientific research and engineering, such as optical communication, optical imaging, optical sensing and so on. Particularly, the photons are employed in information calculation and transmission for the high bandwidth and low loss. [1, 2]. Recently, the non-Hermitian optical system is of great interests of experts in optics[1, 3–5], because that the gain and loss are easily controlled in optical systems. Specifically, a circulator and directional amplifier of fiber-coupled silicon dioxide micro-resonators was realized[6] for a single frequency optical signal. While multi-frequency directional cyclic amplifiers still need further investigations in optical nonlinearity.

The reciprocity of an optical system means that the response of the system does not change when the light wave is backpropagated along the direction of propagation[7]. The reciprocity is valuable in many optical systems and devices, but in special cases the non-reciprocity plays an important role in optical devices, in which light waves propagate considerably different forward and backward[8–10]. The non-reciprocity is important in photonic information processing to route optical signals or prevent the reverse flow of noise. The nonreciprocal characteristics of light can be applied to optical devices[11–13], in which signal transmission and reverse isolation can be achieved in a specific direction, and the interference effect can be effectively reduced to protect the signal source from noise interference. As a result, the non-reciprocal optical devices are more accurate and reliable, which is of great significance in the research of communication technology, information processing,

∗ Email: duchuanxun@lyu.edu.cn † Email: wangyonglong@lyu.edu.cn

precision measurement and topological photonics[12–17]. Various non-reciprocal devices were realized for singlefrequency[6, 18–20], but the multi-channel information processing capability still needs to improve the nonreciprocal optical devices that are easily integrated in optical chips. Therefore, the micro-non-magnetic devices need further investigations to own multi-frequency nonreciprocal characteristics[21].

In the presence of magnetic field, the non-reciprocity can be generated by a variety of low power nonmagnetization methods[22–26], which can be achieved by magnetic field[21, 27, 28], the dynamic modulation of dielectric constant[12, 24, 27, 29, 30], optical nonlinearity[17, 31–33] and so on. In terms of dynamic modulation permittivity and optical nonlinearity, the non-reciprocal mechanics was applied to superconducting microwave circuits[18, 34–38]. For potential applications, it should be first considered that is integration, stability, controllability and other aspects. As the magnetic field absences, the previous achievements become more difficult. However, the high integration, strong stability and easy controllability can be easily achieved in optical devices by using the optical nonlinear effect[16]. For a parity time-symmetric photonic device consisting of two resonators[39], the light propagation was analyzed by the non-Lindbladian master equation of the Scully- Lamb laser model. By semi-classical approximation, two nonlinear coupled differential equations were obtained for the field evolution in a cavity, which can explain the nonreciprocity[40], and demonstrate that the gain saturation effect is the key mechanism of non-reciprocity[39]. It is worthwhile to notice that the known non-reciprocity phenomenon mostly appears at the non-divergent peak of a single frequency. In our work[41], a series of PTsymmetric one-dimensional multimode resonator arrays were built and the transmission spectra was discussed. In the system, the non-reciprocal phenomenon can be achieved by the gain saturation effect. We tried to replace the transition point of the PT unbroken phase by that of broken phase in the parameter space, and realized multiple non-divergent peaks in the transmission spectrum. The results may provide a way to design multi-frequency non-reciprocal devices.

In the present paper, we will try to construct a dualfrequency non-reciprocal optical system by using a non- Hermitian multimode resonator array. In terms of the Scully-Lamb model, we will give a nonlinear equation by introducing a nonlinear term into the original linear equation. With the gain saturation effect[39] and the non- Hermitic resonator array model, the known two-mode resonator system can be extended to a four-mode resonator system. And then the optical non-reciprocity of two frequencies can be achieved. This phenomenon can not only be applied to photodiodes, but also the dualfrequency non-reciprocity phenomenon and the parallel processing of multiple information. And the system can be used to build multi-mode optical directional amplifier and isolators[8, 22, 38, 42–44]. The amplifier structure, shown in Figure 1, consists of an optical fiber coupled with a silicon dioxide ring microresonator with four ports. The signal can be input from one port, the output signal can be detected from the others, and the signal will be amplified with different times for different output ports. If only two of the ports are taken, the function of the isolator can be realized. The function of directional amplifier can be realized by controlling the frequency mismatch between the input light and the cavity resonance. Compared with other directional amplifiers, this system has several advantages, such as dual-frequency control, circulability, and easy integration.

The paper is organized as follows. In Sec. II, the basic model and the linear dynamics equations are briefly introduced. In Sec. III, the theoretical basis of the system is given, and the dual-frequency non-reciprocal transmission can be achieved by a four-mode resonator system, due to the presence of the nonlinear gain saturation. In Sec. IV, a non-reciprocal double-frequency system is constructed and investigated. In Sec. V, conclusions and discussions are given.

II. BASIC MODEL AND LINEAR DYNAMIC EQUATION

As a basic model, a ring resonator array will be considered in this section, and its linear dynamic equations will be discussed. With the linear equations, the position and type of resonance peaks can be determined. In terms of the Scully-Lamb model, by introducing nonlinear terms, the considered model can give rise to nonreciprocal transmission phenomena. The result plays an important role in the present paper. Specifically, the model introduced nonlinear terms can be taken as fundamental elements to construct complex multi-mode nonreciprocal transmission systems and subsequent multimode unidirectional amplifiers.

FIG. 1. Setup of the one-dimensional array of ring resonators. The resonators labeled as R_1 ∼ R_N are coupled with each other with coupling strength κ_{ij} . The coupling loss between waveguide WG1(WG2) and resonator R_1(R_N ) is γ_c.

The considered system is a linear array of N coupled resonators depicted in Fig. 1. In comparing with the work referenced in [40], it is significant that moves from a two-mode to a multi-mode configuration. The passive resonators, which are lossy, can be crafted from silica, while the active resonators, which provide gain, can be made from an erbium-ion-doped silica film. This film is fabricated by the sol-gel technique, where the solution is prepared by blending tetraethoxysilane with isopropanol alcohol, water, and hydrochloric acid. The resonators are in turn denoted as R_1 ∼ R_N , and they have the same frequency ω_0, and their couplings just occur between adjacent resonators, the coupling parameter can be described by the real-valued parameter κ_{i,j} . The internal loss of the ith resonator is given by γ^′_i = ω_0/Q_i being Q_i the Q-factor, and the gain provided by optical pumping is denoted as g^′_i. In addition, the first and last resonators experience a loss γ_c due to their connection with the waveguides WG1 and WG2, respectively. The net gain or loss for the ith resonator can be encapsulated in a single parameter γ_i = g^′_i − γ^′_i − γ_c(δ_{i,1} + δ_{i,N} ) , where gain is indicated by γ_i > 0 and loss by γ_i < 0. The probe signal is introduced through port 1, and the resulting signal can be monitored at port 3 or 4, contingent upon the value of N being even or odd. The coupling strength between the first resonator and the input signal’s driving field, characterized by power P and frequency ω_{in}, is represented by ϵ, with the relationship defined as ϵ ≡ √ γ_cP/h̄ω_{in}. When the input power P does not surpass the threshold for gain saturation effects [45], and as long as the resonator peaks remain bounded, the gain within the active cavity behaves linearly. As a consequence, the dynamics of the optical field can be expressed as a set of linear equations [39, 40, 46],

∂a_n ∂t = − iω_0a_1 + γ_1a_1 + iκ_{1,2}a_2 − ϵexp(−iω_{in}t) (n =1), − iω_0a_n + γ_na_n + iκ_{n,n+1}a_{n+1} + iκ_{n,n−1}a_{n−1} (1 < n <N), − iω_0a_N + γ_N a_N + iκ_{N,N−1}a_{N−1} (n =N), (1)

By substituting a_n = A_nexp(−iω_{in}t) into Eq.(1), the dynamical equations for the field amplitude can be obtained, ∂A_n ∂t = iΔ_{in}A_1 + γ_1A_1 + iκ_{1,2}A_2 − ϵ (n =1), iΔ_{in}A_n + γ_nA_n + iκ_{n,n+1}A_{n+1} + iκ_{n,n−1}A_{n−1} (1 < n <N), iΔ_{in}A_N + γ_N A_N + iκ_{N,N−1}A_{N−1} (n =N), (2)

where Δ_{in} = ω_{in} − ω_0 is the frequency-detuning parameter. In the steady state ∂A_n/∂t = 0, from Eq.(2) one can obtain a series of linear equations in the following form

iΔ_{in}A_1 + γ_1A_1 + iκ_{1,2}A_2 = ϵ (n = 1), iΔ_{in}A_n + γ_nA_n + iκ_{n,n+1}A_{n+1} + iκ_{n,n−1}A_{n−1} = 0 (1 < n < N), iΔ_{in}A_N + γ_N A_N + iκ_{N,N−1}A_{N−1} = 0 (n = N). (3)

It is apparent that A_N can be completely determined by solving Eqs.(3). In the semiclassical approximation, the coupling constant ϵ can be expressed via the amplitude A_{in} of the input driving field as ϵ ≡ √ γ_cA_{in}. [39] Then the transmission spectrum can be calculated by

T (Δ_{in}) = | | | A^{out} A_{in} | | |^2 , (4)

where A_{out} = √ γ_cA_N and A_{in} = ϵ/ √ γ_c. It is easy to check that when the parameter setting of γ_i and κ_{i,j} changes, the distribution of resonant peaks of the graph of T (Δ_{in}) will become different. To study how non-reciprocity happens on these peaks, one can rewrite Eqs.(2) and (3) in matrix form. As a subsequence, the question of finding resonant peaks is converted into an eigenvalue problem about the coefficient matrix.

FIG. 2. A four-mode resonator array with balanced gain and loss. The resonators are coupled adjacent to each other with coupling strength κ. The coupling loss between waveguide WG1(WG2) and resonator R_1(R_N ) is γ_c.

By defining a vector α = (A_1, A_2, ..., A_N )^T with elements being the field amplitudes, and by introducing β = (ϵ, 0, ..., 0)^T describing the input condition, we can rewrite Eq.(2) in the form i∂A_n/∂t = Ĥα − β, where the coefficient matrix Ĥ reads

Ĥ =

Δ_{in} + iγ_1 κ_{1,2} · · · 0

κ_{2,1} Δ_{in} + iγ_2 . . . . . . . 0 · · · Δ_{in} + iγ_N

, (5)

which is known as the Hamiltonian or evolution matrix [39, 40, 46]. With α, β and Ĥ, Eq.(3) can be simplified as Ĥα = β, and then the steady-state solution of α can be given by α = Ĥ^{−1}β. It is worthwhile to notice that the solution of α is protected by the nonsingularity of Ĥ, |Ĥ| ≠ 0. If Ĥ is singular, the vector α and the transmission coefficient T (Δ_{in}) could not be determined. Furthermore, the amplitude A_N can not be determined. This divergence in T (Δ_{in}) indicates that the system cannot achieve a steady state, which leads to an infinite amplification of the light field during its transmission between resonators, akin to a lasing process. This phenomenon is referred to as a resonance state in the continuum (RIC) [47], and is also known as a spectral singularity [48, 49]. For a particular set of γ_i and κ_{i,j} , the frequencies are indicative of the divergent peaks in the transmission spectrum, which is termed supermodes. For the supermodes of the photon frequencies might be complex due to solutions involving imaginary parts. In what follows, for the sake of reality the series of nondivergent peaks will correspond to the real parts of these supermodes. Thus, the issue of resonant peaks is reduced to an eigenvalue problem. This methodology is analogous to the Siegert boundary condition approach, which is commonly used to identify resonant states in open quantum systems [48, 50–52], where resonant states align with the eigenstates of the Schrödinger equation under certain boundary conditions [50]. This correspondence is not unexpected given the formal equivalence between the Schrödinger equation and the classical wave equation.

Practically, the light intensity cannot be infinitely amplified. Actually, the divergent peaks should be replaced by a series of sharp but finite peaks. Intriguingly, non-reciprocal transmission phenomena emerge at nondivergent peaks [40]. The discovery inspires physicists to investigate the underlying mechanisms. As a considered plausible theory, the gain saturation theory was given by Ievgen I. Arkhipov’s group [39]. In the theory, the nonlinear equations is derived from the Scully-Lamb laser model. It is worth noticing that the nonlinear equations combine the linear model’s simplicity and the nonlinear model’s accuracy.

III. GAIN SATURATE EFFECT AND MULTI-MODE NON-RECIPROCAL TRANSMISSION

According to Ref.[39], the Scully-Lamb model’s modification to linear equations can be accomplished by adding a nonlinear term into each gain term. Upon examining the numerical outcomes of the dual-mode PT system (see

Appendix), two key insights emerge: one is the nonlinear equations predicting non-reciprocal peaks, the other is the non-reciprocal peaks manifesting within the nondivergent peaks region of PT symmetry breaking. As the conclusion obtained in Ref.[41], the location of nondivergent peaks aligns with the projection of supermodes onto the real axis in the complex plane. The model is constructed as in Fig.2.

The model consists of four ring resonators in a onedimensional configuration, with equal coupling coefficients and symmetric gain-loss coefficients. The particular constructions preserve the PT symmetry. As a special case of the model depicted in Fig.1, from Eq.(2) the specific linear rate equations can be given by d dt A_1 = iΔA_1 + 1.5γA_1 − iκA_2 − ε; d dt A_2 = iΔA_2 + 0.5γA_2 − iκA_1 − iκA_3; d dt A_3 = iΔA_3 − 0.5γA_3 − iκA_2 − iκA_4; d dt A_4 = iΔA_4 − 1.5γA_4 − iκA_3,

(6)

and the corresponding coefficient matrix is in the following form

H_4 =

Δ_{in} + i1.5γ κ 0 0 κ Δ_{in} + i0.5γ κ 0 0 κ Δ_{in} − i0.5γ κ 0 0 κ Δ_{in} − i1.5γ. . (7)

By numerically solving the secular equation, the supermodes Δ_r of H_4 are obtained, whose real parts (blue) and imaginary parts (red) of Δ_r are described in Fig.3(a). γ is small, the supermodes Δ_r are purely real which corresponds to the blue points in Fig.3(b). In region III, γ is large, Δ_r are purely imaginary, which corresponds to the red ones. While in region II, the real parts and imaginary parts of Δ_r are all non-zero, they are denoted by the green points in Fig.3(b). In other words, the parameter space is divided into three regions: in I, PT unbroken Δ_r as real; II being transition region Δ_r as complex; and in III, PT broken Δ_r as imaginary.

In different regions the transmission spectrum has different behaviors as shown in Figs.3(c)-(f). In region I, the number of divergent peaks equals to that of the supermodes as in Fig.3(d), and in region III, there is a single non-divergent peak on Δ_{in} = 0 as in Fig.3(f). However, in region II, there are more than one non-divergent peaks in the spectrum as in Fig.3(e). Comparing with the green points in Fig.3(b), we find that the locations of non-divergent peaks coincide with the projections of supermodes on to the real-axis. In terms of previous speculations, the multiple non-divergent peaks may appear in the region II successfully.

When the gain saturation effect is taken into account, the linear equation will be reformulated into the following nonlinear form, d dt A_1 = iΔA_1 + 1.5γA_1 − iκA_2 − ε − B |A_1|^2 A_1; d dt A_2 = iΔA_2 + 0.5γA_2 − iκA_1 − iκA_3 − B |A_2|^2 A_2; d dt A_3 = iΔA_3 − 0.5γA_3 − iκA_2 − iκA_4; d dt A_4 = iΔA_4 − 1.5γA_4 − iκA_3; (8) According to Eq.(7), the transmission spectrum can be easily solved with ε = 2GH, γ = 1MH and B = 0.01Hz at κ = 20MH, 1.1MH, 0.1MH, the results are depicted in Fig.4. The results confirm two predictions: One is that the divergent peak from the linear equation becomes a sharp but finite non-divergent peak without nonreciprocal phenomenon, as shown in Figs.4(a)(d), which corresponds to the region I in Fig.3(a). The other is that the divergent peak becomes a non-divergent one but

FIG. 3. (a) The real (blue) and imaginary (red) parts of supermodes of Ĥ_4 as functions of γ/κ. (b)The distribution of supermode Δr on the complex plane with κ = 1MH at γ = 0.5MHz (blue), γ = 0.8MHz (green), γ = 1.8MHz (red). (c)The variation of transmission spectrum as a function of γ/κ and Δ_{in}, where the logarithm of T (ω_l) is shown as the brightness. (d)(e)(f) Transmission spectrum against Δ_{in} in the region I ((d),γ = 0.5MHz), region II ((e),γ = 0.8MHz) and region III ((f),γ = 1.8MHz). Wherein κ = γ_c = 1MHz,ϵ = 0.1MHz.

with non-reciprocal transmission phenomenon, as shown in Figs.4(b)(e), which corresponds to the region II in Fig.3(a).

The emergence of multi-frequency non-reciprocal phenomena as in Figs.4(b) and (e)that is the most important result in the present paper. In the next section, we will further discuss a Dual-Frequency Circulator by using the nonlinearized model.

IV. CONSTRUCTION OF A DUAL-FREQUENCY CIRCULATOR

In this section, we will introduce a nonlinear term into the original linear equation, and will extend a twomode cavity system to a four-mode cavity system, in which a two-frequency non-reciprocity phenomenon can be achieved. Interestingly, the non-reciprocity of the nonlinear model can be employed to construct an optical directional amplifier providing simultaneously multimode optical channels with different magnifications. In other words, the non-reciprocity can provide an access to manipulate simultaneously multi-mode optical channels, which could be applied in optical chip integration.

As an example, a double-mode non-reciprocal optical directional amplifier can be constructed by using four basic units as described in Fig.5. Each unit consists of four ring echo wall resonators as in Fig.2. The non-reciprocal amplifier has four ports, and any two of them can be used as signal input and output respectively. When the signal enters the optical fiber from one of the ports, it will be propagated in two routes (clockwise and counterclockwise) at the same time as sketched in Fig.6. Specifically, in the amplifier any port can be taken as an output to detect signal, and can be taken as an input to continue the signal execution into the next unit. The particular construction can simultaneously provide many channels for signal transmission.

In the example, it is obvious non-reciprocal that the transmission spectrum of the signal propagates in clockwise and in anticlockwise. For the sake of simplicity, we assume that the optical signal propagates a single cycle, and we introduce a metric M to describe the transmission between the ports for the double-mode non-reciprocal amplifier. The element of metric M_{ij} (i, j = 1, 2, 3, 4) describes the transmission between the ith port and the jth port, where the ith port is input and the jth port is output. Specifically, we can describe the transmission for the port 1 to the port 2 as M_{12} = T^3_{41} + T_{14}, that for the port 1 to the port 3 as M_{13} = T^2_{41} + T^2_{14}, for that of the port 1 to the port 4 as M_{14} = T_{41} + T^3_{14}, where T_{41}

FIG. 4. Transmission spectrum T14 and T14 against Δin with ϵ = 2GH, γ = 1MH, B = 0.01Hz, (a) (d) at κ = 20MH,(b) (e) at κ = 1.1MH,(c) (f)at κ = 0.1MH.

FIG. 5. Schematic diagram of multi-mode optical directional amplifier (the blue cavity is a loss cavity and the red cavity is a gain cavity). The device has four ports, of which any two ports can be used as signal input and output.

and T_{14} are the transmission of the basic unit as shown in Figs.4(b)and(e). By numerical calculation, we can obtain that M_{12} is much larger than M_{14}, that is the output of port 2 being much larger than that of port 4. This result directly demonstrates the existence of non-reciprocity in the example. More significant, the numerical results demonstrate that the optical signal is amplified 300 times through a single cycle as described in Fig.7. The results may provide a way that the non-reciprocal amplifier may be collaborated in complex opto-mechanical structures and implemented in integrated photonic circuits.

FIG. 6. Schematic diagram of optical nonreciprocal directional amplifier. When the signal light is routed in a clockwise direction, as shown by the blue arrow, there is a large amplification factor between ports. When the signal light is routed in a counterclockwise direction, as shown by the red arrow, there is a small amplification factor between ports. The green arrow represents our ideal signal routing direction.

V. CONCLUSION

In summary, based on the Scully-Lamb model and the photomechanical interaction, we have constructed a non-reciprocal unit that is a system coupled by four resonators and two optical fibers. Particularly, it is nonreciprocal that in the constructed system the transmission rate has different values in a particular direction and its opposite. For the presence of many ports and simultaneously distinguishable transmission rates in the

FIG. 7. Amplification coefficient matrix of multi-mode optical directional amplifier for single cycle. (a) The ideal magnification matrix. M_{12} = M_{23} = M_{34} = M_{41} = 300 (b) The actual resulting magnification matrix. When the signal light is incident from any port, it is transmitted in a clockwise direction, and the light intensity is continuously amplified. M_{11} = M_{22} = M_{33} = M_{44} = 1

non-reciprocal unit, the dual-frequency non-reciprocity phenomenon can realize parallel transmission and processing of information, and can be applied to photonic integrated circuits or optical devices[18, 22, 34, 35]. As communication applications, one can construct optical isolator, circulators and directional amplifier[22, 38, 42– 44], which can be used to control optical signals in a particular direction at specific frequencies. As magnetooptical storage, one can design magneto-optical materials and devices[53] with the non-reciprocal units.

For an example, the multi-mode optical directional amplifier with four ports was built by using the basic units. For a particular input port, the rest three output ports can have distinguishable amplified times of optical signals, which results from the non-reciprocal. These results may provide an approach for the more and more complex requirements of signal in communication and optical integrated circuits. Moreover, the example can be arbitrarily extended to more ports that can be integrated on chip with other circuit components in barrier-free combination.

ACKNOWLEDGMENTS

This work is jointly supported by the National Nature Science Foundation of China (Grants, No. 12475019,

No.1247030364), and National Lab of Solid State Microstructure of Nanjing University (Grants No.M35040, No.M35053 and No.M37014).

APPENDIX

Gain saturate effect is a pivotal phenomenon in laser physics where the intensity of the intracavity field becomes significant enough to reduce the net gain of the active medium. As the Scully-Lamb quantum laser model is applied to parity-time symmetric whispering-gallery microcavities, the gain saturation effect plays an important role in explaining the non-reciprocity in light propagation. When the input driving field intensity increases, the gain ability of medium will diminish due to saturation, which equivalently decrease the amplification of the signal field. This nonlinear mechanism results in a direction-dependent transmission behavior, which is essential for the non-reciprocal light transmission in the broken PT-symmetric phase. The model demonstrates that gain saturation modifies the eigenmodes and exceptional points of the system, by introducing an additional loss mechanism that depends on the field intensity and propagation direction. In Ref.[39], the authors employ the Scully-Lamb quantum laser model to derive a set of rate equations that describe the dynamics of light propagation in parity-time symmetric whispering-gallery microcavities. Starting from a non-Lindbladian master equation that accounts for gain, loss, and gain saturation, they apply the semiclassical approximation to transform quantum operators into classical amplitudes. By calculating the time derivatives of these amplitudes and incorporating the effects of gain saturation, at a set of nonlinear coupled differential equations are obtained, which can elucidate the interplay between the intracavity fields and the response of photonic system, and reveal the nonreciprocal transmission of light. This theoretical framework bridges the quantum and classical descriptions, and provides a way to learn the action of gain saturation on the non-reciprocal behavior.

One of the simplest examples is a two-mode array with balanced gain and loss, as shown in Fig.8(a). This system can be easily built from the general structure as shown in Fig.1 and Eq.(1) by setting N = 2, γ_1 = γ, γ_2 = −γ and κ_{1,2} = κ_{2,1} = κ, where we have assumed γ, κ > 0. Repeating the progress of Eqs.(1)-(5), we can get the evolution matrix of the two-mode array:

Ĥ_2 = ( Δ_{in} + iγ κ κ Δ_{in} − iγ ) . (S1)

According to Eq.(4), the transmission spectrum can be given by

T (Δ_{in}) = | | | A_{out} A_{in} | | | 2 = | | | A_2 ϵ | | | 2 γ^2_c , (S2)

where A_2 can be solved by α = βĤ^{−1}_2 , wherein α = (A_1, A_2)^T , β = (ϵ, 0)^T . In the complex plane, the distribution of supermodes as γ/κ vary across the EP as shown in Fig.8(d). When γ/κ < 1 , the supermodes Δ_± lie on the real axis denoted by blue points. In

FIG. 8. (a)The sketch of the two-mode PT symmetric system, wherein balanced gain(loss) is labeled by γ(−γ), coupling between the two resonators is κ, and γ_c denotes the couplings between the resonator (R_1 and R_2) and the waveguide (WG1 and WG2). (b) The real part of supermodes Δ_± of Ĥ_2 as a function of γ/κ with κ > 0. (c) The imaginary part of Δ_± of Ĥ_2 as a function of γ/κ with κ > 0. (d)The distribution of supermodes Δ_± on the complex plane where κ = 1MHz. Blue points correspond to PT unbroken region (γ = √ 3/2MHz).

Red points correspond to PT broken region (γ = √ 5/2MHz). (e)(f) Transmission spectrum against input frequency Δ_{in} in the PT unbroken ((e), γ = √ 3/2MHz) and broken ((f), γ = √ 5/2MHz) regions, wherein κ = γ_c = 1MHz, ϵ = 0.1MHz.

FIG. 9. Transmission spectrum T_{14} and T_{14} against Δ_{in} wherein ϵ = 176.05GH, B = 0.01Hz, (a)(c)γ = 3.766MH, κ = 20MH, (b)(e)γ = 3.766MH, κ = 0.2MH.

this region, the transmission spectrum diverges at these points described in Fig.8(e). When γ/κ > 1, the values of Δ_± become purely imaginary as the red points in Fig.8(d). Since the input detuning Δ_{in} is always a real number, the divergent peaks vanish in the transmission spectrum, and are replaced by a broad finite peak at Δ_{in} = 0 which is the projection of Δ_± on the real axis, as shown in Fig.8(f). In fact, according to T (Δ_{in}) = |κγ_c/(Δ^2_{in} + γ^2 − κ^2)|^2, it is easy to check that the spectrum can fits the square of a Breit-Wigner distribution around Δ_{in} = 0 when γ^2 − κ^2 > 0. The peaks are called Breit-Wigner peaks [49].

By considering the gain saturation effect, the linear equation can be reformulated into the following nonlinear form: d dt A_1 = iΔA_1 + γA_1 − κA_2 − B 2 |A_1|^2 A_1 − ϵ, d dt A_2 = iΔA_2 − γA_2 + κA_1.

(S3)

Comparing Eq.(8) and Eq.(S3), it can be seen that the nonlinear equation includes an additional cubic term. When the optical field inside the resonator is weak, that is A_1 being small, this term can be negligible due to the coefficient B being very small. However, when the optical field increases, that is A_1 becoming larger, the cubic term increases dramatically, causing a substantial suppression of the field intensity, thus the field intensity cannot be linearly enhanced without limit.

Then we can calculate the transparency spectrum using this model, as shown in Fig.9. When γ is small, which corresponds to the PT-symmetric unbroken phase depicted in Fig.8(e), the original divergent peaks are constrained and transforms into non-divergent peaks, and exhibit reciprocity as shown in Fig.9(a)(c). Conversely, when γ is large, corresponding to the PT-symmetric broken phase shown in Fig.8(f), the position of the original divergent peak remains unchanged, but the peak value of T_{41} is significantly larger than that of T_{14}, demonstrating non-reciprocity, as shown in Fig.9(b)(d). This agrees with the experimental results reported in ref.[46].

[1] H. Meng, Y. S. Ang, and C. H. Lee, Exceptional points in non-Hermitian Photonics: Applications and Recent Developments, arXiv preprint arXiv:2310.16699 (2023).

[2] Q. Yan, B. Zhao, R. Zhou, R. Ma, Q. Lyu, S. Chu, X.

Hu, and Q. Gong, Advances and applications on non- Hermitian topological photonics, Nanophotonics 12, 2247 (2023).

[3] C. Wang, Z. Fu, W. Mao, J. Qie, A. D. Stone, and L.

Yang, Non-Hermitian optics and photonics: from classical to quantum, Adv. Opt. Photonics 15, 442 (2023).

[4] M.-A. Miri and A. Alù, Exceptional points in optics and photonics, Science 363, eaar7709 (2019).

[5] M. De Carlo, F. De Leonardis, R. A. Soref, L. Colatorti, and V. M. N. Passaro, Non-Hermitian Sensing in Photonics and Electronics: A Review, Sensors 22, 3977 (2022).

[6] Z. Shen, Y.-L. Zhang, Y. Chen, F.-W. Sun, X.-B. Zou, G.-C. Guo, C.-L. Zou, and C.-H. Dong, Reconfigurable optomechanical circulator and directional amplifier, Nat. Commun. 9, 1 (2018).

[7] R. J. Potton, Reciprocity in optics, Rep. Prog. Phys. 67, 717 (2004).

[8] Z. Shen, Y.-L. Zhang, Y. Chen, Y.-F. Xiao, C.-L. Zou, G.-C. Guo, and C.-H. Dong, Nonreciprocal frequency conversion and mode routing in a microresonator, Phys. Rev. Lett. 130, 013601 (2023).

[9] S. V. Kutsaev, A. Krasnok, S. N. Romanenko, A. Y.

Smirnov, K. Taletski, and V. P. Yakovlev, Up-And- Coming Advances in Optical and Microwave Nonreciprocity: From Classical to Quantum Realm, Adv. Photonics Res. 2, 2000104 (2021).

[10] Y. Bromberg, B. Redding, S. M. Popoff, and H. Cao, Control of coherent backscattering by breaking optical reciprocity, Phys. Rev. A 93, 023826 (2016).

[11] J.-C. Zheng, and P.-B. Li, Few-photon isolation in a onedimensional waveguide using chiral quantum coupling, Opt. Express 31, 21881 (2023).

[12] A. Mock, CMOS-compatible compact optical isolator based on space-time modulated coupled resonators, Opt. Express 30, 39207 (2022).

[13] Z. Fan, W. Zhang, Q. Qiu, and J. Yao, Hybrid Frequency- Tunable Parity-Time Symmetric Optoelectronic Oscillator, J. Lightw. Technol. 38, 2127 (2020).

[14] L. Tang, J. Tang, M. Chen, F. Nori, M. Xiao, and K.

Xia, Quantum Squeezing Induced Optical Nonreciprocity, Phys. Rev. Lett. 128, 083604 (2022).

[15] Y. X. Yao, and Q. Ai, Optical Non-Reciprocity in Coupled Resonators by Detailed Balance, Ann. Phys. (Berlin) 535, 2300135 (2023).

[16] W. Cao, C. Wang, W. Chen, S. Hu, H. Wang, L. Yang, and X. Zhang, Fully integrated parity–time-symmetric electronics, Nat. Nanotechnol. 17, 262 (2022).

[17] R. Burgwal, and E. Verhagen, Enhanced nonlinear optomechanics in a coupled-mode photonic crystal device, Nat. Commun. 14, 1526 (2023).

[18] A. Metelmann, and A. A. Clerk, Nonreciprocal quantum interactions and devices via autonomous feedforward, Phys. Rev. A 95, 013837 (2017).

[19] Y. Shoji, and T. Mizumoto, Magneto-optical nonreciprocal devices in silicon photonics, Sci. Technol. Adv. Mater. 15, 014602 (2016).

[20] W. Yan, Z. Wei, Y. Yang, D. Wu, Z. Zhang, X. Song, J.

Qin, and L. Bi, Ultra-broadband magneto-optical isolators and circulators on a silicon nitride photonics platform, Opt. 11, 376 (2024).

[21] X.-X. Hu, Z.-B. Wang, P. Zhang, G.-J. Chen, Y.-L.

Zhang, G. Li, X.-B. Zou, T. Zhang, H. X. Tang, C.- H. Dong, G.-C. Guo, and C.-L. Zou, Noiseless photonic non-reciprocity via optically-induced magnetization, Nat. Commun. 12, 2389 (2021).

[22] C. Caloz, A. Alù, S. Tretyakov, D. Sounas, K. Achouri, and Z.-L. Deck-Léger, Electromagnetic Nonreciprocity, Phys. Rev. A 10, 047001 (2018).

[23] C. Caloz, and Z.-L. Deck-Leger, Spacetime Metamaterials—Part I: General Concepts, IEEE Trans. Antennas Propag. 68, 1569 (2020).

[24] D. L. Sounas, and A. Alù, Non-reciprocal photonics based on time modulation, Nat. Photonics 11, 774 (2017).

[25] S. Fan, Y. Shi, and Q. Lin, Nonreciprocal Photonics Without Magneto-Optics, IEEE Antennas Wireless Propag. Lett. 17, 1948 (2018).

[26] N. A. Estep, D. L. Sounas, J. Soric, and A. Alù, Magnetic-free non-reciprocity and isolation based on parametrically modulated coupled-resonator loops, Nat. Phys. 10, 923 (2014).

[27] K. Fang, Z. Yu, and S. Fan, Realizing effective magnetic field for photons by controlling the phase of dynamic modulation, Nat. Photonics 6, 782 (2012).

[28] L. D. Tzuang, K. Fang, P. Nussenzveig, S. Fan, and M.

Lipson, Non-reciprocal phase shift induced by an effective magnetic flux for light, Nat. Photonics 8, 701 (2014).

[29] H. Lira, Z. Yu, S. Fan, and M. Lipson, Electrically Driven Nonreciprocity Induced by Interband Photonic Transition on a Silicon Chip, Phys. Rev. Lett. 109, 033901 (2012).

[30] K. Fang, Z. Yu, and S. Fan, Photonic Aharonov-Bohm Effect Based on Dynamic Modulation, Phys. Rev. Lett. 108, 153901 (2012).

[31] L. Fan, L. T. Varghese, Y. Xuan, J. Wang, B. Niu, and M. Qi, Direct fabrication of silicon photonic devices on a flexible platform and its application for strain sensing, Opt. Express 20, 20564 (2012).

[32] X. Guo, C.-L. Zou, H. Jung, and H. X. Tang, On-Chip Strong Coupling and Efficient Frequency Conversion between Telecom and Visible Optical Modes, Phys. Rev. Lett. 117, 123902 (2016).

[33] M. Lawrence, D. R. Barton, and J. A. Dionne, Nonreciprocal Flat Optics with Silicon Metasurfaces, Nano Lett. 18, 1104 (2018).

[34] G. A. Peterson, F. Lecocq, K. Cicak, R. W. Simmonds, J.

Aumentado, and J. D. Teufel, Demonstration of Efficient Nonreciprocity in a Microwave Optomechanical Circuit, PRX 7, 031001 (2017).

[35] S. Barzanjeh, M. Wulf, M. Peruzzo, M. Kalaee, P. B.

Dieterle, O. Painter, and J. M. Fink, Mechanical on-chip microwave circulator, Nat. Commun. 8, 953 (2017).

[36] N. R. Bernier, L. D. Tóth, A. Koottandavida, M. A. Ioannou, D. Malz, A. Nunnenkamp, A. K. Feofanov, and T. J. Kippenberg, Nonreciprocal reconfigurable microwave optomechanical circuit, Nat. Commun. 8, 604 (2017).

[37] L. Mercier de Lépinay, C. F. Ockeloen-Korppi, D. Malz, and M. A. Sillanpää, Nonreciprocal Transport Based on Cavity Floquet Modes in Optomechanics, Phys. Rev. Lett. 125, 023603 (2020).

[38] D. Malz, L. D. Tóth, N. R. Bernier, A. K. Feofanov, T.

J. Kippenberg, and A. Nunnenkamp, Quantum-Limited Directional Amplifiers with Optomechanics, Phys. Rev. Lett. 120, 023601 (2018).

[39] I. I. Arkhipov, A. Miranowicz, O. Di Stefano, R. Stassi, S.

Savasta, F. Nori, and Ş. K. Özdemir, Scully-Lamb quantum laser model for parity-time-symmetric whisperinggallery microcavities: Gain saturation effects and nonreciprocity, Phys. Rev. A 99, 053806 (2019).

[40] B. Peng, Ş. K. Özdemir, F. Lei, F. Monifi, M. Gianfreda, G. L. Long, S. Fan, F. Nori, C. M. Bender, and L. Yang, Parity–time-symmetric whispering-gallery microcavities, Nat. Phys. 10, 394 (2014).

[41] C. Du, Y.-T. Chen, L. Du, and J.-H. Wu, High-order exceptional points and novel light transmission spectra in PT symmetric ring resonator array, Phys. Lett. A 503, 129413 (2024).

[42] L. Bi, J. Hu, P. Jiang, D. H. Kim, G. F. Dionne, L.

C. Kimerling, and C. A. Ross, On-chip optical isolation in monolithically integrated non-reciprocal optical resonators, Nat. Photonics 5, 758 (2011).

[43] H. Wu, J. Tang, M. Chen, M. Xiao, Y. Lu, K. Xia, and F. Nori, Passive magnetic-free broadband optical isolator based on unidirectional self-induced transparency, Opt. Express 32, 11010 (2024).

[44] J. Shen, J. Liu, M. Lin, Z. Wu, and S. Deng, A microwave limiter with non-reciprocal limiting threshold, Electron. Lett. 59, e212730 (2023).

[45] Y. Yamamoto, and A. Imamoglu, Mesoscopic quantum optics, Mesoscopic Quantum Optics (1999).

[46] L. Chang, X. Jiang, S. Hua, C. Yang, J. Wen, L. Jiang, G. Li, G. Wang, and M. Xiao, Parity–time symmetry and variable optical isolation in active–passive-coupled microresonators, Nat. Photonics 8, 524 (2014).

[47] S. Garmon, M. Gianfreda, and N. Hatano, Bound states, scattering states, and resonant states in PT-symmetric open quantum systems, Phys. Rev. A 92, 022125 (2015).

[48] W.-R. Cao, Y.-L. Wang, X.-L. Chen, H. Jiang, C.-T. Xu, and H.-S. Zong, The geometric potential of a doublefrequency corrugated surface, Phys. Lett. A 383, 2124 (2019).

[49] G. Breit, and E. Wigner, Capture of slow neutrons, Phys.

Rev. 49, 519 (1936).

[50] K. Shobe, K. Kuramoto, K.-I. Imura, and N.

Hatano, Non-Hermitian Fabry-Pérot resonances in a PTsymmetric system, PRR 3, 013223 (2021).

[51] A. J. Siegert, On the derivation of the dispersion formula for nuclear reactions, Phys. Rev. 56, 750 (1939).

[52] N. Hatano, T. Kawamoto, and J. Feinberg, Probabilistic interpretation of resonant states, Pramana 73, 553 (2009).

[53] M. Cotrufo, A. Cordaro, D. L. Sounas, A. Polman, and A.

Alù, Passive bias-free non-reciprocal metasurfaces based on thermally nonlinear quasi-bound states in the continuum, Nat. Photonics 18, 81 (2023).