arXiv:astro-ph/0308346v1 20 Aug 2003

Astronomy & Astrophysics manuscript no. INTEGRAL51 May 5, 2019 (DOI: will be inserted by hand later)

INTEGRAL Spectrometer SPI’s GRB detection capabilities^⋆

GRBs detected inside SPI’s FoV and with the anticoincidence system ACS

A. von Kienlin^1, V. Beckmann^{3,4}, A. Rau^1, N. Arend^{1,⋆⋆}, K. Bennett^9, B. McBreen^5, P. Connell^6, S. Deluit^4, L. Hanlon^5, M. Kippen^8, G. G. Lichti^1, L. Moran^5, R. Preece^7, J.-P. Roques^2, V. Schönfelder^1, G. Skinner^2, A. Strong^1, and R. Williams^9

1 Max-Planck-Institut für extraterrestrische Physik, Giessenbachstrasse, 85748 Garching, Germany, 2 Centre d’Etudes Spatiales des Rayonnements, 9, avenue du Colonel Roche, 31028 Toulouse, France, 3 Institut für Astronomie und Astrophysik, Universität Tübingen, Sand 1, D-72076 Tübingen, Germany 4 INTEGRAL Science Data Centre, Chemin d’ Écogia 16, CH-1290 Versoix, Switzerland 5 Department of Experimental Physics, University College Dublin, Stillorgan Road, Dublin 4, Ireland 6 Space Research Group, Univ. of Birmingham B15 2TT, Birmingham, United Kingdom 7 Dept. of Physics, UAH, National Space Science & Technology Center, Huntsville, AL 35805, USA 8 Space and Remote Sensing Sciences, NIS-2 Mail Stop D436, Los Alamos National Laboratory, Los Alamos, NM 87545, USA 9 Science Operations and Data Systems Division of ESA/ESTEC, SCI-SDG, Keplerlaan 1, Postbox 299, NL-2200 AG Noordwijk, The Netherlands

Received xxx 00, 2003; accepted xxx 00, 2003

Abstract. The spectrometer SPI, one of the two main instruments of the INTEGRAL spacecraft, offers significant gamma-ray burst detection capabilities. In its 35^o (full width) field of view SPI is able to localise gamma-ray bursts at a mean rate of ∼ 0.8/month. With its large anticoincidence shield of 512 kg of BGO crystals SPI is able to detect gamma-ray bursts quasi omni-directionally with a very high sensitivity. Burst alerts of the anticoincidence shield are distributed by the INTEGRAL Burst Alert System. In the first 8 months of the mission about 0.8/day gamma-ray burst candidates and 0.3/day gamma-ray burst positions were obtained with the anticoincidence shield by interplanetary network triangulations with other spacecrafts.

Key words. Gamma-ray bursts – GRB – Gamma-ray Astronomy – INTEGRAL – SPI

1. Introduction

The detection and investigation of cosmic gamma-ray bursts (GRBs) is an important scientific topic of the INTEGRAL mission. Even now, 35 years after their discovery by the Vela satellites (Klebesadel et al. 1973), this phenomenon is far from being well-understood. A major breakthrough in this field was obtained in the 1990’s with the BATSE detectors (Fishman et al. 1989) on NASA’s Compton Gamma-Ray Observatory (CGRO). In the ten years of the CGRO mission 2704 bursts were

Send offprint requests to: A. von Kienlin (e-mail: azk@mpe.mpg.de) ⋆ Based on observations with INTEGRAL, an ESA project with instruments and science data centre funded by ESA member states (especially the PI countries: Denmark, France, Germany, Italy, Switzerland, Spain), Czech Republic and Poland, and with the participation of Russia and the USA. ⋆⋆ Present address: TU München, Department of Physics, Institute E21, James-Franck-Str., 85748 Garching, Germany registered, which showed an isotropic distribution over the entire sky, but with a deficiency for weak burst compared to a homogeneously distribution (logN-logS distribution with −3/2 power law). It was the Italian/Dutch satellite BeppoSAX (Boella et al.1997) which helped to reveal the cosmological nature of GRBs with the identification of the first X-ray afterglow (Costa et al. 1997), which triggered the first successful follow-up observation at optical wavelengths (van Paradijs et al. 1997) and subsequent direct redshift measurements (Metzger et al. 1997). The redshifts obtained to date for about 30 GRBs range from 0.0085 to 4.5. Observational evidence now strongly suggests that GRBs longer than 2 seconds are associated with hypernovae (Galama et al. 1998, Kawabata et al. 2003, Hjorth et al. 2003). Gamma-ray polarimetry of the intense event GRB021206 using the RHESSI satellite (Coburn & Boggs 2003) indicates that the GRB emission is highly polarised (80%), suggestive of synchrotron ra-

2 A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities

diation from particles in a highly-ordered magnetic field (Granot 2003).

2. GRB detection with the camera of SPI

The aim of the spectrometer SPI is to perform high-resolution spectroscopy of astrophysical sources in the energy range between 20 keV and 8 MeV (Vedrenne et al. 2003). The imaging capability is good, but is exceeded by that of the imager IBIS which complements SPI by having higher imaging resolution, but lower spectroscopic resolving power (Ubertini et al. 2003). Hence we expect the two main INTEGRAL instruments to make contributions to GRB research in different areas. The connection between GRBs and Type Ib/c ‘hypernovae’ (Hjorth et al. 2003) heralds a potentially exciting era for high-resolution γ-ray spectroscopy of the closest of these sources. In addition, the broad energy coverage of SPI is well suited to constrain the spectral shape, both below and above the energy at which the GRB power output is typically peaked (∼ 250 keV). The long-standing controversy over the existence of short-lived spectral features in GRB spectra can also be addressed by SPI’s superb spectroscopic capabilities. On the other hand, IBIS will provide precise GRB locations to the community, which is important for the observation of GRB afterglows. In addition, the capability to cross-calibrate both spectra and images between the two experiments is extremely important, particularly in the case of such short-lived events as GRBs, which cannot be re-observed. Currently GRBs which occur inside SPI’s field of view (FoV) are detected and analysed offline. The implementation of an automatic GRB detection algorithm for SPI (von Kienlin et al. 2003a) into the INTEGRAL burstalert system (IBAS, Mereghetti et al. 2003a) is planned.

2.1. Imaging with the spectrometer SPI

The camera of SPI, which consists of 19 cooled high-purity germanium detectors, residing in a cryostat, is shielded on the side walls and rear side by a large anticoincidence shield (ACS). The FoV of the camera is defined by the upper opening of the ACS. The imaging capability of the instrument is attained by a passive-coded mask mounted 1.7 m above the camera. By observing a series of nearby pointing directions around the source (“dithering”) the imaging capability of SPI is improved by reducing ambiguity effects. For the normal mode of operation two dithering patterns are applied, a square one with 5 × 5 pointings and a hexagonal one with 7 pointings. Each pointing lasts about 30 min. The slew between pointings on a dither pattern lasts as 5-10 minutes. Due to their short duration, dithering will not improve the imaging of SPI for bursts. But during its short duration a burst will be in most cases the brightest γ-ray source for SPI in the whole FoV, so imaging with SPI is still possible. The case when a burst occurred during a slew can be investigated for GRB030131. Despite the modest angular resolution of

SPI, which is of the order of 2.5^∘, it is possible to locate the direction of bursts down to a few arcminutes.

2.2. Analysis methods for GRBs

The analysis of GRBs in the SPI FoV has been performed by using the instrument-specific software, which has been developed by the SPI instrument team in collaboration with the ISDC (Beckmann 2002). In both, image and spectral extraction, the analysis methods are similar and are therefore described here together. SPI is a background-dominated instrument. The overall count rate of the detector plane when observing an empty field is about 880 counts/s, while e.g. the Crab shows a SPI count rate of 33 counts/s. Therefore a careful background handling is essential. In the case of short events as GRBs, the best way to remove the background is to take the observation which encloses the GRB (excluding the time when the GRB was detectable in SPI) as a background. By applying the same parameters as for the GRB analysis a detector spectrum should be extracted. This detector spectrum does not only contain the background, but will also include sources in the FoV and therefore allows an optimised data reduction. The data for the GRB should be extracted from a short time range around the peak, in order to achieve a good signal-to-noise ratio for the result. Source location and spectral extraction are performed applying the iterative-removal-of-sources method, which is implemented in the SPIROS analysis software (Skinner & Connell 2003). For source location no a-priori knowledge of the GRB position is necessary, while in order to extract a spectrum, the best known (e.g. ISGRI derived) source position should be applied.

2.3. Results obtained for the first bursts observed inside SPI’s FoV

Since the start of the mission, six GRBs have been observed within SPI’s FoV. Tab. 1 summarises the important quantities derived with SPI. In all cases the GRB was detected by IBIS and for comparison the important parameters found from the IBIS data are also shown. Below for each of the GRBs a short summary is given, especially with the emphasis on the SPI performance:

GRB021125: The first GRB observed within the FoV of INTEGRAL (in this case the partially-coded FoV) was the one with the brightest fluence of the six GRBs in Tab. 1 (Malaguti et al. 2003). The GRB occurred during a period of the Cyg X-1 in-orbit calibration where SPI was set into a restricted telemetry mode. This was the time period allocated for the IBIS-PICsIT photonby-photon mode calibration, which caused high telemetry loads. Only the telemetry, containing the technicaland science-housekeeping data and the onboard spectra, with an aquisition time of ∼ 30 min, were downlinked. Nevertheless it was possible to determin a GRB–lightcurve and –location by using the counter data of the 19 Ge-

A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities 3

Table 1. Table of GBRs detected inside the FoV of SPI. For comparison the results of IBIS are listed too. The data sets are taken from Malaguti et al. 2003 for GRB021125, from Mereghetti et al. 2003d for GRB021219, from Götz et al. 2003b for GRB030131, from Mereghetti et al. 2003c for GRB030227, from von Kienlin et al. 2003b for GRB030320 and from Beckmann et al. 2003 for GRB030501. The first column lists the date of the GRB, the second the duration of the burst. Column “GRB Location” quotes for SPI and IBIS-ISGRI (and IBIS-PICsIT in one case) the centre (in R.A. and Dec.) and radius r of the error circle (90% confidence value) together with the signal-to-noise (S/N) ratios, with which the GRB was detected. The column “GRB Loc. Offset” lists the the offset angles of centre of the SPI-error circle (SPI) to the one obtained by IBIS and the offset angle of the GRB (IBIS localisation) with respect to the INTEGRAL pointing direction (Point.). The next column specifies the peak flux in the 20 – 200 keV energy range. The GRB fluence is given for the same energy range. The column “Photon Index” gives the result of a model fit of the GRB spectrum with a power law. Several fields of the table are left blank, because the corresponding values are not reported in the references mentioned above. The fluxes and fluences in Crab units were determined in other energy ranges than the standard 20–200 keV range used for the table (see text).

GRB Location GRB Loc. Offset Peak Flux Fluence Photon GRB Durat. Instr.

R.A. (J2000) Dec. (J2000) r S/N SPI Point. [ photons

cm2s

] [ erg cm2 × 10−6 ] Index

SPI 19h 07m 06∘ 25′ 21’ 15.4 3.22 ± 0.50 3.93 ± 0.27 1.88 ± 0.10 030501 ∼ 40 s ISGRI 19h 05m30s 06∘ 18′ 26” 3’ 10.0

19’ 13.25∘ 2.7 ± 1.0 3 ± 1 1.75 ± 0.10

SPI 17h 53.4m −26∘ 2.8′ 33’ 7.2 3.1 13.5 +2.1−2.6 1.51 ± 0.16 030320 ∼ 60 s ISGRI 17h 51m42s −25∘ 18′ 44” 3’ 15

49.8’ 15.5∘ 5.7 11 1.69 +0.07−0.08

SPI 4h 59.1m +20∘31.9′ 31’ 7.7 1.317 ± 0.270 0.96 ± 0.14 2.2 0.45−0.33 030227 ∼ 20 s ISGRI 4h 57m32.2s +20∘29′ 54” 3’

21.6’ 8.55∘ 1.1 0.75 1.85 ± 0.2

SPI – – 8.6∘− 6.4 ± 1.0 Crab 137 ± 8 Crab · s – 030131 ∼ 150 s ISGRI 13h 28m21s +30∘40′ 33” 2.5’ 0’ 10.6∘ ∼ 1.9 (6.5 Crab) 7

SPI 18h 49.3m 31∘ 46.1′ 28’ 8.5 10.7 ± 1.1 Crab 30 ± 3 Crab · s – 021219 ∼ 6 s ISGRI 18h 50m25s +31∘ 56’ 23” 2’ 15.5

17.6’ 9.96∘ ∼ 3.7 0.9 2.0 ± 0.1

SPI 19h 47m55s +28∘23′ 49” 13’ 53 22.9 ± 1.3 Crab 386 ± 44 Crab · s − 021125 ∼ 24 s ISGRI 19h 47m56s +28∘23′ 28” 2’

0.5’ 7.2∘ 14 ± 2 Crab (mean) ∼ 51 (in 20– ∼ 2.2 PICsIT 19h 47m51s +28∘19′ 16” 5’ – – 9 ± 1 Crab (mean) 500 keV range) ∼ 3.7

detectors of SPI’s camera, which are sensitive in the broad energy range from ∼ 20 keV to ∼ 8 MeV. Due to the high S/N-ratio, with which the GRB was seen in these data, the radius of the obtained error circle is approximately twice the one of IBIS/PICsIT. The error circles of IBIS & SPI are overlaping each other, thus confirming the reported GRB location. By comparing the count rate of the GRB event with the one of a Crab observation, recorded at a similar off-axis angle (6.45^∘), one gets the flux and fluence in the 20 keV – 8 MeV range in Crab units. For IBIS it was only possible to extract the mean flux in praticable energy ranges of the instruments (ISGRI: 20–180 keV, PICsIT: 180–500 keV). The mean flux of SPI is 9.2 ± 1.1 Crab and agrees reasonably with the values in Tab. 1. The attempt to extract a GRB spectrum from the SPI on-board spectra failed, because there is still an uncertainty in the determination of the time interval, during which the spectrum was recorded.

GRB021219: Also the second FoV-GRB occurred during the payload performance and verification phase (Mereghetti et al. 2003d). During this time SPI was still in a restricted telemetry mode, due to the telemetry limitations in the beginning of the mission. In this case only the multiple detector events and the events which were processed by the Pulse-Shape-Discriminator (PSD) were downlinked together with the technical- and sciencehousekeeping data. This mode is especially unsuitable for the analysis of GRBs, because the single events, carrying the energy information below 200 keV are disregarded on board. Thus the same analysis method was used as described for GRB021125. The GRB location, lightcurve, fluxes and fluence were determined with the help of the counter data of the 19 Ge-detectors. The obtained error circle overlaps with the position reported by ISGRI. The flux and fluence, again in Crab units, agrees with the one determined for ISGRI.

GRB030131: As the burst occurred during the slew of INTEGRAL, the standard software could not be used to extract the burst as described in section 2.2. As SPI was in a restricted telemetry mode, only multiple events and those single events analysed by the PSD are availabale for the analysis of this burst. Due to the weakness of the burst which adds to the problems of analysing the burst, no reliable position could be derived from the SPI data.

But using again the counter data of the 19 Gedetectors contained in the science-housekeeping data, it was possible to determin the lightcurve shown in Fig. 1. The burst can bee seen as an increase of the flux starting at ∼ 07:38:50 UTC until the end of the most prominent peak at ∼ 07:39:52 UTC. Probable a part of the next 40 s can be also attributed to the burst event. Although the spacecraft startet slewing at ∼ 07:39:06 the derived lightcurve is not affected. The peak flux at 10:39:48 UTC agrees well with the one reported by ISGRI (Götz et al. 2003b). The fluence listed in Tab. 1 was determined for the time period 07:38:50 – 07:39:52 UTC.

GRB030227: This long (20 sec) GRB was the first one which was observed in the SPI field of view, while

4 A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities

Fig. 1. SPI lightcurve of GRB030131 obtained from the detector count rates in the energy range 0.02 – 8 MeV, which are part of the scientific-housekeeping data; time starts from 07:38:00 UT. The flux in Crab units has been derived by comparing the count rate with the one measured for the Crab nebula.

SPI was in full operational mode. It was detected by the IBAS program based on the analysis of the IBIS/ISGRI data (Götz et al. 2003a). Analysis of SPI data on this GRB gave a position 0.36^∘ off the IBIS position. Even though the burst was weak (total fluence for SPI F = (9.6±1.4)·10^{−7}ergs cm^{−2}) a spectral extraction in 2 s wide bins was possible and the SPI data show an indication for hard-to-soft evolution (Mereghetti et al. 2003c). The overall spectrum has a rather steep slope: Γ = 2.2^{0.45}_{−0.33} (90% confidence value).

GRB030320: So far, this is the GRB observed at the largest off-axis angle, near to edge of the field of view of SPI (von Kienlin et al. 2003b). Using the single and multiple detector events SPI was able to localise the GRB in the 100 keV to 1 MeV energy range to an error circle with a radius of 53’ (99% confidence value) which agrees with the IBIS position. The creation of a lightcurve with a 1 s time binning was only possible when using the Gedetector count rates of the science housekeeping data. The lightcurve exhibits two prominent peaks during the ∼ 60 s of prompt emission which are separated by ∼ 35 s. The flux, fluence and the photon index for SPI was derived by analysing the count spectrum with an alpha-test version of XSPEC 12.0. It crops up that in the case of this GRB the XSPEC 12.0 derived results are in better agreement, compared to the results obtained with the method described in chapter 2.2. One has to bear in mind that the instrument response for sources observed at such large off-axis angles is not fully understood, because of deficiencies in the knowledge of the mass model.

The hard-to-soft spectral evolution observed for ISGRI is not apparent in the SPI data, nevertheless it was possible to confirm the derived ISGRI fluxes of the first and second peak of emission.

GRB030501: This long (∼ 40 sec) GRB was detected in the partially-coded FoV of both, IBIS and SPI (Mereghetti et al. 2003b). The position and error circle extracted from the SPI data agree with the one obtained by ISGRI. The spectral extraction from both instruments show a similar peak flux, fluence, and spectral shape (Γ = 1.8 ± 0.1 for a single power law). Also comparison with Ulysses (Hurley et al. 2003b) and RHESSI (Lin et al. 2002) data showed remarkably consistency. Although the flux seems to be correlated with the hardness of the GRB spectrum, there is no clear soft-to-hard evolution seen over the duration of the burst (Beckmann et al. 2003).

2.4. Discussion of the obtained results

The first six GRBs observed with INTEGRAL showed that SPI was always able to detect the same event and to confirm in most cases the results obtained with IBIS. For the three first bursts it has to be considered that the capabilites of SPI were weakened by the telemetry limitations in the beginning of the mission. The next event was the weak GRB030227 and the last two were observed at a large offset angle, where only 3 to 5 of the 19 Gedetectors were irradiated by the GRB. So the demonstration of SPI’s full capabilities in the case of a strong event in the fully-coded FoV still has to take place.

Looking at the current data set summarised in Tab. 1 most of the GRBs were detected with a S/N between 7 and 16, with the exception of GRB021125. At this level SPI is able to localise the GRB down to error radii of 20’ – 30’ and the error circle (90% confidence) overlapped in most cases with the one of IBIS. Also the peak flux, fluence and photon indices agreed approximately with the one derived by IBIS.

The GRB detection rate in the FoV of SPI of ∼ 1 GRB/month in the first six months of the mission and the obtained positioning errors confirmed the simulations and calculations carried out before by Skinner et al. 1997.

3. GRB detection with ACS

3.1. Detection capabilities

The ACS provides a large effective area for the detection of bursts (von Kienlin et al. 2003a), but unfortunately with no or only very coarse positional information. The ACS consists of 91 BGO crystals with a total mass of 512 kg. The energy range for burst detection is determined by the setting of the energy-discriminators for veto generation, which is a tradeoff between background reduction and dead-time for the SPI camera. As a veto shield the ACS has no upper limit of the energy range. The sensitivity to γ-rays depends among other things (e.g projection area) on the attenuation length in the BGO crystals which

A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities 5

have thicknesses ranging from 16 mm at the top to 50 mm at the bottom near to the Ge-camera.

It is not possible to quote an exact lower energy threshold, due to the redundancy concept chosen for the ACS hardware. Each of the 90 BGO crystals is viewed by two photomultipliers (PMTs), which are read out by 90 frontend electronic (FEE) boxes (The 91^{th} BGO crystal is read out by a single PMT and FEE). The redundancy concept of the ACS is obtained by the cross wiring of neighbouring crystal and electronic boxes. In this way always anode signals from two PMTs connected to neighbouring crystals are summed in one FEE. It emerges that a disadvantage of this method is an uncertainty in the energy-threshold value of individual FEEs, caused by different light yields of neighbouring BGO-crystals and different PMT properties like quantum efficiency and amplification. A result of this is that the threshold extends over a wide energy range and is not at all sharp. Since the commissioning phase which took place in the first two months after launch the energy discriminators settings were set at a constant level which corresponds to approximately 75^{+75}_{−25} keV.

For the GRB detection on ground with IBAS the ACS housekeeping (HK) data are monitored. These data include the values of the overall veto counter of the veto control unit (VCU) and the individual ratemeter values of each FEE. Both kinds of HK data are suitable for burst detection. The count rate of the overall veto counter (ORed veto signals of all 91 FEEs) is sampled every 50 ms. A packet, containing 160 consecutive count rates, is transmitted every 8 s to ground. If no gap in the telemetry stream occurs one could have a continuous ACS veto-rate light curve with 50 ms binning. The measurement time of the individual FEE ratemeter can be adjusted between 0.1 and 2 s. An integration time of 1.048 s has been selected for the mission. All 91 FEEs are read out successively in groups of 8 FEEs every 8 s. The readout of all 91 ratemeter values thus needs 96 s. In contrast to the VCU overall veto counter the individual ratemeter values do not yield a continuous stream. Additionally the values of different FEE groups are shifted by a time interval of 8 s. So it is very difficult, to derive the burst-arrival direction from these individual counting rates.

The SPI/ACS Burst-Alert System is one branch of IBAS. The trigger algorithm used looks for a significant excess with respect to a running average, comparable to the trigger algorithm used for other spacecrafts (e.g. Ulysses). All IBAS processes are multi-threaded applications and run as daemon processes. In the current configuration the ACS overall veto-counter values are monitored simultaneously at 8 different timescales (0.05 s, 0.1 s, 0.2 s, 0.4 s, 0.8 s, 1 s, 2 s and 5 s). An alert is generated if two of the monitor programs detect a count-rate excess above a predefined significance level, which can be set individually for each timescale. The monitoring of the ratemeter values of individual FEEs is not yet implemented into the ACS part of IBAS but could help to give a rough estimation of the GRB arrival direction. This information could be used to distinguish between the two arrival-cone intersections of the interplanetary network. The SPI-ACS burst alerts distributed by IBAS are providing the time of occurrence in UTC, the spacecraft orbital position (in R.A., Dec. and distance to geocenter) and a 105 s light-curve (5 s pre burst trigger, 100 s after burst trigger) with 50 ms resolution.

Since December 2002 ACS has been added to the 3^{rd} interplanetary network^1 (IPN) of γ-ray detectors. During the first year of the INTEGRAL mission the IPN will consist Ulysses, Mars Odyssey 2001, Konus-WIND, HETE-II, RHESSI and of course INTEGRAL/SPI-ACS (Hurley 1997). The network will have an excellent configuration during this time, due to the large spacecraft separations between Earth, Mars and Ulysses, which is orbiting around the sun, out of the ecliptic plane.

3.2. Results obtained for the first bursts observed with SPI/ACS

We present here the analysis of GRBs detected with the SPI-ACS during the first eight months (November 2002 - June 2003) of the INTEGRAL mission. Subsequently, the selection criteria are defined and the burst sample will shortly be discussed.

3.2.1. Sample selection

GRBs show a large variety in appearance, e.g. light-curve shape and observer-frame duration. In order to allow a decent statistical analysis, an applicable and robust selection of the sample of GRB events in the SPI-ACS overall rate is required.

Naturally, the best criterion for selecting GRBs from the variety of events in SPI-ACS is the localisation on the sky. As SPI-ACS has no spatial resolution, this selection is fully dependent on the localisation or confirmation of the respective events by other missions [e.g. IPN, HETE- II]. These bursts constitute only a subsample of the GRBs detected by SPI-ACS as different instrumental properties of the according missions (e.g. energy range, sensitivity) do not allow the simultaneous observations/detections of all GRBs of the entire sample. Obviously, it is worthwhile to study also the sample of bursts which are only visible in the SPI-ACS rates and not confirmed elsewhere. Probing the very high energies with the unprecedented sensitivity of the SPI-ACS might open new insights into the burst populations and burst physics.

We define our sample based on the only property measurable by the SPI-ACS, the observer-frame light curve. In Fig. 2 three example light curves are shown, representing the known variety of burst shapes (Fishman & Meegan 1995). The selection criteria for our sample are as follows: an event is categorised as a probable GRB when the total significance above the background exceeds a significance level of σ=12 in at least one time interval during the event. E.g., assuming a typical background value of 3700 counts per 50 ms and taking into

1 3^{rd} IPN website: http://ssl.berkeley.edu/ipn3/index.html

6 A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities

Fig. 2. Overall rate light curves for three typical GRBs detected by SPI-ACS with 50 ms time resolution. We show (from left to right) the extraordinary bright IPN triangulated burst 021206 (Hurley et al. 2003c), the short triangulated event from 17th of January 2003 (Hurley et al. 2003a) and the extensively studied (Stanek et al. 2003, Hjorth et al. 2003 and references therein), nearby (z=0.168; Greiner et al. 2003) GRB 030329.

account the measured FWHM of the ACS background distribution which is larger then the expected poissonion distribution by a factor of 1.6, e.g. a single 50 ms event with 4870 total counts (source+background), a 3x50 ms event with 4500, 4400 and 4250 counts, respectively, will match the selection. Each event is subsequently checked for solar or particle origin using JEM-X and the GOES web page^2 and IREM, respectively. Nevertheless, one has to be aware of the only approximatively known (due to varying background) biasing against faint short bursts. Thus, the SPI-ACS GRB sample described here certainly favours the population of long bright bursts. The complete SPI-ACS GRB sample including statistics is available online^{3,4}.

3.2.2. Analysis and discussion

According to our sample selection described above, a total of 145 GRB candidates were detected during the first 8 months of the mission. 58 of these have been confirmed by other instruments. Using the elapsed mission time, we find an approximate rate of GRBs detected by the SPI-ACS of ∼290 (∼116 confirmed) per year which is in good agreement with the predictions given in Lichti et al. (2000) prior to the start of the mission. The total rate is comparable also to BATSE (Paciesas et al. 1999).

In addition to the number of events, the SPI-ACS overall rate provides the possibility of deriving the burst duration in the instrumental observer frame and the variability of the light curve. As no spectral resolution exists, typical burst parameters such as fluence and peak flux can not be derived. Only the total integrated counts and the counts in the burst maximum can be extracted from the light curve. In the following, only the distribution of the instrumen-

2 http://www.sec.noaa.gov 3 http://www.mpe.mpg.de/gamma/instruments /integral/spi/acs/grb 4 http://isdc.unige.ch/index.cgi?Science+grb

Fig. 3. Distribution of T_{90} for all GRB candidates (solid line) and for 1234 GRBs from the 4th BATSE GRB catalogue (Paciesas et al. 1999; dotted). In order to compare with the SPI-ACS detections, the BATSE distribution is scaled to the elapsed INTEGRAL mission time (8 month). Note the very large fraction of short events compared to BATSE.

tal observer-frame burst duration will be discussed. Other statistical issues (intensity, variability) will be presented in later publications and in Ryde et al. (2003).

Fig. 3 shows the distribution of the measure for the duration T_{90} (the time interval starting after 5% and ending after 95% of the background subtracted event counts have been observed) for the sample of SPI-ACS GRBs in comparison to the observed distribution of 1234 GRBs from the 4^{th} BATSE GRB catalogue (Paciesas et al. 1999). Despite the small sample, a bimodality in the distribution comparable to that found by BATSE is observed. But two main differences emerge: i) the SPI-ACS sample contains a significantly higher fraction of short burst candidates and ii) the maximum of the short distribution is offset towards shorter duration for the SPI-ACS sample.

A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities 7

Fig. 4. Same as Fig. 3 except that here only the confirmed SPI-ACS burst sample (solid line) is displayed. While most of the long duration bursts are confirmed (see Fig. 3) for comparison an obvious lack of short GRBs can be noticed.

The fraction of short (<1 s) duration GRBs is ∼0.48 (70/145) for the SPI-ACS sample compared to 0.20 for BATSE (Paciesas et al. 1999). As BATSE was observing a softer energy band (50-320 keV) and was therefore more sensitive to X-ray rich (long) GRBs than SPI-ACS, a larger short/long ratio could have been expected for our sample. What is remarkable is the sharpness of the short distribution around 0.1 s. Due to the limited time resolution of 50 ms the short end cannot be sufficiently defined and resolved by our data. BATSE was able to trace the distribution to smaller values of T_{90} due to the better time resolution of 200μs.

The offset of the maximum for the short events to smaller T_{90} might be due to the different energy bands of SPI-ACS and BATSE. An apparently shorter duration is measured as it would be if the bursts would have been observed by BATSE. As T_{90} depends strongly on the instrumental characteristics and as it is still unclear how this measure connects to the source frame quantity for a given burst, the discrepancies are neither surprising nor do they necessarily trace different burst populations.

Still, the connection of the short events with real GRBs is not clear as this population is only marginally observed by other instruments as shown in Fig. 4. While a large fraction (73%; 55/75) of the long bursts are confirmed less than 6% (4/70) of the short events were observed by other missions. This might be explained at least twofold. On the one hand we might observe a ’real’ short and very hard GRB population, which could so far only be detected with SPI-ACS due to its high sensitivity at very high energies. As the current IPN members and HETE-II are generally more sensitive at lower energies a high fraction of un-confirmed short (and possible hard) events would not be surprising. These bursts should then have peak energies above 400 keV. On the other hand, a significant contribution to these short events from instrumental effects and/or cosmic ray events can not be ruled out. A small contribution might also arise from soft gamma-ray repeaters

(SGRs). SGRs are a small class of objects that are characterised by brief and intense bursts of hard X-rays and soft gamma rays. Without localisation SGR bursts can not be distinguished from short GRBs within SPI-ACS. The issue of origin of the short events is certainly of high interest and needs a more detailed investigation

4. Conclusions

SPI confirmed so far all six GRBs detected by IBIS within the FoV. With the exception of one GRB SPI was able to derive a GRB position, and for GRBs observed with SPI operating in full telemetry mode, spectra could be extracted. In one case (GRB030227) some evidence for a hard-to-soft spectral evolution was found in both, ISGRI and SPI

The ACS of SPI has detected 145 GRBs during the first 8 months. At first preliminary analysis of their duration reveals significant differences of their distribution with the one of BATSE. The ACS seems to detect very short GRBs (i.e. shorter than 0.2 s). These bursts are much shorter than the typical short burst, which last for ∼ 1 seconds. It is unclear if this new “population” is real or an artifact of the ACS caused by an electrical effect. Also not understood is the deficiency of the normal short (< 2 s) GRBs. It may be due to the fact that the energy threshold of the ACS is somewhat higher than the one of BATSE. It is the hope that with the continuing observations of GRBs with INTEGRAL these discrepancies can be explained.

Acknowledgements. The SPI project has been completed under the responsibility and leadership of CNES. We are grateful to ASI, CEA, CNES, DLR, ESA, INTA, NASA and OSTC for support. The SPI/ACS project is supported by the German ”Ministerium für Bildung und Forschung” through DLR grant 50.OG.9503.0.

References

Beckmann, V. 2002, Proc. XXII Moriond Astrop. Meeting, p.

417, astro-ph/0206506 Beckmann, V., Borkowski, J., Courvoisier, T.J.-L., et al. 2003, A&A, this volume Boella, G., Butler, R. C., Perola, G. C. 1997, A&AS, 122, 299 Coburn, W., & Boggs, S.E. 2003, Nature 423, 415 Costa, E., Frontera, F., Heise, J., et al. 1997, Nature 387, 783 Fishman, G.J., Meegan, C.A., Wilson, R.B., et al. 1989, BATSE: The Burst and Transient Source Experiment on the Gamma Ray Observatory. In Proc. GRO Science Workshop, GSFC, 2 Fishman, G.J. & Meegan, C.A. 1995, ARAA 33, 415 Galama, T.J., Vreeswijk, P.M., van Paradijs, J., et al. 1998, Nature 395, 670 Götz, D., Borkowski, J., Mereghetti, S., 2003a, GCN 1895 Götz, D., Mereghetti, S., Hurley, K., et al. 2003b, A&A, this volume Granot, J. 2003, ApJL submitted, astro-ph/0306322 Greiner, J., Peimbert, M., Estaban, C., et al. 2003, GCN 2020 Hjorth, J., Sollerman, J., Møller, P., et al. 2003, Nature 423, 847

8 A. von Kienlin et al.: INTEGRAL Spectrometer SPI’s GRB detection capabilities

Hurley, K. 1997, in Proc. 2^{nd} INTEGRAL Workshop, ESA SP

382, 491 Hurley, K., Mazets, E., Golenetskii, S.,et al. 2003a, GCN 1829 Hurley, K., von Kienlin, A., Lichti, G. et al., 2003b, GCN 2187 Hurley, K., Cline, T., Smith, D.M., et al. 2003c, GCN 2281 Kawabata, K.S., Deng, J., Wang, L., et al. 2003, ApJL accepted, astro-ph/0306155 Klebesadel, R., Strong, I., Olsen, R. 1973, ApJ 182, L85 Lichti, G.G., Georgii, R., von Kienlin, A., et al. 2000, in Proc.

of the Fifth Compton Symposium, AIP Conf. Proc. 510, 722 Lin, R.P., Dennis, B.R., Hurford, G.J., et al. 2002, Solar

Physics 210, 3 Malaguti, G., Bazzano, A., Beckmann, V., et al. 2003, A&A,

this volume Mereghetti, S., Götz, D., Borkowski, J., et al. 2003a, A&A, this

volume Mereghetti, S., Götz, D., Borkowski, J., et al. 2003b, GCN 2183 Mereghetti, S., Götz, D., Tiengo, A., et al., 2003c, ApJL accepted Mereghetti, S., Götz, D., Beckmann, V., et al. 2003d, A&A,

this volume Metzger, M.R., Djogovski, S.G., Kulkarni, S.R., et al. 1997,

Nature 387, 879 Paciesas, W. S., Meegan, C. A., Pendleton, G. N., et al. 1999,

ApJS 122, 465 Ryde, F., Borgonovo, L., Larsson, S., et al. 2003, A&A, this

volume Skinner, G.K., Connell, P.H., Naya, J.E., et al. 1997, in Proc.

2^{nd} INTEGRAL Workshop, ESA SP 382, 487 Skinner, G. K., & Connell, P. H. 2003, A&A, this volume Stanek, K.Z., Matheson, T., Garnavich P.M., et al. 2003, ApJL

submitted, astro-ph/0304173 Ubertini, P., Lebrun, F., DiCocco, G., et al. 2003, A&A, this

volume van Paradijs, J., Groot, P.J., Galama, T., et al. 1997, Nature

386, 686 Vedrenne, G., Roques, J.-P., Schönfelder, V. et al. 2003, A&A,

this volume von Kienlin, A., Arend, N., & Lichti, G.G. 2001, in Proc. of

the International GRB workshop held in Rome, Springer, 427 von Kienlin, A., Arend, N., Lichti, G.G., et al. 2003a, in SPIE

Conf. Proc. 4851, X-ray and Gamma-ray Telescopes and Instruments for Astronomy, 1336 von Kienlin, A., Beckmann, V., Götz, D., et al. 2003b, A&A,

this volume von Kienlin, A., Arend, N., & Lichti, G.G., et al. 2003c, in

Proc. of the International GRB workshop held in Rome, to be published