arXiv:cond-mat/0107400v1 [cond-mat.dis-nn] 19 Jul 2001

Formation of a stable decagonal quasicrystalline Al-Pd-Mn surface layer

D. Naumović,^1 P. Aebi,^1 L. Schlapbach,^1 C. Beeli,^2 K. Kunze,^3 T. A. Lograsso,^4 D. W. Delaney^4 1Institut de Physique, Université de Fribourg, Pérolles, CH-1700 Fribourg, Switzerland 2Laboratory of Solid State Physics, ETHZ, CH-8093 Zürich, Switzerland 3Institute of Geology, ETHZ, CH-8092 Zürich, Switzerland 4Ames Laboratory, Iowa State University, Ames, Iowa 50011, USA

We report the in situ formation of an ordered equilibrium decagonal Al-Pd-Mn quasicrystal overlayer on the 5-fold symmetric surface of an icosahedral Al-Pd-Mn monograin. The decagonal structure of the epilayer is evidenced by x-ray photoelectron diffraction, low-energy electron diffraction and electron backscatter diffraction. This overlayer is also characterized by a reduced density of states near the Fermi edge as expected for quasicrystals. This is the first time that a millimetersize surface of the stable decagonal Al-Pd-Mn is obtained, studied and compared to its icosahedral counterpart.

61.44.Br, 79.60.-i, 61.14.-x, 61.14.Qp

Quasicrystals are exceptional in many aspects. They emerged from the rather complex Al-Mn phase diagram at the beginning of the 80’s [1]. Their structure is infringing the classic rules of crystallography: they are non periodic, but long-range ordered, and they include forbidden symmetry axes such as five-fold (5f), 8f, 10f or 12f, depending on the alloy [2]. Furthermore, the electronic structure of quasicrystals is quite unexpected. The electrical resistivity is a thousand times higher than their constituents, metals, and inversely proportional to temperature [3]. Despite the lack of periodicity a bandlike behavior is observed in the electronic structure [4,5]. Quasicrystals also exhibit properties which are directly attractive for applications, such as low friction, low adhesion or increased hardness [6].

Even today, producing quasicrystals, and especially monograin samples of stable phases, remains a challenge. In that sense, one of the most fruitful systems is Al- Pd-Mn. In 1990, Tsai et al. discovered a first stable icosahedral (i) quasicrystal (i-Al_{70}Pd_{20}Mn_{10}) in the ternary Al-Pd-Mn system [7]. It is possible to produce high-quality large monograins of this alloy. This facilitates experiments, such as neutron or x-ray diffraction, or surface experiments, to be performed on quasicrystals. A stable, decagonal (d) Al-Pd-Mn quasicrystal was found by Beeli, Nissen and Robadey [8]. It exists only in a very narrow area in the phase diagram [9]. Therefore, it is difficult to obtain a single-phase specimen with high quality of the decagonal structure. Interestingly, a decagonal quasicrystal with high structural quality can be obtained by annealing rapidly quenched tapes of an Al_{69.8}Pd_{12.1}Mn_{18.1} alloy, which contains a metastable icosahedral phase, but has the equilibrium composition of the decagonal phase [8]. Thus the icosahedral long-range order is coherently transformed into decagonal long-range order. Furthermore, single-grain samples can only be produced by non-equilibrium processes via metastable reactions, and, generally, only by chance single grains with diameters of 0.1 mm are produced. Nevertheless, Al-Pd-Mn has the only known phase diagram containing two stable quasicrystalline phases, the icosahedral and the decagonal.

Until now, many surface experiments have been reported on monograin i-Al-Pd-Mn. Clean surfaces are prepared either by fracturing [10–12] or by ion sputtering, and by annealing. Composition changes are induced by preferential sputtering of the lightest elements, or by thermal diffusion. For annealing temperatures lower than 400^oC subsequent or simultaneous to sputtering, a crystalline phase with cubic domains (Al_{55}Pd_{40}Mn_5) [13–18] or a metastable decagonal quasicrystalline (Al_{22}Pd_{56}Mn_{22}) phase [19] was observed, respectively. Further annealing of these surfaces at temperatures between approximately 450^o and 650^oC restores a bulk-terminated icosahedral surface and a bulklike composition. Such surfaces are characterized by a reduced density of states close to the Fermi level (E_F ), in contrast to usual metallic surfaces [4,12,16,17,20]. Annealing at higher temperatures produces either Pd or Mn enrichment of the surface, probably depending on the initial bulk composition. An irreversible precipitation of secondary phases is even reported [21]. The Pd-rich surfaces Al_{>66}Pd_{32}Mn_{<2} [14,22] or Al_{50}Pd_{49}Mn_1 [18] were interpreted as cubic with domains and the Mnrich Al_{75}Pd_6Mn_{19} surface [23] as corresponding to the crystalline orthorhombic Al_3Mn. Both, low- and hightemperature crystalline phases are epitactically grown on the substrate and rather ordered.

In this work, we produce for the first time a large surface of the stable decagonal quasicrystalline d-Al-Pd-Mn. The 10f-symmetric surface of the stable d-Al-Pd-Mn is epitactically grown as a single-domain overlayer on the 5f-symmetric i-Al-Pd-Mn, with the 10f axis of the overlayer parallel to the 5f axis of the substrate. The Mnrich decagonal overlayer is produced in situ by sputtering and annealing the 5f i-Al-Pd-Mn at about 650^oC. The results on geometrical (Fig. 1) and electronic structure (Fig. 2), obtained with low-energy electron diffraction (LEED), x-ray photoelectron diffraction (XPD), electron backscatter diffraction (EBSD) and ultraviolet photoemission (UPS), clearly demonstrate that both the icosahedral surface and the epitactically grown decagonal overlayer can be identified with the corresponding stable bulk phases.

The photoemission experiments were performed in a VG ESCALAB Mk II spectrometer with a base pressure in the 10^{−11} mbar range. The sample stage is modified for motorized sequential angle-scanning data acquisition over the full solid angle [24]. MgK_α radiation (hν=1253.6 eV) was used for x-ray photoelectron spectroscopy (XPS) in order to check the cleanliness of the sample and to determine the composition [25] within the probing depth (mean free path of photoelectrons ∼ 20 Å). XPD served to study the geometrical structure of the surface [26]. In angle-scanned XPD, the intensity variations of photoemitted core-level electrons are recorded as a function of emission angle and stereographically projected in a greyscaled map. For kinetic energies >500 eV, photoelectrons leaving the emitter atom are strongly focused in the forward direction by neighboring atom potentials [26]. So, the intensity is enhanced along densely packed atomic rows or planes. Thus, XPD evidences the average local order around a selected chemical species. UPS measurements are performed with monochromatized He Iα radiation (21.2 eV) [27]. The energy resolution of the analyzer for the UPS measurements was set to 30 meV. All measurements are performed at room temperature.

The symmetry and orientation of substrate and layer were verified ex situ by EBSD [28]. EBSD patterns were recorded using a standard SEM CamScan CS44LB, equipped with a 50 mm diameter area detector (scintillator and high sensitivity TV camera) placed parallel to the incident beam. Diffraction patterns are formed from the spatial intensity distribution of backscattered electrons, which are induced by a focused stationary electron beam (15 kV, 3nA). The sample surface is tilted 70^o against the beam towards the detector. The spatial resolution is in the range of some tenth of a micrometer and anisotropic due to the 70^o tilt. Bands of higher intensity arise between pairs of pseudo-Kikuchi lines, the center of which marks the projection of diffracting symmetry planes onto the detector screen. These bands are detected in digitized EBSD patterns by image processing using a Hough transform [29]. The software OIM2.0 (TSL Inc.) was modified by us incorporating quasicrystallography, so that the model pattern could be recalculated which fits best with the detected diffraction bands for EBSD patterns of any orientation and symmetry.

The i-Al-Pd-Mn quasicrystal ingot was grown using the Bridgman method [30]. Its bulk composition was determined to be Al_{71.6}Pd_{19.6}Mn_{8.6}. The sample was an 1.3 mm thick disk with a diameter of 8 mm. It was oriented perpendicular to a 5f symmetry axis within 0.25^o and polished with diamond paste and colloidal silica.

FIG. 1. LEED patterns taken at 60 eV (high intensity in black) from a monograin i-Al-Pd-Mn cut perpendicularly to a 5f-symmetry axis: (a) the bulk-terminated icosahedral quasicrystalline i-Al68Pd26Mn6 surface obtained after sputtering and annealing at 550^o C; (b) the stable decagonal quasicrystalline d-Al76Pd11Mn13 overlayer obtained after sputtering and annealing at 650^o C. XPD patterns of Pd 3d_{5/2} (E_{kin} = 915 eV, high intensity in white) with indicated normal emission (+), grazing emission (outer circle), 2f- (ellipse), 3f- (triangle), 5f (pentagon) -symmetry axes, taken from, (c), the icosahedral surface described in (a); and, (d), the decagonal surface described in (b). EBSD patterns (high intensity in white; sample normal (+)) taken from, (e), the icosahedral surface described in (a); and, (f), the decagonal surface described in (b). Projections generated by a pattern recognition procedure, with indicated 2f-, 3f-, 5f- (as above), 10f (decagon) -symmetry axes, and 2f- (solid thick line), 5f (dashed thick line)-symmetry planes, (g) identifying (e) as quasicrystalline icosahedral; (h) identifying (f) as quasicrystalline decagonal, with additional 1st order rhombohedral planes (thin solid lines).

For the preparation of the icosahedral surface, sputtering and annealing to 550^oC resulted in XPS compositions of Al_{53}Pd_{41}Mn_6 and Al_{68}Pd_{26}Mn_6, respectively. However, for annealing temperatures of 650^oC, the surface becomes decagonal with a modified composition of Al_{76}Pd_{11}Mn_{13}. In contrast to a metastable decagonal phase Al_{22}Pd_{56}Mn_{22} (an icosahedral surface is recovered after annealing above 400^oC, Ref. [19]), the composition is, in our case, compatible with the stable decagonal quasicrystal composition (Al_{69.8}Pd_{12.1}Mn_{18.1}) [8]. In addition, the decagonal overlayer, once created, remains stable up to 700^oC. After 15 to 30 min sputtering the decagonal surface, the composition is Al_{66}Pd_{15}Mn_{19} and a 5 min annealing at 650^oC is sufficient to recover the decagonal surface. In contrast, typically 5h of sputtering followed by annealing at 550^oC are necessary to recover the icosahedral bulk-terminated surface. Therefore, transformation from the decagonal back to the icosahedral surface is also possible.

Figure 1 displays the experimental data comparing the geometrical structure of the icosahedral bulk-terminated surface, and of the stable decagonal overlayer, measured with LEED, XPD and EBSD. The bulk-terminated icosahedral surface is characterised by a 5f LEED pattern (Fig. 1(a)), while the LEED picture of the decagonal overlayer (Fig. 1(b)) is 10f symmetric. This latter displays four rings of ten fine spots. The relationship between the radii of these four rings is proportional to the golden mean τ, confirming a quasicrystalline ordering of the overlayer. LEED spots are visible over a wide range of energies (12-140 eV). This indicates the long-range lateral ordering of the overlayer 10f surface, compatible with a stable decagonal quasicrystalline phase. Note, that this pattern drastically differs from the one taken from the low- and high-temperature pseudo-10f surface with crystalline domains [13,14,18,22]. Decagonal LEED patterns have been obtained from the d-Al-Ni-Co [31].

The Pd 3d_{5/2} XPD pattern of the bulk-terminated 5f surface is shown in Fig. 1(c). The main high-intensity spots can be easily identified with the 2f-, 3f- and 5fsymmetry axes of the icosahedral group projected stereographically [14,17,32,22], with a 5f-symmetry axis in the center (normal emission). These experimental patterns can be reproduced by single-scattering cluster calculations using clusters as inferred from structural models of the i-Al-Pd-Mn phase, confirming that the near surface region is quasicrystalline [32]. So we conclude that the average local environment around the Pd emitter atoms is icosahedral (idem for Al and Mn, not shown [32]). In contrast, Fig. 1(d) displays the XPD pattern of the Mn-rich stable decagonal overlayer, with an evident overall 10f symmetry and a central 10f-symmetry axis. Here, three rings of equivalent intense spots replaces the alternation of spots identified as 2f-, 3f- and 5f-symmetry axes in Fig. 1(c). This clearly indicates an average short-range decagonal ordering of the overlayer. Strong epitactic-like relationships exist between the icosahedral bulk and the decagonal overlayer. The decagonal XPD pattern resembles the XPD [33] and secondary electron imaging (SEI) [34] patterns taken from d-Al-Ni-Co. Note that the SEI pattern of the decagonal metastable Al_{22}Pd_{56}Mn_{22} overlayer resembles the sputtered d-Al-Ni-Co surface [19]. The XPD patterns of Pdrich pseudo-10f surface [14,22] and of sputtered d-Al-Ni- Co surface [33] were both interpreted as crystalline with bcc domains.

Figures 1(e-f) show the EBSD results obtained ex situ from the icosahedral and decagonal phase created on 5f i-Al-Pd-Mn sample. The EBSD pattern presented in Fig. 1 (e) is identified as corresponding to icosahedral phase (Fig. 1(g)) with a 5f-symmetry axis coinciding with the sample normal (marked by +). Further 2f- and 3f-symmetry axes are situated at crossings of 2f- and 5f-symmetric planes as indicated in Fig. 1 (g). These latter symmetry axes, as well as 5f-symmetric planes, do not exist in the pattern (Fig. 1(f)) identified as decagonal (Fig. 1(h)). Here, a 10f-symmetry axis coincides with the sample normal, and only the radial 2f-symmetric Kikuchi bands crossing the 10f axis persist. As EBSD arises from 200 to 500 Å depth, the thickness of the stable decagonal phase is at least of that order of magnitude. Once the decagonal overlayer formed, the appearance of the icosahedral pattern (alone or superimposed to the decagonal pattern with lower contrast) indicates that some patches (<1%) of the surface are covered with a thinner decagonal overlayer or remain uncovered. In addition, this evidences the strong structural and orientational relationship between the icosahedral bulk and the decagonal overlayer.

FIG. 2. Room-temperature valence-band spectra displaying the near EF region, taken with monochromatized He-I radiation (hν = 21.2 eV), (a) of the crystalline surface with bcc domains (Al53Pd41Mn6; sputtered), (b) of the Mn-rich stable decagonal quasicrystalline overlayer (Al76Pd11Mn13; sputtered and annealed at 650^oC) and (c) of the bulk-terminated icosahedral quasicrystalline surface (Al68Pd26Mn6; sputtered and annealed at 550^o C).

Figure 2 displays valence-band spectra taken at room temperature of the icosahedral bulk-terminated surface, of the stable decagonal overlayer and of a crystalline phase, obtained by sputtering the icosahedral surface. This latter 5f surface consists of five bcc(113) domains rotated by 72^o with respect to each other as seen with XPD [17]. The density of states remains high and linear over the complete range of energy and the Fermi edge is sharp, as expected from a metallic surface (Fig. 2a). In Fig. 2(c), the bulk-terminated icosahedral surface exhibits a completely different behaviour. A distinct decrease of the density of states near E_F , interpreted as the opening of a pseudogap, is observed, as expected from a quasicrystalline surface [4,16,17,20,35]. Finally, the density of states of the stable decagonal overlayer (Fig. 2 (b)) is lowered close to E_F , as for the icosahedral quasicrystalline surface. However, the shape of the curve is slightly different, with a steeper Fermi cutoff. This is probably related to the fact that the decagonal surface is periodic in one dimension (along the surface normal) and that the quantity of Mn (Mn 3d states determine the spectral weight close to E_F [35]) is doubled in the decagonal phase compared to the icosahedral and crystalline bcc phases.

An important point to be discussed is how to ensure the quasicrystallinity of the surface. In previous work on i-Al-Pd-Mn [16,17], we demonstrated that a combination of geometrical and electronic structure techniques can efficiently characterize the quasicrystal surfaces. First, the ordering and the symmetry within differently prepared surfaces were probed with XPD and LEED. But note, that a 5f [17] or 10f [14,22] symmetry can also be due to a combination of domains and not only to the intrinsic quasicrystal symmetry. Second, a distinct suppression of spectral weight of the density of states close to E_F was observed on quasicrystalline terminated surfaces by UPS. Here, one has to be aware that a suppressed density of states is also reported on a crystalline approximant of quasicrystal [12]. Whereas, even a slight disordering of the quasicrystal surface, induced by a one-minute ion sputtering, produces a sharp Fermi edge cutoff, characteristic of a metallic surface, with no apparent composition changes [20]. So, a careful evaluation of the geometrical and electronic structure data, together with the composition, is essential to identify quasicrystallinity or, at least, to exclude crystallinity of the surface.

In summary, this work presents for the first time the formation of an extended and ordered stable decagonal quasicrystalline overlayer on 5f i-Al-Pd-Mn by sputtering and annealing at 650^oC. This overlayer was characterized, at different scales, with three structure techniques, XPD, LEED and EBSD. We clearly identified the icosahedral and decagonal symmetries of the surfaces and evidenced the epitactic-like relationships between the decagonal overlayer and the icosahedral bulk. Furthermore the decagonal overlayer exhibited a suppressed density of states near E_F as seen with UPS , as expected for quasicrystals. The production of the two quasicrystalline, decagonal and icosahedral, alloys of the same elemental Al-Pd-Mn family gives the unique opportunity to study and compare the properties of these two phases.

With grateful thanks to M. Boudard, Ph. Ebert, T. Janssen, P. Thiel for fruitful discussions; to the members of the XPD team and the technical staff for help; and to the Swiss National Science Foundation for financial support.

[1] D. Shechtman et al., Phys. Rev. Lett. 53, 1951 (1984). [2] C. Janot, Quasicrystals: A Primer, 2nd ed. (Oxford University Press, Oxford, 1994).

[3] S.J. Poon, Adv. Phys. 41, 303 (1992). [4] X. Wu et al., Phys. Rev. Lett. 75, 4540 (1995). [5] E. Rotenberg et al., Nature 406, 602 (2000). [6] J.-M. Dubois, Phys. Scr. T49, 17 (1993). [7] A. P. Tsai et al., Philos. Mag. Lett. 61, 9 (1990). [8] C. Beeli, H.-U. Nissen, and J. Robadey, Philos. Mag.

Lett. 63, 87 (1991); C. Beeli et al., in Proceedings of the 5th International Conference on Quasicrystals, Avignon, 1994, edited by C. Janot and R. Mosseri (World Scientific, Singapore, 1995) p. 680.

[9] T. Gödecke and R. Lück, Z. Metallk.86, 109 (1995). [10] Ph. Ebert et al., Phys. Rev. Lett. 77, 3827 (1996); Phys.

Rev. B 57, 2821 (1998); ibid. 60, 874 (1999). [11] G. Neuhold et al., Phys. Rev. B. 58, 734 (1998). [12] V. Fournée et al., Phys. Rev. B 62, 14049 (2000). [13] Z. Shen et al., Phys. Rev. Lett. 78,1050 (1997); Phys.

Rev. B 58, 9961 (1998); Surf.Sci. 450, 1 (2000). [14] D. Naumović et al., in Proceedings of the 6th International Conference on Quasicrystals, Tokyo, 1997, edited by S. Takeuchi and T. Fujiwara (World Scientific, Singapore,1998) p. 749.

[15] B. Bolliger et al., Phys. Rev. Lett. 80, 5369 (1998). [16] D. Naumović et al., Phys. Rev. B 60, R16330 (1999). [17] D. Naumović et al., Mat. Sci. and Eng. A. 294-296, 882 (2000).

[18] F. Schmithüsen et al., Surf. Sci. 444, 113 (2000). [19] B. Bolliger et al., Phys. Rev. Lett. 82, 763 (1999). [20] T. Schaub et al., Eur. Phys. J. B 20,183 (2001). [21] P. A. Thiel, in Physical Properties of Quasicrystals edited by Z.M. Stadnik (Springer-Verlag, Berlin, 1999), p. 327.

[22] D. Naumović et al., Surf. Sci. 433-435, 302 (1999). [23] J. Ledieu et al., Mat. Sci. and Eng. A 294-296, 871 (2000).

[24] J. Osterwalder et al., Phys. Rev. B 44, 13764 (1991). [25] Note that XPS concentrations cannot directly be compared with a true stoichiometry because it is only based on intensity ratios including core-level cross sections; see [14,22].

[26] See, e.g., C.S. Fadley, Surf. Sci. Rep. 19, 231 (1993). [27] Th. Pillo et al., J. Electr. Spectrosc. Relat. Phenom. 97, 243 (1998).

[28] J. A. Venables, and C. J. Harland, Phil. Mag. 27, 1193 (1973).

[29] B. L. Adams, S. I. Wright, and K. Kunze, Met. Trans.

24A, 819 (1993); K. Kunze et al., Text. Microstruct. 20, 41 (1993).

[30] D. W. Delaney, T. E. Bloomer, and T. A. Lograsso, in New Horizons in Quasicrystals (Ref. [32]) p.45.

[31] M. Gierer et al., Surf. Sci. 463, L654 (2000). [32] D. Naumović et al., in New Horizons in Quasicrystals, edited by A.I.Goldman et al. (World Scientific, Singapore, 1997) p.86 (For greyscale Figs. 3 and 4, ask “Dusanka.Naumovic@unifr.ch”).

[33] M. Shimoda et al., Surf. Sci. 454-456, 11 (2000). [34] M. Zurkirch, M. Erbudak, and A. R. Kortan, in Proceedings of the 6th International Conference on Quasicrystals (Ref. [14]) p. 67; M. Zurkirch et al., Phys. Rev. B 58, 14113 (1998).

[35] Z.M. Stadnik et al., Phys. Rev. Lett. 77, 1777 (1996).