arXiv:physics/0008009 v4 9 Sep 2000

E-mail address: tsuyoshi.suwada@kek.jpA monitor is to control stabilize the of beams asufficient number of positrons. The author has amonitor using multi-stripline in this purpose. This the design of the monitor based on a numerical analysis. analysis result shows that the resolution of an is to be less than 0.3% nominal operation conditions.1˚˚INTRODUCTIONto test CP violation in the of is an comprising positron The injector was in inject positron beams into the rings. The be 0.64 nC/bunch 1.3 nC/bunch with a repetition of 50 the positron nC/bunch) in to anumber of positrons. Since the is amachine, a of injector linac is minimizing the tuning maximizing stable operation. Stable control of at the beam-position systems[3] the beams is often to aThus, monitoring tools to control the longitudinal of beams at the of the injector linac. Awith is one of the useful monitoring tools on a analysis involving amultipole analysis of the BESM the of sizes at sections by variation of the distribution in the monitor with the multi-stripline the following be to not the but also to The by is almost to contraction. This phenomenon shows that if the wall of the image is negligibly small, coupling of the inner of the to the beams be well as a potential problem. Thus, any simply to the potential problem on the plane. For a the image by a line be as a problem in which the potential is onthe The the image )is given by

jrRIrRRrRrrR(, , , ) (, ) cos( ),f q fp q f= -+ - -2 22 22 2 (1)

r,,the polar of the linecharge and the pickup point on the duct, respectively; R isthe is the line fig.1). also be by in series of r/,

jrRIrRrRkkk(, , , ) (, ) cos( ).f q fp q f= + -� �Ł �łØºŒ øßœ=¥2 1 2 1 (2)

Line Charge I(r,f)

Conducting

Vacuum Duct

R

Pickup(R,q) q=p/8 x

y q=3p/8 q=13p/8

q=5p/8 q=7p/8 q=9p/8 q=11p/8

q=15p/8

Figure 1: Polar of a line eight

the distribution of a traveling the the image is by integrating the charge density with a weight of the

JR IR jr R x x y y dxdy b x y

( , ) ( , , , ) exp ( ) exp ( ) , ( )

q p

f q s s

= ·

- - - - � Ø º Œ ø ß œ Ø º Œ Œ ø ß œ œ

2

2 2 3 0 2 2 0 2 2

where Ib is the the root half of ) is the of gravity of the beam. Assuming that the of sufficiently small to duct radius, , integration is easily byextending the integration area to x,y, as follows:

JR IR xR yR R x y R xy R b x y

( , ) cos sin cos sin ,( )

q p

q q s s q q

» + +

+ - + - +

Ø ºŒ ø ßœ � � � � Ł � � ł � Ø º Œ Œ ø ß œ œ � � � �

2

1 2

2 2 2 2 4

0 0

2 2

2 0 2 0 2

2 0 0 2

the higher the first to terms to the monopole, moments, The sizes the least a be to to total image charges is given by

J JRdJRd

quad ”� �

( , )cos / ( , ) ,

q q q q q

p p

2 0

2

0

2 (5) (6) = - + - � Ł � � ł � s sx y R x y R

2 2

2

0

2

0

2

2

.

The moment is upon both of positions the sizes from the the position be byusing the dipole moments. It is also by using the n-pickup amplitudes ( Vi [in

Jquad k^k_n k k^k_nV V»� �^{= =1 1}2cos / .q (7)

by summing the n-pickup to out the variation to jitter the sensitivity of the to the of the It is that the absolute sizes not be the (sx2- ) of is the lines invariant sy2=const if the positions 3˚˚NUMERICAL METHODout on a simulation in to the on the sizes. only a of this given in The is on potential problem. In this to an system All of the in the system into many domains, which to elements in a manner. potential of be so as to satisfy the of the that is, so as that the to the by using the superposition of the by allthe analysis was by of the potentials distribution a with a total horizontal of ), was also by using finite number of line was so as to symmetrical potentials on the than

Duct center

Outline point on the duct surface

Outline point on the electrode surface

Imaginary charge

2p/n

Segmentation (n)

Segmentation (m)

e d

Angular width

(Dq)

a

b t Figure 2: Segmentation of the

Radial segmentation m4Azimuthal segmentation n240The number of the was by of using (7), while the ) of the was Figure 3 shows that was eight The be from a point of view in terms of the noise ratio the coupling strength the that the outer )the length ) by of beam-position monitor in the an of 15 satisfies a strike on the of is at the of The total is , from beam. For this width, the minimum is to be ~0.6 nC/bunch, on the of the beam-position so to comprise a 50--transmission line. Table 2 shows of the BESM. on the parameters, Fig. 4 shows that using the design the variation of the moment to the (E/) at the horizontal is =7.2 mm/% the energy is 1.7 GeV, with various sizes. beam-position was in this for the sake of simplicity. Assuming that the noise of the pickup amplitudes is expected to be less than 0.5%,which the minimum 15tStripline length [mm]8A monitor with was on the basis of the analysis beams. Eight with moment a than nC/bunch. The rms resolution of the is to be 0.3% conditions. This is small enough to beams at the 6 REFERENCESDesign Report, KEK Report Design Report on PF KEKB, KEK Report 95-18, 1996.K.Furukawa, et ., the Int�l Conf. onPhysics Systems Trieste, Italy, pp.248-250; KEK-Preprint 99-139 (1999).Wiley & Sons, New York,1975), p.54.T. Kohno T. Takuma, Method of Electric Field (CORONA, Tokyo, 1980).[6] T. Suwada, Proc. the 11th Symposium on Science , Akou-gun, Hyougo, 1997, pp.264-266; KEK Preprint 97-183 (1997).[7] T. Suwada, Proc. the 10th Symposium on Science , Japan, pp.269-271; KEK Preprint 95-136 (1995).T. N.Kamikubota, H.Fukuma, H.Kobayashi, Nucl. Instrum. & Methods. A 440No.2 February (2000) pp.307-319.

5678910051015202530

s

x

2

-

s

y

2

[mm

2

]Number of Electrodes

Figure 3: of the of the sizes upon the number of to be yand sy

-0.2-0.100.10.20.300.511.5 sy=0.1mmsy=2.1mm

sy=4.1mm

J

quadEnergy Spread (sE/E) [%]

Figure 4: of the moment to