arXiv:1004.2932v1 [astro-ph.IM] 16 Apr 2010

On-Sky Demonstration of a Linear Band-limited Mask with Application to Visual Binary Stars

J. Crepp^{1,2}, E. Serabyn^3, J. Carson^{3,4,5}, J. Ge^1, I. Kravchenko^{1,6}

jcrepp@astro.caltech.edu

ABSTRACT

We have designed and built the first band-limited coronagraphic mask used for ground-based high-contrast imaging observations. The mask resides in the focal plane of the near-infrared camera PHARO at the Palomar Hale telescope and receives a well-corrected beam from an extreme adaptive optics system. Its performance on-sky with single stars is comparable to current stateof-the-art instruments: contrast levels of ∼ 10^{−5} or better at 0.8” in K_s after post-processing, depending on how well non-common-path errors are calibrated. However, given the mask’s linear geometry, we are able to conduct additional unique science observations. Since the mask does not suffer from pointing errors down its long axis, it can suppress the light from two different stars simultaneously, such as the individual components of a spatially resolved binary star system, and search for faint tertiary companions. In this paper, we present the design of the mask, the science motivation for targeting binary stars, and our preliminary results, including the detection of a candidate M-dwarf tertiary companion orbiting the visual binary star HIP 48337, which we are continuing to monitor with astrometry to determine its association.

Subject headings: instrumentation: high angular resolution, adaptive optics; binary stars

1. Introduction

The band-limited mask (BLM) is an occulter located in the image plane of the Lyot coronagraph. It suppresses telescope diffraction by manipulating the electric-field amplitude of incident starlight (Kuchner and Traub 2002). Compared to other coronagraphic designs, the BLM makes efficient use of photons (Guyon et al. 2006), is robust to low-order optical aberrations (Kuchner et al. 2005; Shaklan and Green 2005; Crepp et al. 2006) and finite stellar size (Crepp et al. 2009), and has

1University of Florida, 211 Bryant Space Science Center, Gainesville, FL 32611

2California Institute of Technology, 1216 E. California Blvd., Pasadena, CA 91125 3Jet Propulsion Laboratory, 4800 Oak Grove Drive, Pasadena, CA 91109

4Max Planck Institute for Astronomy, Heidelberg, Germany

5College of Charleston, 66 George Street, Charleston, SC 29424

6Oak Ridge National Laboratory, Oak Ridge, TN 37831

generated the deepest contrast in the lab to date (Trauger and Traub 2007). It is a viable option for directly detecting terrestrial exoplanets from space (Levine et al. 2009) and is currently slated for use with the James Webb Space Telescope NIRCAM (Krist et al. 2009).

Although the BLM shows great promise for conducting large dynamic-range observations, one has never been tested on an astrophysical source. Moreover, the most common type of BLM used for numerical simulations and lab experiments has a linear structure – as opposed to an azimuthally symmetric (radial) profile – and can be used to search for tertiary companions by blocking the light from two stars at the same time. This simple geometric feature provides access to an important and as yet unexplored observational parameter space: visual binary stars as high-contrast imaging targets.

To justify use of a BLM (of any shape) from the ground, strehl ratios in excess of ≈ 0.88 S_{qs} are required, where ‘qs’ stands for quasi-static and

S_{qs} < 1 is the Strehl ratio provided by the optical system in the absence of atmospheric turbulence (Crepp et al. 2007). This level of correction corresponds to the ‘extreme’ adaptive optics (AO) regime at near-infrared wavelengths. We have access to an AO system and a 1.6m diameter^1 unobscured and well-corrected off-axis subaperture at Palomar that generates Strehl ratios as high as 96% in the K_s-band under good seeing conditions (Serabyn et al. 2007). Upon satisfying the aforementioned criterion, we have built a BLM for on-sky tests and installed it in the Palomar High Angular Resolution Observer (PHARO, Hayward et al. (2001)) camera on the Hale telescope. The aim of this paper is to demonstrate the general utility of the BLM and to highlight the importance of studying the immediate vicinity of binaries.

2. Scientific Motivation

Binaries are a natural result of the star formation process and constitute ≈ 50% of all stellar systems (Duquennoy and Mayor 1991). To date, however, they have been neglected by most highcontrast imaging surveys (including both visual and unresolved binaries). In the case of visual binaries, this observational bias is due to an inability to suppress the light from both stars simultaneously. Depending on the separation and brightness ratio, the presence of a nearby second star will add pointing errors or overwhelm a portion of the final image. Spatially resolving the pair results in significant contrast degradation and reduces the prospects for discovering faint tertiary companions.

A linear BLM has an intensity transmission that depends on only one Cartesian coordinate and can circumvent this problem. Since there are no pointing penalties down its long axis, simultaneous alignment to both stellar components can provide high-contrast images of the circumbinary environment.^2 We now discuss two specific science applications, noting that unresolved binaries are likewise promising targets.

1Telescope diameter as projected onto the primary mirror. 2Other coronagraphs are also capable of targeting visual binaries, but are most often optimized for single stars.

2.1. Triple Star Systems

Observational multiplicity studies can provide important constraints on star formation theories. Consequently, much work has gone into monitoring the mass ratios and separations of multiple-star systems as a function of age – from proto-stars, to clusters of various size, to mature stars in the field (McKee and Ostriker 2007). From this we have learned that stellar cores fragment into multiple objects, usually 2 − 3 (Goodwin and Kroupa 2005), and that dynamical interactions and other environmental effects (Kraus and Hillenbrand 2007) are largely responsible for determining their final architecture.

Numerical simulations are now able to reproduce many of the bulk statistical properties observed in young stellar systems (Bate 2009). However, such models still require fine tuning as they do not yet include all of the relevant physics. Triple stars offer unique testing grounds for studying the more subtle issues that binaries alone cannot address, such as angular momentum orientation, complex accretion and disk truncation, migration, and the Kozai mechanism (Kozai 1962). For example, the existence of a tertiary companion helps constrain the orbital history of the binary. Preliminary analyses comparing the properties of triple stars to binaries and higher-order multiples have helped to shape our understanding of their origin, their dynamical decay into binary and single stars, and the physical effects that govern their evolution (Tokovinin 2008). Such efforts are, however, currently limited by observational biases inherent to the Multiple Star Catalog (MSC^3, Tokovinin (1997)), which lists all known triples and higher-order multiples. The MSC is incomplete in the solar neighborhood, missing ≈ 90% of triple systems (several hundred) within 50 pc (Tokovinin 2004).

Efficient pathways towards finding new triple star systems, and thus improving our knowledge through statistics, include radial velocity measurements of individual binary components and imaging observations of the regions surrounding binaries. A coronagraph that accommodates visual binaries can fulfill this latter role and uncover low-mass tertiaries that standard AO observations may not be capable of detecting.

3http://www.ctio.noao.edu/∼atokovin/stars/

2.2. Circumbinary Exoplanets

Binary stars must be considered when assessing the statistical properties of exoplanets. In addition to their obvious demographical significance, the binary planet population also has theoretical implications for our understanding of how planets form and evolve. The presence of a second star changes the properties of a protoplanetary disk (Artymowicz and Lubow 1994) and, depending on its separation and relative inclination, may either promote or inhibit the growth of dust grains, planetesimals, and embryos (Payne et al. 2009; Xie and Zhou 2009). Models must be able to account for this extra source of radiation and gravity. For example, the efficiency of the core-accretion process is sensitive to the location of the snow-line (Ida and Lin 2004; Kennedy and Kenyon 2008), which is clearly more complicated in a doublestar system. Another leading theory, gravitational instability (Boss 1998), predicts that gasgiant planet formation may be enhanced by a nearby star: injecting turbulence into the disk increases the likelihood for fragmentation. Theoretical models would clearly benefit from observational constraints in addition to those imposed by single stars alone.

So far, the search for planets in binaries has focused primarily on imaging systems with wide (> 100 AU) separations (Bonavita and Desidera 2007; Mugrauer et al. 2007). However, in recognition of the fact that more closely-spaced binaries can provide unique theoretical testing grounds, radial velocity surveys have begun to target systems with much smaller separations (Hatzes et al. 2003; Eggenberger et al. 2007). These efforts have already revealed an important result: short-period planets in S-type (circumstellar) orbits tend to be more massive than their single star counterparts (Eggenberger 2009; Duchêne 2010). An imaging search for planets in P-type (circumbinary) orbits would complement this work and provide further constraints on formation theories (see also Muterspaugh et al. (2007)). Nevertheless, very few teams have established such programs and those that have use indirect techniques that are relatively insensitive to distant companions. As a result, only a handful of circumbinary planets are currently known, anywhere from 2-4 depending on where the dividing line between brown dwarfs and planets is drawn (Lee et al. 2009; Backer et al.

1993; Correia et al. 2005).

Based on the limited sample size of current surveys (e.g., Konacki et al. (2009) have observed 10 systems using radial velocity techniques with a baseline of 5 years at 2 m/s precision), these likely account for only a small fraction of the population. Other data sets suggest that circumbinary planets may be abundant: (i) circumbinary disks have been detected around pre-main-sequence systems, such as CoKu Tau 4 (Ireland and Kraus 2008), KH 15D (Herbst et al. 2008), AK Sco (Andersen et al. 1989), GW Ori (Mathieu et al. 1991), DQ Tau (Mathieu et al. 1997; Boden et al. 2009), and GG Tau (Dutrey et al. 1994); (ii) moderately-separated binaries do not appear to adversely affect the first steps of planet formation – the growth and crystallization of submicron dust grains (Pascucci et al. 2008); (iii) a recent Spitzer study indicates that ∼ 60% of binaries with separations < 3 AU display excess thermal emission from dusty circumbinary debris produced by planet-induced collisional cascades (Trilling et al. 2007); and (iv) simulations indicate that tertiary companions may remain stable in such configurations for billions of years, over a wide range of mass ratios and eccentricities (Holman and Wiegert 1999).

Finally, visual binaries may also be uniquely useful targets because they can be selected to have near face-on orbits. Assuming circumbinary planets form in roughly the same orbital plane as their stellar hosts, a survey that targets binaries with opportunistically selected orientations will have a higher detection efficiency compared to those that observe systems with unknown inclinations.

3. Mask Design & Fabrication

The bandpass and focal ratio, f, constrain the mask design. Fast optical systems can force the size of features to be prohibitively small, whereas broad wavelength coverage affects the inner-working angle (IWA) and Lyot stop throughput. PHARO accepts an f = 15.64 beam from the Palomar AO system (Troy et al. 2000). The K_s filter served as our primary science channel and defined the desired operating range for observations, λ = 1.99 − 2.31 μm. We decided to build a smooth, binary, fourth-order, linear BLM based on these parameters, our available tools,

Fig. 1.— Microscope image of the BLM prior to cleaning. Each stripe is 28μm tall, slightly smaller than a resolution element in K_s. ‘Ringing’ features from the sinc^2 function (Equ. 1), which are responsible for eliminating diffraction, can be seen on either side of the main occulting region.

experience (Crepp et al. 2006), and the aforementioned science motivation. An eighth-order mask (Kuchner et al. 2005), which has less Lyot stop throughput than a fourth-order mask, could not be justified, given the reduction in flux due to the 1.6m diameter subaperture effective size.

A binary linear BLM consists of a series of small stripes (Fig.1). The key to its operation is that each stripe is smaller than the resolution of the optical system, f λmin, hence allowing it to diffract light like a graded mask (Kuchner and Spergel 2003). To prevent diffracted light leakage from the edges of the filter transmission profiles, we chose conservative values for the minimum and maximum design wavelengths: λmin = 1.79 μm and λmax = 2.39 μm. The mask IWA, defined here as the location where the intensity transmission reaches 0.5, is 2.678 λmax/Dtel = 880 mas. The height, h(x), of a single stripe of the BLM is given by: h(x) = f λmin [ 1 − sinc^2 ( πϵx 2 f λmax )] (1) = 28 [ 1 − sinc^2 ( 0.0179857 x μm )] μm, where ϵ = 0.428 and x has units of μm. This profile was repeated vertically 256 times.

The BLM was fabricated using electron-beam lithography at the University of Florida nanofabrication facility. Aluminum served as the opaque material deposit. Lab measurements placed an upper limit on the intensity transmission directly through the ∼200 nm layer at 1 × 10^{−7}. The minimum feature size was set equal to the layer thickness. The mask was placed on a single 0.7 mm thick Boro-Aluminosilicate glass substrate, Corning model 1737, with a K-band transmission quoted at 92%. No anti-reflection coating was applied.

Figure 1 shows images of the mask before it was shipped to the Jet Propulsion Laboratory (JPL), where it was cut from the substrate with a dicing saw to physical dimensions of 0.60 x 0.30 inches and then cleaned in an ultrasonic bath of acetone to remove a protective layer of photoresist that was applied prior to shipping. We ran simulations to ensure that truncation at the mask edges would not diffract starlight into the search area at contrast levels above 10^{−6}. An Aluminum holder was built to fasten the BLM to the PHARO slit wheel.

4. On-Sky Demonstration

4.1. Single Stars: ϵ Eridani

The star ϵ Eridani is an attractive target to demonstrate new coronagraphic technologies (e.g., Macintosh et al. (2003); Proffitt et al. (2004); Itoh et al. (2006); Janson et al. (2007, 2008); Heinze et al. (2008)). It is nearby (d = 3.2 pcs), bright (V∼ 3.7), relatively young (age≈ 730 Myrs (Song et al. 2000)), known to host a lumpy debris disk (Greaves et al. 1998), and shows radial velocity and astrometric signatures consistent with that of at least one substellar companion with a long period (Hatzes et al. 2000; Benedict et al. 2006).

We observed ϵ Eridani (K2V) on 11-07-2008 UT to test the BLM’s on-sky performance. The seeing was ≈ 0.5” in the K_s band and the AO system was running at 1 kHz, providing an on-axis Strehl ratio of ∼ 90% (see Serabyn et al. 2007 for a discussion of the well-corrected subaperture). We acquired 30 occulted images of ϵ Eridani with an integration time of 14.16s each and 5 unocculted images with an integration time of 4.25s each, using a wellcharacterized neutral-density filter to calibrate the photometry. We also acquired 15 occulted images of a nearby calibrator star, δ Eridani, to suppress quasi-static speckles via PSF subtraction. Only several minutes elapsed on average between acquisition of science images and those of the calibrator to minimize evolution of the speckle pattern. This technique has been successfully employed before at Palomar by Mawet et al. (2009) and Serabyn et al. (2010) who used a phase-mask coronagraph to characterize the debris disk around HD 32297 and reconfirm detection of the HR 8799 planets in the near-infrared.

We processed the data with an in-house reduction code written in Matlab. The procedure utilizes standard flat-fielding, bad pixel correction, and sky background subtraction techniques. After applying a quadratic high-pass Fourier filter to each occulted image, to remove the smooth component of the speckle halo, we used the ‘locally optimized combination of images’ (LOCI) algorithm (Lafrenière et al. 2007) with a box size of 3 × 3 PSF FWHM’s to perform PSF subtraction.

Fig. 2 shows images of the target star, calibrator, and subtraction residuals. The BLM clearly removes the vast majority of diffracted starlight. Only a hint of the first two Airy rings remain in the pre-subtraction images; these residuals are due to the fact that we purposefully use a slightly oversized Lyot stop to increase the throughput of companions and improve spatial resolution. We find that a smaller Lyot stop enables the BLM to remove all on-axis diffracted light in the lab. Onsky Airy rings are extremely stable and subtractout better than speckles – when using the wellcorrected subaperture, though minimizing their initial intensity is likewise important.

To calculate our sensitivity in terms of contrast, we added the photon-noise and speckle noise in quadrature. Fig. 3 shows results for a 2 λmax/Dtel wide region running perpendicular to the mask axis, where the contrast above and below the BLM has been averaged. The LOCI algorithm provides a factor of ∼ 2 − 3 improvement over standard PSF subtraction. We were able to reach 5σ contrast levels of 3.5 × 10^{−5} at 0.8”, 1.3 × 10^{−5} at 2.0”, and 4.0 × 10^{−6} at 4.0”, which correspond to masses of ≈ 24.0M_J , 19.2M_J , and 14.7M_J respectively at an age of 730 Myrs (Baraffe et al. 2003). Though no companions were detected,^4 these observations represent the most sensitive K_s high-contrast images of ϵ Eridani inside of 5” to date, even though the aperture used is much smaller than in previous studies

4The inverse operation, using ϵ Eridani as a calibrator for δ Eridani, also did not reveal any candidates.

(see aforementioned references).

More images would allow us to improve PSF subtraction by constructing a better calibrator reference with the LOCI algorithm and approach the limit set by the photon-noise of the speckles. To decrease this floor further, the non-common-path errors between the AO system and PHARO must be reduced. Precision calibration of non-common-path errors would also improve the speckle symmetry and enable the target star to potentially serve as its own calibrator. Indeed, some symmetry is noticeable in the images in Fig. 2. At the time of our observations, the deformable mirror actuator offsets were tuned manually with the first 10 Zernike polynomials by monitoring the PHARO PSF, resulting in a wavefront error of ∼ 110 nm rms. Work is currently underway to reduce the initial intensity of static speckles with robust diversity-based phase retrieval techniques, such as the Gerchberg and Saxton (1972) algorithm (Bikkannavar et al. 2008). Initial results show promise to improve contrast levels by as much as a factor of ≈ (110 nm / 30 nm)^2 = 13 with the current 17x17 element deformable mirror (R. Burruss, private communication).

4.2. Visual Binaries: HIP 48337

We observed HIP 48337 on 11-10-2008 UT as part of a mini-pilot survey to search for low-mass tertiary companions using the linear BLM. Listed as a binary in SIMBAD and NStED, HIP 48337 has a ‘reliably’ well-determined orbit (grade=3/5) from speckle interferometry measurements, having coverage over more than half of a period according to the USNO 6th Catalog of Visual Binary Orbits (Mason et al. 2002). Its components have similar near-infrared magnitudes (Table 1) and were separated by 0.35” at the time of our first epoch observations.

Upon aligning the linear BLM to block each source, we noticed a faint candidate tertiary companion separated by 1.95” from HIP 48337 A. Fig. 4 shows the original discovery image. The candidate is visible in raw data and comparable in brightness to the AO residuals, which are dominated by temporal errors since HIP 48337 is relatively faint for AO locking (combined apparent magnitude of V=7.89) with the well-corrected subaperture. Although well-separated from the two primary stars, this detection demonstrates the

Fig. 2.— Fully processed K_s images of the star ϵ Eridani and a nearby calibrator, δ Eridani, using the BLM. (left) High-pass Fourier filtered image of the target star prior to PSF subtraction. (middle) PSF calibrator constructed from 15 separate images with the LOCI algorithm. The speckle patterns are highly correlated. (right) Differenced image.

Fig. 3.— Contrast levels (5σ) before and after PSF subtraction for the star ϵ Eridani in K_s. The BLM working in concert with the well-corrected subaperture and LOCI algorithm allows for the unambiguous detection of companions ∼ 10^5 times fainter than the star in the primary search region. The standard PSF subtraction and LOCI curves each include the contributions from speckle and photon noise. The distance where the BLM intensity transmission (IT) reaches 0.5 is indicated by a vertical line.

Fig. 4.— Discovery image of the HIP 48337 C candidate companion taken at Palomar on 11-10-2008 UT in K_s. The primary components, HIP 48337 A,B, are spatially resolved, as shown in the unocculted subimage, and simultaneously attenuated by the linear BLM. The locations of HIP 48337 A,B in the occulted image are each denoted by an ‘x’. The BLM axis is marked by a dashed line.

utility of a linear coronagraphic mask. We could have unambiguously identified the candidate in less than 10 minutes at the same position angle for separations as small as 0.9”. If it is gravitationally bound, then HIP 48337 is one of the many nearby triples missing from the MSC (§2.1).

We measured the relative brightness of each HIP 48337 component in the J, H, K bands using standard aperture photometry, taking into account minor contamination from the other components. These numbers were then converted to apparent magnitudes using the seeing-limited (unresolved) 2MASS measurements of the system combined brightness through the equations:

m_A = m_{AB} + 2.5 log(1 + f_B /f_A) (2) m_B = m_{AB} + 2.5 log(1 + f_A/f_B) (3)

where m_A < m_B are the apparent magnitudes of HIP 48337 A, B respectively, m_{AB} is the combined apparent magnitude from 2MASS, and f_A > f_B are the individual component fluxes in arbitrary units. The apparent magnitude of the HIP 48337 C candidate, which was too faint to be detected by 2MASS, was then calculated from f_C . The results are shown in Table 1.

Converting to absolute magnitudes and comparing the results with Girardi et al. (2002) isochrones suggests the A, B, C components have spectral types of A8-F8, F2-G0, and M0- M4 respectively, assuming they lie on the mainsequence. These inferences are limited by the uncertainty in distance to HIP 48337 (d = 133.0 ± 41.9 pcs). We find that results based on colors alone, which are independent of distance, have similar uncertainties (e.g., comparing to Ducati et al. (2001)). More detailed characterization using spatially-resolved spectra and precision astrometry from the Project 1640 instrument (see Zimmerman et al. (2010); Hinkley et al. (2010)) will be reported in a subsequent paper.

HIP 48337 A B C V 8.54 ± 0.01 8.75 ± 0.02 — J 7.44 ± 0.06 7.73 ± 0.07 12.70 ± 0.16 H 7.23 ± 0.06 7.54 ± 0.07 12.15 ± 0.15 K 7.18 ± 0.06 7.51 ± 0.08 11.82 ± 0.16 M_V 2.92 ± 0.83 3.13 ± 0.84 — M_J 1.82 ± 0.88 2.11 ± 0.89 7.08 ± 0.98 M_H 1.61 ± 0.88 1.92 ± 0.89 6.53 ± 0.98 M_K 1.56 ± 0.88 1.89 ± 0.89 6.20 ± 0.98 ρ (mas) — 354 ± 6 1952 ± 13 θ (deg) — 101.6 ± 0.2 86.0 ± 0.2

Table 1: Physical parameters of HIP 48337. Visual magnitudes are from Hipparcos. Absolute magnitudes for the HIP 48337 C candidate are calculated for an assumed distance of 133 pcs. Angular separations and position angles correspond to observations conducted on 03-21-2009 UT.

5. Summary

We have designed and built the first bandlimited mask (BLM) used for ground-based highcontrast imaging observations. The BLM is installed in the PHARO camera at Palomar and is capable of generating 5σ contrast levels of order 10^{−5} at subarcsecond separations in the K_s band when operating in tandem with an extreme AO system and performing PSF reference subtraction. We have demonstrated this technology on the star ϵ Eridani, achieving a mass sensitivity of ≈ 24.0M_J at 0.8” and ≈ 14.7M_J at 4.0”. These observations are the most sensitive in K_s yet reported for the star inside of 5” to date, even though the aperture used is much smaller than in previous studies. Further improvements to calibration of non-common-path errors between the AO system and PHARO will provide even deeper contrast.

We have outlined two science cases that motivate binary star high-contrast imaging. The search for tertiary companions in P-type orbits can significantly improve our understanding of: (i) star formation, by improving the statistics of the Multiple-Star Catalog (Tokovinin 1997, 2004), which is currently incomplete beyond ∼ 10 pcs, and (ii) planet formation, by complementing the efforts of radial velocity teams searching for planets in S-type orbits. We have already detected a candidate M-dwarf tertiary orbiting the visual binary HIP 48337, showing that a linear BLM is a viable tool for exploring this observational parameter space. It is possible to speculate that the companion, if gravitationally bound, may be exciting the eccentricity of HIP 48337 A,B via the Kozai mechanism: their eccentricity is ∼ 0.93 according to the USNO WDS catalog.

We thank Karl Stapelfeldt for support at the JPL microdevices lab to cut and clean the BLM prior to installation and Dimitri Mawet for helpful discussions at the observatory. J. Carson acknowledges support from the NASA postdoctoral program. This work was funded in part by the UCF-UF-SRI program and NASA grant NNG06GC49G.

REFERENCES

Andersen, J., Lindgren, H., Hazen, M. L., and Mayor, M.

(1989) , A&A 219, 142

Artymowicz, P. and Lubow, S. (1994) , ApJ 421, 651

Backer, D. C., Foster, R. S., and Sallmen, S. (1993) , Nature 365, 817

Baraffe, I., Chabrier, G., Barman, T. S., Allard, F., and Hauschildt, P. H. (2003) , A&A 402, 701

Bate, M. R. (2009) , MNRAS 392, 590

Benedict, G. F., McArthur, B. E., Gatewood, G., Nelan, E., Cochran, W. D., Hatzes, A., Endl, M., Wittenmyer, R., Baliunas, S. L., Walker, G. A. H., Yang, S., Kürster, M., Els, S., and Paulson, D. B. (2006) , AJ 132, 2206

Bikkannavar, S., Ohara, C., and Troy, M. (2008) , In Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series, Vol. 7015 of Presented at the Society of Photo-Optical Instrumentation Engineers (SPIE) Conference

Boden, A. F., Akeson, R. L., Sargent, A. I., Carpenter, J. M., Ciardi, D. R., Bary, J. S., and Skrutskie, M. F. (2009) , ApJ 696, L111

Bonavita, M. and Desidera, S. (2007) , A&A 468, 721

Correia, A. C. M., Udry, S., Mayor, M., Laskar, J., Naef, D., Pepe, F., Queloz, D., and Santos, N. C. (2005) , A&A 440, 751

Crepp, J. R., Ge, J., Vanden Heuvel, A. D., Miller, S. P., and Kuchner, M. J. (2006) , ApJ 646, 1252

Crepp, J. R., Vanden Heuvel, A. D., and Ge, J. (2007) , ApJ 661, 1323

Ducati, J. R., Bevilacqua, C. M., Rembold, S. B., and Ribeiro, D. (2001) , ApJ 558, 309

Duchêne, G. (2010) , ApJ 709, L114

Duquennoy, A. and Mayor, M. (1991) , A&A 248, 485

Dutrey, A., Guilloteau, S., and Simon, M. (1994) , A&A 286, 149

Eggenberger, A. (2009) , ArXiv e-prints

Eggenberger, A., Udry, S., Chauvin, G., Beuzit, J., Lagrange, A., Ségransan, D., and Mayor, M. (2007) , A&A 474, 273

Gerchberg, R. and Saxton, W. (1972) , Optik 35, 237

Girardi, L., Bertelli, G., Bressan, A., Chiosi, C., Groenewegen, M. A. T., Marigo, P., Salasnich, B., and Weiss, A. (2002) , A&A 391, 195

Goodwin, S. and Kroupa, P. (2005) , A&A 439, 565

Greaves, J. S., Holland, W. S., Moriarty-Schieven, G., Jenness, T., Dent, W. R. F., Zuckerman, B., McCarthy, C., Webb, R. A., Butner, H. M., Gear, W. K., and Walker, H. J. (1998) , ApJ 506, L133

Guyon, O., Pluzhnik, E. A., Kuchner, M. J., Collins, B., and Ridgway, S. T. (2006) , ApJS 167, 81

Hatzes, A. P., Cochran, W. D., Endl, M., McArthur, B., Paulson, D. B., Walker, G. A. H., Campbell, B., and Yang, S. (2003) , ApJ 599, 1383

Hatzes, A. P., Cochran, W. D., McArthur, B., Baliunas, S. L., Walker, G. A. H., Campbell, B., Irwin, A. W., Yang, S., Kürster, M., Endl, M., Els, S., Butler, R. P., and Marcy, G. W. (2000) , ApJ 544, L145

Hayward, T. L., Brandl, B., Pirger, B., Blacken, C., Gull, G. E., Schoenwald, J., and Houck, J. R. (2001) , PASP 113, 105

Heinze, A. N., Hinz, P. M., Kenworthy, M., Miller, D., and Sivanandam, S. (2008) , ApJ 688, 583

Herbst, W., Hamilton, C. M., Leduc, K., Winn, J. N., Johns-Krull, C. M., Mundt, R., and Ibrahimov, M. (2008) , Nature 452, 194

Hinkley, S., Oppenheimer, B. R., Brenner, D., Zimmerman, N., Roberts, L. C., Parry, I. R., Soummer, R., Sivaramakrishnan, A., Simon, M., Perrin, M. D., King, D. L., Lloyd, J. P., Bouchez, A., Roberts, J. E., Dekany, R., Beichman, C., Hillenbrand, L., Burruss, R., Shao, M., and Vasisht, G. (2010) , ApJ 712, 421

Holman, M. and Wiegert, P. (1999) , AJ 117, 621

Ida, S. and Lin, D. N. C. (2004) , ApJ 616, 567

Ireland, M. J. and Kraus, A. L. (2008) , ApJ 678, L59

Itoh, Y., Oasa, Y., and Fukagawa, M. (2006) , ApJ 652, 1729

Janson, M., Brandner, W., Henning, T., Lenzen, R., McArthur, B., Benedict, G. F., Reffert, S., Nielsen, E., Close, L., Biller, B., Kellner, S., Günther, E., Hatzes, A., Masciadri, E., Geissler, K., and Hartung, M. (2007) , AJ 133, 2442

Janson, M., Reffert, S., Brandner, W., Henning, T., Lenzen, R., and Hippler, S. (2008) , A&A 488, 771

Kennedy, G. and Kenyon, S. (2008) , ApJ 673, 502

Konacki, M., Muterspaugh, M. W., Kulkarni, S. R., and Hełminiak, K. G. (2009) , ApJ 704, 513

Kozai, Y. (1962) , AJ 67, 591

Kraus, A. L. and Hillenbrand, L. A. (2007) , ApJ 662, 413

Krist, J. E., Balasubramanian, K., Beichman, C. A., Echternach, P. M., Green, J. J., Liewer, K. M., Muller, R. E., Serabyn, E., Shaklan, S. B., Trauger, J. T., Wilson, D. W., Horner, S. D., Mao, Y., Somerstein, S. F., Vasudevan, G., Kelly, D. M., and Rieke, M. J. (2009) , In Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series, Vol. 7440 of Presented at the Society of Photo-Optical Instrumentation Engineers (SPIE) Conference

Kuchner, M. J., Crepp, J. R., and Ge, J. (2005) , ApJ 628, 466 Kuchner, M. J. and Spergel, D. N. (2003) , ApJ 594, 617

Kuchner, M. J. and Traub, W. A. (2002) , ApJ 570, 900

Lafrenière, D., Doyon, R., Marois, C., Nadeau, D., Oppenheimer, B. R., Roche, P. F., Rigaut, F., Graham, J. R., Jayawardhana, R., Johnstone, D., Kalas, P. G., Macintosh, B., and Racine, R. (2007) , ApJ 670, 1367

Lee, J. W., Kim, S., Kim, C., Koch, R. H., Lee, C., Kim, H., and Park, J. (2009) , AJ 137, 3181

Levine, M., Lisman, D., Shaklan, S., Kasting, J., Traub, W., Alexander, J., Angel, R., Blaurock, C., Brown, M., Brown, R., Burrows, C., Clampin, M., Cohen, E., Content, D., Dewell, L., Dumont, P., Egerman, R., Ferguson, H., Ford, V., Greene, J., Guyon, O., Hammel, H., Heap, S., Ho, T., Horner, S., Hunyadi, S., Irish, S., Jackson, C., Kasdin, J., Kissil, A., Krim, M., Kuchner, M., Kwack, E., Lillie, C., Lin, D., Liu, A., Marchen, L., Marley, M., Meadows, V., Mosier, G., Mouroulis, P., Noecker, M., Ohl, R., Oppenheimer, B., Pitman, J., Ridgway, S., Sabatke, E., Seager, S., Shao, M., Smith, A., Soummer, R., Stapelfeldt, K., Tenerell, D., Trauger, J., and Vanderbei, R. (2009) , ArXiv e-prints

Macintosh, B. A., Becklin, E. E., Kaisler, D., Konopacky, Q., and Zuckerman, B. (2003) , ApJ 594, 538

Mason, B. D., Hartkopf, W. I., Urban, S. E., Wycoff, G. L., Pascu, D., Hall, D. M., Hennessy, G. S., Platais, I., Rafferty, T. J., and Holdenried, E. R. (2002) , AJ 124, 2254 Mathieu, R. D., Adams, F. C., and Latham, D. W. (1991) , AJ 101, 2184 Mathieu, R. D., Stassun, K., Basri, G., Jensen, E. L. N., Johns-Krull, C. M., Valenti, J. A., and Hartmann, L. W. (1997) , AJ 113, 1841 Mawet, D., Serabyn, E., Stapelfeldt, K., and Crepp, J.

(2009) , ApJ 702, L47 McKee, C. F. and Ostriker, E. C. (2007) , ARA&A 45, 565 Mugrauer, M., Seifahrt, A., and Neuhäuser, R. (2007) , MNRAS 378, 1328 Muterspaugh, M. W., Konacki, M., Lane, B. F., and Pfahl, E. (2007) , ArXiv e-prints Pascucci, I., Apai, D., Hardegree-Ullman, E. E., Kim, J. S., Meyer, M. R., and Bouwman, J. (2008) , ApJ 673, 477 Payne, M. J., Wyatt, M. C., and Thébault, P. (2009) , MNRAS pp. 1550–+ Proffitt, C. R., Sahu, K., Livio, M., Krist, J., Calzetti, D., Gilliland, R., Grady, C., Lindler, D., Woodgate, B., Heap, S., Clampin, M., Gull, T. R., and Lisse, C. M. (2004) , ApJ 612, 481 Serabyn, E., Wallace, K., Troy, M., Mennesson, B., Haguenauer, P., Gappinger, R., and Burruss, R. (2007) , ApJ 658, 1386 Shaklan, S. B. and Green, J. J. (2005) , ApJ 628, 474 Song, I., Caillault, J., Barrado y Navascués, D., Stauffer, J. R., and Randich, S. (2000) , ApJ 533, L41 Tokovinin, A. (2004) , In Revista Mexicana de Astronomia y Astrofisica Conference Series. (C. Allen and C. Scarfe eds.), Vol. 21 of Revista Mexicana de Astronomia y Astrofisica Conference Series, pp. 7–14 Tokovinin, A. (2008) , MNRAS 389, 925 Tokovinin, A. A. (1997) , A&AS 124, 75 Trauger, J. and Traub, W. (2007) , Nature 446, 771 Trilling, D. E., Stansberry, J. A., Stapelfeldt, K. R., Rieke, G. H., Su, K. Y. L., Gray, R. O., Corbally, C. J., Bryden, G., Chen, C. H., Boden, A., and Beichman, C. A. (2007) , ApJ 658, 1289 Troy, M., Dekany, R. G., Brack, G., Oppenheimer, B. R., Bloemhof, E. E., Trinh, T., Dekens, F. G., Shi, F., Hayward, T. L., and Brandl, B. (2000) , In Proc. SPIE Vol. 4007, p. 31-40, Adaptive Optical Systems Technology, Peter L. Wizinowich; Ed.. (P. L. Wizinowich ed.), Vol. 4007 of Presented at the Society of Photo-Optical Instrumentation Engineers (SPIE) Conference, pp. 31–40 Xie, J. and Zhou, J. (2009) , ApJ 698, 2066 Zimmerman, N., Oppenheimer, B. R., Hinkley, S., Brenner, D., Parry, I. R., Sivaramakrishnan, A., Hillenbrand, L., Beichman, C., Crepp, J. R., Vasisht, G., Roberts, L. C., Burruss, R., King, D. L., Soummer, R., Dekany, R., Shao, M., Bouchez, A., Roberts, J. E., and Hunt, S. (2010) , ApJ 709, 733

This 2-column preprint was prepared with the AAS L^ATEX macros v5.2.