arXiv:1807.00155v1 [astro-ph.SR] 30 Jun 2018

Solar Physics DOI: 10.1007/•••••-•••-•••-••••-•

Visibility of Prominences using the He i D_3 Line Filter on PROBA-3/ASPIICS Coronagraph Solar Physics

S. Jejčič^{1,2} · P. Heinzel^2 · N. Labrosse^3 · A. N. Zhukov^{4,5} · A. Bemporad^6 · S. Fineschi^6 · S. Gunár^2 · © Springer •••• Abstract

We determine an optimal width and shape of the narrow-band filter centered around the He i D_3 line for prominence and coronal mass ejection (CME) observations with the ASPIICS (Association of Spacecraft for Polarimetric and Imaging Investigation of the Corona of the Sun) coronagraph onboard the PROBA-3 (Project for On-board Autonomy) satellite, to be launched in 2020. We analyze He i D_3 line intensities for three representative non-LTE prominence models at temperatures 8, 30 and 100 kK computed by the radiative transfer code and the prominence visible-light (VL) emission due to Thomson scattering on the prominence electrons. We compute various useful relations at prominence lineof-sight (LOS) velocities of 0, 100, and 300 km s^{−1} for 20 Å wide flat filter and three Gaussian filters with full width at half maximum (FWHM) equal to 5, 10, and 20 Å to show the relative brightness contribution of the He i D_3 line and the prominence VL to the visibility in a given narrow-band filter. We also discuss possible signal contamination by Na i D_1 and D_2 lines which otherwise may be useful to detect comets. Results mainly show: i) an optimal narrow-band filter should be flat or somewhere between flat and Gaussian with FWHM of 20 Å in order to detect fast moving prominence structures, ii) the maximum emission in the He i D_3 line is at 30 kK and the minimal at 100 kK, and iii) the ratio of

1 University of Ljubljana, Faculty of Mathematics and Physics, Ljubljana, Slovenia email: sonja.jejcic@guest.arnes.si 2 Astronomical Institute of the Czech Academy of Sciences, Ondřejov, Czech Republic email: pheinzel@asu.cas.cz, stanislav.gunar@asu.cas.cz 3 SUPA School of Physics & Astronomy, University of Glasgow, UK email: nicolas.labrosse@glasgow.ac.uk 4 Solar-Terrestrial Centre of Excellence-SIDC, Royal Observatory of Belgium, Brussels, Belgium email: andrei.zhukov@sidc.be 5 Skobeltsyn Institute of Nuclear Physics, Moscow State University, Moscow, Russia 6 INAF-Turin Astrophysical Observatory, Pino Torinese (TO), Italy email: bemporad1@oato.inaf.it, fineschi@oato.inaf.it

Jejčič et al.

emission in the He i D_3 line to the VL emission can provide a useful diagnostic for the temperature of prominence structures. This ratio is up to 10 for hot prominence structures, up to 100 for cool structures and up to 1000 for warm structures.

Keywords: Instrumentation and Data Management; Prominences, Models

1. Introduction

Coronagraphic observations of the Sun from space were so far limited so that only the outer corona was detected. The instruments like Large Angle and Spectrometric Coronagraph (LASCO) or Ultraviolet Coronagraph Spectrometer (UVCS) on board of the Solar and Heliospheric Observatory (SOHO) (Brueckner et al., 1995; Kohl et al., 1995), or COR2 coronagraphs on the twin Solar Terrestrial Relations Observatory (STEREO) satellites (Howard et al., 2008) used external occulters placed in front of the telescopes, which resulted in occultation significantly exceeding the solar disk radius. This was dictated by the amount of stray light. Note that the stray light is high in internally occulted coronagraphs like STEREO/COR1. However, by placing the external occulting disk further from the telescope itself, one can gradually reduce the stray light, reach lower coronal altitudes, and thus study the innermost corona. This kind of experiment is designed for the upcoming mission Project for On-board Autonomy (PROBA-3) of the European Space Agency (ESA). PROBA-3 is a technology-demonstration mission within the ESAs General Support Technology Programme (GSTP), aimed at testing the so-called formation flight of two satellites (with the expected launch in 2020). The two satellites, separated on their orbits by about 150 meters, will carry a large externally occulted coronagraph, where the occulter will be placed on the front satellite oriented towards the Sun and the telescope will be on the rear one. This coronagraph, called ASPIICS (Association of Spacecraft for Polarimetric and Imaging Investigation of the Corona of the Sun) (Lamy et al., 2010; Renotte et al., 2016) will then be precisely oriented in space in order to observe the Sun and such kind of orientation will fulfill part of the formation-flight tests. With this configuration, the inner corona down to 1.08 solar radii (i.e. about 60 Mm above the limb), can be observed with unprecedented quality of imaging. In a sense, this will simulate total solar eclipses, with the advantage of getting extended time series of coronal images which will allow us, for the first time, to study evolution and dynamics of the inner corona on time scales reaching six hours.

One of the science objectives is also observation of eruptive prominences and coronal mass ejections (CMEs) in the field of view (FOV) of ASPIICS, using filter imaging techniques. The filter wheel is still under the design study and it is the main objective of this paper to propose its transmittance properties. We use our previous experience with the He i D_3 line emission in cool prominencelike structures (Labrosse, 2015) and study their expected visibility through the ASPIICS coronagraph. This visibility critically depends on the physical conditions in eruptive prominences and cores of CMEs, as well as on their velocities in the corona, and depends on the transmittance profile of the narrow-band He i

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

D_3 filter. We also discuss a potential contamination of the signal by prominence emission in nearby sodium doublet Na i D_1 and D_2. The point is that if the filter will be wide enough, the latter lines can be well detected in comets passing through the ASPIICS FOV. Images acquired by space-based coronagraphs have proven to be very useful for observations of near-Sun comets and even sun-grazing (Biesecker et al., 2002) and sun-skirting (Lamy et al., 2013) comets. These comets have been observed in the visible-light (VL) even by the STEREO coronagraphs (Thompson, 2009), and a few of them have been observed also in UV spectra (Bemporad et al., 2007) and EUV images (McCauley et al., 2013). All these observations provided lot of information about the origin and evolution of these small bodies in our solar system (Sekanina, 2003).

While this paper is aimed at proposing the narrow-band filter transmittance characteristics for He i D_3 line, in the following paper we will focus on the diagnostic potential of this He i D_3 line, combined with VL, and that will serve for future analysis of the ASPIICS data. In fact, there already exists the broadband data of this kind for structures at higher altitudes. LASCO-C2 coronagraph on SOHO has several broad-band filters, one of them centered around the He i D_3 lines (the so-called orange filter). Several observations of prominence-like structures with this orange filter exist in the literature (Boulade et al., 1997) and the question thus arises whether the image is dominated by the He i D_3 line or by VL integrated through the broad-band filter. The latter is due to Thomson scattering on electrons which are part of the erupting structure (the coronal component subtracted). The optimum parameters of the He i D_3 filter, contamination with sodium D_1 and D_2 lines and comet detection capability with ASPIICS coronagraph are the main objectives of this article.

2. Narrow-Band Filter Observations of Neutral Helium He i D_3 Line

The ASPIICS coronagraph onboard the PROBA-3 satellite will carry a filter wheel with total of six filter slots: broad-band VL filter between 5400 and 5700 Å, three VL polarizers at angles 0, and ± 60^∘, iron Fe xiv green-line narrow-band 5 Å filter and finally one narrow-band filter to detect plasmas in the neutral helium He i D_3 at 5877.25 Å (we use the vacuum wavelength). The design of the He i D_3 narrow-band filter is still in progress.

The narrow-band filter centered around the He i D_3 line contains the radiation contribution from four sources: i) prominence emission in the He i D_3 line mainly due to scattering of the photospheric radiation on prominence helium atoms, ii) VL emission due to Thomson scattering on prominence electrons, iii) VL emission from the surrounding corona along the line-of-sight (LOS) due to Thomson scattering on coronal electrons, and iv) coronal He i D_3 line emission. Here we do not consider iii) because the LOS contribution of the surrounding corona can be subtracted using the nearby pre-eruption coronal observation and iv) which is below the detection limit due to coronal temperatures much higher than the formation temperature of the He i D_3 line.

We focus on three types of Gaussian filters with FWHM equal to 5, 10, and 20 Å, to study the relative brightness contribution of the He i D_3 line and the

Jejčič et al.

prominence VL to the visibility in a given filter. We also take into account the possible contamination with nearby sodium Na i D_1 and D_2 lines at 5897.56 and 5891.58 Å. The advantage of ASPIICS coronagraph on PROBA-3 is to have nearly simultaneous narrow-band He i D_3 line and broad-band VL observations for the whole FOV down to 1.08 R_⊙ with strongly reduced stray light. But since ASPIICS will not provide spectroscopic He i D_3 observation, there will be no information about the prominence LOS velocity. Without such information we can not quantitatively interpret the prominence He i D_3 emission unless the He i D_3 narrow-band filter has flat response function in the wavelength range corresponding to expected Doppler shifts. In the present work we compare the effect of the prominence LOS velocity for three Gaussian filters with different FWHM, against the reference 20 Å wide flat filter.

3. Modeling of the Prominence Emission in He i D_3 Line

Emergent intensities in the He i D_3 line are computed using the non-LTE (i.e. departures from Local Thermodynamic Equilibrium) radiative-transfer code presented in Labrosse and Gouttebroze (2001) for a grid of prominence models. The code solves the pressure-balance and ionisation equilibrium equations, as well as radiative transfer and statistical equilibrium equations for hydrogen in a onedimensional (1D) plane-parallel slab vertically standing above the solar surface. Once these equations are solved, radiative transfer and statistical equilibrium equations are solved for a 34 level helium atom model, with 29 levels for He i, four levels for He ii, and one continuum level for fully ionised helium. This allows us to obtain the emergent intensities as a function of model input parameters. The input parameters are temperature, gas pressure, microturbulent velocity, radial flow velocity, slab thickness, and altitude above the limb. The slab is externally illuminated by the solar disk. For this exploratory study, we focus on isothermal and isobaric prominence slabs at three altitudes above the limb (60 Mm, 800 Mm, and 1600 Mm, roughly corresponding to 1.08 R_⊙, 2.15 R_⊙, and 3 R_⊙) representative of what could be observed with the ASPIICS coronagraph. We computed a total of 90 models with temperatures ranging from 8 kK to 100 kK, thickness of 1000 km and 5000 km, and microturbulent velocities of 5 km s^{−1}, 15 km s^{−1}, and 20 km s^{−1} (i.e. increasing with temperature). These models are static because there is no Doppler Brightening Effect (DBE) in the He i D_3 line (the photospheric spectrum around the He i D_3 line is flat i.e. continuum) and we neglect the velocity effects on the electron density. DBE is discussed in Heinzel and Rompolt (1987). The helium abundance is fixed at 0.1. The non- LTE code provides the total energy emitted in the helium D_3 line E_{D3}, the maximal intensity of the He i D_3 profile I_0, the mean electron density n_e as well as the optical thickness at the line center of the He i D_3 line τ_0(D_3). Note that the radiative transfer codes have been used for the first time to model hot prominence structures inside the CMEs.

Our initial analysis revealed that the He i D_3 line is formed mainly under two different regimes, namely due to scattering of the incident radiation coming from the disk (for models at low temperatures and low pressures), or collisional

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

Table 1. Temperature T , microturbulent velocity ξ, mean electron density n_e, integrated intensity emitted in the He i D_3 line E_{D3}, optical thickness at the line center of the He i D_3 line τ_0(D_3), and optical thickness of VL τ_{VL} for three representative non-LTE models. Models have fixed gas pressure p = 0.1 dyn cm^{−2}, thickness D = 1000 km, and height above the solar surface h = 60 Mm.

model T ξ n_e E_{D3} τ_0(D_3) τ_{VL} (kK) (km s^{−1}) (10^{10} cm^{−3}) (erg s^{−1} cm^{−2} sr^{−1}) (10^{−3} ) (10^{−7})

1 8 5 2.16 657.5 2.40 14.4 2 30 15 1.26 2237.9 3.50 8.4 3 100 20 0.378 8.4 0.01 2.5

excitation (for models with large temperatures or large pressures). This is in line with the analysis of Labrosse and Gouttebroze (2004). In order to determine the optimal filter around the He i D_3 line for the ASPIICS coronagraph, it is sufficient to select only a subset of our grid of 90 models. Therefore, we present detailed results only for three temperature models: 8 kK, 30 kK, and 100 kK. These correspond to three cases of prominence ejecta which can be observed by the ASPIICS coronagraph – cool, warm, or hot prominence material in the corona. Note that the latter one was identified as a prominence flux-rope in the core of the CME emitting in hydrogen Lyman lines and other hotter lines (Heinzel et al., 2016; Jejčič et al., 2017). At 8 kK, the He i D_3 line formation is dominated by scattering of the incident radiation in the He i D_3 line. At the two higher temperatures, collisional processes will dominate. In particular, all models at 30 kK show maximum emission in the He i D_3 line: at temperatures higher than 30 kK, neutral helium starts to be noticeably ionized, and the intensity of the emergent He i D_3 line decreases with temperature. For this study, all other input parameters are fixed to one set values: altitude above the limb of 60 Mm, gas pressure of 0.1 dyn cm^{−2}, slab thickness of 1000 km. The microturbulent velocity is taken to be 5 km s^{−1} at T = 8 kK, 15 km s^{−1} at T = 30 kK, and 20 km s^{−1} at T = 100 kK (see Table 1). A more detailed analysis of the He i D_3 line intensity and how it will be observed in the ASPIICS filter will be presented in a follow-up paper (Labrosse, Jejčič, and Heinzel, 2018).

4. Visible-Light Emission

The integrated VL intensity of a prominence E_{VL} is due to Thomson scattering of the solar incident radiation on free electrons in the prominence plasma and depends on n_e and D

E_{VL} = σ_T W (h, λ_c) I_{tot} n_e D . (1)

VL emission is thus proportional to the column electron density N_e = n_e D. Here σ_T is the Thomson scattering cross section. Note that the optical thickness is τ_{VL} = σ_T n_e D (see Table 1). W (h, λ_c) is the dilution factor which depends on

Jejčič et al.

Table 2. Computed values of VL intensities I_{tot} and integrated VL emissions E_{VL} for different filters and for three representative prominence models.

Filter Flat Gaussian Broad-band FWHM (Å) 20 5 10 20 300

I_{tot} (10^7 erg s^{−1} cm^{−2} sr^{−1}) 6.46 1.72 3.43 6.87 101.44 E_{VL} (#1) (erg s^{−1} cm^{−2} sr^{−1}) 21.76 5.79 11.58 23.15 335.90 E_{VL}(#2) (erg s^{−1} cm^{−2} sr^{−1}) 12.69 3.38 6.75 13.51 195.94 E_{VL}(#3) (erg s^{−1} cm^{−2} sr^{−1}) 3.81 1.01 2.03 4.05 58.78

height above the solar surface and on the central wavelength of the filter due to the limb darkening of incident radiation. Jejčič and Heinzel (2009; see Appendix therein) show the height and wavelength dependence of the dilution factor in the optical range up to the altitude 100 Mm. Note that here we are interested in VL emission around the He i D_3 line and thus the wavelength of the He i D_3 line center is used. I_{tot} (see Table 2) has to be computed in the wavelength range in which the VL is detected

I_{tot} = ∫ I_0(λ) G(λ) dλ . (2)

Here I_0(λ) is the VL continuum photospheric intensity at a given wavelength using the data from Allen (1973) and G(λ) is the Gaussian-shaped filter transmittance around the He i D_3 line with FWHM equal to 5, 10, and 20 Å for narrow-band filters, or uniform transmittance for 300 Å broad-band VL filter between 5400 and 5700 Å and a narrow-band flat filter with the width of 20 Å (see Section 2). For three representative models discussed in Section 3, VL emission is computed using Equation 1 and the results are presented in Table 2 for all studied filters.

ASPIICS coronagraph will detect the mixture of the He i D_3 and VL contributions through the narrow-band filter

E_{tot}(nb) = E_{D3}(nb) + E_{VL}(nb) . (3)

Here we use (nb) for a narrow-band filter to clearly distinguish from the broadband (bb) filter. Since the instrument will make quasi-simultaneous images in the broad-band VL filter, reconstruction of the pure helium image and pure VL image of the prominence can be done. VL emission in the broad-band filter can be written in the same way as in narrow-band one (see Equations 1 and 2). If broad-band and narrow-band intensities are calibrated in absolute units one can get E_{VL}(nb) = E_{VL}(bb)

W (h, λ_{nb}) W (h, λ_{bb}) ∫ I_0(λ) G_{nb}(λ) dλ ∫ I_0(λ) G_{bb}(λ) dλ

= E_{VL}(bb) α , (4)

where α is a known parameter for a given height through the dilusion factors which depend on the filter (for nb we take wavelength of the He i D_3 line and for

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

Figure 1. Transmittance normalized to the peak values as a function of wavelength around the He i D_3 line for all four studied narrow-band filters together with the Doppler shifted He i D_3 profile at LOS velocity 300 km s^{−1}.

bb we take 5550 Å) and filter transmittance shape. Pure He i D_3 contribution in the narrow-band filter can be then written as

E_{D3}(nb) = E_{tot}(nb) − E_{VL}(nb) . (5)

5. Visibility of the He i D_3 Prominence Structures with ASPIICS Coronagraph

Figure 1 shows the effect of the LOS velocity 300 km s^{−1} on the prominence He i D_3 line due to the filter transmission curves at four different narrow-band filters. Narrow-band 20 Å flat filter is marked in brown and three Gaussian filters have the following color coding: blue for 5 Å, green for 10 Å, and red for 20 Å. This color coding is used for all following plots. Note that for the He i D_3 line the Doppler shift of 1 Å corresponds roughly to the LOS velocity 50 km s^{−1}. This plot clearly shows that at large Doppler shifts of the prominence structure only the flat filter will transmit the whole signal of the He i D_3 line while Gaussian filters will reduce signal by a certain factor. At this rather extreme LOS velocity the helium signal would be reduced by about 20 % in case of the 20 Å filter, by about 60 % in case of the 10 Å filter and it is practically completely reduced by the 5 Å filter. This demonstrates that the optimal choice would be the 20 Å flat narrow-band filter. Possible option is a design of the 20 Å narrow-band filter with transmittance between flat and Gaussian shape.

Figure 2a shows the variation of the integrated intensity emitted in the He i D_3 line with temperature for four narrow-band filters and three LOS velocities, for three prominence models shown in Table 1. Note that we choose two representative LOS velocities 100, and 300 km s^{−1} according to our previous experiences with fast moving prominence structures (Heinzel et al., 2016), and we add a zero velocity as the reference for static prominence structures. E_{D3}

Jejčič et al.

Figure 2. a) Integrated intensity emitted in the He i D_3 line as a function of temperature for the studied models shown in Table 1. b) Ratio of the integrated intensity emitted in the He i D_3 line to the VL emission as a function of temperature for the studied models.

is the highest for warm prominence structures at 30 kK and the lowest for hot prominence model at 100 kK where the helium is almost fully ionized. Flat filter is a reference filter which gives the correct energy emitted in the He i D_3 line because the filter transmittance is uniform. By increasing the prominence LOS velocity from 0 up to 300 km s^{−1}, the energy detected in the He i D_3 line is decreasing for narrower Gaussian filters. Difference between flat and Gaussian filter is highest at 5 Å and lowest at 20 Å.

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

Figure 3. Integrated intensity of the He i D_3 line as a function of VL emission for selected models. Model 1 is presented by solid line, model 2 by dotted line and model 3 by dashed line. We show the effect of various filters and the prominence LOS velocities. Straight black solid line shows where E_{D3} = E_{VL}.

Table 3. Ratio of integrated intensity emitted in the He i D_3 line to the prominence VL emission for different prominence LOS velocities and models. Note that for Gaussian filters FWHMs are presented.

Filter Flat 20 Å Gaussian 5 Å Gaussian 10 Å Gaussian 20 Å

v_{LOS} (km s^{−1}) model 1

0 113.57 56.80 28.40 100 30.22 74.22 51.07 27.65 300 2.47 21.81 22.36

v_{LOS} (km s^{−1}) model 2

0 662.66 331.43 165.70 100 176.31 433.04 297.99 161.36 300 14.40 127.26 130.44

v_{LOS} (km s^{−1}) model 3

0 8.29 4.15 2.07 100 2.21 5.42 3.73 2.02 300 0.18 1.59 1.63

Jejčič et al.

By separating the integrated intensity of the He i D_3 line and prominence VL emission using the broad-band filter as described in Section 4, we can reconstruct similar plot as in Figure 2a. Figure 2b shows the ratio of integrated intensity emitted in the He i D_3 line to the prominence VL emission as a function of temperature for representative models. Ratios are presented in Table 3. Because both the He i D_3 and the narrow-band VL emissions are optically thin (see Table 1), their ratio is independent on the prominence thickness meaning that it may provide a useful diagnostic of the temperature. For a given range of prominence LOS velocities and narrow-band filters the ratio of energy emitted in the He i D_3 line to VL emission is between 0.1 and 10 for hot prominence structures, between 1 and 100 for cool structures, and between 10 and 1000 for warm structures. Figure 3 shows the effect of various filters and the prominence LOS velocities on the integrated intensity of the He i D_3 line and the VL emission. The plot clearly shows that for lower LOS velocities 0, and 100 km s^{−1} the contrast of the He i D_3 line with respect to the prominence VL emission is decreasing with the filter width, while for larger LOS velocities 300 km s^{−1} the contrast is inceasing with the filter width (see connecting lines). In order to be able to detect fast moving structures, we must find a compromise between the filter which will compose the broadest range of LOS velocities and the width providing the best detectibility of the He i D_3 emission. In Figure 3 the majority of points lie above the diagonal which indicates a good detectability of the He i D_3 line emission. For the range of prominence LOS velocities up to 300 km s^{−1}, the Gaussian filter with 20 Å FWHM gives the closest values to the flat filter which indicates that a real design of the narrow-band filter centered around the He i D_3 line should be the 20 Å flat filter or somewhere between flat and Gaussian filter with FWHM of 20 Å.

6. Contamination with Na i D_1 and D_2 Lines and Comet Detection Capability of ASPIICS

Sodium doublet Na i D_1 and D_2 at 5897.56 and 5891.58 Å lies close to the He i D_3 line and may contaminate the signal for fast moving prominence structures. If the narrow-band filter will be wide enough, sodium lines can be well detected in comets passing through the ASPIICS FOV, which represents an interesting option for ASPIICS.

The magnitude of comets observed in VL coronagraphs is not only due to photospheric light scattered by dust grains, but also to emission processes by neutrals or singly ionized atoms. In particular, for many comets a distinct neutral sodium tail has been reported (Biesecker et al., 2002). Strong Na i emission at small heliocentric distances have been detected in many comets (e.g. comet Ikeya- Seki, Preston 1967, Slaughter 1969), and a distinct Na i tail was first imaged by Cremonese et al. (1997) at comet Hale-Bopp (C/1995 O1). This emission is very bright thanks to the high efficiency of sodium D transition (see e.g. Cremonese 1999 for a discussion of sodium tail origin). The sodium tail is in addition to the two most common dust and ion tails, and is responsible for significant differences in the apparent comet magnitudes depending on the band-pass filter used for

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

coronagraphic observations, as discussed by Knight et al. (2010). This brightness increase (by about a factor 10) is relatively more important for ”narrow-band” (such as the ”orange” LASCO-C2 and LASCO-C3 filters, 5400 - 6400 Å) with respect to broad-band (such as the ”clear” LASCO-C3 filter, 4000 - 8500 Å) filters, and is most likely due to the sodium D_1 and D_2 lines, even if contributions from other lines by other atoms or ions cannot be excluded. Significant differences have been observed for instance between light curves for the same comet (ISON C/2012 S1) observed with LASCO and STEREO coronagraphs (Knight and Battams, 2014), and these differences are related mostly to the fact that the bandpasses for COR1 (6500 - 6600 Å) and COR2 (6500 - 7500 Å) coronagraphs do not include the sodium lines.

As reported by Biesecker et al. (2002), the majority of sun-grazing comets usually disappear below heliocentric distances of about 7 R_⊙, hence no emission from these comets is expected in the ASPIICS FOV. Nevertheless, recent spectacular observations of near Sun comet (like ISON C/2012 S1) and sungrazing comets (like Lovejoy C/2011 W3) demonstrate that similar objects could fall in the ASPIICS FOV, and even survive at their perihelion transit. In particular, during the transit of comet ISON it was demonstrated for the first time that similar comets can be observed in VL coronagraphs imaging the inner corona even from the ground (Druckmüller et al., 2014). Hence, the inclusion of the D_1 and D_2 lines in the future ASPIICS He i D_3 band-pass filter centered at 5877.25 Å could allow similar observations for future comets. Nevertheless, this would imply broad band-passes up to 28 Å and 40 Å wide to include, respectively, the sodium D_1 and D_2 lines.

Effects due to the cometary orbital motion should be considered as well. The cometary emission from sodium atoms will be in general Doppler shifted, if the comet will have a significant projected velocity along the LOS, that could be in general directed both towards the observer or away from it. The maximum possible speed for these bodies is equal to the free-fall speed that, by assuming for instance an heliocentric distance of perihelion of 1.2 R_⊙, is about 560 km s^{−1}, corresponding to a maximum expected Doppler shift by about 11 Å. The sodium atoms expelled from the comet will undergo radiation pressure acceleration in the anti-sunward direction, hence these atoms will likely move at a speed lower than the cometary orbital speed. In any case, by assuming a He i band-pass filter centered at 5877.25 Å with a full width by 20 Å, the cometary sodium emission at 5891.58 and 5897.56 Å will start to fall in the band-pass only for Doppler blue-shifts larger than 4 Å and 10 Å, corresponding to velocities larger than 200 km s^{−1} and 500 km s^{−1}. In summary, cometary sodium emission will likely fall out of the narrow-band He i D_3 filter, unless much broader band-passes are chosen. This will significantly reduce the detection probability of comets with this filter, because sodium lines will fall in the filter band-pass only for significant Doppler blueshifts, that are possible but quite unlikely. Nevertheless, bright comets will be observed as well by ASPIICS with the VL filters (5400 - 5700 Å), providing nice imaging of the dust tails in the inner corona, and could be even observed in the ”green line” filter, as recently demonstrated by the AIA observations of comet Lovejoy (McCauley et al., 2013). Hence, by considering that the He i D_3 filter is designed primarily to perform scientific observations of

Jejčič et al.

Figure 4. a) Example of measured profiles of the He i D_3 and the Na i D_1 and D_2 lines. Contribution of Na i D_1 and D_2 lines is negligible. b) Contribution of Na i D_1 and D_2 lines is between 10 and 15 % with respect to the He i D_3 line.

Figure 5. a) Distribution of ratio of energy emitted in Na i D_1 line to the He i D_3 line. b) Distribution of ratio of energy emitted in Na i D_2 to the He i D_3 line.

solar prominences, this probable loss of detection capability of comets can be considered as acceptable.

To study the possible contribution of sodium Na i D_1 and D_2 lines in prominences observed by narrow-band He i D_3 filter, we use the spectra obtained in the past on photographic plates at the Ondřejov Observatory. These spectra contain many prominences observed in the He i D_3 and the sodium D_1 and D_2 lines. Photographic densities were converted to relative intensities with standard procedure using the calibration wedge (Valníček et al., 1959). The photospheric scattered light was subtracted. An example where the contribution of sodium D_1 and D_2 lines in prominences is negligible compared to the He i D_3 line is shown in Figure 4a, while Figure 4b shows an example where contribution of sodium D_1 and D_2 lines in the prominence is important.

In total we analyzed 18 prominence spectra from the Ondřejov Observatory. Results are presented as histograms in Figure 5 showing relative brightness contribution of Na i D_1 and Na i D_2 lines versus the He i D_3 line. Histograms show that peak is below 5 %. These are mostly quiescent prominences, in bright quiescent prominences the ratio can go up to 10 %. These results are consistent with the work of Stellmacher and Wiehr (2005) who got similar results for the Na i D_2 line. Only in a few cases ratio between Na i D_1 and He i D_3 or Na i D_2 and He i D_3 can be larger than 20 %. These extreme cases seem to be related with the DBE in the sodium D_1 and D_2 lines. Note that the sodium doublet

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

Table 4. Total energy emitted in Na i D_1 and D_2 lines with respect to energy emitted in the He i D_3 line at upper limit of radial flow velocity 450 km s^{−1} and for various LOS velocities at blueshift and redshift.

FWHM v_{rad} v_{LOS}^{ED2+ED1}_{ED3}^{ED2+ED1}_{ED3}

(Å) (km s^{−1}) (km s^{−1}) Blueshift Redshift

0 0.036 0.036 20 450 100 0.055 0.024 300 0.128 0.010

0 0.095 0.095 30 450 100 0.116 0.078 300 0.172 0.053

Figure 6. a) Contamination of Gaussian 20 Å narrow-band filter with the Na i D_1 and D_2 lines at LOS velocity ± 300 km s^{−1}. He i D_3 line is marked in red, Na i D_1 and D_2 lines in green and blue. Crosses show the position of all three lines at given LOS velocities. R stands for redshift and B for blueshift. b) Contamination of Gaussian 30 Å narrow-band filter with the Na i D_1 and D_2 lines at LOS velocities ± 300 km s^{−1}.

is very sensitive to DBE, because these photospheric absorption lines are very deep and relatively narrow.

It is important to know how much each line contributes to the narrow-band filter signal to see how important are Na i D_1 and D_2 lines compared to the He i D_3 line and how their ratio depends on the width of the filter. For that we made two examples with Gaussian narrow-band filter with FWHM equal to 20 and 30 Å. In Table 4 we computed the relative contribution of Na i D_1 and D_2 lines and the He i D_3 line to the filter signal at an upper limit of the radial flow velocity v_{rad} = 450 km s^{−1} (which takes into account DBE on the sodium D_1 and D_2 lines) for three different prominence LOS velocities 0, 100, and 300 km s^{−1} moving in two directions: toward the observer (blueshift) or away from the observer (redshift) for two filter widths. In the 20 Å filter the contributions of Na i D_1 and D_2 lines and VL are almost negligible, a prominence will be well visible in He i D_3, exception is only an extreme case with about 13 % of Na i D_1 and D_2 contamination. With the 20 Å wide He i D_3 filter ASPIICS can detect comets in Na i D_1 and D_2 lines only if they move with LOS velocity 300 km s^{−1}

Jejčič et al.

or higher toward the observer (see Figure 6a). In the 30 Å Gaussian filter the prominence VL emission gets brigher which would lower He i D_3 line contrast. Note that at 30 Å wide filter VL emissions of models 1, 2 , and 3 are 34.68, 20.23, and 6.07 erg s^{−1} cm^{−2} sr^{−1}. If there is no LOS motion of the prominence, we will automatically get about 10 % of emission from the Na i D_1 and D_2 lines through the filter. At a LOS velocity 300 km s^{−1} (see Figure 6b), we get 17 % of Na i D_1 and D_2 lines at blueshift which is not negligible contribution and 5 % at redshift. In the 30 Å filter the prominence would be more contaminated by Na i D_1 and D_2 lines and prominence VL emission. However, for that filter comets will be better detected while prominences will be more contaminated with the Na i D_1 and D_2 contribution. Our analysis therefore shows that a 20 Å filter will have an optimal detectability of the He i D_3 line in eruptive prominences.

7. Conclusions

In this study we investigated the properties of an optimal narrow-band filter centered around the neutral helium He i D_3 line at 5877.25 Å for eruptive prominence and CME observations down to 1.08 R_⊙ (60 Mm), with the AS- PIICS coronagraph onboard PROBA-3 satellite. We have studied the expected visibility of prominences through various narrow-band filters in the ASPIICS coronagraph. This depends on the filter transmittance profile and on physical conditions in prominences. We took into consideration four narrow-band filters: three Gaussian filters with FWHM equal to 5, 10, and 20 Å and one 20 Å flat filter. A narrow-band He i D_3 filter contains the radiation contribution mainly from the prominence He i D_3 line and prominence VL emission. The modeled prominence He i D_3 line emission was computed by multilevel 1D non-LTE code for helium and the emergent line profiles were multiplied by the narrow-band filter transmittance. The integrated VL emission in prominences was also computed for all four narrow-band filters. We presented several relations between the prominence He i D_3 line emission and the prominence VL emission depending on three typical prominence LOS (Doppler) velocities: 0, 100 and 300 km s^{−1} in a given narrow-band filter. We have selected three representative prominence models with temperatures 8 kK (cool prominence structures), 30 kK (warm structures), and 100 kK (hot structures). These relations show: i) the maximum emission in the He i D_3 line at 30 kK and the minimal at 100 kK, ii) by increasing the prominence LOS velocity, E_{D3} is decreasing when narrowing the Gaussian filter, iii) the contrast of E_{D3} with respect to E_{VL} for lower LOS velocities 0 and 100 km s^{−1} is decreasing with increasing filter width, while at 300 km s^{−1} is increasing, and finally iv) E_{D3}/E_{VL} can provide a useful diagnostic for the temperature of prominence structures. Models show that this ratio (which depends on prominence LOS velocity and filter width) is between 0.1 and 10 for hot prominence structures, between 1 and 100 for cool structures and between 10 and 1000 for warm structures. Note that He i D_3 filter will produce a mixture of He i D_3 line emission and VL emission (at a given wavelength position of the filter transmittance profile), therefore we can reconstruct the pure helium image of the prominence, as well as pure VL image thanks to simoultaneous broad-band

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

VL continuum observations, but without any information about the prominence LOS velocities. We also show possible contamination of the signal with the nearby sodium doublet Na i D_1 and D_2 in 20 and 30 Å Gaussian filters. Our recomendation is to design a narrow-band 20 Å flat filter or a filter somewhere between flat and Gaussian with FWHM of 20 Å. This is mainly dictated by the lack of information about the prominence LOS velocity. However, a 30 Å filter (flat or almost flat) would better suit expected cometary detections in Na i lines. Such filter will more degrade the He i D_3 prominence contrast, but He i D_3 will be still larger or comparable to VL emission. As we have shown, the prominence images in He i D_3 and VL can be separated using the broad-band VL filter data. But 30 Å filter signal will be more contaminated by prominence sodium lines (Figure 6) and this contribution can not be separated. 20 Å filter centered off-band of He i D_3 towards red was also an option, but then the blushifted prominences would be less detectable. A more detailed analysis of the He i D_3 line, its diagnostics and how it will be observed with the ASPIICS filter, will be presented in the next paper (Labrosse, Jejčič, and Heinzel, 2018).

Acknowledgements SJ acknowledges the financial support from the Slovenian Research Agency No. P1-0188. SJ, PH and SG acknowledge support from the Czech Funding Agency through the grant No. 16-18495S and from the AIAS through RVO-67985815. NL acknowledges support from STFC grant ST/L000741/1. NL, PH and SG also acknowledge support by the International Space Science Institute (ISSI), and namely through the Team of NL dealing with solar prominences. ANZ acknowledges support from the Belgian Federal Science Policy Office through the ESA-PRODEX programme (grant No. 4000117262). SG and PH acknowledge the support from grant 16-17586S of the Czech Science Fundation. Ondřejov archive spectra were digitized by Alicja Heinzel.

References

Allen, C.W.: 1973, Astrophysical Quantities, Athlone Press, London,172. Bemporad, A., Poletto, G., Raymond, J., Giordano, S.: 2007, A review of SOHO/UVCS observations of sungrazing comets. Planss 55, 1021 – 1030. doi:10.1016/j.pss.2006.11.013.

Biesecker, D.A., Lamy, P., St. Cyr, O.C., Llebaria, A., Howard, R.A.: 2002, Sungrazing Comets Discovered with the SOHO/LASCO Coronagraphs 1996-1998. Icarus 157, 323 – 348. doi:10.1006/icar.2002.6827.

Boulade, S., Delannée, C., Koutchmy, S., Lamy, P., Llebaria, A., Howard, R., Schwenn, R., Simnett, G.: 1997, Analysis of a High Latitude Slow CME with Travelling Ejecta. In: Wilson, A. (ed.) Fifth SOHO Workshop: The Corona and Solar Wind Near Minimum Activity, ESA Special Publication 404, 217.

Brueckner, G.E., Howard, R.A., Koomen, M.J., Korendyke, C.M., Michels, D.J., Moses, J.D., Socker, D.G., Dere, K.P., Lamy, P.L., Llebaria, A., Bout, M.V., Schwenn, R., Simnett, G.M., Bedford, D.K., Eyles, C.J.: 1995, The Large Angle Spectroscopic Coronagraph (LASCO). Solar Phys. 162, 357 – 402. doi:10.1007/BF00733434.

Cremonese, G.: 1999, Hale-Bopp and Its Sodium Tails. Space Sci. Rev. 90, 83 – 89.

doi:10.1023/A:1005281611036.

Cremonese, G., Boehnhardt, H., Crovisier, J., Rauer, H., Fitzsimmons, A., Fulle, M., Licandro, J., Pollacco, D., Tozzi, G.P., West, R.M.: 1997, Neutral Sodium from Comet Hale-Bopp: A Third Type of Tail. Astrophys. J. Lett. 490, L199 – L202. doi:10.1086/311040.

Jejčič et al.

Druckmüller, M., Habbal, S.R., Aniol, P., Ding, A., Morgan, H.: 2014, Imaging Comet ISON C/2012 S1 in the Inner Corona at Perihelion. Astrophys. J. Lett. 784, L22. doi:10.1088/2041-8205/784/2/L22.

Heinzel, P., Rompolt, B.: 1987, Hydrogen emission from moving solar prominences. Solar Phys.

110, 171 – 189. doi:10.1007/BF00148210.

Heinzel, P., Susino, R., Jejčič, S., Bemporad, A., Anzer, U.: 2016, Hot prominence detected in the core of a coronal mass ejection: Analysis of SOHO/UVCS Lα and SOHO/LASCO visible-light observations. Astron. Astrophys. 589, A128. doi:10.1051/0004-6361/201527421.

Howard, R.A., Moses, J.D., Vourlidas, A., Newmark, J.S., Socker, D.G., Plunkett, S.P., Korendyke, C.M., Cook, J.W., Hurley, A., Davila, J.M., Thompson, W.T., St Cyr, O.C., Mentzell, E., Mehalick, K., Lemen, J.R., Wuelser, J.P., Duncan, D.W., Tarbell, T.D., Wolfson, C.J., Moore, A., Harrison, R.A., Waltham, N.R., Lang, J., Davis, C.J., Eyles, C.J., Mapson-Menard, H., Simnett, G.M., Halain, J.P., Defise, J.M., Mazy, E., Rochus, P., Mercier, R., Ravet, M.F., Delmotte, F., Auchere, F., Delaboudiniere, J.P., Bothmer, V., Deutsch, W., Wang, D., Rich, N., Cooper, S., Stephens, V., Maahs, G., Baugh, R., Mc- Mullin, D., Carter, T.: 2008, Sun Earth Connection Coronal and Heliospheric Investigation (SECCHI). Space Sci. Rev. 136, 67 – 115. doi:10.1007/s11214-008-9341-4.

Jejčič, S., Heinzel, P.: 2009, Electron Densities in Quiescent Prominences Derived from Eclipse Observations. Solar Phys. 254, 89 – 100. doi:10.1007/s11207-008-9289-2.

Jejčič, S., Susino, R., Heinzel, P., Dzifčáková, E., Bemporad, A., Anzer, U.: 2017, Hot prominence detected in the core of a coronal mass ejection: II. Analysis of Ciii line detected by SOHO/UVCS. Astron. Astrophys., submitted.

Knight, M.M., Battams, K.: 2014, Preliminary Analysis of SOHO/STEREO Observations of Sungrazing Comet ISON (C/2012 S1) around Perihelion. Astrophys. J. Lett. 782, L37. doi:10.1088/2041-8205/782/2/L37.

Knight, M.M., A’Hearn, M.F., Biesecker, D.A., Faury, G., Hamilton, D.P., Lamy, P., Llebaria, A.: 2010, Photometric Study of the Kreutz Comets Observed by SOHO from 1996 to 2005. Astron. J. 139, 926 – 949. doi:10.1088/0004-6256/139/3/926.

Kohl, J.L., Esser, R., Gardner, L.D., Habbal, S., Daigneau, P.S., Dennis, E.F., Nystrom, G.U., Panasyuk, A., Raymond, J.C., Smith, P.L., Strachan, L., van Ballegooijen, A.A., Noci, G., Fineschi, S., Romoli, M., Ciaravella, A., Modigliani, A., Huber, M.C.E., Antonucci, E., Benna, C., Giordano, S., Tondello, G., Nicolosi, P., Naletto, G., Pernechele, C., Spadaro, D., Poletto, G., Livi, S., von der Lühe, O., Geiss, J., Timothy, J.G., Gloeckler, G., Allegra, A., Basile, G., Brusa, R., Wood, B., Siegmund, O.H.W., Fowler, W., Fisher, R., Jhabvala, M.: 1995, The Ultraviolet Coronagraph Spectrometer for the Solar and Heliospheric Observatory. Solar Phys. 162, 313 – 356. doi:10.1007/BF00733433.

Labrosse, N.: 2015, Derivation of the Major Properties of Prominences Using NLTE Modelling.

In: Vial, J.-C., Engvold, O. (eds.) Solar Prominences, Astrophysics and Space Science Library 415, 131. doi:10.1007/978-3-319-10416-4 6.

Labrosse, N., Gouttebroze, P.: 2001, Formation of helium spectrum in solar quiescent prominences. Astron. Astrophys. 380, 323 – 340. doi:10.1051/0004-6361:20011395.

Labrosse, N., Gouttebroze, P.: 2004, Non-LTE Radiative Transfer in Model Prominences. I. Integrated Intensities of He I Triplet Lines. Astrophys. J. 617, 614 – 622. doi:10.1086/425168.

Labrosse, N., Jejčič, S., Heinzel, P.: 2018, Prominence diagnostics with ASPIICS. in prep.. Lamy, P., Damé, L., Vivès, S., Zhukov, A.: 2010, ASPIICS: a giant coronagraph for the ESA/PROBA-3 Formation Flying Mission. In: Space Telescopes and Instrumentation 2010: Optical, Infrared, and Millimeter Wave, Procspie 7731, 773118. doi:10.1117/12.858247.

Lamy, P., Faury, G., Llebaria, A., Knight, M.M., A’Hearn, M.F., Battams, K.: 2013, Sunskirting comets discovered with the LASCO coronagraphs over the decade 1996-2008. Icarus 226, 1350 – 1398. doi:10.1016/j.icarus.2013.07.035.

McCauley, P.I., Saar, S.H., Raymond, J.C., Ko, Y.-K., Saint-Hilaire, P.: 2013, Extremeultraviolet and X-Ray Observations of Comet Lovejoy (C/2011 W3) in the Lower Corona. Astrophys. J. 768, 161. doi:10.1088/0004-637X/768/2/161.

Preston, G.W.: 1967, The spectrum of Ikkeya-Seki (1965f). Astrophys. J. 147, 718 – 742.

doi:10.1086/149049.

Renotte, E., Buckley, S., Cernica, I., Denis, F., Desselle, R., De Vos, L., Fineschi, S., Fleury- Frenette, K., Galano, D., Galy, C., Gillis, J.-M., Graas, E., Graczyk, R., Horodyska, P., Kranitis, N., Kurowski, M., Ladno, M., Liebecq, S., Loreggia, D., Mechmech, I., Melich,

Narrow-Band He i D_3 Line Filter on ASPIICS Coronagraph

R., Mollet, D., Mosdorf, M., Mroczkowski, M., O’Neill, K., Patočka, K., Paschalis, A., Peresty, R., Radzik, B., Rataj, M., Salvador, L., Servaye, J.-S., Stockman, Y., Thizy, C., Walczak, T., Zarzycka, A., Zhukov, A.: 2016, Recent achievements on ASPIICS, an externally occulted coronagraph for PROBA-3. In: Space Telescopes and Instrumentation 2016: Optical, Infrared, and Millimeter Wave, Procspie 9904, 99043D. doi:10.1117/12.2232695.

Sekanina, Z.: 2003, Erosion Model for the Sungrazing Comets Observed with the Solar and Heliospheric Observatory. Astrophys. J. 597, 1237 – 1265. doi:10.1086/378192.

Slaughter, C.D.: 1969, The Emission Spectrum of Comet Ikeya-Seki 1965-f at Perihelion Passage. Astron. J. 74, 929. doi:10.1086/110884.

Stellmacher, G., Wiehr, E.: 2005, Solar prominences with Na and Mg emissions and centrally reversed Balmer lines. Astron. Astrophys. 431, 1069 – 1073. doi:10.1051/0004-6361:20041550.

Thompson, W.T.: 2009, 3D triangulation of a Sun-grazing comet. Icarus 200, 351 – 357.

doi:10.1016/j.icarus.2008.12.011.

Valníček, B., Letfus, V., Blaha, M., Švestka, Z., Seidl, Z.: 1959, The flare spectrograph at Ondřejov. Bulletin of the Astronomical Institutes of Czechoslovakia 10, 149.

SOLA: d3fpb.tex; 6 May 2019; 5:19; p. 18