arXiv:2010.06990v1 [physics.optics] 22 Sep 2020

A novel idea: calculating anisotropic turbulence only by Kolmogorov structure constant C^2_n and power law α

Chao Zhai^∗

School of Computer and Communication Engineering, Northeastern University at Qinhuangdao, Qinhuangdao 066004, China

Abstract As stated in the present research, the anisotropic non-Kolmogorov turbulence model is more in line with the actual turbulence. However, anisotropic factor is vital for the accuracy of calculations, and measuring it precisely is a challenging task. In this paper, utilizing three modeling approaches, we derive four different equivalence formulas between the anisotropic non-Kolmogorov and the Kolmogorov structure constants, and apply them to the extant anisotropic results. It is found that the anisotropic factor is eliminated and the anisotropic turbulence can be predicted only by Kolmogorov structure constant and power law.

Keywords: Atmospheric optics, Atmospheric propagation, Anisotropic non-Kolmogorov turbulence, Equivalence.

1. Introduction

It is widely recognized that atmospheric turbulence severely degrades the performance of laser absorption spectroscopy, laser imaging, and free-space optical communications [1, 2, 3, 4]. In the past few decades, the Kolmogorov turbulence model was extensively utilized in the study of light waves transmission in turbulent atmosphere [5, 6]. However, recently due to the progress of measurement methods, both the experimental data and the theoretical results

∗Corresponding author.

Email address: zhaichao@qhd.neu.edu.cn (Chao Zhai)

Preprint submitted to Results in Physics October 15, 2020

have exhibited that the anisotropic non-Kolmogorov turbulence model can better characterize the eddy impacts on light waves transmission in turbulent media [7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18]. For the anisotropic non-Kolmogorov turbulence model, the structure constant is a function of the anisotropic factor and the spectral power law, which reduces to the Kolmogorov structure constant when the anisotropic factor becomes 1 and the spectral power law becomes 11/3 [19]. Then the need to measure three physical quantities, namely the anisotropic non-Kolmogorov structure constant, the anisotropic factor and the spectral power law, is induced when building a model to predict anisotropic turbulence. Considering that the accurate measurement of anisotropic factor is currently a challenging task, and compared to the Kolmogorov structure constant which can be easily obtained by scintillometer, the anisotropic non-Kolmogorov structure constant is still difficult to obtain precisely, we need to find a novel method to predict anisotropic turbulence. Li et al. developed the equivalence formula between the non-Kolmogorov and the Kolmogorov structure constants, and then verified it through experimental data, which provided a method for predicting the non-Kolmogorov structure constant by utilizing the Kolmogorov structure constant [20]. In this paper, by establishing four different equivalence formulas between the anisotropic non-Kolmogorov and the Kolmogorov structure constants, and applying them to the extant anisotropic results, we demonstrate the possibility of using only Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence. And it is anticipated that this work will contribute to the comprehension of light waves transmission in the anisotropic non-Kolmogorov link and the engineering application of the anisotropic theoretical models.

2. Formulation

As is well-known, the power spectrum model of anisotropic non-Kolmogorov turbulence which considers the uneven distribution of the vertical and the horizontal atmosphere has the following expression [14]

Φ_n (κ, α, μ) = A (α) C^2_n (α, μ) μ^{2−α}κ^{−α}, 3 < α < 4, (1)

where κ is the spatial wavenumber vector, α is the spectral power law, μ is the anisotropic factor that is utilized to characterize the uneven distribution of turbulence cells, C^2_n (α, μ) is the anisotropic non-Kolmogorov structure constant that has units of m^{3−α}, A (α) = Γ (α − 1) cos (απ/2) /4π^2, and Γ (x) denotes the Gamma function. At α = 11/3 and μ = 1, Eq. (1) reduce to the conventional Kolmogorov spectrum, which has the following expression

Φ_n (κ) = 0.033C^2_nκ^{−11/3}, 1/L_0 ≪ κ ≪ 1/l_0, (2)

where C^2_n is the Kolmogorov structure constant that has units of m^{−2/3}, L_0 and l_0 are the outer and the inner scales. In addition, for the limiting case C^2_n (11/3, 1) = C^2_n, the Kolmogorov structure constant can be obtained.

For purpose of developing the relationship between the anisotropic non- Kolmogorov and the Kolmogorov structure constants, it is necessary to start with a definition. In Baykal’s paper [21], the scintillation index of spherical wave is chosen as the basis, so we can define that the equivalent structure constants for the anisotropic non-Kolmogorov spectra are the ones that lead to the same scintillation index of spherical wave. In terms of this definition, the expression relating C^2_n (α, μ) to C^2_n (11/3, 1) = C^2_n is proposed.

In Ref. [19], the scintillation index of Gaussian-beam wave for anisotropic non-Kolmogorov turbulence is obtained by Eq. (26). By setting the receiver beam parameters Θ = Λ = 0 and anisotropic factors μ_x = μ_y = μ, the scintillation index of spherical wave for anisotropic non-Kolmogorov turbulence can be expressed as

u^2 (α, μ) = −^2_α cos (_{απ} 2 ) sin (_{απ} 4 ) μ^{2−α}C^2_n (α, μ) k^{3− α2} L^{α2} ×^{Γ(α−1)Γ}(^{1− α2} )^Γ(^{1+ α2} )^Γ(^{α2} ) Γ(α) . (3)

Here, L is the propagation distance, k = 2π/λ, λ is the wavelength.

For Kolmogorov turbulence, the scintillation index of spherical wave has the following expression [6]

u^2 (11/3) = 0.5C^2_nk^{7/6}L^{11/6}. (4)

By equating Eqs. (3) and (4), the relation between the anisotropic non- Kolmogorov structure constant C^2_n (α, μ) and the Kolmogorov structure constant C^2_n can be obtained,

C^2_n (α, μ) = H (α, μ) C^2_n, (5)

where H (α, μ) = −0.25Γ (α + 1) k^{α2 − 116} L^{116 − α2} μ^{α−2} Γ (α − 1) Γ ( 1 −^α_2 ) Γ ( 1 +^α_2 ) Γ (_α 2 ) cos (_{απ} 2 ) sin (_{απ} 4 ) . (6)

In addition, when μ = 1, Eq. (5) matches the non-Kolmogorov result obtained by Baykal and Gerekciolu perfectly [21].

Applying the equivalence formula (5) to the generalized Rytov variance given by Andrews [19] and the anisotropic non-Kolmogorov turbulence model Eq. (1) respectively, we can obtain the following formulas

σ^2_R (α) =

0.5Γ (α + 1) Γ ( 1 +^α_2 ) Γ (_α 2 ) α C^2_nk^{76} L^{116} , (7)

Φ_n (κ, α) =

−Γ (α + 1) k^{α2 − 116} L^{116 − α2} C^2_nκ^{−α} Γ ( 1 −^α_2 ) Γ ( 1 +^α_2 ) Γ (_α 2 ) sin (_{απ} 4 ) 16π^2

. (8)

From Eqs. (7) and (8), we can find that the anisotropic factor μ has been eliminated and the anisotropic non-Kolmogorov structure constant C^2_n (α, μ) has been replaced by the Kolmogorov structure constant C^2_n, so the feasibility of using Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence is established.

In Zilberman’s paper [22], the turbulent power spectrum is chosen as the basis, and they believe that there is a specific wavenumber κ_n to make the power spectrum for the anisotropic non-Kolmogorov and the Kolmogorov turbulence equal. Based on this assumption, we can obtain the following formula

A (α) C^2_n (α, μ) μ^{2−α}κ^{−α}_n = A (11/3) C^2_nκ^{−11/3}_n , (9) where A (11/3) = 0.033. Considering that κ_n can be chosen as κ_n ≈ (k/L)^{1/2} [22], thus the relation between the anisotropic non-Kolmogorov structure constant C^2_n (α, μ) and the Kolmogorov structure constant C^2_n is given by

C^2_n (α, μ) =

A (11/3) A (α) μ^{α−2}C^2_n (√ k/L )_{α−} 11_3

. (10)

In addition, when μ = 1, Eq. (10) matches the non-Kolmogorov result obtained by Zilberman perfectly [22].

Applying the equivalence formula (10) to the temporal power spectrum of irradiance fluctuations for a plane wave transmission in weak anisotropic turbulence [23] and the anisotropic non-Kolmogorov turbulence model Eq. (1) respectively, we can obtain the following formulas W_{I(pl)} (ω, α) =^{16π2 A(11/3)C2nk} 7 6 L^{11}6 ω_0 (_ω ω_0

)_{1−α Γ}(_{12} )_Γ(_{α2 − 12} ) Γ(^α_2 ) ×Re { 1 −_2F_2 ( 1,^{2−α}_2 ;^3_2 ,^{3−α}_2 ; i^{ω2}_{2ω20} ) −^Γ(^{α2} )^Γ(^{12 − α2} )^Γ(^{12 + α2} ) Γ(^α_2 −^1_2 )Γ(^3_2 +^α_2 ) × ( −i^{ω2}_{2ω20} ) α−1_2 1F_1

(_1 2 ;^{α+3}_2 ; i^{ω2}_{2ω20} )} , (11)

Φ_n (κ, α) = A (11/3) C^2_n (√ k/L )_{α−} 11_3 κ^{−α}. (12) From Eqs. (11) and (12), we can find that the anisotropic factor μ has been eliminated and the anisotropic non-Kolmogorov structure constant C^2_n (α, μ) has been replaced by the Kolmogorov structure constant C^2_n, so the feasibility of using Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence is established.

In Li’s paper [20], the structure function of refractive-index fluctuations is chosen as the basis, and they believe that the structure function of refractiveindex fluctuations for the non-Kolmogorov and the Kolmogorov turbulence become equal when the separation distance r = L_0. However, the anisotropy and the variation of power law will change the distribution of refractive-index in the atmosphere, which in turn affects the value of structure function. Therefore, we choose the turbulent power spectrum instead of the structure function of refractive-index fluctuations as the basis and define that when the separation distance r = L_0, the power spectrum for the anisotropic non-Kolmogorov and the Kolmogorov turbulence become equal. Then the following formula can be obtained, A (α) C^2_n (α, μ) μ^{2−α}L^α_0 = A (11/3) C^2_nL^{11/3}_0 , (13) where the spatial wavenumber vector κ = 1/r. Accordingly, the relation between the anisotropic non-Kolmogorov structure constant C^2_n (α, μ) and the Kolmogorov structure constant C^2_n can be expressed as

C^2_n (α, μ) =

A (11/3) A (α) C^2_nμ^{α−2}L^{11/3−α} 0 . (14)

Applying the equivalence formula (14) to the temporal power spectrum of irradiance fluctuations for a plane wave transmission in weak anisotropic turbulence [23] and the anisotropic non-Kolmogorov turbulence model Eq. (1) respectively, we can obtain the following formulas W_{I(pl)} (ω, α) =^{16π2A(11/3)C2nk3−} α 2 L^α2 L^{11/3−α} 0 ω_0 (_ω ω_0

)_{1−α Γ}(_{12} )_Γ(_{α2 − 12} ) Γ(^α_2 ) ×Re { 1 −_2F_2 ( 1,^{2−α}_2 ;^3_2 ,^{3−α}_2 ; i^{ω2}_{2ω20} ) −^Γ(^{α2} )^Γ(^{12 − α2} )^Γ(^{12 + α2} ) Γ(^α_2 −^1_2 )Γ(^3_2 +^α_2 ) × ( −i^{ω2}_{2ω20} ) α−1_2 1F_1

(_1 2 ;^{α+3}_2 ; i^{ω2}_{2ω20} )} , (15)

Φ_n (κ, α) = A (11/3) C^2_nL^{11/3−α}_0 κ^{−α}. (16) From Eqs. (15) and (16), we can find that the anisotropic factor μ has been eliminated and the anisotropic non-Kolmogorov structure constant C^2_n (α, μ) has been replaced by the Kolmogorov structure constant C^2_n, so the feasibility of using Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence is established.

In order to better describe the anisotropic turbulence, Andrews et al. proposed a new power spectrum model, which has two anisotropic factors to parameterize the asymmetry of turbulence eddies in the orthogonal xy-plane. And it has the following expression [19]

Φ_n (κ, α, μ_x, μ_y) =

A (α) C^2_n (α, μ_x, μ_y) μ_xμ_y ( μ^2_xκ^2_x + μ^2_yκ^2_y

)_{α/2} , 3 < α < 4, (17) where κ_x and κ_y are the x and y components of the spatial wavenumber vector κ, C^2_n (α, μ_x, μ_y) is the anisotropic non-Kolmogorov structure constant that has units of m^{3−α}, μ_x and μ_y are the anisotropic factors. If we assume that symmetric distribution of turbulence cells in the plane orthogonal to the direction of propagation z, i.e., the particular case μ_x = μ_y = μ, the spectrum model can be reduced to Eq. (1).

In Ref. [19], the scintillation index of Gaussian-beam wave for anisotropic non-Kolmogorov turbulence is obtained by Eq. (26). By setting the receiver beam parameters Θ = Λ = 0, the scintillation index of spherical wave for anisotropic non-Kolmogorov turbulence can be expressed as

u^2 (α, μ_x, μ_y) = −^1_{απ} cos (_{απ} 2 ) sin (_{απ} 4 ) C^2_n (α, μ_x, μ_y) k^{3− α2} L^{α2} ×^{Γ(α−1)Γ}(^{1− α2} )^Γ(^{1+ α2} )^Γ(^{α2} )

Γ(α) ∫_{2π} 0 (_{cos2 θ}

μ^2_x + sin^2 θ μ^2_y ) α_{2 −1} dθ. (18)

According to the previous idea, by choosing the scintillation index of spherical wave as the basis and equating Eqs. (18) and (4), we can obtain the relation between the anisotropic non-Kolmogorov structure constant C^2_n (α, μ_x, μ_y) and the Kolmogorov structure constant C^2_n,

C^2_n (α, μ_x, μ_y) = M (α) G (α, μ_x, μ_y) C^2_n, (19)

where M (α) = 0.5Γ (α + 1) πk^{α2 − 116} L^{116 − α2} , (20)

G (α, μ_x, μ_y) = −Γ (α − 1) Γ ( 1 −^α_2 ) Γ ( 1 +^α_2 ) Γ (_α 2 ) × cos (_{απ} 2 ) sin (_{απ} 4 ) ∫_{2π} 0 (_{cos2 θ}

μ^2_x + sin^2 θ μ^2_y ) α_{2 −1} dθ. (21)

In addition, when μ_x = μ_y = μ, Eq. (19) can be reduced to Eq. (5).

Applying the equivalence formula (19) to the generalized Rytov variance given by Andrews [19] and the temporal power spectrum of AOA fluctuations for a plane wave transmission in weak anisotropic turbulence by Cui [24] respectively, we can obtain the following formulas

σ^2_R (α) =

0.5Γ (α + 1) Γ ( 1 +^α_2 ) Γ (_α 2 ) α C^2_nk^{76} L^{116} , (22)

W_{θ(pl)} (ω, α) =^{0.25Γ(α+1)k} α 4 − 13 12 L^{2512 − α4}

−Γ(1−^α_2 )Γ(1+^α_2 )Γ(^α_2 ) sin(^{απ}_4 ) C^{2n} 1 ω_0 Γ

(_1 2 ) (_ω ω_0

) 1−α_2 (_{c2D2} 4 ) α−5_4 exp ( −^{c2D2kω2} 8Lω^2_0 ) × { [1 − cos (2β)] W 3−α_{4 ,} 3−α_4 [(_{c2D2} 4 )_{kω2} Lω^2_0 ] + 2^ω_{ω0} cos (2β) (_k L ) 1_2 × (_{c2D2} 4 ) 1_2

W 1−α_{4 ,} 1−α_4 [(_{c2 D2} 4 )_{kω2} Lω^2_0 ]} . (23)

From Eqs. (22) and (23), we can find that the anisotropic factors μ_x and μ_y have been eliminated and the anisotropic non-Kolmogorov structure constant C^2_n (α, μ_x, μ_y) has been replaced by the Kolmogorov structure constant C^2_n, so the feasibility of using Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence is established.

In fact, Beason also gives the relationship between the anisotropic non- Kolmogorov structure constant C^2_n (α, μ_x, μ_y) and the Kolmogorov structure constant C^2_n [25]. Then applying it to the generalized Rytov variance and the temporal power spectrum of AOA fluctuations for plane wave, we can also find the elimination phenomenon, so our conclusion is confirmed. In addition, although the form differs greatly, the calculation result of Eq. (19) is consistent with Beason’s paper.

3. Conclusion

Based on three modeling approaches, four different equivalence formulas between the anisotropic non-Kolmogorov and the Kolmogorov structure constants are derived in this paper. And applying them to the extant anisotropic results, the anisotropic factor is eliminated and the possibility of using only Kolmogorov structure constant C^2_n and power law α to predict anisotropic turbulence is established. It should be noted that this work will contribute to the comprehension of light waves transmission in the anisotropic non-Kolmogorov link and the engineering application of the anisotropic theoretical models.

4. Disclosures

The authors declare no conflicts of interest.

5. Acknowledgments

This work was supported by the National Natural Science Foundation of China under Grant 61901097.

References

[1] J. C. Ricklin, S. M. Hammel, F. D. Eaton, S. L. Lachinova, Atmospheric channel effects on free-space laser communication, J. Opt. Fiber. Commun. Rep. 3 (2) (2006) 111–158.

[2] K. Kazaura, K. Omae, T. Suzuki, M. Matsumoto, E. Mutafungwa, T. O.

Korhonen, T. Murakami, K. Takahashi, H. Matsumoto, K. Wakamori, Y. Arimoto, Enhancing performance of next generation FSO communication systems using soft computing-based predictions, Opt. Exp. 14 (12) (2006) 4958–4968.

[3] X. Guo, F. Zheng, C. Li, X. Yang, N. Li, S. Liu, J. Wei, X. Qiu, Q. He, A portable sensor for in-situ measurement of ammonia based on near-infrared laser absorption spectroscopy, Opt Lasers Eng 115 (2019) 243–248.

[4] C. Li, L. Shao, H. Meng, J. Wei, X. Qiu, Q. He, W. Ma, L. Deng, Y. Chen, High-speed multi-pass tunable diode laser absorption spectrometer based on frequency-modulation spectroscopy, Opt. Exp. 26 (22) (2018) 29330– 29339.

[5] V. I. Tatarskii, Wave Propagation in a Turbulent Medium, McGraw-Hill Press, 1961.

[6] L. C. Andrews, R. L. Phillips, Laser Beam Propagation through Random Media, SPIE Optical Engineering Press, 2005.

[7] R. Manning, An anisotropic turbulence model for wave propagation near the surface of the Earth, IEEE Trans. Antenna Propag. 34 (2) (1986) 258– 261.

[8] A. I. Kon, Qualitative theory of amplitude and phase fluctuations in a medium with anisotropic turbulent irregularities, Waves in Random Media 4 (3) (1994) 297–306.

[9] M. S. Belen’kii, J. D. Barchers, S. J. Karis, C. L. Osmon, J. M. Brown, R. Q.

Fugate, Preliminary experimental evidence of anisotropy of turbulence and the effect of non-Kolmogorov turbulence on wavefront tilt statistics, Proc. SPIE 3762 (1999) 396–406.

[10] L. Biferale, I. Procaccia, Anisotropy in turbulent flows and in turbulent transport, Phys. Rep. 414 (2005) 43–164.

[11] C. Robert, J. M. Conan, V. Michau, J. B. Renard, C. Robert, F. Dalaudier, Retrieving parameters of the anisotropic refractive index fluctuations spectrum in the stratosphere from balloon-borne observations of stellar scintillation, J. Opt. Soc. Am. A 25 (2) (2008) 379–393.

[12] I. Toselli, B. Agrawal, S. Restaino, Light propagation through anisotropic turbulence, J. Opt. Soc. Am. A 28 (3) (2011) 483–488.

[13] L. C. Andrews, R. L. Phillips, R. Crabbs, T. Leclerc, Deep turbulence propagation of a Gaussian-beam wave in anisotropic non-Kolmogorov turbulence, Proc. SPIE 8874 (2013) 887402.

[14] L. Cui, Analysis of angle of arrival fluctuations for optical waves’ propagation through weak anisotropic non-Kolmogorov turbulence, Opt. Exp. 23 (5) (2015) 6313–6325.

[15] L. Cui, B. Xue, F. Zhou, Generalized anisotropic turbulence spectra and applications in the optical waves’ propagation through anisotropic turbulence, Opt. Exp. 23 (23) (2015) 30088–30103.

[16] F. Wang, I. Toselli, J. Li, O. Korotkova, Measuring anisotropy ellipse of atmospheric turbulence by intensity correlations of laser light, Opt. Lett. 42 (6) (2017) 1129–1132.

[17] M. Beason, C. Smith, J. Coffaro, S. Belichki, J. Spychalsky, F. Titus, R. Crabbs, L. Andrews, R. Phillips, Near ground measure and theoretical model of plane wave covariance of intensity in anisotropic turbulence, Opt. Lett. 43 (11) (2018) 2607–2610.

[18] C. Zhai, Fiber-coupling efficiency of a Gaussian-beam in anisotropic non- Kolmogorov turbulence in the presence of random angular jitter, Results in Physics 16 (2020) 102985.

[19] L. C. Andrews, R. L. Phillips, R. Crabbs, Propagation of a Gaussian-beam wave in general anisotropic turbulence, Proc. SPIE 9224 (2014) 922402.

[20] Y. Li, W. Zhu, X. Wu, R. Rao, Equivalent refractive-index structure constant of non-Kolmogorov turbulence, Opt. Exp. 23 (18) (2015) 23004– 23012.

[21] Y. Baykal, H. Gerçekcioğlu, Equivalence of structure constants in non- Kolmogorov and Kolmogorov spectra, Opt. Lett. 36 (23) (2011) 4554–4556.

[22] A. Zilberman, E. Golbraikh, N. S. Kopeika, Propagation of electromagnetic waves in Kolmogorov and non-Kolmogorov atmospheric turbulence: threelayer altitude model, Appl. Opt. 47 (34) (2008) 6385–6391.

[23] L. Cui, Analysis of temporal power spectra for optical waves propagating through weak anisotropic non-Kolmogorov turbulence, J. Opt. Soc. Am. A 32 (6) (2015) 1199–1208.

[24] L. Cui, Influence of general distribution of anisotropic turbulence cells on the temporal power spectra of optical waves, Optik 169 (2018) 156–165.

[25] B. Melissa, A. Larry, T. Italo, Calculating structure function constant from measured Cn^2 in non-Kolmogorov and anisotropic turbulence including inner scale effects, Appl. Opt. 58 (25) (2019) 6813–6819.