arXiv:2301.03294v2 [cs.IT] 22 Feb 2023

Construction of Optimal Binary Z-Complementary Code Sets with New Lengths

Gobinda Ghosh, Sudhan Majhi, Shubabrata Paul

Abstract—Z-complementary code sets (ZCCSs) are used in multicarrier code-division multiple access (MC-CDMA) systems, for interference-free communication over multiuser and quasi-asynchronous environments. In this letter, we propose three new constructions of optimal binary ( R2^{k+1}, 2^{k+1}, Rγ, γ ) -ZCCS, ( R2^{k+1}, 2^{k+1}, R2^{m2} , 2^{m2} ) - ZCCS and ( 2^{k+1}, 2^{k+1}, 3γ, 2γ ) -ZCCS based on generalized Boolean functions (GBFs), where γ = 2^{m1 −1} + 2^{m1 −3}, m1 ≥ 5, k ≥ 1, m2 ≥ 1 and R is any even number. The proposed ZCCSs cover many unreported lengths and large set sizes.

Index Terms—CCC, GBF, MC-CDMA, ZCCS, ZCZ.

I. INTRODUCTION

M^{ULTICARRIER code-division multiple access (MC-}

CDMA) is a popular wireless technique used in many communication systems due to its efficient fast Fourier transform (FFT) based implementation, resistance to intersymbol interference, and high spectral efficiency [1]. However, MC-CDMA can be affected by multiple-access interference (MAI) [2] and multipath interference (MPI) [3]. Adopting proper spreading codes, such as complete complementary codes (CCC) [4] and Z-complementary code sets (ZCCSs) [5], aforementioned problems can be resolved. ZCCS has large code size thus support larger number of users compared to CCC. However, there is a limitation of having flexibility on length and size of the ZCCS code. Fan et al. in [6] proposed ZCCSs, refers to a set of matrices or codes that exhibits zero correlation zone (ZCZ), for MC-CDMA. ZCCS’s correlation properties allow for the deployment of interference-free MC-CDMA in quasisynchronous channels without the need for power regulation [1]. For an (M, N, L, Z)-ZCCS, we have M ≤ N⌊^L_Z ⌋, where M, N, L, Z refers to the set size, number of sub-carrier, length and ZCZ width respectively. When the equality sign is true, ZCCS is said to be an optimal [7]. Binary sequences are easy to use electronically because of modulo-2 arithmetic. Furthermore, modulo-2 arithmetic is isomorphic with the use of {1, −1}, which simplifies both the modulation and correlation processes in signal processing [8]. However, it is often challenging to obtain flexible lengths for binary sequences.

In the literature, numerous ZCCSs have been proposed by using direct [9]–[17] and indirect [18]–[20] constructions. In [9]–[12] binary ZCCS of length power-of-two have been presented. In [13]–[15] ZCCS of non-power-of-two (NPT) length have been presented through generalized Boolean function (GBF); however, they are unable to achieve the binary phase. Sarkar et al. in [16] proposed q-ary

(2^{n+1}, 2^{n+1}, 2^{m−1} + 2, 2^{m−2} + 2^{ψ(m−3)+1})-ZCCS where m ≥ 3 using GBF. In [17], Sun et al. proposed q-ary (2^{k+1}, 2^{k+1}, 3.2^m, 2^{m+1})-ZCCS where m, k ≥ 1 using GBF. Adhikary et al. in [21] proposed an optimal binary (2^{n+1}, 2^{n+1}, N,^{N(N+1)}_2 )-ZCCS by indirect method, where N = 2^{α+1}10^β26^γ , α, β and γ ≥ 1.

Motivated by the scarcity of NPT-length binary optimal ZCCS, this letter proposes three GBF-based direct constructions of binary optimal ZCCS with length Rγ, R2^{m2} and 3γ where γ = 2^{m1−1} + 2^{m1−3}, m_1 ≥ 5, m_2 ≥ 1 and R is any even number. Furthermore, for the first time, the suggested design provides an NPT length set size of the kind R2^{k+1} for k ≥ 1. So, the suggested constructions make a new class of ZCCSs with a length and set size that has never been reported before. II. PRELIMINARY In this section, we introduce some basic ideas and lemmas that will be applied to the rest of the proposed building.

Let u = (u_0, . . . , u_{L−1}) and v = (v_0, . . . , v_{L−1}) consist of two complex valued sequences. We define the aperiodic cross-correlation sum (ACCS) between u and v as

Θ(u, v)(τ) = ∑_{L−1−τ} k=0 u_kv^∗_{k+τ} , 0 ≤ τ < L, ∑_{L+τ −1} k=0 u_{k−τ} v^∗_k, −L < τ < 0, 0, otherwise, (1)

where ∗ stands for the complex conjugate. If u = v, then the corresponding function is known as the aperiodic autocorrelation sum (AACS) of u, refer to ψ(u).

Let C_i = {u^i_k : 0 ≤ k < N} and C_j = {u^j_k : 0 ≤ k < N} be collections of N sequences, where u^i_k = (u^i_{k,0}, . . . , u^i_{k,L−1}) and u^j_k = (u^j_{k,0}, . . . , u^j_{k,L−1}). For two sets of sequence C_i and C_j , the ACCS is defined by

Θ(C_i, C_j )(τ) = N−1∑ k=0 Θ(u^i_k, u^j_k).

Definition 1: Let C = {C_0, . . . , C_{M−1}} be collection of M such sequence sets. The code set C is called a (M, N, L, Z)- ZCCS ( [9]) if

Θ(C_{μ1} , C_{μ2} )(τ) =

NL, τ = 0, μ_1 = μ_2, 0, 0 < |τ| < Z, μ_1 = μ_2, 0, |τ| < Z, μ_1 ≠ μ_2, (2)

where 0 ≤ μ_1, μ_2 ≤ M − 1. When M = N and Z = L, we denote the set C by (M, M, L)-CCC. A. Generalized Boolean Functions (GBFs)

A generalized Boolean function (GBF) f with m variables is a mapping from the set {0, 1}^m to the set Z_q = {0, . . . , q − 1} where, q is a positive integer. The sequence of a GBF f is a Z_q-valued sequence of length N = 2^m defined by ψ(f) = (ω^{f0}_q , . . . , ω^{f2m −1}q ) where ω_q = exp(^{2π√−1}_q ), f_r = f(r_0, . . . , r_{m−1}) and (r_0, . . . , r_{m−1}) is the binary representation of the integer r. We denote ψ_j (f) be the truncated sequence after taking first j terms from ψ(f) i.e., ψ_j (f) = (ω^{f0}_q , . . . , ω^{fj−1}_q ) and ψ^j (f) be the truncated sequence after taking last j terms from ψ(f) i.e, ψ^j (f) = (ω^{f2m −j}_q , . . . , ω^{f2m−1}_q ). Let C = {f^1, . . . , f^r} represents an ordered set of r GBFs, each with m variables. We define the codes ψ(C) = (ψ(f^1), . . . , ψ(f^r)), ψ_j (C) = (ψ_j (f^1), . . . , ψ_j (f^r)) and ψ^j (C) = (ψ^j (f^1), . . . , ψ^j (f^r)).

Lemma 1: (Construction of CCC [22]) Let m_1 ≥ 5, q = 2, Q be a quadratic form in m_1 −4 variables. Let G(Q) be the labeled graph corresponding to Q (see [22]). Assume that G(Q) has k ≤ m_1−5 distinct vertices labeled by 0 ≤ p_0 < p_1 < · · · < p_{k−1} < m − 4 such that after removing those k vertices along with all of the edges connecting them yields a path. Let β_1 be any of the end vertices of the path. For any d, d_i ∈ Z_2, let us define a GBF g : {0, 1}^{m1} → Z_2 as

g(z_0, . . . , z_{m1−1}) = Q + m_1−5∑

i=0 d_iz_i + d + α + β,

where α = z̄_{m1−1} (z̄_{m1−4} (z_{m1−3} + z_{m1−2}) + z_{m1−2}z_{m1−3}) , β = z_{β1} (z̄_{m1−1} (z_{m1−2}z̄_{m1−3}z̄_{m1−4} + z_{m1−2}z_{m1−3}) + z_{m1−1}z̄_{m1−2}z̄_{m1−3}). Let us consider the functions g^{a,n} : {0, 1}^{m1} → Z_2 and s^{a,n} : {0, 1}^{m1} → Z_2 as

g^{a,n}(z_0, . . . , z_{m1−1}) = g + k−1∑ α=0 (a_α + n_α) z_{pα} + az_{β1} , (3)

s^{a,n}(z_0, . . . , z_{m1−1}) = ḡ + k−1∑ α=0 (a_α + n_α) z̄_{pα} + āz_{β1} , (4)

where ḡ(z_0, . . . , z_{m1−1}) = g(z̄_0, . . . , z̄_{m1−1}), z̄_{pα} = 1 − z_{pα} , z̄_i = 1 − z_i, ā = 1 − a, a ∈ {0, 1}, a = (a_0, . . . , a_{k−1}, a) ∈ {0, 1}^{k+1}, (n_0, . . . , n_{k−1}) is the binary vector representation of the integer n for 0 ≤ n < 2^k. Define an ordered set of GBF S_n = { g^{a,n} : a ∈ {0, 1}^{k+1} } and S̄_n = { s^{a,n} : a ∈ {0, 1}^{k+1} } . Then the code set { ψ_γ (S_n) : 0 ≤ n < 2^k } ∪ {( ψ^γ (S̄_n) )_∗ : 0 ≤ n < 2^k } forms a binary (2^{k+1}, 2^{k+1}, 2^{m1−1} +2^{m1−3})-CCC where ( ψ^γ (S̄_n) )_∗ is the complex conjugate of ψ^γ (S̄_n) and γ = 2^{m1−1} + 2^{m1−3}.

Let g^{a,n} and s^{a,n} be the GBFs of m_1 variables z_0, . . . , z_{m1−1} as defined in (3) and (4) respectively. Consider a set

S = {c = (c_0, . . . , c_{l−1}) : 0 ≤ c_i ≤ 1}. (5)

We define the GBFs M^{a,n,c} : {0, 1}^{m1+l} → Z_2 and N^{a,n,c} : {0, 1}^{m1+l} → Z_2 with the help of g^{a,n} and s^{a,n} as M^{a,n,c} = g^{a,n} + ∑_{l−1} i=0 c_iz_{m1+i} and N^{a,n,c} = s^{a,n} + ∑_{l−1} i=0c_iz_{m1+i} respectively.

The sequence ψ(M^{a,n,c}) and ψ(N^{a,n,c}) can be viewed as 2^l parts, i.e., ψ(M^{a,n,c}) = (u_0, . . . , u_2l_{−1}), ψ(N^{a,n,c}) = (v_0, . . . , v_2l_{−1}), where u_j = ψ(g^{a,n})ω ∑_{l−1} i=0 c_ij_i 2 , v_j = ψ(s^{a,n})ω ∑_{l−1} i=0 c_ij_i 2 , (j_0, . . . , j_{l−1}) is the binary representation of j and 0 ≤ j ≤ 2^l − 1. Let γ = 2^{m1−1} + 2^{m1−3}, we define a truncated sequence M^{a,n,c}_{γ,R} = (u^γ_0 , . . . , u^γ_{R−1}) and N^{a,n,c}_{γ,R} = (v^γ_0 , . . . , v^γ_{R−1}) obtained from ψ(M^{a,n,c}) and ψ(N^{a,n,c}) respectively where u^γ_r = ψ_γ (g^{a,n})ω ∑_{l−1} i=0 c_ir_i 2 , v^γ_r = ψ^γ (s^{a,n})ω ∑_{l−1} i=0 c_ir_i 2 , 0 ≤ r < R, R is an even number such that 2 ≤ R ≤ 2^l, and (r_0, . . . , r_{l−1}) is the binary vector representation of the integer r. Now, we define

Ω^c_n= { M^{a,n,c}_{γ,R} : a ∈ {0, 1}^{k+1} } , (6)

Λ^c_n= { ( N^{a,n,c}_{γ,R} )_∗ : a ∈ {0, 1}^{k+1} } . (7)

III. FIRST CONSTRUCTION OF ZCCS In this section, we provide the construction of optimal binary ( R2^k, 2^{k+1}, Rγ, γ ) -ZCCS, where γ = 2^{m1−1} +2^{m1−3}.

Theorem 1: Let m_1 ≥ 5, q = 2 , S_R ⊆ S containing any R elements from the set S and suppose Ω^c_n and Λ^c_n be the set of sequences defined in (6) and (7). Then the code set G = { Ω^c_n, Λ^c_n : 0≤n< 2^k, c ∈ S_R } forms an optimal binary

(R2^{k+1}, 2^{k+1}, Rγ, γ)-ZCCS over Z_2, where R ≥ 2 is an even integer and R ≤ 2^l.

Proof: Let (α_0, . . . , α_{l−1}) be the vector representation of an integer α, where 0 ≤ α ≤ R − 1. For c, c^′ ∈ S_R, 0 ≤ n, n^′ < 2^k, τ = 0, we have Θ ( Ω^c_n, Ω^{c′}_n′ ) (0) = ∑ a Θ ( M^{a,n,c}_{γ,R} , M^{a,n′,c′}_{γ,R} ) (0)

= ∑ a Θ ( ψ_γ (g^{a,n}), ψ_γ (g^{a,n′} ) ) (0) R−1∑ α=0 l−1∏ i=0 ω^{(ci−c′i)αi} 2 = Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (0) R−1∑ α=0 l−1∏ i=0 ω^{(ci−c′i)αi} 2 = { R2^{k+1}γ, (n, c) = (n^′, c^′), 0, (n, c) ≠ (n^′, c^′).

(8)

Now, by (6), (7) and Lemma 1, the ACCS between Ω^c_n and Ω^{c′}_n′ for 0 < |τ| < γ can be expressed as Θ ( Ω^c_n, Ω^{c′}_n′ ) (τ) = ∑ a Θ ( ψ_γ (g^{a,n}), ψ_γ (g^{a,n′} ) ) (τ) R−1∑ α=0 l−1∏ i=0 ω^{(ci−c′i)αi} 2 + ∑ a Θ ( ψ_γ (g^{a,n}), ψ_γ (g^{a,n′} ) ) (τ − γ) R−2∑ α=0 l−1∏ i=0 ω^{ci(αi)−c′i(α′i)} 2 = Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (τ) R−1∑ α=0 l−1∏ i=0 ω^{(ci−c′i)αi} 2 + Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (τ − γ) R−2∑ α=0 l−1∏ i=0 ω^{ci(αi )−c′i(α′i )} 2 , (9) where (α^′_0, . . . , α^′_{l−1}) is the binary representation of α + 1. From Lemma 1, we obtain Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (τ) = 0, 0 < |τ| < γ. (10) From (9) and (10), we have

Θ ( Ω^c_n, Ω^{c′}_n′ ) (τ) = 0, 0 < |τ| < γ. (11) In the similar way, it can be shown that Θ ( Λ^c_n, Λ^{c′}_n′ ) (τ) = { R2^{k+1}γ, (n, c) = (n^′, c^′), τ = 0, 0, (n, c) ≠ (n^′, c^′), 0 ≤ |τ| < γ. (12)

Now, by (6), (7) and Lemma 1, the ACCS between Ω^c_n and Λ^{c′}_n′ for τ = 0 can be expressed as Θ ( Ω^c_n, Λ^{c′}_n′ ) (0) = Θ ( ψ_γ (S_n), ( ψ^γ (S̄_n′ ) )_∗ ) (0) R−1∑ α=0 l−1∏ i=0 ω^{(ci+c′i)αi} 2 (13)

From Lemma 1, we obtain Θ ( ψ_γ (S_n), ( ψ^γ (S̄_n′ ) )_∗ ) (0) = 0. (14)

From (13) and (14) we have Θ ( Ω^c_n, Λ^{c′}_n′ ) (0) = 0. (15)

Now, by (6), (7) and Lemma 1, the ACCS between Ω^c_n and Λ^{c′}_n′ for 0 < |τ| < γ can be expressed as Θ ( Ω^c_n, Λ^{c′}_n′ ) (τ) = Θ ( ψ_γ (S_n), ( ψ^γ (S̄_n′ ) )_∗ ) (τ) R−1∑ α=0 l−1∏ i=0 ω^{(ci+c′i)αi} 2 + Θ ( ψ_γ (S_n), ( ψ^γ (S̄_n′ ) )_∗ ) (τ − γ) R−2∑ α=0 l−1∏ i=0 ω^{ci(αi)+c′i(α′i )} 2 . (16)

From Lemma 1, we obtain Θ ( ψ_γ (S_n), ( ψ^γ (S̄_n′ ) )_∗ ) (τ) = 0, 0 < |τ| < γ. (17) From (16) and (17) we have Θ ( Ω^c_n, Λ^{c′}_n′ ) (τ) = 0, 0 < |τ| < γ. (18) Thus, from (8), (11), (12), (15), and (18), it can be concluded that the set G forms an optimal binary ( R2^{k+1}, 2^{k+1}, Rγ, γ ) -ZCCS.

IV. SECOND CONSTRUCTION OF ZCCS In this section we provide optimal binary (R2^{k+1}, 2^{k+1}, R2^{m2} , 2^{m2} )-ZCCS through GBF.

Lemma 2: (Construction of CCC [4]) Let q be an even, m_2 ≥ 1, f be a GBF of m_2 variables. Consider a graph G(f) which contains a set of k unique vertices labeled as 0 ≤ p_0 < · · · < p_{k−1} < m_2 such that if these k vertices are removed from the graph, it will be a path. Let β_1 be any of the end vertices of the path. Let us consider the functions f^{a,n} : {0, 1}^{m2} → Z_q and h^{a,n} : {0, 1}^{m2} → Z_q as f^{a,n}(z_0, . . . , z_{m2−1})=f +^q_2 ( ∑_{k−1} α=0 (a_α + n_α) z_{pα} +az_{β1} ) , h^{a,n}(z_0, . . . , z_{m2−1}) = f̄ +^q_2 ( ∑_{k−1} α=0(a_α +n_α)z̄_{pα} + āz_{β1} ) . Define an ordered sets G_n = { f^{a,n} : a ∈ {0, 1}^{k+1} } and Ḡ_n = {ha,n : a ∈ {0, 1}k+1} . Then {ψ(G_n), (ψ(Ḡ_n))^∗ : 0 ≤ n < 2^k} forms q-ary (2^{k+1}, 2^{k+1}, 2^{m2} )-CCC.

We define a GBF R^{a,n,c} : {0, 1}^{m2+l} → Z_q and S^{a,n,c} : {0, 1}^{m2+l} → Z_q as R^{a,n,c} = f^{a,n} +^q_2 ∑_{l−1} i=0 c_iz_{m2+i} and S^{a,n,c} = h^{a,n} +^q_2 ∑_{l−1} i=0c_iz_{m2+i} respectively. Therefore, we have ψ(R^{a,n,c}) = (e_0, . . . , e_2l_{−1}), ψ(S^{a,n,c}) = (p_0, . . . , p_2l_{−1}), where e_j = ψ(f^{a,n})ω ∑_{l−1} i=0 c_ij_i 2 , p_j = ψ(h^{a,n})ω ∑_{l−1} i=0 c_ij_i 2 . We define truncated sequence U^{a,n,c} = (e_0, . . . , e_{R−1}) and V^{a,n,c} = (p_0, . . . , p_{R−1}) obtained from ψ(R^{a,n,c}) and ψ(S^{a,n,c}) respectively. Now, in the similar way as Lemma 1 we can define

Φ^c_n= { U^{a,n,c} : a ∈ {0, 1}^{k+1} } , (19)

Δ^c_n= { (V^{a,n,c})^∗ : a ∈ {0, 1}^{k+1} } . (20)

Theorem 2: Consider a set S = {c = (c_1, . . . , c_l) : c_i ∈ {0, 1}}, suppose Φ^c_n and Δ^c_n be the set of sequences as defined in (19) and (20) respectively. Let S_R ⊆ S consists any R

elements from the set S, then the code set G = { Φ^c_n, Δ^c_n : 0≤ n < 2^k, c ∈ S_R } forms an q-ary (R2^k, 2^{k+1}, R2^{m2} , 2^{m2} )-

ZCCS over Z_2, where q, R ≥ 2 are even integers and R ≤ 2^l.

Proof: The proof is exactly analogous to the Theorem 1.

V. THIRD CONSTRUCTION OF ZCCS In this section, we provide optimal binary (2^{k+1}, 2^{k+1}, 3γ, 2γ)-ZCCS construction by using GBF.

We define the function F^{a,n} : {0, 1}^{m1+2} → Z_2 and G^{a,n} : {0, 1}^{m1+2} → Z_2 with the help of g^{a,n} and s^{a,n} as F^{a,n} = g^{a,n} + z_{m1+1} and G^{a,n} = s^{a,n} + z_{m1+1} respectively. The sequences ψ(F^{a,n}) and ψ(G^{a,n}) can be written as ψ(F^{a,n}) = ( ψ(g^{a,n}), ψ(g^{a,n}), −ψ(g^{a,n}), −ψ(g^{a,n}) ) , ψ(G^{a,n}) = ( ψ(s^{a,n}), ψ(s^{a,n}), −ψ(s^{a,n}), −ψ(s^{a,n}) ) . (21)

We define the truncated sequence ψ_T (F^{a,n}) and ψ_T (G^{a,n}) obtained from ψ(F^{a,n}) and ψ(G^{a,n}) as

ψ_T (F^{a,n}) = ( ψ_γ (g^{a,n}), ψ_γ (g^{a,n}), −ψ_γ (g^{a,n}) ) , (22) ψ_T (G^{a,n}) = ( ψ^γ (s^{a,n}), ψ^γ (s^{a,n}), −ψ^γ (s^{a,n}) ) . (23)

where ψ_γ (g^{a,n}) = (ω^{ga,n0}_2 , . . . , ω^{ga,nγ−1}_2 ) and ψ^γ (s^{a,n}) = (ω^s a,n 2m−γ 2 , . . . , ω^s a,n 2m−1 2 ), g^{a,n}_r = g^{a,n}(r_0, . . . , r_{m−1}), s^{a,n}_r = s^{a,n}(r_0, . . . , r_{m−1}), (r_0, . . . .r_{m−1}) is the binary vector representation of the integer r and 0 ≤ r ≤ 2^m − 1 .

Theorem 3: Let ψ_T (F^{a,n}) and ψ_T (G^{a,n}) be the sequences as defined in (22) and (23) respectively. We define the order sets C_n = {ψ_T (F^{a,n}) : a ∈ {0, 1}^{k+1}}, C̄_n = {ψ_T (Ga,n) : a ∈ {0, 1}k+1}. Then the code set { C_n : 0 ≤ n < 2^k } ∪ {( C̄_n)^∗ : 0 ≤ n < 2k } , forms an optimal binary (2^{k+1}, 2^{k+1}, 3γ, 2γ)-ZCCS.

Proof: For 0 ≤ n, n^′ < 2^k, τ = 0 the AACS between C_n and C_n′ can be derive as Θ ( C_n, C_n′ ) (0) = ∑ a Θ ( ψ_T (F^{a,n}), ψ_T (F^{a,n′} ) ) (0) = 3 ∑ a Θ ( ψ_γ (g^{a,n}), ψ_γ (g^{a,n′} ) ) (0) = 3Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (0) (24)

By using Lemma 1 and (24), we have Θ ( C_n, C_n′ ) (0) = { 32^{k+1}γ n = n^′; 0 n ≠ n^′. (25)

When 0 < τ < γ Θ ( C_n, C_n′ ) (τ) = 3Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (τ)+Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (γ − τ) − Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (γ − τ). (26)

Using Lemma 1 and (26), we have Θ ( C_n, C_n′ ) (τ) = 0. (27)

When τ = γ Θ ( C_n, C_n′ ) (γ) = Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (0) − Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (0) = 0 (28)

When γ < |τ| < 2γ − 1, we have Θ ( C_n, C_n′ ) (τ) =Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (τ −γ)−Θ ( ψ_γ (S_n),ψ_γ (S_n′ ) ) (τ − γ) − Θ ( ψ_γ (S_n), ψ_γ (S_n′ ) ) (2γ − τ). (29)

Using Lemma 1 and (29), we have Θ ( C_n, C_n′ ) (τ) = 0. (30)

In a similar way it can be shown that Θ (( C̄_n)^∗,(C̄_{n′} )^∗ ) (τ)= { 32^{k+1}γ n = n^′, τ = 0; 0 n ≠ n^′, 0 ≤ |τ| ≤ 2γ − 1. (31)

By similar argument, ∀τ, 0 ≤ |τ| ≤ 2γ − 1 and we have Θ ( C_n, (¯ C_n′ )_∗ ) (τ) = 0. (32)

Hence, from (25),(27),(30),(31) and (32) the result follws.

Example 1: For m_1 = 8, q = 2, l = 1, R = 2, let us assume Q : {0, 1}^4 → Z_q be a quadratic form in variables z_0, z_1, z_2, z_3, i.e., Q (z_0, z_1, z_2, z_3) = z_0z_1 + z_1z_2 + z_2z_3 + z_3z_0 + z_0z_2. Let d_0 = 1, d_1 = 1, d_2 = 1, d_3 = 1, d = 0, and define the GBF g : {0, 1}^8 → Z_2 with the help of Q as g(z_0, . . . , z_7) = Q +

∑_3

i=0 d_iz_i + d + α + β, where α = z̄_7 ( z̄_4(z_5 + z_6) + z_6z_5 ) , β = z_2 ( z̄_7(z_6z̄_5z̄_4 +z_6z_5) + z_7z̄_6z̄_5 ) . Let k = 2, c = c_0 and a = (a_0, a_1, a) ∈ {0, 1}^3 where, 0 ≤ c_0 < 1 and 0 ≤ n ≤ 3. Consider the function g^{a,n} : {0, 1}^8 → Z_2 and s^{a,n} : {0, 1}^8 → Z_2 as g^{a,n} = g +

∑_1 α=0(a_α + n_α)z_α + az_1, s^{a,n} = g̃ +

∑_1 α=0(a_α + n_α)z̄_α + (1 − a)z_1. Therefore, M^{a,n,c0} = g^{a,n} + c_0z_8, N^{a,n,c0} = s^{a,n} + c_0z_8. We have γ = 160 and M^{a,n,c0}_{160,2} and N^{a,n,c0}_{160,2} are the truncated sequences obtained from M^{a,n,c0} and N^{a,n,c0} respectively as M^{a,n,c0}_{160,2} = (A^{160}_0 , A^{160}_1 ), N^{a,n,c0} 160,2 = (B 160 0 , B^{160}_1 ), where, A^{160}_0 = ψ_{160}(g^{a,n}), A^{160}_1 = ψ_{160}(g^{a,n})ω^{c0}_2 , B^{160}_0 = ψ^{160}(s^{a,n}), B^{160}_1 = ψ^{160}(s^{a,n})ω^{c0}_2 .

Again from (6) and (7), we have Ω^c_n= { M^{a,n,c}_{160,2} : a ∈ {0, 1}^3 } , Λ^c_n = { ( N^{a,n,c}_{160,2} )_∗ : a ∈ {0, 1}^3 } . Therefore, by Theorem 1,

the set G = { Ω^c_n, Λ^c_n : 0 ≤ n ≤ 3, 0 ≤ c_1 ≤ 1 } , forms an binary optimal (16, 8, 320, 160)-ZCCS.

Example 2: For m_1 = 8, q = 2, k = 2, a = (a_0, a_1, a) ∈ {0, 1}^3 and 0 ≤ n ≤ 3. Consider the function g^{a,n} : {0, 1}^8 → Z_2 and s^{a,n} : {0, 1}^8 → Z_2 be same as (3) and (4) respectively. Therefore, we have F^{a,n} = g^{a,n} + z_9 and G^{a,n} = s^{a,n} + z_9. After truncation, we left with the sequences ψ_T (F^{a,n}) = ( ψ_{160}(g^{a,n}), ψ_{160}(g^{a,n}), −ψ_{160}(g^{a,n}) ) , ψ_T (G^{a,n}) = ( ψ^{160}(s^{a,n}), ψ^{160}(s^{a,n}), −ψ^{160}(s^{a,n}) ) . Therefore, we have C_n = {ψ_T (F^{a,n}) : a ∈ {0, 1}^3}, C̄_n = {ψ_T (G^{a,n}) : a ∈ {0, 1}^3}. Hence, by Theorem 3, we conclude that the set {C_n : 0 ≤ n < 4} ∪ {( C̄_n)^∗ : 0 ≤ n < 4 } , forms an optimal binary (8, 8, 480, 320)-ZCCS. A. Comparative Analysis with Prior Works

Using an orthogonal binary ZCP, Adhikary et al. in [21] proposed an optimal binary (2^{n+1}, 2^{n+1}, N,^{N(N+1)}_2 )-ZCCS where N = 2^{α+1}10^β26^γ. The GBFs-based constructions in [16], [17] provide binary optimal (2^{n+1}, 2^{n+1}, 2^{m−1} + 2, 2^{m−2} + 2^{ψ(m−3)+1})-ZCCS and (2^{k+1}, 2^{k+1}, 3.2^m, 2^{m+1})- ZCCS respectively. Our approach does not depend on any initial sequence and matrices and provides three new classes of optimal binary ( R2^{k+1}, 2^{k+1}, Rγ, γ ) -ZCCS, ( R2^{k+1}, 2^{k+1}, R2^{m2} , 2^{m2} ) -ZCCS and ( 2^{k+1}, 2^{k+1}, 3γ, 2γ ) - ZCCS. TABLE I compares our work with [16], [17], and [21].

TABLE I: COMPARISON WITH EXISTING BINARY OPTIMAL NPT ZCCS

Source Based On Parameters Conditions [16] Direct (2^{n+1}, 2^{n+1}, 2^{m−1} + 2, 2^{m−2} + 2^{ψ(m−3)+1}) v ≤ m, q ≥ 2, m ≥ 2 [17] Direct (2^{k+1}, 2^{k+1}, 3.2^m, 2^{m+1}) m, k ∈ Z^+ [21] Indirect (2^{n+1}, N, 2^{n+1}, Z) N ≥ 3, N = length of OB-ZCP Thm. 1 Direct ( R2^{k+1}, 2^{k+1}, Rγ, γ ) m ≥ 5, k ∈ Z^+, γ = 2^{m−1} + 2^{m−3}, R is even Thm. 2 Direct ( R2^{k+1}, 2^{k+1}, R2^m, 2^m ) m ≥ 5, k ∈ Z^+, R is even Thm. 3 Direct ( 2^{k+1}, 2^{k+1}, 3γ, 2γ ) m ≥ 5, k ∈ Z^+, γ = 2^{m−1} + 2^{m−3}

Remark 1: By the similar calculation as in [9, Remark 3] and [15, Remark 3], Theorem 1, and Theorem 3, produce at least 2^{m1−3 (m1−3)!}_{2k!} 2(^{k2}) number of non-overlapping ZCCSs and Theorem 2, produces at least q^{m2 +1 m2!}_{2k!} (q−1)^{k(m2 −k)}q(^{k2}) number of non-overlapping ZCCSs.

Remark 2: [13], [15] offer NPT-length ZCCS through GBF, but their phase depends on the length. For example, ZCCS of length 60, [13], [15] have a phase of sequences of 30, however, we have 2. Due to noise and interference, transmitted symbols over Z_σ with large value of σ require additional bits for quantization, increasing symbol error probability [24]. Our method yields high NPT length ZCCS with binary phase, unlike [13], [15]. VI. C_{ONCLUSION}

Three families of new optimal binary ZCCSs with novel parameters are proposed in this work. The structures are based on GBFs and we propose three distinct direct methods to generate optimal binary ( R2^{k+1}, 2^{k+1}, Rγ, γ ) -ZCCS, ( R2^{k+1}, 2^{k+1}, R2^{m2} , 2^{m2} ) -ZCCS and ( 2^{k+1}, 2^{k+1}, 3γ, 2γ ) - ZCCS respectively, where γ = 2^{m1−1} + 2^{m1−3}, m_1 ≥ 5, k ≥ 1, m_2 ≥ 1 and R is any even number. Our methods create three new classes of binary ZCCSs with unique lengths and set sizes, which are not found in any existing literature.

REFERENCES

[1] H. Chen, The next generation CDMA technologies. John Wiley & Sons, 2007.

[2] D. Carey, D. Roviras, and B. Senadji, “Comparison of multiple access interference in asynchronous MC-CDMA and DS-CDMA systems,” in Proceedings Seventh International Symposium on Signal Processing and Its Applications, vol. 2, 2003, pp. 351–354.

[3] P. Nagaradjane, A. Swaminathan, K. Dhyaneshwaran, B. R.

Narayanasamy, and A. Ramakrishnan, “Multipath interference mitigation technique for MC DS/CDMA systems,” in International Conference on Control, Automation, Communication and Energy Conservation, 2009, pp. 1–3.

[4] A. Rathinakumar and A. Chaturvedi, “Complete mutually orthogonal Golay complementary sets from Reed–Muller codes,” IEEE Trans. Inf. Theory, vol. 54, no. 3, pp. 1339–1346, 2008.

[5] J. A. Davis and J. Jedwab, “Peak-to-mean power control in OFDM, Golay complementary sequences, and Reed-Muller codes,” IEEE Trans. Inf. Theory, vol. 45, no. 7, pp. 2397–2417, Nov. 1999.

[6] P. Fan, W. Yuan, and Y. Tu, “Z-complementary binary sequences,” IEEE Signal Process. Lett., vol. 14, no. 8, pp. 509–512, 2007.

[7] Z. L. Liu, Y. L. Guan, B. C. Ng, and H.-H. Chen, “Correlation and set size bounds of complementary sequences with low correlation zone,” IEEE Trans. Commun., vol. 59, no. 12, pp. 3285–3289, 2011.

[8] J. G. Proakis, Digital signal processing: principles, algorithms, and applications, 4/E. Pearson Education India, 2007.

[9] P. Sarkar, S. Majhi, and Z. Liu, “Optimal Z-complementary code set from generalized Reed-Muller codes,” IEEE Trans. Commun, vol. 67, no. 3, pp. 1783–1796, 2018.

[10] S. Wu and C. Chen, “Optimal Z-complementary sequence sets with good peak-to-average power-ratio property,” IEEE Signal Process. Lett., vol. 25, no. 10, pp. 1500–1504, 2018.

[11] P. Sarkar and S. Majhi, “A direct construction of optimal ZCCS with maximum column sequence PMEPR two for MC-CDMA system,” IEEE Commun. Lett., vol. 25, no. 2, pp. 337–341, 2020.

[12] S. Wu, A. Şahin, Z. Huang, and C. Chen, “Z-complementary code sets with flexible lengths from generalized Boolean functions,” IEEE Access, vol. 9, pp. 4642–4652, 2020.

[13] P. Sarkar, S. Majhi, and Z. Liu, “Pseudo-Boolean Functions for Optimal Z-complementary Code Sets with Flexible Lengths,” IEEE Signal Process. Lett., vol. 28, pp. 1350–1354, 2021.

[14] B. Shen, H. Meng, Y. Yang, and Z. Zhou, “New constructions of Z-complementary code sets and mutually orthogonal complementary sequence sets,” Designs, Codes and Cryptography, pp. 1–19, 2022.

[15] G. Ghosh, S. Majhi, P. Sarkar, and A. K. Upadhaya, “Direct construction of optimal Z-complementary code sets with even lengths by using generalized Boolean functions,” IEEE Signal Process. Lett., vol. 29, pp. 872–876, 2022.

[16] P. Sarkar, A. Roy, and S. Majhi, “Construction of Z-complementary code sets with non-power-of-two lengths based on generalized Boolean functions,” IEEE Commun. Lett., vol. 24, no. 8, pp. 1607–1611, 2020.

[17] C. Xie, Y. Sun, and Y. Ming, “Constructions of optimal binary Zcomplementary sequence sets with large zero correlation zone,” IEEE Signal Process. Lett., vol. 28, pp. 1694–1698, 2021.

[18] A. Adhikary and S. Majhi, “New construction of optimal aperiodic Zcomplementary sequence sets of odd-lengths,” vol. 55, no. 19, pp. 1043– 1045, 2019.

[19] T. Yu, A. R. Adhikary, Y. Wang, and Y. Yang, “New class of optimal Z-complementary code sets,” IEEE Signal Process. Lett., vol. 29, pp. 1477–1481, 2022.

[20] S. Das, U. Parampalli, S. Majhi, Z. Liu, and S. Budišin, “New optimal Z-complementary code sets based on generalized paraunitary matrices,” IEEE Trans. Signal Process, vol. 68, pp. 5546–5558, 2020.

[21] A. Adhikary and S. Majhi, “New construction of optimal aperiodic Zcomplementary sequence sets of odd-lengths,” Electron. Lett., vol. 55, no. 19, pp. 1043–1045, 2019.

[22] P. Kumar, S. Majhi, and S. Paul, “A direct construction of Golay complementary pairs and binary complete complementary codes of length non-power of two,” IEEE Trans. Commun., 2023.

[23] P. Ke and Z. Zhou, “A generic construction of Z-periodic complementary sequence sets with flexible flock size and zero correlation zone length,” IEEE Signal Process. Lett., vol. 22, no. 9, pp. 1462–1466, Sep. 2015.

[24] M. Lotter and L. Linde, “A comparison of three families of spreading sequences for cdma applications,” in Proceedings of IEEE South African Symposium on Communications and Signal Processing, 1994, pp. 68–75.